{"text_format":"1","workbook":"xlsx","n_sheets":72,"sheets":["Log-fil","Oversigt over Sheetsark i JAGG","Opstart","Dataark_Opstart","Vejledning_Opstart","Enkeltstoffer","Dataark_Enkeltstoffer","Beregning_Enkeltstoffer","Udskrift_Enkeltstoffer","Vejledning_Enkeltstoffer","Grundvand","Dataark_Grundvand","Beregning_Grundvand","Udskrift_Grundvand","Vejledning_Grundvand","Indeklima","Indeklima_Krybekælder","Dataark_Indeklima","Beregning_Indeklima","Udskrift_Indeklima","Udskrift_Indeklima_KK","Vejledning_Indeklima","Udeluft","Dataark_Udeluft","Beregning_Udeluft","Udskrift_Udeluft","Vejledning_Udeluft","Vertikal Transport","Dataark_Vertikal_Transport","Beregning_Vertikal_Transport","Udskrift_Vertikal_Transport","Vejledning_Vertikal_Transport","Oliestoffer","Dataark_Oliestoffer","Beregning_Oliestoffer","Udskrift_Oliestoffer","Vejledning_Oliestoffer","Grundvand-Olie","Dataark_Grundvand-Olie","Beregning_Grundvand-Olie","Udskrift_Grundvand-Olie","Vejledning_Grundvand-Olie","Indeklima-Olie","Indeklima-Olie_Krybekælder","Dataark_Indeklima-Olie","Beregning_Indeklima-Olie","Udskrift_Indeklima-Olie","Udskrift_Indeklima_KK-Olie","Vejledning_Indeklima-Olie","Udeluft-Olie","Dataark_Udeluft-Olie","Beregning_Udeluft-olie","Udskrift_Udeluft-Olie","Vejledning_Udeluft-Olie","Vertikal Transport-Olie","Dataark_Vertikal-Olie","Beregning_Vertikal-Olie","Vejledning_Vertikal-Olie","Udskrift_Vertikal-Olie","Aquifermateriale","Eget Aquifermateriale","Beton","Min Beton","Jordtyper","Mine Jordtyper","Membraner","Mine Membraner","Netto Nedbør","Egen Netto Nedbør","Stofdatabase","Egen Stofdatabase","Etageadskillelse"],"not_rendered":{"charts":93,"images":389,"macros":1,"external_links":1,"defined_names":9886,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Log-fil","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":true,"merged":[]}
["Initialer","Filnavn","Ændringer","Bemærkning","Dato"]
["VIHU","JAGG_310809","Justeringer af layout på Ude, Ver, Uds Enk, Gru og Ind. Har opdateret navngivning på Ver og referet celler til D_Ver.","Jeg har skrvet kommentaret i D_Ver, som der skal findes en løsning på.","2009-08-31"]
["JAF","JAGG_020909","Har indtastet stofdata i enkeltstof ark. Var nød til at slette sidst linie i VBA kode for module 10 Fejlfukk = fejlfunk, idet jeg har en dansk version af Office 2007 og fejlfunk er en funktion ???. Det virker nu ihvert fald på mit maskin. Har tastet bedre inputdata i Vertikal ark,  derfor kan figur beregnes \n","Har svaret på en del af Victors spørgsmål, om hvor data kommer fra og der er et par parametre som skal beregnes - men har ikke indført beregningsfornel i beregningsark. Vertikal transport kan ikke nedbrydningskonstant =0","2009-09-02"]
[null,"JAGG_160909","Fået listetabel for kemiske stoffer til at virke. Har arbejdet med konstanter på Enk og D_Enk. Har lavet datahenvisninger i Ver og D_Ver. Har tilføjet nogle få nye kommentarer til D_Ver","Jeg har ændret input af kemiske stoffer, således at alle brugerdata indføres på Enk."]
["JAF","Jagg_170909","i datark enkeltstoffer har indsat formel for Koc. I datark vertikal transport har kopiet visse linier for retardation ( stofafhængig) og Dispersion ( ikke stofafhængig )  til de rigtig blok og har rette formel for disse- de oprindeligelinier skal slettes. Jeg har indsat formel for Mydata i sølje for indtastet data  for en række stofparametre som f.eks. henry og Koc.På brugerfladen har rettet formel for Volumenvægt således at der kan håndteres entet standard data eller indtastet data og har navngivne D-Ver_rhob. ","Der er en række visuel basic fejl på  mit pc og forskellig knap kan ikke køre derfor har jeg blot rette formel og navn ( office 2007 er dansk) ","2009-09-16"]
["ANI","JAGG_250909","Der er foretaget rettelser i Vertikal transport og implementeret ét beregningsark for alle vertikale Err. Funktioner. Det har umiddelbart forbedret performance betydeligt! Der er ikke hentet data om på input arket.",null,"2009-09-25"]
["JAF","Jagg_270909","Ændret Datark_enkeltstoffer G37 og G39 fra Hvis(værdi(….. Til Hvis(er.tal(f37);f37; e37) samt for stof 2, 3 og 4. Ligeledes i dataark_vertikal tansport er J27 ændret til H27 og ligeledes J28, 29 samt for stof 2, 3 og 4. I beregningsark _vertikal transport er der fejl i formel i h17 - skal være ^1,5 ( ikke ^2,5)beregning_vertikalark er formel i  \n","Kontrol af Vertikal transport beregning - der skal være muligt at anvende 0 som nedbrydningskonstant- derfor er rettet. Fejl i formel for effektiv diffusion koefficient er rettet","2009-09-27"]
["VIHU","JAGG_071009","Opdateret userforms i forhold til stoffer. Andre ændringer i makroer",null,"2009-10-07"]
["JAF","JAGG 091009","har tilføjet de sidste henvisning i brugerflade og datark ivertikal transport. Har rette et par fejl i brugerfalden for grundvand","indstilling er sat til manual beregning","2009-10-09"]
["ANI","JAGG_191009","Har påbegyndt implementering af Grundvandsberegninger. Samt dataark for grundvandsberegninger",null,"2009-10-19"]
["ANI","JAGG_231009","Fortsat implementering af grundvandsberegninger",null,"2009-10-23"]
["VIHU","JGGG_291009","Grundvandsbrugerflade er opdateret. Bedre integration mellem brugerflade og dataark. Oliekomponent dataark og bergegningsark tilføjet",null,"2009-10-29"]
["ANI","JAGG_301009","Fortsat implementering af grundvandsberegninger",null,"2009-10-30"]
["JAF","JAGG_311009","Kontrol og rettelser til Grundvandsdel og vertikaltransport","Påbegyndt indsætning af navne til vising af værdi i brugerfladen samt figurer","2009-10-31"]
["ANI","JAGG_021109","Implementering af Beregningsark til grundvandsberegninger.","Der mangler fortsat afgørelse omkring afstandsdataets dataflow mellem dataark, beregningsark og brugerflade.","2009-11-02"]
["ANI","JAGG_041109","Implementering af beregningsark til udeluft samt tilføjelse af navne på afstandsdata for grundvandsbereginger jf. d. 02-11-2009",null,"2009-11-02"]
["VIHU","JAGG_131109","Grundvand brugerflade opdateret efter aftale med JAF. Oliemodulet sammenhæng mellem Olie, D_Olie og B_Olie",null,"2009-11-13"]
["VIHU","JAGG_021209","Lizzis stofdatabase er tilføjet",null,"2009-12-02"]
["VIHU","JAGG_101209","Udskriftsark af grundvand og udluft rettet til. Tilføjelse af funktioner i Udeluft, Grundvand, Indeklima og Enkeltstoffer, som sletter al bruger data. Ændring af dataaflevring fra systemværdier. Alle værdier afleveres direkte til dataark","Der er nogle ting, som NIRAS må se på ift udskriftsarkene, idet de relevante data mangler i dataark","2009-12-10"]
["jaf","JAGG 040110","Rettelse og kontrol af alle ark for enkeltstoffer, udeluft, grundvand og vertikal , herunder mangler data til udskrifter jf. VIHU","Mangler at indsatte henvisning til flere data i udskrift for vertikal stoffer","2010-01-04"]
["TVB","JAGG 220110","Alle ark er ordned efer gangordning\nAlle felter på alle indtastningsark, dataark, beregningsark og visningsark er skrivebeskyttet, undtagen felter der skal kunne skrives i",null,"2010-01-22"]
["VIHU","JAGG 250110_c","Funktion. så det er muligt at opdatere egen liste er ordnet. Knapper til at bevæde sig er ordnet",null,"2010-01-25","Kode: JAGG2"]
["JAF","JAGG 230410","Rettelse og kontrol af alle ark for enkeltstoffer, udeluft, grundvand og vertikal , herunder mangler data til udskrifter jf. notat af 26-012010 samt ved workshoppenVIHU",null,"2010-04-23"]
["JAF","JAGG 270410","I.udkast til udeluftolie","Henvisning følger ikke protokol med dataark og beregningsark endnu","2010-04-27"]
["JAF","JAGG 280510","Grundvandolie _dataark, beregningsark + Udskriftsark\nUdeluftolie_ udskriftsark+rettelser",null,"2010-05-28"]
["VIHU","JAGG_10-05-28_VIHU","Indklima-olie: navngivet samt dataark. Overførselknapper fra udeluft of grundvand virker - enkeltstoffer/oliemodul",null,"2010-05-28"]
["VIHU","JAGG_10-05-31_VIHU","Overførselknap indklima. Navngivning Beregning_indeklima. Udskiftet stofdatabase. Udskrift Enkeltstoffer opdateret",null,"2010-05-31"]
["VIHU","JAGG_10-06-01_VIHU","Udskriftsark er blevet gennemgået. Knapper for slet indhold er blevet ordnet",null,"2010-06-01"]
["VIHU","JAGG_10-09-09_VIHU","Indeklima og Indeklima-Olie er blevet delt op på to ark. Knapper er tilføjet og funktionalitet på knapper er tjekket",null,"2010-07-09"]
["VIHU","JAGG-BETA-3","verførsel af data og nulstil for ind og indolie er ordnet",null,"2010-07-12"]
["JAF","JAGG-BETA-6","Beregninger kontrolleret og små fejl rettet, herunder ved ændringer mellem let og tung olie forudeluft og grundvandsmoduller.Mulighed for anvendelse af én nedbrydningskonstant for grunvand olie er tilføjet. DESUDEN er der tilføjet modul for vertikal transport af oliestoffer. Knapper til navigation, nulstilling af alle værdier og til kommentering mangler redigering - navn til kommentar er dog defineret.",null,"2010-08-11"]
["TVB","JAGG-BETA-6,4","Indeklima beregninger for oliemodulet er lagt ind, både med udskriftsark og vejledninger. Der er foretaget mindre rettelser i specielt udskriftarkenes valideringsregler. Alle ark er gennemgået med hensyn til funktionalitet af knapper",null,"2010-12-03"]
["VIHU","JAGG-BETA-6_7","Rettelser lavet",null,"2010-12-21"]
["TVB","JAGG-GAMMA","Navne på celler og datas oprindelse er rettet på alle data og beregningsark, rækkefølgen af fanebladene er rettet til GV, IND, UD, Vertikal"]

{"sheet":"Oversigt over Sheetsark i JAGG","index":1,"n_rows":157,"n_cols":7,"rows_kept":157,"cut":false,"hidden":true,"merged":[[152,0,153,0],[152,1,153,1],[152,2,153,2],[152,3,153,3],[154,0,155,0],[154,1,155,1],[154,2,155,2],[154,3,155,3],[147,0,149,0],[147,1,149,3],[150,0,151,0],[150,1,151,1],[150,2,151,3],[101,0,102,0],[101,1,102,1],[101,2,102,2],[101,3,102,3],[86,0,87,0],[86,1,87,1],[99,0,100,0],[99,1,100,1],[99,2,100,3],[82,0,83,0],[82,1,83,1],[82,2,83,3],[84,0,85,0],[84,1,85,1],[84,2,85,2],[84,3,85,3],[60,2,61,3],[62,0,63,0],[62,1,63,1],[62,2,63,2],[62,3,63,3],[51,0,52,0],[51,1,52,1],[80,0,81,0],[60,0,61,0],[60,1,61,1],[64,0,65,0],[64,1,65,1],[47,0,48,0],[47,1,48,1],[47,2,48,3],[49,0,50,0],[49,1,50,1],[49,2,50,2],[49,3,50,3],[31,2,32,3],[33,0,34,0],[33,1,34,1],[33,2,34,2],[33,3,34,3],[21,0,22,0],[21,1,22,1],[35,0,36,0],[35,1,36,1],[31,0,32,0],[31,1,32,1],[17,0,18,0],[17,1,18,1],[17,2,18,3],[19,0,20,0],[19,1,20,1],[19,2,20,2],[19,3,20,3],[0,0,0,3],[1,0,1,3],[5,0,6,0],[5,1,6,1],[5,2,6,3]]}
["Ark",null,null,null,"Initialer","Udført","Aktion"]
["Logfil"]
["Opstart",null,null,"Vejledning","VIHU","OK","GENERELT: Lukker ikke vejlednings ark ved navigation til andre ark"]
[null,null,null,"Dataark","VIHU","OK","GENERELT: Lukker ikke data ark ved navigation til andre ark"]
[null,null,null,null,"VIHU","OK","NULSTIL ALLE FEJLER"]
[null,null,"Opstart_dataark",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Opstart",null,"TVB",null,"OK"]
[]
["Enkeltstoffer"]
[null,null,"Jordtype",null,"TVB","OK"]
[null,null,"Egenliste",null,"VIHU","OK","Egenliste jordtype: \nVandmættet porøsitet bør ikke fremgå, da værdien ikke anvendes men beregnes. Hvis værdien beholdes skal den være  uden benævnelse - slet \"kg/l\"\neller med \"m³/m³\" (kubik-tegnet skrives [Alt]+0179 på numerisk tastatur)"]
[null,null,"Stof","1, 2, 3, 4","TVB","OK"]
[null,null,"Egenliste",null,"TVB","OK"]
[null,null,"Bemærkningfelter",null,"TVB","OK"]
[null,null,"Nulstil",null,"TVB","OK"]
[null,null,"Navigeringsknapper",null,"TVB","OK"]
[null,null,"Dataark_Enkeltstoffer",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregning_Enkeltstoffer","TVB",null,"OK"]
[]
[null,null,"Udskrift_Enkeltstoffer",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Enkeltstoffer",null,"TVB",null,"OK"]
[]
["Vertikal transport"]
[null,null,"Nettonedbør",null,"TVB",null,"OK"]
[null,null,"Jordtype",null,"TVB",null,"OK"]
[null,null,"Aerob/anaerob",null,"TVB",null,"OK"]
[null,null,"Bemærkninger",null,"TVB",null,"OK"]
[null,null,"Stofkurver",null,"TVB",null,"OK"]
[null,null,"Dataark_Vertikal_Transport",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregning_ Vertikal_Transport","TVB",null,"OK"]
[]
[null,null,"Udskrift_ Vertikal_Transport",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Vertikal_Transport",null,"TVB",null,"OK"]
[]
["Grundvand"]
[null,null,"Skift mellem A og B beregning",null,"TVB",null,"OK"]
[null,null,"Nettonedbør",null,"TVB",null,"OK"]
[null,null,"Kildestyrke koncentration",null,"TVB",null,"OK"]
[null,null,"Aerob/anaerob",null,"TVB",null,"OK"]
[null,null,"Vis detailoplysninger",null,"TVB",null,"OK"]
[null,null,"Stofkurver",null,"TVB",null,"OK"]
[null,null,"Bemærkninger",null,"TVB",null,"OK"]
[null,null,"Dataark_grundvand",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregning_ Grundvand","TVB",null,"OK"]
[]
[null,null,"Udskrift_ Grundvand",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_grundvand",null,"TVB",null,"OK"]
[]
["Udeluft"]
[null,null,"Jordtyper",null,"TVB",null,"OK"]
[null,null,"Bemærkninger",null,"TVB",null,"OK"]
[null,null,"Vis/skjul detaljer",null,"TVB",null,"OK"]
[]
[null,null,"Dataark_Udeluft",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregning_ Udeluft","TVB",null,"OK"]
[]
[null,null,"Udskrift_ Udeluft",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Udeluft",null,"TVB",null,"OK"]
[]
["Indeklima"]
["Terrændæk",null,"Membran og kapilærbrydende lag",null,"TVB",null,"OK"]
[null,null,"Jordtype",null,"TVB",null,"OK"]
[null,null,"Betontype",null,"TVB",null,"OK"]
[null,null,"Vis detaljer",null,"TVB",null,"OK"]
[null,null,"Bemærkninger",null,"TVB",null,"OK"]
["krybekælder",null,"Betondæk og kapilærbrydende lag",null,"TVB",null,"OK"]
[null,null,"Jordtype",null,"TVB",null,"OK"]
[null,null,"Etageadskillelse",null,"TVB",null,"OK"]
[null,null,"Bemærkninger",null,"TVB",null,"OK"]
[]
[]
[null,"Indeklima Krybekælder",null,null,"TVB",null,"OK"]
[]
[null,null,"Dataark_ Indeklima",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregning_ Indeklima","TVB",null,"OK"]
[]
[null,null,"Udskrift_ Indeklima",null,"TVB",null,"OK"]
[]
[null,null,"Udskrift_ Indeklima_krybekælder"]
[]
[null,null,"Vejledning_Udeluft",null,"TVB",null,"OK"]
[]
["Oliestoffer",null,null,null,"LISA",null,"Vi skal lige se på vurderingen af fri fase"]
[null,null,"Jordtype",null,"TVB","OK"]
[null,null,"Egenliste",null,"VIHU","OK","Se under enkeltstoffer"]
[null,null,"Skift mellem Olieprofiler",null,"TVB","OK"]
[null,null,"Navigeringsknapper",null,"TVB","OK"]
[null,null,"Nulstill værdier",null,"TVB","OK"]
[]
[null,null,"Dataark_oliestoffer",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregninger_Oliestoffer","TVB",null,"OK"]
[]
[null,null,"Udskrift_Olieestoffer",null,"VIHU","OK","Flueben ved bemærkning fugacitet virker ikke"]
[]
[null,null,"Vejledning_Oliestoffer",null,"TVB",null,"OK"]
[]
[null,"Grundvand-Olie",null,null,"TVB",null,"OK"]
[]
[]
[null,null,"Dataark Grundvand-Olie",null,"TVB",null,"OK"]
[]
[null,null,null,"Bereningsark Grundvand-Olie","TVB",null,"OK"]
[]
[null,null,"Udskriftsark Grundvand-Olie",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Grundvand-Olie",null,"TVB",null,"OK"]
[]
[null,"Udeluft-Olie",null,null,"VIHU","OK","Bemærknings felter kan der ikke skrives i"]
[]
[]
[null,null,"Dataark_Udeluft-Olie",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregningsark_Udeluft-Olie","TVB",null,"OK"]
[]
[null,null,"Udskriftark_Udeluft-Olie",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Udeluft-Olie",null,"TVB",null,"OK"]
[]
[null,"Indeklima-Olie",null,null,"TVB",null,"OK"]
[]
[]
[null,null,"Dataark_Indeklima-Olie",null,"TVB",null,"OK"]
[]
[]
[null,null,null,"Beregningsark_Indeklima-Olie","TVB",null,"OK"]
[]
[null,null,"Udskriftark_Indeklima-Olie",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_Indeklima-Olie",null,"TVB",null,"OK"]
[]
[null,"Indeklima_Krybekælder-Olie",null,null,"TVB",null,"OK"]
[null,null,null,null,"TVB",null,"OK"]
[null,null,"Udskriftark_KrybekælderIndeklima-Olie",null,"TVB",null,"OK"]
[]
[null,null,"Vejledning_KrybekælderIndeklima-Olie",null,"TVB",null,"OK (samme som Indeklima"]
[]
[null,"Vertikal transport-olie",null,null,"TVB",null,"OK"]
[]
[]
[null,null,"Dataark_Vertikal-olie",null,"TVB",null,"OK"]
[]
[null,null,null,"Beregning_ Vertikal-olie","TVB",null,"OK"]
[]
[null,null,null,"Udskrift_ Vertikal-olie","TVB",null,"OK"]
[null,null,null,null,"TVB","JA","Konitunal formating skal laves om til OLIE"]
[null,null,null,"Vejledning_Vertikal-olie","TVB",null,"OK"]

{"sheet":"Opstart","index":2,"n_rows":34,"n_cols":27,"rows_kept":34,"cut":false,"hidden":false,"merged":[[26,3,26,8],[28,3,28,8],[13,3,13,13],[15,3,15,8],[17,3,17,8],[15,11,15,13],[26,11,26,13],[19,3,19,8],[21,3,21,8]]}
["Risikovurdering af forurenede grunde"]
["Version 2.1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Log over ændringer"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version 2.1 den 01-02-2016:","Væsentlig revidering af fugacitetsberegninger i Olie & benzin modulet"]
["Miljøstyrelsen, Cirkulær Økonomi & Affald",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Implementerin DTU's modul V1D for vertikal transport både for Enkeltstoffer og Olie & benzin modulet"]
["Haraldsgade 53",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layoutmæssige rettelser, f.eks. stavefejl, forkerte enheder, og antal af betydnede cifre i udskriftark"]
["2100 København Ø ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version 2.1 den 07-03-2019:","Rettelse af små skønhedsfejl i beregningsmoduler og layout samt opdatering af nedbrydningsrater iht. Tabel 15 i Miljøprojekt 2013 fra 2018."]
["Tlf. +45 72 54 40 "]
["E-post: mst@mst.dk",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version 2.1 den 17-11-2022:","Alle 22 PFAS-forbindelser samt NN-DMS og TFA er tilføjet  til stofdatabasen. "]
["Vejledning fra Miljøstyrelsen, Oprydning på forurenede lokaliteter nr. 6 1998",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grundvandskriterierne for sum af hhv.  22 PFAS, 4 PFAS  og pesticider er tilføjet mhp. beregninger i grundvandsmodul."]
[]
[]
["Lokaliteten",null,null,"Indtast navn, adresse m.v. for den lokalitet hvor JAGG-beregningerne foretages"]
[]
["Navn:"]
[]
["Adresse:",null,null,null,null,null,null,null,null,null,"Postnr./by"]
[]
["Lokalitetsnummer"]
[]
["Matrikelnummer:"]
[]
["Note:"]
[]
["Beregningene udført af"]
[null,null,null,"Indtast firmanavn til identifikation af hvem der har foretaget JAGG-beregningerne"]
[]
["Firmanavn",null,null,null,null,null,null,null,null,null,"Projekt nr."]
[]
["Navn/initialer"]
[]
[]
["Udfør beregningene "]
[null,null,null,"Vælg hvorvidt der ønskes udført beregninger for enkeltstoffer eller for olie- og benzinblandinger"]
[null,null,null,"Figuren nedenfor viser sammenhænget mellem modulerne, samt hvorledes der navigeres mellem disse"]

{"sheet":"Dataark_Opstart","index":3,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
["Dataark - Opstart"]
["Jord"]
["Lokaliteten"]
["navn:",{"$f":"IF(ISBLANK(Ops_navn),\"\",Ops_navn)","v":""}]
["adresse:",{"$f":"IF(ISBLANK(Ops_adr),\"\",Ops_adr)","v":""}]
["postnr/by:",{"$f":"IF(ISBLANK(Ops_post),\"\",Ops_post)","v":""}]
["Lokalitetsnummer:",{"$f":"IF(ISBLANK(Ops_lok),\"\",Ops_lok)","v":""}]
["Matrikel nummer:",{"$f":"IF(ISBLANK(Ops_mat),\"\",Ops_mat)","v":""}]
["Note:",{"$f":"IF(ISBLANK(Ops_note),\"\",Ops_note)","v":""}]
[]
["Beregningene udført af"]
["Firmanavn",{"$f":"IF(ISBLANK(Ops_firma),\"\",Ops_firma)","v":""}]
["navn/initialer",{"$f":"IF(ISBLANK(Ops_init),\"\",Ops_init)","v":""}]
["Projekt nr.",{"$f":"IF(ISBLANK(Ops_pro),\"\",Ops_pro)","v":""}]

{"sheet":"Vejledning_Opstart","index":4,"n_rows":36,"n_cols":2,"rows_kept":36,"cut":false,"hidden":true,"merged":[[1,1,1,8],[2,1,2,8]]}
[null,"Vejledning  - Opstart"]
[null,"Formålet med opstarts skærmbilledet er at give mulighed for at indtaste stamoplysninger\nom den enkelte lokalitet som JAGG beregningerne udføres for."]
[null,"De indtastede stamoplysninger vil blive vist i forbindelse med alle beregninger som gennemføres i JAGG,\nog oplysningerne vil også fremgå af udskriftssiderne."]
[]
[null,"Fra dataarket er der mulighed for gå til to typer af beregninger: Enkeltstoffer eller Olie og Benzin"]
[null,"ved at klikke på de respektive knapper øverst til højre i skærmbilledet (1)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Enkeltstoffer giver mulighed for at foretage beregninger med op til fire forskellige stoffer samtidigt, eller"]
[null,"at foretage beregningerne for det samme stof men med fire forskellige koncentrationer. Modulet giver "]
[null,"også mulighed for samtidigt at foretage beregningerne udefra en jordprøve, en vandprøve og/eller en poreluftprøve"]
[]
[null,"Olie og benzin modulet giver mulighed for at foretage en samlet beregninger af alle de kemiske stoffer"]
[null,"som normalt indgår i en jordanalyse af kulbrinter."]
[]
[null,"Knappen \"Nulstil værdier\" (2) sletter alle indtastede værdier på alle ark i regnearket."]
[]
[null,"Knappen \"Reset Knapformat\" (3). I visse tilfælde kan man risikere at knapperne i regnearket ændrer plads og eller "]
[null,"størrelse. Knappen hjælper med at genoprette det oprindelige skærm design."]

{"sheet":"Enkeltstoffer","index":5,"n_rows":129,"n_cols":41,"rows_kept":129,"cut":false,"hidden":true,"merged":[[97,35,97,38],[42,31,44,37],[34,16,34,17],[36,7,36,8],[44,7,44,8],[42,22,42,23],[40,22,40,23],[36,22,36,23],[38,22,38,23],[40,16,40,17],[40,19,40,20],[44,16,44,17],[38,19,38,20],[44,19,44,20],[42,16,42,17],[42,19,42,20],[44,22,44,23],[42,28,42,29],[40,25,40,26],[40,28,40,29],[36,25,36,26],[96,25,96,29],[97,25,97,29],[70,28,71,29],[44,5,44,6],[34,13,34,14],[11,4,11,8],[11,10,11,11],[11,13,11,14],[11,22,11,23],[11,28,11,29],[11,25,11,26],[11,19,11,20],[11,16,11,17],[32,25,32,29],[17,25,17,26],[21,27,21,28],[18,25,20,26],[20,28,20,29],[14,28,16,29],[17,28,17,29],[18,28,18,29],[19,28,19,29],[13,25,16,26],[36,28,36,29],[38,25,38,26],[38,28,38,29],[42,25,42,26],[7,7,7,15],[42,13,42,14],[36,13,36,14],[18,16,20,17],[7,19,7,23],[19,10,19,11],[18,10,18,11],[14,10,16,11],[14,13,16,14],[17,22,17,23],[18,22,18,23],[19,22,19,23],[20,22,20,23],[20,4,20,8],[14,22,16,23],[9,7,9,11],[9,13,9,17],[9,19,9,23],[9,25,9,29],[48,16,48,17],[48,19,48,20],[48,22,48,23],[46,16,46,17],[64,7,65,8],[64,13,65,14],[54,13,54,14],[54,16,54,17],[44,28,44,29],[44,13,44,14],[48,13,48,14],[31,25,31,29],[32,7,32,11],[32,13,32,17],[32,19,32,23],[50,28,50,29],[103,7,103,11],[97,7,97,11],[101,7,101,11],[96,7,96,11],[97,13,97,17],[101,13,101,17],[56,7,56,8],[70,10,71,11],[76,13,76,17],[83,7,83,11],[89,7,89,11],[70,7,71,8],[83,13,83,17],[74,13,74,17],[56,13,56,14],[56,16,56,17],[80,13,80,17],[70,13,71,14],[96,13,96,17],[89,13,89,17],[58,16,59,17],[58,7,59,8],[61,7,62,8],[58,13,59,14],[105,7,105,11],[111,7,111,11],[34,10,34,11],[42,7,42,8],[42,10,42,11],[38,7,38,8],[74,7,74,11],[76,7,76,11],[78,7,78,11],[54,7,54,8],[54,10,54,11],[56,10,56,11],[80,7,80,11],[46,7,46,8],[46,10,46,11],[48,7,48,8],[34,7,34,8],[38,10,38,11],[58,10,59,11],[67,7,68,8],[36,10,36,11],[44,10,44,11],[109,7,109,11],[48,10,48,11],[105,13,105,17],[105,19,105,23],[105,25,105,29],[101,19,101,23],[103,19,103,23],[101,25,101,29],[96,19,96,23],[111,25,111,29],[117,19,117,23],[103,13,103,17],[109,13,109,17],[109,19,109,23],[109,25,109,29],[113,13,113,17],[111,13,111,17],[111,19,111,23],[103,25,103,29],[113,25,113,29],[117,13,117,17],[3,7,3,23],[5,19,5,23],[124,7,124,11],[124,13,124,17],[124,19,124,23],[5,7,5,15],[40,7,40,8],[40,10,40,11],[40,13,40,14],[86,7,86,11],[36,19,36,20],[18,19,20,20],[20,10,20,11],[18,13,18,14],[19,13,19,14],[20,13,20,14],[16,4,16,8],[14,16,16,17],[17,16,17,17],[17,19,17,20],[14,19,16,20],[17,10,17,11],[17,13,17,14],[18,4,19,8],[86,19,86,23],[70,16,71,17],[70,22,71,23],[76,19,76,23],[64,28,65,29],[46,25,46,26],[46,28,46,29],[48,25,48,26],[46,22,46,23],[74,25,74,29],[86,25,86,29],[83,19,83,23],[78,19,78,23],[46,19,46,20],[78,13,78,17],[64,16,65,17],[89,25,89,29],[86,13,86,17],[70,19,71,20],[48,28,48,29],[44,25,44,26],[83,25,83,29],[46,13,46,14],[134,3,134,8],[113,7,113,11],[117,7,117,11],[121,7,121,11],[119,7,119,11],[119,19,119,23],[121,19,121,23],[117,25,117,29],[119,25,119,29],[121,25,121,29],[113,19,113,23],[126,19,126,23],[124,25,124,29],[126,7,126,11],[126,25,126,29],[126,13,126,17],[121,13,121,17],[119,13,119,17],[128,7,128,11],[128,13,128,17],[128,19,128,23],[128,25,128,29],[22,24,22,26],[36,16,36,17],[38,13,38,14],[38,16,38,17],[28,7,28,11],[29,7,29,11],[28,13,28,17],[29,13,29,17],[28,19,28,23],[29,19,29,23],[28,25,28,29],[34,25,34,26],[34,28,34,29],[34,19,34,20],[34,22,34,23],[29,25,29,29],[31,7,31,11],[31,13,31,17],[31,19,31,23],[89,19,89,23],[97,19,97,23],[74,19,74,23],[54,19,54,20],[54,22,54,23],[54,25,54,26],[54,28,54,29],[56,19,56,20],[56,22,56,23],[56,25,56,26],[78,25,78,29],[56,28,56,29],[58,28,59,29],[58,22,59,23],[80,19,80,23],[80,25,80,29],[70,25,71,26],[58,19,59,20],[61,19,62,20],[58,25,59,26],[61,25,62,26],[64,19,65,20],[64,25,65,26],[76,25,76,29],[50,31,50,32],[50,7,50,8],[50,10,50,11],[50,13,50,14],[50,16,50,17],[50,19,50,20],[50,22,50,23],[50,25,50,26],[52,5,52,6],[52,7,52,8],[52,10,52,11],[52,13,52,14],[52,16,52,17],[52,19,52,20],[52,22,52,23],[52,25,52,26],[52,28,52,29],[67,31,67,32],[67,10,68,11],[67,16,68,17],[67,22,68,23],[67,28,68,29],[61,10,62,11],[64,10,65,11],[61,31,61,32],[61,16,62,17],[61,22,62,23],[61,28,62,29],[64,22,65,23],[67,13,68,14],[67,19,68,20],[67,25,68,26],[61,13,62,14]]}
["Kemiske data og fugacitet for enkeltstoffer"]
["Lokaliteten"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
["Beregning udføres for :",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
[]
["Jordtype",null,null,null,null,null,"Vælg jordart for fugacitetsberegning eller indtast egne jordartsdata"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bulk-masse-fylde\n(kg/l)"]
[null,null,null,null,null,null,null,null,null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,null,"Volumen\naf jordskellet",null,null,"Korn-rumvægt\n(kg/l)",null,null,null,null,null,"% Indhold organisk kulstof"]
[]
[null,null,null,null,"Jordtype"]
[null,null,null,null,null,null,null,null,null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ",null,null,"d",null,null,"r",null,null,"foc"]
[null,null,null,null,{"$f":"IF(D_Enk_jordtype_syst<>\"\",D_Enk_jordtype_syst,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_VL_int<>\"\",D_Enk_VL_int,\"\")","v":""},null,null,{"$f":"IF(D_Enk_VV_int<>\"\",D_Enk_VV_int,\"\")","v":""},null,null,{"$f":"D_Enk_porositet","v":0},null,null,{"$f":"D_Enk_VJ","v":1},null,null,{"$f":"IF(D_Enk_d_int<>\"\",D_Enk_d_int,\"\")","v":""},null,null,{"$f":"D_Enk_p","v":0},null,null,{"$f":"IF(D_Enk_foc_int<>\"\",D_Enk_foc_int,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Enk_VL_syst<>\"\",D_Enk_VL_syst,\"\")","v":""},null,null,{"$f":"IF(D_Enk_VV_syst<>\"\",D_Enk_VV_syst,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_Enk_d_syst<>\"\",D_Enk_d_syst,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_foc_syst<>\"\",D_Enk_foc_syst,\"\")","v":""},null,null,{"$f":"IF(D_Enk_porositet>0.45,\"Er det korrekt at den samlede porøsitet er >0,45? - tjek VL og VV\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Enk_My_VL),\"Tjek decimal\",IF(ISTEXT(Enk_My_VV),\"Tjek decimal\",IF(ISTEXT(Enk_My_d),\"Tjek decimal\",IF(ISTEXT(Enk_My_foc),\"Tjek decimal\",\"\"))))","v":""}]
[]
[]
["Kemiske data",null,null,null,null,null,null,"Vælg stof for fugacitetsberegning eller indtast egne stofspecifikke data"]
[]
[]
[]
[]
["Stofnavn",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_syst_1<>\"\",D_Enk_stofnavn_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_syst_2<>\"\",D_Enk_stofnavn_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_syst_3<>\"\",D_Enk_stofnavn_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_syst_4<>\"\",D_Enk_stofnavn_syst_4,\"\")","v":""}]
[]
[]
["CAS-nummer",null,null,null,null,null,null,{"$f":"IF(D_Enk_CASnr_syst_1<>\"\",D_Enk_CASnr_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_CASnr_syst_2<>\"\",D_Enk_CASnr_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_CASnr_syst_3<>\"\",D_Enk_CASnr_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_CASnr_syst_4<>\"\",D_Enk_CASnr_syst_4,\"\")","v":""}]
[]
[]
["Molmasse",null,null,null,null,"m",null,{"$f":"IF(D_Enk_m_syst_1<>\"\",D_Enk_m_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_m_syst_2<>\"\",D_Enk_m_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_m_syst_3<>\"\",D_Enk_m_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_m_syst_4<>\"\",D_Enk_m_syst_4,\"\")","v":""},null,null,null,null,null,"g/mol"]
[]
["Damptryk ",null,null,null,null,"p",null,{"$f":"IF(D_Enk_p_syst_1<>\"\",D_Enk_p_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_p_syst_2<>\"\",D_Enk_p_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_p_syst_3<>\"\",D_Enk_p_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_p_syst_4<>\"\",D_Enk_p_syst_4,\"\")","v":""},null,null,null,null,null,"Pa"]
[]
["Vandopløselighed",null,null,null,null,"S",null,{"$f":"IF(D_Enk_S_syst_1<>\"\",D_Enk_S_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_S_syst_2<>\"\",D_Enk_S_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_S_syst_3<>\"\",D_Enk_S_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_S_syst_4<>\"\",D_Enk_S_syst_4,\"\")","v":""},null,null,null,null,null,"mg/l"]
[]
["Henry's konstant",null,null,null,null,"KH",null,{"$f":"IF(D_Enk_KH_syst_1<>\"\",D_Enk_KH_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KH_syst_2<>\"\",D_Enk_KH_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KH_syst_3<>\"\",D_Enk_KH_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KH_syst_4<>\"\",D_Enk_KH_syst_4,\"\")","v":""},null,null,null,null,null,"dimensionsløs (bruges i vertikal transport modul)"]
[]
["Log oktanol/vand ford. koeff.",null,null,null,null,"log Kow",null,{"$f":"IF(D_Enk_KOW_syst_1<>\"\",D_Enk_KOW_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KOW_syst_2<>\"\",D_Enk_KOW_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KOW_syst_3<>\"\",D_Enk_KOW_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KOW_syst_4<>\"\",D_Enk_KOW_syst_4,\"\")","v":""},null,null,null,null,null,"Husk at både Koc og Log Kow skal indtases såfremt der anvendes egne data"]
[]
["Koc",null,null,null,null,"Koc",null,{"$f":"IF(D_Enk_KOC_syst_1<>\"\",D_Enk_KOC_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KOC_syst_2<>\"\",D_Enk_KOC_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KOC_syst_3<>\"\",D_Enk_KOC_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_KOC_syst_4<>\"\",D_Enk_KOC_syst_4,\"\")","v":""}]
[]
["Grundvandskvalitetskriterie, GV",null,null,null,null,null,null,{"$f":"IF(D_Enk_GV_krit_syst_1<>\"\",D_Enk_GV_krit_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_GV_krit_syst_2<>\"\",D_Enk_GV_krit_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_GV_krit_syst_3<>\"\",D_Enk_GV_krit_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_GV_krit_syst_4<>\"\",D_Enk_GV_krit_syst_4,\"\")","v":""},null,null,null,null,null,"µg/l"]
[]
["Afdampningskriterie, luft",null,null,null,null,null,null,{"$f":"IF(D_Enk_afd_krit_syst_1<>\"\",D_Enk_afd_krit_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_afd_krit_syst_2<>\"\",D_Enk_afd_krit_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_afd_krit_syst_3<>\"\",D_Enk_afd_krit_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_afd_krit_syst_4<>\"\",D_Enk_afd_krit_syst_4,\"\")","v":""},null,null,null,null,null,"mg/m3"]
[]
["Jordkvalitetskriterie",null,null,null,null,null,null,{"$f":"IF(D_Enk_jordkval_krit_syst_1<>\"\",D_Enk_jordkval_krit_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_jordkval_krit_syst_2<>\"\",D_Enk_jordkval_krit_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_jordkval_krit_syst_3<>\"\",D_Enk_jordkval_krit_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_jordkval_krit_syst_4<>\"\",D_Enk_jordkval_krit_syst_4,\"\")","v":""},null,null,null,null,null,"mg/kg TS"]
[]
["Diffusionskoefficient i luft",null,null,null,null,"DL",null,{"$f":"IF(D_Enk_DL_syst_1<>\"\",D_Enk_DL_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_DL_syst_2<>\"\",D_Enk_DL_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_DL_syst_3<>\"\",D_Enk_DL_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_DL_syst_4<>\"\",D_Enk_DL_syst_4,\"\")","v":""},null,null,null,null,null,"m2/s"]
[]
["Diffusionskoefficient i vand",null,null,null,null,"DW",null,{"$f":"IF(D_Enk_Ddw_syst_1<>\"\",D_Enk_Ddw_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_Ddw_syst_2<>\"\",D_Enk_Ddw_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_Ddw_syst_3<>\"\",D_Enk_Ddw_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_Ddw_syst_4<>\"\",D_Enk_Ddw_syst_4,\"\")","v":""},null,null,null,null,null,"m2/s"]
[]
["Vindhastighed",null,null,null,null,null,null,{"$f":"IF(D_Enk_v_syst_1<>\"\",D_Enk_v_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_v_syst_2<>\"\",D_Enk_v_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_v_syst_3<>\"\",D_Enk_v_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_v_syst_4<>\"\",D_Enk_v_syst_4,\"\")","v":""},null,null,null,null,null,"m/s"]
[]
["1. ordens nedbrydn. grundvand",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_1<>\"\",D_Enk_k1anaerob_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_2<>\"\",D_Enk_k1anaerob_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_3<>\"\",D_Enk_k1anaerob_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_4<>\"\",D_Enk_k1anaerob_syst_4,\"\")","v":""}]
["anaerobe forhold",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_2<>\"\",D_Enk_k1anaerob_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_3<>\"\",D_Enk_k1anaerob_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_syst_4<>\"\",D_Enk_k1anaerob_syst_4,\"\")","v":""},null,null,null,null,null,"dag-1"]
[]
["1. ordens nedbrydn. grundvand",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_1<>\"\",D_Enk_k1aerob_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_2<>\"\",D_Enk_k1aerob_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_3<>\"\",D_Enk_k1aerob_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_4<>\"\",D_Enk_k1aerob_syst_4,\"\")","v":""}]
["aerobe forhold",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_2<>\"\",D_Enk_k1aerob_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_3<>\"\",D_Enk_k1aerob_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_syst_4<>\"\",D_Enk_k1aerob_syst_4,\"\")","v":""},null,null,null,null,null,"dag-1"]
[]
["1. ordens nedbrydn. vertikal transport",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_1<>\"\",D_Enk_k1anaerob_umættet_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_2<>\"\",D_Enk_k1anaerob_umættet_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_3<>\"\",D_Enk_k1anaerob_umættet_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_4<>\"\",D_Enk_k1anaerob_umættet_syst_4,\"\")","v":""}]
["anaerobe forhold",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_1<>\"\",D_Enk_k1anaerob_umættet_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_2<>\"\",D_Enk_k1anaerob_umættet_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_3<>\"\",D_Enk_k1anaerob_umættet_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_4<>\"\",D_Enk_k1anaerob_umættet_syst_4,\"\")","v":""},null,null,null,null,null,"dag-1"]
[]
["1. ordens nedbrydn. vertikal transport",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_1<>\"\",D_Enk_k1aerob_uz_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_2<>\"\",D_Enk_k1aerob_uz_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_3<>\"\",D_Enk_k1aerob_uz_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_4<>\"\",D_Enk_k1aerob_uz_syst_4,\"\")","v":""}]
["aerobe forhold",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_1<>\"\",D_Enk_k1aerob_uz_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_2<>\"\",D_Enk_k1aerob_uz_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_3<>\"\",D_Enk_k1aerob_uz_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1aerob_uz_syst_4<>\"\",D_Enk_k1aerob_uz_syst_4,\"\")","v":""},null,null,null,null,null,"dag-1"]
[]
["1. ordens nedbrydn. poreluft",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_1<>\"\",D_Enk_k1anaerob_poreluft_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_2<>\"\",D_Enk_k1anaerob_poreluft_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_3<>\"\",D_Enk_k1anaerob_poreluft_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_4<>\"\",D_Enk_k1anaerob_poreluft_syst_4,\"\")","v":""}]
["aerobe forhold",null,null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_1<>\"\",D_Enk_k1anaerob_poreluft_syst_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_2<>\"\",D_Enk_k1anaerob_poreluft_syst_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_3<>\"\",D_Enk_k1anaerob_poreluft_syst_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_k1anaerob_poreluft_syst_4<>\"\",D_Enk_k1anaerob_poreluft_syst_4,\"\")","v":""},null,null,null,null,null,"dag-1"]
[]
[]
[null,null,null,null,null,"ML, max",null,{"$f":"D_Enk_MLmax_1","v":0},null,null,null,null,null,{"$f":"[0]!D_Enk_MLmax_2","v":0},null,null,null,null,null,{"$f":"[0]!D_Enk_MLmax_3","v":0},null,null,null,null,null,{"$f":"[0]!D_Enk_MLmax_4","v":0},null,null,null,null,null,"mg/m³ jordvol."]
[]
[null,null,null,null,null,"MV, max",null,{"$f":"D_Enk_MVmax_1","v":0},null,null,null,null,null,{"$f":"D_Enk_MVmax_2","v":0},null,null,null,null,null,{"$f":"D_Enk_MVmax_3","v":0},null,null,null,null,null,{"$f":"D_Enk_MVmax_4","v":0},null,null,null,null,null,"mg/m³ jordvol."]
[]
[null,null,null,null,null,"MJ, max",null,{"$f":"D_Enk_MJmax_1","v":0},null,null,null,null,null,{"$f":"D_Enk_MJmax_2","v":0},null,null,null,null,null,{"$f":"D_Enk_MJmax_3","v":0},null,null,null,null,null,{"$f":"D_Enk_MJmax_4","v":0},null,null,null,null,null,"mg/m³ jordvol."]
[]
[null,null,null,null,null,"Mættede  damptryk, CL,max",null,{"$f":"D_Enk_CLmax_1","v":""},null,null,null,null,null,{"$f":"D_Enk_CLmax_2","v":""},null,null,null,null,null,{"$f":"D_Enk_CLmax_3","v":""},null,null,null,null,null,{"$f":"D_Enk_CLmax_4","v":""},null,null,null,null,null,"mg/m³"]
[]
[]
["Maksimal fordeling, luft",null,null,null,null,"fl",null,{"$f":"D_Enk_fl_1","v":""},null,null,null,null,null,{"$f":"D_Enk_fl_2","v":""},null,null,null,null,null,{"$f":"D_Enk_fl_3","v":""},null,null,null,null,null,{"$f":"D_Enk_fl_4","v":""}]
[]
[]
["Maksimal fordeling, vand",null,null,null,null,"fv",null,{"$f":"D_Enk_fv_1","v":""},null,null,null,null,null,{"$f":"D_Enk_fv_2","v":""},null,null,null,null,null,{"$f":"D_Enk_fv_3","v":""},null,null,null,null,null,{"$f":"D_Enk_fv_4","v":""}]
[]
[]
["Maksimal fordeling, jord",null,null,null,null,"fj",null,{"$f":"D_Enk_fj_1","v":""},null,null,null,null,null,{"$f":"D_Enk_fj_2","v":""},null,null,null,null,null,{"$f":"D_Enk_fj_3","v":""},null,null,null,null,null,{"$f":"D_Enk_fj_4","v":""}]
[]
[]
[]
["Fugacitet",null,null,"For hvert stof indtast målepunkt og evt prøvetagningsdato samt den målte værdi"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"H10","v":""},{"$f":"N10","v":""},{"$f":"T10","v":""},{"$f":"Z10","v":""}]
[]
["Målepunkt",null,null,null,null,null,null,"",null,null,null,null,null,"",null,null,null,null,null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"H97","v":""},{"$f":"N97","v":""},{"$f":"T97","v":""},{"$f":"Z97","v":""}]
["Dato",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tjek af enheder"]
[]
[]
[]
["Målt konc. i poreluft",null,null,null,null,"CL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³",null,null,{"$f":"IF(ISTEXT(Enk_My_CL_1),\"Tjek decimal\",IF(ISTEXT(Enk_My_CL_2),\"Tjek decimal\",IF(ISTEXT(Enk_My_CL_3),\"Tjek decimal\",IF(ISTEXT(Enk_My_CL_4),\"Tjek decimal\",\"\"))))","v":""},{"$f":"H102*1000000","v":0},{"$f":"N102*1000000","v":0},{"$f":"T102*1000000","v":0},{"$f":"Z102*1000000","v":0},null,"ng/m³"]
[]
["Beregnet jordkoncentration",null,null,null,null,"Ct",null,{"$f":"D_Enk_Ct_L_1","v":0},null,null,null,null,null,{"$f":"D_Enk_Ct_L_2","v":0},null,null,null,null,null,{"$f":"D_Enk_Ct_L_3","v":0},null,null,null,null,null,{"$f":"D_Enk_Ct_L_4","v":0},null,null,null,null,null,"mg/kg TS",null,null,null,{"$f":"H104*1000","v":0},{"$f":"N104*1000","v":0},{"$f":"T104*1000","v":0},{"$f":"Z104*1000","v":0},null,"µg/kg TS"]
[]
["Beregnet vandskoncentration",null,null,null,null,"CV",null,{"$f":"D_Enk_Cv_L_1","v":0},null,null,null,null,null,{"$f":"D_Enk_Cv_L_2","v":0},null,null,null,null,null,{"$f":"D_Enk_Cv_L_3","v":0},null,null,null,null,null,{"$f":"D_Enk_Cv_L_4","v":0},null,null,null,null,null,"mg/l",null,null,null,{"$f":"H106*1000000","v":0},{"$f":"N106*1000000","v":0},{"$f":"T106*1000000","v":0},{"$f":"Z106*1000000","v":0},null,"ng/l"]
[]
[]
[]
["Målt konc. i grundvand",null,null,null,null,"CV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l",null,null,{"$f":"IF(ISTEXT(Enk_My_CV_1),\"Tjek decimal\",IF(ISTEXT(Enk_My_CV_2),\"Tjek decimal\",IF(ISTEXT(Enk_My_CV_3),\"Tjek decimal\",IF(ISTEXT(Enk_My_CV_4),\"Tjek decimal\",\"\"))))","v":""},{"$f":"H110*1000000","v":0},{"$f":"N110*1000000","v":0},{"$f":"T110*1000000","v":0},{"$f":"Z110*1000000","v":0},null,"ng/l"]
[]
["Beregnet poreluftskonc.",null,null,null,null,"CL",null,{"$f":"D_Enk_Cl_V_1","v":0},null,null,null,null,null,{"$f":"D_Enk_Cl_V_2","v":0},null,null,null,null,null,{"$f":"D_Enk_Cl_V_3","v":0},null,null,null,null,null,{"$f":"D_Enk_Cl_V_4","v":0},null,null,null,null,null,"mg/m³",null,null,null,{"$f":"H112*1000000","v":0},{"$f":"N112*1000000","v":0},{"$f":"T112*1000000","v":0},{"$f":"Z112*1000000","v":0},null,"ng/m³"]
[]
["Beregnet jordkonc.",null,null,null,null,"Ct",null,{"$f":"D_Enk_Ct_V_1","v":0},null,null,null,null,null,{"$f":"D_Enk_Ct_V_2","v":0},null,null,null,null,null,{"$f":"D_Enk_Ct_V_3","v":0},null,null,null,null,null,{"$f":"D_Enk_Ct_V_4","v":0},null,null,null,null,null,"mg/kg TS",null,null,null,{"$f":"H114*1000","v":0},{"$f":"N114*1000","v":0},{"$f":"T114*1000","v":0},{"$f":"Z114*1000","v":0},null,"µg/kg TS"]
[]
[]
[]
["Målt konc. i jorden",null,null,null,null,"Ct",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/kg TS",null,null,{"$f":"IF(ISTEXT(Enk_My_Ct_1),\"Tjek decimal\",IF(ISTEXT(Enk_My_Ct_2),\"Tjek decimal\",IF(ISTEXT(Enk_My_Ct_3),\"Tjek decimal\",IF(ISTEXT(Enk_My_Ct_4),\"Tjek decimal\",\"\"))))","v":""},{"$f":"H118*1000","v":0},{"$f":"N118*1000","v":0},{"$f":"T118*1000","v":0},{"$f":"Z118*1000","v":0},null,"µg/kg TS"]
[]
["Beregnet poreluftskonc.",null,null,null,null,"CL",null,{"$f":"D_Enk_Cl_J_1","v":0},null,null,null,null,null,{"$f":"D_Enk_Cl_J_2","v":0},null,null,null,null,null,{"$f":"D_Enk_Cl_J_3","v":0},null,null,null,null,null,{"$f":"D_Enk_Cl_J_4","v":0},null,null,null,null,null,"mg/m³",null,null,null,{"$f":"H120*1000000","v":0},{"$f":"N120*1000000","v":0},{"$f":"T120*1000000","v":0},{"$f":"Z120*1000000","v":0},null,"ng/m³"]
[]
["Beregnet vandskoncentration",null,null,null,null,"CV",null,{"$f":"D_Enk_Cv_J_1","v":0},null,null,null,null,null,{"$f":"D_Enk_Cv_J_2","v":0},null,null,null,null,null,{"$f":"D_Enk_Cv_J_3","v":0},null,null,null,null,null,{"$f":"D_Enk_Cv_J_4","v":0},null,null,null,null,null,"mg/l",null,null,null,{"$f":"H122*1000000","v":0},{"$f":"N122*1000000","v":0},{"$f":"T122*1000000","v":0},{"$f":"Z122*1000000","v":0},null,"ng/l"]
[]
[]
["Fri fase?",null,null,null,null,null,null,{"$f":"D_Enk_FF_1","v":"nej"},null,null,null,null,null,{"$f":"D_Enk_FF_2","v":"nej"},null,null,null,null,null,{"$f":"D_Enk_FF_3","v":"nej"},null,null,null,null,null,{"$f":"D_Enk_FF_4","v":"nej"}]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"D_Enk_Brugerdata_1","v":"Nej"},null,null,null,null,null,{"$f":"D_Enk_Brugerdata_2","v":"Nej"},null,null,null,null,null,{"$f":"D_Enk_Brugerdata_3","v":"Nej"},null,null,null,null,null,{"$f":"D_Enk_Brugerdata_4","v":"Nej"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42]

{"sheet":"Dataark_Enkeltstoffer","index":6,"n_rows":97,"n_cols":18,"rows_kept":97,"cut":false,"hidden":true,"merged":[[18,12,18,14],[62,3,62,5],[62,6,62,8],[62,9,62,11],[62,12,62,14],[18,3,18,5],[18,6,18,8],[18,9,18,11],[52,3,52,5],[52,6,52,8],[52,9,52,11],[52,12,52,14]]}
[]
[]
["Dataark - Enkeltstoffer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
["Jord"]
["Navn","Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes"]
["Jordtype",null,null,null,null,{"$f":"Enk_My_Jord","v":0},{"$f":"IF(ISTEXT(F7),F7,IF(E7<>0,E7,\"\"))","v":""},null,null,null,null,null,null,null,null,null,"D_Enk_jordtype","input"]
["Poreluftvolumen","VL",null,null,null,{"$f":"IF(ISNUMBER(Enk_My_VL),Enk_My_VL,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(F8),F8,E8)","v":0},null,null,null,null,null,null,null,null,null,"D_Enk_VL","input"]
["Vandindhold","VV",null,null,null,{"$f":"IF(ISNUMBER(Enk_My_VV),Enk_My_VV,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(F9),F9,E9)","v":0},null,null,null,null,null,null,null,null,null,"D_Enk_VV","input"]
["Samlet\nporøsitet","e=VL+VV",null,null,null,null,{"$f":"B_Enk_porositet","v":0},null,null,null,null,null,null,null,null,null,"D_Enk_porositet","beregnes"]
["Volumen af jordskellet","VJ",null,null,null,null,{"$f":"B_Enk_VJ","v":1},null,null,null,null,null,null,null,null,null,"D_Enk_VJ","beregnes"]
["Kornrumvægt","d","kg/l",null,null,{"$f":"IF(VALUE(Enk_My_d),Enk_My_d,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(F12),F12,E12)","v":0},null,null,null,null,null,null,null,null,null,"D_Enk_d","input"]
["Volumenvægt","r","kg/l",null,null,null,{"$f":"B_Enk_p","v":0},null,null,null,null,null,null,null,null,null,"D_Enk_p","beregnes"]
["% organisk indhold","foc(%)",null,null,null,{"$f":"IF(VALUE(Enk_My_foc),Enk_My_foc,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(F14),F14,E14)","v":0},null,null,null,null,null,null,null,null,null,null,"input"]
["Indhold af organisk kulstof (relativ vægtandel)","foc",null,{"$f":"D14/100","v":0},{"$f":"E14/100","v":0},null,{"$f":"G14/100","v":0},null,null,null,null,null,null,null,null,null,"D_Enk_foc","beregnes i dataark"]
[]
[]
["Stofegenskaber"]
[null,null,null,"Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4"]
["Navn","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes"]
["Forureningskomponent",null,null,null,{"$f":"Enk_My_stofnavn_1","v":0},{"$f":"IF(ISTEXT(E21),E21,IF(D21<>0,D21,\"\"))","v":""},null,{"$f":"Enk_My_stofnavn_2","v":0},{"$f":"IF(ISTEXT(H21),H21,IF(G21<>0,G21,\"\"))","v":""},null,{"$f":"Enk_My_stofnavn_3","v":0},{"$f":"IF(ISTEXT(K21),K21,IF(J21<>0,J21,\"\"))","v":""},null,{"$f":"Enk_My_stofnavn_4","v":0},{"$f":"IF(ISTEXT(N21),N21,IF(M21<>0,M21,\"\"))","v":""},null,"D_Enk_stofnavn_n","input"]
["CAS-nummer",null,null,null,{"$f":"Enk_My_CASnr_1","v":0},{"$f":"IF(ISTEXT(E22),E22,IF(D22<>0,D22,\"\"))","v":""},null,{"$f":"Enk_My_CASnr_2","v":0},{"$f":"IF(ISTEXT(H22),H22,IF(G22<>0,G22,\"\"))","v":""},null,{"$f":"Enk_My_CASnr_3","v":0},{"$f":"IF(ISTEXT(K22),K22,IF(J22<>0,J22,\"\"))","v":""},null,{"$f":"Enk_My_CASnr_3","v":0},{"$f":"IF(ISTEXT(N22),N22,IF(M22<>0,M22,\"\"))","v":""},null,"D_Enk_CASnr_n","input"]
["Jordkvalitetskriterie",null,"mg/kg",null,{"$f":"Enk_My_jordkval_krit_1","v":0},null,null,{"$f":"Enk_My_jordkval_krit_2","v":0},null,null,{"$f":"Enk_My_jordkval_krit_2","v":0},null,null,{"$f":"Enk_My_jordkval_krit_4","v":0},null,null,"D_Enk_jordkval_krit_n","input"]
["Afskæringskriterie",null,"mg/kg",null,null,{"$f":"IF(VALUE(E24),E24,D24)","v":0},null,null,{"$f":"IF(VALUE(H24),H24,G24)","v":0},null,null,{"$f":"IF(VALUE(K24),K24,J24)","v":0},null,null,{"$f":"IF(VALUE(N24),N24,M24)","v":0},null,"D_Enk_afsk_krit_n","input"]
["Fluxberegninger"]
["Molmasse","m","gram/mol",null,{"$f":"Enk_My_m_1","v":0},0,null,{"$f":"Enk_My_m_2","v":0},0,null,{"$f":"Enk_My_m_3","v":0},0,null,{"$f":"Enk_My_m_4","v":0},{"$f":"IF(VALUE(N26),N26,M26)","v":0},null,"D_Enk_m_n","input"]
["Damptryk","p","Pa",null,{"$f":"Enk_My_p_1","v":0},0,null,{"$f":"Enk_My_p_2","v":0},0,null,{"$f":"Enk_My_p_3","v":0},0,null,{"$f":"Enk_My_p_4","v":0},0,null,"D_Enk_p_n","input"]
["Vandopløselighed","S","mg/l",null,{"$f":"Enk_My_S_1","v":0},0,null,{"$f":"Enk_My_S_2","v":0},0,null,{"$f":"Enk_My_S_3","v":0},0,null,{"$f":"Enk_My_S_4","v":0},0,null,"D_Enk_S_n","input"]
["log Oktanol/vand ford. koeff.","log Kow",null,null,{"$f":"Enk_My_KOW_1","v":0},0,null,{"$f":"Enk_My_KOW_2","v":0},0,null,{"$f":"Enk_My_KOW_3","v":0},0,null,{"$f":"Enk_My_KOW_4","v":0},0,null,"D_Enk_KOW_n","input"]
["Koc","Koc",null,null,{"$f":"Enk_My_KOC_1","v":0},0,null,{"$f":"Enk_My_KOC_2","v":0},0,null,{"$f":"Enk_My_KOC_3","v":0},0,null,{"$f":"Enk_My_KOC_4","v":0},0,null,"D_Enk_KOC_n","input"]
["Henrys konstant","KH",null,null,{"$f":"Enk_My_KH_1","v":0},0,null,{"$f":"Enk_My_KH_2","v":0},0,null,{"$f":"Enk_My_KH_3","v":0},0,null,{"$f":"Enk_My_KH_4","v":0},0,null,"D_Enk_KH_n","input"]
["Poreluftberegninger"]
["Diffusionskoefficient luft","DL","m²/s",null,{"$f":"Enk_My_DL_1","v":0},{"$f":"IF(VALUE(E33),E33,D33)","v":0},null,{"$f":"Enk_My_DL_2","v":0},{"$f":"IF(VALUE(H33),H33,G33)","v":0},null,{"$f":"Enk_My_DL_3","v":0},{"$f":"IF(VALUE(K33),K33,J33)","v":0},null,{"$f":"Enk_My_DL_4","v":0},{"$f":"IF(VALUE(N33),N33,M33)","v":0},null,"D_Enk_DL_n","input"]
["Vindhastighed (stofafhængig)","v","m/s",null,{"$f":"Enk_My_v_1","v":0},{"$f":"IF(VALUE(E34),E34,D34)","v":0},null,{"$f":"Enk_My_v_2","v":0},{"$f":"IF(VALUE(H34),H34,G34)","v":0},null,{"$f":"Enk_My_v_3","v":0},{"$f":"IF(VALUE(K34),K34,J34)","v":0},null,{"$f":"Enk_My_v_4","v":0},{"$f":"IF(VALUE(N34),N34,M34)","v":0},null,"D_Enk_v_n","input"]
["Afdampningskriterie","afd-krit","mg/m³",null,{"$f":"Enk_My_afd_krit_1","v":0},{"$f":"IF(VALUE(E35),E35,D35)","v":0},null,{"$f":"Enk_My_afd_krit_2","v":0},{"$f":"IF(VALUE(H35),H35,G35)","v":0},null,{"$f":"Enk_My_afd_krit_3","v":0},{"$f":"IF(VALUE(K35),K35,J35)","v":0},null,{"$f":"Enk_My_afd_krit_4","v":0},{"$f":"IF(VALUE(N35),N35,M35)","v":0},null,"D_Enk_afd_krit_n","input"]
["1. ordens nedbrydningskonstant aerob - poreluft","k1_aerob_poreluft","dag-1",null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_poreluft_1),Enk_My_k1aerob_poreluft_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(E36),E36,D36)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_poreluft_2),Enk_My_k1aerob_poreluft_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(H36),H36,G36)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_poreluft_3),Enk_My_k1aerob_poreluft_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(K36),K36,J36)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_poreluft_4),Enk_My_k1aerob_poreluft_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(N36),N36,M36)","v":0},null,"D_Enk_k1anaerob_poreluft_n","input"]
["Interval 1. ordens nedbryd.konst. aerob - poreluft","k1_aerob_poreluft_int","dag-1",null,null,{"$f":"D_Enk_k1anaerob_poreluft_int_syst_1","v":0},null,null,{"$f":"D_Enk_k1anaerob_poreluft_int_syst_2","v":0},null,null,{"$f":"D_Enk_k1anaerob_poreluft_int_syst_3","v":0},null,null,null,null,"D_Enk_k1anaerob_poreluft_int_n","input"]
["Grundvandsberegninger"]
["1. ordens nedbrydningskonstant aerobtvand","k1_aerob_grundvand","år-1",null,{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_1),Enk_MY_k1aerob_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(E39),E39,IF(ISNUMBER(D39),D39,\"\"))","v":""},null,{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_2),Enk_MY_k1aerob_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(H39),H39,IF(ISNUMBER(G39),G39,\"\"))","v":""},null,{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_3),Enk_MY_k1aerob_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(K39),K39,J39)","v":0},null,{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_4),Enk_MY_k1aerob_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(N39),N39,IF(ISNUMBER(M39),M39,\"\"))","v":""},null,"D_Enk_k1aerob_n","input"]
["Interval 1. ordens nedbrydn.kons. aerobtvand","k1_aerob_grundvand_int","år-1",null,null,{"$f":"D_Enk_k1aerob_int_syst_1","v":0},null,null,{"$f":"D_Enk_k1aerob_int_syst_2","v":0},null,null,{"$f":"D_Enk_k1aerob_int_syst_3","v":0},null,null,{"$f":"D_Enk_k1aerob_int_syst_4","v":0},null,"D_Enk_k1aerob_int_n","input"]
["1. ordens nedbrydningskonstant anaerobtvand","k1_anaerob_grundvand","år-1",null,{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_1),Enk_MY_k1anaerob_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(E41),E41,IF(ISNUMBER(D41),D41,\"\"))","v":""},null,{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_2),Enk_MY_k1anaerob_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(H41),H41,IF(ISNUMBER(G41),G41,\"\"))","v":""},null,{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_3),Enk_MY_k1anaerob_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(K41),K41,IF(ISNUMBER(J41),J41,\"\"))","v":""},null,{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_4),Enk_MY_k1anaerob_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(N41),N41,IF(ISNUMBER(M41),M41,\"\"))","v":""},null,"D_Enk_k1anaerob_n","input"]
["Interval 1. ordens nedbryd.kons. anaerobtvand","k1_anaerob_grundvand_int","år-1",null,null,{"$f":"D_Enk_k1anaerob_int_syst_1","v":0},null,null,{"$f":"D_Enk_k1anaerob_int_syst_2","v":0},null,null,{"$f":"D_Enk_k1anaerob_int_syst_3","v":0},null,null,{"$f":"D_Enk_k1anaerob_int_syst_4","v":0},null,"D_Enk_k1anaerob_int_n","input"]
["Grundvands-kvalitetskriterie","GV-krit","µg/l",null,{"$f":"Enk_My_GV_krit_1","v":0},{"$f":"IF(VALUE(E43),E43,D43)","v":0},null,{"$f":"Enk_My_GV_krit_2","v":0},{"$f":"IF(VALUE(H43),H43,G43)","v":0},null,{"$f":"Enk_My_GV_krit_3","v":0},{"$f":"IF(VALUE(K43),K43,J43)","v":0},null,{"$f":"Enk_My_GV_krit_4","v":0},{"$f":"IF(VALUE(N43),N43,M43)","v":0},null,null,"input"]
["Grundvandkvalitetskriterie, omregnet","GV-krit","mg/l",null,null,{"$f":"IF(VALUE(F43/1000),(F43/1000),\"\")","v":""},null,null,{"$f":"IF(VALUE(I43/1000),(I43/1000),\"\")","v":""},null,null,{"$f":"IF(VALUE(L43/1000),(L43/1000),\"\")","v":""},null,null,{"$f":"IF(VALUE(O43/1000),(O43/1000),\"\")","v":""},null,"D_Enk_GV_krit_n","beregnes i dataark"]
["Diffusionskoefficient vand","DW","m²/s",null,{"$f":"Enk_My_Ddw_1","v":0},{"$f":"IF(VALUE(E45),E45,D45)","v":0},null,{"$f":"Enk_My_Ddw_2","v":0},{"$f":"IF(VALUE(H45),H45,G45)","v":0},null,{"$f":"Enk_My_Ddw_3","v":0},{"$f":"IF(VALUE(K45),K45,J45)","v":0},null,{"$f":"Enk_My_Ddw_4","v":0},{"$f":"IF(VALUE(N45),N45,M45)","v":0},null,"D_Enk_Ddw_n","input"]
["Umættetzone beregninger"]
["1. ordens nedbrydningskonstant aerob - umættet zone","k1_aerob_umættet","dage-1",null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_1),Enk_My_k1aerob_umættet_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(E47),E47,D47)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_2),Enk_My_k1aerob_umættet_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(H47),H47,G47)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_3),Enk_My_k1aerob_umættet_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(K47),K47,J47)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_4),Enk_My_k1aerob_umættet_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(N47),N47,M47)","v":0},null,"D_Enk_k1aerob_uz_n","input"]
["Interval 1. ordens nedbryd.kons. u aerobe.","k1_aerob_umættet_int",null,null,null,{"$f":"D_Enk_k1aerob_uz_int_syst_1","v":0},null,null,{"$f":"D_Enk_k1aerob_uz_int_syst_2","v":0},null,null,{"$f":"D_Enk_k1aerob_uz_int_syst_3","v":0},null,null,{"$f":"D_Enk_k1aerob_uz_int_syst_4","v":0},null,"D_Enk_k1aerob_uz_int_n","input"]
["1. ordens nedbrydningskonstant anaerob - umættet zone","k1_anaerob_umættet","dage-1",null,{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_1),Enk_My_k1anaerob_umættet_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(E49),E49,D49)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_2),Enk_My_k1anaerob_umættet_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(H49),H49,G49)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_3),Enk_My_k1anaerob_umættet_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(K49),K49,J49)","v":0},null,{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_4),Enk_My_k1anaerob_umættet_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(N49),N49,M49)","v":0},null,"D_Enk_k1anaerob_umættet_n","input"]
["Interval 1. ordens nedbryd.kons. U. anaerob.","k1_anaerob_umættet_int",null,null,null,{"$f":"D_Enk_k1anaerob_umættet_int_syst_1","v":0},null,null,{"$f":"D_Enk_k1anaerob_umættet_int_syst_2","v":0},null,null,{"$f":"D_Enk_k1anaerob_umættet_int_syst_3","v":0},null,null,null,null,"D_Enk_k1anaerob_umættet_int_n","input"]
[]
["Maksimale stofkoncentrationer"]
[null,null,null,"Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4"]
[null,null,null,"Beregnet","Indtastet","Anvendes",{"$f":"D54","v":"Beregnet"},"Indtastet","Anvendes",{"$f":"D54","v":"Beregnet"},"Indtastet","Anvendes",{"$f":"D54","v":"Beregnet"},"Indtastet","Anvendes"]
[null,"ML,max","mg/m³ pr. jordvol.",null,null,{"$f":"B_Enk_MLmax_1","v":0},null,null,{"$f":"B_Enk_MLmax_2","v":0},null,null,{"$f":"B_Enk_MLmax_3","v":0},null,null,{"$f":"B_Enk_MLmax_4","v":0},null,"D_Enk_MLmax_n","beregnes"]
[null,"MV, max","mg/m³ pr. jordvol.",null,null,{"$f":"B_Enk_MVmax_1","v":0},null,null,{"$f":"B_Enk_MVmax_2","v":0},null,null,{"$f":"B_Enk_MVmax_3","v":0},null,null,{"$f":"B_Enk_MVmax_4","v":0},null,"D_Enk_MVmax_n","beregnes"]
[null,"MJ, max","mg/m³ pr. jordvol.",null,null,{"$f":"B_Enk_MJmax_1","v":0},null,null,{"$f":"B_Enk_MJmax_2","v":0},null,null,{"$f":"B_Enk_MJmax_3","v":0},null,null,{"$f":"B_Enk_MJmax_4","v":0},null,"D_Enk_MJmax_n","beregnes"]
["Maksimal ford. luft","fl","brokdel",null,null,{"$f":"B_Enk_fl_1","v":""},null,null,{"$f":"B_Enk_fl_2","v":""},null,null,{"$f":"B_Enk_fl_3","v":""},null,null,{"$f":"B_Enk_fl_4","v":""},null,"D_Enk_fl_n","beregnes"]
["Maksimal ford. vand","fv","brokdel",null,null,{"$f":"B_Enk_fv_1","v":""},null,null,{"$f":"B_Enk_fv_2","v":""},null,null,{"$f":"B_Enk_fv_3","v":""},null,null,{"$f":"B_Enk_fv_4","v":""},null,"D_Enk_fv_n","beregnes"]
["Maksimal ford. jord","fj","brokdel",null,null,{"$f":"B_Enk_fj_1","v":""},null,null,{"$f":"B_Enk_fj_2","v":""},null,null,{"$f":"B_Enk_fj_3","v":""},null,null,{"$f":"B_Enk_fj_4","v":""},null,"D_Enk_fj_n","beregnes"]
["Mættede dampptryk","CLmax","Mg/m³",null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",B_Enk_Clmax_1,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",B_Enk_Clmax_2,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",B_Enk_Clmax_3,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",B_Enk_Clmax_4,\"\")","v":""}]
[]
["Fugacitets beregninger",null,null,"Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4"]
["Navn","Forkortelse","Enhed","Beregnet","Indtastet","Anvendes","Beregnet","Indtastet","Anvendes","Beregnet","Indtastet","Anvendes","Beregnet","Indtastet","Anvendes"]
["Forureningskomponent",null,null,{"$f":"Enk_stofnavn_1","v":""},null,null,{"$f":"Enk_stofnavn_2","v":""},null,null,{"$f":"Enk_stofnavn_3","v":""},null,null,{"$f":"Enk_stofnavn_4","v":""},null,null,null,null,"Overført værdi"]
["Målepunkt","MP",null,null,{"$f":"Enk_MP_1","v":""},{"$f":"IF(E66<>0,E66,\"\")","v":""},null,{"$f":"Enk_MP_2","v":""},{"$f":"IF(H66<>0,H66,\"\")","v":""},null,{"$f":"Enk_MP_3","v":""},{"$f":"IF(K66<>0,K66,\"\")","v":""},null,{"$f":"Enk_MP_4","v":""},{"$f":"IF(N66<>0,N66,\"\")","v":""},null,"D_Enk_MP_n","input"]
["dato","dato",null,null,{"$f":"Enk_dato_1","v":"00:00:00"},{"$f":"IF(VALUE(E67),E67,\" \")","v":" "},null,{"$f":"Enk_dato_2","v":"00:00:00"},{"$f":"IF(VALUE(H67),H67,\" \")","v":" "},null,{"$f":"Enk_dato_3","v":0},{"$f":"IF(VALUE(K67),K67,\" \")","v":" "},null,{"$f":"Enk_dato_4","v":0},{"$f":"IF(VALUE(N67),N67,\" \")","v":" "},null,"D_Enk_dato_n","input"]
["Målt koncentration i poreluft","CL","mg/m³",null,{"$f":"Enk_My_CL_1","v":0},{"$f":"E68","v":0},null,{"$f":"Enk_My_CL_2","v":0},{"$f":"H68","v":0},null,{"$f":"Enk_My_CL_3","v":0},{"$f":"K68","v":0},null,{"$f":"Enk_My_CL_4","v":0},{"$f":"N68","v":0},null,"D_Enk_CL_n","input"]
["Beregnet jordkoncentration","Ct","mg/kg TS",null,null,{"$f":"B_Enk_Ct_L_1","v":0},null,null,{"$f":"B_Enk_Ct_L_2","v":0},null,null,{"$f":"B_Enk_Ct_L_3","v":0},null,null,{"$f":"B_Enk_Ct_L_4","v":0},null,"D_Enk_Ct_L_n","beregnes"]
["Beregnet vandkoncentration","CV","mg/l",null,null,{"$f":"B_Enk_Cv_L_1","v":0},null,null,{"$f":"B_Enk_Cv_L_2","v":0},null,null,{"$f":"B_Enk_Cv_L_3","v":0},null,null,{"$f":"B_Enk_Cv_L_4","v":0},null,"D_Enk_Cv_L_n","beregnes"]
["Målt konc. i grundvand","CV","mg/l",null,{"$f":"Enk_My_CV_1","v":0},{"$f":"E71","v":0},null,{"$f":"Enk_My_CV_2","v":0},{"$f":"H71","v":0},null,{"$f":"Enk_My_CV_3","v":0},{"$f":"K71","v":0},null,{"$f":"Enk_My_CV_4","v":0},{"$f":"N71","v":0},null,"D_Enk_CV_n","input"]
["Beregnet poreluftskonc.","CL","mg/m³",null,null,{"$f":"B_Enk_Cl_V_1","v":0},null,null,{"$f":"B_Enk_Cl_V_2","v":0},null,null,{"$f":"B_Enk_Cl_V_3","v":0},null,null,{"$f":"B_Enk_Cl_V_4","v":0},null,"D_Enk_Cl_V_n","beregnes"]
["Beregnet jordkonc.","Ct","mg/kg TS",null,null,{"$f":"B_Enk_Ct_V_1","v":0},null,null,{"$f":"B_Enk_Ct_V_2","v":0},null,null,{"$f":"B_Enk_Ct_V_3","v":0},null,null,{"$f":"B_Enk_Ct_V_4","v":0},null,"D_Enk_Ct_V_n","beregnes"]
["Målt koncentration i jorden","Ct","mg/kg TS",null,{"$f":"Enk_My_Ct_1","v":0},{"$f":"E74","v":0},null,{"$f":"Enk_My_Ct_2","v":0},{"$f":"H74","v":0},null,{"$f":"Enk_My_Ct_3","v":0},{"$f":"K74","v":0},null,{"$f":"Enk_My_Ct_4","v":0},{"$f":"N74","v":0},null,"D_Enk_CT_n","input"]
["Beregnet poreluftskonc.","CL","mg/m³",null,null,{"$f":"B_Enk_Cl_J_1","v":0},null,null,{"$f":"B_Enk_Cl_J_2","v":0},null,null,{"$f":"B_Enk_Cl_J_3","v":0},null,null,{"$f":"B_Enk_Cl_J_4","v":0},null,"D_Enk_Cl_J_n","beregnes"]
["Beregnet vandkoncentration","CV","mg/l",null,null,{"$f":"B_Enk_Cv_J_1","v":0},null,null,{"$f":"B_Enk_Cv_J_2","v":0},null,null,{"$f":"B_Enk_Cv_J_3","v":0},null,null,{"$f":"B_Enk_Cv_J_4","v":0},null,"D_Enk_Cv_J_n","beregnes"]
["Endelig koncentration i poreluft","CL","mg/m³",null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Enk_CL_1<>0,D_Enk_CL_1,IF(D_Enk_Cl_V_1<>0,D_Enk_Cl_V_1,IF(D_Enk_Cl_J_1<>0,D_Enk_Cl_J_1,\"\"))),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Enk_CL_2<>0,D_Enk_CL_2,IF(D_Enk_Cl_V_2<>0,D_Enk_Cl_V_2,IF(D_Enk_Cl_J_2<>0,D_Enk_Cl_J_2,\"\"))),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Enk_CL_3<>0,D_Enk_CL_3,IF(D_Enk_Cl_V_3<>0,D_Enk_Cl_V_3,IF(D_Enk_Cl_J_3<>0,D_Enk_Cl_J_3,\"\"))),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Enk_CL_4<>0,D_Enk_CL_4,IF(D_Enk_Cl_V_4<>0,D_Enk_Cl_V_4,IF(D_Enk_Cl_J_4<>0,D_Enk_Cl_J_4,\"\"))),\"\")","v":""},null,"D_Enk_CL_endelig_n","beregnes i dataark"]
["Endelig koncentration i vand","CV","mg/l",null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Enk_CV_1<>0,D_Enk_CV_1,IF(D_Enk_Cv_L_1<>0,D_Enk_Cv_L_1,IF(D_Enk_Cv_J_1<>0,D_Enk_Cv_J_1,\"\"))),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Enk_CV_2<>0,D_Enk_CV_2,IF(D_Enk_Cv_L_2<>0,D_Enk_Cv_L_2,IF(D_Enk_Cv_J_2<>0,D_Enk_Cv_J_2,\"\"))),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Enk_CV_3<>0,D_Enk_CV_3,IF(D_Enk_Cv_L_3<>0,D_Enk_Cv_L_3,IF(D_Enk_Cv_J_3<>0,D_Enk_Cv_J_3,\"\"))),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Enk_CV_4<>0,D_Enk_CV_4,IF(D_Enk_Cv_L_4<>0,D_Enk_Cv_L_4,IF(D_Enk_Cv_J_4<>0,D_Enk_Cv_J_4,\"\"))),\"\")","v":""},null,"D_Enk_CV_endelig_n","beregnes i dataark"]
["Endelig koncentration i Jord","Ct","mg/kg TS",null,null,{"$f":"IF(D_Enk_CT_1<>0,D_Enk_CT_1,IF(D_Enk_Ct_L_1<>0,D_Enk_Ct_L_1,IF(D_Enk_Ct_V_1<>0,D_Enk_Ct_V_1,\"\")))","v":""},null,null,{"$f":"IF(D_Enk_CT_2<>0,D_Enk_CT_2,IF(D_Enk_Ct_L_2<>0,D_Enk_Ct_L_2,IF(D_Enk_Ct_V_2<>0,D_Enk_Ct_V_2,\"\")))","v":""},null,null,{"$f":"IF(D_Enk_CT_3<>0,D_Enk_CT_3,IF(D_Enk_Ct_L_3<>0,D_Enk_Ct_L_3,IF(D_Enk_Ct_V_3<>0,D_Enk_Ct_V_3,\"\")))","v":""},null,null,{"$f":"IF(D_Enk_CT_4<>0,D_Enk_CT_4,IF(D_Enk_Ct_L_4<>0,D_Enk_Ct_L_4,IF(D_Enk_Ct_V_4<>0,D_Enk_Ct_V_4,\"\")))","v":""},null,null,"beregnes i dataark"]
["Fri fase ud fra poreluft",null,null,null,null,{"$f":"B_Enk_FF_P_1","v":"nej"},null,null,{"$f":"B_Enk_FF_P_2","v":"nej"},null,null,{"$f":"B_Enk_FF_P_3","v":"nej"},null,null,{"$f":"B_Enk_FF_P_4","v":"nej"},null,"D_Enk_FF_P_n","beregnes"]
["Fri fase ud fra grundvand",null,null,null,null,{"$f":"B_Enk_FF_V_1","v":"nej"},null,null,{"$f":"B_Enk_FF_V_2","v":"nej"},null,null,{"$f":"B_Enk_FF_V_3","v":"nej"},null,null,{"$f":"B_Enk_FF_V_4","v":"nej"},null,"D_Enk_FF_V_n","beregnes"]
["Fri fase ud fra jord",null,null,null,null,{"$f":"B_Enk_FF_J_1","v":"nej"},null,null,{"$f":"B_Enk_FF_J_2","v":"nej"},null,null,{"$f":"B_Enk_FF_J_3","v":"nej"},null,null,{"$f":"B_Enk_FF_J_4","v":"nej"},null,"D_Enk_FF_J_n","beregnes"]
["Fri fase ??",null,null,null,null,{"$f":"B_Enk_FF_1","v":"nej"},null,null,{"$f":"B_Enk_FF_2","v":"nej"},null,null,{"$f":"B_Enk_FF_3","v":"nej"},null,null,{"$f":"B_Enk_FF_4","v":"nej"},null,"D_Enk_FF_n","beregnes"]
["Anvendt Brugerdata",null,null,null,{"$f":"SUM(E21,E24:E31,$F7:$F9,$F12,$F14)","v":0},{"$f":"IF(E84>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(H21,H24:H31,$F7:$F9,$F12,$F14)","v":0},{"$f":"IF(H84>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(K21,K24:K31,$F7:$F9,$F12,$F14)","v":0},{"$f":"IF(K84>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(N21,N24:N31,$F7:$F9,$F12,$F14)","v":0},{"$f":"IF(N84>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,"D_Enk_Brugerdata_n","beregnes i dataark"]
["Anvendt Brugerdata til udeluft",null,null,null,{"$f":"SUM(E33:E37)","v":0},null,null,{"$f":"SUM(H33:H37)","v":0},null,null,{"$f":"SUM(K33:K37)","v":0},null,null,{"$f":"SUM(N33:N37)","v":0}]
["Anvendt Brugerdata til flux",null,null,null,{"$f":"SUM($F8:$F14,E26:E31)","v":0},null,null,{"$f":"SUM($F8:$F14,H26:H31)","v":0},null,null,{"$f":"SUM($F8:$F14,K26:K31)","v":0},null,null,{"$f":"SUM($F8:$F14,N26:N31)","v":0},null,null,"D_enk_brugerflux_n","beregnes i dataark"]
["Anvendt Brugerdata til grundvand",null,null,null,{"$f":"SUM(E39:E45)","v":0},null,null,{"$f":"SUM(H39:H45)","v":0},null,null,{"$f":"SUM(K39:K45)","v":0},null,null,{"$f":"SUM(N39:N45)","v":0},null,null,null,"beregnes i dataark"]
[]
["Bemærkninger"]
["Midlertidigt id nr:","Com_Enk_Kem","Enk_Jord",null,null,null,null,null,null,null,null,null,null,null,null,null,"Com_Ind_VenFor","Import . Bemærkningsfelt"]
[]
["Jordtype:","D_Enk_Jord_Com",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Enk_Jord_Com","Import . Bemærkningsfelt"]
[null,false]
["Kemisk data:","D_Enk_Kem_Com",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Enk_Kem_Com","Import . Bemærkningsfelt"]
[null,false]
["Fugacitet:","D_Enk_Fug_Com",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Enk_Fug_Com","Import . Bemærkningsfelt"]
[null,false]

{"sheet":"Beregning_Enkeltstoffer","index":7,"n_rows":66,"n_cols":12,"rows_kept":66,"cut":false,"hidden":true,"merged":[[2,1,2,9],[39,2,39,8],[4,2,4,6],[15,2,15,5],[30,2,30,8],[19,2,19,8]]}
[]
[]
[null,"Beregning Enkeltstoffer",null,null,null,null,null,null,null,null,null,"Systemnavn"]
[]
[null,null,"Jord"]
[null,"Bemærkninger","Navn","Forkortelse","Enhed","Anvendt","Beregnet"]
[null,null,"Jordtype",null,null,{"$f":"D_Enk_Jordtype","v":""},null,null,null,null,null,"B_Enk_jordtype"]
[null,null,"Poreluftvolumen","VL",null,{"$f":"D_Enk_VL","v":0},null,null,null,null,null,"B_Enk_VL"]
[null,null,"Vandindhold","VV",null,{"$f":"D_Enk_VV","v":0},null,null,null,null,null,"B_Enk_VV"]
[null,null,"Samlet\nporøsitet","e=VL+VV",null,{"$f":"G10","v":0},{"$f":"B_Enk_VL+B_Enk_VV","v":0},null,null,null,null,"B_Enk_porositet"]
[null,null,"Volumen af jordskellet","VJ",null,{"$f":"G11","v":1},{"$f":"1-B_Enk_porositet","v":1},null,null,null,null,"B_Enk_VJ"]
[null,null,"Kornrumvægt","d","kg/l",{"$f":"D_Enk_d","v":0},null,null,null,null,null,"B_Enk_d"]
[null,null,"Volumenvægt","r","kg/l",{"$f":"G13","v":0},{"$f":"B_Enk_d*B_Enk_VJ","v":0},null,null,null,null,"B_Enk_p"]
[null,null,"Indhold af organisk kulstof","foc",null,{"$f":"D_Enk_foc","v":0},null,null,null,null,null,"B_Enk_foc"]
[]
[null,null,"Konstanter"]
[null,null,"Gaskonstanten","R","J/mol*K",8.3140000000000001,null,null,null,null,null,"B_enk_R"]
[null,null,"Temperatur","K","Kelvin",298,null,null,null,null,null,"B_Enk_K"]
[]
[null,null,"Stofegenskaber"]
[null,null,null,null,null,"STOF 1","STOF 2","STOF 3","STOF 4"]
[null,null,"Navn","Forkortelse","Enhed","Anvendt","Anvendt","Anvendt","Anvendt"]
[null,null,"Forureningskomponent","-","-",{"$f":"D_Enk_stofnavn_1","v":""},{"$f":"D_Enk_stofnavn_2","v":""},{"$f":"D_Enk_stofnavn_3","v":""},{"$f":"D_Enk_stofnavn_4","v":""},null,null,"B_Enk_stofnavn_n"]
[null,null,"Molmasse","m","gram/mol",{"$f":"D_Enk_m_1","v":0},{"$f":"D_Enk_m_2","v":0},{"$f":"D_Enk_m_3","v":0},{"$f":"D_Enk_m_4","v":0},null,null,"B_Enk_m_n"]
[null,null,"Damptryk","p","Pa",{"$f":"D_Enk_p_1","v":0},{"$f":"D_Enk_p_2","v":0},{"$f":"D_Enk_p_3","v":0},{"$f":"D_Enk_p_4","v":0},null,null,"B_Enk_p_n"]
[null,null,"Vandopløselighed","S","mg/l",{"$f":"D_Enk_S_1","v":0},{"$f":"D_Enk_S_2","v":0},{"$f":"D_Enk_S_3","v":0},{"$f":"D_Enk_S_4","v":0},null,null,"B_Enk_S_n"]
[null,null,"log oktanol/vand ford. koeff.","log Kow",null,{"$f":"D_Enk_KOW_1","v":0},{"$f":"D_Enk_KOW_2","v":0},{"$f":"D_Enk_KOW_3","v":0},{"$f":"D_Enk_KOW_4","v":0},null,null,"B_Enk_KOW_n"]
[null,null,"Koc","Koc",null,{"$f":"D_Enk_KOC_1","v":0},{"$f":"D_Enk_KOC_2","v":0},{"$f":"D_Enk_KOC_3","v":0},{"$f":"D_Enk_KOC_4","v":0},null,null,"B_Enk_KOC_n"]
[null,null,"Henrys konstant","KH",null,{"$f":"D_Enk_KH_1","v":0},{"$f":"D_Enk_KH_2","v":0},{"$f":"D_Enk_KH_3","v":0},{"$f":"D_Enk_KH_4","v":0},null,null,"B_Enk_KH_n"]
[null,"MST nr.7 1998 "]
[null,"App. 5.3","Maksimale stofkoncentrationer"]
[null,"Ligning 2",null,"ML,max","mg/m³ pr. jordvol.",{"$f":"FugLigning2(B_Enk_VL,B_Enk_Clmax_1)","v":0},{"$f":"FugLigning2(B_Enk_VL,B_Enk_Clmax_2)","v":0},{"$f":"FugLigning2(B_Enk_VL,B_Enk_Clmax_3)","v":0},{"$f":"FugLigning2(B_Enk_VL,B_Enk_Clmax_4)","v":0},null,null,"B_Enk_MLmax_n"]
[null,"Ligning 3",null,"CL,max","mg/m³ pr. jordvol.",{"$f":"FugLigning3(B_Enk_p_1,B_Enk_m_1,B_enk_R,B_Enk_K)","v":0},{"$f":"FugLigning3(B_Enk_p_2,B_Enk_m_2,B_enk_R,B_Enk_K)","v":0},{"$f":"FugLigning3(B_Enk_p_3,B_Enk_m_3,B_enk_R,B_Enk_K)","v":0},{"$f":"FugLigning3(B_Enk_p_4,B_Enk_m_4,B_enk_R,B_Enk_K)","v":0},null,null,"B_Enk_Clmax_n"]
[null,"Ligning 4",null,"MV, max","mg/m³ pr. jordvol.",{"$f":"FugLigning4(B_Enk_VV,B_Enk_S_1)","v":0},{"$f":"FugLigning4(B_Enk_VV,B_Enk_S_2)","v":0},{"$f":"FugLigning4(B_Enk_VV,B_Enk_S_3)","v":0},{"$f":"FugLigning4(B_Enk_VV,B_Enk_S_4)","v":0},null,null,"B_Enk_MVmax_n"]
[null,"Ligning 9",null,"MJ, max","mg/m³ pr. jordvol.",{"$f":"FugLigning9(B_Enk_VJ,B_Enk_d,B_Enk_KOC_1,B_Enk_foc,B_Enk_S_1)","v":0},{"$f":"FugLigning9(B_Enk_VJ,B_Enk_d,B_Enk_KOC_2,B_Enk_foc,B_Enk_S_2)","v":0},{"$f":"FugLigning9(B_Enk_VJ,B_Enk_d,B_Enk_KOC_3,B_Enk_foc,B_Enk_S_3)","v":0},{"$f":"FugLigning9(B_Enk_VJ,B_Enk_d,B_Enk_KOC_4,B_Enk_foc,B_Enk_S_4)","v":0},null,null,"B_Enk_MJmax_n"]
[null,"Ligning 11 modificeret","Maksimal ford. luft","fl",null,{"$f":"IF(ISNUMBER(B_Enk_MLmax_1/(B_Enk_MLmax_1+B_Enk_MVmax_1+B_Enk_MJmax_1)),B_Enk_MLmax_1/(B_Enk_MLmax_1+B_Enk_MVmax_1+B_Enk_MJmax_1),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MLmax_2/(B_Enk_MLmax_2+B_Enk_MVmax_2+B_Enk_MJmax_2)),B_Enk_MLmax_2/(B_Enk_MLmax_2+B_Enk_MVmax_2+B_Enk_MJmax_2),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MLmax_3/(B_Enk_MLmax_3+B_Enk_MVmax_3+B_Enk_MJmax_3)),B_Enk_MLmax_3/(B_Enk_MLmax_3+B_Enk_MVmax_3+B_Enk_MJmax_3),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MLmax_4/(B_Enk_MLmax_4+B_Enk_MVmax_4+B_Enk_MJmax_4)),B_Enk_MLmax_4/(B_Enk_MLmax_4+B_Enk_MVmax_4+B_Enk_MJmax_4),\"\")","v":""},null,null,"B_Enk_fl_n"]
[null,"Ligning 11 modificeret","Maksimal ford. vand","fv",null,{"$f":"IF(ISNUMBER(B_Enk_MVmax_1/(B_Enk_MLmax_1+B_Enk_MVmax_1+B_Enk_MJmax_1)),B_Enk_MVmax_1/(B_Enk_MLmax_1+B_Enk_MVmax_1+B_Enk_MJmax_1),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MVmax_2/(B_Enk_MLmax_2+B_Enk_MVmax_2+B_Enk_MJmax_2)),B_Enk_MVmax_2/(B_Enk_MLmax_2+B_Enk_MVmax_2+B_Enk_MJmax_2),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MVmax_3/(B_Enk_MLmax_3+B_Enk_MVmax_3+B_Enk_MJmax_3)),B_Enk_MVmax_3/(B_Enk_MLmax_3+B_Enk_MVmax_3+B_Enk_MJmax_3),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MVmax_4/(B_Enk_MLmax_4+B_Enk_MVmax_4+B_Enk_MJmax_4)),B_Enk_MVmax_4/(B_Enk_MLmax_4+B_Enk_MVmax_4+B_Enk_MJmax_4),\"\")","v":""},null,null,"B_Enk_fv_n"]
[null,"Ligning 11 modificeret","Maksimal ford. jord","fj",null,{"$f":"IF(ISNUMBER(B_Enk_MJmax_1/(B_Enk_MLmax_1+B_Enk_MVmax_1+B_Enk_MJmax_1)),B_Enk_MJmax_1/(B_Enk_MLmax_1+B_Enk_MVmax_1+B_Enk_MJmax_1),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MJmax_2/(B_Enk_MLmax_2+B_Enk_MVmax_2+B_Enk_MJmax_2)),B_Enk_MJmax_2/(B_Enk_MLmax_2+B_Enk_MVmax_2+B_Enk_MJmax_2),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MJmax_3/(B_Enk_MLmax_3+B_Enk_MVmax_3+B_Enk_MJmax_3)),B_Enk_MJmax_3/(B_Enk_MLmax_3+B_Enk_MVmax_3+B_Enk_MJmax_3),\"\")","v":""},{"$f":"IF(ISNUMBER(B_Enk_MJmax_4/(B_Enk_MLmax_4+B_Enk_MVmax_4+B_Enk_MJmax_4)),B_Enk_MJmax_4/(B_Enk_MLmax_4+B_Enk_MVmax_4+B_Enk_MJmax_4),\"\")","v":""},null,null,"B_Enk_fj_n"]
[]
[null,null,"Fugacitets beregninger"]
[null,null,"Målepunkt","MP",null,{"$f":"D_Enk_MP_1","v":""},{"$f":"D_Enk_MP_2","v":""},{"$f":"D_Enk_MP_3","v":""},{"$f":"D_Enk_MP_4","v":""},null,null,"B_Enk_MP_n"]
[null,null,"dato","dato",null,{"$f":"D_Enk_dato_1","v":" "},{"$f":"D_Enk_dato_2","v":" "},{"$f":"D_Enk_dato_3","v":" "},{"$f":"D_Enk_dato_4","v":" "},null,null,"B_Enk_dato_n"]
[null,null,"Målt koncentration i poreluft","CL","mg/m³",{"$f":"D_Enk_CL_1","v":0},{"$f":"D_Enk_CL_2","v":0},{"$f":"D_Enk_CL_3","v":0},{"$f":"D_Enk_CL_4","v":0},null,null,"B_Enk_CL_n"]
[null,"Ligning 14c","Beregnet jordkoncentration","Ct","mg/kg TS",{"$f":"IF(ISNUMBER(FugLigning14c(B_Enk_CL_1,B_Enk_VL,B_Enk_fl_1,B_Enk_p)),FugLigning14c(B_Enk_CL_1,B_Enk_VL,B_Enk_fl_1,B_Enk_p),0)","v":0},{"$f":"IF(ISNUMBER(FugLigning14c(B_Enk_CL_2,B_Enk_VL,B_Enk_fl_2,B_Enk_p)),FugLigning14c(B_Enk_CL_2,B_Enk_VL,B_Enk_fl_2,B_Enk_p),0)","v":0},{"$f":"IF(ISNUMBER(FugLigning14c(B_Enk_CL_3,B_Enk_VL,B_Enk_fl_3,B_Enk_p)),FugLigning14c(B_Enk_CL_3,B_Enk_VL,B_Enk_fl_3,B_Enk_p),0)","v":0},{"$f":"IF(ISNUMBER(FugLigning14c(B_Enk_CL_4,B_Enk_VL,B_Enk_fl_4,B_Enk_p)),FugLigning14c(B_Enk_CL_4,B_Enk_VL,B_Enk_fl_4,B_Enk_p),0)","v":0},null,null,"B_Enk_Ct_L_n"]
[null,"Ligning 14d","Beregnet vandskoncentration","CV","mg/l",{"$f":"IF(ISNUMBER(MIN(FugLigning14d(B_Enk_fv_1,B_Enk_VL,B_Enk_CL_1,B_Enk_fl_1,B_Enk_VV),B_Enk_S_1)),MIN(FugLigning14d(B_Enk_fv_1,B_Enk_VL,B_Enk_CL_1,B_Enk_fl_1,B_Enk_VV),B_Enk_S_1),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14d(B_Enk_fv_2,B_Enk_VL,B_Enk_CL_2,B_Enk_fl_2,B_Enk_VV),B_Enk_S_2)),MIN(FugLigning14d(B_Enk_fv_2,B_Enk_VL,B_Enk_CL_2,B_Enk_fl_2,B_Enk_VV),B_Enk_S_2),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14d(B_Enk_fv_3,B_Enk_VL,B_Enk_CL_3,B_Enk_fl_3,B_Enk_VV),B_Enk_S_3)),MIN(FugLigning14d(B_Enk_fv_3,B_Enk_VL,B_Enk_CL_3,B_Enk_fl_3,B_Enk_VV),B_Enk_S_3),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14d(B_Enk_fv_4,B_Enk_VL,B_Enk_CL_4,B_Enk_fl_4,B_Enk_VV),B_Enk_S_4)),MIN(FugLigning14d(B_Enk_fv_4,B_Enk_VL,B_Enk_CL_4,B_Enk_fl_4,B_Enk_VV),B_Enk_S_4),0)","v":0},null,null,"B_Enk_Cv_L_n"]
[null,null,"Målt konc. i grundvand","CV","mg/l",{"$f":"D_Enk_CV_1","v":0},{"$f":"D_Enk_CV_2","v":0},{"$f":"D_Enk_CV_3","v":0},{"$f":"D_Enk_CV_4","v":0},null,null,"B_Enk_CV_n"]
[null,"Ligning 14e","Beregnet poreluftskonc.","CL","mg/m³",{"$f":"IF(ISNUMBER(MIN(FugLigning14e(B_Enk_CV_1,B_Enk_VV,B_Enk_fl_1,B_Enk_VL,B_Enk_fv_1),B_Enk_Clmax_1)),MIN(FugLigning14e(B_Enk_CV_1,B_Enk_VV,B_Enk_fl_1,B_Enk_VL,B_Enk_fv_1),B_Enk_Clmax_1),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14e(B_Enk_CV_2,B_Enk_VV,B_Enk_fl_2,B_Enk_VL,B_Enk_fv_2),B_Enk_Clmax_2)),MIN(FugLigning14e(B_Enk_CV_2,B_Enk_VV,B_Enk_fl_2,B_Enk_VL,B_Enk_fv_2),B_Enk_Clmax_2),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14e(B_Enk_CV_3,B_Enk_VV,B_Enk_fl_3,B_Enk_VL,B_Enk_fv_3),B_Enk_Clmax_3)),MIN(FugLigning14e(B_Enk_CV_3,B_Enk_VV,B_Enk_fl_3,B_Enk_VL,B_Enk_fv_3),B_Enk_Clmax_3),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14e(B_Enk_CV_4,B_Enk_VV,B_Enk_fl_4,B_Enk_VL,B_Enk_fv_4),B_Enk_Clmax_4)),MIN(FugLigning14e(B_Enk_CV_4,B_Enk_VV,B_Enk_fl_4,B_Enk_VL,B_Enk_fv_4),B_Enk_Clmax_4),0)","v":0},null,null,"B_Enk_Cl_V_n"]
[null,"Ligning 14f","Beregnet jordkonc.","Ct","mg/kg TS",{"$f":"IF(ISNUMBER(FugLigning14f(B_Enk_CV_1,B_Enk_VV,B_Enk_fv_1,B_Enk_p)),FugLigning14f(B_Enk_CV_1,B_Enk_VV,B_Enk_fv_1,B_Enk_p),0)","v":0},{"$f":"IF(ISNUMBER(FugLigning14f(B_Enk_CV_2,B_Enk_VV,B_Enk_fv_2,B_Enk_p)),FugLigning14f(B_Enk_CV_2,B_Enk_VV,B_Enk_fv_2,B_Enk_p),0)","v":0},{"$f":"IF(ISNUMBER(FugLigning14f(B_Enk_CV_3,B_Enk_VV,B_Enk_fv_3,B_Enk_p)),FugLigning14f(B_Enk_CV_3,B_Enk_VV,B_Enk_fv_3,B_Enk_p),0)","v":0},{"$f":"IF(ISNUMBER(FugLigning14f(B_Enk_CV_4,B_Enk_VV,B_Enk_fv_4,B_Enk_p)),FugLigning14f(B_Enk_CV_4,B_Enk_VV,B_Enk_fv_4,B_Enk_p),0)","v":0},null,null,"B_Enk_Ct_V_n"]
[null,null,"Målt koncentration i jorden","Ct","mg/kg TS",{"$f":"D_Enk_CT_1","v":0},{"$f":"D_Enk_CT_2","v":0},{"$f":"D_Enk_CT_3","v":0},{"$f":"D_Enk_CT_4","v":0},null,null,"B_Enk_CT_n"]
[null,"Ligning 14b","Beregnet poreluftskonc.","CL","mg/m³",{"$f":"IF(ISNUMBER(MIN(B_Enk_Clmax_1,FugLigning14(B_Enk_fl_1,B_Enk_CT_1,B_Enk_p,B_Enk_VL))),MIN(B_Enk_Clmax_1,FugLigning14(B_Enk_fl_1,B_Enk_CT_1,B_Enk_p,B_Enk_VL)),0)","v":0},{"$f":"IF(ISNUMBER(MIN(B_Enk_Clmax_2,FugLigning14(B_Enk_fl_2,B_Enk_CT_2,B_Enk_p,B_Enk_VL))),MIN(B_Enk_Clmax_2,FugLigning14(B_Enk_fl_2,B_Enk_CT_2,B_Enk_p,B_Enk_VL)),0)","v":0},{"$f":"IF(ISNUMBER(MIN(B_Enk_Clmax_3,FugLigning14(B_Enk_fl_3,B_Enk_CT_3,B_Enk_p,B_Enk_VL))),MIN(B_Enk_Clmax_3,FugLigning14(B_Enk_fl_3,B_Enk_CT_3,B_Enk_p,B_Enk_VL)),0)","v":0},{"$f":"IF(ISNUMBER(MIN(B_Enk_Clmax_4,FugLigning14(B_Enk_fl_4,B_Enk_CT_4,B_Enk_p,B_Enk_VL))),MIN(B_Enk_Clmax_4,FugLigning14(B_Enk_fl_4,B_Enk_CT_4,B_Enk_p,B_Enk_VL)),0)","v":0},null,null,"B_Enk_Cl_J_n"]
[null,"Ligning 14","Beregnet vandskoncentration","CV","mg/l",{"$f":"IF(ISNUMBER(MIN(FugLigning14b(B_Enk_fv_1,B_Enk_CT_1,B_Enk_p,B_Enk_VV),B_Enk_S_1)),MIN(FugLigning14b(B_Enk_fv_1,B_Enk_CT_1,B_Enk_p,B_Enk_VV),B_Enk_S_1),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14b(B_Enk_fv_2,B_Enk_CT_2,B_Enk_p,B_Enk_VV),B_Enk_S_2)),MIN(FugLigning14b(B_Enk_fv_2,B_Enk_CT_2,B_Enk_p,B_Enk_VV),B_Enk_S_2),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14b(B_Enk_fv_3,B_Enk_CT_3,B_Enk_p,B_Enk_VV),B_Enk_S_3)),MIN(FugLigning14b(B_Enk_fv_3,B_Enk_CT_3,B_Enk_p,B_Enk_VV),B_Enk_S_3),0)","v":0},{"$f":"IF(ISNUMBER(MIN(FugLigning14b(B_Enk_fv_4,B_Enk_CT_4,B_Enk_p,B_Enk_VV),B_Enk_S_4)),MIN(FugLigning14b(B_Enk_fv_4,B_Enk_CT_4,B_Enk_p,B_Enk_VV),B_Enk_S_4),0)","v":0},null,null,"B_Enk_Cv_J_n"]
[null,null,"Fri fase ud fra poreluft",null,null,{"$f":"IF(IF(ISNUMBER(FugLigning14d(B_Enk_fv_1,B_Enk_VL,B_Enk_CL_1,B_Enk_fl_1,B_Enk_VV)),FugLigning14d(B_Enk_fv_1,B_Enk_VL,B_Enk_CL_1,B_Enk_fl_1,B_Enk_VV),0)>D_Enk_S_1,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IF(ISNUMBER(FugLigning14d(B_Enk_fv_2,B_Enk_VL,B_Enk_CL_2,B_Enk_fl_2,B_Enk_VV)),FugLigning14d(B_Enk_fv_2,B_Enk_VL,B_Enk_CL_2,B_Enk_fl_2,B_Enk_VV),0)>D_Enk_S_2,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IF(ISNUMBER(FugLigning14d(B_Enk_fv_3,B_Enk_VL,B_Enk_CL_3,B_Enk_fl_3,B_Enk_VV)),FugLigning14d(B_Enk_fv_3,B_Enk_VL,B_Enk_CL_3,B_Enk_fl_3,B_Enk_VV),0)>D_Enk_S_3,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IF(ISNUMBER(FugLigning14d(B_Enk_fv_4,B_Enk_VL,B_Enk_CL_4,B_Enk_fl_4,B_Enk_VV)),FugLigning14d(B_Enk_fv_4,B_Enk_VL,B_Enk_CL_4,B_Enk_fl_4,B_Enk_VV),0)>D_Enk_S_4,\"ja\",\"nej\")","v":"nej"},null,null,"B_Enk_FF_P_n"]
[null,null,"Fri fase ud fra grundvand",null,null,{"$f":"IF(D_Enk_CV_1>D_Enk_S_1,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(D_Enk_CV_2>D_Enk_S_2,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(D_Enk_CV_3>D_Enk_S_3,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(D_Enk_CV_4>D_Enk_S_4,\"ja\",\"nej\")","v":"nej"},null,null,"B_Enk_FF_V_n"]
[null,null,"Fri fase ud fra jord",null,null,{"$f":"IF(IF(ISNUMBER(FugLigning14b(B_Enk_fv_1,B_Enk_CT_1,B_Enk_p,B_Enk_VV)),FugLigning14b(B_Enk_fv_1,B_Enk_CT_1,B_Enk_p,B_Enk_VV),0)>B_Enk_S_1,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IF(ISNUMBER(FugLigning14b(B_Enk_fv_2,B_Enk_CT_2,B_Enk_p,B_Enk_VV)),FugLigning14b(B_Enk_fv_2,B_Enk_CT_2,B_Enk_p,B_Enk_VV),0)>B_Enk_S_2,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IF(ISNUMBER(FugLigning14b(B_Enk_fv_3,B_Enk_CT_3,B_Enk_p,B_Enk_VV)),FugLigning14b(B_Enk_fv_3,B_Enk_CT_3,B_Enk_p,B_Enk_VV),0)>B_Enk_S_3,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IF(ISNUMBER(FugLigning14b(B_Enk_fv_4,B_Enk_CT_4,B_Enk_p,B_Enk_VV)),FugLigning14b(B_Enk_fv_4,B_Enk_CT_4,B_Enk_p,B_Enk_VV),0)>B_Enk_S_4,\"ja\",\"nej\")","v":"nej"},null,null,"B_Enk_FF_J_n"]
[null,null,"Fri fase ??",null,null,{"$f":"IF(OR(B_Enk_FF_P_1=\"ja\",B_Enk_FF_V_1=\"ja\",B_Enk_FF_J_1=\"ja\"),\"Risiko for frifase\",\"nej\")","v":"nej"},{"$f":"IF(OR(B_Enk_FF_P_2=\"ja\",B_Enk_FF_V_2=\"ja\",B_Enk_FF_J_2=\"ja\"),\"Risiko for frifase\",\"nej\")","v":"nej"},{"$f":"IF(OR(B_Enk_FF_P_3=\"ja\",B_Enk_FF_V_3=\"ja\",B_Enk_FF_J_3=\"ja\"),\"Risiko for frifase\",\"nej\")","v":"nej"},{"$f":"IF(OR(B_Enk_FF_P_4=\"ja\",B_Enk_FF_V_4=\"ja\",B_Enk_FF_J_4=\"ja\"),\"Risiko for frifase\",\"nej\")","v":"nej"},null,null,"B_Enk_FF_n"]
[null,null,"Anvendt Brugerdata",null,null,{"$f":"D_Enk_Brugerdata_1","v":"Nej"},{"$f":"D_Enk_Brugerdata_2","v":"Nej"},{"$f":"D_Enk_Brugerdata_3","v":"Nej"},{"$f":"D_Enk_Brugerdata_4","v":"Nej"},null,null,"B_Enk_Brugerdata_n"]
[]
[null,null,"Bemærkninger"]
[null,null,"Midlertidigt id nr:"]
[]
[null,null,"Jordtype:",null,null,null,null,null,null,null,null,"D_Enk_Jord_Com"]
[null,null,null,false]
[null,null,"Kemisk data:",null,null,null,null,null,null,null,null,"D_Enk_Kem_Com"]
[null,null,null,false]
[null,null,"Fugacitet:",null,null,null,null,null,null,null,null,"D_Enk_Fug_Com"]
[null,null,null,false]

{"sheet":"Udskrift_Enkeltstoffer","index":8,"n_rows":94,"n_cols":17,"rows_kept":94,"cut":false,"hidden":true,"merged":[[92,1,105,9],[37,8,37,9],[50,2,50,3],[50,4,50,5],[50,6,50,7],[50,8,50,9],[62,1,75,9],[77,1,90,9],[52,2,52,3],[52,4,52,5],[52,6,52,7],[52,8,52,9],[55,7,55,9],[56,7,56,9],[55,1,55,4],[56,1,56,4],[36,0,36,1],[37,6,37,7],[22,6,22,7],[22,8,22,9],[37,2,37,3],[37,4,37,5],[21,8,21,9],[22,2,22,3],[22,4,22,5],[8,2,8,5],[9,4,9,5],[10,4,10,5],[11,4,11,5],[12,4,12,5],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[18,2,18,3],[19,6,20,7],[21,2,21,3],[21,4,21,5],[21,6,21,7],[13,4,13,5],[14,4,14,5],[15,4,15,5],[18,4,18,5],[2,8,2,10],[14,2,14,3],[15,2,15,3],[19,2,20,3],[19,4,20,5],[18,8,18,9],[19,8,20,9],[18,6,18,7],[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,10],[3,8,3,10],[4,8,4,10]]}
["Fugacitetsberegninger"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr./by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jord"]
["Kommentar",{"$f":"IF(D_Enk_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Standard data",null,"Indtastede data (angives med fed)"]
["Jordtype",null,{"$f":"D_Enk_Jordtype","v":""}]
["Poreluftvolumen","VL",{"$f":"IF(ISNUMBER(D_Enk_VL_syst),D_Enk_VL_syst,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_VL),Enk_My_VL,\"\")","v":""}]
["Vandindhold","VV",{"$f":"IF(ISNUMBER(D_Enk_VV_syst),D_Enk_VV_syst,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_VV),Enk_My_VV,\"\")","v":""}]
["Samlet porøsitet","e=VL+VV",{"$f":"IF(ISNUMBER(D_Enk_porositet),D_Enk_porositet,\"\")","v":0}]
["Volumen af jordskellet","VJ",{"$f":"D_Enk_VJ","v":1}]
["Kornrumvægt","d",{"$f":"IF(ISNUMBER(D_Enk_d_syst),D_Enk_d_syst,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_d),Enk_My_d,\"\")","v":""},null,"kg/l"]
["Volumenvægt","r",{"$f":"IF(ISNUMBER(D_Enk_p),D_Enk_p,\"\")","v":0},null,null,null,"kg/l"]
["Indhold af organisk kulstof","foc",{"$f":"IF(ISNUMBER(D_Enk_foc_syst),D_Enk_foc_syst,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_foc),Enk_My_foc,\"\")","v":""},null,"%"]
[]
["Stoffer"]
["Kommentar",{"$f":"IF(D_Enk_Kem_ComUds,\"ja\",\"nej\")","v":"nej"},"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
["Forureningskomponent",null,{"$f":"D_Enk_stofnavn_1","v":""},null,{"$f":"D_Enk_stofnavn_2","v":""},null,{"$f":"D_Enk_stofnavn_3","v":""},null,{"$f":"D_Enk_stofnavn_4","v":""},null,null,null,{"$f":"C20","v":""},{"$f":"E20","v":""},{"$f":"G20","v":""},{"$f":"I20","v":""}]
[]
["Målepunkt","MP",{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""},null,null,null,{"$f":"C22","v":""},{"$f":"E22","v":""},{"$f":"G22","v":""},{"$f":"I22","v":""}]
["Dato","dato",{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
["Molmasse","m",{"$f":"IF(ISNUMBER(D_Enk_m_syst_1),D_Enk_m_syst_1,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_m_1),Enk_My_m_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_m_syst_2),D_Enk_m_syst_2,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_m_2),Enk_My_m_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_m_syst_3),D_Enk_m_syst_3,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_m_3),Enk_My_m_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_m_syst_4),D_Enk_m_syst_4,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_m_4),Enk_My_m_4,\"\")","v":""},"g/mol"]
["Damptryk","p",{"$f":"IF(ISNUMBER(D_Enk_p_syst_1),D_Enk_p_syst_1,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_p_1),Enk_My_p_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_p_syst_2),D_Enk_p_syst_2,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_p_2),Enk_My_p_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_p_syst_3),D_Enk_p_syst_3,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_p_3),Enk_My_p_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_p_syst_4),D_Enk_p_syst_4,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_p_4),Enk_My_p_4,\"\")","v":""},"Pa"]
["Vandopløselighed","S",{"$f":"IF(ISNUMBER(D_Enk_S_syst_1),D_Enk_S_syst_1,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_S_1),Enk_My_S_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_S_syst_2),D_Enk_S_syst_2,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_S_2),Enk_My_S_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_S_syst_3),D_Enk_S_syst_3,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_S_3),Enk_My_S_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_S_syst_4),D_Enk_S_syst_4,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_S_4),Enk_My_S_4,\"\")","v":""},"mg/l"]
["log oktanol/vand ford. koeff.","log KOW",{"$f":"IF(ISNUMBER(D_Enk_KOW_syst_1),D_Enk_KOW_syst_1,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOW_1),Enk_My_KOW_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KOW_syst_2),D_Enk_KOW_syst_2,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOW_2),Enk_My_KOW_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KOW_syst_3),D_Enk_KOW_syst_3,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOW_3),Enk_My_KOW_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KOW_syst_4),D_Enk_KOW_syst_4,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOW_4),Enk_My_KOW_4,\"\")","v":""}]
["KOC","KOC",{"$f":"IF(ISNUMBER(D_Enk_KOC_syst_1),D_Enk_KOC_syst_1,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOC_1),Enk_My_KOC_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KOC_syst_2),D_Enk_KOC_syst_2,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOC_2),Enk_My_KOC_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KOC_syst_3),D_Enk_KOC_syst_3,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOC_3),Enk_My_KOC_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KOC_syst_4),D_Enk_KOC_syst_4,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KOC_4),Enk_My_KOC_4,\"\")","v":""}]
["Henrys konstant","KH",{"$f":"IF(ISNUMBER(D_Enk_KH_syst_1),D_Enk_KH_syst_1,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KH_1),Enk_My_KH_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KH_syst_2),D_Enk_KH_syst_2,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KH_2),Enk_My_KH_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KH_syst_3),D_Enk_KH_syst_3,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KH_3),Enk_My_KH_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Enk_KH_syst_4),D_Enk_KH_syst_4,\"\")","v":""},{"$f":"IF(ISNUMBER(Enk_My_KH_4),Enk_My_KH_4,\"\")","v":""}]
[]
["Maksimal ford. luft","fl",{"$f":"D_Enk_fl_1","v":""},null,{"$f":"D_Enk_fl_2","v":""},null,{"$f":"D_Enk_fl_3","v":""},null,{"$f":"D_Enk_fl_4","v":""}]
["Maksimal ford. vand","fv",{"$f":"D_Enk_fv_1","v":""},null,{"$f":"D_Enk_fv_2","v":""},null,{"$f":"D_Enk_fv_3","v":""},null,{"$f":"D_Enk_fv_4","v":""}]
["Maksimal ford. jord","fj",{"$f":"D_Enk_fj_1","v":""},null,{"$f":"D_Enk_fj_2","v":""},null,{"$f":"D_Enk_fj_3","v":""},null,{"$f":"D_Enk_fj_4","v":""}]
[]
["Mættede damptryk","CLmax",{"$f":"D_Enk_CLmax_1","v":""},null,{"$f":"D_Enk_CLmax_2","v":""},null,{"$f":"D_Enk_CLmax_3","v":""},null,{"$f":"D_Enk_CLmax_4","v":""},null,"mg/m³"]
[]
["Fugacitetsberegninger",null,"Angiv signifikant ciffer",null,3]
["Kommentar",{"$f":"IF(D_Enk_Fug_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Målt konc. i poreluft","CL",{"$f":"IF(Enk_My_CL_1>0,Enk_My_CL_1,\"\")","v":""},null,{"$f":"IF(Enk_My_CL_2>0,Enk_My_CL_2,\"\")","v":""},null,{"$f":"IF(Enk_My_CL_3>0,Enk_My_CL_3,\"\")","v":""},null,{"$f":"IF(Enk_My_CL_4>0,Enk_My_CL_4,\"\")","v":""},null,"mg/m³",null,{"$f":"C39*1000000","v":{"$error":"#VALUE!"}},{"$f":"E39*1000000","v":{"$error":"#VALUE!"}},{"$f":"G39*1000000","v":{"$error":"#VALUE!"}},{"$f":"I39*1000000","v":{"$error":"#VALUE!"}},"ng/m³"]
["Beregnet jordkonc.","Ct",{"$f":"IF(D_Enk_Ct_L_1>0,ROUND(D_Enk_Ct_L_1,enk_ciffer-(INT(LOG(D_Enk_Ct_L_1))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Ct_L_2>0,(ROUND(D_Enk_Ct_L_2,3-(INT(LOG(D_Enk_Ct_L_2))+1))),\"\")","v":""},null,{"$f":"IF(D_Enk_Ct_L_3>0,ROUND(D_Enk_Ct_L_3,enk_ciffer-(INT(LOG(D_Enk_Ct_L_3))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Ct_L_4>0,ROUND(D_Enk_Ct_L_4,enk_ciffer-(INT(LOG(D_Enk_Ct_L_4))+1)),\"\")","v":""},null,"mg/kg TS",null,{"$f":"C40*1000","v":{"$error":"#VALUE!"}},{"$f":"E40*1000","v":{"$error":"#VALUE!"}},{"$f":"G40*1000","v":{"$error":"#VALUE!"}},{"$f":"I40*1000","v":{"$error":"#VALUE!"}},"µg/kg TS"]
["Beregnet vandskonc.","CV",{"$f":"IF(D_Enk_Cv_L_1>0,ROUND(D_Enk_Cv_L_1,enk_ciffer-(INT(LOG(D_Enk_Cv_L_1))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cv_L_2>0,ROUND(D_Enk_Cv_L_2,3-(INT(LOG(D_Enk_Cv_L_2))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cv_L_3>0,ROUND(D_Enk_Cv_L_3,enk_ciffer-(INT(LOG(D_Enk_Cv_L_3))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cv_L_4>0,ROUND(D_Enk_Cv_L_4,enk_ciffer-(INT(LOG(D_Enk_Cv_L_4))+1)),\"\")","v":""},null,"mg/l",null,{"$f":"C41*1000000","v":{"$error":"#VALUE!"}},{"$f":"E41*1000000","v":{"$error":"#VALUE!"}},{"$f":"G41*1000000","v":{"$error":"#VALUE!"}},{"$f":"I41*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
[]
["Målt konc. i grundvand","CV",{"$f":"IF(ISNUMBER(Enk_My_CV_1),Enk_My_CV_1,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_CV_2),Enk_My_CV_2,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_CV_3),Enk_My_CV_3,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_CV_4),Enk_My_CV_4,\"\")","v":""},null,"mg/l",null,{"$f":"C43*1000000","v":{"$error":"#VALUE!"}},{"$f":"E43*1000000","v":{"$error":"#VALUE!"}},{"$f":"G43*1000000","v":{"$error":"#VALUE!"}},{"$f":"I43*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
["Beregnet poreluftskonc.","CL",{"$f":"IF(D_Enk_Cl_V_1>0,(ROUND(D_Enk_Cl_V_1,enk_ciffer-(INT(LOG(D_Enk_Cl_V_1))+1))),\"\")","v":""},null,{"$f":"IF(D_Enk_Cl_V_2>0,(ROUND(D_Enk_Cl_V_2,enk_ciffer-(INT(LOG(D_Enk_Cl_V_2))+1))),\"\")","v":""},null,{"$f":"IF(D_Enk_Cl_V_3>0,(ROUND(D_Enk_Cl_V_3,enk_ciffer-(INT(LOG(D_Enk_Cl_V_3))+1))),\"\")","v":""},null,{"$f":"IF(D_Enk_Cl_V_4>0,(ROUND(D_Enk_Cl_V_4,enk_ciffer-(INT(LOG(D_Enk_Cl_V_4))+1))),\"\")","v":""},null,"mg/m³",null,{"$f":"C44*1000000","v":{"$error":"#VALUE!"}},{"$f":"E44*1000000","v":{"$error":"#VALUE!"}},{"$f":"G44*1000000","v":{"$error":"#VALUE!"}},{"$f":"I44*1000000","v":{"$error":"#VALUE!"}},"ng/m³"]
["Beregnet jordkonc.","Ct",{"$f":"IF(D_Enk_Ct_V_1>0,ROUND(D_Enk_Ct_V_1,enk_ciffer-(INT(LOG(D_Enk_Ct_V_1))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Ct_V_2>0,ROUND(D_Enk_Ct_V_2,enk_ciffer-(INT(LOG(D_Enk_Ct_V_2))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Ct_V_3>0,ROUND(D_Enk_Ct_V_3,enk_ciffer-(INT(LOG(D_Enk_Ct_V_3))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Ct_V_4>0,ROUND(D_Enk_Ct_V_4,enk_ciffer-(INT(LOG(D_Enk_Ct_V_4))+1)),\"\")","v":""},null,"mg/kg TS",null,{"$f":"C45*1000","v":{"$error":"#VALUE!"}},{"$f":"E45*1000","v":{"$error":"#VALUE!"}},{"$f":"G45*1000","v":{"$error":"#VALUE!"}},{"$f":"I45*1000","v":{"$error":"#VALUE!"}},"µg/kg TS"]
[]
["Målt konc. i jorden","Ct",{"$f":"IF(ISNUMBER(Enk_My_Ct_1),Enk_My_Ct_1,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_Ct_2),Enk_My_Ct_2,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_Ct_3),Enk_My_Ct_3,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Enk_My_Ct_4),Enk_My_Ct_4,\"\")","v":""},null,"mg/kg TS",null,{"$f":"C47*1000","v":{"$error":"#VALUE!"}},{"$f":"E47*1000","v":{"$error":"#VALUE!"}},{"$f":"G47*1000","v":{"$error":"#VALUE!"}},{"$f":"I47*1000","v":{"$error":"#VALUE!"}},"µg/kg TS"]
["Beregnet poreluftskonc.","CL",{"$f":"IF(D_Enk_Cl_J_1>0,ROUND(D_Enk_Cl_J_1,enk_ciffer-(INT(LOG(D_Enk_Cl_J_1))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cl_J_2>0,ROUND(D_Enk_Cl_J_2,enk_ciffer-(INT(LOG(D_Enk_Cl_J_2))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cl_J_3>0,ROUND(D_Enk_Cl_J_3,enk_ciffer-(INT(LOG(D_Enk_Cl_J_3))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cl_J_4>0,ROUND(D_Enk_Cl_J_4,enk_ciffer-(INT(LOG(D_Enk_Cl_J_4))+1)),\"\")","v":""},null,"mg/m³",null,{"$f":"C48*1000000","v":{"$error":"#VALUE!"}},{"$f":"E48*1000000","v":{"$error":"#VALUE!"}},{"$f":"G48*1000000","v":{"$error":"#VALUE!"}},{"$f":"I48*1000000","v":{"$error":"#VALUE!"}},"ng/m³"]
["Beregnet vandskonc.","CV",{"$f":"IF(D_Enk_Cv_J_1>0,ROUND(D_Enk_Cv_J_1,enk_ciffer-(INT(LOG(D_Enk_Cv_J_1))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cv_J_2>0,ROUND(D_Enk_Cv_J_2,enk_ciffer-(INT(LOG(D_Enk_Cv_J_2))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cv_J_3>0,ROUND(D_Enk_Cv_J_3,enk_ciffer-(INT(LOG(D_Enk_Cv_J_3))+1)),\"\")","v":""},null,{"$f":"IF(D_Enk_Cv_J_4>0,ROUND(D_Enk_Cv_J_4,enk_ciffer-(INT(LOG(D_Enk_Cv_J_4))+1)),\"\")","v":""},null,"mg/l",null,{"$f":"C49*1000000","v":{"$error":"#VALUE!"}},{"$f":"E49*1000000","v":{"$error":"#VALUE!"}},{"$f":"G49*1000000","v":{"$error":"#VALUE!"}},{"$f":"I49*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
[]
["Risiko for fri fase?",null,{"$f":"D_Enk_FF_1","v":"nej"},null,{"$f":"D_Enk_FF_2","v":"nej"},null,{"$f":"D_Enk_FF_3","v":"nej"},null,{"$f":"D_Enk_FF_4","v":"nej"}]
[]
["Anvendt Brugerdata?",null,{"$f":"D_Enk_Brugerdata_1","v":"Nej"},null,{"$f":"D_Enk_Brugerdata_2","v":"Nej"},null,{"$f":"D_Enk_Brugerdata_3","v":"Nej"},null,{"$f":"D_Enk_Brugerdata_4","v":"Nej"}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler."]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Jord_Com <> \"\", D_Enk_Jord_Com, \"\")","v":""}]
["om jordtype"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Kem_Com <> \"\", D_Enk_Kem_Com, \"\")","v":""}]
["om kemiske data"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Fug_Com<>\"\",D_Enk_Fug_Com,\"\")","v":""}]
["om fugacitet"]

{"sheet":"Vejledning_Enkeltstoffer","index":9,"n_rows":104,"n_cols":2,"rows_kept":104,"cut":false,"hidden":true,"merged":[[1,1,1,15],[5,1,5,15],[6,1,8,15],[9,1,28,15],[29,1,29,15],[92,1,93,15],[96,1,100,15],[103,1,103,15],[2,1,4,15],[30,1,30,15],[31,1,35,15],[36,1,36,15],[45,1,51,15],[52,1,55,15],[37,1,43,15],[44,1,44,15],[57,1,59,14],[62,1,63,15],[65,1,73,15],[76,1,86,15],[88,1,89,15]]}
[null,"Vejledning  - Enkeltstoffer"]
[null,"Formål"]
[null,"I dette ark defineres de forureningsdata, som skal anvendes i beregningerne, ved at indtaste oplysninger om målte data og undersøgelsesforhold."]
[]
[]
[null,"FUGACITETSBEREGNINGER"]
[null,"Såfremt der indtastes data om jordarten, hvorfra prøverne er udtaget, beregnes fasefordelingen i de andre medier (fugacitetsberegninger) iht. de målte data. Nærmere detaljer om beregningerne er beskrevet i Miljøstyrelsens vejledninger nr. 6 og 7 fra 1998."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Jordtype:"]
[null,"Man kan vælge en standardjordtype fra listen eller oprette eller hente egenskaber fra egen liste ved at markere den ønskede jordtype.\n\nDet er også muligt at anvende og oprette egne \"jordtyper\" ved at klikke på knappen \"Egen liste\""]
[]
[]
[]
[]
[null,"Kemiske data:"]
[null,"Der kan indtastes data for op til fire målepunkter. Disse kan være data for fire forskellige stoffer eller for forskellige koncentrationer i forskellige medier eller målepunkter. Man kan vælge op til fire stoffer fra standardlisten eller oprette eller hente stofegenskaber fra egen liste. \n\nVed at klikke på Vis detailoplysninger vises de anvendte fysisk-kemiske egenskaber, og der kan indtastes andre (egne) værdier."]
[]
[]
[]
[]
[]
[]
[null,"Valg af modul for risikoberegning:"]
[null,"Efter indtastning af målte værdier vælges det ønskede risikovurderingsmodul:\n     \n    Vertikal transport (umættet zone) til det først betydende grundvandsmagasin\n    Grundvand (transport i det først betydende grundvandsmagasin)\n    Udeluft\n    Indeklima"]
[]
[]
[]
[]
[]
[]
[null,"Ved beregninger for vertikal transport, grundvand, udeluft eller indeklima overføres enten de målte data eller, såfremt der ikke foreligger målte data for de relevante medier (luft, vand), de beregnede koncentrationer iht. fugacitetsberegninger. "]
[]
[]
[]
[null,"Generelt"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTVÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Grundvand","index":10,"n_rows":228,"n_cols":37,"rows_kept":228,"cut":false,"hidden":true,"merged":[[11,4,11,5],[247,7,247,32],[247,4,247,5],[11,7,11,32],[109,7,109,11],[109,13,109,17],[109,19,109,23],[109,25,109,29],[63,7,63,11],[63,13,63,17],[63,19,63,23],[63,25,63,29],[83,7,83,11],[83,13,83,17],[83,19,83,23],[83,25,83,29],[68,7,68,11],[68,13,68,17],[68,19,68,23],[68,25,68,29],[70,7,70,11],[70,13,70,17],[85,19,85,23],[85,25,85,29],[87,7,87,11],[87,13,87,17],[89,25,89,29],[70,19,70,23],[42,25,42,26],[42,28,42,29],[40,34,42,35],[42,31,42,32],[101,7,101,11],[101,13,101,17],[101,19,101,23],[101,25,101,29],[79,7,79,11],[79,13,79,17],[77,7,77,11],[77,13,77,17],[91,7,91,11],[91,13,91,17],[98,7,99,11],[98,13,99,17],[87,25,87,29],[89,19,89,23],[85,7,85,11],[85,13,85,17],[77,19,77,23],[77,25,77,29],[44,25,44,26],[44,28,44,29],[38,31,38,32],[38,25,38,26],[38,34,38,35],[41,19,41,20],[41,22,41,23],[41,25,41,26],[39,31,39,32],[39,25,39,26],[39,19,39,20],[40,19,40,20],[39,34,39,35],[41,28,41,29],[44,31,44,32],[44,34,44,35],[43,19,43,20],[43,22,43,23],[43,25,43,26],[107,7,107,11],[107,13,107,17],[107,19,107,23],[107,25,107,29],[43,31,43,32],[43,28,43,29],[59,7,59,11],[59,13,59,17],[57,7,57,11],[74,13,74,17],[79,19,79,23],[79,25,79,29],[91,19,91,23],[91,25,91,29],[98,19,99,23],[98,25,99,29],[94,5,94,29],[89,7,89,11],[89,13,89,17],[87,19,87,23],[45,19,45,20],[45,22,45,23],[45,25,45,26],[45,28,45,29],[122,19,122,23],[122,25,122,29],[45,34,45,35],[57,25,57,29],[43,34,43,35],[44,19,44,20],[44,22,44,23],[120,7,120,11],[118,7,118,11],[111,7,111,11],[116,7,116,11],[120,13,120,17],[120,19,120,23],[120,25,120,29],[118,13,118,17],[118,19,118,23],[118,25,118,29],[111,13,111,17],[111,19,111,23],[111,25,111,29],[116,13,116,17],[116,19,116,23],[116,25,116,29],[122,7,122,11],[122,13,122,17],[113,7,113,11],[113,13,113,17],[113,19,113,23],[113,25,113,29],[45,31,45,32],[60,25,60,29],[59,19,59,23],[59,25,59,29],[74,19,74,23],[74,25,74,29],[53,5,54,29],[60,7,60,11],[60,13,60,17],[60,19,60,23],[70,25,70,29],[72,7,72,11],[72,13,72,17],[72,19,72,23],[72,25,72,29],[74,7,74,11],[57,13,57,17],[57,19,57,23],[105,7,105,11],[139,28,139,29],[134,25,134,26],[135,25,135,26],[136,25,136,26],[124,25,124,29],[132,28,132,29],[136,10,136,11],[137,10,137,11],[138,10,138,11],[134,28,134,29],[135,28,135,29],[136,28,136,29],[137,28,137,29],[138,28,138,29],[135,10,135,11],[124,19,124,23],[132,22,132,23],[132,19,132,20],[132,25,132,26],[139,19,139,20],[139,22,139,23],[138,22,138,23],[137,22,137,23],[138,4,138,5],[135,7,135,8],[139,4,139,5],[134,4,134,5],[135,4,135,5],[136,4,136,5],[137,4,137,5],[137,25,137,26],[138,25,138,26],[139,25,139,26],[136,22,136,23],[135,22,135,23],[134,22,134,23],[139,13,139,14],[138,7,138,8],[136,7,136,8],[137,7,137,8],[139,7,139,8],[137,19,137,20],[138,19,138,20],[134,19,134,20],[135,19,135,20],[136,19,136,20],[134,10,134,11],[124,0,125,4],[130,7,130,17],[132,7,132,8],[132,13,132,14],[132,4,132,5],[124,7,124,11],[124,13,124,17],[132,10,132,11],[132,16,132,17],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[12,7,12,29],[13,6,16,17],[13,20,16,29],[40,25,40,26],[39,28,39,29],[40,28,40,29],[38,19,38,20],[38,22,38,23],[38,28,38,29],[7,19,7,23],[19,10,19,11],[21,10,21,11],[25,10,25,11],[25,7,25,8],[9,7,9,11],[9,13,9,17],[9,19,9,23],[9,25,9,29],[21,28,21,29],[46,0,47,4],[49,0,50,4],[44,7,44,8],[47,7,47,8],[50,7,50,8],[27,7,27,11],[39,22,39,23],[40,22,40,23],[38,10,38,11],[40,7,41,11],[39,16,39,17],[38,16,38,18],[38,13,38,15],[40,16,40,17],[41,16,41,17],[42,16,42,17],[39,13,39,14],[28,7,28,11],[32,7,32,10],[42,7,42,11],[42,19,42,20],[42,22,42,23],[42,13,42,14],[159,7,159,17],[134,7,134,8],[139,10,139,11],[134,16,134,17],[135,16,135,17],[136,16,136,17],[137,16,137,17],[138,16,138,17],[139,16,139,17],[134,13,134,14],[135,13,135,14],[136,13,136,14],[137,13,137,14],[138,13,138,14],[161,4,161,5],[161,7,161,8],[161,10,161,11],[161,13,161,14],[161,16,161,17],[161,19,161,20],[161,22,161,23],[161,25,161,26],[161,28,161,29],[163,4,163,5],[163,7,163,8],[163,10,163,11],[163,13,163,14],[163,16,163,17],[163,19,163,20],[163,22,163,23],[163,25,163,26],[163,28,163,29],[164,4,164,5],[164,7,164,8],[164,10,164,11],[164,13,164,14],[164,16,164,17],[164,19,164,20],[164,22,164,23],[164,25,164,26],[164,28,164,29],[165,4,165,5],[165,7,165,8],[165,10,165,11],[165,13,165,14],[165,16,165,17],[165,19,165,20],[165,22,165,23],[165,25,165,26],[165,28,165,29],[166,4,166,5],[166,7,166,8],[166,10,166,11],[166,13,166,14],[166,16,166,17],[166,19,166,20],[166,22,166,23],[166,25,166,26],[166,28,166,29],[167,4,167,5],[167,7,167,8],[167,10,167,11],[167,13,167,14],[167,16,167,17],[167,19,167,20],[167,22,167,23],[167,25,167,26],[167,28,167,29],[168,4,168,5],[168,7,168,8],[168,10,168,11],[168,13,168,14],[168,16,168,17],[168,19,168,20],[168,22,168,23],[168,25,168,26],[168,28,168,29],[188,7,188,17],[190,4,190,5],[190,7,190,8],[190,10,190,11],[190,13,190,14],[190,16,190,17],[190,19,190,20],[190,22,190,23],[190,25,190,26],[190,28,190,29],[192,4,192,5],[192,7,192,8],[192,10,192,11],[192,13,192,14],[192,16,192,17],[192,19,192,20],[192,22,192,23],[192,25,192,26],[192,28,192,29],[193,4,193,5],[193,7,193,8],[193,10,193,11],[193,13,193,14],[193,16,193,17],[193,19,193,20],[193,22,193,23],[193,25,193,26],[193,28,193,29],[194,4,194,5],[194,7,194,8],[194,10,194,11],[194,13,194,14],[194,16,194,17],[194,19,194,20],[194,22,194,23],[194,25,194,26],[194,28,194,29],[195,4,195,5],[195,7,195,8],[195,10,195,11],[195,13,195,14],[195,16,195,17],[195,19,195,20],[195,22,195,23],[195,25,195,26],[195,28,195,29],[196,4,196,5],[196,7,196,8],[196,10,196,11],[196,13,196,14],[196,16,196,17],[196,19,196,20],[196,22,196,23],[196,25,196,26],[196,28,196,29],[197,4,197,5],[197,7,197,8],[197,10,197,11],[197,13,197,14],[197,16,197,17],[197,19,197,20],[197,22,197,23],[197,25,197,26],[197,28,197,29],[218,7,218,17],[220,4,220,5],[220,7,220,8],[220,10,220,11],[220,13,220,14],[220,16,220,17],[220,19,220,20],[220,22,220,23],[220,25,220,26],[220,28,220,29],[222,4,222,5],[222,7,222,8],[222,10,222,11],[222,13,222,14],[222,16,222,17],[222,19,222,20],[222,22,222,23],[222,25,222,26],[222,28,222,29],[223,4,223,5],[223,7,223,8],[223,10,223,11],[223,13,223,14],[223,16,223,17],[223,19,223,20],[223,22,223,23],[223,25,223,26],[223,28,223,29],[224,4,224,5],[224,7,224,8],[224,10,224,11],[224,13,224,14],[224,16,224,17],[224,19,224,20],[224,22,224,23],[224,25,224,26],[224,28,224,29],[226,28,226,29],[225,4,225,5],[225,7,225,8],[225,10,225,11],[225,13,225,14],[225,16,225,17],[225,19,225,20],[225,22,225,23],[225,25,225,26],[225,28,225,29],[105,13,105,17],[105,19,105,23],[105,25,105,29],[103,7,103,11],[103,13,103,17],[103,19,103,23],[103,25,103,29],[227,4,227,5],[227,7,227,8],[227,10,227,11],[227,13,227,14],[227,16,227,17],[227,19,227,20],[227,22,227,23],[227,25,227,26],[227,28,227,29],[226,4,226,5],[226,7,226,8],[226,10,226,11],[226,13,226,14],[226,16,226,17],[226,19,226,20],[226,22,226,23],[226,25,226,26]]}
["Grundvandskoncentrationen i det første betydende magasin"]
["Lokaliteten"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
["Beregning udføres for :",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
[]
["Det forurenede område",null,null,null,null,null,null,"Der skal vælges mellem to beregningstyper:"]
[null,null,null,null,null,null,"A - Beregnet koncentration - ud fra en målt konc. \ni kilden (porevand, terrænnært grundvand)\n[Data overføres fra modulet Enkeltstoffer eller\n Vertikal transport]",null,null,null,null,null,null,null,null,null,null,null,null,null,"B - Målt koncentration i toppen af første betydende magasin\n[Data overføres fra modulet Enkeltstoffer]"]
[]
[]
[]
[]
[]
["Længde af kildeområde",null,null,null,null,"Y",null,null,null,null,null,null,"m",null,{"$f":"IF(ISTEXT(Gru_Y),\"Tjek decimal\",\"\")","v":""}]
[]
["Bredde af kildeområde",null,null,null,null,"X",null,null,null,null,null,null,"m",null,{"$f":"IF(ISTEXT(Gru_X),\"Tjek decimal\",\"\")","v":""},null,null,null,null,null,"Areal af det forurenede område ",null,null,null,null,null,null,null,{"$f":"D_Gru_A","v":""},null,null,"m2"]
[]
[]
[]
["Nettonedbør",null,null,null,null,"N",null,{"$f":"IF(D_Gru_N_syst<>\"\",D_Gru_N_syst,\"\")","v":""},null,null,null,null,"mm/år"]
[]
["Kommune/Egn",null,null,null,null,null,null,{"$f":"IF(D_Gru_Kommune_syst<>\"\",D_Gru_Kommune_syst,\"\")","v":""}]
[]
[]
[null,null,null,null,null,null,"Angiv filterlængde"]
[]
[null,null,null,"Filterlængde",null,null,"l",null,null,null,null,"m",null,{"$f":"IF(ISTEXT(Gru_FilterL),\"Tjek decimal\",\"\")","v":""}]
[]
[]
[]
["Det første betydende magasin",null,null,null,null,null,null,null,"Indtast data for det første betydende magasin, hvori risiko skal beregnes"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Hydraulisk gradient\n(m/m)",null,null,"Hydraulisk lednings-\nevne",null,null,"Effektiv porøsitet",null,null,"Vand-mættede porøsitet",null,null,"Bulk-masse-fylde\n(kg/l)",null,null,"% indhold organisk kulstof",null,null,"Tykkelse af magasin\n(m)",null,null,"Opblandings-dybde\n(m)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"i",null,null,"k",null,null,"eff.",null,null,"ew",null,null,"r",null,null,"foc",null,null,"maxdm",null,null,"dm"]
[null,null,null,null,null,null,null,{"$f":"IF(D_Gru_Aqui_syst<>\"\",D_Gru_Aqui_syst,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_Gru_trin1a_k_int<>\"\",D_Gru_trin1a_k_int,\"\")","v":""},null,null,{"$f":"IF(D_Gru_trin2a_eeff_int<>\"\",D_Gru_trin2a_eeff_int,\"\")","v":""},null,null,{"$f":"IF(D_Gru_trin3_eW_int<>\"\",D_Gru_trin3_eW_int,\"\")","v":""},null,null,{"$f":"IF(D_Gru_rhob_int<>\"\",D_Gru_rhob_int,\"\")","v":""},null,null,{"$f":"IF(D_Gru_foc_int<>\"\",D_Gru_foc_int,\"\")","v":""},null,null,null,null,null,{"$f":"D_Gru_trin2a_dm_2a","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Gru_trin1a_k_syst<>\"\",D_Gru_trin1a_k_syst,\"\")","v":""},null,null,{"$f":"IF(D_Gru_trin2a_eeff_syst<>\"\",D_Gru_trin2a_eeff_syst,\"\")","v":""},null,null,{"$f":"IF(D_Gru_trin3_eW_syst<>\"\",D_Gru_trin3_eW_syst,\"\")","v":""},null,null,{"$f":"IF(D_Gru_rhob_syst<>\"\",D_Gru_rhob_syst,\"\")","v":""},null,null,{"$f":"IF(D_Gru_foc_syst<>\"\",D_Gru_foc_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Gru_i),\"Tjek decimal\",IF(ISTEXT(Gru_My_k),\"Tjek decimal\",IF(ISTEXT(Gru_My_eff),\"Tjek decimal\",IF(ISTEXT(Gru_My_ew),\"Tjek decimal\",IF(ISTEXT(Gru_My_p),\"Tjek decimal\",IF(ISTEXT(Gru_My_foc),\"Tjek decimal\",IF(ISTEXT(Gru_maxdm),\"Tjek decimal\",\"\")))))))","v":""}]
[]
["Gns. porevandhastighed",null,null,null,null,"Vp",null,{"$f":"D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},null,null,"m/år"]
[]
["Afstand til teoretisk beregningspunkt"]
[null,null,null,null,null,"L",null,{"$f":"D_Gru_trin1b_LL","v":{"$error":"#VALUE!"}},null,null,"m"]
[]
["Transporttid til teoretisk \nberegningspunkt"]
[null,null,null,null,null,"ttid",null,{"$f":"D_Gru_trin2a_t","v":{"$error":"#VALUE!"}},null,null,"år"]
[]
[]
["Forurening",null,null,null,null,"Data for forureningen er overført fra fugacitetsmodulet eller et af modulerne for umættet zone\nIndtast eventuel baggrundskoncentration. "]
[]
[]
[]
["Stofnavn (fra enkeltstoffer)",null,null,null,null,null,null,{"$f":"D_Gru_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Gru_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Gru_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Gru_stofnavn_4","v":""}]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
[]
["Forureningsdata: Trin 1a"]
["Baggrundskoncentration",null,null,null,null,"Cg",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l",null,null,{"$f":"IF(ISTEXT(Gru_Trin1a_my_Cg_1),\"Tjek decimal\",IF(ISTEXT(Gru_Trin1a_my_Cg_2),\"Tjek decimal\",IF(ISTEXT(Gru_Trin1a_my_Cg_3),\"Tjek decimal\",IF(ISTEXT(Gru_Trin1a_my_Cg_4),\"Tjek decimal\",\"\"))))","v":""}]
[]
[]
["Kildestyrkekoncentration",null,null,null,null,"C0",null,"Vælg kildestyrkekoncentrationen for beregningen"]
[]
[null,null,null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp1_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp1_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp1_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp1_4","v":""},null,null,null,null,null,"mg/l"]
[]
[null,null,null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp2_1","v":false},null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp2_2","v":false},null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp2_3","v":false},null,null,null,null,null,{"$f":"D_Gru_trin1a_C0_temp2_4","v":false},null,null,null,null,null,"mg/l",{"$f":"IF(D_Gru_trin1a_temp2_TrueFalse,D_ver_model,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,1,null,null,null,null,null,2,null,null,null,null,null,3,null,null,null,null,null,4,null,null,null,null,null,"mg/l"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l",null,null,{"$f":"IF(ISTEXT(Gru_Trin1a_my_C0_1),\"Tjek decimal\",IF(ISTEXT(Gru_Trin1a_my_C0_2),\"Tjek decimal\",IF(ISTEXT(Gru_Trin1a_my_C0_3),\"Tjek decimal\",IF(ISTEXT(Gru_Trin1a_my_C0_4),\"Tjek decimal\",\"\"))))","v":""}]
[]
["Forureningsdata:Trin 1b"]
["Målt koncentration (fra enkeltstoffer)",null,null,null,null,"C1",null,{"$f":"D_Enk_CV_1","v":0},null,null,null,null,null,{"$f":"D_Enk_CV_2","v":0},null,null,null,null,null,{"$f":"D_Enk_CV_3","v":0},null,null,null,null,null,{"$f":"D_Enk_CV_4","v":0},null,null,null,null,null,"mg/l"]
[]
["Test af andre værdier",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l"]
[]
["Beregning: Grundvand"]
[]
["Grundvandskvalitetskriterie",null,null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_4","v":""},null,null,null,null,null,"mg/l"]
[]
["Grundvandskoncentration: Trin 1",null,null,null,null,"C1",null,{"$f":"D_gru_trin1_GVkonc_1","v":""},null,null,null,null,null,{"$f":"D_gru_trin1_GVkonc_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1_GVkonc_3","v":""},null,null,null,null,null,{"$f":"D_gru_trin1_GVKonc_4","v":""},null,null,null,null,null,"mg/l"]
[]
["Overskridelse af kriteriet Trin 1",null,null,null,null,null,null,{"$f":"D_Gru_trin1_oversk_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1_oversk_2","v":""},null,null,null,null,null,{"$f":"D_gru_trin1_oversk_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1_oversk_4","v":""},null,null,null,null,null,"gange"]
[]
["Grundvandskoncentration: Trin 2",null,null,null,null,"C2",null,{"$f":"D_Gru_Trin2_GVKonc_1","v":""},null,null,null,null,null,{"$f":"D_Gru_Trin2_GVKonc_2","v":""},null,null,null,null,null,{"$f":"D_Gru_Trin2_GVKonc_3","v":""},null,null,null,null,null,{"$f":"D_Gru_Trin2_GVKonc_4","v":""},null,null,null,null,null,"mg/l"]
[]
["Overskridelse af kriteriet Trin 2",null,null,null,null,null,null,{"$f":"D_gru_trin2_overskr_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin2_overskr_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin2_overskr_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin2_overskr_4","v":""},null,null,null,null,null,"gange"]
[]
["Trin 3  inclusiv sorption og nedbryding"]
[null,null,null,null,null,"Angiv om der er tale om aerobe eller anaerobe nedbrydningsforhold"]
["Nedbrydningsforhold"]
[]
[]
[null,null,null,null,null,null,null,{"$f":"D_Gru_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Gru_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Gru_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Gru_stofnavn_4","v":""}]
["Stofnavn (fra enkeltstoffer)"]
[]
["Fordelingskoefficient",null,null,null,null,"Log KD",null,{"$f":"D_Gru_trin3_logKD_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_logKD_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_logKD_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_logKD_4","v":""}]
[]
["Anvendt nedbrydningskonstant",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Gru_trin3_k1_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Gru_trin3_k1_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Gru_trin3_k1_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Gru_trin3_k1_4,\"\")","v":""},null,null,null,null,null,"dage-1"]
[]
["GV-Konc. m. nedbr.: Trin 3",null,null,null,null,null,null,{"$f":"D_Gru_trin3_ned_C3_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_ned_C3_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_ned_C3_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_ned_C3_4","v":""},null,null,null,null,null,"mg/l"]
[]
["GV-Konc. m. sorpt. og nedbr.: Trin 3",null,null,null,null,"C3",null,{"$f":"D_Gru_trin3_C3_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_C3_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_C3_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_C3_4","v":""},null,null,null,null,null,"mg/l"]
[]
["Grundvandskvalitetskriterie",null,null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin1a_Krit_4","v":""},null,null,null,null,null,"mg/l"]
[]
["Overskridelse af kriteriet Trin 3",null,null,null,null,null,null,{"$f":"D_Gru_trin3_Krit_Overskr_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_Krit_Overskr_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_Krit_Overskr_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_Krit_Overskr_4","v":""},null,null,null,null,null,"gange"]
[]
["Anvendt brugerdata",null,null,null,null,null,null,{"$f":"D_GRU_brugerdata_1","v":""},null,null,null,null,null,{"$f":"D_GRU_brugerdata_2","v":""},null,null,null,null,null,{"$f":"D_GRU_brugerdata_3","v":""},null,null,null,null,null,{"$f":"D_GRU_brugerdata_4","v":""}]
[]
[]
["Log Kow (oktanol/vand)",null,null,null,null,"Log Kow",null,{"$f":"D_Gru_trin3_logKOW_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_logKOW_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_logKOW_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_logKOW_4","v":""}]
[]
["Forureningsflux vertikalt (Trin 1a)",null,null,null,null,"Jo",null,{"$f":"D_gru_trin3_fluxvert_1","v":""},null,null,null,null,null,{"$f":"D_gru_trin3_fluxvert_2","v":""},null,null,null,null,null,{"$f":"D_gru_trin3_fluxvert_3","v":""},null,null,null,null,null,{"$f":"D_Gru_Trin3_fluxvert_4","v":""},null,null,null,null,null,"g/år"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
["Retardationskoefficient",null,null,null,null,"R",null,{"$f":"D_Gru_trin3_R_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_R_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_R_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_R_4","v":""}]
[]
["Forureningshastighed",null,null,null,null,"Vs",null,{"$f":"D_Gru_trin3_VS_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_VS_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_VS_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_VS_4","v":""},null,null,null,null,null,"m/år"]
[]
["Transporttid med sorption\ntil teoretisk beregn.pkt.",null,null,null,null,null,null,{"$f":"D_Gru_trin3_t_sorp_1","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_t_sorp_2","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_t_sorp_3","v":""},null,null,null,null,null,{"$f":"D_Gru_trin3_t_sorp_4","v":""},null,null,null,null,null,"dage"]
[]
[]
[null,null,null,null,null,"Vælg stoftabel for afstandsdata"]
[]
[]
["Data for stof 1",null,null,null,null,null,null,{"$f":"D_Gru_stofnavn_1","v":""}]
[]
["Afstand",null,null,null,null,null,null,{"$f":"D_Gru_stof1_Afstand_1_2","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_1_3","v":10},null,null,{"$f":"D_Gru_stof1_Afstand_1_4","v":20},null,null,{"$f":"D_Gru_stof1_Afstand_1_5","v":30},null,null,{"$f":"D_Gru_stof1_Afstand_1_6","v":40},null,null,{"$f":"D_Gru_stof1_Afstand_1_7","v":50},null,null,{"$f":"D_Gru_stof1_Afstand_1_8","v":75},null,null,{"$f":"D_Gru_stof1_Afstand_1_9","v":100},null,null,"m"]
[]
["Transporttid",null,null,null,{"$f":"D_Gru_stof1_Afstand_2_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_2_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Opblandingsdybde",null,null,null,{"$f":"D_Gru_stof1_Afstand_3_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_3_9","v":{"$error":"#VALUE!"}},null,null,"m"]
["Forureningskoncentration, C2",null,null,null,{"$f":"D_Gru_stof1_Afstand_4_1","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_2","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_3","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_4","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_5","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_6","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_7","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_8","v":0},null,null,{"$f":"D_Gru_stof1_Afstand_4_9","v":0},null,null,"mg/l"]
["Konc. med nedbrydning, C3",null,null,null,{"$f":"D_Gru_stof1_Afstand_5_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_5_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
["Transporttid (sorpt.)",null,null,null,{"$f":"D_Gru_stof1_Afstand_6_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_6_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Konc. m. sorpt. og nedbr.,C3",null,null,null,{"$f":"D_Gru_stof1_Afstand_7_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof1_Afstand_7_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Data for stof 2",null,null,null,null,null,null,{"$f":"D_Gru_stofnavn_2","v":""}]
[]
["Afstand",null,null,null,null,null,null,{"$f":"D_Gru_stof2_Afstand_1_2","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_1_3","v":10},null,null,{"$f":"D_Gru_stof2_Afstand_1_4","v":20},null,null,{"$f":"D_Gru_stof2_Afstand_1_5","v":30},null,null,{"$f":"D_Gru_stof2_Afstand_1_6","v":40},null,null,{"$f":"D_Gru_stof2_Afstand_1_7","v":50},null,null,{"$f":"D_Gru_stof2_Afstand_1_8","v":75},null,null,{"$f":"D_Gru_stof2_Afstand_1_9","v":100},null,null,"m"]
[]
["Transporttid",null,null,null,{"$f":"D_Gru_stof2_Afstand_2_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_2_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Opblandingsdybde, m",null,null,null,{"$f":"D_Gru_stof2_Afstand_3_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_3_9","v":{"$error":"#VALUE!"}},null,null,"m"]
["Forureningskoncentration C2",null,null,null,{"$f":"D_Gru_stof2_Afstand_4_1","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_2","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_3","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_4","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_5","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_6","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_7","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_8","v":0},null,null,{"$f":"D_Gru_stof2_Afstand_4_9","v":0},null,null,"mg/l"]
["Konc. med nedbrydning C3",null,null,null,{"$f":"D_Gru_stof2_Afstand_5_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_5_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
["Transporttid (sorpt.)",null,null,null,{"$f":"D_Gru_stof2_Afstand_6_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_6_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Konc. m. sorpt. og nedbr. C3",null,null,null,{"$f":"D_Gru_stof2_Afstand_7_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof2_Afstand_7_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Data for stof 3",null,null,null,null,null,null,{"$f":"D_Gru_stofnavn_3","v":""}]
[]
["Afstand",null,null,null,null,null,null,{"$f":"D_Gru_stof3_Afstand_1_2","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_1_3","v":10},null,null,{"$f":"D_Gru_stof3_Afstand_1_4","v":20},null,null,{"$f":"D_Gru_stof3_Afstand_1_5","v":30},null,null,{"$f":"D_Gru_stof3_Afstand_1_6","v":40},null,null,{"$f":"D_Gru_stof3_Afstand_1_7","v":50},null,null,{"$f":"D_Gru_stof3_Afstand_1_8","v":75},null,null,{"$f":"D_Gru_stof3_Afstand_1_9","v":100},null,null,"m"]
[]
["Transporttid",null,null,null,{"$f":"D_Gru_stof3_Afstand_2_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_2_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Opblandingsdybde, m",null,null,null,{"$f":"D_Gru_stof3_Afstand_3_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_3_9","v":{"$error":"#VALUE!"}},null,null,"m"]
["Forureningskoncentration C2",null,null,null,{"$f":"D_Gru_stof3_Afstand_4_1","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_2","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_3","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_4","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_5","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_6","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_7","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_8","v":0},null,null,{"$f":"D_Gru_stof3_Afstand_4_9","v":0},null,null,"mg/l"]
["Konc. med nedbrydning C3",null,null,null,{"$f":"D_Gru_stof3_Afstand_5_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_5_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
["Transporttid (sorpt.)",null,null,null,{"$f":"D_Gru_stof3_Afstand_6_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_6_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Konc. m. sorpt. og nedbr. C3",null,null,null,{"$f":"D_Gru_stof3_Afstand_7_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof3_Afstand_7_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Data for stof 4",null,null,null,null,null,null,{"$f":"D_Gru_stofnavn_4","v":""}]
[]
["Afstand",null,null,null,null,null,null,{"$f":"D_Gru_stof4_Afstand_1_2","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_1_3","v":10},null,null,{"$f":"D_Gru_stof4_Afstand_1_4","v":20},null,null,{"$f":"D_Gru_stof4_Afstand_1_5","v":30},null,null,{"$f":"D_Gru_stof4_Afstand_1_6","v":40},null,null,{"$f":"D_Gru_stof4_Afstand_1_7","v":50},null,null,{"$f":"D_Gru_stof4_Afstand_1_8","v":75},null,null,{"$f":"D_Gru_stof4_Afstand_1_9","v":100},null,null,"m"]
[]
["Transporttid",null,null,null,{"$f":"D_Gru_stof4_Afstand_2_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_2_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Opblandingsdybde, m",null,null,null,{"$f":"D_Gru_stof4_Afstand_3_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_3_9","v":{"$error":"#VALUE!"}},null,null,"m"]
["Forureningskoncentration C2",null,null,null,{"$f":"D_Gru_stof4_Afstand_4_1","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_2","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_3","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_4","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_5","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_6","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_7","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_8","v":0},null,null,{"$f":"D_Gru_stof4_Afstand_4_9","v":0},null,null,"mg/l"]
["Konc. med nedbrydning C3",null,null,null,{"$f":"D_Gru_stof4_Afstand_5_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_5_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]
["Transporttid (sorpt.)",null,null,null,{"$f":"D_Gru_stof4_Afstand_6_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_6_9","v":{"$error":"#VALUE!"}},null,null,"år"]
["Konc. m. sorpt. og nedbr. C3",null,null,null,{"$f":"D_Gru_stof4_Afstand_7_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_5","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_6","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_7","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_8","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gru_stof4_Afstand_7_9","v":{"$error":"#VALUE!"}},null,null,"mg/l"]

{"sheet":"Dataark_Grundvand","index":11,"n_rows":182,"n_cols":19,"rows_kept":182,"cut":false,"hidden":true,"merged":[[70,4,70,6],[70,7,70,9],[70,10,70,12],[70,13,70,15],[1,1,1,15],[53,4,53,6],[53,7,53,9],[53,10,53,12],[53,13,53,15],[77,4,77,6],[77,7,77,9],[77,10,77,12],[77,13,77,15],[95,4,95,6],[95,7,95,9],[95,10,95,12],[95,13,95,15]]}
[]
[null,"Dataark-Grundvand",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Målt/beregnet koncentration","SAND/FALSK"]
[null,"Målt koncentration",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_målt","Styrende parametre"]
[null,"Beregnet koncentration",true,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_beregn","Styrende parametre"]
[null,"Nebrydningsforhold",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Styrende parametre"]
[null,"Aerobe forhold",true,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_aerob","Styrende parametre"]
[null,"Anaerobe forhold",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_anaerob","Styrende parametre"]
[null,"Koncentrationer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Styrende parametre"]
[null,"True/False fra enkeltstoffer",true,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_temp1_TrueFalse","Styrende parametre"]
[null,"True/False fra Vertikaltransport",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_temp2_TrueFalse","Styrende parametre"]
[null,"Udgår",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_temp3_TrueFalse","Styrende parametre"]
[null,"True/False fra Test andre værdier",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_temp4_TrueFalse","Styrende parametre"]
[null,"Valg af stof til visning af afstandsdata",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Styrende parametre"]
[null,"Stof1",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_Afstand_Stof1_TrueFalse","Styrende parametre"]
[null,"Stof2",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_Afstand_Stof2_TrueFalse","Styrende parametre"]
[null,"Stof3",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_Afstand_Stof3_TrueFalse","Styrende parametre"]
[null,"Stof4",false,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Gru_Afstand_Stof4_TrueFalse","Styrende parametre"]
[]
[null,"Vanddata"]
[null,"Parameter","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes"]
[null,"Hydraulisk ledningsevne (m/s)","k","m/s",null,null,{"$f":"Gru_My_k","v":0},{"$f":"IF(VALUE(G23),G23,IF(F23<>0,F23,\"\"))","v":""},"D_Gru_trin1a_k_syst",null,null,null,null,null,null,null,null,"D_Gru_trin1a_k","input, jorddata-hydraulik"]
[null,"Hydraulisk ledningsevne (m/år)","kår","m/år",null,{"$f":"B_Gru_trin1a_kår","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_kår","beregnes"]
[null,"Hydraulisk gradient","i","-",null,null,{"$f":"Gru_i","v":0},"",null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_i","input"]
[null,"Vandflux","Q0","m3/år",null,{"$f":"B_Gru_trin1a_Q0","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_Q0","beregnes"]
[null,"Darcy hastighed (vand)","VD","m/år",null,{"$f":"B_Gru_trin1a_VD","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_VD","beregnes"]
[null,"Grundvandsflux","Qg","m3/år",null,{"$f":"B_Gru_trin1a_Qg","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,"D_Gru_trin1a_Qg","beregnes"]
[null,"Gns. porevandshastighed","VP","m/år",null,{"$f":"B_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"D_Gru_trin2a_VP",null,null,null,null,null,null,null,null,"D_Gru_trin2a_VP","beregnes"]
[null,"Grundvandsflux","Qg_2a","m3/år",null,{"$f":"B_Gru_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"D_Gru_trin2a_Qg_2a",null,null,null,null,null,null,null,null,"D_Gru_trin2a_Qg_2a","beregnes"]
[]
[null,"Lokalitetsspecifikke data"]
[null,"Parameter","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes"]
[null,"Areal af forurenet område","A","m2",null,null,{"$f":"Gru_Y*Gru_X","v":0},{"$f":"IF(VALUE(G34),G34,IF(F34<>0,F34,\"\"))","v":""},null,null,null,null,null,null,null,null,null,"D_Gru_A","input"]
[null,"Længde af forurenet område","Y","m",null,null,{"$f":"Gru_Y","v":0},null,"Input Gru_Y"]
[null,"Bredde af forurenet område","X","m",null,null,{"$f":"Gru_X","v":0},"","Input Gru_X",null,null,null,null,null,null,null,null,"D_Gru_B","input"]
[null,"Nettoinfiltration","N","mm/år",null,null,{"$f":"Gru_My_Nedbør","v":0},"",null,null,null,null,null,null,null,null,null,"D_Gru_N","nedbørsdata"]
[null,"Egnsnavn",null,null,null,null,{"$f":"Gru_Kommune","v":""},{"$f":"IF(ISTEXT(G38),G38,IF(F38<>0,F38,\"\"))","v":""},null,null,null,null,null,null,null,null,null,"D_Gru_Kommune","Egnsnavn"]
[null,"Aquifermaterial",null,null,null,null,{"$f":"Gru_My_Aqui","v":0},{"$f":"IF(ISTEXT(G39),G39,IF(F39<>0,F39,\"\"))","v":""},"D_Gru_Aqui_syst"]
[null,"Opblandingstykkelse_trin1a","dm_1a","m",null,0.25,null,0.25,null,null,null,null,null,null,null,null,null,"D_Gru_dm_1a","default=0,25, (input)"]
[null,"Porøsitet, vandmættet ","eW","-",null,null,{"$f":"Gru_My_ew","v":0},{"$f":"IF(VALUE(G41),G41,IF(F41<>0,F41,\"\"))","v":""},"D_Gru_trin3_eW_syst",null,null,null,null,null,null,null,null,"D_Gru_trin3_eW","fra trin1a"]
[null,"Bulkmassefylde","(rho)b","kg/l",null,null,{"$f":"Gru_My_p","v":0},"","D_Gru_rhob_syst",null,null,null,null,null,null,null,null,"D_Gru_rhob"]
[null,"% Indhold organisk kulstof","foc (%)","-",null,null,{"$f":"Gru_My_foc","v":0},"","D_Gru_foc_syst"]
[null,"Fraktion organisk indhold","foc",null,null,{"$f":"F43/100","v":0},{"$f":"G43/100","v":0},{"$f":"H43/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"D_Gru_foc"]
[null,"Effiktiv porøsitet","eeff","-",null,null,{"$f":"Gru_My_eff","v":0},"","D_Gru_trin2a_eeff_syst",null,null,null,null,null,null,null,null,"D_Gru_trin2a_eeff","jorddata"]
[null,"Tykkelse af grundvandsmagasin","dm_max","m",null,null,{"$f":"Gru_maxdm","v":0},"",null,null,null,null,null,null,null,null,null,"D_Gru_trin2a_dm_max","input"]
[null,"Langsgående dispersivitet","(alfa)L","m",null,{"$f":"B_Gru_trin2a_aL","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,"D_Gru_trin2a_aL","beregnes"]
[null,"Transporttid","t","år",null,{"$f":"B_Gru_trin2a_t","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"D_Gru_trin2a_t",null,null,null,null,null,null,null,null,"D_Gru_trin2a_t","beregnes"]
[null,"Opblandingstykkelse_trin2a","dm_2a","m",null,{"$f":"B_Gru_trin2a_dm_2a","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,"D_Gru_trin2a_dm_2a","beregnes"]
[null,"Effektiv filterlængde","l","m",null,{"$f":"Gru_FilterL","v":0},null,{"$f":"IF(VALUE(G50),G50,IF(F50<>0,F50,\"\"))","v":""},null,null,null,null,null,null,null,null,null,"D_Gru_trin1b_l","input"]
[null,"Afstand til teoretisk beregningspunkt","L","m",null,{"$f":"B_Gru_trin1b_LL","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(G51),G51,IF(F51<>0,F51,\"\"))","v":{"$error":"#VALUE!"}},"D_Gru_trin1b_LL",null,null,null,null,null,null,null,null,"D_Gru_trin1b_LL","beregnes"]
[]
[null,"GRUNDVAND (Kildestyrkekoncentration - trin1a)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof2",null,null,"Stof3",null,null,"Sotf4",null,null,null,"Systemnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes"]
[null,"Forureningskomponent","stofnavn_n","-",null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,{"$f":"D_Enk_stofnavn_4","v":""},null,"D_Gru_trin1a_stofnavn_n","input, fugacitet, umættet"]
[null,"Fra enkeltstoffer",null,null,{"$f":"D_Enk_CV_endelig_1","v":""},null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(F57),F57,IF(E57<>0,E57,\"\")),\"\")","v":""},{"$f":"D_Enk_CV_endelig_2","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(VALUE(I57),I57,IF(H57<>0,H57,\"\")),\"\")","v":""},{"$f":"D_Enk_CV_endelig_3","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(VALUE(L57),L57,IF(K57<>0,K57,\"\")),\"\")","v":""},{"$f":"D_Enk_CV_endelig_4","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(VALUE(O57),O57,IF(N57<>0,N57,\"\")),\"\")","v":""},null,"D_Gru_trin1a_C0_temp1_n"]
[null,"Fra Vertikal transport",null,null,{"$f":"D_Ver_Cz_1","v":false},null,{"$f":"IF(VALUE(F58),F58,IF(E58<>0,E58,\"\"))","v":false},{"$f":"D_Ver_Cz_2","v":false},null,{"$f":"IF(VALUE(I58),I58,IF(H58<>0,H58,\"\"))","v":false},{"$f":"D_Ver_Cz_3","v":false},null,{"$f":"IF(VALUE(L58),L58,IF(K58<>0,K58,\"\"))","v":false},{"$f":"D_Ver_Cz_4","v":false},null,{"$f":"IF(VALUE(O58),O58,IF(N58<>0,N58,\"\"))","v":false},null,"D_Gru_trin1a_C0_temp2_n"]
[null,"Udgår",null,null,{"$f":"Gru_Trin1a_B_C0_1","v":1},null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(F59),F59,IF(E59<>0,E59,\"\")),\"\")","v":""},{"$f":"Gru_Trin1a_B_C0_2","v":2},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(VALUE(I59),I59,IF(H59<>0,H59,\"\")),\"\")","v":""},{"$f":"Gru_Trin1a_B_C0_3","v":3},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(VALUE(L59),L59,IF(K59<>0,K59,\"\")),\"\")","v":""},{"$f":"Gru_Trin1a_B_C0_4","v":4},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(VALUE(O59),O59,IF(N59<>0,N59,\"\")),\"\")","v":""},null,"D_Gru_trin1a_C0_temp3_n"]
[null,"Test andre værdier",null,null,null,{"$f":"Gru_Trin1a_my_C0_1","v":0},"",null,{"$f":"Gru_Trin1a_my_C0_2","v":0},"",null,{"$f":"Gru_Trin1a_my_C0_3","v":0},"",null,{"$f":"Gru_Trin1a_my_C0_4","v":0},"",null,"D_Gru_trin1a_C0_temp4_n"]
[null,"Er porevand beregnet vha fugacitet",null,null,null,{"$f":"IF(B_Gru_trin1a_C0_1=Enk_My_CV_1,\"0\",\"ja\")","v":"0"},null,null,{"$f":"IF(B_Gru_trin1a_C0_2=Enk_My_CV_2,\"0\",\"Ja\")","v":"0"},null,null,{"$f":"IF(B_Gru_trin1a_C0_3=Enk_My_CV_3,\"0\",\"Ja\")","v":"0"},null,null,{"$f":"IF(B_Gru_trin1a_C0_4=Enk_My_CV_4,\"0\",\"Ja\")","v":"0"}]
[null,"Kildekoncentration","C0_n","mg/L",{"$f":"B_Gru_trin1a_C0_1","v":""},null,"",{"$f":"B_Gru_trin1a_C0_2","v":""},null,"",{"$f":"B_Gru_trin1a_C0_3","v":""},null,"",{"$f":"B_Gru_trin1a_C0_4","v":""},null,"",null,"D_Gru_trin1a_C0_n","beregnes"]
[null,"Baggrundskonc.","Cg_n","mg/L",0,{"$f":"Gru_Trin1a_my_Cg_1","v":0},{"$f":"IF(VALUE(F63),F63,E63)","v":0},0,{"$f":"Gru_Trin1a_my_Cg_2","v":0},{"$f":"IF(VALUE(I63),I63,H63)","v":0},0,{"$f":"Gru_Trin1a_my_Cg_3","v":0},{"$f":"IF(VALUE(L63),L63,K63)","v":0},0,{"$f":"Gru_Trin1a_my_Cg_4","v":0},{"$f":"IF(VALUE(O63),O63,N63)","v":0},null,"D_Gru_trin1a_Cg_n","(input), default=0"]
[null,"Flux","J0_n","g/år",{"$f":"B_Gru_trin1a_J0_1","v":""},null,"",{"$f":"B_Gru_trin1a_J0_2","v":""},null,"",{"$f":"B_Gru_trin1a_J0_3","v":""},null,"",{"$f":"B_Gru_trin1a_J0_4","v":""},null,"",null,"D_Gru_trin1a_J0_n","beregnes"]
[null,"Naturlig flux","Jg_n","g/år",{"$f":"B_Gru_trin1a_Jg_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F65),F65,E65)","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin1a_Jg_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I65),I65,H65)","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin1a_Jg_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L65),L65,K65)","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin1a_Jg_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O65),O65,N65)","v":{"$error":"#VALUE!"}},null,"D_Gru_trin1a_Jg_n","beregnes"]
[null,"Forureningskoncentration_C1","C1a_n","mg/L",{"$f":"B_Gru_trin1a_C1_1","v":""},null,"",{"$f":"B_Gru_trin1a_C1_2","v":""},null,"",{"$f":"B_Gru_trin1a_C1_3","v":""},null,"",{"$f":"B_Gru_trin1a_C1_4","v":""},null,"",null,"D_Gru_trin1a_C1_n","beregnes"]
[null,"Grundvandskriteriet-overført fra enkeltstoffer",null,"mg/l",null,null,{"$f":"D_Enk_GV_Krit_1","v":""},null,null,{"$f":"D_enk_GV_Krit_2","v":""},null,null,{"$f":"D_Enk_GV_Krit_3","v":""},null,null,{"$f":"D_Enk_GV_Krit_4","v":""},null,"D_Gru_trin1a_Krit_n"]
[null,"Overskridelse af GV-krit for trin 1",null,"gange",{"$f":"B_Gru_trin1a_Krit_Overskr_1","v":"Intet kriterie"},null,"Intet kriterie",{"$f":"B_Gru_trin1a_Krit_Overskr_2","v":"Intet kriterie"},null,"Intet kriterie",{"$f":"B_Gru_trin1a_Krit_Overskr_3","v":"Intet kriterie"},null,"Intet kriterie",{"$f":"B_Gru_trin1a_Krit_Overskr_4","v":"Intet kriterie"},null,"Intet kriterie",null,"D_Gru_trin1a_Krit_Overskr_n","beregnes"]
[]
[null,"GRUNDVAND (Kildestyrkekoncentration - trin2a)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof2",null,null,"Stof3",null,null,"Sotf4",null,null,null,"Konstantnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes",null,"stof 1"]
[null,"Naturlig flux","Jg_2a_n","g/år",{"$f":"B_Gru_trin2a_Jg_2a_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F73),F73,E73)","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin2a_Jg_2a_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I73),I73,H73)","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin2a_Jg_2a_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L73),L73,K73)","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin2a_Jg_2a_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O73),O73,N73)","v":{"$error":"#VALUE!"}},null,"D_Gru_trin2a_Jg_2a_n","beregnes"]
[null,"Forureningskoncentration_C2","C2a_n","mg/L",{"$f":"B_Gru_trin2a_C2_1","v":""},null,{"$f":"IF(VALUE(F74),F74,IF(E74<>0,E74,\"\"))","v":""},{"$f":"B_Gru_trin2a_C2_2","v":""},null,{"$f":"IF(VALUE(I74),I74,IF(H74<>0,H74,\"\"))","v":""},{"$f":"B_Gru_trin2a_C2_3","v":""},null,{"$f":"IF(VALUE(L74),L74,IF(K74<>0,K74,\"\"))","v":""},{"$f":"B_Gru_trin2a_C2_4","v":""},null,{"$f":"IF(VALUE(O74),O74,IF(N74<>0,N74,\"\"))","v":""},null,"D_Gru_trin2a_C2_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 2",null,null,{"$f":"B_Gru_trin2a_Krit_Overskr_1","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F75),F75,IF(E75<>0,E75,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin2a_Krit_Overskr_2","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I75),I75,IF(H75<>0,H75,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin2a_Krit_Overskr_3","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L75),L75,IF(K75<>0,K75,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin2a_Krit_Overskr_4","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O75),O75,IF(N75<>0,N75,\"\"))","v":"Intet kriterie"},null,"D_Gru_trin2a_Krit_Overskr_n","beregnes"]
[]
[null,"GRUNDVAND (Kildestyrkekoncentration - trin1b+2b)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof2",null,null,"Stof3",null,null,"Sotf4",null,null,null,"Konstantnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes",null,"stof 1"]
[null,"Forureningskoncentration, målt","C1bm_n","mg/L",{"$f":"Gru_C1bm_1","v":0},{"$f":"Gru_My_C1bm_1","v":0},{"$f":"IF(VALUE(F80),F80,IF(E80<>0,E80,\"\"))","v":""},{"$f":"Gru_C1bm_2","v":0},{"$f":"Gru_My_C1bm_2","v":0},{"$f":"IF(VALUE(I80),I80,IF(H80<>0,H80,\"\"))","v":""},{"$f":"Gru_C1bm_3","v":0},{"$f":"Gru_My_C1bm_3","v":0},{"$f":"IF(VALUE(L80),L80,IF(K80<>0,K80,\"\"))","v":""},{"$f":"Gru_C1bm_4","v":0},{"$f":"Gru_My_C1bm_4","v":0},{"$f":"IF(VALUE(O80),O80,IF(N80<>0,N80,\"\"))","v":""},null,"D_Gru_trin1b_C1bm_n","input, fugacitet"]
[null,"Forureningskoncentration_C1_trin1b","C1b_n","mg/L",{"$f":"B_Gru_trin1b_C1b_1","v":""},null,{"$f":"IF(VALUE(F81),F81,IF(E81<>0,E81,\"\"))","v":""},{"$f":"B_Gru_trin1b_C1b_2","v":""},null,{"$f":"IF(VALUE(I81),I81,IF(H81<>0,H81,\"\"))","v":""},{"$f":"B_Gru_trin1b_C1b_3","v":""},null,{"$f":"IF(VALUE(L81),L81,IF(K81<>0,K81,\"\"))","v":""},{"$f":"B_Gru_trin1b_C1b_4","v":""},null,{"$f":"IF(VALUE(O81),O81,IF(N81<>0,N81,\"\"))","v":""},null,"D_Gru_trin1b_C1b_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 1",null,null,{"$f":"B_Gru_trin1b_Krit_Overskr_1","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F82),F82,IF(E82<>0,E82,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin1b_Krit_Overskr_2","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I82),I82,IF(H82<>0,H82,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin1b_Krit_Overskr_3","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L82),L82,IF(K82<>0,K82,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin1b_Krit_Overskr_4","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O82),O82,IF(N82<>0,N82,\"\"))","v":"Intet kriterie"},null,"D_Gru_trin1b_Krit_Overskr_n","beregnes"]
[null,"Forureningskoncentration_C2_trin2b","C2b_n","mg/L",{"$f":"B_Gru_trin2b_C2b_1","v":""},null,{"$f":"IF(VALUE(F83),F83,IF(E83<>0,E83,\"\"))","v":""},{"$f":"B_Gru_trin2b_C2b_2","v":""},null,{"$f":"IF(VALUE(I83),I83,IF(H83<>0,H83,\"\"))","v":""},{"$f":"B_Gru_trin2b_C2b_3","v":""},null,{"$f":"IF(VALUE(L83),L83,IF(K83<>0,K83,\"\"))","v":""},{"$f":"B_Gru_trin2b_C2b_4","v":""},null,{"$f":"IF(VALUE(O83),O83,IF(N83<>0,N83,\"\"))","v":""},null,"D_Gru_trin2b_C2b_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 2",null,null,{"$f":"B_Gru_trin2b_Krit_Overskr_1","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F84),F84,IF(E84<>0,E84,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin2b_Krit_Overskr_2","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I84),I84,IF(H84<>0,H84,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin2b_Krit_Overskr_3","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L84),L84,IF(K84<>0,K84,\"\"))","v":"Intet kriterie"},{"$f":"B_Gru_trin2b_Krit_Overskr_4","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O84),O84,IF(N84<>0,N84,\"\"))","v":"Intet kriterie"},null,"D_Gru_trin2b_Krit_Overskr_n","beregnes"]
[]
[null,"Endelig beregning for",{"$f":"IF(D_Gru_beregn=TRUE,\"Beregnet koncentrationer for trin 1a og 2a\",\"Målt koncentrationer i trin 1b\")","v":"Beregnet koncentrationer for trin 1a og 2a"}]
[]
[null,"Grundvandskoncentration: Trin 1",null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C1_1,D_Gru_trin1b_C1b_1),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C1_2,D_Gru_trin1b_C1b_2),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C1_3,D_Gru_trin1b_C1b_3),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C1_4,D_Gru_trin1b_C1b_4),\"\")","v":""}]
[null,"Overskridelse af kriteriet Trin 1",null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Gru_beregn,D_Gru_trin1a_Krit_Overskr_1,D_Gru_trin1b_Krit_Overskr_1),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Gru_beregn,D_Gru_trin1a_Krit_Overskr_2,D_Gru_trin1b_Krit_Overskr_2),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Gru_beregn,D_Gru_trin1a_Krit_Overskr_3,D_Gru_trin1b_Krit_Overskr_3),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Gru_beregn,D_Gru_trin1a_Krit_Overskr_4,D_Gru_trin1b_Krit_Overskr_4),\"\")","v":""}]
[null,"Grundvandskoncentration: Trin 2",null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Gru_beregn,D_Gru_trin2a_C2_1,D_Gru_trin2b_C2b_1),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Gru_beregn,D_Gru_trin2a_C2_2,D_Gru_trin2b_C2b_2),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Gru_beregn,D_Gru_trin2a_C2_3,D_Gru_trin2b_C2b_3),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Gru_beregn,D_Gru_trin2a_C2_4,D_Gru_trin2b_C2b_4),\"\")","v":""}]
[null,"Overskridelse af kriteriet Trin 2",null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin2a_Krit_Overskr_1,D_Gru_trin2b_Krit_Overskr_1),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin2a_Krit_Overskr_2,D_Gru_trin2b_Krit_Overskr_2),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin2a_Krit_Overskr_3,D_Gru_trin2b_Krit_Overskr_3),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin2a_Krit_Overskr_4,D_Gru_trin2b_Krit_Overskr_4),\"\")","v":""}]
[null,"Forueningsflux, vertikal Trin 1a",null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_J0_1,\"\"),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_J0_2,\"\"),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_J0_3,\"\"),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_Gru_beregn=TRUE,D_Gru_trin1a_J0_4,\"\"),\"\")","v":""}]
[]
[]
[null,"GRUNDVAND (Konc. med sorption og nedbrydning - trin3)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4",null,null,null,"Konstantnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes"]
[null,"Forureningskoncentration","C2_n","mg/L",{"$f":"B_Gru_trin3_C2_1","v":""},null,{"$f":"IF(VALUE(F98),F98,IF(E98<>0,E98,\"\"))","v":""},{"$f":"B_Gru_trin3_C2_2","v":""},null,{"$f":"IF(VALUE(I98),I98,IF(H98<>0,H98,\"\"))","v":""},{"$f":"B_Gru_trin3_C2_3","v":""},null,{"$f":"IF(VALUE(L98),L98,IF(K98<>0,K98,\"\"))","v":""},{"$f":"B_Gru_trin3_C2_4","v":""},null,{"$f":"IF(VALUE(O98),O98,IF(N98<>0,N98,\"\"))","v":""},null,"D_Gru_trin3_C2_n","beregnes"]
[null,"Fordelingskoefficienten","KD_n","-",{"$f":"B_Gru_trin3_KB_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F99),F99,IF(E99<>0,E99,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin3_KB_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I99),I99,IF(H99<>0,H99,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin3_KB_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L99),L99,IF(K99<>0,K99,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_trin3_KB_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O99),O99,IF(N99<>0,N99,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Gru_trin3_KD_n","beregnes"]
[null,"logkow","logKOW",null,{"$f":"D_Enk_KOW_syst_1","v":0},{"$f":"Enk_My_KOW_1","v":0},{"$f":"IF(VALUE(F100),F100,IF(E100<>0,E100,\"\"))","v":""},{"$f":"D_Enk_KOW_syst_2","v":0},{"$f":"Enk_My_KOW_2","v":0},{"$f":"IF(VALUE(I100),I100,IF(H100<>0,H100,\"\"))","v":""},{"$f":"D_Enk_KOW_syst_3","v":0},{"$f":"Enk_My_KOW_3","v":0},{"$f":"IF(VALUE(L100),L100,IF(K100<>0,K100,\"\"))","v":""},{"$f":"D_Enk_KOW_syst_4","v":0},{"$f":"Enk_My_KOW_4","v":0},{"$f":"IF(VALUE(O100),O100,IF(N100<>0,N100,\"\"))","v":""},null,"D_Gru_trin3_logKOW_n"]
[null,"logKD","logKD",null,{"$f":"B_Gru_trin3_logKB_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(E101),E101,\"\")","v":""},{"$f":"B_Gru_trin3_logKB_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H101),H101,\"\")","v":""},{"$f":"B_Gru_trin3_logKB_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K101),K101,\"\")","v":""},{"$f":"B_Gru_trin3_logKB_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N101),N101,\"\")","v":""},null,"D_Gru_trin3_logKB_n","beregnes"]
[null,"1. ordens nedbrydningskonstant","k1_n","dage-1",{"$f":"B_Gru_trin3_k1_1","v":0},null,{"$f":"E102","v":0},{"$f":"B_Gru_trin3_k1_2","v":0},null,{"$f":"H102","v":0},{"$f":"B_Gru_trin3_k1_3","v":0},null,{"$f":"K102","v":0},{"$f":"B_Gru_trin3_k1_4","v":0},null,{"$f":"N102","v":0},null,"D_Gru_trin3_k1_n","beregnes"]
[null,"1. ordens nedbrydningskonstant aerob","-","dage-1",{"$f":"D_Enk_k1aerob_syst_1","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_1),Enk_MY_k1aerob_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(F103),F103,IF(ISNUMBER(E103),E103,\"\"))","v":0},{"$f":"D_Enk_k1aerob_syst_2","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_2),Enk_MY_k1aerob_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(I103),I103,IF(ISNUMBER(H103),H103,\"\"))","v":0},{"$f":"D_Enk_k1aerob_syst_3","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_3),Enk_MY_k1aerob_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(L103),L103,IF(ISNUMBER(K103),K103,\"\"))","v":0},{"$f":"D_Enk_k1aerob_syst_4","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1aerob_4),Enk_MY_k1aerob_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(O103),O103,IF(ISNUMBER(N103),N103,\"\"))","v":0},null,"D_Gru_trin3_k1_aerob_n","stofdata"]
[null,"1. ordens nedbrydningskonstant anaerob","-","dage-1",{"$f":"D_Enk_k1anaerob_syst_1","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_1),Enk_MY_k1anaerob_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(F104),F104,IF(ISNUMBER(E104),E104,\"\"))","v":0},{"$f":"D_Enk_k1anaerob_syst_2","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_2),Enk_MY_k1anaerob_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(I104),I104,IF(ISNUMBER(H104),H104,\"\"))","v":0},{"$f":"D_Enk_k1anaerob_syst_3","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_3),Enk_MY_k1anaerob_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(L104),L104,IF(ISNUMBER(K104),K104,\"\"))","v":0},{"$f":"D_Enk_k1anaerob_syst_4","v":0},{"$f":"IF(ISNUMBER(Enk_MY_k1anaerob_4),Enk_MY_k1anaerob_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(O104),O104,IF(ISNUMBER(N104),N104,\"\"))","v":0},null,"D_Gru_trin3_k1_anaerob_n","stofdata"]
[null,"Forureningskonc._C3_med nedbr.","ned_C3_n","mg/L",{"$f":"B_Gru_trin3_ned_C3_1","v":""},null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",E105,\"\")","v":""},{"$f":"B_Gru_trin3_ned_C3_2","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",H105,\"\")","v":""},{"$f":"B_Gru_trin3_ned_C3_3","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",K105,\"\")","v":""},{"$f":"B_Gru_trin3_ned_C3_4","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",N105,\"\")","v":""},null,"D_Gru_trin3_ned_C3_n","Beregnes"]
[null,"Forureningskonc._C3_med sorpt.+nedbryd","C3_n","mg/L",{"$f":"B_Gru_trin3_C3_1","v":""},null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",E106,\"\")","v":""},{"$f":"B_Gru_trin3_C3_2","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",H106,\"\")","v":""},{"$f":"B_Gru_trin3_C3_3","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",K106,\"\")","v":""},{"$f":"B_Gru_trin3_C3_4","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",N106,\"\")","v":""},null,"D_Gru_trin3_C3_n","beregnes"]
[null,"Retardationsfaktor","R","-",{"$f":"B_Gru_trin3_R_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(E107),E107,\"\")","v":""},{"$f":"B_Gru_trin3_R_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H107),H107,\"\")","v":""},{"$f":"B_Gru_trin3_R_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K107),K107,\"\")","v":""},{"$f":"B_Gru_trin3_R_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N107),N107,\"\")","v":""},null,"D_Gru_trin3_R_n","beregnes"]
[null,"Gns. porevandshastighed m. sorption","VS","m/år",{"$f":"B_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(E108),E108,\"\")","v":""},{"$f":"B_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H108),H108,\"\")","v":""},{"$f":"B_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K108),K108,\"\")","v":""},{"$f":"B_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N108),N108,\"\")","v":""},null,"D_Gru_trin3_VS_n","beregnes"]
[null,"Transporttid med sorption","t_sorp","dage",{"$f":"B_Gru_trin3_t_sorp_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(E109),E109,\"\")","v":""},{"$f":"B_Gru_trin3_t_sorp_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H109),H109,\"\")","v":""},{"$f":"B_Gru_trin3_t_sorp_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K109),K109,\"\")","v":""},{"$f":"B_Gru_trin3_t_sorp_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N109),N109,\"\")","v":""},null,"D_Gru_trin3_t_sorp_n","beregnes"]
[null,"Overskridelse af Gv-Krit for trin 3",null,null,{"$f":"B_Gru_trin3_Krit_Overskr_1","v":"Intet kriterie"},null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(F110),F110,IF(E110<>0,E110,\"\")),\"\")","v":""},{"$f":"B_Gru_trin3_Krit_Overskr_2","v":"Intet kriterie"},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(VALUE(I110),I110,IF(H110<>0,H110,\"\")),\"\")","v":""},{"$f":"B_Gru_trin3_Krit_Overskr_3","v":"Intet kriterie"},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(VALUE(L110),L110,IF(K110<>0,K110,\"\")),\"\")","v":""},{"$f":"B_Gru_trin3_Krit_Overskr_4","v":"Intet kriterie"},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(VALUE(O110),O110,IF(N110<>0,N110,\"\")),\"\")","v":""},null,"D_Gru_trin3_Krit_Overskr_n","beregnes"]
[]
[null,"Anvendt brugerdata",null,null,null,{"$f":"SUM(G23,G37,G41:G45,F60,F80,F100,F103:F104)","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(F112>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM(G23,G37,G41:G45,I60,I80,I100,I103:I104)","v":0},{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(I112>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM(G23,G37,G41:G45,L60,L80,L100,L103:L104)","v":0},{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(L112>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM(G23,G37,G41:G45,O60,O80,O100,O103:O104)","v":0},{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(O112>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""}]
[]
[null,"Stof 1",null,null,{"$f":"D_Gru_stofnavn_1","v":""}]
[null,"Afstand",null,null,{"$f":"Gru_afstand_bruger_1","v":0},0,10,20,30,40,50,75,100,"D_Gru_stof1_Afstand_1_n"]
[null,"Kvalitetskriteriet",null,null,null,{"$f":"D_Enk_GV_Krit_1","v":""},null,null,null,null,null,null,{"$f":"D_Enk_GV_Krit_1","v":""}]
[null,"Afstand til teoretisk beregningspunkt",null,{"$f":"D_Gru_trin1b_LL","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Transporttid",null,null,{"$f":"B_Gru_stof1_AfstanB_2_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_2_9","v":{"$error":"#VALUE!"}},"D_Gru_stof1_Afstand_2_n"]
[null,"Opblandingsdybde,m",null,null,{"$f":"B_Gru_stof1_AfstanB_3_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_3_9","v":{"$error":"#VALUE!"}},"D_Gru_stof1_Afstand_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"B_Gru_stof1_AfstanB_4_1","v":0},{"$f":"B_Gru_stof1_AfstanB_4_2","v":0},{"$f":"B_Gru_stof1_AfstanB_4_3","v":0},{"$f":"B_Gru_stof1_AfstanB_4_4","v":0},{"$f":"B_Gru_stof1_AfstanB_4_5","v":0},{"$f":"B_Gru_stof1_AfstanB_4_6","v":0},{"$f":"B_Gru_stof1_AfstanB_4_7","v":0},{"$f":"B_Gru_stof1_AfstanB_4_8","v":0},{"$f":"B_Gru_stof1_AfstanB_4_9","v":0},"D_Gru_stof1_Afstand_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"B_Gru_stof1_AfstanB_5_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_5_9","v":{"$error":"#VALUE!"}},"D_Gru_stof1_Afstand_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"B_Gru_stof1_AfstanB_6_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_6_9","v":{"$error":"#VALUE!"}},"D_Gru_stof1_Afstand_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,0,{"$f":"B_Gru_stof1_AfstanB_7_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof1_AfstanB_7_9","v":{"$error":"#VALUE!"}},"D_Gru_stof1_Afstand_7_n"]
[]
[]
[]
[]
[]
[]
[null,"Stof 2",null,null,{"$f":"D_Gru_stofnavn_2","v":""}]
[null,"Afstand",null,null,{"$f":"Gru_afstand_bruger_2","v":0},0,10,20,30,40,50,75,100,"D_Gru_stof2_Afstand_1_n"]
[null,"Kvalitetskriteriet",null,null,null,{"$f":"D_enk_GV_Krit_2","v":""},null,null,null,null,null,null,{"$f":"D_enk_GV_Krit_2","v":""}]
[null,"Afstand til teoretisk beregningspunkt",null,{"$f":"D_Gru_trin1b_LL","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Transporttid",null,null,{"$f":"B_Gru_stof2_AfstanB_2_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_2_9","v":{"$error":"#VALUE!"}},"D_Gru_stof2_Afstand_2_n"]
[null,"Opblandingsdybde,m",null,null,{"$f":"B_Gru_stof2_AfstanB_3_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_3_9","v":{"$error":"#VALUE!"}},"D_Gru_stof2_Afstand_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"B_Gru_stof2_AfstanB_4_1","v":0},{"$f":"B_Gru_stof2_AfstanB_4_2","v":0},{"$f":"B_Gru_stof2_AfstanB_4_3","v":0},{"$f":"B_Gru_stof2_AfstanB_4_4","v":0},{"$f":"B_Gru_stof2_AfstanB_4_5","v":0},{"$f":"B_Gru_stof2_AfstanB_4_6","v":0},{"$f":"B_Gru_stof2_AfstanB_4_7","v":0},{"$f":"B_Gru_stof2_AfstanB_4_8","v":0},{"$f":"B_Gru_stof2_AfstanB_4_9","v":0},"D_Gru_stof2_Afstand_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"B_Gru_stof2_AfstanB_5_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_5_9","v":{"$error":"#VALUE!"}},"D_Gru_stof2_Afstand_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"B_Gru_stof2_AfstanB_6_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_6_9","v":{"$error":"#VALUE!"}},"D_Gru_stof2_Afstand_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,0,{"$f":"B_Gru_stof2_AfstanB_7_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof2_AfstanB_7_9","v":{"$error":"#VALUE!"}},"D_Gru_stof2_Afstand_7_n"]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 3",null,null,{"$f":"D_Gru_stofnavn_3","v":""}]
[null,"Afstand",null,null,{"$f":"Gru_Afstand_bruger_3","v":0},0,10,20,30,40,50,75,100,"D_Gru_stof3_Afstand_1_n"]
[null,"Kvalitetskriteriet",null,null,null,{"$f":"D_Enk_GV_Krit_3","v":""},null,null,null,null,null,null,{"$f":"D_Enk_GV_Krit_3","v":""}]
[null,"Afstand til teoretisk beregningspunkt",null,{"$f":"D_Gru_trin1b_LL","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Transporttid",null,null,{"$f":"B_Gru_stof3_AfstanB_2_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_2_9","v":{"$error":"#VALUE!"}},"D_Gru_stof3_Afstand_2_n"]
[null,"Opblandingsdybde,m",null,null,{"$f":"B_Gru_stof3_AfstanB_3_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_3_9","v":{"$error":"#VALUE!"}},"D_Gru_stof3_Afstand_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"B_Gru_stof3_AfstanB_4_1","v":0},{"$f":"B_Gru_stof3_AfstanB_4_2","v":0},{"$f":"B_Gru_stof3_AfstanB_4_3","v":0},{"$f":"B_Gru_stof3_AfstanB_4_4","v":0},{"$f":"B_Gru_stof3_AfstanB_4_5","v":0},{"$f":"B_Gru_stof3_AfstanB_4_6","v":0},{"$f":"B_Gru_stof3_AfstanB_4_7","v":0},{"$f":"B_Gru_stof3_AfstanB_4_8","v":0},{"$f":"B_Gru_stof3_AfstanB_4_9","v":0},"D_Gru_stof3_Afstand_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"B_Gru_stof3_AfstanB_5_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_5_9","v":{"$error":"#VALUE!"}},"D_Gru_stof3_Afstand_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"B_Gru_stof3_AfstanB_6_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_6_9","v":{"$error":"#VALUE!"}},"D_Gru_stof3_Afstand_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,0,{"$f":"B_Gru_stof3_AfstanB_7_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof3_AfstanB_7_9","v":{"$error":"#VALUE!"}},"D_Gru_stof3_Afstand_7_n"]
[]
[]
[]
[]
[]
[]
[null,"Stof 4",null,null,{"$f":"D_Gru_stofnavn_4","v":""}]
[null,"Afstand",null,null,{"$f":"Gru_afstand_bruger_4","v":0},0,10,20,30,40,50,75,100,"D_Gru_stof4_Afstand_1_n"]
[null,"Kvalitetskriteriet",null,null,null,{"$f":"D_Enk_GV_Krit_4","v":""},null,null,null,null,null,null,{"$f":"D_Enk_GV_Krit_4","v":""}]
[null,"Afstand til teoretisk beregningspunkt",null,{"$f":"D_Gru_trin1b_LL","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Transporttid",null,null,{"$f":"B_Gru_stof4_AfstanB_2_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_2_9","v":{"$error":"#VALUE!"}},"D_Gru_stof4_Afstand_2_n"]
[null,"Opblandingsdybde,m",null,null,{"$f":"B_Gru_stof4_AfstanB_3_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_3_9","v":{"$error":"#VALUE!"}},"D_Gru_stof4_Afstand_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"B_Gru_stof4_AfstanB_4_1","v":0},{"$f":"B_Gru_stof4_AfstanB_4_2","v":0},{"$f":"B_Gru_stof4_AfstanB_4_3","v":0},{"$f":"B_Gru_stof4_AfstanB_4_4","v":0},{"$f":"B_Gru_stof4_AfstanB_4_5","v":0},{"$f":"B_Gru_stof4_AfstanB_4_6","v":0},{"$f":"B_Gru_stof4_AfstanB_4_7","v":0},{"$f":"B_Gru_stof4_AfstanB_4_8","v":0},{"$f":"B_Gru_stof4_AfstanB_4_9","v":0},"D_Gru_stof4_Afstand_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"B_Gru_stof4_AfstanB_5_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_5_9","v":{"$error":"#VALUE!"}},"D_Gru_stof4_Afstand_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"B_Gru_stof4_AfstanB_6_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_6_9","v":{"$error":"#VALUE!"}},"D_Gru_stof4_Afstand_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,0,{"$f":"B_Gru_stof4_AfstanB_7_1","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_2","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_3","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_4","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_5","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_6","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_7","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_8","v":{"$error":"#VALUE!"}},{"$f":"B_Gru_stof4_AfstanB_7_9","v":{"$error":"#VALUE!"}},"D_Gru_stof4_Afstand_7_n"]
[]
[null,"Bemærkninger"]
[null,"Det forurenede område:","D_Gru_DFO_ComUds"]
[null,null,false]
[null,"Magasin:","D_Gru_Mag_ComUds"]
[null,null,false]
[null,"Forurening:","D_Gru_For_ComUds"]
[null,null,false]
[null,"Beregning:","D_Gru_Ber_ComUds"]
[null,null,false]

{"sheet":"Beregning_Grundvand","index":12,"n_rows":118,"n_cols":19,"rows_kept":118,"cut":false,"hidden":true,"merged":[[29,4,29,6],[29,7,29,9],[29,10,29,12],[29,13,29,15],[1,1,1,15],[20,4,20,6],[20,7,20,9],[20,10,20,12],[20,13,20,15],[36,4,36,6],[36,7,36,9],[36,10,36,12],[36,13,36,15],[44,4,44,6],[44,7,44,9],[44,10,44,12],[44,13,44,15]]}
[]
[null,"Beregningslag",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Vanddata"]
[null,"Stoffer","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes",null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[null,"Hydraulisk ledningsevne (m/år)","kår","m/år",{"$f":"D_trin1a_k*(60*60*24*365.25)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F6),F6,IF(E6<>0,E6,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin1a_kår","beregnes"]
[null,"Vandflux","Q0","m3/år",{"$f":"(D_Gru_N*D_Gru_A)/1000","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin1a_Q0","beregnes"]
[null,"Darcy hastighed (vand)","VD","m/år",{"$f":"B_Gru_trin1a_kår*D_Gru_trin1a_i","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin1a_VD","beregnes"]
[null,"Grundvandsflux","Qg","m3/år",{"$f":"D_Gru_B*D_Gru_dm_1a*B_Gru_trin1a_VD","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin1a_Qg","beregnes"]
[null,"Gns. porevandshastighed","VP","m/år",{"$f":"B_Gru_trin1a_VD/D_Gru_trin2a_eeff","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin2a_VP","beregnes"]
[null,"Grundvandsflux","Qg_2a","m3/år",{"$f":"D_Gru_B*B_Gru_trin2a_dm_2a*B_Gru_trin1a_VD","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin2a_Qg_2a","beregnes"]
[]
[null,"Lokalitetsspecifikke data"]
[null,"Stoffer","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes",null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[null,"Langsgående dispersivitet","(alfa)L","m",{"$f":"0.0000042*POWER(B_Gru_trin1b_LL,2)+0.0036*B_Gru_trin1b_LL-0.008","v":{"$error":"#VALUE!"}},null,{"$f":"IF(E15<0,1E-36,E15)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin2a_aL","beregnes"]
[null,"Transporttid","t","år",{"$f":"D_Gru_trin1b_LL/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F16),F16,IF(E16<>0,E16,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin2a_t","beregnes"]
[null,"Opblandingstykkelse_trin2a","dm_2a","m",{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*D_Gru_trin2a_aL*D_Gru_trin2a_VP*D_Gru_trin2a_t)))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F17),F17,IF(E17<>0,E17,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin2a_dm_2a","beregnes"]
[null,"Afstand til teoretisk beregningspunkt","L","m",{"$f":"MIN(B_Gru_trin2a_VP,100)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F18),F18,IF(E18<>0,E18,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_Gru_trin1b_LL","beregnes"]
[]
[null,"GRUNDVAND (Kildestyrkekoncentration - trin1a)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof2",null,null,"Stof3",null,null,"Sotf4",null,null,null,"Systemnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes",null,"stof 1"]
[null,"Kildekoncentration","C0_n","mg/L",{"$f":"IF(D_Gru_trin1a_temp1_TrueFalse=TRUE,D_Gru_trin1a_C0_temp1_1,IF(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_C0_temp2_1,IF(D_Gru_trin1a_temp3_TrueFalse=TRUE,D_Gru_trin1a_C0_temp3_1,IF(D_Gru_trin1a_temp4_TrueFalse=TRUE,D_Gru_trin1a_C0_temp4_1,))))","v":""},null,{"$f":"IF(VALUE(F23),F23,IF(E23<>0,E23,\"\"))","v":""},{"$f":"IF(D_Gru_trin1a_temp1_TrueFalse=TRUE,D_Gru_trin1a_C0_temp1_2,IF(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_C0_temp2_2,IF(D_Gru_trin1a_temp3_TrueFalse=TRUE,D_Gru_trin1a_C0_temp3_2,IF(D_Gru_trin1a_temp4_TrueFalse=TRUE,D_Gru_trin1a_C0_temp4_2,))))","v":""},null,{"$f":"IF(VALUE(I23),I23,IF(H23<>0,H23,\"\"))","v":""},{"$f":"IF(D_Gru_trin1a_temp1_TrueFalse=TRUE,D_Gru_trin1a_C0_temp1_3,IF(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_C0_temp2_3,IF(D_Gru_trin1a_temp3_TrueFalse=TRUE,D_Gru_trin1a_C0_temp3_3,IF(D_Gru_trin1a_temp4_TrueFalse=TRUE,D_Gru_trin1a_C0_temp4_3,))))","v":""},null,{"$f":"IF(VALUE(L23),L23,IF(K23<>0,K23,\"\"))","v":""},{"$f":"IF(D_Gru_trin1a_temp1_TrueFalse=TRUE,D_Gru_trin1a_C0_temp1_4,IF(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_C0_temp2_4,IF(D_Gru_trin1a_temp3_TrueFalse=TRUE,D_Gru_trin1a_C0_temp3_4,IF(D_Gru_trin1a_temp4_TrueFalse=TRUE,D_Gru_trin1a_C0_temp4_4,))))","v":""},null,{"$f":"IF(VALUE(O23),O23,IF(N23<>0,N23,\"\"))","v":""},null,"B_Gru_trin1a_C0_n","beregnes"]
[null,"Flux","J0_n","g/år",{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_1),D_Gru_trin1a_C0_1*D_Gru_trin1a_Q0,\"\")","v":""},null,{"$f":"IF(VALUE(F24),F24,IF(E24<>0,E24,\"\"))","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_2),D_Gru_trin1a_C0_2*D_Gru_trin1a_Q0,\"\")","v":""},null,{"$f":"IF(VALUE(I24),I24,IF(H24<>0,H24,\"\"))","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_3),D_Gru_trin1a_C0_3*D_Gru_trin1a_Q0,\"\")","v":""},null,{"$f":"IF(VALUE(L24),L24,IF(K24<>0,K24,\"\"))","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_4), (D_Gru_trin1a_C0_4*D_Gru_trin1a_Q0),\"\")","v":""},null,{"$f":"IF(VALUE(O24),O24,IF(N24<>0,N24,\"\"))","v":""},null,"B_Gru_trin1a_J0_n","beregnes"]
[null,"Naturlig flux","Jg_n","g/år",{"$f":"D_Gru_trin1a_Qg*D_Gru_trin1a_Cg_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F25),F25,E25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_trin1a_Qg*D_Gru_trin1a_Cg_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I25),I25,H25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_trin1a_Qg*D_Gru_trin1a_Cg_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L25),L25,K25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_trin1a_Qg*D_Gru_trin1a_Cg_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O25),O25,N25)","v":{"$error":"#VALUE!"}},null,"B_Gru_trin1a_Jg_n","beregnes"]
[null,"Forureningskoncentration_C1","C1a_n","mg/L",{"$f":"IF(ISNUMBER((D_Gru_trin1a_J0_1+D_Gru_trin1a_Jg_1)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg)),(D_Gru_trin1a_J0_1+D_Gru_trin1a_Jg_1)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg),\"\")","v":""},null,{"$f":"IF(VALUE(F26),F26,IF(E26<>0,E26,\"\"))","v":""},{"$f":"IF(ISNUMBER((D_Gru_trin1a_J0_2+D_Gru_trin1a_Jg_2)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg)),(D_Gru_trin1a_J0_2+D_Gru_trin1a_Jg_2)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg),\"\")","v":""},null,{"$f":"IF(VALUE(I26),I26,IF(H26<>0,H26,\"\"))","v":""},{"$f":"IF(ISNUMBER((D_Gru_trin1a_J0_3+D_Gru_trin1a_Jg_3)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg)),(D_Gru_trin1a_J0_3+D_Gru_trin1a_Jg_3)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg),\"\")","v":""},null,{"$f":"IF(VALUE(L26),L26,IF(K26<>0,K26,\"\"))","v":""},{"$f":"IF(ISNUMBER((D_Gru_trin1a_J0_4+D_Gru_trin1a_Jg_4)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg)),(D_Gru_trin1a_J0_4+D_Gru_trin1a_Jg_4)/(D_Gru_trin1a_Q0+D_Gru_trin1a_Qg),\"\")","v":""},null,{"$f":"IF(VALUE(O26),O26,IF(N26<>0,N26,\"\"))","v":""},null,"B_Gru_trin1a_C1_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 1",null,"gange",{"$f":"IF(D_Gru_trin1a_Krit_1=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C1_1),IF(D_Gru_trin1a_C1_1>D_Gru_trin1a_Krit_1,D_Gru_trin1a_C1_1/D_Gru_trin1a_Krit_1,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F27),F27,IF(E27<>0,E27,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_2=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C1_2),IF(D_Gru_trin1a_C1_2>D_Gru_trin1a_Krit_2,D_Gru_trin1a_C1_2/D_Gru_trin1a_Krit_2,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I27),I27,IF(H27<>0,H27,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_3=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C1_3),IF(D_Gru_trin1a_C1_3>D_Gru_trin1a_Krit_3,D_Gru_trin1a_C1_3/D_Gru_trin1a_Krit_3,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L27),L27,IF(K27<>0,K27,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_4=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C1_4),IF(D_Gru_trin1a_C1_4>D_Gru_trin1a_Krit_4,D_Gru_trin1a_C1_4/D_Gru_trin1a_Krit_4,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O27),O27,IF(N27<>0,N27,\"\"))","v":"Intet kriterie"},null,"B_Gru_trin1a_Krit_Overskr_n","beregnes"]
[]
[null,"GRUNDVAND (Kildestyrkekoncentration - trin2a)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof2",null,null,"Stof3",null,null,"Sotf4",null,null,null,"Konstantnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes",null,"stof 1"]
[null,"Naturlig flux","Jg_2a_n","g/år",{"$f":"D_Gru_trin1a_Cg_1*D_Gru_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F32),F32,E32)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_trin1a_Cg_2*D_Gru_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I32),I32,H32)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_trin1a_Cg_3*D_Gru_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L32),L32,K32)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_trin1a_Cg_4*D_Gru_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O32),O32,N32)","v":{"$error":"#VALUE!"}},null,"B_Gru_trin2a_Jg_2a_n","beregnes"]
[null,"Forureningskoncentration_C2","C2a_n","mg/L",{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_1),(D_Gru_trin1a_J0_1+D_Gru_trin2a_Jg_2a_1)/(D_Gru_trin1a_Q0+D_Gru_trin2a_Qg_2a),\"\")","v":""},null,{"$f":"IF(VALUE(F33),F33,IF(E33<>0,E33,\"\"))","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_2),(D_Gru_trin1a_J0_2+D_Gru_trin2a_Jg_2a_2)/(D_Gru_trin1a_Q0+D_Gru_trin2a_Qg_2a),\"\")","v":""},null,{"$f":"IF(VALUE(I33),I33,IF(H33<>0,H33,\"\"))","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_3),(D_Gru_trin1a_J0_3+D_Gru_trin2a_Jg_2a_3)/(D_Gru_trin1a_Q0+D_Gru_trin2a_Qg_2a),\"\")","v":""},null,{"$f":"IF(VALUE(L33),L33,IF(K33<>0,K33,\"\"))","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin1a_C0_4),(D_Gru_trin1a_J0_4+D_Gru_trin2a_Jg_2a_4)/(D_Gru_trin1a_Q0+D_Gru_trin2a_Qg_2a),\"\")","v":""},null,{"$f":"IF(VALUE(O33),O33,IF(N33<>0,N33,\"\"))","v":""},null,"B_Gru_trin2a_C2_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 2",null,null,{"$f":"IF(D_Gru_trin1a_Krit_1=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C0_1),IF(D_Gru_trin2a_C2_1>D_Gru_trin1a_Krit_1,D_Gru_trin2a_C2_1/D_Gru_trin1a_Krit_1,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F34),F34,IF(E34<>0,E34,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_2=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C0_2),IF(D_Gru_trin2a_C2_2>D_Gru_trin1a_Krit_2,D_Gru_trin2a_C2_2/D_Gru_trin1a_Krit_2,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I34),I34,IF(H34<>0,H34,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_3=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C0_3),IF(D_Gru_trin2a_C2_3>D_Gru_trin1a_Krit_3,D_Gru_trin2a_C2_3/D_Gru_trin1a_Krit_3,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L34),L34,IF(K34<>0,K34,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_4=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1a_C0_4),IF(D_Gru_trin2a_C2_4>D_Gru_trin1a_Krit_4,D_Gru_trin2a_C2_4/D_Gru_trin1a_Krit_4,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O34),O34,IF(N34<>0,N34,\"\"))","v":"Intet kriterie"},null,"B_Gru_trin2a_Krit_Overskr_n","beregnes"]
[]
[null,"GRUNDVAND (Kildestyrkekoncentration - trin1b+2b)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof2",null,null,"Stof3",null,null,"Sotf4",null,null,null,"Konstantnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes",null,"stof 1"]
[null,"Forureningskoncentration_C1_trin1b","C1b_n","mg/L",{"$f":"D_Gru_trin1b_C1bm_1*D_Gru_trin1b_l/0.25","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(E39),E39,\"\")","v":""},{"$f":"D_Gru_trin1b_C1bm_2*D_Gru_trin1b_l/0.25","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H39),H39,\"\")","v":""},{"$f":"D_Gru_trin1b_C1bm_3*D_Gru_trin1b_l/0.25","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K39),K39,\"\")","v":""},{"$f":"D_Gru_trin1b_C1bm_4*D_Gru_trin1b_l/0.25","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N39),N39,\"\")","v":""},null,"B_Gru_trin1b_C1b_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 1",null,null,{"$f":"IF(D_Gru_trin1a_Krit_1=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1b_C1b_1),IF(D_Gru_trin1b_C1b_1>D_Gru_trin1a_Krit_1,D_Gru_trin1b_C1b_1/D_Gru_trin1a_Krit_1,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F40),F40,IF(E40<>0,E40,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_2=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1b_C1b_2),IF(D_Gru_trin1b_C1b_2>D_Gru_trin1a_Krit_2,D_Gru_trin1b_C1b_2/D_Gru_trin1a_Krit_2,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I40),I40,IF(H40<>0,H40,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_3=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1b_C1b_3),IF(D_Gru_trin1b_C1b_3>D_Gru_trin1a_Krit_3,D_Gru_trin1b_C1b_3/D_Gru_trin1a_Krit_3,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L40),L40,IF(K40<>0,K40,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_4=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin1b_C1b_4),IF(D_Gru_trin1b_C1b_4>D_Gru_trin1a_Krit_4,D_Gru_trin1b_C1b_4/D_Gru_trin1a_Krit_4,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O40),O40,IF(N40<>0,N40,\"\"))","v":"Intet kriterie"},null,"B_Gru_trin1b_Krit_Overskr_n","beregnes"]
[null,"Forureningskoncentration_C2_trin2b","C2b_n","mg/L",{"$f":"D_Gru_trin1b_C1b_1*(D_Gru_dm_1a/D_Gru_trin2a_dm_2a)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(E41),E41,\"\")","v":""},{"$f":"D_Gru_trin1b_C1b_2*(D_Gru_dm_1a/D_Gru_trin2a_dm_2a)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H41),H41,\"\")","v":""},{"$f":"D_Gru_trin1b_C1b_3*(D_Gru_dm_1a/D_Gru_trin2a_dm_2a)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K41),K41,\"\")","v":""},{"$f":"D_Gru_trin1b_C1b_4*(D_Gru_dm_1a/D_Gru_trin2a_dm_2a)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N41),N41,\"\")","v":""},null,"B_Gru_trin2b_C2b_n","beregnes"]
[null,"Overskridelse af GV-krit for trin 2",null,null,{"$f":"IF(D_Gru_trin1a_Krit_1=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin2b_C2b_1),IF(D_Gru_trin2b_C2b_1>D_Gru_trin1a_Krit_1,D_Gru_trin2b_C2b_1/D_Gru_trin1a_Krit_1,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(F42),F42,IF(E42<>0,E42,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_2=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin2b_C2b_2),IF(D_Gru_trin2b_C2b_2>D_Gru_trin1a_Krit_2,D_Gru_trin2b_C2b_2/D_Gru_trin1a_Krit_2,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(I42),I42,IF(H42<>0,H42,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_3=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin2b_C2b_3),IF(D_Gru_trin2b_C2b_3>D_Gru_trin1a_Krit_3,D_Gru_trin2b_C2b_3/D_Gru_trin1a_Krit_3,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(L42),L42,IF(K42<>0,K42,\"\"))","v":"Intet kriterie"},{"$f":"IF(D_Gru_trin1a_Krit_4=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin2b_C2b_4),IF(D_Gru_trin2b_C2b_4>D_Gru_trin1a_Krit_4,D_Gru_trin2b_C2b_4/D_Gru_trin1a_Krit_4,\"nej\"),\"\"))","v":"Intet kriterie"},null,{"$f":"IF(VALUE(O42),O42,IF(N42<>0,N42,\"\"))","v":"Intet kriterie"},null,"B_Gru_trin2b_Krit_Overskr_n","beregnes"]
[]
[null,"GRUNDVAND (Konc. med sorption og nedbrydning - trin3)"]
[null,"Stoffer","Forkortelse","Enhed","Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4",null,null,null,"Konstantnavn","Oprindelsessted"]
[null,null,null,null,"Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes"]
[null,"Forureningskoncentration","C2_n","mg/L",{"$f":"IF(D_Gru_beregn=TRUE,D_Gru_trin2a_C2_1,IF(D_Gru_målt=TRUE,D_Gru_trin2b_C2b_1,))","v":""},null,{"$f":"IF(VALUE(F47),F47,IF(E47<>0,E47,\"\"))","v":""},{"$f":"IF(D_Gru_beregn=TRUE,D_Gru_trin2a_C2_2,IF(D_Gru_målt=TRUE,D_Gru_trin2b_C2b_2,))","v":""},null,{"$f":"IF(VALUE(I47),I47,IF(H47<>0,H47,\"\"))","v":""},{"$f":"IF(D_Gru_beregn=TRUE,D_Gru_trin2a_C2_3,IF(D_Gru_målt=TRUE,D_Gru_trin2b_C2b_3,))","v":""},null,{"$f":"IF(VALUE(L47),L47,IF(K47<>0,K47,\"\"))","v":""},{"$f":"IF(D_Gru_beregn=TRUE,D_Gru_trin2a_C2_4,IF(D_Gru_målt=TRUE,D_Gru_trin2b_C2b_4,))","v":""},null,{"$f":"IF(VALUE(O47),O47,IF(N47<>0,N47,\"\"))","v":""},null,"B_Gru_trin3_C2_n","beregnes"]
[null,"Fordelingskoefficienten","KD_n","-",{"$f":"10^D_Gru_trin3_logKD_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"10^D_Gru_trin3_logKD_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I48),I48,IF(H48<>0,H48,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"10^D_Gru_trin3_logKD_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L48),L48,IF(K48<>0,K48,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"10^D_Gru_trin3_logKD_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O48),O48,IF(N48<>0,N48,\"\"))","v":{"$error":"#VALUE!"}},null,"B_Gru_trin3_KB_n","beregnes"]
[null,"logKD","logKD",null,{"$f":"1.04*D_Gru_trin3_logKOW_1+LOG(D_Gru_foc)-0.84","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1.04*D_Gru_trin3_logKOW_2+LOG(D_Gru_foc)-0.84","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1.04*D_Gru_trin3_logKOW_3+LOG(D_Gru_foc)-0.84","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1.04*D_Gru_trin3_logKOW_4+LOG(D_Gru_foc)-0.84","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"B_Gru_trin3_logKB_n","beregnes"]
[null,"1. ordens nedbrydningskonstant","k1_n","dage-1",{"$f":"IF(D_Gru_aerob=TRUE,D_Gru_trin3_k1_aerob_1,IF(D_Gru_anaerob=TRUE,D_Gru_trin3_k1_anaerob_1,))","v":0},null,{"$f":"E50","v":0},{"$f":"IF(D_Gru_aerob=TRUE,D_Gru_trin3_k1_aerob_2,IF(D_Gru_anaerob=TRUE,D_Gru_trin3_k1_anaerob_2,))","v":0},null,{"$f":"H50","v":0},{"$f":"IF(D_Gru_aerob=TRUE,D_Gru_trin3_k1_aerob_3,IF(D_Gru_anaerob=TRUE,D_Gru_trin3_k1_anaerob_3,))","v":0},null,{"$f":"K50","v":0},{"$f":"IF(D_Gru_aerob=TRUE,D_Gru_trin3_k1_aerob_4,IF(D_Gru_anaerob=TRUE,D_Gru_trin3_k1_anaerob_4,))","v":0},null,{"$f":"N50","v":0},null,"B_Gru_trin3_k1_n","beregnes"]
[null,"Forureningskonc._C3_med nedbr.","ned_C3_n","mg/L",{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_1),D_Gru_trin3_C2_1*EXP(-D_Gru_trin3_k1_1*D_Gru_trin2a_t*365.25),\"\")","v":""},null,{"$f":"E51","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_2),D_Gru_trin3_C2_2*EXP(-D_Gru_trin3_k1_2*D_Gru_trin2a_t*365.25),\"\")","v":""},null,{"$f":"H51","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_3),D_Gru_trin3_C2_3*EXP(-D_Gru_trin3_k1_3*D_Gru_trin2a_t*365.25),\"\")","v":""},null,{"$f":"K51","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_4),D_Gru_trin3_C2_4*EXP(-D_Gru_trin3_k1_4*D_Gru_trin2a_t*365.25),\"\")","v":""},null,{"$f":"IF(ISNUMBER(N51),N51,\"\")","v":""},null,"B_Gru_trin3_ned_C3_n","beregnes"]
[null,"Forureningskonc._C3_med sorpt.+nedbryd","C3_n","mg/L",{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_1),D_Gru_trin3_C2_1*EXP(-D_Gru_trin3_k1_1*D_Gru_trin3_t_sorp_1),\"\")","v":""},null,{"$f":"IF(ISNUMBER(E52),E52,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_2),D_Gru_trin3_C2_2*EXP(-D_Gru_trin3_k1_2*D_Gru_trin3_t_sorp_2),\"\")","v":""},null,{"$f":"IF(ISNUMBER(H52),H52,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_3),D_Gru_trin3_C2_3*EXP(-D_Gru_trin3_k1_3*D_Gru_trin3_t_sorp_3),\"\")","v":""},null,{"$f":"IF(ISNUMBER(K52),K52,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Gru_trin3_C2_4),D_Gru_trin3_C2_4*EXP(-D_Gru_trin3_k1_4*D_Gru_trin3_t_sorp_4),\"\")","v":""},null,{"$f":"IF(ISNUMBER(N52),N52,\"\")","v":""},null,"B_Gru_trin3_C3_n","beregnes"]
[null,"Retardationsfaktor","R","-",{"$f":"1+D_Gru_rhob/D_Gru_trin3_eW*D_Gru_trin3_KD_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1+D_Gru_rhob/D_Gru_trin3_eW*D_Gru_trin3_KD_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1+D_Gru_rhob/D_Gru_trin3_eW*D_Gru_trin3_KD_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1+D_Gru_rhob/D_Gru_trin3_eW*D_Gru_trin3_KD_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"B_Gru_trin3_R_n","beregnes"]
[null,"Gns. porevandshastighed m. sorption","VS","m/år",{"$f":"D_Gru_trin2a_VP/D_Gru_trin3_R_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Gru_trin2a_VP/D_Gru_trin3_R_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Gru_trin2a_VP/D_Gru_trin3_R_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Gru_trin2a_VP/D_Gru_trin3_R_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"B_Gru_trin3_VS_n","beregnes"]
[null,"Transporttid med sorption","t_sorp","dage",{"$f":"D_Gru_trin1b_LL/D_Gru_trin3_VS_1*365.25","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Gru_trin1b_LL/D_Gru_trin3_VS_2*365.25","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Gru_trin1b_LL/D_Gru_trin3_VS_3*365.25","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Gru_trin1b_LL/D_Gru_trin3_VS_4*365.25","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"B_Gru_trin3_t_sorp_n","beregnes"]
[null,"Overskridelse af Gv-Krit for trin 3",null,null,{"$f":"IF(D_Gru_trin1a_Krit_1=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin3_C3_1),IF(D_Gru_trin3_C3_1>D_Gru_trin1a_Krit_1,D_Gru_trin3_C3_1/D_Gru_trin1a_Krit_1,\"nej\"),\"\"))","v":"Intet kriterie"},null,"Intet kriterie",{"$f":"IF(D_Gru_trin1a_Krit_2=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin3_C3_2),IF(D_Gru_trin3_C3_2>D_Gru_trin1a_Krit_2,D_Gru_trin3_C3_2/D_Gru_trin1a_Krit_2,\"nej\"),\"\"))","v":"Intet kriterie"},null,"Intet kriterie",{"$f":"IF(D_Gru_trin1a_Krit_3=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin3_C3_3),IF(D_Gru_trin3_C3_3>D_Gru_trin1a_Krit_3,D_Gru_trin3_C3_3/D_Gru_trin1a_Krit_3,\"nej\"),\"\"))","v":"Intet kriterie"},null,"Intet kriterie",{"$f":"IF(D_Gru_trin1a_Krit_4=\"\",\"Intet kriterie\",IF(ISNUMBER(D_Gru_trin3_C3_4),IF(D_Gru_trin3_C3_4>D_Gru_trin1a_Krit_4,D_Gru_trin3_C3_4/D_Gru_trin1a_Krit_4,\"nej\"),\"\"))","v":"Intet kriterie"},null,"Intet kriterie",null,"B_Gru_trin3_Krit_Overskr_n","beregnes"]
[]
[null,"Stof 1",{"$f":"D_Gru_stofnavn_1","v":""},null,{"$f":"D_Gru_stof1_Afstand_1_1","v":0},0,10,20,30,40,50,75,100]
[null,"Transporttid",null,null,{"$f":"D_Gru_stof1_Afstand_1_1/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_2/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_3/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_4/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_5/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_6/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_7/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_8/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_9/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},"B_Gru_stof1_AfstanB_2_n"]
[null,"Langsgående dispersivitet",null,null,{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_1,2)+0.0036*D_Gru_stof1_Afstand_1_1-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_1,2)+0.0036*D_Gru_stof1_Afstand_1_1-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_2,2)+0.0036*D_Gru_stof1_Afstand_1_2-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_2,2)+0.0036*D_Gru_stof1_Afstand_1_2-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_3,2)+0.0036*D_Gru_stof1_Afstand_1_3-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_3,2)+0.0036*D_Gru_stof1_Afstand_1_3-0.008))","v":2.8419999999999994E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_4,2)+0.0036*D_Gru_stof1_Afstand_1_4-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_4,2)+0.0036*D_Gru_stof1_Afstand_1_4-0.008))","v":6.5679999999999988E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_5,2)+0.0036*D_Gru_stof1_Afstand_1_5-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_5,2)+0.0036*D_Gru_stof1_Afstand_1_5-0.008))","v":0.10378000000000001},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_6,2)+0.0036*D_Gru_stof1_Afstand_1_6-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_6,2)+0.0036*D_Gru_stof1_Afstand_1_6-0.008))","v":0.14271999999999999},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_7,2)+0.0036*D_Gru_stof1_Afstand_1_7-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_7,2)+0.0036*D_Gru_stof1_Afstand_1_7-0.008))","v":0.1825},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_8,2)+0.0036*D_Gru_stof1_Afstand_1_8-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_8,2)+0.0036*D_Gru_stof1_Afstand_1_8-0.008))","v":0.28562500000000002},{"$f":"IF((0.0000042*POWER(D_Gru_stof1_Afstand_1_9,2)+0.0036*D_Gru_stof1_Afstand_1_9-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof1_Afstand_1_9,2)+0.0036*D_Gru_stof1_Afstand_1_9-0.008))","v":0.39399999999999996}]
[null,"Opblandingsdybde,m",null,null,{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*E60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_1)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*F60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_2)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*G60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_3)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*H60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_4)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*I60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_5)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*J60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_6)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*K60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_7)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*L60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_8)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*M60*D_Gru_trin2a_VP*D_Gru_stof1_Afstand_2_9)))","v":{"$error":"#VALUE!"}},"B_Gru_stof1_AfstanB_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_1*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_1*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_1))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_2*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_2*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_2))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_3*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_3*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_3))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_4*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_4*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_4))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_5*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_5*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_5))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_6*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_6*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_6))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_7*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_7*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_7))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_8*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_8*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_8))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_1),(D_Gru_trin1a_J0_1+D_Gru_B*D_Gru_stof1_Afstand_3_9*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_1)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof1_Afstand_3_9*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_1*(0.25/D_Gru_stof1_Afstand_3_9))","v":0},"B_Gru_stof1_AfstanB_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"D_Gru_stof1_Afstand_4_1*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_2*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_3*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_4*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_5*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_6*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_7*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_8*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_9*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_2_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof1_AfstanB_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"D_Gru_stof1_Afstand_1_1/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_2/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_3/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_4/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_5/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_6/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_7/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_8/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_1_9/D_Gru_trin3_VS_1","v":{"$error":"#VALUE!"}},"B_Gru_stof1_AfstanB_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,null,{"$f":"D_Gru_stof1_Afstand_4_1*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_2*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_3*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_4*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_5*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_6*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_7*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_8*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof1_Afstand_4_9*EXP(-D_Gru_trin3_k1_1*D_Gru_stof1_Afstand_6_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof1_AfstanB_7_n"]
[]
[]
[]
[]
[]
[]
[null,"Stof 2",{"$f":"D_Gru_stofnavn_2","v":""},null,{"$f":"Gru_afstand_bruger_2","v":0},0,10,20,30,40,50,75,100]
[null,"Transporttid",null,null,{"$f":"D_Gru_stof2_Afstand_1_1/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_2/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_3/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_4/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_5/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_6/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_7/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_8/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_9/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},"B_Gru_stof2_AfstanB_2_n"]
[null,"Langsgående dispersivitet",null,null,{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_1,2)+0.0036*D_Gru_stof2_Afstand_1_1-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_1,2)+0.0036*D_Gru_stof2_Afstand_1_1-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_2,2)+0.0036*D_Gru_stof2_Afstand_1_2-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_2,2)+0.0036*D_Gru_stof2_Afstand_1_2-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_3,2)+0.0036*D_Gru_stof2_Afstand_1_3-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_3,2)+0.0036*D_Gru_stof2_Afstand_1_3-0.008))","v":2.8419999999999994E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_4,2)+0.0036*D_Gru_stof2_Afstand_1_4-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_4,2)+0.0036*D_Gru_stof2_Afstand_1_4-0.008))","v":6.5679999999999988E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_5,2)+0.0036*D_Gru_stof2_Afstand_1_5-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_5,2)+0.0036*D_Gru_stof2_Afstand_1_5-0.008))","v":0.10378000000000001},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_6,2)+0.0036*D_Gru_stof2_Afstand_1_6-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_6,2)+0.0036*D_Gru_stof2_Afstand_1_6-0.008))","v":0.14271999999999999},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_7,2)+0.0036*D_Gru_stof2_Afstand_1_7-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_7,2)+0.0036*D_Gru_stof2_Afstand_1_7-0.008))","v":0.1825},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_8,2)+0.0036*D_Gru_stof2_Afstand_1_8-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_8,2)+0.0036*D_Gru_stof2_Afstand_1_8-0.008))","v":0.28562500000000002},{"$f":"IF((0.0000042*POWER(D_Gru_stof2_Afstand_1_9,2)+0.0036*D_Gru_stof2_Afstand_1_9-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof2_Afstand_1_9,2)+0.0036*D_Gru_stof2_Afstand_1_9-0.008))","v":0.39399999999999996}]
[null,"Opblandingsdybde,m",null,null,{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*E74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_1)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*F74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_2)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*G74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_3)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*H74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_4)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*I74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_5)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*J74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_6)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*K74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_7)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*L74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_8)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*M74*D_Gru_trin2a_VP*D_Gru_stof2_Afstand_2_9)))","v":{"$error":"#VALUE!"}},"B_Gru_stof2_AfstanB_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_1*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_1*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_1))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_2*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_2*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_2))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_3*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_3*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_3))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_4*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_4*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_4))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_5*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_5*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_5))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_6*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_6*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_6))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_7*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_7*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_7))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_8*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_8*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_8))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_2),(D_Gru_trin1a_J0_2+D_Gru_B*D_Gru_stof2_Afstand_3_9*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_2)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof2_Afstand_3_9*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_2*(0.25/D_Gru_stof2_Afstand_3_9))","v":0},"B_Gru_stof2_AfstanB_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"D_Gru_stof2_Afstand_4_1*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_2*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_3*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_4*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_5*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_6*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_7*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_8*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_9*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_2_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof2_AfstanB_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"D_Gru_stof2_Afstand_1_1/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_2/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_3/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_4/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_5/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_6/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_7/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_8/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_1_9/D_Gru_trin3_VS_2","v":{"$error":"#VALUE!"}},"B_Gru_stof2_AfstanB_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,null,{"$f":"D_Gru_stof2_Afstand_4_1*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_2*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_3*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_4*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_5*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_6*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_7*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_8*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof2_Afstand_4_9*EXP(-D_Gru_trin3_k1_2*D_Gru_stof2_Afstand_6_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof2_AfstanB_7_n"]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 3",{"$f":"D_Gru_stofnavn_3","v":""},null,{"$f":"Gru_Afstand_bruger_3","v":0},0,10,20,30,40,50,75,100]
[null,"Transporttid",null,null,{"$f":"D_Gru_stof3_Afstand_1_1/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_2/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_3/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_4/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_5/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_6/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_7/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_8/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_9/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},"B_Gru_stof3_AfstanB_2_n"]
[null,"Langsgående dispersivitet",null,null,{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_1,2)+0.0036*D_Gru_stof3_Afstand_1_1-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_1,2)+0.0036*D_Gru_stof3_Afstand_1_1-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_2,2)+0.0036*D_Gru_stof3_Afstand_1_2-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_2,2)+0.0036*D_Gru_stof3_Afstand_1_2-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_3,2)+0.0036*D_Gru_stof3_Afstand_1_3-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_3,2)+0.0036*D_Gru_stof3_Afstand_1_3-0.008))","v":2.8419999999999994E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_4,2)+0.0036*D_Gru_stof3_Afstand_1_4-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_4,2)+0.0036*D_Gru_stof3_Afstand_1_4-0.008))","v":6.5679999999999988E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_5,2)+0.0036*D_Gru_stof3_Afstand_1_5-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_5,2)+0.0036*D_Gru_stof3_Afstand_1_5-0.008))","v":0.10378000000000001},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_6,2)+0.0036*D_Gru_stof3_Afstand_1_6-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_6,2)+0.0036*D_Gru_stof3_Afstand_1_6-0.008))","v":0.14271999999999999},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_7,2)+0.0036*D_Gru_stof3_Afstand_1_7-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_7,2)+0.0036*D_Gru_stof3_Afstand_1_7-0.008))","v":0.1825},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_8,2)+0.0036*D_Gru_stof3_Afstand_1_8-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_8,2)+0.0036*D_Gru_stof3_Afstand_1_8-0.008))","v":0.28562500000000002},{"$f":"IF((0.0000042*POWER(D_Gru_stof3_Afstand_1_9,2)+0.0036*D_Gru_stof3_Afstand_1_9-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof3_Afstand_1_9,2)+0.0036*D_Gru_stof3_Afstand_1_9-0.008))","v":0.39399999999999996}]
[null,"Opblandingsdybde,m",null,null,{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*E89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_1)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*F89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_2)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*G89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_3)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*H89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_4)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*I89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_5)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*J89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_6)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*K89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_7)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*L89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_8)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*M89*D_Gru_trin2a_VP*D_Gru_stof3_Afstand_2_9)))","v":{"$error":"#VALUE!"}},"B_Gru_stof3_AfstanB_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_1*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_1*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_1))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_2*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_2*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_2))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_3*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_3*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_3))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_4*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_4*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_4))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_5*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_5*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_5))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_6*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_6*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_6))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_7*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_7*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_7))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_8*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_8*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_8))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_3),(D_Gru_trin1a_J0_3+D_Gru_B*D_Gru_stof3_Afstand_3_9*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_3)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof3_Afstand_3_9*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_3*(0.25/D_Gru_stof3_Afstand_3_9))","v":0},"B_Gru_stof3_AfstanB_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"D_Gru_stof3_Afstand_4_1*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_2*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_3*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_4*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_5*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_6*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_7*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_8*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_9*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_2_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof3_AfstanB_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"D_Gru_stof3_Afstand_1_1/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_2/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_3/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_4/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_5/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_6/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_7/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_8/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_1_9/D_Gru_trin3_VS_3","v":{"$error":"#VALUE!"}},"B_Gru_stof3_AfstanB_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,null,{"$f":"D_Gru_stof3_Afstand_4_1*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_2*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_3*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_4*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_5*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_6*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_7*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_8*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof3_Afstand_4_9*EXP(-D_Gru_trin3_k1_3*D_Gru_stof3_Afstand_6_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof3_AfstanB_7_n"]
[]
[]
[]
[]
[]
[]
[null,"Stof 4",{"$f":"D_Gru_stofnavn_4","v":""},null,{"$f":"Gru_afstand_bruger_4","v":0},0,10,20,30,40,50,75,100]
[null,"Transporttid",null,null,{"$f":"D_Gru_stof4_Afstand_1_1/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_2/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_3/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_4/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_5/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_6/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_7/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_8/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_9/D_Gru_trin2a_VP","v":{"$error":"#VALUE!"}},"B_Gru_stof4_AfstanB_2_n"]
[null,"Langsgående dispersivitet",null,null,{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_1,2)+0.0036*D_Gru_stof4_Afstand_1_1-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_1,2)+0.0036*D_Gru_stof4_Afstand_1_1-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_2,2)+0.0036*D_Gru_stof4_Afstand_1_2-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_2,2)+0.0036*D_Gru_stof4_Afstand_1_2-0.008))","v":9.9999999999999994E-37},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_3,2)+0.0036*D_Gru_stof4_Afstand_1_3-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_3,2)+0.0036*D_Gru_stof4_Afstand_1_3-0.008))","v":2.8419999999999994E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_4,2)+0.0036*D_Gru_stof4_Afstand_1_4-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_4,2)+0.0036*D_Gru_stof4_Afstand_1_4-0.008))","v":6.5679999999999988E-2},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_5,2)+0.0036*D_Gru_stof4_Afstand_1_5-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_5,2)+0.0036*D_Gru_stof4_Afstand_1_5-0.008))","v":0.10378000000000001},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_6,2)+0.0036*D_Gru_stof4_Afstand_1_6-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_6,2)+0.0036*D_Gru_stof4_Afstand_1_6-0.008))","v":0.14271999999999999},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_7,2)+0.0036*D_Gru_stof4_Afstand_1_7-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_7,2)+0.0036*D_Gru_stof4_Afstand_1_7-0.008))","v":0.1825},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_8,2)+0.0036*D_Gru_stof4_Afstand_1_8-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_8,2)+0.0036*D_Gru_stof4_Afstand_1_8-0.008))","v":0.28562500000000002},{"$f":"IF((0.0000042*POWER(D_Gru_stof4_Afstand_1_9,2)+0.0036*D_Gru_stof4_Afstand_1_9-0.008)<0,1E-36,(0.0000042*POWER(D_Gru_stof4_Afstand_1_9,2)+0.0036*D_Gru_stof4_Afstand_1_9-0.008))","v":0.39399999999999996}]
[null,"Opblandingsdybde,m",null,null,{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*E103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_1)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*F103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_2)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*G103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_3)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*H103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_4)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*I103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_5)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*J103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_6)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*K103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_7)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*L103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_8)))","v":{"$error":"#VALUE!"}},{"$f":"MAX(D_Gru_dm_1a,MIN(IF(D_Gru_trin2a_dm_max>0,D_Gru_trin2a_dm_max,1E+36),SQRT((72/900)*M103*D_Gru_trin2a_VP*D_Gru_stof4_Afstand_2_9)))","v":{"$error":"#VALUE!"}},"B_Gru_stof4_AfstanB_3_n"]
[null,"Forureningskoncentration, C2",null,null,{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_1*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_1*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_1))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_2*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_2*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_2))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_3*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_3*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_3))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_4*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_4*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_4))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_5*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_5*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_5))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_6*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_6*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_6))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_7*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_7*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_7))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_8*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_8*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_8))","v":0},{"$f":"IF(D_Gru_beregn=TRUE,IF(ISNUMBER(D_Gru_trin1a_J0_4),(D_Gru_trin1a_J0_4+D_Gru_B*D_Gru_stof4_Afstand_3_9*D_Gru_trin1a_VD*D_Gru_trin1a_Cg_4)/(D_Gru_trin1a_Q0+D_Gru_B*D_Gru_stof4_Afstand_3_9*D_Gru_trin1a_VD),0),D_Gru_trin1b_C1b_4*(0.25/D_Gru_stof4_Afstand_3_9))","v":0},"B_Gru_stof4_AfstanB_4_n"]
[null,"Konc. med nedbrydning, C3",null,null,{"$f":"D_Gru_stof4_Afstand_4_1*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_2*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_3*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_4*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_5*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_6*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_7*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_8*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_9*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_2_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof4_AfstanB_5_n"]
[null,"Transporttid (sorpt.)",null,null,{"$f":"D_Gru_stof4_Afstand_1_1/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_2/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_3/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_4/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_5/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_6/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_7/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_8/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_1_9/D_Gru_trin3_VS_4","v":{"$error":"#VALUE!"}},"B_Gru_stof4_AfstanB_6_n"]
[null,"Konc. m. sorpt. og nedbr., C3",null,null,{"$f":"D_Gru_stof4_Afstand_4_1*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_1*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_2*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_2*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_3*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_3*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_4*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_4*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_5*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_5*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_6*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_6*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_7*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_7*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_8*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_8*365.25)","v":{"$error":"#VALUE!"}},{"$f":"D_Gru_stof4_Afstand_4_9*EXP(-D_Gru_trin3_k1_4*D_Gru_stof4_Afstand_6_9*365.25)","v":{"$error":"#VALUE!"}},"B_Gru_stof4_AfstanB_7_n"]
[]
[null,"Bemærkninger"]
[null,"Det forurenede område:"]
[null,null,"D_Gru_DFO_Com"]
[null,"Magasin:"]
[null,null,"D_Gru_Mag_Com"]
[null,"Forurening:"]
[null,null,"D_Gru_For_Com"]
[null,"Beregning:"]
[null,null,"D_Gru_Ber_Com"]

{"sheet":"Udskrift_Grundvand","index":13,"n_rows":181,"n_cols":18,"rows_kept":181,"cut":false,"hidden":true,"merged":[[135,1,135,10],[24,4,24,5],[25,4,25,5],[32,6,32,7],[32,2,32,3],[32,4,32,5],[35,4,35,5],[27,4,27,5],[33,2,34,3],[60,2,60,3],[65,6,65,7],[65,8,65,9],[74,1,85,9],[87,1,98,9],[37,8,37,9],[38,6,38,7],[38,2,38,3],[38,4,38,5],[36,2,36,3],[60,8,60,9],[60,6,60,7],[60,4,60,5],[55,2,55,5],[35,8,35,9],[4,8,4,10],[3,8,3,10],[2,8,2,10],[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,10],[7,0,7,1],[11,2,11,3],[12,2,12,3],[16,5,16,7],[21,2,21,3],[21,4,21,5],[11,7,11,8],[43,6,43,7],[46,6,46,7],[113,1,123,9],[64,2,64,3],[33,8,34,9],[32,8,32,9],[36,4,36,5],[36,8,36,9],[15,5,15,7],[15,2,15,4],[16,2,16,4],[20,2,20,5],[37,6,37,7],[38,8,38,9],[43,4,43,5],[25,2,25,3],[22,2,22,3],[22,4,22,5],[23,2,23,3],[150,1,150,10],[42,8,42,9],[48,2,48,3],[48,4,48,5],[42,6,42,7],[42,4,42,5],[46,8,46,9],[46,2,46,3],[44,2,44,3],[45,2,45,3],[44,4,44,5],[44,6,44,7],[44,8,44,9],[45,4,45,5],[45,6,45,7],[45,8,45,9],[64,6,64,7],[64,8,64,9],[65,2,65,3],[65,4,65,5],[46,4,46,5],[42,2,42,3],[43,8,43,9],[43,2,43,3],[165,1,165,10],[180,1,180,10],[26,4,26,5],[125,1,133,9],[50,2,50,3],[50,4,50,5],[50,6,50,7],[50,8,50,9],[63,6,63,7],[51,2,51,3],[100,1,111,9],[63,8,63,9],[51,8,51,9],[64,4,64,5],[63,2,63,3],[63,4,63,5],[55,0,55,1],[36,6,36,7],[49,2,49,3],[49,4,49,5],[61,2,61,3],[61,4,61,5],[61,6,61,7],[61,8,61,9],[35,6,35,7],[23,4,23,5],[24,2,24,3],[62,2,62,3],[62,4,62,5],[62,6,62,7],[62,8,62,9],[33,4,34,5],[33,6,34,7],[27,2,27,3],[35,2,35,3],[51,4,51,5],[51,6,51,7],[49,6,49,7],[49,8,49,9],[48,6,48,7],[48,8,48,9],[37,2,37,3],[37,4,37,5],[28,2,28,3],[29,2,29,3]]}
["Grundvand"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
[]
["Det forurenede område"]
["Kommentar",{"$f":"IF( D_Gru_DFO_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Beregningstypen",null,{"$f":"IF( D_Gru_beregn,\"A: Beregnet koncentration\",\"B: Målt koncentration\")","v":"A: Beregnet koncentration"}]
[]
["Areal af det forurenede område","A",{"$f":"IF(D_Gru_målt,\"\",(IF(Gru_Y<>\"\",D_Gru_A,\"\")))","v":""},null,"m²","Filterlængde    l",null,{"$f":"IF(D_Gru_målt,(IF(Gru_FilterL<>\"\",Gru_FilterL,\"\")),\"\")","v":""},null,"m"]
["Bredde af det forurenede område","B",{"$f":"IF(D_Gru_målt,\"\",(IF(Gru_X<>\"\",Gru_X,\"\")))","v":""},null,"m"]
[]
[null,null,"Standard data",null,"Indtastede data (angives med fed)"]
["Nettonedbør","N",{"$f":"IF(D_Gru_målt,\"\",(IF(D_Gru_N_syst<>\"\",D_Gru_N_syst,\"\")))","v":""},null,null,{"$f":"IF(D_Gru_målt,\"\",(IF(Gru_My_Nedbør<>\"\",Gru_My_Nedbør,\"\")))","v":""},null,null,"mm/år"]
["Kommune/Egn",null,{"$f":"IF(D_Gru_målt,\"\",(IF(D_Gru_Kommune_syst<>\"\",D_Gru_Kommune_syst,\"\")))","v":""},null,null,{"$f":"IF(D_Gru_målt,\"\",(IF(Gru_My_Kommune<>\"\",Gru_My_Kommune,\"\")))","v":""}]
[]
["Det først betydende magasin"]
["Kommentar",{"$f":"IF( D_Gru_Mag_ComUds,\"ja\",\"nej\")","v":"nej"},"Standard data",null,"Indtastede data (angives med fed)"]
["Aguifer",null,{"$f":"D_Gru_Aqui","v":""}]
["Effektiv porøsitet","eeff",{"$f":"IF(D_Gru_trin2a_eeff_syst<>\"\",D_Gru_trin2a_eeff_syst,\"\")","v":""},null,{"$f":"IF(Gru_My_eff<>\"\",Gru_My_eff,\"\")","v":""}]
["Porøsitet, vandmættet ","eW",{"$f":"IF(D_Gru_trin3_eW_syst<>\"\",D_Gru_trin3_eW_syst,\"\")","v":""},null,{"$f":"IF(Gru_My_ew<>\"\",Gru_My_ew,\"\")","v":""}]
["Bulkmassefylde","(rho)b",{"$f":"IF(D_Gru_rhob_syst<>\"\",D_Gru_rhob_syst,\"\")","v":""},null,{"$f":"IF(Gru_My_p<>\"\",Gru_My_p,\"\")","v":""},null,"kg/l"]
["% organisk indhold","foc",{"$f":"IF(D_Gru_foc_syst<>\"\",D_Gru_foc_syst,\"\")","v":""},null,{"$f":"IF(Gru_My_foc<>\"\",Gru_My_foc,\"\")","v":""}]
["Tykkelse af GV-magasin","dm_max",null,null,{"$f":"IF(Gru_maxdm<>\"\",Gru_maxdm,\"\")","v":""},null,"m"]
["Hydraulisk gradient","i",null,null,{"$f":"IF(Gru_i<>\"\",Gru_i,\"\")","v":""},null,"m/m"]
["Hydraulisk ledningsevne","k",{"$f":"IF(D_Gru_trin1a_k_syst<>\"\",D_Gru_trin1a_k_syst,\"\")","v":""},null,{"$f":"IF(Gru_My_k<>\"\",Gru_My_k,\"\")","v":""},null,"m/s"]
["Gns. Porevandshastighed","Vp",{"$f":"IF(D_Gru_trin2a_VP<>\"\",D_Gru_trin2a_VP,\"\")","v":{"$error":"#VALUE!"}},null,null,null,"m/år"]
["Beregningspunkt","L",{"$f":"IF(D_Gru_trin1b_LL<>\"\",D_Gru_trin1b_LL,\"\")","v":{"$error":"#VALUE!"}},null,null,null,"m"]
[]
["Stoffer og stofegenskaber"]
["Kommentar",{"$f":"IF( D_Gru_For_ComUds,\"ja\",\"nej\")","v":"nej"},"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
["Forureningskomponent",null,{"$f":"D_Gru_stofnavn_1","v":""},null,{"$f":"D_Gru_stofnavn_2","v":""},null,{"$f":"D_Gru_stofnavn_3","v":""},null,{"$f":"D_Gru_stofnavn_4","v":""},null,null,null,null,{"$f":"C34","v":""},{"$f":"E34","v":""},{"$f":"G34","v":""},{"$f":"I34","v":""}]
[]
["Målepunkt",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""},null,null,null,null,{"$f":"C36","v":""},{"$f":"E36","v":""},{"$f":"G36","v":""},{"$f":"I36","v":""}]
["Dato",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
["Målt GV-koncentration",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(Enk_My_CV_1>0,Enk_My_CV_1,\"\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(Enk_My_CV_2>0,Enk_My_CV_2,\"\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(Enk_My_CV_3>0,Enk_My_CV_3,\"\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(Enk_My_CV_4>0,Enk_My_CV_4,\"\"),\"\")","v":""},null,"mg/l"]
["Baggrundskoncentration",null,{"$f":"IF(Gru_Trin1a_my_Cg_1<>\"\",Gru_Trin1a_my_Cg_1,\"\")","v":""},null,{"$f":"IF(Gru_Trin1a_my_Cg_2<>\"\",Gru_Trin1a_my_Cg_2,\"\")","v":""},null,{"$f":"IF(Gru_Trin1a_my_Cg_3<>\"\",Gru_Trin1a_my_Cg_3,\"\")","v":""},null,{"$f":"IF(Gru_Trin1a_my_Cg_4<>\"\",Gru_Trin1a_my_Cg_4,\"\")","v":""},null,"mg/l"]
[]
["Beregning: Grundvand",null,"Angiv signifikant ciffer",null,3]
[]
["Kommentar",{"$f":"IF( D_Gru_Ber_ComUds,\"ja\",\"nej\")","v":"nej"},"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
["Kildestyrken anvendt i beregning",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",(IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C0_1,IF(D_Gru_målt=TRUE,D_Gru_trin1b_C1bm_1))),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",(IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C0_2,IF(D_Gru_målt=TRUE,D_Gru_trin1b_C1bm_2))),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",(IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C0_3,IF(D_Gru_målt=TRUE,D_Gru_trin1b_C1bm_3))),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",(IF(D_Gru_beregn=TRUE,D_Gru_trin1a_C0_4,IF(D_Gru_målt=TRUE,D_Gru_trin1b_C1bm_4))),\"\")","v":""},null,"mg/l",null,"Kildestyrken",{"$f":"C44*1000000","v":{"$error":"#VALUE!"}},{"$f":"E44*1000000","v":{"$error":"#VALUE!"}},{"$f":"G44*1000000","v":{"$error":"#VALUE!"}},{"$f":"I44*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
["Beregnet værdi anvendt",null,{"$f":"IF(ISNUMBER(C44),IF(OR(C46=\"ja\",C47=\"ja\",(ISNUMBER(Enk_My_CV_1))),\"nej\",\"ja\"),\"\")","v":""},null,{"$f":"IF(ISNUMBER(E44),IF(OR(E46=\"ja\",E47=\"ja\",(ISNUMBER(Enk_My_CV_2))),\"nej\",\"ja\"),\"\")","v":""},null,{"$f":"IF(ISNUMBER(G44),IF(OR(G46=\"ja\",G47=\"ja\",(ISNUMBER(Enk_My_CV_3))),\"nej\",\"ja\"),\"\")","v":""},null,{"$f":"IF(ISNUMBER(I44),IF(OR(I46=\"ja\",I47=\"ja\",(ISNUMBER(Enk_My_CV_4))),\"nej\",\"ja\"),\"\")","v":""}]
[{"$f":"IF(C46=\"Ja\",CONCATENATE(\"Værdier fra \",D_ver_model), \"Værdien fra vertikaltransport anvendt\")","v":"Værdien fra vertikaltransport anvendt"},null,{"$f":"IF(D_Gru_målt=TRUE,\"nej\",IF(OR(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_temp3_TrueFalse=TRUE,),\"Ja\",\"Nej\"))","v":"Nej"},null,{"$f":"IF(D_Gru_målt=TRUE,\"nej\",IF(OR(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_temp3_TrueFalse=TRUE,),\"Ja\",\"Nej\"))","v":"Nej"},null,{"$f":"IF(D_Gru_målt=TRUE,\"nej\",IF(OR(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_temp3_TrueFalse=TRUE,),\"Ja\",\"Nej\"))","v":"Nej"},null,{"$f":"IF(D_Gru_målt=TRUE,\"nej\",IF(OR(D_Gru_trin1a_temp2_TrueFalse=TRUE,D_Gru_trin1a_temp3_TrueFalse=TRUE,),\"Ja\",\"Nej\"))","v":"Nej"}]
["Testværdi anvendt",null,{"$f":"IF(ISNUMBER(C44),IF(D_Gru_målt=TRUE,(IF(ISNUMBER(Gru_My_C1bm_1),\"ja\",\"nej\")),(IF(AND(D_Gru_trin1a_temp4_TrueFalse=TRUE),\"ja\",\"nej\"))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(E44),IF(D_Gru_målt=TRUE,(IF(ISNUMBER(Gru_My_C1bm_2),\"ja\",\"nej\")),(IF(AND(D_Gru_trin1a_temp4_TrueFalse=TRUE),\"ja\",\"nej\"))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(G44),IF(D_Gru_målt=TRUE,(IF(ISNUMBER(Gru_My_C1bm_3),\"ja\",\"nej\")),(IF(AND(D_Gru_trin1a_temp4_TrueFalse=TRUE),\"ja\",\"nej\"))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(I44),IF(D_Gru_målt=TRUE,(IF(ISNUMBER(Gru_My_C1bm_4),\"ja\",\"nej\")),(IF(AND(D_Gru_trin1a_temp4_TrueFalse=TRUE),\"ja\",\"nej\"))),\"\")","v":""}]
["Grundvandskvalitetskriterie",null,{"$f":"IF(D_Enk_GV_krit_syst_1<>\"\",D_Enk_GV_krit_syst_1/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_1<>\"\",Enk_My_GV_krit_1/1000,\"\")","v":""},{"$f":"IF(D_Enk_GV_krit_syst_2<>\"\",D_Enk_GV_krit_syst_2/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_2<>\"\",Enk_My_GV_krit_2/1000,\"\")","v":""},{"$f":"IF(D_Enk_GV_krit_syst_3<>\"\",D_Enk_GV_krit_syst_3/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_3<>\"\",Enk_My_GV_krit_3/1000,\"\")","v":""},{"$f":"IF(D_Enk_GV_krit_syst_4<>\"\",D_Enk_GV_krit_syst_4/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_4<>\"\",Enk_My_GV_krit_4/1000,\"\")","v":""},"mg/l"]
["Grundvandskoncentration: Trin 1",null,{"$f":"IF(ISNUMBER(D_gru_trin1_GVkonc_1),ROUND(D_gru_trin1_GVkonc_1,Gru_ciffer-(INT(LOG(D_gru_trin1_GVkonc_1))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_gru_trin1_GVkonc_2),ROUND(D_gru_trin1_GVkonc_2,Gru_ciffer-(INT(LOG(D_gru_trin1_GVkonc_2))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin1_GVkonc_3),ROUND(D_Gru_trin1_GVkonc_3,Gru_ciffer-(INT(LOG(D_Gru_trin1_GVkonc_3))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_gru_trin1_GVKonc_4),ROUND(D_gru_trin1_GVKonc_4,Gru_ciffer-(INT(LOG(D_gru_trin1_GVKonc_4))+1)),\"\")","v":""},null,"mg/l",null,"Trin 1-beregning",{"$f":"C49*1000000","v":{"$error":"#VALUE!"}},{"$f":"E49*1000000","v":{"$error":"#VALUE!"}},{"$f":"G49*1000000","v":{"$error":"#VALUE!"}},{"$f":"I49*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
["Overskridelse af kriteriet Trin 1",null,{"$f":"IF(D_Gru_trin1_oversk_1<>\"\",IF(ISNUMBER(D_Gru_trin1_oversk_1),ROUND(D_Gru_trin1_oversk_1,Gru_ciffer-(INT(LOG(D_Gru_trin1_oversk_1))+1)),D_Gru_trin1_oversk_1),\"\")","v":""},null,{"$f":"IF(D_Gru_trin1_oversk_2<>\"\",IF(ISNUMBER(D_Gru_trin1_oversk_2),ROUND(D_Gru_trin1_oversk_2,Gru_ciffer-(INT(LOG(D_Gru_trin1_oversk_2))+1)),D_Gru_trin1_oversk_2),\"\")","v":""},null,{"$f":"IF(D_gru_trin1_oversk_3<>\"\",IF(ISNUMBER(D_gru_trin1_oversk_3),ROUND(D_gru_trin1_oversk_3,Gru_ciffer-(INT(LOG(D_gru_trin1_oversk_3))+1)),D_gru_trin1_oversk_3),\"\")","v":""},null,{"$f":"IF(D_Gru_trin1_oversk_4<>\"\",IF(ISNUMBER(D_Gru_trin1_oversk_4),ROUND(D_Gru_trin1_oversk_4,Gru_ciffer-(INT(LOG(D_Gru_trin1_oversk_4))+1)),D_Gru_trin1_oversk_4),\"\")","v":""}]
["Grundvandskoncentration: Trin 2",null,{"$f":"IF(ISNUMBER(D_Gru_Trin2_GVKonc_1),ROUND(D_Gru_Trin2_GVKonc_1,Gru_ciffer-(INT(LOG(D_Gru_Trin2_GVKonc_1))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_Trin2_GVKonc_2),ROUND(D_Gru_Trin2_GVKonc_2,Gru_ciffer-(INT(LOG(D_Gru_Trin2_GVKonc_2))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_Trin2_GVKonc_3),ROUND(D_Gru_Trin2_GVKonc_3,Gru_ciffer-(INT(LOG(D_Gru_Trin2_GVKonc_3))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_Trin2_GVKonc_4),ROUND(D_Gru_Trin2_GVKonc_4,Gru_ciffer-(INT(LOG(D_Gru_Trin2_GVKonc_4))+1)),\"\")","v":""},null,"mg/l",null,"Trin 2-beregning",{"$f":"C51*1000000","v":{"$error":"#VALUE!"}},{"$f":"E51*1000000","v":{"$error":"#VALUE!"}},{"$f":"G51*1000000","v":{"$error":"#VALUE!"}},{"$f":"I51*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
["Overskridelse af kriteriet Trin 2",null,{"$f":"IF(D_gru_trin2_overskr_1<>\"\",IF(ISNUMBER(D_gru_trin2_overskr_1),(ROUND(D_gru_trin2_overskr_1,Gru_ciffer-(INT(LOG(D_gru_trin2_overskr_1))+1))),D_gru_trin2_overskr_1),\"\")","v":""},null,{"$f":"IF(D_Gru_trin2_overskr_2<>\"\",IF(ISNUMBER(D_Gru_trin2_overskr_2),(ROUND(D_Gru_trin2_overskr_2,Gru_ciffer-(INT(LOG(D_Gru_trin2_overskr_2))+1))),D_Gru_trin2_overskr_2),\"\")","v":""},null,{"$f":"IF(D_Gru_trin2_overskr_3<>\"\",IF(ISNUMBER(D_Gru_trin2_overskr_3),(ROUND(D_Gru_trin2_overskr_3,Gru_ciffer-(INT(LOG(D_Gru_trin2_overskr_3))+1))),D_Gru_trin2_overskr_3),\"\")","v":""},null,{"$f":"IF(D_Gru_trin2_overskr_4<>\"\",IF(ISNUMBER(D_Gru_trin2_overskr_4),(ROUND(D_Gru_trin2_overskr_4,Gru_ciffer-(INT(LOG(D_Gru_trin2_overskr_4))+1))),D_Gru_trin2_overskr_4),\"\")","v":""}]
[]
["Trin 3  inklusive sorption og nedbryding"]
[]
["Nedbrydningsforhold:",null,{"$f":"IF( D_Gru_aerob,\"Aerobe forhold\",\"Anaerobe forhold\")","v":"Aerobe forhold"}]
[]
["1. ordens nedbrydningskonst. aerob",null,{"$f":"IF(D_Enk_k1aerob_syst_1<>\"\",D_Enk_k1aerob_syst_1,\"\")","v":""},{"$f":"IF(Enk_MY_k1aerob_1<>\"\",Enk_MY_k1aerob_1,\"\")","v":""},{"$f":"IF(D_Enk_k1aerob_syst_2<>\"\",D_Enk_k1aerob_syst_2,\"\")","v":""},{"$f":"IF(Enk_MY_k1aerob_2<>\"\",Enk_MY_k1aerob_2,\"\")","v":""},{"$f":"IF(D_Enk_k1aerob_syst_3<>\"\",D_Enk_k1aerob_syst_3,\"\")","v":""},{"$f":"IF(Enk_MY_k1aerob_3<>\"\",Enk_MY_k1aerob_3,\"\")","v":""},{"$f":"IF(D_Enk_k1aerob_syst_4<>\"\",D_Enk_k1aerob_syst_4,\"\")","v":""},{"$f":"IF(Enk_MY_k1aerob_4<>\"\",Enk_MY_k1aerob_4,\"\")","v":""},"dage-1"]
["1. ordens nedbrydningskonst. anaerob",null,{"$f":"IF(D_Enk_k1anaerob_syst_1<>\"\",D_Enk_k1anaerob_syst_1,\"\")","v":""},{"$f":"IF(Enk_MY_k1anaerob_1<>\"\",Enk_MY_k1anaerob_1,\"\")","v":""},{"$f":"IF(D_Enk_k1anaerob_syst_2<>\"\",D_Enk_k1anaerob_syst_2,\"\")","v":""},{"$f":"IF(Enk_MY_k1anaerob_2<>\"\",Enk_MY_k1anaerob_2,\"\")","v":""},{"$f":"IF(D_Enk_k1anaerob_syst_3<>\"\",D_Enk_k1anaerob_syst_3,\"\")","v":""},{"$f":"IF(Enk_MY_k1anaerob_3<>\"\",Enk_MY_k1anaerob_3,\"\")","v":""},{"$f":"IF(D_Enk_k1anaerob_syst_4<>\"\",D_Enk_k1anaerob_syst_4,\"\")","v":""},{"$f":"IF(Enk_MY_k1anaerob_4<>\"\",Enk_MY_k1anaerob_4,\"\")","v":""},"dage-1"]
["log kOW",null,{"$f":"IF(D_Enk_KOW_syst_1<>\"\",D_Enk_KOW_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_KOW_1<>\"\",Enk_My_KOW_1,\"\")","v":""},{"$f":"IF(D_Enk_KOW_syst_2<>\"\",D_Enk_KOW_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_KOW_2<>\"\",Enk_My_KOW_2,\"\")","v":""},{"$f":"IF(D_Enk_KOW_syst_3<>\"\",D_Enk_KOW_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_KOW_3<>\"\",Enk_My_KOW_3,\"\")","v":""},{"$f":"IF(D_Enk_KOW_syst_4<>\"\",D_Enk_KOW_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_KOW_4<>\"\",Enk_My_KOW_4,\"\")","v":""}]
["Retardationskoefficient",null,{"$f":"D_Gru_trin3_R_1","v":""},null,{"$f":"D_Gru_trin3_R_2","v":""},null,{"$f":"D_Gru_trin3_R_3","v":""},null,{"$f":"D_Gru_trin3_R_4","v":""}]
["Forureningsflux vertikal (Trin 1a)",null,{"$f":"IF(ISNUMBER(D_gru_trin3_fluxvert_1),IF(D_gru_trin3_fluxvert_1<>0,ROUND(D_gru_trin3_fluxvert_1,2-INT((LOG(D_gru_trin3_fluxvert_1))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_gru_trin3_fluxvert_2),IF(D_gru_trin3_fluxvert_2<>0,ROUND(D_gru_trin3_fluxvert_2,2-INT((LOG(D_gru_trin3_fluxvert_2))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_gru_trin3_fluxvert_3),IF(D_gru_trin3_fluxvert_3<>0,ROUND(D_gru_trin3_fluxvert_3,2-INT((LOG(D_gru_trin3_fluxvert_3))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_Trin3_fluxvert_4),IF(D_Gru_Trin3_fluxvert_4<>0,ROUND(D_Gru_Trin3_fluxvert_4,2-INT((LOG(D_Gru_Trin3_fluxvert_4))+1)),0),\"\")","v":""},null,"g/år"]
["(GV-konc. med kun nedbryd.: Trin 3)",null,{"$f":"IF(ISNUMBER(D_Gru_trin3_ned_C3_1),IF(D_Gru_trin3_ned_C3_1<>0,ROUND(D_Gru_trin3_ned_C3_1,Gru_ciffer-INT((LOG(D_Gru_trin3_ned_C3_1))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin3_ned_C3_2),IF(D_Gru_trin3_ned_C3_2<>0,ROUND(D_Gru_trin3_ned_C3_2,Gru_ciffer-INT((LOG(D_Gru_trin3_ned_C3_2))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin3_ned_C3_3),IF(D_Gru_trin3_ned_C3_3<>0,ROUND(D_Gru_trin3_ned_C3_3,Gru_ciffer-INT((LOG(D_Gru_trin3_ned_C3_3))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin3_ned_C3_4),IF(D_Gru_trin3_ned_C3_4<>0,ROUND(D_Gru_trin3_ned_C3_4,Gru_ciffer-INT((LOG(D_Gru_trin3_ned_C3_4))+1)),0),\"\")","v":""},null,"mg/l"]
["GV-konc. med sorpt. og nedbryd: Trin 3",null,{"$f":"IF(ISNUMBER(D_Gru_trin3_C3_1),IF(D_Gru_trin3_C3_1<>0,ROUND(D_Gru_trin3_C3_1,Gru_ciffer-INT((LOG(D_Gru_trin3_C3_1))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin3_C3_2),IF(D_Gru_trin3_C3_2<>0,ROUND(D_Gru_trin3_C3_2,Gru_ciffer-INT((LOG(D_Gru_trin3_C3_2))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin3_C3_3),IF(D_Gru_trin3_C3_3<>0,ROUND(D_Gru_trin3_C3_3,Gru_ciffer-INT((LOG(D_Gru_trin3_C3_3))+1)),0),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Gru_trin3_C3_4),IF(D_Gru_trin3_C3_4<>0,ROUND(D_Gru_trin3_C3_4,Gru_ciffer-INT((LOG(D_Gru_trin3_C3_4))+1)),0),\"\")","v":""},null,"mg/l",null,"Trin 3-beregning",{"$f":"C64*1000000","v":{"$error":"#VALUE!"}},{"$f":"E64*1000000","v":{"$error":"#VALUE!"}},{"$f":"G64*1000000","v":{"$error":"#VALUE!"}},{"$f":"I64*1000000","v":{"$error":"#VALUE!"}},"ng/l"]
["Overskridelse af kriteriet Trin 3",null,{"$f":"IF(D_Gru_trin3_Krit_Overskr_1<>\"\",IF(ISNUMBER(D_Gru_trin3_Krit_Overskr_1),ROUND(D_Gru_trin3_Krit_Overskr_1,Gru_ciffer-(INT(LOG(D_Gru_trin3_Krit_Overskr_1))+1)),D_Gru_trin3_Krit_Overskr_1),\"\")","v":""},null,{"$f":"IF(D_Gru_trin3_Krit_Overskr_2<>\"\",IF(ISNUMBER(D_Gru_trin3_Krit_Overskr_2),ROUND(D_Gru_trin3_Krit_Overskr_2,Gru_ciffer-(INT(LOG(D_Gru_trin3_Krit_Overskr_2))+1)),D_Gru_trin3_Krit_Overskr_2),\"\")","v":""},null,{"$f":"IF(D_Gru_trin3_Krit_Overskr_3<>\"\",IF(ISNUMBER(D_Gru_trin3_Krit_Overskr_3),ROUND(D_Gru_trin3_Krit_Overskr_3,Gru_ciffer-(INT(LOG(D_Gru_trin3_Krit_Overskr_3))+1)),D_Gru_trin3_Krit_Overskr_3),\"\")","v":""},null,{"$f":"IF(D_Gru_trin3_Krit_Overskr_4<>\"\",IF(ISNUMBER(D_Gru_trin3_Krit_Overskr_4),ROUND(D_Gru_trin3_Krit_Overskr_4,Gru_ciffer-(INT(LOG(D_Gru_trin3_Krit_Overskr_4))+1)),D_Gru_trin3_Krit_Overskr_4),\"\")","v":""}]
["Anvendt brugerdata",null,{"$f":"D_GRU_brugerdata_1","v":""},null,{"$f":"D_GRU_brugerdata_2","v":""},null,{"$f":"D_GRU_brugerdata_3","v":""},null,{"$f":"D_GRU_brugerdata_4","v":""}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af          "]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_Gru_DFO_Com <> \"\", D_Gru_DFO_Com, \"\")","v":""}]
["om det forurenede område"]
["(herunder nettonedbør)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Gru_Mag_Com <> \"\", D_Gru_Mag_Com, \"\")","v":""}]
["om magasinparametre"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Gru_For_Com<>\"\",D_Gru_For_Com,\"\")","v":""}]
["om forurening"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Gru_Ber_Com<>\"\",D_Gru_Ber_Com,\"\")","v":""}]
["om beregning, f.eks. om"]
["aerobe eller anaerobe forhold"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Kem_Com<>\"\",D_Enk_Kem_Com,\"\")","v":""}]
["om fysisk/kemiske data"]
[]
[]
[]
[]
[]
[]
[]
[]
["Koncentrationsudvikling:",{"$f":"D_Gru_stofnavn_1","v":""}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Koncentrationsudvikling:",{"$f":"D_Gru_stofnavn_2","v":""}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Koncentrationsudvikling:",{"$f":"D_Gru_stofnavn_3","v":""}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Koncentrationsudvikling:",{"$f":"D_Gru_stofnavn_4","v":""}]

{"sheet":"Vejledning_Grundvand","index":14,"n_rows":92,"n_cols":2,"rows_kept":92,"cut":false,"hidden":true,"merged":[[24,1,24,15],[15,1,15,15],[1,1,1,15],[2,1,6,15],[8,1,8,15],[9,1,9,15],[10,1,11,15],[12,1,12,15],[13,1,13,15],[14,1,14,15],[7,1,7,15],[16,1,16,15],[17,1,18,15],[19,1,19,15],[20,1,20,15],[21,1,23,15],[78,1,78,15],[79,1,81,15],[48,1,49,15],[50,1,50,15],[51,1,59,15],[60,1,60,15],[61,1,61,15],[62,1,72,15],[73,1,73,15],[74,1,74,15],[75,1,76,15],[77,1,77,15],[47,1,47,15],[25,1,25,15],[26,1,27,15],[28,1,28,15],[29,1,29,15],[30,1,32,15],[34,1,34,15],[35,1,37,14],[38,1,38,15],[40,1,45,15],[46,1,46,15],[33,1,33,15],[83,1,83,15],[84,1,88,15],[89,1,89,15],[90,1,90,15],[91,1,92,15]]}
[null,"Vejledning - Grundvand"]
[null,"Formål"]
[null,"I dette regneark kan der foretages en beregning af konsekvenser for grundvand, jf. appendiks 5.6 i MST´s Oprydningsvejledning fra 1998. \n\nA - Baseret på kildestyrkekoncentrationen \nB - Baseret på den målte koncentration i det første betydende grundvandsmagasin "]
[]
[]
[]
[]
[]
[null,"BEREGNINGER:"]
[null,"Det forurenede areal - trin 1A"]
[null,"Arealet og bredden af det forurenede område skal indtastes og der vælges enten nedbørs-data fra standardlisten, \"Egen liste\" eller indtastes egenværdier.\nDet er også muligt at anvende og oprette egne nedbørsdata."]
[]
[]
[null,"Det forurenede areal - trin 1B"]
[null,"Kun filterlængden skal indtastes."]
[]
[null,"Det første betydende magasin"]
[null,"Vælg aquifermateriale og indtast de hydrauliske parametre for det første betydende magasin, hvori risikoen skal beregnes."]
[]
[]
[null,"Forureningsdata - trin 1A"]
[null,"I trin 1a kan man vælge, hvilke forureningsdata, der skal anvendes i beregningen, dvs. de målte eller de beregnede koncentrationer fra fugacitetsmodulet, de beregnede porevands-koncentrationer fra vertikaltransport i den umættede zone (modul A/C) eller egne testværdier."]
[]
[]
[]
[null,"Forureningsdata - trin 1B"]
[null,"I trin 1b kan man kun anvende målte koncentrationer i grundvandet , som overføres direkte fra \"Enkeltstoffer\", men der kan dog altid indtastes andre testværdier."]
[]
[]
[null,"Nedbrydning i trin 3"]
[null,"Der vælges, om der er tale om aerobe eller anaerobe forhold. Nedbrydnings-konstanter hentes fra kemiske data i \"Enkeltstoffer\", hvor det er muligt at indsætte andre værdier, såfremt der ikke ønskes anvendt standardværdier fra databasen."]
[]
[]
[]
[null,"GENERELT"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under olie & benzin modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under olie & benzin modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTVÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Indeklima","index":15,"n_rows":125,"n_cols":35,"rows_kept":125,"cut":false,"hidden":true,"merged":[[231,7,231,11],[231,13,231,17],[231,19,231,23],[231,25,231,29],[96,25,96,29],[85,10,85,11],[85,25,85,26],[85,28,85,29],[87,7,87,8],[87,10,87,11],[90,7,92,26],[87,25,87,26],[103,19,103,23],[97,13,97,17],[97,19,97,23],[97,25,97,29],[109,28,109,29],[105,7,105,11],[105,13,105,17],[105,19,105,23],[109,7,109,8],[94,25,94,29],[117,19,117,23],[117,25,117,29],[103,7,103,11],[109,10,109,11],[103,25,103,29],[103,13,103,17],[97,7,97,11],[101,7,101,11],[101,13,101,17],[101,19,101,23],[99,19,99,23],[99,25,99,29],[109,16,109,17],[109,19,109,20],[109,13,109,14],[99,7,99,11],[109,22,109,23],[105,25,105,29],[99,13,99,17],[109,25,109,26],[101,25,101,29],[67,10,67,11],[69,7,69,8],[73,25,75,33],[77,7,77,11],[69,10,69,11],[79,10,79,11],[94,13,94,17],[79,28,79,29],[81,7,81,8],[94,19,94,23],[67,7,67,8],[79,25,79,26],[94,7,94,11],[81,10,81,11],[81,25,81,26],[81,28,81,29],[83,10,83,11],[83,25,83,26],[83,28,83,29],[65,7,65,8],[65,10,65,11],[65,28,65,29],[61,7,61,8],[65,25,65,26],[60,25,60,26],[59,7,59,8],[61,10,61,11],[33,28,35,29],[57,7,57,8],[54,6,54,11],[39,5,39,8],[59,25,59,26],[59,28,59,29],[57,10,57,11],[63,7,63,8],[63,10,63,11],[63,28,63,29],[39,10,39,11],[41,10,42,11],[37,16,38,17],[41,16,42,17],[39,22,39,23],[41,5,42,8],[39,13,39,14],[43,16,43,17],[37,19,37,20],[38,22,38,23],[41,13,42,14],[37,5,38,8],[35,13,35,14],[38,19,38,20],[33,25,35,26],[33,5,34,8],[35,5,35,8],[43,10,43,11],[33,13,34,14],[35,10,35,11],[96,7,96,11],[96,13,96,17],[96,19,96,23],[39,19,39,20],[47,7,49,31],[43,5,43,8],[41,19,41,20],[41,22,41,23],[37,25,39,26],[41,25,43,26],[43,19,43,20],[37,10,38,11],[37,22,37,23],[37,13,38,14],[61,28,61,29],[61,25,61,26],[62,25,62,26],[63,25,63,26],[67,28,67,29],[67,25,67,26],[55,6,55,11],[59,10,59,11],[42,22,42,23],[43,13,43,14],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[13,8,15,32],[31,19,31,20],[31,22,31,23],[18,28,18,29],[29,19,29,20],[29,22,29,23],[29,25,31,26],[29,28,31,29],[18,13,18,14],[7,19,7,23],[16,27,17,30],[16,31,17,32],[16,10,17,11],[17,5,17,8],[19,5,20,8],[10,7,10,11],[19,31,19,32],[20,31,20,32],[19,16,20,17],[21,5,21,8],[41,28,43,29],[41,31,43,32],[45,31,45,32],[39,16,39,17],[45,16,45,17],[42,19,42,20],[21,16,21,17],[23,22,23,23],[35,22,35,23],[25,19,25,20],[25,22,25,23],[35,16,35,17],[23,28,25,29],[23,31,25,32],[29,31,31,32],[23,25,25,26],[35,19,35,20],[43,22,43,23],[37,31,39,32],[37,28,39,29],[33,31,35,32],[21,31,21,32],[124,7,124,11],[124,13,124,17],[124,19,124,23],[124,25,124,29],[112,7,112,11],[112,13,112,17],[112,19,112,23],[112,25,112,29],[120,19,120,23],[120,25,120,29],[120,13,120,17],[122,7,122,11],[122,13,122,17],[122,19,122,23],[122,25,122,29],[114,7,114,11],[120,7,120,11],[117,7,117,11],[117,13,117,17],[114,13,114,17],[114,19,114,23],[114,25,114,29],[10,13,10,17],[10,19,10,23],[10,25,10,29],[19,18,21,19],[23,18,25,18],[16,13,17,14],[16,16,17,17],[16,19,17,20],[16,22,17,23],[16,25,17,26],[25,16,25,17],[23,19,23,20],[18,22,18,23],[12,5,12,32],[18,25,18,26],[18,16,18,17],[24,22,24,23],[18,19,18,20],[18,10,18,11],[25,5,25,8],[23,5,24,8],[24,19,24,20],[31,5,31,8],[31,10,31,11],[31,16,31,17],[34,19,34,20],[34,22,34,23],[29,16,30,17],[33,10,34,11],[33,16,34,17],[30,22,30,23],[33,19,33,20],[33,22,33,23],[30,19,30,20],[31,13,31,14],[29,13,30,14],[29,10,30,11],[29,5,30,8]]}
["Beregning af indeklimakoncentration"]
["i bygning med terrændæk"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,"For krybekælder: benyt knap til højre"]
["Beregning udføres for :",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
[]
["Influenszone og membran",null,null,null,null,null,null,null,"Indtast data for evt. membran og kapillarbrydende lag og for jordlag mellem prøvetagningspunktet og bygningen. "]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Jordlag Dybde fra",null,null,"Jordlag Dybde til",null,null,"Lag-tykkelse",null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,"Volumen\naf jordskellet",null,null,null,"Materiale-konstant"]
[null,null,null,null,null,"Jordtype/Membran"]
[null,null,null,null,null,null,null,null,null,null,"m u.gulv",null,null,"m u.gulv",null,null,"(m)",null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ"]
[null,null,null,null,null,{"$f":"D_Ind_navnb_1_syst","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_Xb_1_syst","v":0},null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_Nb_1_int","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_Nb_1_sys","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_b_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"D_Ind_navnb_2_syst","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_VLb_2_int","v":0},null,null,{"$f":"D_Ind_VVb_2_int","v":0},null,null,{"$f":"[0]!D_Ind_eb_2","v":0},null,null,{"$f":"[0]!D_Ind_VJb_2","v":1},null,null,{"$f":"[0]!D_Ind_Nb_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_VLb_2_syst","v":0},null,null,{"$f":"D_Ind_VVb_2_syst","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_b_mangeljt_2","v":""}]
[]
["Jordparametre"]
[]
[null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_1_syst<>\"\",D_Ind_jordtype_1_syst,\"\")","v":""},null,null,null,null,{"$f":"IF(D_Ind_jordtype_1=0,\"\",B_Ind_Xb_tot)","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_1_int<>\"\",D_Ind_VL_1_int,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_1_int<>\"\",D_Ind_VV_1_int,\"\")","v":""},null,null,{"$f":"D_Ind_e_1","v":0},null,null,{"$f":"D_Ind_VJ_1","v":1},null,null,{"$f":"D_Ind_N_1","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_1_syst<>\"\",D_Ind_VL_1_syst,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_1_syst<>\"\",D_Ind_VV_1_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_X_1","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_2_syst<>\"\",D_Ind_jordtype_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_2_int<>\"\",D_Ind_VL_2_int,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_2_int<>\"\",D_Ind_VV_2_int,\"\")","v":""},null,null,{"$f":"D_Ind_e_2","v":0},null,null,{"$f":"D_Ind_VJ_2","v":1},null,null,{"$f":"D_Ind_N_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_2_syst<>\"\",D_Ind_VL_2_syst,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_2_syst<>\"\",D_Ind_VV_2_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_2=0,\"\",D_Ind_lagfra_2)","v":""},null,null,null,null,null,{"$f":"D_Ind_X_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_mangeljt_2","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_3_syst<>\"\",D_Ind_jordtype_3_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_3_int<>\"\",D_Ind_VL_3_int,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_3_int<>\"\",D_Ind_VV_3_int,\"\")","v":""},null,null,{"$f":"D_Ind_e_3","v":0},null,null,{"$f":"D_Ind_VJ_3","v":1},null,null,{"$f":"D_Ind_N_3","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_3_syst<>\"\",D_Ind_VL_3_syst,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_3_syst<>\"\",D_Ind_VV_3_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_3=0,\"\",D_Ind_lagfra_3)","v":""},null,null,null,null,null,{"$f":"D_Ind_X_3","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_mangeljt_3","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_4_syst<>\"\",D_Ind_jordtype_4_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_4_int<>\"\",D_Ind_VL_4_int,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_4_int<>\"\",D_Ind_VV_4_int,\"\")","v":""},null,null,{"$f":"D_Ind_e_4","v":0},null,null,{"$f":"D_Ind_VJ_4","v":1},null,null,{"$f":"D_Ind_N_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_VL_4_syst<>\"\",D_Ind_VL_4_syst,\"\")","v":""},null,null,{"$f":"IF(D_Ind_VV_4_syst<>\"\",D_Ind_VV_4_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ind_jordtype_4=0,\"\",D_Ind_lagfra_4)","v":""},null,null,null,null,null,{"$f":"D_Ind_X_4","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_mangeljt_4","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ind_negativ_X_tot","v":" "}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Samlede lagtykkelse",null,{"$f":"D_Ind_X_tot","v":0},null,"m",null,null,null,null,null,null,null,null,null,null,"Samlet materialekonstant KW",null,{"$f":"D_Ind_N_tot","v":{"$error":"#DIV/0!"}}]
[]
["Bygningsdata",null,null,null,null,null,null,"Vælg type af terrændæk, eller indtast egen data"]
[]
[]
["Terrændæk"]
[]
[]
[]
["Type af terrændæk",null,null,null,null,null,{"$f":"IF(D_Ind_Inddæk_syst<>\"\",D_Ind_Inddæk_syst,\"\")","v":""}]
[]
[]
["Betontværsnit",null,null,null,null,"hb",null,{"$f":"IF(D_Ind_hb_syst<>\"\",D_Ind_hb_syst,\"\")","v":""},null,null,null,null,null,"mm"]
[]
["Relativ luftfugtighed",null,null,null,null,"RF",null,{"$f":"IF(D_Ind_RF_syst<>\"\",D_Ind_RF_syst,\"\")","v":""},null,null,null,null,null,"%",null,null,"Armeringsdiameter",null,null,null,null,null,null,"da",null,{"$f":"IF(D_Ind_daCh<>\"\",D_Ind_daCh,\"\")","v":""},null,null,null,null,null,"mm"]
[]
["Vand/cement-tallet",null,null,null,null,"v/c",null,{"$f":"IF(D_Ind_wc_syst<>\"\",D_Ind_wc_syst,\"\")","v":""},null,null,null,null,null,null,null,null,"Armeringskonstant",null,null,null,null,null,null,"k",null,{"$f":"IF(D_Ind_k_syst<>\"\",D_Ind_k_syst,\"\")","v":""}]
[]
["Cementindhold",null,null,null,null,"CM",null,{"$f":"IF(D_Ind_CM_syst<>\"\",D_Ind_CM_syst,\"\")","v":""},null,null,null,null,null,"kg/m3",null,null,"Afstand mellem armeringsjern",null,null,null,null,null,null,"Db",null,{"$f":"IF(D_Ind_Db_syst<>\"\",D_Ind_Db_syst,\"\")","v":""},null,null,null,null,null,"mm"]
[]
["Svindtid",null,null,null,null,"ts",null,{"$f":"IF(D_Ind_ts_syst<>\"\",D_Ind_ts_syst,\"\")","v":""},null,null,null,null,null,"døgn",null,null,"Dynamisk viskositet af luft",null,null,null,null,null,null,"m",null,{"$f":"D_Ind_my_syst","v":1.8E-5},null,null,null,null,null,"kg/(m * s)"]
[]
["Elasticitetskoeff. Beton",null,null,null,null,"Eb",null,{"$f":"D_Ind_Eb_syst","v":20000},null,null,null,null,null,"MPa",null,null,"Elasticitetskoeff. Stål",null,null,null,null,null,null,"Es",null,{"$f":"D_Ind_Es_syst","v":210000},null,null,null,null,null,"MPa"]
[]
["Materialekonst. for beton",null,null,null,null,"Nb",null,{"$f":"IF(D_Ind_Nb_syst<>\"\",D_Ind_Nb_syst,\"\")","v":""}]
[]
[]
[]
["Bygningsdata",null,null,null,null,null,null,"Indtast bygnings data",null,null,null,null,null,null,null,null,"Beregnede bygningsdata",null,null,null,null,null,null,null,null,"Anvend beregnede bygningsdata,\neller indtast målte data"]
[]
[]
[]
["Rumtype/anvendelse"]
[]
["Loftshøjde",null,null,null,null,"Lh",null,null,null,null,null,null,null,"m",null,null,"Revnevidde",null,null,null,null,null,null,"w",null,{"$f":"D_Ind_w_Ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mm"]
[]
["Luftskifte",null,null,null,null,"Ls",null,{"$f":"D_Ind_Ls_Sys","v":8.2999999999999998E-5},null,null,null,null,null,"s-1",null,null,"Gnmsn. revneafstand",null,null,null,null,null,null,"lw",null,{"$f":"D_Ind_lw_Ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mm"]
[]
["Gulvbredde",null,null,null,null,"lb",null,null,null,null,null,null,null,"m",null,null,"Total revnelængde",null,null,null,null,null,null,"ltot",null,{"$f":"D_Ind_ltot_Ber","v":0},null,null,null,null,null,"m"]
[]
["Gulvlængde",null,null,null,null,"ll",null,null,null,null,null,null,null,"m",null,null,"Vol. strøm gennem beton",null,null,null,null,null,null,"qb",null,{"$f":"D_Ind_q_Ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,"m³/s "]
[]
["Trykforskel over betondæk",null,null,null,null,"DP",null,{"$f":"D_Ind_DP_Sys","v":5},null,null,null,null,null,"Pa",null,null,"Vol. strøm gennem beton pr. m²",null,null,null,null,null,null,"Qb",null,{"$f":"D_Ind_q/(Ind_My_Lb*Ind_My_Ll)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"m³/(s · m²)"]
[]
[]
["Forurening",null,null,null,null,null,null,"Data for forureningen er overført fra fugacitetsmodulet \nIndtast baggrundskoncentration "]
[]
[]
[]
["Stofnavn",null,null,null,null,null,null,{"$f":"[0]!D_Ind_stofnavn_1","v":""},null,null,null,null,null,{"$f":"[0]!D_Ind_stofnavn_2","v":""},null,null,null,null,null,{"$f":"[0]!D_Ind_stofnavn_3","v":""},null,null,null,null,null,{"$f":"[0]!D_Ind_stofnavn_4","v":""}]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"D_Enk_MP_1","v":""},null,null,null,null,null,{"$f":"D_Enk_MP_2","v":""},null,null,null,null,null,{"$f":"D_Enk_MP_3","v":""},null,null,null,null,null,{"$f":"D_Enk_MP_4","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"D_Enk_dato_1","v":" "},null,null,null,null,null,{"$f":"D_Enk_dato_2","v":" "},null,null,null,null,null,{"$f":"D_Enk_dato_3","v":" "},null,null,null,null,null,{"$f":"D_Enk_dato_4","v":" "}]
[]
["Poreluftskoncentration",null,null,null,null,"CL",null,{"$f":"D_Ind_CL_1_1","v":""},null,null,null,null,null,{"$f":"D_Ind_CL_2_1","v":""},null,null,null,null,null,{"$f":"D_Ind_CL_3_1","v":""},null,null,null,null,null,{"$f":"D_Ind_CL_4_1","v":""},null,null,null,null,null,"mg/m³"]
[]
["Test af andre værdier",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³"]
[]
["Baggrundskoncentration",null,null,null,null,"C0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³"]
[]
["Diffusionskoefficient i luft",null,null,null,null,"DL",null,{"$f":"D_Enk_DL_1","v":0},null,null,null,null,null,{"$f":"D_Enk_DL_2","v":0},null,null,null,null,null,{"$f":"D_Enk_DL_3","v":0},null,null,null,null,null,{"$f":"D_Enk_DL_4","v":0},null,null,null,null,null,"m²/s"]
[]
["Beregning: Indeklima"]
[]
["Stoffluxgennem beton",null,null,null,null,"J",null,{"$f":"D_Ind_Jz_1_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Jz_2_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Jz_3_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Jz_4_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mg/(s· m²)"]
[]
[]
["Poreluftkonc. under gulv",null,null,null,null,"Cp",null,{"$f":"D_Ind_Cp_1_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Cp_2_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Cp_3_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Cp_4_syst","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mg/m³"]
[]
["Diffusivt bidrag til indeluft",null,null,null,null,"Cdi",null,{"$f":"D_Ind_Cdi_1","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Cdi_2","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Cdi_3","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Cdi_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mg/m³"]
[]
[]
["Totalt bidrag til indeluft",null,null,null,null,"Ci",null,{"$f":"D_Ind_Ci_1","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Ci_2","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Ci_3","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Ind_Ci_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mg/m³"]
[]
[]
["Afdampningskriterie",null,null,null,null,null,null,{"$f":"D_Ind_afd_krit_1","v":0},null,null,null,null,null,{"$f":"D_Ind_afd_krit_2","v":0},null,null,null,null,null,{"$f":"D_Ind_afd_krit_3","v":0},null,null,null,null,null,{"$f":"D_Ind_afd_krit_4","v":0},null,null,null,null,null,"mg/m³"]
[]
["Overskridelse af kriteriet",null,null,null,null,null,null,{"$f":"D_Ind_oskr_1","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_Ind_oskr_2","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_Ind_oskr_3","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_Ind_oskr_4","v":"Intet kriterie"},null,null,null,null,null,"gange"]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"Dataark_Indeklima!H108","v":"Nej"},null,null,null,null,null,{"$f":"Dataark_Indeklima!L108","v":"Nej"},null,null,null,null,null,{"$f":"Dataark_Indeklima!P108","v":"Nej"},null,null,null,null,null,{"$f":"Dataark_Indeklima!T108","v":"Nej"}]

{"sheet":"Indeklima_Krybekælder","index":16,"n_rows":112,"n_cols":35,"rows_kept":112,"cut":false,"hidden":true,"merged":[[13,5,13,32],[113,7,113,11],[113,13,113,17],[113,19,113,23],[113,25,113,29],[76,14,76,33],[78,14,78,33],[11,7,11,11],[11,13,11,17],[11,19,11,23],[11,25,11,29],[104,7,104,11],[104,13,104,17],[104,19,104,23],[104,25,104,29],[96,7,96,11],[96,13,96,17],[96,19,96,23],[96,25,96,29],[92,7,92,11],[92,13,92,17],[92,19,92,23],[92,25,92,29],[94,7,94,11],[94,13,94,17],[94,19,94,23],[94,25,94,29],[88,7,88,11],[88,13,88,17],[111,7,111,11],[111,13,111,17],[111,19,111,23],[111,25,111,29],[107,7,107,11],[107,13,107,17],[107,19,107,23],[107,25,107,29],[109,7,109,11],[109,13,109,17],[109,19,109,23],[109,25,109,29],[88,19,88,23],[88,25,88,29],[90,7,90,11],[90,13,90,17],[90,19,90,23],[90,25,90,29],[100,0,101,4],[100,5,100,6],[100,7,100,11],[100,13,100,17],[100,19,100,23],[100,25,100,29],[101,5,101,6],[101,7,101,11],[101,13,101,17],[101,19,101,23],[101,25,101,29],[81,7,83,26],[85,7,85,11],[85,13,85,17],[85,19,85,23],[85,25,85,29],[87,7,87,11],[87,13,87,17],[87,19,87,23],[87,25,87,29],[72,10,72,11],[74,10,74,11],[76,7,76,8],[76,10,76,11],[57,10,57,11],[59,10,59,11],[64,7,64,11],[68,10,68,11],[70,10,70,11],[66,7,66,8],[66,10,66,11],[46,16,46,17],[46,31,46,32],[51,7,51,11],[53,10,53,11],[55,7,55,8],[55,10,55,11],[42,25,44,26],[42,28,44,29],[42,31,44,32],[43,19,43,20],[43,22,43,23],[44,5,44,8],[44,10,44,11],[44,13,44,14],[44,16,44,17],[44,19,44,20],[42,5,43,8],[42,10,43,11],[42,13,43,14],[42,16,43,17],[42,19,42,20],[42,22,42,23],[44,22,44,23],[38,31,40,32],[39,19,39,20],[39,22,39,23],[40,5,40,8],[40,10,40,11],[40,13,40,14],[40,16,40,17],[40,19,40,20],[36,22,36,23],[38,5,39,8],[38,10,39,11],[38,13,39,14],[38,16,39,17],[38,19,38,20],[38,22,38,23],[34,25,36,26],[34,28,36,29],[38,25,40,26],[38,28,40,29],[34,31,36,32],[35,19,35,20],[35,22,35,23],[36,5,36,8],[36,10,36,11],[36,13,36,14],[36,16,36,17],[30,28,32,29],[30,31,32,32],[31,19,31,20],[31,22,31,23],[32,5,32,8],[32,10,32,11],[32,13,32,14],[32,16,32,17],[32,19,32,20],[30,5,31,8],[30,10,31,11],[30,13,31,14],[30,16,31,17],[30,19,30,20],[30,22,30,23],[32,22,32,23],[30,25,32,26],[26,31,26,32],[27,31,27,32],[28,5,28,8],[28,16,28,17],[28,31,28,32],[22,5,23,8],[22,16,23,17],[22,31,23,32],[24,5,24,8],[24,16,24,17],[24,31,24,32],[22,18,24,19],[26,18,28,19],[18,25,19,26],[18,27,19,30],[18,31,19,32],[19,5,19,8],[20,10,20,11],[20,13,20,14],[20,16,20,17],[20,19,20,20],[20,22,20,23],[20,25,20,26],[20,28,20,29],[78,7,78,8],[74,7,74,8],[70,7,70,8],[72,7,72,8],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[18,10,19,11],[18,13,19,14],[18,16,19,17],[18,19,19,20],[18,22,19,23],[26,5,27,8],[26,16,27,17],[36,19,36,20],[34,5,35,8],[34,10,35,11],[34,13,35,14],[34,16,35,17],[34,19,34,20],[34,22,34,23],[40,22,40,23]]}
["Beregning af indeklimakoncentration"]
["i bygning med krybekælder"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,"For terrændæk/kælder: benyt knap til højre"]
[]
["Beregning udføres for :",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
[]
["Ventilleret krybekælder"]
[]
["Jordparametre og gulv i krybekælderen",null,null,null,null,null,null,null,null,null,null,null,"Indtast data om krybekælderens gulv og om jordlag"]
[]
[null,null,null,null,null,null,null,null,null,null,"Jordlag Dybde fra",null,null,"Jordlag Dybde til",null,null,"Lag-tykkelse",null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,"Volumen\naf jordskellet",null,null,null,"Materiale-konstant"]
[null,null,null,null,null,"Jordtype/Membran"]
[null,null,null,null,null,null,null,null,null,null,"m u.gulv",null,null,"m u.gulv",null,null,"(m)",null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ"]
[]
[null,null,null,null,null,{"$f":"IF(D_IndK_navnb_1_syst<>\"\",D_IndK_navnb_1_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_Xb_1_syst<>\"\",D_IndK_Xb_1_syst,\"\")","v":""},null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_Nb_1_syst<>\"\",D_IndK_Nb_1_syst,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_b_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndK_navnb_2_syst<>\"\",D_IndK_navnb_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_Xb_2_syst<>\"\",D_IndK_Xb_2_syst,\"\")","v":""},null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_Nb_2_int<>\"\",D_IndK_Nb_2_int,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_Nb_2_syst<>\"\",D_IndK_Nb_2_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_b_mangeljt_2","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_1_syst<>\"\",D_IndK_jordtype_1_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_1_int<>\"\",D_IndK_VL_1_int,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_1_int<>\"\",D_IndK_VV_1_int,\"\")","v":""},null,null,{"$f":"D_IndK_e_1","v":0},null,null,{"$f":"D_IndK_VJ_1","v":1},null,null,{"$f":"D_IndK_N_1","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_1_syst<>\"\",D_IndK_VL_1_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_1_syst<>\"\",D_IndK_VV_1_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_1=0,\"\",D_IndK_lagfra_1)","v":""},null,null,null,null,null,{"$f":"D_IndK_X_1","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_2_syst<>\"\",D_IndK_jordtype_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_2_int<>\"\",D_IndK_VL_2_int,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_2_int<>\"\",D_IndK_VV_2_int,\"\")","v":""},null,null,{"$f":"D_IndK_e_2","v":0},null,null,{"$f":"D_IndK_VJ_2","v":1},null,null,{"$f":"D_IndK_N_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_2_syst<>\"\",D_IndK_VL_2_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_2_syst<>\"\",D_IndK_VV_2_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_2=0,\"\",D_IndK_lagfra_2)","v":""},null,null,null,null,null,{"$f":"D_IndK_X_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_mangeljt_2","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_3_syst<>\"\",D_IndK_jordtype_3_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_3_int<>\"\",D_IndK_VL_3_int,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_3_int<>\"\",D_IndK_VV_3_int,\"\")","v":""},null,null,{"$f":"D_IndK_e_3","v":0},null,null,{"$f":"D_IndK_VJ_3","v":1},null,null,{"$f":"D_IndK_N_3","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_3_syst<>\"\",D_IndK_VL_3_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_3_syst<>\"\",D_IndK_VV_3_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_3=0,\"\",D_IndK_lagfra_3)","v":""},null,null,null,null,null,{"$f":"D_IndK_X_3","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_mangeljt_3","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_4_syst<>\"\",D_IndK_jordtype_4_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_4_int<>\"\",D_IndK_VL_4_int,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_4_int<>\"\",D_IndK_VV_4_int,\"\")","v":""},null,null,{"$f":"D_IndK_e_4","v":0},null,null,{"$f":"D_IndK_VJ_4","v":1},null,null,{"$f":"D_IndK_N_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_VL_4_syst<>\"\",D_IndK_VL_4_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndK_VV_4_syst<>\"\",D_IndK_VV_4_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndK_jordtype_4=0,\"\",D_IndK_lagfra_4)","v":""},null,null,null,null,null,{"$f":"D_IndK_X_4","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_mangeljt_4","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndK_negativ_X_tot","v":" "}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Samlede lagtykkelse",null,{"$f":"D_IndK_X_tot","v":0},null,"m for jordlag",null,null,null,null,null,null,null,null,null,null,"Samlet materialekonstant KW",null,{"$f":"D_IndK_N_tot","v":{"$error":"#DIV/0!"}}]
[]
[]
["Bygningsdata",null,null,null,null,null,null,"Indtast data om etagen over krybekælderen"]
[]
["Rumtype/anvendelse"]
[]
["Loftshøjde",null,null,null,null,"Lh",null,null,null,null,null,null,"m"]
[]
["Luftskifte",null,null,null,null,"Ls",null,{"$f":"D_IndK_Ls_syst","v":8.2999999999999998E-5},null,null,null,null,"s-1"]
[]
["Gulvbredde",null,null,null,null,"lb",null,null,null,null,null,null,"m"]
[]
["Gulvlængde",null,null,null,null,"ll",null,null,null,null,null,null,"m"]
[]
[]
["Data for krybekælder",null,null,null,null,null,null,"Indtast data om krybekælderen"]
[]
[null,null,null,null,null,null,null,{"$f":"D_IndKk_anv","v":0}]
[]
["Reduktionsfaktoren",null,null,null,null,null,"Rkr",{"$f":"IF(ISNUMBER(D_IndKk_Rkr_syst),D_IndKk_Rkr_syst,\"\")","v":""}]
[]
["Loftshøjde",null,null,null,null,null,"Lh",null,null,null,null,null,"m"]
[]
["Gulvbredde",null,null,null,null,null,"lb",{"$f":"D_IndK_Lb","v":0},null,null,null,null,"m"]
[]
["Gulvlængde",null,null,null,null,null,"ll",{"$f":"D_IndK_Ll","v":0},null,null,null,null,"m"]
[]
["Luftskifte",null,null,null,null,null,"Ls",{"$f":"D_IndKk_Ls_berg","v":{"$error":"#DIV/0!"}},null,null,null,null,"s-1"]
["Vol. strøm gennem loft i"]
["krybekælderen",null,null,null,null,null,"qgv",{"$f":"D_IndK_qgv_Beregn","v":{"$error":"#DIV/0!"}},null,null,null,null,"m³/s",null,{"$f":"D_IndK_q_check","v":{"$error":"#DIV/0!"}}]
[]
["Reduktionsfaktor beregn.",null,null,null,null,null,"Rkr",{"$f":"D_IndKk_Rkr_bereg","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_IndK_Rkr_check","v":{"$error":"#DIV/0!"}}]
[]
[]
["Forurening",null,null,null,null,null,null,"Data for forureningen er overført fra fugacitetsmodulet \nIndtast baggrundskoncentration samt eventuel manglende diffusionskoefficient"]
[]
[]
[]
["Stofnavn",null,null,null,null,null,null,{"$f":"D_Ind_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Ind_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Ind_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Ind_stofnavn_4","v":""}]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"D_Enk_MP_1","v":""},null,null,null,null,null,{"$f":"D_Enk_MP_2","v":""},null,null,null,null,null,{"$f":"D_Enk_MP_3","v":""},null,null,null,null,null,{"$f":"D_Enk_MP_4","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"D_Enk_dato_1","v":" "},null,null,null,null,null,{"$f":"D_Enk_dato_2","v":" "},null,null,null,null,null,{"$f":"D_Enk_dato_3","v":" "},null,null,null,null,null,{"$f":"D_Enk_dato_4","v":" "}]
[]
["Poreluftskoncentration",null,null,null,null,"CL",null,{"$f":"D_IndK_CL_1","v":0},null,null,null,null,null,{"$f":"D_IndK_CL_2","v":0},null,null,null,null,null,{"$f":"D_IndK_CL_3","v":0},null,null,null,null,null,{"$f":"D_IndK_CL_4","v":0},null,null,null,null,null,"mg/m³"]
[]
["Test af andre værdier",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³"]
[]
["Baggrundskoncentration",null,null,null,null,"C0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³"]
[]
["Diffusionskoefficient i luft",null,null,null,null,"DL",null,{"$f":"D_Ind_DL_1","v":0},null,null,null,null,null,{"$f":"D_Ind_DL_2","v":0},null,null,null,null,null,{"$f":"D_Ind_DL_3","v":0},null,null,null,null,null,{"$f":"D_Ind_DL_4","v":0},null,null,null,null,null,"m²/s"]
[]
["Beregning: Indeklima"]
[]
["Luft konc. i krybekælder",null,null,null,null,"Ck-beregn",null,{"$f":"D_IndKk_Ckr_1_beregn","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndKk_Ckr_2_beregn","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndKk_Ckr_3_beregn","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndKk_Ckr_4_beregn","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mg/m³"]
[null,null,null,null,null,"Ck-målt"]
[]
[]
["Totalt bidrag til indeluft",null,null,null,null,"Ci",null,{"$f":"D_IndK_Ci_1","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndK_Ci_2","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndK_Ci_3","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndK_Ci_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mg/m³"]
[]
[]
["Afdampningskriterie",null,null,null,null,null,null,{"$f":"D_Ind_afd_krit_1","v":0},null,null,null,null,null,{"$f":"D_Ind_afd_krit_2","v":0},null,null,null,null,null,{"$f":"D_Ind_afd_krit_3","v":0},null,null,null,null,null,{"$f":"D_Ind_afd_krit_4","v":0},null,null,null,null,null,"mg/m³"]
[]
["Overskridelse af kriteriet",null,null,null,null,null,null,{"$f":"D_IndK_oskr_1","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_IndK_oskr_2","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_IndK_oskr_3","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_IndK_oskr_4","v":"Intet kriterie"},null,null,null,null,null,"gange"]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"Dataark_Indeklima!H196","v":"Nej"},null,null,null,null,null,{"$f":"Dataark_Indeklima!L196","v":"Nej"},null,null,null,null,null,{"$f":"Dataark_Indeklima!P196","v":"Nej"},null,null,null,null,null,{"$f":"Dataark_Indeklima!T196","v":"Nej"}]

{"sheet":"Dataark_Indeklima","index":17,"n_rows":207,"n_cols":27,"rows_kept":207,"cut":false,"hidden":true,"merged":[[60,1,60,23],[70,1,70,23],[83,1,83,23],[109,1,109,23],[85,4,85,7],[85,8,85,11],[85,12,85,15],[85,16,85,19],[51,10,51,11],[46,10,46,11],[47,10,47,11],[48,10,48,11],[49,10,49,11],[50,10,50,11],[42,1,42,23],[1,1,1,23],[21,1,21,23],[40,1,40,23],[6,1,6,23],[23,4,23,7],[23,8,23,11],[23,12,23,15],[23,16,23,19],[8,4,8,7],[8,8,8,11],[124,1,124,23],[126,1,126,23],[128,4,128,7],[128,8,128,11],[135,4,135,7],[135,8,135,11],[135,12,135,15],[135,16,135,19],[197,1,197,23],[150,1,150,23],[160,1,160,23],[175,1,175,23],[177,4,177,7],[177,8,177,11],[177,12,177,15],[177,16,177,19]]}
[]
[null,"Dataark - Indeklima",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Terrændæk, kælder",false]
[null,"Krybekælder",true]
[]
[null,"Influenszone og membran"]
[]
[null,null,null,null,"Membran (1)",null,null,null,"Kapilarbrydende lag (2)"]
[null,null,"Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Navn",null,null,null,null,{"$f":"Ind_My_Memb","v":0},{"$f":"IF(ISTEXT(G11),G11,F11)","v":0},null,null,{"$f":"Ind_My_Kab_2","v":0},{"$f":"IF(ISTEXT(K11),K11,J11)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_navnb_n","Indput"]
[null,"Tykkelse af lag","Xb","m",null,null,{"$f":"Ind_My_Xb_1","v":0},{"$f":"IF(VALUE(G12),G12,F12)","v":0},null,null,{"$f":"Ind_My_Xb_2","v":0},{"$f":"K12","v":0},{"$f":"B_Ind_Xb_tot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Xb_n","Indput"]
[null,"Poreluftvolumen","VL",null,null,null,null,null,null,null,{"$f":"Ind_My_Kab_VL_2","v":0},{"$f":"IF(VALUE(K13),K13,J13)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_VLb_n","Indput"]
[null,"Vand-indhold","VV",null,null,null,null,null,null,null,{"$f":"Ind_My_Kab_VV_2","v":0},{"$f":"IF(VALUE(K14),K14,J14)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_VVb_n","Indput"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,null,null,null,null,null,{"$f":"B_Ind_eb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_eb_n","beregnes"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,null,null,null,null,{"$f":"B_Ind_VJb_2","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_VJb_n","beregnes"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,null,null,{"$f":"Ind_My_Nb_n","v":0},{"$f":"IF(VALUE(G17),G17,F17)","v":0},null,null,null,{"$f":"B_Ind_Nb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Nb_n","beregnes"]
[null,"Korigeret materialekonstant","N-kor",null,null,null,null,{"$f":"B_Ind_Nb_kor_1","v":1},null,null,null,{"$f":"B_Ind_Nb_kor_2","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Nb_kor_n","beregnes"]
[null,"Check af manglende type",null,null,null,null,null,{"$f":"IF(AND(D_Ind_Xb_1>0,D_Ind_navnb_1=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ind_Xb_2>0,D_Ind_navnb_2=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_b_mangeljt_x","Beregnes i dataark"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,null,null,null,{"$f":"B_Ind_Nb_mel_1","v":0},null,null,null,{"$f":"B_Ind_Nb_mel_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Nb_mel_n","beregnes"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,null,{"$f":"Ind_My_Jord1","v":0},{"$f":"IF(ISTEXT(G26),G26,F26)","v":0},null,null,{"$f":"Ind_My_Jord2","v":0},{"$f":"IF(ISTEXT(K26),K26,J26)","v":0},null,null,{"$f":"Ind_My_Jord3","v":0},{"$f":"IF(ISTEXT(O26),O26,N26)","v":0},null,null,{"$f":"Ind_My_Jord4","v":0},{"$f":"IF(ISTEXT(S26),S26,R26)","v":0},null,null,null,null,null,"D_Ind_jordtype_n","Indput"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,{"$f":"B_Ind_Xb_tot","v":0},{"$f":"Ind_Jord_df","v":0},{"$f":"IF(VALUE(G27),G27,F27)","v":0},null,{"$f":"D_Ind_lagtil_1","v":0},null,{"$f":"J27","v":0},null,{"$f":"D_Ind_lagtil_2","v":0},null,{"$f":"N27","v":0},null,{"$f":"D_Ind_lagtil_3","v":0},null,{"$f":"R27","v":0},null,null,null,null,null,"D_Ind_lagfra_n","Indput"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"Ind_Jord_dt1","v":0},{"$f":"G28","v":0},null,null,{"$f":"Ind_Jord_dt2","v":0},{"$f":"K28","v":0},null,null,{"$f":"Ind_Jord_dt3","v":0},{"$f":"O28","v":0},null,null,{"$f":"Ind_Jord_dt4","v":0},{"$f":"IF(VALUE(S28),S28,R28)","v":0},null,null,null,null,null,"D_Ind_lagtil_n","Indput"]
[null,"Tykkelse af jordlag","X","m",null,null,null,{"$f":"B_Ind_X_1","v":0},null,null,null,{"$f":"B_Ind_X_2","v":0},null,null,null,{"$f":"B_Ind_X_3","v":0},null,null,null,{"$f":"B_Ind_X_4","v":0},{"$f":"B_Ind_X_tot","v":0},null,null,null,null,"D_Ind_X_n","beregnes"]
[null,"Check af negativ højde",null,null,null,null,null,{"$f":"B_Ind_negativ_X_1","v":0},null,null,null,{"$f":"B_Ind_negativ_X_2","v":0},null,null,null,{"$f":"B_Ind_negativ_X_3","v":0},null,null,null,{"$f":"B_Ind_negativ_X_4","v":0},{"$f":"B_Ind_negativ_X_tot","v":" "},null,null,null,null,"D_Ind_negativ_X_n","beregnes"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"Ind_My_VL1","v":0},{"$f":"IF(VALUE(G31),G31,F31)","v":0},null,null,{"$f":"Ind_My_VL2","v":0},{"$f":"IF(VALUE(K31),K31,J31)","v":0},null,null,{"$f":"Ind_My_VL3","v":0},{"$f":"IF(VALUE(O31),O31,N31)","v":0},null,null,{"$f":"Ind_My_VL4","v":0},{"$f":"IF(VALUE(S31),S31,R31)","v":0},null,null,null,null,null,"D_Ind_VL_n","Indput"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"Ind_My_VV1","v":0},{"$f":"IF(VALUE(G32),G32,F32)","v":0},null,null,{"$f":"Ind_My_VV2","v":0},{"$f":"IF(VALUE(K32),K32,J32)","v":0},null,null,{"$f":"Ind_My_VV3","v":0},{"$f":"IF(VALUE(O32),O32,N32)","v":0},null,null,{"$f":"Ind_My_VV4","v":0},{"$f":"IF(VALUE(S32),S32,R32)","v":0},null,null,null,null,null,"D_Ind_VV_n","Indput"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,null,{"$f":"B_Ind_e_1","v":0},null,null,null,{"$f":"B_Ind_e_2","v":0},null,null,null,{"$f":"B_Ind_e_3","v":0},null,null,null,{"$f":"B_Ind_e_4","v":0},null,null,null,null,null,"D_Ind_e_n","beregnes"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,{"$f":"B_Ind_VJ_1","v":1},null,null,null,{"$f":"B_Ind_VJ_2","v":1},null,null,null,{"$f":"B_Ind_VJ_3","v":1},null,null,null,{"$f":"B_Ind_VJ_4","v":1},null,null,null,null,null,"D_Ind_VJ_n","beregnes"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,null,null,null,{"$f":"B_Ind_N_1","v":0},null,null,null,{"$f":"B_Ind_N_2","v":0},null,null,null,{"$f":"B_Ind_N_3","v":0},null,null,null,{"$f":"B_Ind_N_4","v":0},null,null,null,null,null,"D_Ind_N_n","beregnes"]
[null,"Korigeret materialekonstant","N-kor",null,null,null,null,{"$f":"B_Ind_N_kor_1","v":1},null,null,null,{"$f":"B_Ind_N_kor_2","v":1},null,null,null,{"$f":"B_Ind_N_kor_3","v":1},null,null,null,{"$f":"B_Ind_N_kor_4","v":1},null,null,null,null,null,"D_Ind_N_kor_n","beregnes"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,null,null,null,{"$f":"B_Ind_N_mel_1","v":0},null,null,null,{"$f":"B_Ind_N_mel_2","v":0},null,null,null,{"$f":"B_Ind_N_mel_3","v":0},null,null,null,{"$f":"B_Ind_N_mel_4","v":0},null,null,null,null,null,"D_Ind_N_mel_n","beregnes"]
[null,"Check af manglende jordtype",null,null,null,null,null,{"$f":"IF(AND(D_Ind_lagtil_1>0,D_Ind_jordtype_1=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ind_lagtil_2>0,D_Ind_jordtype_2=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ind_lagtil_3>0,D_Ind_jordtype_3=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ind_lagtil_4>0,D_Ind_jordtype_4=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,null,null,"D_Ind_mangeljt_x","Beregnes i dataark"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_Ind_N_tot","v":{"$error":"#DIV/0!"}},null,null,null,null,"D_Ind_N_tot","beregnes"]
[]
[null,"Bygningsdata"]
[]
[null,"Terrændæk"]
[]
[null,null,"Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Type af terrændæk",null,null,null,{"$f":"Ind_My_Inddæk","v":0},{"$f":"IF(ISTEXT(F46),F46,E46)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Inddæk","Indput"]
[null,"Betontværsnit","hb","mm",null,{"$f":"Ind_My_hb","v":0},{"$f":"IF(VALUE(F47),F47,E47)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_hb","Indput"]
[null,"Relativ luftfugtighed","RF","%",null,{"$f":"Ind_My_RF","v":0},{"$f":"IF(VALUE(F48),F48,E48)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_RF","Indput"]
[null,"Vand/cement-tallet","v/c",null,null,{"$f":"Ind_My_wc","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_wc","Indput"]
[null,"Cementindhold","CM","kg/m3",null,{"$f":"Ind_My_CM","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_CM","Indput"]
[null,"Svindtid","ts","døgn",null,{"$f":"Ind_My_ts","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_ts","Indput"]
[null,"Materialekonst. for beton","Nb",null,null,{"$f":"Ind_My_Nb","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Nb","Indput"]
[null,"Armeringsdiameter","da","mm",null,{"$f":"Ind_My_da","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_da","Indput"]
[null,"Armeringskonstant","k",null,null,{"$f":"Ind_My_k","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_k","Indput"]
[null,"Afstand mellem armeringsjern","Db","mm",null,{"$f":"IF(VALUE(Ind_My_Db),Ind_My_Db,\"\")","v":""},{"$f":"IF(ISNUMBER(F55),F55,IF(ISNUMBER(E55),E55,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Db","Indput"]
[null,"Dynamisk viskositet af luft","m","kg/(m * s)",1.8E-5,{"$f":"Ind_My_my","v":0},1.8E-5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_my","Systemværdi"]
[null,"Elasticitetskoeff. Stål","Es","MPa",210000,{"$f":"Ind_My_Es","v":0},210000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Es","Systemværdi"]
[null,"Elasticitetskoeff. Beton","Eb","MPa",20000,{"$f":"Ind_My_Eb","v":0},20000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Eb","Systemværdi"]
[null,"Materialekonstant for terrændæk (app. 5.3 lign 68B)","KN","m³/(m²·s)",null,null,{"$f":"B_Ind_Kn","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Kn","beregnes"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Rumtype/anvendelse",null,null,null,{"$f":"Ind_My_anv","v":0},{"$f":"IF(ISTEXT(F64),F64,E64)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_anv","Indput"]
[null,"Loftshøjde","Lh","m",null,{"$f":"Ind_My_Lh","v":0},{"$f":"IF(VALUE(F65),F65,E65)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Lh","Indput"]
[null,"Luftskifte","Ls","s-1",8.2999999999999998E-5,{"$f":"Ind_My_Ls","v":0},{"$f":"IF(VALUE(F66),F66,E66)","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ls","Systemværdi"]
[null,"Gulvbredde","lb","m",null,{"$f":"Ind_My_Lb","v":0},{"$f":"IF(VALUE(F67),F67,E67)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Lb","Indput"]
[null,"Gulvlængde","ll","m",null,{"$f":"Ind_My_Ll","v":0},{"$f":"IF(VALUE(F68),F68,E68)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ll","Indput"]
[null,"Trykforskel over betondæk","DP","Pa",5,{"$f":"Ind_My_DP","v":0},{"$f":"IF(VALUE(F69),F69,E69)","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_DP","Systemværdi"]
[]
[null,"Beregnede bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Beregnet værdi","Indtastet","Anvendes"]
[null,"Revnevidde \n(app 5.3 lign. 73 eller MST nr. 7 1998 - lign 40)","w","mm",{"$f":"B_Ind_w_Ber","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_w","v":0},{"$f":"IF(VALUE(F74),F74,E74)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_w","beregnes"]
[null,"Basissvindet (MST nr. 7 1998 - lign 31)","ec","%",{"$f":"B_Ind_ec_Ber","v":5.3293413173652694E-2},null,{"$f":"D_Ind_ec_Ber","v":5.3293413173652694E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_ec","beregnes"]
[null,"Beton-sammensætningskoefficient \n(MST nr. 7 1998 - lign 32)","kb",null,{"$f":"B_Ind_Kb_Ber","v":0},null,{"$f":"D_Ind_Kb_Ber","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Kb","beregnes"]
[null,"Gnmsn. Revneafstand\n(MST nr. 7 1998 - lign 41+42)","lw","mm",{"$f":"B_Ind_lw_Ber","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_Lw","v":0},{"$f":"IF(VALUE(F77),F77,E77)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_lw","beregnes"]
[null,"Total revnelængde\n(app 5.3 lign. 72 eller MST nr. 7 1998 - lign 43)","ltot","m",{"$f":"B_Ind_ltot_Ber","v":0},{"$f":"Ind_My_ltot","v":0},{"$f":"IF(VALUE(F78),F78,E78)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_ltot","beregnes"]
[null,"Vol. strøm gennem beton\n(app 5.3 lign. 70 eller MST nr. 7 1998 - lign 44)","qb","m³/(s )",{"$f":"B_Ind_q_Ber","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_q","v":0},{"$f":"IF(VALUE(F79),F79,E79)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_q","beregnes"]
[null,"Vol. strøm i bygningen","qbyg","m³/(s )",{"$f":"B_ind_qbyg_ber","v":0},null,{"$f":"D_ind_qbyg_ber","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ind_qbyg","beregnes"]
[null,"CHECK af volumenstrøm gennem beton","q_check","%",{"$f":"B_ind_qcheck_ber","v":{"$error":"#VALUE!"}},null,{"$f":"D_ind_qcheck_ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ind_qcheck","beregnes"]
[null,"Den frie svindtøjning\nMST nr. 7 1998 - lign 30 til lign36","eg","%",{"$f":"B_Ind_eg_Ber","v":{"$error":"#VALUE!"}},null,{"$f":"D_Ind_eg_Ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_eg","beregnes"]
[]
[null,"Stoffer"]
[]
[null,null,null,null,"Stof 1",null,null,null,"Stof 2",null,null,null,"Stof 3",null,null,null,"Stof 4"]
[null,"Navn","Forkortelse","Enhed","Systemværdi","Indtastet","Testværdi","Anvendes","Systemværdi","Indtastet","Testværdi","Anvendes","Systemværdi","Indtastet","Testværdi","Anvendes","Systemværdi","Indtastet","Testværdi","Anvendes"]
[null,"Forureningskomponent",null,null,{"$f":"Enk_stofnavn_1","v":""},{"$f":"Enk_My_stofnavn_1","v":0},null,{"$f":"IF(ISTEXT(F88),F88,IF(E88<>0,E88,\"\"))","v":""},{"$f":"Enk_stofnavn_2","v":""},{"$f":"Enk_My_stofnavn_2","v":0},null,{"$f":"IF(ISTEXT(J88),J88,IF(I88<>0,I88,\"\"))","v":""},{"$f":"Enk_stofnavn_3","v":""},{"$f":"Enk_My_stofnavn_3","v":0},null,{"$f":"IF(ISTEXT(N88),N88,IF(M88<>0,M88,\"\"))","v":""},{"$f":"Enk_stofnavn_4","v":""},{"$f":"Enk_My_stofnavn_4","v":0},null,{"$f":"IF(ISTEXT(R88),R88,IF(Q88<>0,Q88,\"\"))","v":""},null,null,null,null,null,"D_Ind_stofnavn_n","Indput"]
[null,"Poreluftskoncentration / test af andre værdier","CL","mg/m³",null,{"$f":"IF(D_Enk_CL_1<>0,D_Enk_CL_1,IF(D_Enk_Cl_V_1<>0,D_Enk_Cl_V_1,IF(D_Enk_Cl_J_1<>0,D_Enk_Cl_J_1,\"\")))","v":""},{"$f":"IF(VALUE(Ind_My_CL_1),Ind_My_CL_1,\"\")","v":""},{"$f":"IF(ISNUMBER(G89),G89,IF(ISNUMBER(F89),F89, E89))","v":0},null,{"$f":"IF(D_Enk_CL_2<>0,D_Enk_CL_2,IF(D_Enk_Cl_V_2<>0,D_Enk_Cl_V_2,IF(D_Enk_Cl_J_2<>0,D_Enk_Cl_J_2,\"\")))","v":""},{"$f":"IF(VALUE(Ind_My_CL_2),Ind_My_CL_2,\"\")","v":""},{"$f":"IF(ISNUMBER(K89),K89,IF(ISNUMBER(J89),J89, I89))","v":0},null,{"$f":"IF(D_Enk_CL_3<>0,D_Enk_CL_3,IF(D_Enk_Cl_V_3<>0,D_Enk_Cl_V_3,IF(D_Enk_Cl_J_3<>0,D_Enk_Cl_J_3,\"\")))","v":""},{"$f":"IF(VALUE(Ind_My_CL_3),Ind_My_CL_3,\"\")","v":""},{"$f":"IF(ISNUMBER(O89),O89,IF(ISNUMBER(N89),N89, M89))","v":0},null,{"$f":"IF(D_Enk_CL_4<>0,D_Enk_CL_4,IF(D_Enk_Cl_V_4<>0,D_Enk_Cl_V_4,IF(D_Enk_Cl_J_4<>0,D_Enk_Cl_J_4,\"\")))","v":""},{"$f":"IF(VALUE(Ind_My_CL_4),Ind_My_CL_4,\"\")","v":""},{"$f":"IF(ISNUMBER(S89),S89,IF(ISNUMBER(R89),R89, Q89))","v":0},null,null,null,null,null,"D_Ind_CL_n","Overført fra Enkeltstofer/Input"]
[null,"Baggrundskoncentration","C0","mg/m³",null,{"$f":"Ind_My_C0_1","v":0},null,{"$f":"IF(VALUE(F90),F90,E90)","v":0},null,{"$f":"Ind_My_C0_2","v":0},null,{"$f":"IF(VALUE(J90),J90,I90)","v":0},null,{"$f":"Ind_My_C0_3","v":0},null,{"$f":"IF(VALUE(N90),N90,M90)","v":0},null,{"$f":"Ind_My_C0_4","v":0},null,{"$f":"IF(VALUE(R90),R90,Q90)","v":0},null,null,null,null,null,"D_Ind_C0_n","Indput"]
[null,"Diffusionskoefficient luft","DL","m²/s",{"$f":"D_Enk_DL_1","v":0},null,null,{"$f":"E91","v":0},{"$f":"D_Enk_DL_2","v":0},null,null,{"$f":"I91","v":0},{"$f":"D_Enk_DL_3","v":0},null,null,{"$f":"M91","v":0},{"$f":"D_Enk_DL_4","v":0},null,null,{"$f":"Q91","v":0},null,null,null,null,null,"D_Ind_DL_n","Overført fra Enkeltstofer"]
[null,null,null,null,"Systemværdi","Beregnet værdi",null,"Anvendes","Systemværdi","Beregnet værdi",null,"Anvendes","Systemværdi","Beregnet værdi",null,"Anvendes","Systemværdi","Beregnet værdi",null,"Anvendes"]
[null,null,null,null,"dag-1","sek-1",null,"Sek-1","dag-1","sek-1",null,"Sek-1","dag-1","sek-1",null,"Sek-1","dag-1","sek-1",null,"Sek-1"]
[null,"Nedbrydningskonstant i poreluft","k1",null,{"$f":"D_Enk_k1anaerob_poreluft_1","v":0},{"$f":"IF(E94>0,B_Ind_k1_1,0)","v":0},null,{"$f":"F94","v":0},{"$f":"D_Enk_k1anaerob_poreluft_2","v":0},{"$f":"IF(I94>0,B_Ind_k1_2,0)","v":0},null,{"$f":"J94","v":0},{"$f":"D_Enk_k1anaerob_poreluft_3","v":0},{"$f":"IF(M94>0,B_Ind_k1_3,0)","v":0},null,{"$f":"N94","v":0},{"$f":"D_Enk_k1anaerob_poreluft_4","v":0},{"$f":"IF(Q94>0,B_Ind_k1_4,0)","v":0},null,{"$f":"R94","v":0},null,null,null,null,null,"D_Ind_k1_n","Overført fra Enkeltstoffer"]
[null,"Anvendt Brugerdata fra kemiske data",null,null,null,{"$f":"Dataark_Enkeltstoffer!E85","v":0},null,null,null,{"$f":"Dataark_Enkeltstoffer!H85","v":0},null,null,null,{"$f":"Dataark_Enkeltstoffer!K85","v":0},null,null,null,{"$f":"Dataark_Enkeltstoffer!N85","v":0}]
[null,"Indeklima beregninger",null,null,"Beregnet værdi","Indtastet",null,"Anvendes","Beregnet værdi","Indtastet",null,"Anvendes","Beregnet værdi","Indtastet",null,"Anvendes","Beregnet værdi","Indtastet",null,"Anvendes"]
[null,"Flux gennem betongulv (app. 5.3 ligning 63)","Jz","mg/(m² s)",{"$f":"B_Ind_Jz_1","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_Jz_1","v":0},null,{"$f":"IF(VALUE(F97),F97,E97)","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Jz_2","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_Jz_2","v":0},null,{"$f":"IF(VALUE(J97),J97,I97)","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Jz_3","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_Jz_3","v":0},null,{"$f":"IF(VALUE(N97),N97,M97)","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Jz_4","v":{"$error":"#VALUE!"}},{"$f":"Ind_My_Jz_4","v":0},null,{"$f":"IF(VALUE(R97),R97,Q97)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_Ind_Jz_n","beregnes"]
[null,"Kjord (app. 53 ligning 75)","Kjord","m³/(m²·s)",{"$f":"B_Ind_Kjord_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"E98","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Kjord_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"I98","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Kjord_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"M98","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Kjord_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"Q98","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_Ind_Kjord_n","beregnes"]
[null,"Totalt bidrag til indeluft","Ci","mg/m³",{"$f":"B_Ind_Ci_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(F99),F99,E99)","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Ci_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(J99),J99,I99)","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Ci_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(N99),N99,M99)","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_Ci_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(R99),R99,Q99)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_Ind_Ci_n","beregnes"]
[null,"Poreluftkonc. under gulv","Cp","mg/m³",{"$f":"Beregning_Indeklima!B_Ind_Cp_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(F100),F100,E100)","v":{"$error":"#VALUE!"}},{"$f":"Beregning_Indeklima!B_Ind_Cp_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(ISTEXT(Enk_stofnavn_2),IF(VALUE(J100),J100,I100),\"\")","v":{"$error":"#VALUE!"}},{"$f":"Beregning_Indeklima!B_Ind_Cp_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(ISTEXT(Enk_stofnavn_3),IF(VALUE(N100),N100,M100),\"\")","v":{"$error":"#VALUE!"}},{"$f":"Beregning_Indeklima!B_Ind_Cp_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(ISTEXT(Enk_stofnavn_4),IF(VALUE(R100),R100,Q100),\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_Ind_Cp_n","beregnes"]
[null,"Diffusivt bidrag til indeluft","Cdi","mg/m³",{"$f":"Beregning_Indeklima!B_Ind_Cdi_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(F101),F101,E101)","v":{"$error":"#VALUE!"}},{"$f":"Beregning_Indeklima!B_Ind_Cdi_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(ISTEXT(Enk_stofnavn_2),IF(VALUE(J101),J101,I101),\"\")","v":{"$error":"#VALUE!"}},{"$f":"Beregning_Indeklima!B_Ind_Cdi_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(ISTEXT(Enk_stofnavn_3),IF(VALUE(N101),N101,M101),\"\")","v":{"$error":"#VALUE!"}},{"$f":"Beregning_Indeklima!B_Ind_Cdi_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(ISTEXT(Enk_stofnavn_4),IF(VALUE(R101),R101,Q101),\"\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_Ind_Cdi_n","Overført fra Enkeltstofer"]
[null,"Afdampningskriterie","afd-krit","mg/m³",null,null,null,{"$f":"D_Enk_afd_krit_1","v":0},null,null,null,{"$f":"D_Enk_afd_krit_2","v":0},null,null,null,{"$f":"D_Enk_afd_krit_3","v":0},null,null,null,{"$f":"D_Enk_afd_krit_4","v":0},null,null,null,null,null,"D_Ind_afd_krit_n","Overført fra Enkeltstofer"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,null,null,{"$f":"B_Ind_oskr_1","v":"Intet kriterie"},null,null,null,{"$f":"B_Ind_oskr_2","v":"Intet kriterie"},null,null,null,{"$f":"B_Ind_oskr_3","v":"Intet kriterie"},null,null,null,{"$f":"B_Ind_oskr_4","v":"Intet kriterie"},null,null,null,null,null,"D_Ind_oskr_n","beregnes"]
[null,"Afdampningskriterie sum","afd-krit-sum","mg/m³",null,null,null,{"$f":"D_Enk_afd_krit_sum_1","v":{"$error":"#NAME?"}},null,null,null,{"$f":"D_Enk_afd_krit_sum_2","v":{"$error":"#NAME?"}},null,null,null,{"$f":"D_Enk_afd_krit_sum_3","v":{"$error":"#NAME?"}},null,null,null,{"$f":"D_Enk_afd_krit_sum_4","v":{"$error":"#NAME?"}},null,null,null,null,null,"D_Ind_afd_krit_sum_n","Overført fra Enkeltstoffer"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,null,null,{"$f":"B_Ind_oskr_sum_1","v":" "},null,null,null,{"$f":"B_Ind_oskr_sum_2","v":" "},null,null,null,{"$f":"B_Ind_oskr_sum_3","v":" "},null,null,null,{"$f":"B_Ind_oskr_sum_4","v":" "},null,null,null,null,null,"D_Ind_oskr_sum_n","beregnes"]
[null,"Fri fase ??",null,null,null,null,null,{"$f":"D_Enk_FF_1","v":"nej"},null,null,null,{"$f":"D_Enk_FF_2","v":"nej"},null,null,null,{"$f":"D_Enk_FF_3","v":"nej"},null,null,null,{"$f":"D_Enk_FF_4","v":"nej"},null,null,null,null,null,"D_Ind_FF_n","beregnes"]
[]
[null,"Anvendt Brugerdata",null,null,null,{"$f":"SUM(F95:F106,G31:G34,K31:K34,O31:O34,S31:S34)","v":0},null,{"$f":"IF(F108>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(J95:J106,K31:K34,O31:O34,S31:S34,G31:G34)","v":0},null,{"$f":"IF(J108>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(N95:N106,O31:O34,S31:S34,G31:G34,K31:K34)","v":0},null,{"$f":"IF(N108>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(R95:R106,S31:S34,G31:G34,K31:K34,O31:O34)","v":0},null,{"$f":"IF(R108>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,null,null,null,null,"D_Ind_Brugerdata_n","Beregnes i dataark"]
[]
[null,"Bemærkninger"]
[]
[null,"Jordparametre:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Jord_Com","Indput - bemærkningsfelt"]
[null,null,false]
[null,"Influenszone og membran:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Inf_Com","Indput - bemærkningsfelt"]
[null,null,false]
[null,"Terrændæk:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ter_Com","Indput - bemærkningsfelt"]
[null,null,false]
[null,"Bygningsdata:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Byg_Com","Indput - bemærkningsfelt"]
[null,null,false]
[null,"Forurening:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_For_Com","Indput - bemærkningsfelt"]
[null,null,false]
[null,"Beregning - Indeklima:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ind_Com","Indput - bemærkningsfelt"]
[null,null,false]
[]
[null,"Dataark - Indeklima Krybekælder"]
[]
[null,"Betongulv, membran og jord"]
[]
[null,null,null,null,"Betongulv (1)",null,null,null,"Membran (2)"]
[null,null,"Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Navn",null,null,null,null,{"$f":"IndK_My_Gulv","v":0},{"$f":"IF(ISTEXT(G131),G131,F131)","v":0},null,null,{"$f":"IndK_My_Memb","v":0},{"$f":"IF(ISTEXT(K131),K131,J131)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_navnb_n","Indput"]
[null,"Tykkelse af lag","Xb","m",null,null,{"$f":"IndK_My_Xb_1","v":0},{"$f":"IF(VALUE(G132),G132,F132)","v":0},null,null,{"$f":"IndK_My_Xb_2","v":0},{"$f":"IF(VALUE(K132),K132,J132)","v":0},{"$f":"B_IndK_Xb_tot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Xb_n","Indput"]
[null,"Check af manglende type",null,null,null,null,null,{"$f":"IF(AND(D_IndK_Xb_1>0,D_IndK_navnb_1=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndK_Xb_2>0,D_IndK_navnb_2=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_b_mangeljt_x","Beregnes i dataark"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,null,null,{"$f":"IndK_My_Nb_1","v":0},{"$f":"IF(VALUE(G134),G134,F134)","v":0},null,null,{"$f":"IndK_My_Nb_2","v":0},{"$f":"IF(VALUE(K134),K134,J134)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Nb_n","Indput"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,null,{"$f":"IndK_My_Jord1","v":0},{"$f":"IF(ISTEXT(G138),G138,F138)","v":0},null,null,{"$f":"IndK_My_Jord2","v":0},{"$f":"IF(ISTEXT(K138),K138,J138)","v":0},null,null,{"$f":"IndK_My_Jord3","v":0},{"$f":"IF(ISTEXT(O138),O138,N138)","v":0},null,null,{"$f":"IndK_My_Jord4","v":0},{"$f":"IF(ISTEXT(S138),S138,R138)","v":0},null,null,null,null,null,"D_IndK_jordtype_n","Indput"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,{"$f":"B_IndK_lagfra_1","v":0},null,{"$f":"IF(VALUE(G139),G139,F139)","v":0},null,{"$f":"B_IndK_lagfra_2","v":0},null,{"$f":"J139","v":0},null,{"$f":"B_IndK_lagfra_3","v":0},null,{"$f":"N139","v":0},null,{"$f":"B_IndK_lagfra_4","v":0},null,{"$f":"R139","v":0},null,null,null,null,null,"D_IndK_lagfra_n","beregnes"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"IndK_Jord_dt1","v":0},{"$f":"G140","v":0},null,null,{"$f":"IndK_Jord_dt2","v":0},{"$f":"K140","v":0},null,null,{"$f":"IndK_Jord_dt3","v":0},{"$f":"O140","v":0},null,null,{"$f":"IndK_Jord_dt4","v":0},{"$f":"IF(VALUE(S140),S140,R140)","v":0},null,null,null,null,null,"D_IndK_lagtil_n","Indput"]
[null,"Tykkelse af jordlag","X","m",null,null,null,{"$f":"B_IndK_X_1","v":0},null,null,null,{"$f":"B_IndK_X_2","v":0},null,null,null,{"$f":"B_IndK_X_3","v":0},null,null,null,{"$f":"B_IndK_X_4","v":0},{"$f":"B_IndK_X_tot","v":0},null,null,null,null,"D_IndK_X_n","beregnes"]
[null,"Check af negativ højde",null,null,null,null,null,{"$f":"B_IndK_negativ_X_1","v":0},null,null,null,{"$f":"B_IndK_negativ_X_2","v":0},null,null,null,{"$f":"B_IndK_negativ_X_3","v":0},null,null,null,{"$f":"B_IndK_negativ_X_4","v":0},{"$f":"B_IndK_negativ_X_tot","v":" "},null,null,null,null,"D_IndK_negativ_X_n","beregnes"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"IndK_My_VL1","v":0},{"$f":"IF(VALUE(G143),G143,F143)","v":0},null,null,{"$f":"IndK_My_VL2","v":0},{"$f":"IF(VALUE(K143),K143,J143)","v":0},null,null,{"$f":"IndK_My_VL3","v":0},{"$f":"IF(VALUE(O143),O143,N143)","v":0},null,null,{"$f":"IndK_My_VL4","v":0},{"$f":"IF(VALUE(S143),S143,R143)","v":0},null,null,null,null,null,"D_IndK_VL_n","Indput"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"IndK_My_VV1","v":0},{"$f":"IF(VALUE(G144),G144,F144)","v":0},null,null,{"$f":"IndK_My_VV2","v":0},{"$f":"IF(VALUE(K144),K144,J144)","v":0},null,null,{"$f":"IndK_My_VV3","v":0},{"$f":"IF(VALUE(O144),O144,N144)","v":0},null,null,{"$f":"IndK_My_VV4","v":0},{"$f":"IF(VALUE(S144),S144,R144)","v":0},null,null,null,null,null,"D_IndK_VV_n","Indput"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,null,{"$f":"B_IndK_e_1","v":0},null,null,null,{"$f":"B_IndK_e_2","v":0},null,null,null,{"$f":"B_IndK_e_3","v":0},null,null,null,{"$f":"B_IndK_e_4","v":0},null,null,null,null,null,"D_IndK_e_n","beregnes"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,{"$f":"B_IndK_VJ_1","v":1},null,null,null,{"$f":"B_IndK_VJ_2","v":1},null,null,null,{"$f":"B_IndK_VJ_3","v":1},null,null,null,{"$f":"B_IndK_VJ_4","v":1},null,null,null,null,null,"D_IndK_VJ_n","beregnes"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,null,null,null,{"$f":"B_IndK_N_1","v":0},null,null,null,{"$f":"B_IndK_N_2","v":0},null,null,null,{"$f":"B_IndK_N_3","v":0},null,null,null,{"$f":"B_IndK_N_4","v":0},null,null,null,null,null,"D_IndK_N_n","beregnes"]
[null,"Check af manglende jordtype",null,null,null,null,null,{"$f":"IF(AND(D_IndK_lagtil_1>0,D_IndK_jordtype_1=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndK_lagtil_2>0,D_IndK_jordtype_2=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndK_lagtil_3>0,D_IndK_jordtype_3=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndK_lagtil_4>0,D_IndK_jordtype_4=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,null,null,"D_IndK_mangeljt_x","Indput"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_IndK_N_tot","v":{"$error":"#DIV/0!"}},null,null,null,null,"D_IndK_N_tot","Beregnes i dataark"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Rumtype/anvendelse",null,null,null,{"$f":"IndK_anv","v":0},{"$f":"IF(ISTEXT(F154),F154,E154)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_anv","Indput"]
[null,"Loftshøjde","Lh","m",null,{"$f":"IndK_Lh","v":0},{"$f":"IF(VALUE(F155),F155,E155)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Lh","Indput"]
[null,"Luftskifte","Ls","s-1",8.2999999999999998E-5,{"$f":"IndK_Ls","v":0},{"$f":"IF(VALUE(F156),F156,E156)","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Ls","Systemværdi"]
[null,"Gulvbredde","lb","m",null,{"$f":"IndK_Lb","v":0},{"$f":"IF(VALUE(F157),F157,E157)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Lb","Indput"]
[null,"Gulvlængde","ll","m",null,{"$f":"IndK_Ll","v":0},{"$f":"IF(VALUE(F158),F158,E158)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Ll","Indput"]
[null,"Volumenstrøm i beboelse","Qbeboelse","m³/s",{"$f":"B_IndK_qbb","v":0},null,{"$f":"E159","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"beregnes"]
[]
[null,"Krybekælder"]
[]
[null,null,"Forkortelse","Enhed","Beregnet værdi","Indtastet","Anvendes"]
[null,"Etageadskillelse",null,null,null,null,{"$f":"IF(ISTEXT(F164),F164,E164)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_anv","Indput"]
[null,"Reduktionsfaktoren","Rkr",null,null,{"$f":"IndKk_Rkr","v":0},{"$f":"IF(VALUE(F165),F165,E165)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_Rkr","Indput"]
[null,"Loftshøjde","Lh","m",null,{"$f":"IndKk_Lh","v":0},{"$f":"F166","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_Lh","Indput"]
[null,"Gulvbredde","lb","m",{"$f":"D_IndK_Lb","v":0},{"$f":"IndKk_Lb","v":0},{"$f":"IF(VALUE(F167),F167,E167)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_Lb","Indput"]
[null,"Gulvlængde","ll","m",{"$f":"D_IndK_Ll","v":0},{"$f":"IndKk_Ll","v":0},{"$f":"IF(VALUE(F168),F168,E168)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_Ll","Indput"]
[null,"Luftskifte","Ls","m",{"$f":"B_IndKk_Ls_berg","v":{"$error":"#DIV/0!"}},{"$f":"IndKk_Ls","v":0},{"$f":"IF(VALUE(F169),F169,E169)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_Ls","beregnes"]
[null,"Vol. strøm gennem Krybekældergulv","qgv","m³/(s )",{"$f":"B_IndK_qgv_berg","v":{"$error":"#DIV/0!"}},{"$f":"IndK_qgv","v":0},{"$f":"IF(VALUE(F170),F170,E170)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_qgv","beregnes"]
[null,"Vol. strøm i krybekælderen","qbyg","m³/(s )",null,null,{"$f":"B_IndKk_qbyg_berg","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_qbyg","beregnes"]
[null,"Check af volumenstrøm",null,null,null,null,{"$f":"B_IndK_q_check","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_q_check","beregnes"]
[null,"Beregnet reduktionsfaktor","Rkr, beregnet",null,null,null,{"$f":"B_IndKk_Rkr_bereg","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndKk_Rkr_bereg","beregnes"]
[null,"Check af reduktionsfaktor",null,null,null,null,{"$f":"B_IndK_Rkr_check","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndK_Rkr_check","beregnes"]
[]
[null,"Stoffer"]
[]
[null,null,null,null,"Stof 1",null,null,null,"Stof 2",null,null,null,"Stof 3",null,null,null,"Stof 4"]
[null,"Navn","Forkortelse","Enhed","Systemværdi","Indtastet","Testværdi","Anvendes","Systemværdi","Indtastet","Testværdi","Anvendes","Systemværdi","Indtastet","Testværdi","Anvendes","Systemværdi","Indtastet","Testværdi","Anvendes"]
[null,"Forureningskomponent",null,null,{"$f":"Enk_stofnavn_1","v":""},{"$f":"Enk_My_stofnavn_1","v":0},null,{"$f":"IF(ISTEXT(F180),F180,IF(E180<>0,E180,\"\"))","v":""},{"$f":"Enk_stofnavn_2","v":""},{"$f":"Enk_My_stofnavn_2","v":0},null,{"$f":"IF(ISTEXT(J180),J180,IF(I180<>0,I180,\"\"))","v":""},{"$f":"Enk_stofnavn_3","v":""},{"$f":"Enk_My_stofnavn_3","v":0},null,{"$f":"IF(ISTEXT(N180),N180,IF(M180<>0,M180,\"\"))","v":""},{"$f":"Enk_stofnavn_4","v":""},{"$f":"Enk_My_stofnavn_4","v":0},null,{"$f":"IF(ISTEXT(R180),R180,IF(Q180<>0,Q180,\"\"))","v":""},null,null,null,null,null,null,"Overført fra Enkeltstoffer"]
[null,"Poreluftskoncentration / test af andre værdier","CL","mg/m³",null,{"$f":"IF(D_Enk_CL_1<>0,D_Enk_CL_1,IF(D_Enk_Cl_V_1<>0,D_Enk_Cl_V_1,IF(D_Enk_Cl_J_1<>0,D_Enk_Cl_J_1,\"\")))","v":""},{"$f":"IF(VALUE(IndK_My_CL_1),IndK_My_CL_1,\"\")","v":""},{"$f":"IF(ISNUMBER(G181),G181,IF(ISNUMBER(F181),F181, E181))","v":0},null,{"$f":"IF(D_Enk_CL_2<>0,D_Enk_CL_2,IF(D_Enk_Cl_V_2<>0,D_Enk_Cl_V_2,IF(D_Enk_Cl_J_2<>0,D_Enk_Cl_J_2,\"\")))","v":""},{"$f":"IF(VALUE(IndK_My_CL_2),IndK_My_CL_2,\"\")","v":""},{"$f":"IF(ISNUMBER(K181),K181,IF(ISNUMBER(J181),J181, I181))","v":0},null,{"$f":"IF(D_Enk_CL_3<>0,D_Enk_CL_3,IF(D_Enk_Cl_V_3<>0,D_Enk_Cl_V_3,IF(D_Enk_Cl_J_3<>0,D_Enk_Cl_J_3,\"\")))","v":""},{"$f":"IF(VALUE(IndK_My_CL_3),IndK_My_CL_3,\"\")","v":""},{"$f":"IF(ISNUMBER(O181),O181,IF(ISNUMBER(N181),N181, M181))","v":0},null,{"$f":"IF(D_Enk_CL_4<>0,D_Enk_CL_4,IF(D_Enk_Cl_V_4<>0,D_Enk_Cl_V_4,IF(D_Enk_Cl_J_4<>0,D_Enk_Cl_J_4,\"\")))","v":""},{"$f":"IF(VALUE(IndK_My_CL_4),IndK_My_CL_4,\"\")","v":""},{"$f":"IF(ISNUMBER(S181),S181,IF(ISNUMBER(R181),R181, Q181))","v":0},null,null,null,null,null,"D_IndK_CL_n","Indput"]
[null,"Baggrundskoncentration","C0","mg/m³",null,{"$f":"Indk_My_C0_1","v":0},null,{"$f":"IF(VALUE(F182),F182,E182)","v":0},null,{"$f":"Indk_My_C0_2","v":0},null,{"$f":"IF(VALUE(J182),J182,I182)","v":0},null,{"$f":"Indk_My_C0_3","v":0},null,{"$f":"IF(VALUE(N182),N182,M182)","v":0},null,{"$f":"Indk_My_C0_4","v":0},null,{"$f":"IF(VALUE(R182),R182,Q182)","v":0},null,null,null,null,null,"D_Indk_C0_n","Indput"]
[null,"Diffusionskoefficient luft","DL","m²/s",{"$f":"D_Enk_DL_1","v":0},null,null,{"$f":"IF(VALUE(F183),F183,E183)","v":0},{"$f":"D_Enk_DL_2","v":0},null,null,{"$f":"IF(VALUE(J183),J183,I183)","v":0},{"$f":"D_Enk_DL_3","v":0},null,null,{"$f":"IF(VALUE(N183),N183,M183)","v":0},{"$f":"D_Enk_DL_4","v":0},null,null,{"$f":"IF(VALUE(R183),R183,Q183)","v":0},null,null,null,null,null,"D_IndK_DL_n","Overført fra Enkeltstoffer"]
[null,null,null,null,"Systemværdi","Beregnet værdi",null,"Anvendes","Systemværdi","Beregnet værdi",null,"Anvendes","Systemværdi","Beregnet værdi",null,"Anvendes","Systemværdi","Beregnet værdi",null,"Anvendes"]
[null,null,null,null,"dag-1","sek-1",null,"Sek-1","dag-1","sek-1",null,"Sek-1","dag-1","sek-1",null,"Sek-1","dag-1","sek-1",null,"Sek-1"]
[null,"Nedbrydningskonstant i poreluft","k1",null,{"$f":"D_Enk_k1anaerob_poreluft_1","v":0},{"$f":"IF(E186>0,B_Ind_k1_1,0)","v":0},null,{"$f":"F186","v":0},{"$f":"D_Enk_k1anaerob_poreluft_2","v":0},{"$f":"IF(I186>0,B_Ind_k1_2,0)","v":0},null,{"$f":"J186","v":0},{"$f":"D_Enk_k1anaerob_poreluft_3","v":0},{"$f":"IF(M186>0,B_Ind_k1_3,0)","v":0},null,{"$f":"N186","v":0},{"$f":"D_Enk_k1anaerob_poreluft_4","v":0},{"$f":"IF(Q186>0,B_Ind_k1_4,0)","v":0},null,{"$f":"R186","v":0},null,null,null,null,null,null,"Overført fra Enkeltstoffer"]
[null,"Anvendt Brugerdata fra kemiske data",null,null,null,{"$f":"Dataark_Enkeltstoffer!E85","v":0},null,null,null,{"$f":"Dataark_Enkeltstoffer!H85","v":0},null,null,null,{"$f":"Dataark_Enkeltstoffer!K85","v":0},null,null,null,{"$f":"Dataark_Enkeltstoffer!N85","v":0}]
[null,"Indeklima beregninger",null,null,"Beregnet værdi","Indtastet",null,"Anvendes","Beregnet værdi","Indtastet",null,"Anvendes","Beregnet værdi","Indtastet",null,"Anvendes","Beregnet værdi","Indtastet",null,"Anvendes"]
[null,"Flux gennem jorden (app. 5.3 ligning 80)","Jz","mg/(m² s)",{"$f":"B_IndKk_Jz_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(F189),F189,E189)","v":{"$error":"#VALUE!"}},{"$f":"B_IndKk_Jz_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(J189),J189,I189)","v":{"$error":"#VALUE!"}},{"$f":"B_IndKk_Jz_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(N189),N189,M189)","v":{"$error":"#VALUE!"}},{"$f":"B_IndKk_Jz_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(R189),R189,Q189)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_IndKk_Jz_n","beregnes"]
[null,"Luftkoncentrationen i krybekælderen\n(app. 5.3 ligning 81)","Ckr","mg/m³",{"$f":"B_IndKk_Ckr_1","v":{"$error":"#VALUE!"}},{"$f":"IndKk_My_Ckr_1","v":0},null,{"$f":"IF(ISNUMBER(IndKk_My_Ckr_1),IndKk_My_Ckr_1, D_IndKk_Ckr_1_beregn)","v":{"$error":"#VALUE!"}},{"$f":"B_IndKk_Ckr_2","v":{"$error":"#VALUE!"}},{"$f":"IndKk_My_Ckr_2","v":0},null,{"$f":"IF(ISNUMBER(IndKk_My_Ckr_2),IndKk_My_Ckr_2, D_IndKk_Ckr_2_beregn)","v":{"$error":"#VALUE!"}},{"$f":"B_IndKk_Ckr_3","v":{"$error":"#VALUE!"}},{"$f":"IndKk_My_Ckr_3","v":0},null,{"$f":"IF(ISNUMBER(IndKk_My_Ckr_3),IndKk_My_Ckr_3, D_IndKk_Ckr_3_beregn)","v":{"$error":"#VALUE!"}},{"$f":"B_IndKk_Ckr_4","v":{"$error":"#VALUE!"}},{"$f":"IndKk_My_Ckr_4","v":0},null,{"$f":"IF(ISNUMBER(IndKk_My_Ckr_4),IndKk_My_Ckr_4, D_IndKk_Ckr_4_beregn)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_IndKk_Ckr_n","beregnes"]
[null,"Totalt bidrag til indeluft","Ci","mg/m³",{"$f":"B_IndK_Ci_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(F191),F191,E191)","v":{"$error":"#VALUE!"}},{"$f":"B_IndK_Ci_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(J191),J191,I191)","v":{"$error":"#VALUE!"}},{"$f":"B_IndK_Ci_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(N191),N191,M191)","v":{"$error":"#VALUE!"}},{"$f":"B_IndK_Ci_4","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(VALUE(R191),R191,Q191)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"D_IndK_Ci_n","beregnes"]
[null,"Afdampningskriterie","afd-krit","mg/m³",null,null,null,{"$f":"D_Enk_afd_krit_1","v":0},null,null,null,{"$f":"D_Enk_afd_krit_2","v":0},null,null,null,{"$f":"D_Enk_afd_krit_3","v":0},null,null,null,{"$f":"D_Enk_afd_krit_4","v":0},null,null,null,null,null,null,"Overført fra Enkeltstoffer"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,null,null,{"$f":"B_IndK_oskr_1","v":"Intet kriterie"},null,null,null,{"$f":"B_IndK_oskr_2","v":"Intet kriterie"},null,null,null,{"$f":"B_IndK_oskr_3","v":"Intet kriterie"},null,null,null,{"$f":"B_IndK_oskr_4","v":"Intet kriterie"},null,null,null,null,null,"D_Ind_oskr_n"]
[null,"Fri fase ??",null,null,null,null,null,{"$f":"D_Enk_FF_1","v":"nej"},null,null,null,{"$f":"D_Enk_FF_2","v":"nej"},null,null,null,{"$f":"D_Enk_FF_3","v":"nej"},null,null,null,{"$f":"D_Enk_FF_4","v":"nej"},null,null,null,null,null,null,"Overført fra Enkeltstoffer"]
[]
[null,"Anvendt Brugerdata",null,null,null,{"$f":"SUM(F187:F194,G143:G146,K143:K146,O143:O146,S143:S146)","v":0},null,{"$f":"IF(F196>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(J187:J194,K143:K146,O143:O146,S143:S146,G143:G146)","v":0},null,{"$f":"IF(J196>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(N187:N194,O143:O146,S143:S146,G143:G146,K143:K146)","v":0},null,{"$f":"IF(N196>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,{"$f":"SUM(R187:R194,S143:S146,G143:G146,K143:K146,O143:O146)","v":0},null,{"$f":"IF(R196>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"},null,null,null,null,null,"D_Ind_Brugerdata_n"]
[]
[null,"Bemærkninger"]
[]
[null,"Jordparametre:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ven_Jord_Com","Indput - bemærkningsfelt"]
[null,null,{"$f":"NOT(ISBLANK(D_Ind_Ven_Jord_Com))","v":false}]
[null,"Bygningsdata:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ven_Byg_Com","Indput - bemærkningsfelt"]
[null,null,{"$f":"NOT(ISBLANK(D_Ind_Ven_Byg_Com))","v":false}]
[null,"Krybekælderdata",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ven_Kryb_Com","Indput - bemærkningsfelt"]
[null,null,{"$f":"NOT(ISBLANK(D_Ind_Ven_Kryb_Com))","v":false}]
[null,"Forurenet område",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ind_Ven_For_Com","Indput - bemærkningsfelt"]
[null,null,{"$f":"NOT(ISBLANK(D_Ind_Ven_For_Com))","v":false}]

{"sheet":"Beregning_Indeklima","index":18,"n_rows":179,"n_cols":20,"rows_kept":179,"cut":false,"hidden":true,"merged":[[120,4,120,5],[120,6,120,7],[120,8,120,9],[120,10,120,11],[46,11,46,12],[86,4,86,5],[86,10,86,11],[86,8,86,9],[56,1,56,15],[66,1,66,15],[84,1,84,15],[107,1,107,23],[108,1,108,15],[110,4,110,5],[110,6,110,7],[118,1,118,15],[41,11,41,12],[42,11,42,12],[43,11,43,12],[44,11,44,12],[45,11,45,12],[1,1,1,15],[17,1,17,15],[35,1,35,15],[3,1,3,15],[37,1,37,15],[19,4,19,5],[19,6,19,7],[19,8,19,9],[19,10,19,11],[5,4,5,5],[5,6,5,7],[136,1,136,15],[146,1,146,15],[161,1,161,15],[163,4,163,5],[163,8,163,9],[163,10,163,11]]}
[]
[null,"Beregning- Indeklima",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn"]
[]
[null,"Influenszone og membran"]
[]
[null,null,null,null,"Membran (1)",null,"Kapilarbrydende lag (2)"]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Navn",null,null,{"$f":"D_Ind_navnb_1","v":0},null,{"$f":"D_Ind_navnb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_navnb_n"]
[null,"Tykkelse af lag","Xb","m",{"$f":"D_Ind_Xb_1","v":0},{"$f":"E9/1000","v":0},{"$f":"D_Ind_Xb_2","v":0},null,{"$f":"B_Ind_Xb_1+B_Ind_Xb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_Ind_Xb_n"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"D_Ind_VLb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_VLb_n"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"D_Ind_VVb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_VVb_n"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,{"$f":"H12","v":0},{"$f":"B_Ind_VLb_2+B_Ind_VVb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,"B_Ind_eb_n"]
[null,"Volumen af jordskellet","VJ",null,null,null,{"$f":"H13","v":1},{"$f":"1-B_Ind_eb_2","v":1},null,null,null,null,null,null,null,null,null,null,null,"B_Ind_VJb_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,{"$f":"D_Ind_Nb_1","v":0},null,{"$f":"H14","v":0},{"$f":"IF((B_Ind_eb_2)=0,0,((B_Ind_VLb_2)^2.5)/(B_Ind_eb_2))","v":0},null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Nb_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F15","v":1},{"$f":"IF((B_Ind_Nb_1)=0,1,(B_Ind_Nb_1))","v":1},{"$f":"H15","v":1},{"$f":"IF((B_Ind_Nb_2)=0,1,(B_Ind_Nb_2))","v":1},null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Nb_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F16","v":0},{"$f":"B_Ind_Xb_1*B_Ind_N_kor_1*B_Ind_N_kor_2*B_Ind_N_kor_3*B_Ind_N_kor_4*B_Ind_Nb_kor_2","v":0},{"$f":"H16","v":0},{"$f":"B_Ind_Xb_2*B_Ind_N_kor_1*B_Ind_N_kor_2*B_Ind_N_kor_3*B_Ind_N_kor_4*B_Ind_Nb_kor_1","v":0},null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Nb_mel_n"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Jordtype",null,null,{"$f":"D_Ind_jordtype_1","v":0},null,{"$f":"D_Ind_jordtype_2","v":0},null,{"$f":"D_Ind_jordtype_3","v":0},null,{"$f":"D_Ind_jordtype_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_jordtype_n"]
[null,"Jordlag, Dybde fra","x1","m u.t.",{"$f":"D_Ind_lagfra_1","v":0},null,{"$f":"D_Ind_lagfra_2","v":0},null,{"$f":"D_Ind_lagfra_3","v":0},null,{"$f":"D_Ind_lagfra_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_lagfra_n"]
[null,"Jordlag, Dybde til","x2","m u.t.",{"$f":"D_Ind_lagtil_1","v":0},null,{"$f":"D_Ind_lagtil_2","v":0},null,{"$f":"D_Ind_lagtil_3","v":0},null,{"$f":"D_Ind_lagtil_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_lagtil_n"]
[null,"Tykkelse af jordlag","X","m",{"$f":"F25","v":0},{"$f":"IF(ISNUMBER(Ind_Jord_dt1),B_Ind_lagtil_1-B_Ind_lagfra_1,0)","v":0},{"$f":"H25","v":0},{"$f":"IF(ISNUMBER(Ind_Jord_dt2),B_Ind_lagtil_2-B_Ind_lagfra_2,0)","v":0},{"$f":"J25","v":0},{"$f":"IF(ISNUMBER(Ind_Jord_dt3),B_Ind_lagtil_3-B_Ind_lagfra_3,0)","v":0},{"$f":"L25","v":0},{"$f":"IF(ISNUMBER(Ind_Jord_dt4),B_Ind_lagtil_4-B_Ind_lagfra_4,0)","v":0},{"$f":"B_Ind_X_1+B_Ind_X_2+B_Ind_X_3+B_Ind_X_4+B_Ind_Xb_tot","v":0},null,null,null,null,null,null,"B_Ind_X_n"]
[null,"Check af negativ højde",null,null,{"$f":"F26","v":0},{"$f":"IF(B_Ind_X_1<0,1,0)","v":0},{"$f":"H26","v":0},{"$f":"IF(B_Ind_X_2<0,1,0)","v":0},{"$f":"J26","v":0},{"$f":"IF(B_Ind_X_3<0,1,0)","v":0},{"$f":"L26","v":0},{"$f":"IF(B_Ind_X_4<0,1,0)","v":0},{"$f":"IF(B_Ind_negativ_X_1+B_Ind_negativ_X_2+B_Ind_negativ_X_3+B_Ind_negativ_X_4>0,\"FEJL!! Der er jordlag med negativ højde\",\" \")","v":" "},null,null,null,null,null,null,"B_Ind_negativ_X_n"]
[null,"Poreluftvolumen","VL",null,{"$f":"D_Ind_VL_1","v":0},null,{"$f":"D_Ind_VL_2","v":0},null,{"$f":"D_Ind_VL_3","v":0},null,{"$f":"D_Ind_VL_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_VL_n"]
[null,"Vand-indhold","VV",null,{"$f":"D_Ind_VV_1","v":0},null,{"$f":"D_Ind_VV_2","v":0},null,{"$f":"D_Ind_VV_3","v":0},null,{"$f":"D_Ind_VV_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_VV_n"]
[null,"Samlet porøsitet","e=VL+VV",null,{"$f":"F29","v":0},{"$f":"B_Ind_VL_1+B_Ind_VV_1","v":0},{"$f":"H29","v":0},{"$f":"B_Ind_VL_2+B_Ind_VV_2","v":0},{"$f":"J29","v":0},{"$f":"B_Ind_VL_3+B_Ind_VV_3","v":0},{"$f":"L29","v":0},{"$f":"B_Ind_VL_4+B_Ind_VV_4","v":0},null,null,null,null,null,null,null,"B_Ind_e_n"]
[null,"Volumen af jordskellet","VJ",null,{"$f":"F30","v":1},{"$f":"1-B_Ind_e_1","v":1},{"$f":"H30","v":1},{"$f":"1-B_Ind_e_2","v":1},{"$f":"J30","v":1},{"$f":"1-B_Ind_e_3","v":1},{"$f":"L30","v":1},{"$f":"1-B_Ind_e_4","v":1},null,null,null,null,null,null,null,"B_Ind_VJ_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,{"$f":"F31","v":0},{"$f":"IF((B_Ind_e_1)=0,0,((B_Ind_VL_1)^2.5)/(B_Ind_e_1))","v":0},{"$f":"H31","v":0},{"$f":"IF((B_Ind_e_2)=0,0,((B_Ind_VL_2)^2.5)/(B_Ind_e_2))","v":0},{"$f":"J31","v":0},{"$f":"IF((B_Ind_e_3)=0,0,((B_Ind_VL_3)^2.5)/(B_Ind_e_3))","v":0},{"$f":"L31","v":0},{"$f":"IF((B_Ind_e_4)=0,0,((B_Ind_VL_4)^2.5)/(B_Ind_e_4))","v":0},null,null,null,null,null,null,null,"B_Ind_N_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F32","v":1},{"$f":"IF((B_Ind_N_1)=0,1,(B_Ind_N_1))","v":1},{"$f":"H32","v":1},{"$f":"IF((B_Ind_N_2)=0,1,(B_Ind_N_2))","v":1},{"$f":"J32","v":1},{"$f":"IF((B_Ind_N_3)=0,1,(B_Ind_N_3))","v":1},{"$f":"L32","v":1},{"$f":"IF((B_Ind_N_4)=0,1,(B_Ind_N_4))","v":1},null,null,null,null,null,null,null,"B_Ind_N_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F33","v":0},{"$f":"B_Ind_X_1*B_Ind_N_kor_2*B_Ind_N_kor_3*B_Ind_N_kor_4*B_Ind_Nb_kor_1*B_Ind_Nb_kor_2","v":0},{"$f":"H33","v":0},{"$f":"B_Ind_X_2*B_Ind_N_kor_1*B_Ind_N_kor_3*B_Ind_N_kor_4*B_Ind_Nb_kor_1*B_Ind_Nb_kor_2","v":0},{"$f":"J33","v":0},{"$f":"B_Ind_X_3*B_Ind_N_kor_1*B_Ind_N_kor_2*B_Ind_N_kor_4*B_Ind_Nb_kor_1*B_Ind_Nb_kor_2","v":0},{"$f":"L33","v":0},{"$f":"B_Ind_X_4*B_Ind_N_kor_1*B_Ind_N_kor_2*B_Ind_N_kor_3*B_Ind_Nb_kor_1*B_Ind_Nb_kor_2","v":0},null,null,null,null,null,null,null,"B_Ind_N_mel_n"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,null,null,null,null,null,{"$f":"(B_Ind_N_kor_1*B_Ind_N_kor_2*B_Ind_N_kor_3*B_Ind_N_kor_4*B_Ind_Nb_kor_1*B_Ind_Nb_kor_2)/(B_Ind_N_mel_1+B_Ind_N_mel_2+B_Ind_N_mel_3+B_Ind_N_mel_4+B_Ind_Nb_mel_1+B_Ind_Nb_mel_2)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,"B_Ind_N_tot"]
[]
[null,"Bygningsdata"]
[]
[null,"Terrændæk"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet"]
[null,"Type af terrændæk",null,null,{"$f":"D_Ind_Inddæk","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Inddæk"]
[null,"Betontværsnit","hb","mm",{"$f":"D_Ind_hb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_hb"]
[null,"Relativ luftfugtighed","RF","%",{"$f":"D_Ind_RF","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_RF"]
[null,"Vand/cement-tallet","v/c",null,{"$f":"D_Ind_wc","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_wc"]
[null,"Cementindhold","CM","kg/m3",{"$f":"D_Ind_CM","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_CM"]
[null,"Svindtid","ts","døgn",{"$f":"D_Ind_ts","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_ts"]
[null,"Materialekonst. for beton","Nb",null,{"$f":"D_Ind_Nb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Nb"]
[null,"Armeringsdiameter","da","mm",{"$f":"D_Ind_da","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_da"]
[null,"Armeringskonstant","k",null,{"$f":"D_Ind_k","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_k"]
[null,"Afstand mellem armeringsjern","Db","mm",{"$f":"D_Ind_Db","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Db"]
[null,"Dynamisk viskositet af luft","m","kg/(m * s)",{"$f":"D_Ind_my","v":1.8E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_my"]
[null,"Elasticitetskoeff. Stål","Es","MPa",{"$f":"D_Ind_Es","v":210000},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Es"]
[null,"Elasticitetskoeff. Beton","Eb","MPa",{"$f":"D_Ind_Eb","v":20000},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Eb"]
[]
[null,"Materialekonstant for terrændæk (app. 5.3 lign 68B)","KN","m³/(m²·s)","Beregnet værdi",{"$f":"G55","v":{"$error":"#DIV/0!"}},{"$f":"B_Ind_Nb/(B_Ind_hb/1000)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Kn"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet",null,null,null,"MST nr. 7 1998 - lign 25","aw=Acef/Sdw"]
[null,"Rumtype/anvendelse",null,null,{"$f":"D_Ind_anv","v":0},null,null,null,null,"MST nr. 7 1998 - lign 26","Acef=hb·ll",null,null,null,null,null,null,null,null,"B_Ind_anv"]
[null,"Loftshøjde (hb)","Lh","m",{"$f":"D_Ind_Lh","v":0},null,null,null,null,"MST nr. 7 1998 - lign 27","dw=k·da",null,null,null,null,null,null,null,null,"B_Ind_Lh"]
[null,"Luftskifte (Lb)","Ls","s-1",{"$f":"D_Ind_Ls","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Ls"]
[null,"Gulvbredde","lb","m",{"$f":"D_Ind_Lb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Lb"]
[null,"Gulvlængde","ll","m",{"$f":"D_Ind_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_Ll"]
[null,"Trykforskel over betondæk","DP","Pa",{"$f":"D_Ind_DP","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Ind_DP"]
[]
[null,"Beregnede bygningsdata"]
[null,null,null,null,null,null,null,null,"Begge betontyper"]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet",null,null,"Uarmeret betondæk",null,"Armeret betondæk",null,null,"Ligning 29+27","aw=(hb·Db)/(k·da)"]
[null,"Revnevidde \n(app 5.3 lign. 73 eller MST nr. 7 1998 - lign 40)","w","mm",{"$f":"D_Ind_w","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(B_Ind_Db),IndLigning40(B_Ind_hb,B_Ind_Db,B_Ind_k,B_Ind_da,B_Ind_Es, B_Ind_Eb,B_Ind_eg),IndLigning73(B_Ind_eg,B_Ind_Lb,B_Ind_Ll, B_Ind_ltot))","v":{"$error":"#VALUE!"}},null,null,"app 5.3 lign. 73","w=eg·lb·ll/ltot","Ligning 40","w=5·10-5·ss·(aw)½",null,"Ligning 39+28","ss=(Es·eg)/[(1+(Es/Eb)·j)·100]",null,null,null,null,"B_Ind_w"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligning 37","j=(p·da2)/(4·hb·Db)"]
[null,"Basissvindet (MST nr. 7 1998 - lign 31)","ec","%",{"$f":"D_Ind_ec","v":5.3293413173652694E-2},{"$f":"0.089*(100-B_Ind_RF)/(167-B_Ind_RF)","v":5.3293413173652694E-2},null,null,"Ligning 31","ec=[0,089·(100-RF)]/[167-RF]",null,null,null,null,null,null,null,null,null,"B_Ind_ec"]
[null,"Beton-sammensætningskoefficient \n(MST nr. 7 1998 - lign 32)","kb",null,{"$f":"D_Ind_Kb","v":0},{"$f":"IndLigning32(B_Ind_CM,B_Ind_wc)","v":0},null,null,"Ligning 32","kb=0,007·CM·(v/c+0,333)·v/c",null,null,null,null,null,null,null,null,null,"B_Ind_Kb"]
[null,"Gnmsn. Revneafstand\n(MST nr. 7 1998 - lign 41+42)","lw","mm",{"$f":"D_Ind_lw","v":{"$error":"#VALUE!"}},{"$f":"IndLigning41_42(B_Ind_hb,B_Ind_Db,B_Ind_k,B_Ind_da)","v":{"$error":"#VALUE!"}},null,null,null,null,"Ligning 41+42","lw=1,5 ·aw/p",null,null,null,null,null,null,null,"B_Ind_lw"]
[null,"Total revnelængde\n(app 5.3 lign. 72 eller MST nr. 7 1998 - lign 43)","ltot","m",{"$f":"D_Ind_ltot","v":0},{"$f":"IF(ISNUMBER(B_Ind_Db),IndLigning43(B_Ind_Lb,B_Ind_lw,B_Ind_Ll),IndLigning72(B_Ind_Lb,B_Ind_Ll))","v":0},null,null,"app 5.3 lign. 72","ltot=2·(lb+ll)","Ligning 43","ltot=[(lb·1000)/(lw)-1]·ll+[(ll·1000)/(lw)-1]·lb",null,null,null,null,null,null,null,"B_Ind_ltot"]
[null,"Vol. strøm gennem beton\n(app 5.3 lign. 70 eller MST nr. 7 1998 - lign 44)","qb","m³/(s )",{"$f":"D_Ind_q","v":{"$error":"#VALUE!"}},{"$f":"IndLigning44_70(B_Ind_ltot,B_Ind_w,B_Ind_DP,B_Ind_my,B_Ind_hb)","v":{"$error":"#VALUE!"}},null,null,"Lingning 44 / 70","qb=(ltot·w3·DP·10-6)/(12·m·hb)",null,null,null,null,null,null,null,null,null,"B_Ind_q"]
[null,"Vol. strøm i bygningen","qbyg","m³/(s )",{"$f":"D_ind_qbyg","v":0},{"$f":"B_Ind_Ls*B_Ind_Lh*B_Ind_Lb*B_Ind_Ll","v":0},null,null,null,"qbyg=Ls*Lh*lb*ll",null,null,null,null,null,null,null,null,null,"B_ind_qbyg"]
[null,"CHECK af volumenstrøm gennem beton","q_check","%",{"$f":"D_ind_qcheck","v":{"$error":"#VALUE!"}},{"$f":"B_Ind_q/B_ind_qbyg","v":{"$error":"#VALUE!"}},null,null,null,"q_check=qc/qbyg",null,null,null,null,null,null,null,null,null,"B_ind_qcheck"]
[null,"Vol. strøm gennem beton pr. kvadratmeter gulv \n(MST nr. 7 1998 - lign 45)","Qb","m³/(s· m²)",null,{"$f":"B_Ind_q/(B_Ind_Lb*B_Ind_Ll)","v":{"$error":"#VALUE!"}},null,null,"Ligning 30+34+33","eg=ec·kb·kd·kt=ec·kb·[0,25·(852+2·hb)/(132+2·hb)]·kt"]
[null,"Den frie svindtøjning\nMST nr. 7 1998 - lign 30 til lign36","eg","%",{"$f":"D_Ind_eg","v":{"$error":"#VALUE!"}},{"$f":"IndLigning30_33_34(B_Ind_ec,B_Ind_Kb,B_Ind_hb,B_Ind_ts)","v":{"$error":"#VALUE!"}},null,null,"Ligning 35","kt=tsa/(tsa+t0)",null,null,null,null,null,null,null,null,null,"B_Ind_eg"]
[null,null,null,null,null,null,null,null,"Ligning 36","a=0,75+0,125·b"]
[null,null,null,null,null,null,null,null,null,"b=(ln(0,025·2·hb))/ln2"]
[null,null,null,null,null,null,null,null,null,"t0=9·((10)½)ab"]
[]
[null,"Stoffer"]
[]
[null,null,null,null,"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
[null,"Navn","Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet"]
[null,"Forureningskomponent",null,null,{"$f":"D_Ind_stofnavn_1","v":""},null,{"$f":"D_Ind_stofnavn_2","v":""},null,{"$f":"D_Ind_stofnavn_3","v":""},null,{"$f":"D_Ind_stofnavn_4","v":""},null,null,null,null,null,null,null,null,"B_Ind_stofnavn_n"]
[null,"Poreluftskoncentration / test af andre værdier","CL","mg/m³",{"$f":"D_Ind_CL_1-D_Ind_C0_1","v":0},{"$f":"D_Ind_CL_1","v":0},{"$f":"D_Ind_CL_2-D_Ind_C0_2","v":0},{"$f":"D_Ind_CL_2","v":0},{"$f":"D_Ind_CL_3-D_Ind_C0_3","v":0},{"$f":"D_Ind_CL_3","v":0},{"$f":"D_Ind_CL_4-D_Ind_C0_4","v":0},{"$f":"D_Ind_CL_4","v":0},null,null,null,null,null,null,null,"B_Ind_CL_n"]
[null,"Baggrundskoncentration","C0","mg/m³",{"$f":"D_Ind_C0_1","v":0},null,{"$f":"D_Ind_C0_2","v":0},null,{"$f":"D_Ind_C0_3","v":0},null,{"$f":"D_Ind_C0_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_C0_n"]
[null,"Diffusionskoefficient luft","DL","m²/s",{"$f":"D_Ind_DL_1","v":0},null,{"$f":"D_Ind_DL_2","v":0},null,{"$f":"D_Ind_DL_3","v":0},null,{"$f":"D_Ind_DL_4","v":0},null,null,null,null,null,null,null,null,"B_Ind_DL_n"]
[null,null,null,null,"dag-1","sek-1","dag-1","sek-1","dag-1","sek-1","dag-1","sek-1"]
[null,"Nedbrydningskonstant i poreluft","k1","dag-1",{"$f":"Dataark_Indeklima!E94","v":0},{"$f":"IF(E94>0,E94/(24*60*60),1E-20)","v":9.9999999999999995E-21},{"$f":"Dataark_Indeklima!I94","v":0},{"$f":"IF(G94>0,G94/(24*60*60),1E-20)","v":9.9999999999999995E-21},{"$f":"Dataark_Indeklima!M94","v":0},{"$f":"IF(I94>0,I94/(24*60*60),1E-20)","v":9.9999999999999995E-21},{"$f":"Dataark_Indeklima!Q94","v":0},{"$f":"IF(K94>0,K94/(24*60*60),1E-20)","v":9.9999999999999995E-21},null,null,null,null,null,null,null,"B_Ind_k1_n"]
[null,"Indeklima beregninger"]
[null,"Flux gennem jorden (app. 5.3 ligning 63)","Jz","mg/(m² s)",null,{"$f":"IndLigning63(B_Ind_CL_1,B_Ind_X_tot,B_Ind_N_tot,B_Ind_DL_1,B_Ind_k1_1)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning63(B_Ind_CL_2,B_Ind_X_tot,B_Ind_N_tot,B_Ind_DL_2,B_Ind_k1_2)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning63(B_Ind_CL_3,B_Ind_X_tot,B_Ind_N_tot,B_Ind_DL_3,B_Ind_k1_3)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning63(B_Ind_CL_4,B_Ind_X_tot,B_Ind_N_tot,B_Ind_DL_4,B_Ind_k1_4)","v":{"$error":"#VALUE!"}},"Ligning 63","Jz=CL*X*sqrt(N_tot*DL*k1)*cosh((X-X)*sqrt(k1/(N_tot*DL))] / sinh[x*sqrt(k1/(N_tot*DL))]",null,null,null,null,null,"B_Ind_Jz_n"]
[null,"Kjord (app. 53 ligning 75)","Kjord","m³/(m²·s)",null,{"$f":"B_Ind_Jz_1/B_Ind_CL_1","v":{"$error":"#VALUE!"}},null,{"$f":"B_Ind_Jz_2/B_Ind_CL_2","v":{"$error":"#VALUE!"}},null,{"$f":"B_Ind_Jz_3/B_Ind_CL_3","v":{"$error":"#VALUE!"}},null,{"$f":"B_Ind_Jz_4/B_Ind_CL_4","v":{"$error":"#VALUE!"}},"Ligning 75","Kjord=Jz/CL",null,null,null,null,null,"B_Ind_Kjord_n"]
[null,"Stofspecifik materialekonstant","KN",null,null,{"$f":"B_Ind_Kn*B_Ind_DL_1","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Ind_Kn*B_Ind_DL_2","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Ind_Kn*B_Ind_DL_3","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Ind_Kn*B_Ind_DL_4","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,"B_Ind_Kn_x"]
[null,"Totalt bidrag til indeluft (app. 53 ligning 77)","Ci","mg/m³",null,{"$f":"IndLigning77(B_Ind_Kn_1,B_Ind_Lb,B_Ind_Ll,B_Ind_Ls,B_Ind_CL_1,B_Ind_Kjord_1,B_Ind_q,B_Ind_Lh)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning77(B_Ind_Kn_2,B_Ind_Lb,B_Ind_Ll,B_Ind_Ls,B_Ind_CL_2,B_Ind_Kjord_2,B_Ind_q,B_Ind_Lh)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning77(B_Ind_Kn_3,B_Ind_Lb,B_Ind_Ll,B_Ind_Ls,B_Ind_CL_3,B_Ind_Kjord_3,B_Ind_q,B_Ind_Lh)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning77(B_Ind_Kn_4,B_Ind_Lb,B_Ind_Ll,B_Ind_Ls,B_Ind_CL_4,B_Ind_Kjord_4,B_Ind_q,B_Ind_Lh)","v":{"$error":"#VALUE!"}},"Ligning 77","Ci=[(Kn+(qb/Ab))*Cl]/[(Lh*Ls)+(Kn/Kjord)*(Lh*Ls)+Kn+(1/kjord)*(Lh*Ls)*(qb/Ab)]",null,null,null,null,null,"B_Ind_Ci_n"]
[null,"Poreluftkonc. under gulv (app. 53 ligning 78)","Cp","mg/m³",null,{"$f":"IndLigning78(B_Ind_Ci_1,B_Ind_Lh,B_Ind_Ls,B_Ind_Kn_1,B_Ind_q,B_Ind_Lb,B_Ind_Ll)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning78(B_Ind_Ci_2,B_Ind_Lh,B_Ind_Ls,B_Ind_Kn_2,B_Ind_q,B_Ind_Lb,B_Ind_Ll)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning78(B_Ind_Ci_3,B_Ind_Lh,B_Ind_Ls,B_Ind_Kn_3,B_Ind_q,B_Ind_Lb,B_Ind_Ll)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning78(B_Ind_Ci_4,B_Ind_Lh,B_Ind_Ls,B_Ind_Kn_4,B_Ind_q,B_Ind_Lb,B_Ind_Ll)","v":{"$error":"#VALUE!"}},"Ligning 78","Cp=Ci*[(Lh*Ls)+Kn] / [Kn+(qb/(lb*Ll))]",null,null,null,null,null,"B_Ind_Cp_n"]
[null,"Diffusivt bidrag til indeluft  (app. 53 ligning 67A)","Cdi","mg/m³",null,{"$f":"IndLigning67A(B_Ind_Kn_1, B_Ind_Cp_1, B_Ind_Ci_1, B_Ind_Lh, B_Ind_Ls)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning67A(B_Ind_Kn_2,B_Ind_Cp_2,B_Ind_Ci_2,B_Ind_Lh,B_Ind_Ls)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning67A(B_Ind_Kn_3,B_Ind_Cp3,B_Ind_Ci_3,B_Ind_Lh,B_Ind_Ls)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning67A(B_Ind_Kn_4,B_Ind_Cp_4,B_Ind_Ci_4,B_Ind_Lh,B_Ind_Ls)","v":{"$error":"#VALUE!"}},"Lign 67A","Cdi=J/(Lh*Ls)=KN*(Ci-Cp)/(Lh*Ls)",null,null,null,null,null,"B_Ind_Cdi_n"]
[null,"Afdampningskriterie","afd-krit","mg/m³",{"$f":"D_Ind_afd_krit_1","v":0},null,{"$f":"D_Ind_afd_krit_2","v":0},null,{"$f":"D_Ind_afd_krit_3","v":0},null,{"$f":"D_Ind_afd_krit_4","v":0},null,null,"lign67","J=KN*(Ci-Cp)",null,null,null,null,"B_Ind_afd_krit_n"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,{"$f":"IF(D_Ind_afd_krit_1=0,\"Intet kriterie\",IF(B_Ind_Ci_1>B_Ind_afd_krit_1,B_Ind_Ci_1/B_Ind_afd_krit_1,\"Nej\"))","v":"Intet kriterie"},null,{"$f":"IF(D_Ind_afd_krit_2=0,\"Intet kriterie\",IF(B_Ind_Ci_2>B_Ind_afd_krit_2,B_Ind_Ci_2/B_Ind_afd_krit_2,\"Nej\"))","v":"Intet kriterie"},null,{"$f":"IF(D_Ind_afd_krit_3=0,\"Intet kriterie\",IF(B_Ind_Ci_3>B_Ind_afd_krit_3,B_Ind_Ci_3/B_Ind_afd_krit_3,\"Nej\"))","v":"Intet kriterie"},null,{"$f":"IF(D_Ind_afd_krit_4=0,\"Intet kriterie\",IF(B_Ind_Ci_4>B_Ind_afd_krit_4,B_Ind_Ci_4/B_Ind_afd_krit_4,\"Nej\"))","v":"Intet kriterie"},null,"Ligning 77","Kn={B_Ind_Kn}",null,"Kjord={B_Ind_Kjord}",null,null,"B_Ind_oskr_n"]
[null,"Afdampningskriterie","afd-krit-sum","mg/m³",{"$f":"D_Ind_afd_krit_sum_1","v":{"$error":"#NAME?"}},null,{"$f":"D_Ind_afd_krit_sum_2","v":{"$error":"#NAME?"}},null,{"$f":"D_Ind_afd_krit_sum_3","v":{"$error":"#NAME?"}},null,{"$f":"D_Ind_afd_krit_sum_4","v":{"$error":"#NAME?"}},null,null,null,"Ab={B_Ind_lb}*{B_Ind_ll}",null,"qb={B_Ind_q}",null,null,"B_Ind_afd_krit_sum_n"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,{"$f":"IF(ISNUMBER(E104),IF(F99>E104,F99/E104,\"Nej\"),\" \")","v":" "},null,{"$f":"IF(ISNUMBER(G104),IF(H99>G104,H99/G104,\"Nej\"),\" \")","v":" "},null,{"$f":"IF(ISNUMBER(I104),IF(J99>I104,J99/I104,\"Nej\"),\" \")","v":" "},null,{"$f":"IF(ISNUMBER(K104),IF(L99>K104,L99/K104,\"Nej\"),\" \")","v":" "},null,null,"Lb={B_Ind_Ls}",null,"hb={B_Ind_Lh}",null,null,"B_Ind_oskr_sum_n"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CL={B_Ind_CL}"]
["x"]
[null,"Beregning - Indeklima Krybekælder"]
[null,"Betongulv, membran og jord"]
[]
[null,null,null,null,"Betongulv (1)",null,"Membran (2)"]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Navn",null,null,{"$f":"D_IndK_navnb_1","v":0},null,{"$f":"D_IndK_navnb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_navnb_n"]
[null,"Tykkelse af lag","Xb","m",{"$f":"D_IndK_Xb_1","v":0},{"$f":"E114/1000","v":0},{"$f":"D_IndK_Xb_2","v":0},{"$f":"G114/1000","v":0},{"$f":"B_IndK_Xb_1+B_IndK_Xb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_IndK_Xb_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,{"$f":"D_IndK_Nb_1","v":0},null,{"$f":"D_IndK_Nb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Nb_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F116","v":1},{"$f":"IF((B_IndK_Nb_1)=0,1,(B_IndK_Nb_1))","v":1},{"$f":"H116","v":1},{"$f":"IF((B_IndK_Nb_2)=0,1,(B_IndK_Nb_2))","v":1},null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Nb_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F117","v":0},{"$f":"(B_IndK_Xb_1)*B_IndK_N_kor_1*B_IndK_N_kor_2*B_IndK_N_kor_3*B_IndK_N_kor_4*B_IndK_Nb_kor_2","v":0},{"$f":"H117","v":0},{"$f":"(B_IndK_Xb_2)*B_IndK_N_kor_1*B_IndK_N_kor_2*B_IndK_N_kor_3*B_IndK_N_kor_4*B_IndK_Nb_kor_1","v":0},null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Nb_mel_n"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Jordtype",null,null,{"$f":"D_IndK_jordtype_1","v":0},null,{"$f":"D_IndK_jordtype_2","v":0},null,{"$f":"D_IndK_jordtype_3","v":0},null,{"$f":"D_IndK_jordtype_4","v":0}]
[null,"Jordlag, Dybde fra","x1","m u.t.",{"$f":"F124","v":0},{"$f":"I114","v":0},{"$f":"B_IndK_lagtil_1","v":0},null,{"$f":"B_IndK_lagtil_2","v":0},null,{"$f":"B_IndK_lagtil_3","v":0},null,null,null,null,null,null,null,null,"B_IndK_lagfra_n"]
[null,"Jordlag, Dybde til","x2","m u.t.",{"$f":"D_IndK_lagtil_1","v":0},null,{"$f":"D_IndK_lagtil_2","v":0},null,{"$f":"D_IndK_lagtil_3","v":0},null,{"$f":"D_IndK_lagtil_4","v":0},null,null,null,null,null,null,null,null,"B_IndK_lagtil_n"]
[null,"Tykkelse af jordlag","X","m",{"$f":"F126","v":0},{"$f":"IF(ISNUMBER(IndK_Jord_dt1),B_IndK_lagtil_1-B_IndK_lagfra_1,0)","v":0},{"$f":"H126","v":0},{"$f":"IF(ISNUMBER(IndK_Jord_dt2),B_IndK_lagtil_2-B_IndK_lagfra_2,0)","v":0},{"$f":"J126","v":0},{"$f":"IF(ISNUMBER(IndK_Jord_dt3),B_IndK_lagtil_3-B_IndK_lagfra_3,0)","v":0},{"$f":"L126","v":0},{"$f":"IF(ISNUMBER(IndK_Jord_dt4),B_IndK_lagtil_4-B_IndK_lagfra_4,0)","v":0},{"$f":"B_IndK_X_1+B_IndK_X_2+B_IndK_X_3+B_IndK_X_4+I114","v":0},null,null,null,null,null,null,"B_IndK_X_n"]
[null,"Check af negativ højde",null,null,{"$f":"F127","v":0},{"$f":"IF(B_IndK_X_1<0,1,0)","v":0},{"$f":"H127","v":0},{"$f":"IF(B_IndK_X_2<0,1,0)","v":0},{"$f":"J127","v":0},{"$f":"IF(B_IndK_X_3<0,1,0)","v":0},{"$f":"L127","v":0},{"$f":"IF(B_IndK_X_4<0,1,0)","v":0},{"$f":"IF(B_IndK_negativ_X_1+B_IndK_negativ_X_2+B_IndK_negativ_X_3+B_IndK_negativ_X_4>0,\"FEJL!! Der er jordlag med negativ højde\",\" \")","v":" "},null,null,null,null,null,null,"B_IndK_negativ_X_n"]
[null,"Poreluftvolumen","VL",null,{"$f":"D_IndK_VL_1","v":0},null,{"$f":"D_IndK_VL_2","v":0},null,{"$f":"D_IndK_VL_3","v":0},null,{"$f":"D_IndK_VL_4","v":0},null,null,null,null,null,null,null,null,"B_IndK_VL_n"]
[null,"Vand-indhold","VV",null,{"$f":"D_IndK_VV_1","v":0},null,{"$f":"D_IndK_VV_2","v":0},null,{"$f":"D_IndK_VV_3","v":0},null,{"$f":"D_IndK_VV_4","v":0},null,null,null,null,null,null,null,null,"B_IndK_VV_n"]
[null,"Samlet porøsitet","e=VL+VV",null,{"$f":"F130","v":0},{"$f":"B_IndK_VL_1+B_IndK_VV_1","v":0},{"$f":"H130","v":0},{"$f":"B_IndK_VL_2+B_IndK_VV_2","v":0},{"$f":"J130","v":0},{"$f":"B_IndK_VL_3+B_IndK_VV_3","v":0},{"$f":"L130","v":0},{"$f":"B_IndK_VL_4+B_IndK_VV_4","v":0},null,null,null,null,null,null,null,"B_IndK_e_n"]
[null,"Volumen af jordskellet","VJ",null,{"$f":"F131","v":1},{"$f":"1-B_IndK_e_1","v":1},{"$f":"H131","v":1},{"$f":"1-B_IndK_e_2","v":1},{"$f":"J131","v":1},{"$f":"1-B_IndK_e_3","v":1},{"$f":"L131","v":1},{"$f":"1-B_IndK_e_4","v":1},null,null,null,null,null,null,null,"B_IndK_VJ_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,{"$f":"F132","v":0},{"$f":"IF((B_IndK_e_1)=0,0,((B_IndK_VL_1)^2.5)/(B_IndK_e_1))","v":0},{"$f":"H132","v":0},{"$f":"IF((B_IndK_e_2)=0,0,((B_IndK_VL_2)^2.5)/(B_IndK_e_2))","v":0},{"$f":"J132","v":0},{"$f":"IF((B_IndK_e_3)=0,0,((B_IndK_VL_3)^2.5)/(B_IndK_e_3))","v":0},{"$f":"L132","v":0},{"$f":"IF((B_IndK_e_4)=0,0,((B_IndK_VL_4)^2.5)/(B_IndK_e_4))","v":0},null,null,null,null,null,null,null,"B_IndK_N_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F133","v":1},{"$f":"IF((B_IndK_N_1)=0,1,(B_IndK_N_1))","v":1},{"$f":"H133","v":1},{"$f":"IF((B_IndK_N_2)=0,1,(B_IndK_N_2))","v":1},{"$f":"J133","v":1},{"$f":"IF((B_IndK_N_3)=0,1,(B_IndK_N_3))","v":1},{"$f":"L133","v":1},{"$f":"IF((B_IndK_N_4)=0,1,(B_IndK_N_4))","v":1},null,null,null,null,null,null,null,"B_IndK_N_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F134","v":0},{"$f":"(B_IndK_X_1)*B_IndK_N_kor_2*B_IndK_N_kor_3*B_IndK_N_kor_4*B_IndK_Nb_kor_1*B_IndK_Nb_kor_2","v":0},{"$f":"H134","v":0},{"$f":"(B_IndK_X_2)*B_IndK_N_kor_1*B_IndK_N_kor_3*B_IndK_N_kor_4*B_IndK_Nb_kor_1*B_IndK_Nb_kor_2","v":0},{"$f":"J134","v":0},{"$f":"(B_IndK_X_3)*B_IndK_N_kor_1*B_IndK_N_kor_2*B_IndK_N_kor_4*B_IndK_Nb_kor_1*B_IndK_Nb_kor_2","v":0},{"$f":"L134","v":0},{"$f":"(B_IndK_X_4)*B_IndK_N_kor_1*B_IndK_N_kor_2*B_IndK_N_kor_3*B_IndK_Nb_kor_1*B_IndK_Nb_kor_2","v":0},null,null,null,null,null,null,null,"B_IndK_N_mel_n"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,null,null,null,null,null,{"$f":"(B_IndK_N_kor_1*B_IndK_N_kor_2*B_IndK_N_kor_3*B_IndK_N_kor_4*B_IndK_Nb_kor_1*B_IndK_Nb_kor_2)/(B_IndK_N_mel_1+B_IndK_N_mel_2+B_IndK_N_mel_3+B_IndK_N_mel_4+B_IndK_Nb_mel_1+B_IndK_Nb_mel_2)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,"B_IndK_N_tot"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet"]
[null,"Rumtype/anvendelse",null,null,{"$f":"D_IndK_anv","v":0}]
[null,"Loftshøjde","Lh","m",{"$f":"D_IndK_Lh","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Lh"]
[null,"Luftskifte","Ls","s-1",{"$f":"D_IndK_Ls","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Ls"]
[null,"Gulvbredde","lb","m",{"$f":"IndK_Lb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Lb"]
[null,"Gulvlængde","ll","m",{"$f":"IndK_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Ll"]
[null,"Volumenstrøm i beboelse","Qbeboelse","m³/s",{"$f":"B_IndK_Ls*B_IndK_Lh*B_IndK_Lb*B_IndK_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_qbb"]
[]
[null,"Krybekælder"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet"]
[null,"Etageadskillelse",null,null,{"$f":"D_IndKk_anv","v":0}]
[null,"Reduktionsfaktoren","Rkr",null,{"$f":"D_IndKk_Rkr","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndKk_Rkr"]
[null,"Loftshøjde","Lh,kr","m",{"$f":"D_IndKk_Lh","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndKk_Lh"]
[null,"Gulvbredde","lb,kr","m",{"$f":"D_IndKk_Lb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndKk_Lb"]
[null,"Gulvlængde","ll,kr","m",{"$f":"D_IndKk_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndKk_Ll"]
[null,"Luftskifte","Ls,kr","s-1",{"$f":"D_IndKk_Ls","v":{"$error":"#DIV/0!"}},{"$f":"(B_IndK_qbb)/(B_IndKk_Lh*(B_IndKk_Lb*B_IndKk_Ll))","v":{"$error":"#DIV/0!"}},null,null,null,"Ls,kr=(Lh·Ls·lb·ll)/(Lh,kr·Ls,kr·lb,kr·ll,kr)  idet Rkr=1",null,null,null,null,null,null,null,null,null,"B_IndKk_Ls"]
[null,"Vol. strøm i krybekælder","Qbygn","m³/(s )",{"$f":"B_IndKk_qbyg_berg","v":{"$error":"#DIV/0!"}},{"$f":"B_IndKk_Ls*B_IndKk_Ll*B_IndKk_Lb*B_IndKk_Lh","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndKk_qbyg"]
[null,"Vol. strøm mellem krybekælder og stueetage","q,gv","m³/(s·m² )",{"$f":"D_IndK_qgv","v":{"$error":"#DIV/0!"}},{"$f":"IF(B_IndKk_qbyg>B_IndK_qbb/B_IndKk_Rkr,B_IndK_qbb/(B_IndKk_Rkr*(B_IndKk_Lb*B_IndKk_Ll)),B_IndKk_qbyg/(B_IndKk_Lb*B_IndKk_Ll))","v":{"$error":"#DIV/0!"}},null,null,null,"qgv=(Lh,kr·Ls,kr·lb,kr·ll,kr)/Rkr",null,null,null,null,null,null,null,null,null,"B_IndK_qgv"]
[null,"Check af volumenstrøm",null,null,null,{"$f":"IF(B_IndK_qgv*B_IndKk_Lh>B_IndKk_qbyg,\"FEJL: Luftstrømmen igennem etageadskillelsen er større end luftskiftet i krybekælderen\",\"\")","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_q_check"]
[null,"Beregnet reduktionsfaktor","R,kr",null,null,{"$f":"B_IndK_qbb/(B_IndK_qgv*B_IndKk_Lb*B_IndKk_Ll)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndKk_Rkr_bereg"]
[null,"Check af reduktionsfaktor",null,null,null,{"$f":"IF(B_IndKk_Rkr_bereg<1,\"FEJL: Luftstrømmen igennem etageadskillelsen er større end luftudskiftet i beboelsen\",\"\")","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"B_IndK_Rkr_check"]
[]
[null,"Stoffer"]
[]
[null,null,null,null,"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
[null,"Navn","Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet"]
[null,"Forureningskomponent",null,null,{"$f":"D_Ind_stofnavn_1","v":""},null,{"$f":"D_Ind_stofnavn_2","v":""},null,{"$f":"D_Ind_stofnavn_3","v":""},null,{"$f":"D_Ind_stofnavn_4","v":""},null,null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,"Poreluftskoncentration / test af andre værdier","CL","mg/m³",{"$f":"D_IndK_CL_1-D_Indk_C0_1","v":0},{"$f":"D_IndK_CL_1","v":0},{"$f":"D_IndK_CL_2-D_Indk_C0_2","v":0},{"$f":"D_IndK_CL_2","v":0},{"$f":"D_IndK_CL_3-D_Indk_C0_3","v":0},{"$f":"D_IndK_CL_3","v":0},{"$f":"D_IndK_CL_4-D_Indk_C0_4","v":0},{"$f":"D_IndK_CL_4","v":0},null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,"Baggrundskoncentration","C0","mg/m³",{"$f":"D_Indk_C0_1","v":0},null,{"$f":"D_Indk_C0_2","v":0},null,{"$f":"D_Indk_C0_3","v":0},null,{"$f":"D_Indk_C0_4","v":0},null,null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,"Diffusionskoefficient luft","DL","m²/s",{"$f":"D_IndK_DL_1","v":0},null,{"$f":"D_IndK_DL_2","v":0},null,{"$f":"D_IndK_DL_3","v":0},null,{"$f":"D_IndK_DL_4","v":0},null,null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,null,null,null,"dag-1","sek-1","dag-1","sek-1","dag-1","sek-1","dag-1","sek-1"]
[null,"Nedbrydningskonstant i poreluft","k1","dag-1",{"$f":"Dataark_Indeklima!E186","v":0},9.9999999999999995E-21,{"$f":"Dataark_Indeklima!I186","v":0},{"$f":"IF(G171>0,G171/(60*60*24),1E-20)","v":9.9999999999999995E-21},{"$f":"Dataark_Indeklima!M186","v":0},{"$f":"IF(I171>0,I171/(60*60*24),1E-20)","v":9.9999999999999995E-21},{"$f":"Dataark_Indeklima!Q186","v":0},{"$f":"IF(K171>0,K171/(60*60*24),1E-20)","v":9.9999999999999995E-21},null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,"Indeklima beregninger"]
[null,"Flux gennem jorden (app. 5.3 ligning 80)","Jz","mg/(m² s)",null,{"$f":"IndLigning80(B_IndK_CL_1,B_IndK_X_tot,B_IndK_N_tot,D_IndK_DL_1,B_Ind_k1_1)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning80(B_IndK_CL_2,B_IndK_X_tot,B_IndK_N_tot,D_IndK_DL_2,B_Ind_k1_2)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning80(B_IndK_CL_3,B_IndK_X_tot,B_IndK_N_tot,D_IndK_DL_3,B_Ind_k1_3)","v":{"$error":"#VALUE!"}},null,{"$f":"IndLigning80(B_IndK_CL_4,B_IndK_X_tot,B_IndK_N_tot,D_IndK_DL_4,B_Ind_k1_4)","v":{"$error":"#VALUE!"}},null,"Ligning 80","Jz=CL*X*sqrt(N_tot*DL*k1) / sinh[x*sqrt(k1/(N_tot*DL))]",null,null,null,null,"B_IndKk_Jz_n"]
[null,"Luftkoncentrationen i krybekælderen\n(app. 5.3 ligning 81)","Ckr","mg/m³",null,{"$f":"B_IndKk_Jz_1/(B_IndKk_Lh*B_IndKk_Ls)","v":{"$error":"#VALUE!"}},null,{"$f":"B_IndKk_Jz_2/(B_IndKk_Lh*B_IndKk_Ls)","v":{"$error":"#VALUE!"}},null,{"$f":"B_IndKk_Jz_3/(B_IndKk_Lh*B_IndKk_Ls)","v":{"$error":"#VALUE!"}},null,{"$f":"B_IndKk_Jz_4/(B_IndKk_Lh*B_IndKk_Ls)","v":{"$error":"#VALUE!"}},null,"Ligning 81","Ckr=Jz/Lkr*hkr",null,null,null,null,"B_IndKk_Ckr_n"]
[null,"Totalt bidrag til indeluft","Ci","mg/m³",null,{"$f":"D_IndKk_Ckr_1/B_IndKk_Rkr_bereg","v":{"$error":"#VALUE!"}},null,{"$f":"D_IndKk_Ckr_2/B_IndKk_Rkr_bereg","v":{"$error":"#VALUE!"}},null,{"$f":"D_IndKk_Ckr_3/B_IndKk_Rkr_bereg","v":{"$error":"#VALUE!"}},null,{"$f":"D_IndKk_Ckr_4/B_IndKk_Rkr_bereg","v":{"$error":"#VALUE!"}},null,null,"Ci=Ckr/Rkr",null,null,null,null,"B_IndK_Ci_n"]
[null,"Afdampningskriterie","afd-krit","mg/m³",{"$f":"D_Ind_afd_krit_1","v":0},null,{"$f":"D_Ind_afd_krit_2","v":0},null,{"$f":"D_Ind_afd_krit_3","v":0},null,{"$f":"D_Ind_afd_krit_4","v":0},null,null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,{"$f":"IF(D_Ind_afd_krit_1=0,\"Intet kriterie\",IF(B_IndK_Ci_1>B_Ind_afd_krit_1,B_IndK_Ci_1/B_Ind_afd_krit_1,\"Nej\"))","v":"Intet kriterie"},null,{"$f":"IF(D_Ind_afd_krit_2=0,\"Intet kriterie\",IF(B_IndK_Ci_2>B_Ind_afd_krit_2,B_IndK_Ci_2/B_Ind_afd_krit_2,\"Nej\"))","v":"Intet kriterie"},null,{"$f":"IF(D_Ind_afd_krit_3=0,\"Intet kriterie\",IF(B_IndK_Ci_3>B_Ind_afd_krit_3,B_IndK_Ci_3/B_Ind_afd_krit_3,\"Nej\"))","v":"Intet kriterie"},null,{"$f":"IF(D_Ind_afd_krit_4=0,\"Intet kriterie\",IF(B_IndK_Ci_4>B_Ind_afd_krit_4,B_IndK_Ci_4/B_Ind_afd_krit_4,\"Nej\"))","v":"Intet kriterie"},null,null,null,null,null,null,null,"B_IndK_oskr_n"]
[null,"Afdampningskriterie","afd-krit-sum","mg/m³",{"$f":"D_Ind_afd_krit_sum_1","v":{"$error":"#NAME?"}},null,{"$f":"D_Ind_afd_krit_sum_2","v":{"$error":"#NAME?"}},null,{"$f":"D_Ind_afd_krit_sum_3","v":{"$error":"#NAME?"}},null,{"$f":"D_Ind_afd_krit_sum_4","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,null,"Anvendes også under Indeklima-terrændæk"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,{"$f":"IF(ISNUMBER(E178),IF(F175>E178,F175/E178,\"Nej\"),\" \")","v":" "},null,{"$f":"IF(ISNUMBER(G178),IF(H175>G178,H175/G178,\"Nej\"),\" \")","v":" "},null,{"$f":"IF(ISNUMBER(I178),IF(J175>I178,J175/I178,\"Nej\"),\" \")","v":" "},null,{"$f":"IF(ISNUMBER(K178),IF(L175>K178,L175/K178,\"Nej\"),\" \")","v":" "},null,null,null,null,null,null,null,"B_IndK_oskr_sum_n"]

{"sheet":"Udskrift_Indeklima","index":19,"n_rows":161,"n_cols":11,"rows_kept":161,"cut":false,"hidden":true,"merged":[[23,0,24,0],[138,0,139,0],[104,1,113,9],[115,1,124,9],[46,2,46,3],[46,4,46,5],[46,6,46,7],[46,8,46,9],[126,1,135,9],[48,2,48,3],[48,4,48,5],[71,1,80,9],[82,1,91,9],[35,2,35,3],[35,4,35,5],[35,6,35,7],[35,8,35,9],[36,2,36,3],[36,4,36,5],[36,6,36,7],[36,8,36,9],[45,8,45,9],[48,6,48,7],[48,8,48,9],[49,2,49,3],[49,4,49,5],[49,6,49,7],[49,8,49,9],[60,1,69,9],[39,2,39,3],[39,4,39,5],[39,6,39,7],[39,8,39,9],[41,2,41,3],[41,4,41,5],[41,6,41,7],[41,8,41,9],[40,2,40,3],[40,4,40,5],[40,6,40,7],[40,8,40,9],[15,6,15,7],[15,8,15,9],[18,2,18,3],[18,4,18,5],[18,6,18,7],[18,8,18,9],[20,2,20,3],[21,2,21,3],[25,2,25,3],[25,4,25,5],[19,2,19,9],[37,8,38,9],[10,2,10,3],[10,8,10,9],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[7,2,7,3],[7,7,7,10],[8,2,8,3],[8,8,8,9],[9,2,9,3],[9,8,9,9],[13,2,13,3],[13,4,13,5],[13,6,13,7],[13,8,13,9],[14,2,14,3],[14,4,14,5],[14,6,14,7],[14,8,14,9],[27,2,27,5],[15,2,15,3],[15,4,15,5],[30,4,30,5],[31,4,31,5],[31,2,31,3],[45,2,45,3],[45,4,45,5],[45,6,45,7],[28,4,28,5],[37,2,38,3],[37,4,38,5],[37,6,38,7],[153,3,154,4],[153,5,154,6],[155,0,155,1],[155,3,155,4],[155,5,155,6],[150,3,150,4],[140,5,140,6],[141,5,141,6],[142,5,142,6],[143,5,143,6],[144,5,144,6],[145,5,145,6],[146,5,146,6],[147,5,147,6],[148,5,148,6],[149,5,149,6],[150,5,150,6],[145,3,145,4],[146,3,146,4],[147,3,147,4],[148,3,148,4],[149,3,149,4],[140,3,140,4],[141,3,141,4],[158,3,158,4],[159,3,159,4],[160,3,160,6],[156,5,156,6],[157,5,157,6],[158,5,158,6],[159,5,159,6],[156,3,156,4],[157,3,157,4],[2,1,2,5],[3,1,3,5],[4,1,4,5],[2,8,2,10],[3,8,3,10],[4,8,4,10],[5,1,5,10],[152,5,152,6],[37,0,38,0],[44,2,44,3],[44,4,44,5],[44,6,44,7],[44,8,44,9],[142,3,142,4],[143,3,143,4],[144,3,144,4],[93,1,102,9],[23,2,24,3],[23,4,24,5],[138,5,139,6],[138,3,139,4],[28,2,28,3],[29,2,29,3],[30,2,30,3]]}
["Indeklimaberegning "]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nummer:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jordparametre",null,"Indtastede data angives med fed"]
["Kommentar",{"$f":"IF( D_Ind_Inf_ComUds,\"ja\",\"nej\")","v":"nej"},"Membran",null,null,null,null,"Kapillarbrydende lag"]
["Membran type",null,{"$f":"IF(AND(D_Ind_navnb_1_syst=\"\",Ind_My_Memb=\"\"),\"\",D_Ind_navnb_1)","v":""},null,null,"Jord type",null,null,{"$f":"IF(AND(D_Ind_navnb_2_syst=\"\",Ind_My_Kab_2=\"\"),\"\",D_Ind_navnb_2)","v":""}]
["Tykkelse",null,{"$f":"IF(D_Ind_Xb_1<>0,D_Ind_Xb_1,\"\")","v":""},null,"mm","Tykkelse",null,null,{"$f":"IF(D_Ind_Xb_2<>0,D_Ind_Xb_2,\"\")","v":""},null,"m"]
["Materialekonstant",null,{"$f":"IF(B_Ind_Nb_1<>0,D_Ind_Nb_1,\"\")","v":""},null,null,"Materialekonstant",null,null,{"$f":"IF(B_Ind_Nb_2<>0,D_Ind_Nb_2,\"\")","v":""}]
[]
["Kommentar",{"$f":"IF( D_Ind_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
["Jordtype",null,{"$f":"IF(AND(D_Ind_jordtype_1_syst=\"\",Ind_My_Jord1=\"\"),\"\",D_Ind_jordtype_1)","v":""},null,{"$f":"IF(AND(D_Ind_jordtype_2_syst=\"\",Ind_My_Jord2=\"\"),\"\",D_Ind_jordtype_2)","v":""},null,{"$f":"IF(AND(D_Ind_jordtype_3_syst=\"\",Ind_My_Jord3=\"\"),\"\",D_Ind_jordtype_3)","v":""},null,{"$f":"IF(AND(D_Ind_jordtype_4_syst=\"\",Ind_My_Jord4=\"\"),\"\",D_Ind_jordtype_4)","v":""}]
["Jordlag, Dybde fra",null,{"$f":"IF($C$14<>\"\",D_Ind_lagfra_1,\"\")","v":""},null,{"$f":"IF($E$14<>\"\",D_Ind_lagfra_2,\"\")","v":""},null,{"$f":"IF($G$14<>\"\",D_Ind_lagfra_3,\"\")","v":""},null,{"$f":"IF($I$14<>\"\",D_Ind_lagfra_4,\"\")","v":""},null,"m u.t."]
["Jordlag, Dybde til",null,{"$f":"IF(D_Ind_lagtil_1<>0,D_Ind_lagtil_1,\"\")","v":""},null,{"$f":"IF(D_Ind_lagtil_2<>0,D_Ind_lagtil_2,\"\")","v":""},null,{"$f":"IF(D_Ind_lagtil_3<>0,D_Ind_lagtil_3,\"\")","v":""},null,{"$f":"IF(D_Ind_lagtil_4<>0,D_Ind_lagtil_4,\"\")","v":""},null,"m u.t."]
["Poreluftvolumen","VL",{"$f":"IF(D_Ind_VL_1_syst<>\"\",D_Ind_VL_1_syst,\"\")","v":""},{"$f":"IF(Ind_My_VL1<>\"\",Ind_My_VL1,\"\")","v":""},{"$f":"IF(D_Ind_VL_2_syst<>\"\",D_Ind_VL_2_syst,\"\")","v":""},{"$f":"IF(Ind_My_VL2<>\"\",Ind_My_VL2,\"\")","v":""},{"$f":"IF(D_Ind_VL_3_syst<>\"\",D_Ind_VL_3_syst,\"\")","v":""},{"$f":"IF(Ind_My_VL3<>\"\",Ind_My_VL3,\"\")","v":""},{"$f":"IF(D_Ind_VL_4_syst<>\"\",D_Ind_VL_4_syst,\"\")","v":""},{"$f":"IF(Ind_My_VL4<>\"\",Ind_My_VL4,\"\")","v":""}]
["Vand-indhold","VV",{"$f":"IF(D_Ind_VV_1_syst<>\"\",D_Ind_VV_1_syst,\"\")","v":""},{"$f":"IF(Ind_My_VV1<>\"\",Ind_My_VV1,\"\")","v":""},{"$f":"IF(D_Ind_VV_2_syst<>\"\",D_Ind_VV_2_syst,\"\")","v":""},{"$f":"IF(Ind_My_VV2<>\"\",Ind_My_VV2,\"\")","v":""},{"$f":"IF(D_Ind_VV_3_syst<>\"\",D_Ind_VV_3_syst,\"\")","v":""},{"$f":"IF(Ind_My_VV3<>\"\",Ind_My_VV3,\"\")","v":""},{"$f":"IF(D_Ind_VV_4_syst<>\"\",D_Ind_VV_4_syst,\"\")","v":""},{"$f":"IF(Ind_My_VV4<>\"\",Ind_My_VV4,\"\")","v":""}]
["Materialekonstant",null,{"$f":"IF(D_Ind_lagtil_1<>0,D_Ind_N_1,\"\")","v":""},null,{"$f":"IF(D_Ind_lagtil_2<>0,D_Ind_N_2,\"\")","v":""},null,{"$f":"IF(D_Ind_lagtil_3<>0,D_Ind_N_3,\"\")","v":""},null,{"$f":"IF(D_Ind_lagtil_4<>0,D_Ind_N_4,\"\")","v":""}]
[]
["Samlet materialekonstant"," KW",{"$f":"B_Ind_N_tot","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Ind_negativ_X_tot","v":" "}]
["Tykkelse af jordlag",null,{"$f":"D_Ind_X_tot","v":0},null,"m"]
["Terrændæk",null,"Kommentar",null,{"$f":"IF( D_Ind_Ter_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Type af terrændæk",null,{"$f":"IF(D_Ind_Inddæk_syst<>0,D_Ind_Inddæk_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_Inddæk<>\"\",D_Ind_Inddæk,\"\")","v":""}]
[]
["Betontværsnit","hb",{"$f":"IF(D_Ind_hb_syst<>\"\",D_Ind_hb_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_hb<>\"\",D_Ind_hb,\"\")","v":""},null,"mm","Øvrige detaljer se side 3"]
["Bygningsdata",null,"Kommentar",null,{"$f":"IF( D_Ind_Byg_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Rumtype/anvendelse",null,{"$f":"IF(D_Ind_anv<>0,D_Ind_anv,\"\")","v":""}]
["Loftshøjde","Lh",null,null,{"$f":"IF(D_Ind_Lh<>\"\",D_Ind_Lh,\"\")","v":0},null,"m"]
["Gulvbredde/-længde","lb/ll",null,null,{"$f":"IF(D_Ind_Lb<>\"\",D_Ind_Lb,\"\")","v":0},{"$f":"IF(D_Ind_Ll<>\"\",D_Ind_Ll,\"\")","v":0},"m"]
["Luftskifte","Ls",{"$f":"D_Ind_Ls_Sys","v":8.2999999999999998E-5},null,{"$f":"IF(Ind_My_Ls<>\"\",D_Ind_Ls,\"\")","v":""},null,"s-1"]
["Trykforskel over betondæk","DP",{"$f":"D_Ind_DP_Sys","v":5},null,{"$f":"IF(Ind_My_DP<>\"\",D_Ind_DP,\"\")","v":""},null,"Pa"]
[]
["Stoffer",null,"Angiv signifikant ciffer",null,null,4]
["Kommentar stoffer",{"$f":"IF( D_Ind_For_ComUds,\"ja\",\"nej\")","v":"nej"},"Kommentar beregning",null,null,{"$f":"IF( D_Ind_Ind_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Målepunkt",null,{"$f":"D_Enk_MP_1","v":""},null,{"$f":"D_Enk_MP_2","v":""},null,{"$f":"D_Enk_MP_3","v":""},null,{"$f":"D_Enk_MP_4","v":""}]
["Dato",null,{"$f":"D_Enk_dato_1","v":" "},null,{"$f":"D_Enk_dato_2","v":" "},null,{"$f":"D_Enk_dato_3","v":" "},null,{"$f":"D_Enk_dato_4","v":" "}]
["Forureningskomponent",null,{"$f":"D_Ind_stofnavn_1","v":""},null,{"$f":"D_Ind_stofnavn_2","v":""},null,{"$f":"D_Ind_stofnavn_3","v":""},null,{"$f":"D_Ind_stofnavn_4","v":""}]
[]
["Poreluftskoncentration ","CL",{"$f":"IF(D_Ind_CL_1<>0,D_Ind_CL_1,\"\")","v":""},null,{"$f":"IF(D_Ind_CL_2<>0,D_Ind_CL_2,\"\")","v":""},null,{"$f":"IF(D_Ind_CL_3<>0,D_Ind_CL_3,\"\")","v":""},null,{"$f":"IF(D_Ind_CL_4<>0,D_Ind_CL_4,\"\")","v":""},null,"mg/m³"]
["Ikkemålt værdi anvendt",null,{"$f":"IF(D_Ind_CL_1<>0,IF(ISNUMBER(Ind_My_CL_1),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Ind_CL_2<>0,IF(ISNUMBER(Ind_My_CL_2),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Ind_CL_3<>0,IF(ISNUMBER(Ind_My_CL_3),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Ind_CL_4<>0,IF(ISNUMBER(Ind_My_CL_4),\"Ja\",\"Nej\"),\"\")","v":""}]
["Baggrundskoncentration","C0",{"$f":"IF(Ind_My_C0_1<>\"\",D_Ind_C0_1,\"\")","v":""},null,{"$f":"IF(Ind_My_C0_2<>\"\",D_Ind_C0_2,\"\")","v":""},null,{"$f":"IF(Ind_My_C0_3<>\"\",D_Ind_C0_3,\"\")","v":""},null,{"$f":"IF(Ind_My_C0_4<>\"\",D_Ind_C0_4,\"\")","v":""},null,"mg/m³"]
["Diffusionskoefficient luft","DL",{"$f":"IF(D_Enk_DL_syst_1<>\"\",D_Enk_DL_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_DL_1<>\"\",Enk_My_DL_1,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_2<>\"\",D_Enk_DL_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_DL_2<>\"\",Enk_My_DL_2,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_3<>\"\",D_Enk_DL_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_DL_3<>\"\",Enk_My_DL_3,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_4<>\"\",D_Enk_DL_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_DL_4<>\"\",Enk_My_DL_4,\"\")","v":""},"m²/s"]
["Stofflux gennem beton","J",{"$f":"IF(ISNUMBER(D_Ind_Jz_1_syst),D_Ind_Jz_1_syst,\"\")","v":""},{"$f":"IF(Ind_My_Jz_1<>\"\",Ind_My_Jz_1,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Ind_Jz_2_syst),D_Ind_Jz_2_syst,\"\")","v":""},{"$f":"IF(Ind_My_Jz_2<>\"\",Ind_My_Jz_2,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Ind_Jz_3_syst),D_Ind_Jz_3_syst,\"\")","v":""},{"$f":"IF(Ind_My_Jz_3<>\"\",Ind_My_Jz_3,\"\")","v":""},{"$f":"IF(ISNUMBER(D_Ind_Jz_4_syst),D_Ind_Jz_4_syst,\"\")","v":""},{"$f":"IF(Ind_My_Jz_4<>\"\",Ind_My_Jz_4,\"\")","v":""},"mg/m²·s"]
["Poreluft koncentration u. gulv","Cp",{"$f":"IF(D_Ind_stofnavn_1<>\"\",(ROUND(D_Ind_Cp_1,Inde_ciffer-(INT(LOG(D_Ind_Cp_1))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_2<>\"\",(ROUND(D_Ind_Cp_2,Inde_ciffer-(INT(LOG(D_Ind_Cp_2))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_3<>\"\",(ROUND(D_Ind_Cp_3,Inde_ciffer-(INT(LOG(D_Ind_Cp_3))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_4<>\"\",(ROUND(D_Ind_Cp_4,Inde_ciffer-(INT(LOG(D_Ind_Cp_4))+1))),\"\")","v":""},null,"mg/m³"]
["Diffusivt bidrag til indeluft","Cdi",{"$f":"IF(D_Ind_stofnavn_1<>\"\",(ROUND(D_Ind_Cdi_1,Inde_ciffer-(INT(LOG(D_Ind_Cdi_1))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_2<>\"\",(ROUND(D_Ind_Cdi_2,Inde_ciffer-(INT(LOG(D_Ind_Cdi_2))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_3<>\"\",(ROUND(D_Ind_Cdi_3,Inde_ciffer-(INT(LOG(D_Ind_Cdi_3))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_4<>\"\",(ROUND(D_Ind_Cdi_4,Inde_ciffer-(INT(LOG(D_Ind_Cdi_4))+1))),\"\")","v":""},null,"mg/m³"]
["Totalbidrag til indeluft","Ci",{"$f":"IF(D_Ind_stofnavn_1<>\"\",(ROUND(D_Ind_Ci_1,Inde_ciffer-(INT(LOG(D_Ind_Ci_1))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_2<>\"\",(ROUND(D_Ind_Ci_2,Inde_ciffer-(INT(LOG(D_Ind_Ci_2))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_3<>\"\",(ROUND(D_Ind_Ci_3,Inde_ciffer-(INT(LOG(D_Ind_Ci_3))+1))),\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_4<>\"\",(ROUND(D_Ind_Ci_4,Inde_ciffer-(INT(LOG(D_Ind_Ci_4))+1))),\"\")","v":""},null,"mg/m³"]
["Afdampningskriterie",null,{"$f":"IF(D_Enk_afd_krit_syst_1<>\"\",D_Enk_afd_krit_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_1<>\"\",Enk_My_afd_krit_1,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_2<>\"\",D_Enk_afd_krit_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_2<>\"\",Enk_My_afd_krit_2,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_3<>\"\",D_Enk_afd_krit_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_3<>\"\",Enk_My_afd_krit_3,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_4<>\"\",D_Enk_afd_krit_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_4<>\"\",Enk_My_afd_krit_4,\"\")","v":""},"mg/m³"]
["Overskridelse af kriteriet",null,{"$f":"IF(D_Ind_stofnavn_1<>\"\",D_Ind_oskr_1,\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_2<>\"\",D_Ind_oskr_2,\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_3<>\"\",D_Ind_oskr_3,\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_4<>\"\",D_Ind_oskr_4,\"\")","v":""}]
["Anvendt brugerdata",null,{"$f":"IF(D_Ind_stofnavn_1<>\"\",D_Ind_Brugerdata_1,\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_2<>\"\",D_Ind_Brugerdata_2,\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_3<>\"\",D_Ind_Brugerdata_3,\"\")","v":""},null,{"$f":"IF(D_Ind_stofnavn_4<>\"\",D_Ind_Brugerdata_4,\"\")","v":""}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
[]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_Ind_Jord_Com<>\"\",D_Ind_Jord_Com,\"\")","v":""}]
["om jordlag"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger om",{"$f":"IF(D_Ind_Inf_Com<>\"\",D_Ind_Inf_Com,\"\")","v":""}]
["Influenszone og membran"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ind_For_Com<>\"\",D_Ind_For_Com,\"\")","v":""}]
["om forurening"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Kem_Com<>\"\",D_Enk_Kem_Com,\"\")","v":""}]
["om kemiske stoffer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ind_Ind_Com<>\"\",D_Ind_Ind_Com,\"\")","v":""}]
["beregninger"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ind_Byg_Com<>\"\",D_Ind_Byg_Com,\"\")","v":""}]
["om bygningsdata"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ind_Ter_Com<>\"\",D_Ind_Ter_Com,\"\")","v":""}]
["om terrændæk"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Detailoplysninger om terrændæk"]
["Type af terrændæk",null,null,{"$f":"IF(D_Ind_Inddæk_syst<>0,D_Ind_Inddæk_syst,\"\")","v":""},null,{"$f":"IF(D_Ind_Inddæk<>0,D_Ind_Inddæk,\"\")","v":""}]
[]
["Relativ luftfugtighed",null,"RF",{"$f":"IF(D_Ind_RF_syst<>0,D_Ind_RF_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_RF<>\"\",D_Ind_RF,\"\")","v":""},null,"%"]
["Vand/cement-tallet",null,"v/c",{"$f":"IF(D_Ind_wc_syst<>0,D_Ind_wc_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_wc<>\"\",D_Ind_wc,\"\")","v":""}]
["Cementindhold",null,"CM",{"$f":"IF(D_Ind_CM_syst<>0,D_Ind_CM_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_CM<>\"\",D_Ind_CM,\"\")","v":""},null,"kg/m³"]
["Svindtid",null,"ts",{"$f":"IF(D_Ind_ts_syst<>0,D_Ind_ts_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_ts<>\"\",D_Ind_ts,\"\")","v":""},null,"døgn"]
["Materialekonst. for beton",null,"Nb",{"$f":"IF(D_Ind_Nb_syst<>0,D_Ind_Nb_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_Nb<>\"\",D_Ind_Nb,\"\")","v":""}]
["Armeringsdiameter",null,"da",{"$f":"IF(D_Ind_daCh<>0,D_Ind_daCh,\"\")","v":""},null,{"$f":"IF(Ind_My_da<>\"\",D_Ind_da,\"\")","v":""},null,"mm"]
["Armeringskonstant",null,"k",{"$f":"IF(D_Ind_k_syst<>0,D_Ind_k_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_k<>\"\",D_Ind_k,\"\")","v":""}]
["Afstand mellem \narmeringsjern",null,"Db",{"$f":"IF(D_Ind_Db_syst<>0,D_Ind_Db_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_Db<>\"\",D_Ind_Db,\"\")","v":""},null,"mm"]
["Dynamisk viskositet af luft",null,"m",{"$f":"IF(D_Ind_my_syst<>0,D_Ind_my_syst,\"\")","v":1.8E-5},null,{"$f":"IF(Ind_My_my<>\"\",D_Ind_my,\"\")","v":""},null,"kg/m·s"]
["Elasticitetskoeff. Beton",null,"Eb",{"$f":"IF(D_Ind_Eb_syst<>0,D_Ind_Eb_syst,\"\")","v":20000},null,{"$f":"IF(Ind_My_Eb<>\"\",D_Ind_Eb,\"\")","v":""},null,"MPa"]
["Elasticitetskoeff. Stål (MPa)",null,"Es",{"$f":"IF(D_Ind_Es_syst<>0,D_Ind_Es_syst,\"\")","v":210000},null,{"$f":"IF(Ind_My_Es<>\"\",D_Ind_Es,\"\")","v":""},null,"MPa"]
[]
["Beregnede data om terrændæk"]
[null,null,null,"Beregnede værdier",null,"Indtastede (målte) værdier"]
[]
["Materialekonstant for terrændæk",null,"KN",{"$f":"D_Ind_Kn","v":{"$error":"#DIV/0!"}}]
["Revnevidde ",null,"w",{"$f":"IF(D_Ind_w_Ber,D_Ind_w_Ber,\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Ind_My_w<>\"\",D_Ind_w,\"\")","v":""},null,"mm"]
["Gnmsn. Revneafstand",null,"lw",{"$f":"IF(D_Ind_lw_Ber,D_Ind_lw_Ber,\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Ind_My_Lw<>\"\",D_Ind_lw,\"\")","v":""},null,"mm"]
["Total revnelængde",null,"ltot",{"$f":"IF(D_Ind_ltot_Ber,D_Ind_ltot_Ber,\"\")","v":""},null,{"$f":"IF(Ind_My_ltot<>\"\",D_Ind_ltot,\"\")","v":""},null,"mm"]
["Vol. strøm gennem beton",null,"qb",{"$f":"IF(D_Ind_q_Ber,D_Ind_q_Ber,\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Ind_My_q<>\"\",D_Ind_q,\"\")","v":""},null,"m³/s"]
["Vol. strøm i bygningen",null,"qbyg",{"$f":"D_ind_qbyg","v":0},null,null,null,"m³/s"]

{"sheet":"Udskrift_Indeklima_KK","index":20,"n_rows":105,"n_cols":11,"rows_kept":105,"cut":false,"hidden":true,"merged":[[26,2,26,3],[33,6,33,7],[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,10],[2,8,2,10],[3,8,3,10],[4,8,4,10],[7,4,7,5],[8,2,9,3],[8,4,9,5],[14,2,14,3],[14,4,14,5],[13,2,13,3],[13,4,13,5],[42,1,43,1],[24,8,24,9],[34,2,34,3],[34,4,34,5],[34,6,34,7],[34,8,34,9],[33,2,33,3],[33,4,33,5],[37,6,37,7],[42,2,42,3],[42,4,42,5],[42,6,42,7],[42,8,42,9],[33,8,33,9],[27,2,27,3],[37,8,37,9],[59,1,68,9],[70,1,79,9],[81,1,90,9],[47,2,47,3],[47,4,47,5],[47,6,47,7],[47,8,47,9],[48,2,48,3],[48,4,48,5],[48,6,48,7],[48,8,48,9],[52,1,52,4],[53,1,53,4],[52,7,52,9],[53,7,53,9],[92,1,101,9],[103,1,112,9],[28,2,28,3],[26,8,26,9],[27,8,27,9],[28,8,28,9],[38,2,38,3],[38,4,38,5],[38,6,38,7],[38,8,38,9],[39,2,39,3],[39,4,39,5],[39,6,39,7],[39,8,39,9],[37,2,37,3],[37,4,37,5],[13,6,13,7],[13,8,13,9],[14,6,14,7],[14,8,14,9],[16,8,16,9],[19,8,19,9],[15,2,15,3],[15,4,15,5],[15,6,15,7],[15,8,15,9],[24,0,25,0],[24,2,25,3],[16,2,16,3],[16,4,16,5],[16,6,16,7],[21,2,21,3],[22,2,22,3],[19,2,19,3],[19,4,19,5],[19,6,19,7],[35,0,36,0],[35,2,36,3],[35,4,36,5],[35,6,36,7],[35,8,36,9],[45,2,45,3],[45,4,45,5],[45,6,45,7],[45,8,45,9],[43,2,43,3],[43,4,43,5],[43,6,43,7],[43,8,43,9],[44,2,44,3],[44,4,44,5],[44,6,44,7],[44,8,44,9]]}
["Indeklimaberegning "]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nummer:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jordparametre",null,"Indtastede data angives med fed"]
["Kommentar",{"$f":"IF( D_Ind_Ven_Jord_Com<>\"\",\"ja\",\"nej\")","v":"nej"},"Gulv i kr.kælder",null,"Membran"]
["Gulv/Membran type",null,{"$f":"IF(D_IndK_navnb_1=0,\"\",D_IndK_navnb_1)","v":""},null,{"$f":"IF(D_IndK_navnb_2=0,\"\",D_IndK_navnb_2)","v":""}]
[]
["Tykkelse","mm",{"$f":"IF(D_IndK_Xb_1_syst<>0,D_IndK_Xb_1_syst,\"\")","v":""},{"$f":"IF(IndK_My_Xb_1<>\"\",IndK_My_Xb_1,\"\")","v":""},{"$f":"IF(D_IndK_Xb_2_syst<>0,D_IndK_Xb_2_syst,\"\")","v":""},{"$f":"IF(IndK_My_Xb_2<>\"\",IndK_My_Xb_2,\"\")","v":""}]
["Materialekonstant",null,{"$f":"IF(D_IndK_Nb_1_syst<>0,D_IndK_Nb_1_syst,\"\")","v":""},{"$f":"IF(IndK_My_Nb_1<>\"\",IndK_My_Nb_1,\"\")","v":""},{"$f":"IF(D_IndK_Nb_2_syst<>0,D_IndK_Nb_2_syst,\"\")","v":""},{"$f":"IF(IndK_My_Nb_2<>\"\",IndK_My_Nb_2,\"\")","v":""}]
[]
[null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
["Jordtype",null,{"$f":"IF(AND(D_IndK_jordtype_1_syst=\"\",IndK_My_Jord1=\"\"),\"\",D_IndK_jordtype_1)","v":""},null,{"$f":"IF(AND(D_IndK_jordtype_2_syst=\"\",IndK_My_Jord2=\"\"),\"\",D_IndK_jordtype_2)","v":""},null,{"$f":"IF(AND(D_IndK_jordtype_3_syst=\"\",IndK_My_Jord3=\"\"),\"\",D_IndK_jordtype_3)","v":""},null,{"$f":"IF(AND(D_IndK_jordtype_4_syst=\"\",IndK_My_Jord4=\"\"),\"\",D_IndK_jordtype_4)","v":""}]
["Jordlag, Dybde fra",null,{"$f":"IF(D_IndK_lagtil_1<>0,D_IndK_lagfra_1,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_2<>0,D_IndK_lagfra_2,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_3<>0,D_IndK_lagfra_3,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_4<>0,D_IndK_lagfra_4,\"\")","v":""},null,"m u.t."]
["Jordlag, Dybde til",null,{"$f":"IF(D_IndK_lagtil_1<>0,D_IndK_lagtil_1,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_2<>0,D_IndK_lagtil_2,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_3<>0,D_IndK_lagtil_3,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_4<>0,D_IndK_lagtil_4,\"\")","v":""},null,"m u.t."]
["Poreluftvolumen","VL",{"$f":"IF(D_IndK_VL_1_syst<>\"\",D_IndK_VL_1_syst,\"\")","v":""},{"$f":"IF(IndK_My_VL1<>\"\",IndK_My_VL1,\"\")","v":""},{"$f":"IF(D_IndK_VL_2_syst<>\"\",D_IndK_VL_2_syst,\"\")","v":""},{"$f":"IF(IndK_My_VL2<>\"\",IndK_My_VL2,\"\")","v":""},{"$f":"IF(D_IndK_VL_3_syst<>\"\",D_IndK_VL_3_syst,\"\")","v":""},{"$f":"IF(IndK_My_VL3<>\"\",IndK_My_VL3,\"\")","v":""},{"$f":"IF(D_IndK_VL_4_syst<>\"\",D_IndK_VL_4_syst,\"\")","v":""},{"$f":"IF(IndK_My_VL4<>\"\",IndK_My_VL4,\"\")","v":""}]
["Vand-indhold","VV",{"$f":"IF(D_IndK_VV_1_syst<>\"\",D_IndK_VV_1_syst,\"\")","v":""},{"$f":"IF(IndK_My_VV1<>\"\",IndK_My_VV1,\"\")","v":""},{"$f":"IF(D_IndK_VV_2_syst<>\"\",D_IndK_VV_2_syst,\"\")","v":""},{"$f":"IF(IndK_My_VV2<>\"\",IndK_My_VV2,\"\")","v":""},{"$f":"IF(D_IndK_VV_3_syst<>\"\",D_IndK_VV_3_syst,\"\")","v":""},{"$f":"IF(IndK_My_VV3<>\"\",IndK_My_VV3,\"\")","v":""},{"$f":"IF(D_IndK_VV_4_syst<>\"\",D_IndK_VV_4_syst,\"\")","v":""},{"$f":"IF(IndK_My_VV4<>\"\",IndK_My_VV4,\"\")","v":""}]
["Materialekonstant",null,{"$f":"IF(D_IndK_lagtil_1<>0,D_IndK_N_1,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_2<>0,D_IndK_N_2,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_3<>0,D_IndK_N_3,\"\")","v":""},null,{"$f":"IF(D_IndK_lagtil_4<>0,D_IndK_N_4,\"\")","v":""}]
[]
["Samlet materialekonstant"," KW",{"$f":"B_IndK_N_tot","v":{"$error":"#DIV/0!"}}]
["Tykkelse af jordlag",null,{"$f":"D_IndK_X_tot","v":0},null,"m",{"$f":"D_IndK_negativ_X_tot","v":" "}]
["Bygningsdata",null,"Kommentar",null,{"$f":"IF( D_Ind_Ven_Byg_Com<>\"\",\"ja\",\"nej\")","v":"nej"},null,null,"Kommentar krybekælder",{"$f":"IF( D_Ind_Ven_Kryb_Com<>\"\",\"ja\",\"nej\")","v":"nej"}]
["Rumtype/anvendelse",null,{"$f":"IF(D_IndK_anv<>0,D_IndK_anv,\"\")","v":""},null,null,null,"Etageadskillelse",null,{"$f":"IF(D_IndKk_anv<>0,D_IndKk_anv,\"\")","v":""}]
[null,null,null,null,null,null,"Reduktionsfaktor","Rkr",{"$f":"IF(D_IndKk_Rkr_syst<>0,D_IndKk_Rkr_syst,\"\")","v":""},{"$f":"IF(IndKk_Rkr<>\"\",D_IndKk_Rkr,\"\")","v":""}]
["Loftshøjde","Lh",{"$f":"IF(D_IndK_Lh<>0,D_IndK_Lh,\"\")","v":""},null,"m",null,"Loftshøjde","Lh",{"$f":"IF(D_IndKk_Lh<>0,D_IndKk_Lh,\"\")","v":""},null,"m"]
["Gulvbredde","lb",{"$f":"IF(D_IndK_Lb<>0,D_IndK_Lb,\"\")","v":""},null,"m",null,"Gulvbredde","lb",{"$f":"IF(D_IndKk_Lb<>0,D_IndKk_Lb,\"\")","v":""},null,"m"]
["Gulvlængde","ll",{"$f":"IF(D_IndK_Ll<>0,D_IndK_Ll,\"\")","v":""},null,"m",null,"Gulvlængde","ll",{"$f":"IF(D_IndKk_Ll<>0,D_IndKk_Ll,\"\")","v":""},null,"m"]
["Luftskifte","Ls",{"$f":"D_IndK_Ls_syst","v":8.2999999999999998E-5},{"$f":"IF(IndK_Ls<>\"\",D_IndK_Ls,\"\")","v":""},"m³/s",null,"Luftskifte","Ls",{"$f":"D_IndKk_Ls_berg","v":{"$error":"#DIV/0!"}},{"$f":"IF(IndKk_Ls<>\"\",D_IndKk_Ls,\"\")","v":""},"m³/s"]
[null,null,null,null,null,null,"Volumenstrøm gennem etageadskillelsen","qgv",{"$f":"IF(D_IndK_qgv_Beregn<>0,D_IndK_qgv_Beregn,\"\")","v":{"$error":"#DIV/0!"}},{"$f":"IF(IndK_qgv<>\"\",IndK_qgv,\"\")","v":""}]
["Stoffer",null,"Angiv signifikant ciffer",null,3]
["Kommentar om stoffer og beregning",null,null,null,{"$f":"IF( D_Ind_Ven_For_Com<>\"\",\"ja\",\"nej\")","v":"nej"}]
["Målepunkt",null,{"$f":"D_Enk_MP_1","v":""},null,{"$f":"D_Enk_MP_2","v":""},null,{"$f":"D_Enk_MP_3","v":""},null,{"$f":"D_Enk_MP_4","v":""}]
["Dato",null,{"$f":"D_Enk_dato_1","v":" "},null,{"$f":"D_Enk_dato_2","v":" "},null,{"$f":"D_Enk_dato_3","v":" "},null,{"$f":"D_Enk_dato_4","v":" "}]
["Forureningskomponent",null,{"$f":"D_Ind_stofnavn_1","v":""},null,{"$f":"D_Ind_stofnavn_2","v":""},null,{"$f":"D_Ind_stofnavn_3","v":""},null,{"$f":"D_Ind_stofnavn_4","v":""}]
[]
["Poreluftskoncentration ","CL",{"$f":"IF(D_IndK_CL_1<>0,D_IndK_CL_1,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,D_IndK_CL_2,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,D_IndK_CL_3,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,D_IndK_CL_4,\"\")","v":""},null,"mg/m³"]
["Ikke målt værdi anvendt",null,{"$f":"IF(D_IndK_CL_1<>0,IF(ISNUMBER(IndK_My_CL_1),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,IF(ISNUMBER(IndK_My_CL_2),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,IF(ISNUMBER(IndK_My_CL_3),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,IF(ISNUMBER(IndK_My_CL_4),\"Ja\",\"Nej\"),\"\")","v":""}]
["Baggrundskoncentration","C0",{"$f":"IF(D_IndK_CL_1<>0,D_Indk_C0_1,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,D_Indk_C0_2,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,D_Indk_C0_3,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,D_Indk_C0_4,\"\")","v":""},null,"mg/m³"]
["Diffusionskoefficient luft","DL",{"$f":"IF(D_Enk_DL_syst_1<>\"\",D_Enk_DL_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_DL_1<>\"\",Enk_My_DL_1,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_2<>\"\",D_Enk_DL_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_DL_2<>\"\",Enk_My_DL_2,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_3<>\"\",D_Enk_DL_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_DL_3<>\"\",Enk_My_DL_3,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_4<>\"\",D_Enk_DL_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_DL_4<>\"\",Enk_My_DL_4,\"\")","v":""},"m²/s"]
[]
["konc. i krybekælder beregnet","Ckr",{"$f":"IF(D_IndK_CL_1<>0,(ROUND(D_IndKk_Ckr_1_beregn,Indk_ciffer-(INT(LOG(D_IndKk_Ckr_1_beregn))+1))),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,(ROUND(D_IndKk_Ckr_2_beregn,Indk_ciffer-(INT(LOG(D_IndKk_Ckr_2_beregn))+1))),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,(ROUND(D_IndKk_Ckr_3_beregn,Indk_ciffer-(INT(LOG(D_IndKk_Ckr_3_beregn))+1))),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,(ROUND(D_IndKk_Ckr_4_beregn,Indk_ciffer-(INT(LOG(D_IndKk_Ckr_4_beregn))+1))),\"\")","v":""},null,"mg/m²·s"]
["indtastet",null,{"$f":"IF(IndKk_My_Ckr_1<>\"\",IndKk_My_Ckr_1,\"\")","v":""},null,{"$f":"IF(IndKk_My_Ckr_2<>\"\",IndKk_My_Ckr_2,\"\")","v":""},null,{"$f":"IF(IndKk_My_Ckr_3<>\"\",IndKk_My_Ckr_3,\"\")","v":""},null,{"$f":"IF(IndKk_My_Ckr_4<>\"\",IndKk_My_Ckr_4,\"\")","v":""},null,"mg/m³"]
[]
["Totalbidrag til indeluft","Ci",{"$f":"IF(D_IndK_CL_1<>0,(ROUND(D_IndK_Ci_1,Indk_ciffer-(INT(LOG(D_IndK_Ci_1))+1))),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,(ROUND(D_IndK_Ci_2,Indk_ciffer-(INT(LOG(D_IndK_Ci_2))+1))),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,(ROUND(D_IndK_Ci_3,Indk_ciffer-(INT(LOG(D_IndK_Ci_3))+1))),\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,(ROUND(D_IndK_Ci_4,Indk_ciffer-(INT(LOG(D_IndK_Ci_4))+1))),\"\")","v":""},null,"mg/m³"]
["Afdampningskriterie",null,{"$f":"IF(D_Enk_afd_krit_syst_1<>\"\",D_Enk_afd_krit_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_1<>\"\",Enk_My_afd_krit_1,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_2<>\"\",D_Enk_afd_krit_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_2<>\"\",Enk_My_afd_krit_2,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_3<>\"\",D_Enk_afd_krit_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_3<>\"\",Enk_My_afd_krit_3,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_4<>\"\",D_Enk_afd_krit_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_4<>\"\",Enk_My_afd_krit_4,\"\")","v":""},"mg/m³"]
["Overskridelse af kriteriet",null,{"$f":"IF(D_IndK_CL_1<>0,D_IndK_oskr_1,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,D_IndK_oskr_2,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,D_IndK_oskr_3,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,D_IndK_oskr_4,\"\")","v":""}]
["Anvendt brugerdata",null,{"$f":"IF(D_IndK_CL_1<>0,D_IndK_Brugerdata_1,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_2<>0,D_IndK_Brugerdata_2,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_3<>0,D_IndK_Brugerdata_3,\"\")","v":""},null,{"$f":"IF(D_IndK_CL_4<>0,D_IndK_Brugerdata_4,\"\")","v":""}]
[]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_Ind_Ven_Jord_Com<>\"\",D_Ind_Ven_Jord_Com,\"\")","v":""}]
["om jordlag"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger om",{"$f":"IF(D_Ind_Ven_Byg_Com<>\"\",D_Ind_Ven_Byg_Com,\"\")","v":""}]
["bygningsdata"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger om",{"$f":"IF(D_Ind_Ven_Kryb_Com<>\"\",D_Ind_Ven_Kryb_Com,\"\")","v":""}]
["Krybekælderen"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger om",{"$f":"IF(D_Enk_Kem_Com<>\"\",D_Enk_Kem_Com,\"\")","v":""}]
["kemiske stoffer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger om",{"$f":"IF(D_Ind_Ven_For_Com<>\"\",D_Ind_Ven_For_Com,\"\")","v":""}]
["forureningen og beregning"]

{"sheet":"Vejledning_Indeklima","index":21,"n_rows":165,"n_cols":2,"rows_kept":165,"cut":false,"hidden":true,"merged":[[110,1,112,10],[164,1,164,10],[123,1,124,11],[126,1,134,11],[137,1,147,11],[157,1,161,11],[153,1,154,11],[149,1,150,11],[115,1,120,11],[99,1,99,11],[100,1,102,11],[104,1,105,11],[95,1,97,10],[107,1,107,11],[84,1,86,5],[88,1,88,10],[89,1,92,5],[94,1,94,10],[63,1,63,11],[64,1,64,5],[81,1,82,5],[65,1,67,5],[69,1,72,5],[74,1,79,5],[51,1,53,11],[55,1,55,11],[56,1,58,11],[60,1,61,11],[44,1,46,11],[48,1,48,11],[50,1,50,10],[28,1,41,5],[13,1,24,5],[25,1,26,5],[43,1,43,10],[2,1,2,11],[3,1,5,11],[7,1,8,11],[6,1,6,11],[10,1,10,11],[12,1,12,5]]}
[]
[null,"Vejledning  - Indeklima"]
[null,"Formål"]
[null,"I dette ark kan der foretages beregning af bidraget til indeklimaet fra en forurening der afdamper gennem den umættet zone, og trænger ind i en bygning. Beregningerne kan foretages for bygninger med et betondæk (enten kælderdæk eller terrændæk) eller for bygninger med krybekælder.\n\nNærmere detaljer om beregningerne er beskrevet i Miljørapport. \"Opgradering af JAGG. Indeklimamodul 2010\". Miljøstyrelsen."]
[]
[]
[]
[null,"Nærmere detaljer om beregningerne er beskrevet i Miljørapport. \"Opgradering af JAGG. Indeklimamodul 2010\". Miljøstyrelsen."]
[]
[]
[null,"Beregninger for betondæk"]
[]
[null,"Umættet zone:"]
[null,"Den umættede zone som forureningen skal afdampe gennem skal indledningsvis beskrives. Den umættede zone medtager både de jordlag som findes mellem forureningen og betondækket, et eventuelt kapillarbrydende lag og en eventuel membran. De ønskede lag kan vælges som standardtyper ved at klikke på knappen \"Jordtype\", \"Membran\" eller \"Kapillarbrydende lag\". Alternativt kan der vælges lag fra \"Egen Liste\", eller der kan manuelt indtastes værdier i de hvide felter. Se iøvrigt bemærkninger om anvendelse af valglister under afsnittet generelt.\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Når det ønskede lag er valgt, angives lagets tykkelse, porøsitet og/eller materialekonstant"]
[]
[]
[null,"NB! I beregningerne af gastransport i den umættede zone kan der medtages nedbrydning, hvis der under fanebladet enkeltstodffer indtastes en nedbrydnings-konstant for det pågældende stof. Der må kun anven-des lokalitetsspecifikke nedbrydningskonstanter i beregningen. Såfremt der ikke haves en lokalitets-specifik nedbrydningskonstant sættes nedbrydningen til \"0\". \nDet skal porienteres, at nedbrydningskonstanter fra de andre moduler (grundvand og vertikal transport) ikke kan anvendes i indeklimamodulets beregninger, da nedbrydningen i beregnes i forhold til poreluftkoncen-trationen og ikke som i de andre i moduler forhold til porevandskoncentrationen"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Terrændæk:"]
[null,"Det ønskede betondæk kan vælges som standardtyper ved at klikke på knappen \"Terrændæk\". Alternativt kan der vælges dæktyper fra \"Egen Liste\", eller der kan manuelt indtastes værdier i de hvide felter. Tykkelsen af dækket indtastes."]
[]
[]
[]
[null,"Såfremt man ønsker at se eller rette de detaljerede data om terrændækket klikkes på knappen \"vis detailoplysninger\"\n"]
[]
[null,"Bygningsdata:"]
[null,"Oplysninger om det/de rum som der ønskes risikovurderet i forhold til indtastes. Såfremt der beregnes på et ikke armeret betongulv, skal størrelsen af betondækket indtastes. Betondækkets størrelse er ikke nødvendigvis det samme som husets fodaftryk. Bygningen vil oftest bestå af flere mindre betondæk, opdelt af fundamentet."]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata for poreluft overføres fra arket \"Enkeltstoffer\". Hvis der i arket \"Enkeltstoffer\" er indtastet en målt poreluftskoncentration overføres denne, ellers overføres luftkoncentrationen beregnet udfra en indtastet vandkoncentration eller alternativt en indtastet jordkoncentration."]
[]
[]
[]
[null,"Det er muligt at teste andre koncentrationer ved at indtaste koncentrationer i de hvide felter. Af udskriften vil det fremgå, at der i givet fald er anvendt ikke målte koncentrationer."]
[]
[]
[null,"Beregninger for krybekælder"]
[null,"Umættet zone:"]
[null,"Som beskrevet under afsnittet \"Beregninger for betondæk\" skal den umættede zone indledningsvis beskrives.\n"]
[]
[]
[]
[null,"Ved beregninger med krybekælder medtager den umættede zone både de jordlag som findes mellem forureningen og betondækket, en eventuel membran, samt et eventuelt gulv i krybekælderen."]
[]
[]
[]
[]
[null,"De ønskede lag kan vælges som standardtyper ved at klikke på knappen \"Jordtype\", \"Membran\" eller \"Beton type\". Alternativt kan der vælges lag fra \"Egen Liste\", eller der kan manuelt indtastes værdier i de hvide felter. Se iøvrigt bemærkninger om anvendelse af valglister under afsnittet generelt.\n"]
[]
[]
[]
[]
[]
[]
[null,"Når det ønskede lag er valgt, angives lagets tykkelse, porøsitet og/eller materialekonstant"]
[]
[]
[null,"NB! I beregningerne af gastransport i den umættede zone kan der medtages nedbrydning. Se nærmere herom under afsnittet \"Beregninger for betondæk\"."]
[]
[]
[]
[null,"Bygningsdata:"]
[null,"Oplysninger om etagen over krybekælderen indtastes. Hvis forureningens fordeling i krybekælderen  ikke er kendt, tages der udgangspunkt i at hele stueetagen påvirkes."]
[]
[]
[]
[]
[null,"Krybekælder:"]
[null,"Oplysninger om krybekælderen indtastes. Hvis forureningens fordeling i krybekælderen  ikke er kendt, tages der udgangspunkt i at hele krybekælderen påvirkes. Etageadskildelsen mellem krybekælder og stueetage vælges fra standardvalglisten"]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata for poreluft overføres fra arket \"Enkeltstoffer\". Hvis der i arket \"Enkeltstoffer\" er indtastet en målt poreluftskoncentration overføres denne, ellers overføres luftkoncentrationen beregnet udfra en indtastet vandkoncentration eller alternativt en indtastet jordkoncentration."]
[]
[]
[]
[null,"Det er muligt at teste andre koncentrationer ved at indtaste koncentrationer i de hvide felter. Af udskriften vil det fremgå, at der i givet fald er anvendt ikke målte koncentrationer."]
[]
[]
[null,"Det er også muligt at indtaste koncentrationer målt i krybekælderen."]
[]
[null,"Generelt"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under olie & benzin modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under olie & benzin modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikkke på den ønskede værdi\n· At vælge en forekomst ved at skreve dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiskestoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet.Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lysseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"Sletning af enkeltværdier:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne incl. resultat af mellemberegninger"]

{"sheet":"Udeluft","index":22,"n_rows":81,"n_cols":36,"rows_kept":81,"cut":false,"hidden":true,"merged":[[9,7,9,11],[9,13,9,17],[9,19,9,23],[9,25,9,29],[54,25,54,29],[64,7,64,11],[64,13,64,17],[64,19,64,23],[64,25,64,29],[54,7,54,11],[54,13,54,17],[54,19,54,23],[32,6,32,8],[40,25,40,26],[42,25,42,26],[12,7,14,31],[40,19,40,20],[42,19,42,20],[44,19,44,20],[18,31,20,32],[19,19,19,20],[26,6,27,8],[30,6,31,8],[28,6,28,8],[66,7,66,11],[66,13,66,17],[66,19,66,23],[66,25,66,29],[56,7,56,11],[56,13,56,17],[62,19,62,23],[59,19,59,23],[57,7,57,11],[62,25,62,29],[60,7,60,11],[60,13,60,17],[60,19,60,23],[62,13,62,17],[62,7,62,11],[59,7,59,11],[59,13,59,17],[60,25,60,29],[59,25,59,29],[56,25,56,29],[57,13,57,17],[57,19,57,23],[57,25,57,29],[56,19,56,23],[7,19,7,23],[39,0,40,4],[51,7,52,11],[51,13,52,17],[51,19,52,23],[40,22,40,23],[47,7,50,26],[26,31,28,32],[27,19,27,20],[42,22,42,23],[44,22,44,23],[51,25,52,29],[31,22,31,23],[32,19,32,20],[32,22,32,23],[30,19,30,20],[30,22,30,23],[30,25,32,26],[30,28,32,29],[18,25,20,26],[18,28,20,29],[24,19,24,20],[24,22,24,23],[22,19,22,20],[3,7,3,23],[5,19,5,23],[26,22,26,23],[26,25,28,26],[22,28,24,29],[22,31,24,32],[23,19,23,20],[26,19,26,20],[34,31,34,32],[30,31,32,32],[22,22,22,23],[23,22,23,23],[22,25,24,26],[15,31,16,32],[16,6,16,8],[15,10,16,11],[5,7,5,15],[7,7,7,15],[26,28,28,29],[27,22,27,23],[28,19,28,20],[28,22,28,23],[34,16,34,17],[31,19,31,20],[18,6,19,8],[22,6,23,8],[24,6,24,8],[20,6,20,8],[18,16,20,17],[22,16,24,17],[20,10,20,11],[20,13,20,14],[80,25,80,29],[80,7,80,11],[72,7,72,11],[77,7,77,11],[72,13,72,17],[77,13,77,17],[80,13,80,17],[72,19,72,23],[80,19,80,23],[75,7,75,11],[75,13,75,17],[75,19,75,23],[75,25,75,29],[77,25,77,29],[72,25,72,29],[77,19,77,23],[17,31,17,32],[17,16,17,17],[17,19,17,20],[17,22,17,23],[17,25,17,26],[17,28,17,29],[15,27,16,30],[15,16,16,17],[15,19,16,20],[15,22,16,23],[15,25,16,26],[11,6,11,30],[82,7,82,11],[82,13,82,17],[82,19,82,23],[82,25,82,29],[26,16,28,17],[30,10,32,11],[26,10,28,11],[22,10,24,11],[30,16,32,17],[44,25,44,26],[39,19,39,20],[39,22,39,23],[24,13,24,14],[28,13,28,14],[32,13,32,14],[17,10,17,11],[15,13,16,14],[17,13,17,14],[18,19,18,20],[18,22,18,23],[19,22,19,23],[20,19,20,20],[20,22,20,23]]}
["Beregning af"]
["udeluftkoncentrationen"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
["Beregning udføres for :",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
[]
["Jordparametre",null,null,null,null,null,null,"Indtast data om jordlag mellem prøvetagningspunktet og jordoverfladen\n"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Jordlag Dybde fra",null,null,"Jordlag Dybde til",null,null,"Lag-tykkelse",null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,"Volumen\naf jordskellet",null,null,null,"Materiale-konstant"]
[null,null,null,null,null,null,"Jordtype"]
[null,null,null,null,null,null,null,null,null,null,"m u.t",null,null,"m u.t",null,null,"(m)",null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ",null,null,"N"]
[null,null,null,null,null,null,{"$f":"IF(D_Ude_jordtype_syst1<>\"\",D_Ude_jordtype_syst1,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"D_Ude_X_1","v":0},null,null,{"$f":"IF(D_Ude_VL_int1<>\"\",D_Ude_VL_int1,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_int1<>\"\",D_Ude_VV_int1,\"\")","v":""},null,null,{"$f":"D_Ude_porositet_1","v":0},null,null,{"$f":"D_Ude_VJ_1","v":1},null,null,{"$f":"D_Ude_N_1","v":0}]
["",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ude_VL_syst1<>\"\",D_Ude_VL_syst1,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_syst1<>\"\",D_Ude_VV_syst1,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_ude_mangeljt_1","v":""},{"$f":"IF(ISTEXT(Ude_jord_dt1),\"Tjek decimal\",IF(ISTEXT(Ude_My_VL1),\"Tjek decimal\",IF(ISTEXT(Ude_My_VV1),\"Tjek decimal\",\"\")))","v":""}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(D_Ude_jordtype_syst2<>\"\",D_Ude_jordtype_syst2,\"\")","v":""},null,null,null,{"$f":"D_Ude_lagfra_2","v":0},null,null,null,null,null,{"$f":"D_Ude_X_2","v":0},null,null,{"$f":"IF(D_Ude_VL_int2<>\"\",D_Ude_VL_int2,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_int2<>\"\",D_Ude_VV_int2,\"\")","v":""},null,null,{"$f":"D_Ude_porositet_2","v":0},null,null,{"$f":"D_Ude_VJ_2","v":1},null,null,{"$f":"D_Ude_N_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ude_VL_syst2<>\"\",D_Ude_VL_syst2,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_syst2<>\"\",D_Ude_VV_syst2,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_ude_mangeljt_2","v":""},{"$f":"IF(ISTEXT(Ude_jord_dt2),\"Tjek decimal\",IF(ISTEXT(Ude_My_VL2),\"Tjek decimal\",IF(ISTEXT(Ude_My_VV2),\"Tjek decimal\",\"\")))","v":""}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(D_Ude_jordtype_syst3<>\"\",D_Ude_jordtype_syst3,\"\")","v":""},null,null,null,{"$f":"D_Ude_lagfra_3","v":0},null,null,null,null,null,{"$f":"D_Ude_X_3","v":0},null,null,{"$f":"IF(D_Ude_VL_int3<>\"\",D_Ude_VL_int3,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_int3<>\"\",D_Ude_VV_int3,\"\")","v":""},null,null,{"$f":"D_Ude_porositet_3","v":0},null,null,{"$f":"D_Ude_VJ_3","v":1},null,null,{"$f":"D_Ude_N_3","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ude_VL_syst3<>\"\",D_Ude_VL_syst3,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_syst3<>\"\",D_Ude_VV_syst3,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_ude_mangeljt_3","v":""},{"$f":"IF(ISTEXT(Ude_jord_dt3),\"Tjek decimal\",IF(ISTEXT(Ude_My_VL3),\"Tjek decimal\",IF(ISTEXT(Ude_My_VV3),\"Tjek decimal\",\"\")))","v":""}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(D_Ude_jordtype_syst4<>\"\",D_Ude_jordtype_syst4,\"\")","v":""},null,null,null,{"$f":"D_Ude_lagfra_4","v":0},null,null,null,null,null,{"$f":"D_Ude_X_4","v":0},null,null,{"$f":"IF(D_Ude_VL_int4<>\"\",D_Ude_VL_int4,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_syst3<>\"\",D_Ude_VV_int4,\"\")","v":""},null,null,{"$f":"D_Ude_porositet_4","v":0},null,null,{"$f":"D_Ude_VJ_4","v":1},null,null,{"$f":"D_Ude_N_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ude_VL_syst4<>\"\",D_Ude_VL_syst4,\"\")","v":""},null,null,{"$f":"IF(D_Ude_VV_syst4<>\"\",D_Ude_VV_syst4,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_ude_mangeljt_4","v":""},{"$f":"IF(ISTEXT(Ude_jord_dt4),\"Tjek decimal\",IF(ISTEXT(Ude_My_VL4),\"Tjek decimal\",IF(ISTEXT(Ude_My_VV4),\"Tjek decimal\",\"\")))","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Ude_negativ_X","v":" "}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Samlede lagtykkelse",null,{"$f":"D_Ude_X_tot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Samlede ækvivalente jordtykkelse",null,{"$f":"D_Ude_N_tot","v":{"$error":"#DIV/0!"}}]
[]
[]
["Det forurenede område",null,null,null,null,null,null,"Indtast data om det forurenede område, eller anvend standardværdier"]
[]
["Længde af det \nforurenede område",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Standard ",null,null,"Brugerdata",null,null,"Anvendt i beregning"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"l",null,{"$f":"Dataark_Udeluft!E27","v":100},null,null,null,null,null,{"$f":"D_Ude_l","v":100},null,null,"m"]
[]
["Opblandingshøjde ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"h",null,{"$f":"Dataark_Udeluft!E28","v":8},null,null,null,null,null,{"$f":"D_Ude_h","v":8},null,null,"m"]
[]
["Opblandingshøjde/længde",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"h/l",null,{"$f":"Dataark_Udeluft!E29","v":0.08},null,null,{"$f":"D_Ude_hl","v":0.08},null,null,{"$f":"D_Ude_hl","v":0.08}]
[]
[]
["Forurening",null,null,null,null,null,null,"Data for forureningen er overført fra fugacitetsmodulet \nIndtast eventuel baggrundskoncentration eller test af andre værdier"]
[]
[]
[]
[null,null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
["Stofnavn (fra enkeltstoffer)"]
[]
["CAS-nummer",null,null,null,null,null,null,{"$f":"D_Ude_CASnr_1","v":""},null,null,null,null,null,{"$f":"D_Ude_CASnr_2","v":""},null,null,null,null,null,{"$f":"D_Ude_CASnr_3","v":""},null,null,null,null,null,{"$f":"D_Ude_CASnr_4","v":""}]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
[]
["Poreluftskoncentration",null,null,null,null,"CL",null,{"$f":"IF(ISNUMBER(D_Enk_CL_endelig_1),ROUND(D_Enk_CL_endelig_1,3-(INT(LOG(D_Enk_CL_endelig_1))+1)),\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_Enk_CL_endelig_2),ROUND(D_Enk_CL_endelig_2,3-(INT(LOG(D_Enk_CL_endelig_2))+1)),\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_Enk_CL_endelig_3),ROUND(D_Enk_CL_endelig_3,3-(INT(LOG(D_Enk_CL_endelig_3))+1)),\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_Enk_CL_endelig_4),ROUND(D_Enk_CL_endelig_4,3-(INT(LOG(D_Enk_CL_endelig_4))+1)),\"\")","v":""},null,null,null,null,null,"mg/m³"]
[null,"Test af andre værdier",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³",null,null,{"$f":"IF(ISTEXT(Ude_My_CL_1),\"Tjek decimal\",IF(ISTEXT(Ude_My_CL_2),\"Tjek decimal\",IF(ISTEXT(Ude_My_CL_3),\"Tjek decimal\",IF(ISTEXT(Ude_My_CL_4),\"Tjek decimal\",\"\"))))","v":""}]
[]
["Baggrundskoncentration",null,null,null,null,"C0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/m³",null,null,{"$f":"IF(ISTEXT(Ude_C0_1),\"Tjek decimal\",IF(ISTEXT(Ude_C0_2),\"Tjek decimal\",IF(ISTEXT(Ude_C0_3),\"Tjek decimal\",IF(ISTEXT(Ude_C0_4),\"Tjek decimal\",\"\"))))","v":""}]
[]
["Diffusionskoefficient i luft",null,null,null,null,"DL",null,{"$f":"D_Ude_DL_1","v":""},null,null,null,null,null,{"$f":"D_Ude_DL_2","v":""},null,null,null,null,null,{"$f":"D_Ude_DL_3","v":""},null,null,null,null,null,{"$f":"D_Ude_DL_4","v":""},null,null,null,null,null,"m²/s"]
[]
["Vindhastighed (stofafhængig)",null,null,null,null,"v",null,{"$f":"D_Ude_v_1","v":""},null,null,null,null,null,{"$f":"D_Ude_v_2","v":""},null,null,null,null,null,{"$f":"D_Ude_v_3","v":""},null,null,null,null,null,{"$f":"D_Ude_v_4","v":""},null,null,null,null,null,"m/s"]
[]
[]
["Beregning: Udeluft"]
[]
[]
["Total bidrag til udeluft",null,null,null,null,"Cu",null,{"$f":"IF(ISNUMBER(D_Ude_Cu_1),ROUND(D_Ude_Cu_1,3-(INT(LOG(D_Ude_Cu_1))+1)),\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_Ude_Cu_2),ROUND(D_Ude_Cu_2,3-(INT(LOG(D_Ude_Cu_2))+1)),\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_Ude_Cu_3),ROUND(D_Ude_Cu_3,3-(INT(LOG(D_Ude_Cu_3))+1)),\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_Ude_Cu_4),ROUND(D_Ude_Cu_4,3-(INT(LOG(D_Ude_Cu_4))+1)),\"\")","v":""},null,null,null,null,null,"mg/m³"]
[]
[]
["Afdampningskriterie",null,null,null,null,null,null,{"$f":"D_Ude_afd_krit_1","v":0},null,null,null,null,null,{"$f":"D_Ude_afd_krit_2","v":0},null,null,null,null,null,{"$f":"D_Ude_afd_krit_3","v":0},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Ude_afd_krit_4,\"\")","v":""},null,null,null,null,null,"mg/m³"]
[]
["Overskridelse af kriteriet",null,null,null,null,null,null,{"$f":"D_Ude_afd_krit_vurdering_1","v":""},null,null,null,null,null,{"$f":"D_Ude_afd_krit_vurdering_2","v":""},null,null,null,null,null,{"$f":"D_Ude_afd_krit_vurdering_3","v":""},null,null,null,null,null,{"$f":"D_Ude_afd_krit_vurdering_4","v":""},null,null,null,null,null,"gange"]
[]
[]
["Anvendt brugerdata?",null,null,null,null,null,null,{"$f":"D_Ude_Brugerdata_1","v":""},null,null,null,null,null,{"$f":"D_Ude_Brugerdata_2","v":""},null,null,null,null,null,{"$f":"D_Ude_Brugerdata_3","v":""},null,null,null,null,null,{"$f":"D_Ude_Brugerdata_4","v":""}]

{"sheet":"Dataark_Udeluft","index":23,"n_rows":57,"n_cols":24,"rows_kept":57,"cut":false,"hidden":true,"merged":[[23,1,23,16],[1,1,1,16],[30,1,30,16],[3,1,3,16],[5,16,5,19],[5,12,5,15],[5,8,5,11],[5,4,5,7],[33,17,33,18],[32,4,32,6],[32,7,32,9],[32,10,32,12],[32,13,32,15]]}
[]
[null,"Dataark - Udeluft",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,null,{"$f":"Ude_My_jord1","v":0},{"$f":"IF(ISTEXT(G8),G8,F8)","v":0},null,null,{"$f":"Ude_My_jord2","v":0},{"$f":"IF(ISTEXT(K8),K8,J8)","v":0},null,null,{"$f":"Ude_My_jord3","v":0},{"$f":"IF(ISTEXT(O8),O8,N8)","v":0},null,null,{"$f":"Ude_My_jord4","v":0},{"$f":"IF(ISTEXT(S8),S8,R8)","v":0},null,null,"D_Ude_jordtype_n","Imput"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,null,{"$f":"Ude_jord_df","v":0},{"$f":"IF(D_Ude_jordtype_1<>\"\",G9,\"\")","v":0},null,{"$f":"D_Ude_lagtil_1","v":0},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J9,\"\")","v":0},null,{"$f":"D_Ude_lagtil_2","v":0},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N9,\"\")","v":0},null,{"$f":"D_Ude_lagtil_3","v":0},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R9,\"\")","v":0},null,null,"D_Ude_lagfra_n","Imput"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"Ude_jord_dt1","v":0},{"$f":"IF(D_Ude_jordtype_1<>\"\",G10,\"\")","v":0},null,null,{"$f":"Ude_jord_dt2","v":0},{"$f":"IF(D_Ude_jordtype_2<>\"\",K10,\"\")","v":0},null,null,{"$f":"Ude_jord_dt3","v":0},{"$f":"IF(D_Ude_jordtype_3<>\"\",O10,\"\")","v":0},null,null,{"$f":"Ude_jord_dt4","v":0},{"$f":"IF(D_Ude_jordtype_4<>\"\",S10,\"\")","v":0},null,null,"D_Ude_lagtil_n","Imput"]
[null,"Tykkelse af jordlag","X","m",null,{"$f":"B_Ude_X_1","v":0},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F11,\"\")","v":0},null,{"$f":"B_Ude_X_2","v":0},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J11,\"\")","v":0},null,{"$f":"B_Ude_X_3","v":0},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N11,\"\")","v":0},null,{"$f":"B_Ude_X_4","v":0},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R11,\"\")","v":0},null,null,"D_Ude_X_n","Beregnet i dataark_udeluft"]
[null,"Check af negativ højde",null,null,null,{"$f":"B_Ude_negativ_X_1","v":0},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F12,\"\")","v":0},null,{"$f":"B_Ude_negativ_X_2","v":0},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J12,\"\")","v":0},null,{"$f":"B_Ude_negativ_X_3","v":0},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N12,\"\")","v":0},null,{"$f":"B_Ude_negativ_X_4","v":0},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R12,\"\")","v":0},{"$f":"IF(F12+J12+N12+R12>0,\"FEJL! Der er jordlag med negativ højde\",\" \")","v":" "},null,"D_Ude_negativ_X_n","Beregnet i dataark_udeluft"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"IF(ISNUMBER(Ude_My_VL1),Ude_My_VL1,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_1<>\"\",IF(ISNUMBER(G13),G13,F13),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(Ude_My_VL2),Ude_My_VL2,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_2<>\"\",IF(ISNUMBER(K13),K13,J13),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(Ude_My_VL3),Ude_My_VL3,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_3<>\"\",IF(ISNUMBER(O13),O13,N13),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(Ude_My_VL4),Ude_My_VL4,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_4<>\"\",IF(ISNUMBER(S13),S13,R13),\"\")","v":0},null,null,"D_Ude_VL_n","Imput"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"IF(ISNUMBER(Ude_My_VV1),Ude_My_VV1,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_1<>\"\",IF(ISNUMBER(G14),G14,F14),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(Ude_My_VV2),Ude_My_VV2,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_2<>\"\",IF(ISNUMBER(K14),K14,J14),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(Ude_My_VV3),Ude_My_VV3,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_3<>\"\",IF(ISNUMBER(O14),O14,N14),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(Ude_My_VV4),Ude_My_VV4,\"-\")","v":"-"},{"$f":"IF(D_Ude_jordtype_4<>\"\",IF(ISNUMBER(S14),S14,R14),\"\")","v":0},null,null,"D_Ude_VV_n","Imput"]
[null,"Samlet\nporøsitet","e=VL+VV",null,null,{"$f":"B_Ude_porositet_1","v":0},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F15,\"\")","v":0},null,{"$f":"B_Ude_porositet_2","v":0},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J15,\"\")","v":0},null,{"$f":"B_Ude_porositet_3","v":0},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N15,\"\")","v":0},null,{"$f":"B_Ude_porositet_4","v":0},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R15,\"\")","v":0},null,null,"D_Ude_porositet_n","Beregnet i dataark_udeluft"]
[null,"Volumen af jordskellet","VJ",null,null,{"$f":"B_Ude_VJ_1","v":1},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F16,\"\")","v":1},null,{"$f":"B_Ude_VJ_2","v":1},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J16,\"\")","v":1},null,{"$f":"B_Ude_VJ_3","v":1},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N16,\"\")","v":1},null,{"$f":"B_Ude_VJ_4","v":1},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R16,\"\")","v":1},null,null,"D_Ude_VJ_n","Beregnet i dataark_udeluft"]
[null,"Materialekonstant (app 5.3 - nyt lign. 64 ersatter lign 18)","t",null,null,{"$f":"B_Ude_N_1","v":0},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F17,\"\")","v":0},null,{"$f":"B_Ude_N_2","v":0},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J17,\"\")","v":0},null,{"$f":"B_Ude_N_3","v":0},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N17,\"\")","v":0},null,{"$f":"B_Ude_N_4","v":0},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R17,\"\")","v":0},null,null,"D_Ude_N_n","Beregnet i dataark_udeluft"]
[null,"Korigeret materialekonstant",null,null,null,{"$f":"B_Ude_N_koor_1","v":1},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F18,\"\")","v":1},null,{"$f":"B_Ude_N_koor_2","v":1},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J18,\"\")","v":1},null,{"$f":"B_Ude_N_koor_3","v":1},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N18,\"\")","v":1},null,{"$f":"B_Ude_N_koor_4","v":1},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R18,\"\")","v":1},null,null,"D_Ude_N_koor_n","Beregnet i dataark_udeluft"]
[null,"Mellemregning (app. 5.3 - Lign 51)",null,null,null,{"$f":"B_Ude_Bereg_1","v":0},null,{"$f":"IF(D_Ude_jordtype_1<>\"\",F19,\"\")","v":0},null,{"$f":"B_Ude_Bereg_2","v":0},null,{"$f":"IF(D_Ude_jordtype_2<>\"\",J19,\"\")","v":0},null,{"$f":"B_Ude_Bereg_3","v":0},null,{"$f":"IF(D_Ude_jordtype_3<>\"\",N19,\"\")","v":0},null,{"$f":"B_Ude_Bereg_4","v":0},null,{"$f":"IF(D_Ude_jordtype_4<>\"\",R19,\"\")","v":0},null,null,"D_Ude_Bereg_n","Beregnet i dataark_udeluft"]
[null,"Check af manglende jordtype",null,null,null,null,null,{"$f":"IF(AND(D_Ude_lagtil_1>0,D_Ude_jordtype_1=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ude_lagtil_2>0,D_Ude_jordtype_2=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ude_lagtil_3>0,D_Ude_jordtype_3=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_Ude_lagtil_4>0,D_Ude_jordtype_4=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,"D_ude_mangeljt_x"]
[null,"Samlet ækivalente materialekonstant/tykkelse  (app 5.3 - lign. 51)","t*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_Ude_N_tot","v":{"$error":"#DIV/0!"}},null,"D_Ude_N_tot","Beregnet i dataark_udeluft"]
[null,"Tykkelse af jordlag","X","m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_Ude_X_tot","v":0},null,"D_Ude_X_tot","Beregnet i dataark_udeluft"]
[]
[null,"Det forurenede område"]
[]
[null,null,null,null,"Systemværdi","Indtastet","Beregnet","Anvendes"]
[null,"Længde af det forurenede område","l","m",100,{"$f":"Ude_l","v":0},{"$f":"IF(F27>0,F27,E27)","v":100},{"$f":"IF(VALUE(F27),F27,E27)","v":100},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ude_l","Imput"]
[null,"Opblandingshøjde ","h","m",8,{"$f":"Ude_h","v":0},{"$f":"IF(F28>0,F28,H27*E29)","v":8},{"$f":"IF(VALUE(F28),F28,G28)","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ude_h","Imput"]
[null,"Opblandingshøjde/længde","h/l"," -",{"$f":"E28/E27","v":0.08},{"$f":"IF(OR(F27=0,F28=0),\"\",F28/F27)","v":""},{"$f":"G28/G27","v":0.08},{"$f":"H28/H27","v":0.08},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ude_hl","Imput"]
[]
[null,"Stoffer"]
[]
[null,null,null,null,"Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4"]
[null,"Navn","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes"]
[null,"Forureningskomponent",null,null,null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_1),D_Enk_stofnavn_1,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_2),D_Enk_stofnavn_2,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_3),D_Enk_stofnavn_3,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_4),D_Enk_stofnavn_4,\"\")","v":""},null,null,null,null,null,null,"D_Ude_stofnavn_n","Overført fra Enkeltstoffer"]
[null,"CAS-nummer",null,null,null,null,{"$f":"IF(D_Enk_CASnr_1<>\"\",D_Enk_CASnr_1,\"\")","v":""},null,null,{"$f":"IF(D_Enk_CASnr_2<>\"\",D_Enk_CASnr_2,\"\")","v":""},null,null,{"$f":"IF(D_Enk_CASnr_3<>\"\",D_Enk_CASnr_3,\"\")","v":""},null,null,{"$f":"IF(D_Enk_CASnr_4<>\"\",D_Enk_CASnr_4,\"\")","v":""}]
[null,"Poreluftskoncentration / test af andre værdier","CL","mg/m³",{"$f":"D_Enk_CL_endelig_1","v":""},{"$f":"Ude_My_CL_1","v":0},{"$f":"IF(D_Ude_stofnavn_1<>\"\",IF(VALUE(F37),F37,E37),\"\")","v":""},{"$f":"D_Enk_CL_endelig_2","v":""},{"$f":"Ude_My_CL_2","v":0},{"$f":"IF(D_Ude_stofnavn_2<>\"\",IF(VALUE(I37),I37,H37),\"\")","v":""},{"$f":"D_Enk_CL_endelig_3","v":""},{"$f":"Ude_My_CL_3","v":0},{"$f":"IF(D_Ude_stofnavn_3<>\"\",IF(VALUE(L37),L37,K37),\"\")","v":""},{"$f":"D_Enk_CL_endelig_4","v":""},{"$f":"Ude_My_CL_4","v":0},{"$f":"IF(D_Ude_stofnavn_4<>\"\",IF(VALUE(O37),O37,N37),\"\")","v":""},null,null,null,null,null,null,"D_Ude_CL_n","Overført fra Enkeltstoffer"]
[null,"Hvis poreluftberegnet er der anvendt brugerdata?",null,null,null,{"$f":"IF(D_Ude_CL_1=Enk_My_CL_1,\"0\",\"Ja\")","v":"0"},null,null,{"$f":"IF(D_Ude_CL_2=Enk_My_CL_2,\"0\",\"Ja\")","v":"0"},null,null,{"$f":"IF(D_Ude_CL_3=Enk_My_CL_3,\"0\",\"Ja\")","v":"0"},null,null,{"$f":"IF(D_Ude_CL_4=Enk_My_CL_4,\"0\",\"Ja\")","v":"0"}]
[null,"Baggrundskoncentration","C0","mg/m³",null,{"$f":"Ude_C0_1","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(F39<>0,F39,0),\"\")","v":""},null,{"$f":"Ude_C0_2","v":0},{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(I39<>0,I39,0),\"\")","v":""},null,{"$f":"Ude_C0_3","v":0},{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(L39<>0,L39,0),\"\")","v":""},null,{"$f":"Ude_C0_4","v":0},{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(O39<>0,O39,0),\"\")","v":""},null,null,null,null,null,null,"D_Ude_C0_n","Imput"]
[null,"Diffusionskoefficient luft","DL","m²/s",{"$f":"D_Enk_DL_syst_1","v":0},{"$f":"Enk_My_DL_1","v":0},{"$f":"IF(D_Ude_stofnavn_1<>\"\",D_Enk_DL_1,\"\")","v":""},{"$f":"D_Enk_DL_syst_2","v":0},{"$f":"Enk_My_DL_2","v":0},{"$f":"IF(D_Ude_stofnavn_2<>\"\",D_Enk_DL_2,\"\")","v":""},{"$f":"D_Enk_DL_syst_3","v":0},{"$f":"Enk_My_DL_3","v":0},{"$f":"IF(D_Ude_stofnavn_3<>\"\",D_Enk_DL_3,\"\")","v":""},{"$f":"D_Enk_DL_syst_4","v":0},{"$f":"Enk_My_DL_4","v":0},{"$f":"IF(D_Ude_stofnavn_4<>\"\",D_Enk_DL_4,\"\")","v":""},null,null,null,null,null,null,"D_Ude_DL_n","Overført fra Enkeltstoffer"]
[null,"Vindhastighed (stofafhængig)","v","m/s",{"$f":"D_Enk_v_syst_1","v":0},{"$f":"Enk_My_v_1","v":0},{"$f":"IF(D_Ude_stofnavn_1<>\"\",D_Enk_v_1,\"\")","v":""},{"$f":"D_Enk_v_syst_2","v":0},{"$f":"Enk_My_v_2","v":0},{"$f":"IF(D_Ude_stofnavn_2<>\"\",D_Enk_v_2,\"\")","v":""},{"$f":"D_Enk_v_syst_3","v":0},{"$f":"Enk_My_v_3","v":0},{"$f":"IF(D_Ude_stofnavn_3<>\"\",D_Enk_v_3,\"\")","v":""},{"$f":"D_Enk_v_syst_4","v":0},{"$f":"Enk_My_v_4","v":0},{"$f":"IF(D_Ude_stofnavn_4<>\"\",D_Enk_v_4,\"\")","v":""},null,null,null,null,null,null,"D_Ude_v_n","Overført fra Enkeltstoffer"]
[]
[null,"Udeluft beregninger"]
[null,"Afdampningsflux (app. 5,2 - lign 17)","J","mg/(m² s)",null,null,{"$f":"B_Ude_J_1","v":""},null,null,{"$f":"B_Ude_J_2","v":""},null,null,{"$f":"B_Ude_J_3","v":""},null,null,{"$f":"B_Ude_J_4","v":""},null,null,null,null,null,null,"D_Ude_J_n","Beregnet"]
[null,"Total bidrag til udeluft (app 5.2 - lign 20)","Cu","mg/m³",null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",B_Ude_Cu_1,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",B_Ude_Cu_2,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",B_Ude_Cu_3,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",B_Ude_Cu_4,\"\")","v":""},null,null,null,null,null,null,"D_Ude_Cu_n","Beregnet"]
[null,"Afdampningskriterie","afd-krit","mg/m³",{"$f":"D_Enk_afd_krit_syst_1","v":0},{"$f":"Enk_My_afd_krit_1","v":0},{"$f":"D_Enk_afd_krit_1","v":0},null,{"$f":"Enk_My_afd_krit_2","v":0},{"$f":"D_Enk_afd_krit_2","v":0},null,{"$f":"Enk_My_afd_krit_3","v":0},{"$f":"D_Enk_afd_krit_3","v":0},null,{"$f":"Enk_My_afd_krit_4","v":0},{"$f":"D_Enk_afd_krit_4","v":0},null,null,null,null,null,null,"D_Ude_afd_krit_n","Overført fra Enkeltstoffer"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",B_Ude_afB_krit_vurdering_1,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",B_Ude_afB_krit_vurdering_2,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",B_Ude_afB_krit_vurdering_3,\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",B_Ude_afB_krit_vurdering_4,\"\")","v":""},null,null,null,null,null,null,"D_Ude_afd_krit_vurdering_n","Beregnet"]
[null,"Fri fase ??",null,null,null,null,{"$f":"IF(OR(Enk_FF_P_1=\"ja\",Enk_FF_V_1=\"ja\",Enk_FF_J_1=\"ja\"),\"Ja\",\"Nej\")","v":{"$error":"#NAME?"}},null,null,{"$f":"IF(OR(Enk_FF_P_1=\"ja\",Enk_FF_V_1=\"ja\",Enk_FF_J_1=\"ja\"),\"Ja\",\"Nej\")","v":{"$error":"#NAME?"}},null,null,{"$f":"IF(OR(Enk_FF_P_1=\"ja\",Enk_FF_V_1=\"ja\",Enk_FF_J_1=\"ja\"),\"Ja\",\"Nej\")","v":{"$error":"#NAME?"}},null,null,{"$f":"IF(OR(Enk_FF_P_1=\"ja\",Enk_FF_V_1=\"ja\",Enk_FF_J_1=\"ja\"),\"Ja\",\"Nej\")","v":{"$error":"#NAME?"}},null,null,null,null,null,null,"D_Ude_FF_n","Benyttes ikke!!!"]
[null,"Anvendt Brugerdata",null,null,null,{"$f":"SUM(F37:F48,G13:G16,K13:K16,O13:O16,S13:S16)","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(F49>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM(I37:I48,G13:G16,K13:K16,O13:O16,S13:S16)","v":0},{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(I49>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM(L37:L48,G13:G16,K13:K16,O13:O16,S13:S16)","v":0},{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(L49>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM(O37:O48,G13:G16,K13:K16,O13:O16,S13:S16)","v":0},{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(O49>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,null,null,null,null,null,"D_Ude_Brugerdata_n"]
[]
[null,"Bemærkninger"]
[null,"Jordparametre:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ude_Jord_Com","Import . Bemærkningsfelt"]
[null,null,false]
[null,"Forurenet område:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ude_ForOm_Com","Import . Bemærkningsfelt"]
[null,null,false]
[null,"Forurening:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ude_For_Com","Import . Bemærkningsfelt"]
[null,null,false]

{"sheet":"Beregning_Udeluft","index":24,"n_rows":26,"n_cols":19,"rows_kept":26,"cut":false,"hidden":true,"merged":[[5,4,5,5],[5,6,5,7],[5,8,5,9],[5,10,5,11],[1,1,1,16],[3,1,3,16],[18,1,18,16],[20,4,20,6],[20,7,20,9],[20,10,20,12],[20,13,20,15]]}
[]
[null,"Beregning - Udeluft",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Beregnet","Anvendes","Beregnet","Anvendes","Beregnet","Anvendes","Beregnet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,{"$f":"D_Ude_jordtype_1","v":0},null,{"$f":"D_Ude_jordtype_2","v":0},null,{"$f":"D_Ude_jordtype_3","v":0},null,{"$f":"D_Ude_jordtype_4","v":0},null,null,null,null,null,null,"B_Ude_jordtype_n"]
[null,"Tykkelse af jordlag","X","m",{"$f":"IF(ISNUMBER(Ude_jord_dt1),D_Ude_lagtil_1-D_Ude_lagfra_1,0)","v":0},{"$f":"E9","v":0},{"$f":"IF(ISNUMBER(Ude_jord_dt2),D_Ude_lagtil_2-D_Ude_lagfra_2,0)","v":0},{"$f":"G9","v":0},{"$f":"IF(ISNUMBER(Ude_jord_dt3),D_Ude_lagtil_3-D_Ude_lagfra_3,0)","v":0},{"$f":"I9","v":0},{"$f":"IF(ISNUMBER(Ude_jord_dt4),D_Ude_lagtil_4-D_Ude_lagfra_4,0)","v":0},{"$f":"K9","v":0},null,null,null,null,null,null,"B_Ude_X_n"]
[null,"Check af negativ højde",null,null,{"$f":"IF(D_Ude_X_1<0,1,0)","v":0},{"$f":"E10","v":0},{"$f":"IF(D_Ude_X_2<0,1,0)","v":0},{"$f":"G10","v":0},{"$f":"IF(D_Ude_X_3<0,1,0)","v":0},{"$f":"I10","v":0},{"$f":"IF(D_Ude_X_4<0,1,0)","v":0},{"$f":"K10","v":0},{"$f":"IF(E10+G10+I10+K10>0,\"FEJL!! Der er jordlag med negativ højde\",\" \")","v":" "},null,null,null,null,null,"B_Ude_negativ_X_n"]
[null,"Samlet\nporøsitet","e=VL+VV",null,{"$f":"D_Ude_VV_1+D_Ude_VL_1","v":0},0,{"$f":"D_Ude_VV_2+D_Ude_VL_2","v":0},0,{"$f":"D_Ude_VV_3+D_Ude_VL_3","v":0},0,{"$f":"D_Ude_VV_4+D_Ude_VL_4","v":0},0,null,null,null,null,null,null,"B_Ude_porositet_n"]
[null,"Volumen af jordskellet","VJ",null,{"$f":"1-D_Ude_porositet_1","v":1},1,{"$f":"1-D_Ude_porositet_2","v":1},1,{"$f":"1-D_Ude_porositet_3","v":1},1,{"$f":"1-D_Ude_porositet_4","v":1},1,null,null,null,null,null,null,"B_Ude_VJ_n"]
[null,"Materialekonstant (app 5.3 - nyt lign. 64 ersatter lign 18)","t",null,{"$f":"IF(D_Ude_VL_1=0,0,(D_Ude_VL_1^2.5)/D_Ude_porositet_1)","v":0},0,{"$f":"IF(D_Ude_VL_2=0,0,(D_Ude_VL_2^2.5)/D_Ude_porositet_2)","v":0},0,{"$f":"IF(D_Ude_VL_3=0,0,(D_Ude_VL_3^2.5)/D_Ude_porositet_3)","v":0},0,{"$f":"IF(D_Ude_VL_4=0,0,(D_Ude_VL_4^2.5)/D_Ude_porositet_4)","v":0},0,null,null,null,null,null,null,"B_Ude_N_n"]
[null,"Korigeret materialekonstant",null,null,{"$f":"IF(D_Ude_N_1=0,1,D_Ude_N_1)","v":1},1,{"$f":"IF(D_Ude_N_2=0,1,D_Ude_N_2)","v":1},1,{"$f":"IF(D_Ude_N_3=0,1,D_Ude_N_3)","v":1},1,{"$f":"IF(D_Ude_N_4=0,1,D_Ude_N_4)","v":1},1,null,null,null,null,null,null,"B_Ude_N_koor_n"]
[null,"Mellemregning (app. 5.3 - Lign 51)",null,null,{"$f":"D_Ude_X_1*(D_Ude_N_koor_2*D_Ude_N_koor_3*D_Ude_N_koor_4)","v":0},0,{"$f":"D_Ude_X_2*(D_Ude_N_koor_1*D_Ude_N_koor_3*D_Ude_N_koor_4)","v":0},0,{"$f":"D_Ude_X_3*(D_Ude_N_koor_1*D_Ude_N_koor_2*D_Ude_N_koor_4)","v":0},0,{"$f":"D_Ude_X_4*(D_Ude_N_koor_1*D_Ude_N_koor_2*D_Ude_N_koor_3)","v":0},0,null,null,null,null,null,null,"B_Ude_Bereg_n"]
[null,"Samlet ækivalente jordlagtykkelse  (app 5.3 - lign. 51)","t*",null,null,null,null,null,null,null,null,null,{"$f":"(D_Ude_N_koor_1*D_Ude_N_koor_2*D_Ude_N_koor_3*D_Ude_N_koor_4)/(D_Ude_Bereg_1+D_Ude_Bereg_2+D_Ude_Bereg_3+D_Ude_Bereg_4)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"B_Ude_N_tot"]
[null,"Tykkelse af jordlag","X","m",null,null,null,null,null,null,null,null,{"$f":"D_Ude_X_4+D_Ude_X_3+D_Ude_X_2+D_Ude_X_1","v":0},null,null,null,null,null,"B_Ude_X_tot"]
[]
[null,"Stoffer"]
[]
[null,null,null,null,"Stof 1",null,null,"Stof 2",null,null,"Stof 3",null,null,"Stof 4"]
[null,"Navn","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes","Systemværdi","Indtastet","Anvendes"]
[null,"Forureningskomponent",null,null,null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_1),D_Enk_stofnavn_1,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_2),D_Enk_stofnavn_2,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_3),D_Enk_stofnavn_3,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(D_Enk_stofnavn_4),D_Enk_stofnavn_4,\"\")","v":""},null,null,"B_Ude_stofnavn_n"]
[null,"Afdampningsflux (app. 5,2 - lign 17)","J","mg/(m² s)",null,null,{"$f":"IF(D_Ude_stofnavn_1<>\"\",-D_Ude_N_tot*D_Ude_DL_1*(D_Ude_C0_1-D_Ude_CL_1),\"\")","v":""},null,null,{"$f":"IF(D_Ude_stofnavn_2<>\"\",-D_Ude_N_tot*D_Ude_DL_2*(D_Ude_C0_2-D_Ude_CL_2),\"\")","v":""},null,null,{"$f":"IF(D_Ude_stofnavn_3<>\"\",-D_Ude_N_tot*D_Ude_DL_3*(D_Ude_C0_3-D_Ude_CL_3),\"\")","v":""},null,null,{"$f":"IF(D_Ude_stofnavn_4<>\"\",-D_Ude_N_tot*D_Ude_DL_4*(D_Ude_C0_4-D_Ude_CL_4),\"\")","v":""},null,null,"B_Ude_J_n"]
[null,"Total bidrag til udeluft (app 5.2 - lign 20)","Cu","mg/m³",null,null,{"$f":"IF(D_Ude_stofnavn_1<>\"\",D_Ude_J_1/(D_Ude_v_1*D_Ude_hl),\"\")","v":""},null,null,{"$f":"IF(D_Ude_stofnavn_2<>\"\",D_Ude_J_2/(D_Ude_v_2*D_Ude_hl),\"\")","v":""},null,null,{"$f":"IF(D_Ude_stofnavn_3<>\"\",D_Ude_J_3/(D_Ude_v_3*D_Ude_hl),\"\")","v":""},null,null,{"$f":"IF(D_Ude_stofnavn_4<>\"\",D_Ude_J_4/(D_Ude_v_4*D_Ude_hl),\"\")","v":""},null,null,"B_Ude_Cu_n"]
[null,"Overskridelse af afdampningskriteriet",null,"gange",null,null,{"$f":"IF(D_Ude_afd_krit_1=0,\"Intet kriterie\",IF(D_Ude_Cu_1>D_Ude_afd_krit_1,D_Ude_Cu_1/D_Ude_afd_krit_1,\"Nej\"))","v":"Intet kriterie"},null,null,{"$f":"IF(D_Ude_afd_krit_2=0,\"Intet kriterie\",IF(D_Ude_Cu_2>D_Ude_afd_krit_2,D_Ude_Cu_2/D_Ude_afd_krit_2,\"Nej\"))","v":"Intet kriterie"},null,null,{"$f":"IF(D_Ude_afd_krit_3=0,\"Intet kriterie\",IF(D_Ude_Cu_3>D_Ude_afd_krit_3,D_Ude_Cu_3/D_Ude_afd_krit_3,\"Nej\"))","v":"Intet kriterie"},null,null,{"$f":"IF(D_Ude_afd_krit_4=0,\"Intet kriterie\",IF(D_Ude_Cu_4>D_Ude_afd_krit_4,D_Ude_Cu_4/D_Ude_afd_krit_4,\"Nej\"))","v":"Intet kriterie"},null,null,"B_Ude_afB_krit_vurdering_n"]

{"sheet":"Udskrift_Udeluft","index":25,"n_rows":96,"n_cols":11,"rows_kept":96,"cut":false,"hidden":true,"merged":[[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,10],[2,8,2,10],[3,8,3,10],[4,8,4,10],[94,1,105,9],[22,8,22,9],[41,8,41,9],[42,8,42,9],[41,2,41,3],[42,2,42,3],[41,4,41,5],[42,4,42,5],[41,6,41,7],[42,6,42,7],[40,8,40,9],[40,2,40,3],[40,4,40,5],[40,6,40,7],[24,2,24,3],[24,4,24,5],[45,2,45,3],[45,4,45,5],[45,6,45,7],[45,8,45,9],[43,2,43,3],[43,4,43,5],[43,6,43,7],[43,8,43,9],[81,1,92,9],[46,2,46,3],[46,4,46,5],[46,6,46,7],[46,8,46,9],[56,1,66,9],[68,1,79,9],[24,8,24,9],[38,0,38,1],[34,4,34,5],[35,4,35,5],[36,4,36,5],[24,6,24,7],[23,2,23,3],[23,4,23,5],[23,6,23,7],[22,2,22,3],[22,4,22,5],[22,6,22,7],[14,4,14,5],[18,8,18,9],[21,8,21,9],[21,2,21,3],[21,4,21,5],[21,6,21,7],[19,2,20,3],[19,4,20,5],[19,6,20,7],[19,8,20,9],[15,4,15,5],[18,2,18,3],[18,4,18,5],[18,6,18,7],[11,8,11,9],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[23,8,23,9],[8,2,8,3],[8,4,8,5],[8,6,8,7],[8,8,8,9],[9,2,9,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[10,2,10,3],[10,4,10,5],[10,6,10,7],[10,8,10,9],[11,2,11,3],[11,4,11,5],[11,6,11,7]]}
["Udeluftberegning "]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nummer:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jordparametre"]
["Kommentar",{"$f":"IF(D_Ude_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Indtastede data (angives med fed)"]
[null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
["Jordlag, Dybde fra","m u.t.",{"$f":"IF(Ude_jord_df<>\"\",Ude_jord_df,\"\")","v":""},null,{"$f":"IF(Ude_jord_dt2<>\"\",D_Ude_lagfra_2,\"\")","v":""},null,{"$f":"IF(Ude_jord_dt3<>\"\",D_Ude_lagfra_3,\"\")","v":""},null,{"$f":"IF(Ude_jord_dt4<>\"\",D_Ude_lagfra_4,\"\")","v":""}]
["Jordlag, Dybde til","m u.t.",{"$f":"IF(Ude_jord_dt1<>\"\",Ude_jord_dt1,\"\")","v":""},null,{"$f":"IF(Ude_jord_dt2<>\"\",Ude_jord_dt2,\"\")","v":""},null,{"$f":"IF(Ude_jord_dt3<>\"\",Ude_jord_dt3,\"\")","v":""},null,{"$f":"IF(Ude_jord_dt4<>\"\",Ude_jord_dt4,\"\")","v":""}]
["Jordtype",null,{"$f":"IF(AND(D_Ude_jordtype_syst1=\"\",Ude_My_jord1=\"\"),\"\",D_Ude_jordtype_1)","v":""},null,{"$f":"IF(AND(D_Ude_jordtype_syst2=\"\",Ude_My_jord2=\"\"),\"\",D_Ude_jordtype_2)","v":""},null,{"$f":"IF(AND(D_Ude_jordtype_syst3=\"\",Ude_My_jord3=\"\"),\"\",D_Ude_jordtype_3)","v":""},null,{"$f":"IF(AND(D_Ude_jordtype_syst4=\"\",Ude_My_jord4=\"\"),\"\",D_Ude_jordtype_4)","v":""}]
["Materialekonstant",null,{"$f":"IF(AND(D_Ude_jordtype_syst1=\"\",Ude_My_jord1=\"\"),\"\",D_Ude_N_1)","v":""},null,{"$f":"IF(AND(D_Ude_jordtype_syst2=\"\",Ude_My_jord2=\"\"),\"\",D_Ude_N_2)","v":""},null,{"$f":"IF(AND(D_Ude_jordtype_syst3=\"\",Ude_My_jord3=\"\"),\"\",D_Ude_N_3)","v":""},null,{"$f":"IF(AND(D_Ude_jordtype_syst4=\"\",Ude_My_jord4=\"\"),\"\",D_Ude_N_4)","v":""}]
[]
["Samlet ækivalent jordlagtykkelse  (app 5.3 - lign. 51)",null,null,null,{"$f":"D_Ude_N_tot","v":{"$error":"#DIV/0!"}},null,"m"]
["Tykkelse af jordlag",null,null,null,{"$f":"D_Ude_X_tot","v":0},null,"m",{"$f":"D_Ude_negativ_X","v":" "}]
[]
["Stoffer"]
["Kommentar",{"$f":"IF(D_Ude_For_ComUds,\"ja\",\"nej\")","v":"nej"},"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
["Forureningskomponent",null,{"$f":"D_Ude_stofnavn_1","v":""},null,{"$f":"D_Ude_stofnavn_2","v":""},null,{"$f":"D_Ude_stofnavn_3","v":""},null,{"$f":"D_Ude_stofnavn_4","v":""}]
[]
["Poreluftskoncentration ","CL",{"$f":"IF(ISNUMBER(D_Ude_CL_1),ROUND(D_Ude_CL_1,Ude_ciffer-(INT(LOG(D_Ude_CL_1))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_CL_2),ROUND(D_Ude_CL_2,Ude_ciffer-(INT(LOG(D_Ude_CL_2))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_CL_3),ROUND(D_Ude_CL_3,Ude_ciffer-(INT(LOG(D_Ude_CL_3))+1)),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_CL_4),ROUND(D_Ude_CL_4,Ude_ciffer-(INT(LOG(D_Ude_CL_4))+1)),\"\")","v":""},null,"mg/m³"]
["Beregnet værdi anvendt",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(C24=\"Ja\", \"Nej\",IF(D_Ude_CL_1=Enk_My_CL_1,\"Nej\",\"Ja\")),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(E24=\"Ja\", \"Nej\",IF(D_Ude_CL_2=Enk_My_CL_2,\"Nej\",\"Ja\")),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(G24=\"Ja\", \"Nej\",IF(D_Ude_CL_3=Enk_My_CL_3,\"Nej\",\"Ja\")),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(I24=\"Ja\", \"Nej\",IF(D_Ude_CL_4=Enk_My_CL_4,\"Nej\",\"Ja\")),\"\")","v":""}]
["Testværdi anvendt",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(ISNUMBER(Ude_My_CL_1),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(ISNUMBER(Ude_My_CL_2),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(ISNUMBER(Ude_My_CL_3),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(ISNUMBER(Ude_My_CL_4),\"Ja\",\"Nej\"),\"\")","v":""}]
["Baggrundskoncentration","C0",{"$f":"D_Ude_C0_1","v":""},null,{"$f":"D_Ude_C0_2","v":""},null,{"$f":"D_Ude_C0_3","v":""},null,{"$f":"D_Ude_C0_4","v":""},null,"mg/m³"]
[]
["Stofegenskaber"]
["Kommentar",{"$f":"IF(D_Enk_Kem_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Diffusionskoefficient luft","DL",{"$f":"IF(D_Enk_DL_syst_1<>\"\",D_Enk_DL_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_DL_1<>\"\",Enk_My_DL_1,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_2<>\"\",D_Enk_DL_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_DL_2<>\"\",Enk_My_DL_2,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_3<>\"\",D_Enk_DL_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_DL_3<>\"\",Enk_My_DL_3,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_4<>\"\",D_Enk_DL_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_DL_4<>\"\",Enk_My_DL_4,\"\")","v":""},"m²/s"]
["Vindhastighed ","v",{"$f":"IF(D_Enk_v_syst_1<>\"\",D_Enk_v_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_v_1<>\"\",Enk_My_v_1,\"\")","v":""},{"$f":"IF(D_Enk_v_syst_2<>\"\",D_Enk_v_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_v_2<>\"\",Enk_My_v_2,\"\")","v":""},{"$f":"IF(D_Enk_v_syst_3<>\"\",D_Enk_v_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_v_3<>\"\",Enk_My_v_3,\"\")","v":""},{"$f":"IF(D_Enk_v_syst_4<>\"\",D_Enk_v_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_v_4<>\"\",Enk_My_v_4,\"\")","v":""},"m/s"]
["(stofafhængig)"]
[]
["Det forurenede område "]
["Kommentar",{"$f":"IF(D_Ude_ForOm_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Længde af det forurenede område","l",null,null,{"$f":"IF(D_Ude_l<>\"\",D_Ude_l,\"\")","v":100},null,"m"]
["Opblandingshøjde ","h",null,null,{"$f":"IF(D_Ude_h<>\"\",D_Ude_h,\"\")","v":8},null,"m"]
["Opblandingshøjde/længde","h/l",null,null,{"$f":"IF(D_Ude_hl<>\"\",D_Ude_hl,\"\")","v":0.08}]
[]
["Beregning: Udeluft",null,"Angiv signifikant ciffer",null,2]
[]
[null,null,"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
["Målepunkt","MP",{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""}]
["Dato","dato",{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
["Totalbidrag til udeluft",null,{"$f":"IF(ISNUMBER(D_Ude_Cu_1),(ROUND(D_Ude_Cu_1,Ude_ciffer-(INT(LOG(D_Ude_Cu_1))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_Cu_2),(ROUND(D_Ude_Cu_2,Ude_ciffer-(INT(LOG(D_Ude_Cu_2))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_Cu_3),(ROUND(D_Ude_Cu_3,Ude_ciffer-(INT(LOG(D_Ude_Cu_3))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_Cu_4),(ROUND(D_Ude_Cu_4,Ude_ciffer-(INT(LOG(D_Ude_Cu_4))+1))),\"\")","v":""},null,"mg/m³"]
["Afdampningskriterie",null,{"$f":"IF(D_Enk_afd_krit_syst_1<>\"\",D_Enk_afd_krit_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_1<>\"\",Enk_My_afd_krit_1,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_2<>\"\",D_Enk_afd_krit_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_2<>\"\",Enk_My_afd_krit_2,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_3<>\"\",D_Enk_afd_krit_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_3<>\"\",Enk_My_afd_krit_3,\"\")","v":""},{"$f":"IF(D_Enk_afd_krit_syst_4<>\"\",D_Enk_afd_krit_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_afd_krit_4<>\"\",Enk_My_afd_krit_4,\"\")","v":""},"mg/m³"]
["Overskridelse af kriteriet",null,{"$f":"IF(ISNUMBER(D_Ude_afd_krit_vurdering_1),(ROUND(D_Ude_afd_krit_vurdering_1,Ude_ciffer-(INT(LOG(D_Ude_afd_krit_vurdering_1))+1))),D_Ude_afd_krit_vurdering_1)","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_afd_krit_vurdering_2),(ROUND(D_Ude_afd_krit_vurdering_2,Ude_ciffer-(INT(LOG(D_Ude_afd_krit_vurdering_2))+1))),D_Ude_afd_krit_vurdering_2)","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_afd_krit_vurdering_3),(ROUND(D_Ude_afd_krit_vurdering_3,Ude_ciffer-(INT(LOG(D_Ude_afd_krit_vurdering_3))+1))),D_Ude_afd_krit_vurdering_3)","v":""},null,{"$f":"IF(ISNUMBER(D_Ude_afd_krit_vurdering_4),(ROUND(D_Ude_afd_krit_vurdering_4,Ude_ciffer-(INT(LOG(D_Ude_afd_krit_vurdering_4))+1))),D_Ude_afd_krit_vurdering_4)","v":""}]
["Anvendt brugerdata?",null,{"$f":"D_Ude_Brugerdata_1","v":""},null,{"$f":"D_Ude_Brugerdata_2","v":""},null,{"$f":"D_Ude_Brugerdata_3","v":""},null,{"$f":"D_Ude_Brugerdata_4","v":""}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_Ude_Jord_Com<>\"\",D_Ude_Jord_Com,\"\")","v":""}]
["om jordlag"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ude_ForOm_Com<>\"\",D_Ude_ForOm_Com,\"\")","v":""}]
["om forurenet område"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ude_For_Com<>\"\",D_Ude_For_Com,\"\")","v":""}]
["om forurening"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Kem_Com<>\"\",D_Enk_Kem_Com,\"\")","v":""}]
["om kemiske stoffer"]

{"sheet":"Vejledning_Udeluft","index":26,"n_rows":89,"n_cols":2,"rows_kept":89,"cut":false,"hidden":true,"merged":[[11,1,14,15],[1,1,1,15],[9,1,9,15],[10,1,10,15],[2,1,8,15],[23,1,23,15],[24,1,29,15],[30,1,30,15],[15,1,15,15],[16,1,16,15],[17,1,21,15],[22,1,22,15],[48,1,56,15],[57,1,57,15],[58,1,58,15],[59,1,69,15],[70,1,70,15],[31,1,31,15],[32,1,34,14],[35,1,35,15],[37,1,42,15],[47,1,47,15],[45,1,46,15],[43,1,43,15],[44,1,44,15],[71,1,71,15],[72,1,73,15],[74,1,74,15],[75,1,75,15],[76,1,78,15],[80,1,80,15],[81,1,85,15],[86,1,86,15],[87,1,87,15],[88,1,89,15]]}
[null,"Vejledning - Udeluft"]
[null,"Formål"]
[null,"I dette regneark kan der foretages en beregning af konsekvenser for udeluft, jf. appendiks 5.3 i MST´s Oprydningsvejledning fra 1998. Ligning 18 er dog, rettet \nfra  N= VL3,33/(VL+VV)²  \ntil  N= VL2,5/(VL+VV)\nHvilket giver mindre ændringer på de beregnede koncentrationer i forhold til tidligere udgaver af JAGG"]
[]
[]
[]
[]
[]
[]
[null,"Beregninger"]
[null,"Jordtype:"]
[null,"Man kan vælge op til 4 forskellige jordlag enten som standardjordtyper fra listen eller oprette eller hente egenskaber fra egen liste ved at markere den ønskede jordtype. \n\nDet er også muligt at anvende og oprette egne \"jordtyper\" ved at klikke på knappen \"Egen liste\". "]
[]
[]
[]
[]
[null,"Det forurenede område:"]
[null,"Såfremt der kun indtastes oplysninger om længden af det forurenede område, vil opblandingshøjden blive justeret i henhold til en default opblandingsforhold på 0,08, jf. MST´s Oprydningsvejledning. Ved at indtaste en opblandingshøjde, for eksempel 1,6 m (indåndingshøjden), fås et lavere eller højere udeluftbidrag, afhængig af længden af det forurenede område. Opblandingshøjden er højde, hvorved der kan forventes fuld opblanding af forurening i atmosfæren for enden af det forurenede område, nedstrøms vind-retningen. "]
[]
[]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata, dvs. målte eller beregnede poreluftkoncentrationer fra fugacitetsmodulet overføres til udeluftmodulet.\n\nDer er også mulighed for at indtaste en baggrundskoncentration for udeluft, men denne påvirker kun diffusionsfluxen og vil derfor sjældent have betydning for bidraget til udeluften.\n\nHerudover kan der afprøves andre poreluftkoncentrationer, og i så fald ses en bemærkning i både brugerfladen og udskriften om, der er anvendt brugerdata. "]
[]
[]
[]
[]
[]
[]
[null,"GENERELT"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under olie & benzin modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under olie & benzin modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTVÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Vertikal Transport","index":27,"n_rows":405,"n_cols":34,"rows_kept":405,"cut":false,"hidden":true,"merged":[[99,32,101,38],[118,32,119,38],[111,25,111,29],[79,19,79,23],[80,7,80,11],[80,13,80,17],[80,19,80,23],[60,22,60,23],[70,10,70,11],[70,13,70,14],[59,16,61,17],[60,10,60,11],[66,10,66,11],[118,25,119,29],[82,7,82,11],[83,25,83,29],[83,13,83,17],[83,19,83,23],[105,13,105,17],[105,19,105,23],[105,25,105,29],[107,13,107,17],[107,19,107,23],[103,7,103,11],[9,25,9,29],[116,7,116,11],[116,13,116,17],[116,19,116,23],[116,25,116,29],[28,10,28,11],[30,10,30,11],[44,13,44,17],[33,10,33,11],[38,7,38,11],[40,7,40,11],[55,22,57,23],[58,28,58,29],[79,13,79,17],[80,25,80,29],[82,19,82,23],[82,25,82,29],[107,25,107,29],[109,7,109,11],[79,25,79,29],[55,25,57,26],[114,25,114,29],[114,19,114,23],[111,7,111,11],[103,19,103,23],[109,13,109,17],[103,25,103,29],[105,7,105,11],[111,13,111,17],[109,25,109,29],[101,13,101,17],[101,19,101,23],[101,25,101,29],[107,7,107,11],[101,7,101,11],[103,13,103,17],[3,7,3,23],[5,7,5,15],[5,19,5,23],[77,7,77,11],[77,13,77,17],[77,19,77,23],[54,7,54,31],[77,25,77,29],[60,13,60,14],[25,7,25,28],[42,7,43,11],[45,7,45,11],[44,7,44,11],[45,19,45,23],[59,19,61,20],[7,7,7,15],[7,19,7,23],[44,19,44,23],[9,7,9,11],[9,13,9,17],[9,19,9,23],[58,13,58,14],[58,16,58,17],[59,28,59,29],[16,32,19,37],[14,25,14,30],[55,28,57,29],[12,7,12,30],[58,19,58,20],[58,22,58,23],[341,1,341,5],[109,19,109,23],[114,7,114,11],[68,10,68,11],[66,13,66,14],[68,13,68,14],[14,10,14,14],[14,3,14,7],[14,17,14,22],[270,1,270,5],[111,19,111,23],[118,7,119,11],[118,13,119,17],[118,19,119,23],[85,13,85,17],[83,7,83,11],[35,7,35,11],[59,22,59,23],[58,25,58,26],[61,28,61,29],[23,10,23,15],[23,17,23,23],[23,25,23,30],[48,14,48,30],[61,10,61,11],[36,7,36,11],[30,26,30,28],[59,4,60,8],[55,16,57,17],[59,10,59,11],[55,19,57,20],[49,16,49,26],[46,16,46,26],[61,13,61,14],[23,3,23,8],[48,0,48,3],[28,0,28,4],[59,25,61,26],[11,3,11,30],[411,7,411,29],[73,7,75,29],[61,22,61,23],[59,13,59,14],[61,4,61,8],[98,25,99,29],[60,28,60,29],[33,7,33,8],[57,4,57,8],[58,10,58,11],[43,13,43,17],[48,7,48,11],[45,13,45,17],[85,19,85,23],[98,7,99,11],[98,13,99,17],[98,19,99,23],[79,7,79,11],[82,13,82,17],[85,7,85,11],[85,25,85,29],[55,10,57,11],[55,13,57,14]]}
["Vertikal transport til det førstkommende betydende grundvandsmagasin"]
[]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
["Beregning udføres for :",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
[]
[null,null,null,null,null,null,null,"Der skal vælges mellem de følgende beregningsmodeller for vertikal transport af organiske stoffer igennem et jordlag ned til førstkommende grundvandsmagasin"]
[]
[null,null,null,"Model A+C*",null,null,null,null,null,null,"Model B\n DTU V1D model 1a**",null,null,null,null,null,null,"Model B\n DTU V1D model 1b**",null,null,null,null,null,null,null,"Model B\n DTU V1D model 2**"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Der henvises til følgende Miljøprojekter:\n\n* JAGG 2 - Vertikal transport ned til førstkommende betydende magasin.\nChristensen, A.G., Binning, P. J., Troldborg, M., Kjeldsen, P. og Broholm, M.\nMiljøprojekt nr. 1828, 2016.\nMiljøstyrelsen\n\n** A risk assessment tool for contaminated sites in low-permeability fractured media.\nChambon, J., Bjerg, P.L. og Binning, P.J.\nEnvironmental Project No. 1786, 2015.\nThe Danish Environmental Protection Agency"]
[null,"Tid = 0"]
[]
[]
[]
[null,"Tid = x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.sara.env.dtu.dk/Modelvaerktoejer"]
[]
[null,null,null,"Stationære forhold kan opnås.\nKontinuer kilde. Dermed kan der beregnes en flux og en koncentration, som kan overføres til grundvandsmodulet. ",null,null,null,null,null,null,"Indledende stigende og herefter faldende koncentrationsbidrag til det førstkommende grundvandsmagasin.",null,null,null,null,null,null,"Stationære forhold kan opnås.\nKontinuer kilde. Dermed kan der beregnes en flux og koncentration, som kan overføres til grundvandsmodulet. ",null,null,null,null,null,null,null,"Aftagende koncentrationsbidrag til førstkommende grundvandsmagasin, da kilden i matrix udvaskes. "]
[]
["Kildeområde",null,null,null,null,null,null,"Indtast data om kildeområde.\n"]
[]
[]
["Længde af kildeområde",null,null,null,null,"Y",null,null,null,null,null,null,null,"m",{"$f":"IF(ISTEXT(Ver_Y),\"Tjek decimal\",\"\")","v":""}]
[]
["Bredde af kildeområde",null,null,null,null,"X",null,null,null,null,null,null,null,"m",{"$f":"IF(ISTEXT(Ver_X),\"Tjek decimal\",\"\")","v":""},null,null,null,"Areal af det forurenede område ",null,null,null,null,null,null,null,{"$f":"D_Ver_areal","v":{"$error":"#VALUE!"}},null,null,"m2"]
[]
[]
["Nettonedbør",null,null,null,null,"N",null,{"$f":"IF(ISNUMBER(D_Ver_infiltration_syst),D_Ver_infiltration_syst,\"\")","v":""},null,null,null,null,null,"mm/år"]
[]
["Kommune/Egn",null,null,null,null,null,null,{"$f":"IF(D_Ver_Egn_syst<>\"\",D_Ver_Egn_syst,\"\")","v":""}]
[]
[]
["Afstand til grundvandsspejl",null,null,null,null,"z",null,null,null,null,null,null,null,"m",{"$f":"IF(ISTEXT(Ver_z),\"Tjek decimal\",\"\")","v":""}]
[]
["Porevandshastighed",null,null,null,null,"Vw",null,{"$f":"D_ver_Vw_year","v":""},null,null,null,null,null,"m/år","(Porevandshastigheden vises kun efter indtastning af jordparametre)"]
[]
[null,null,null,null,null,null,null,"Normalinterval\n(stiger med afstand z)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Beregnet iht.  z "]
[null,null,null,null,null,null,null,"2-20 m",null,null,null,null,null,"jf. app. 5.8 figur 2.0",null,null,null,null,null,"Brugerdata"]
["Longitudinal dispersivitet",null,null,null,null,"αL,W",null,"0,004-0,07",null,null,null,null,null,{"$f":"D_Ver_alfaLw_beregn","v":6.5679999999999988E-2},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Ver_alfaLw),\"Tjek decimal\",\"\")","v":""}]
[]
[]
["Varighed af spild",null,null,null,null,"a",null,null,null,null,null,null,null,"år",{"$f":"IF(OR(D_vert_AC,D_vert_DTU_1b,D_vert_DTU_2),\"DTU V1D model 1a er ikke valgt og dette felt skal derfor være tomt\",IF(ISNUMBER(Ver_a_tjek),\"\",\"DTU V1D model 1a  er valgt - Tast varighed af spild\"))","v":"DTU V1D model 1a er ikke valgt og dette felt skal derfor være tomt"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(D_vert_AC,D_vert_DTU_1b,D_vert_DTU_2),0,Ver_a_tjek)","v":0}]
["(DTUV1D-model 1a)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(D_vert_AC,D_vert_DTU_1b,D_vert_DTU_2),1,\"\")","v":1}]
[]
[]
[]
["Jordparametre"]
[null,null,null,null,null,null,null,"Vælg jordart for fugacitetsberegning eller indtast egne jordartsdata"]
[null,null,null,null,null,null,null,null,null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,null,"Volumen\naf jordskellet",null,null,"Korn-rumvægt\n(kg/l)",null,null,"Bulkmasse-\nfylde\n (kg/l)",null,null,"% indhold af organisk kulstof"]
[]
[null,null,null,null,"Jordtype"]
[null,null,null,null,null,null,null,null,null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ",null,null,"d",null,null,"r",null,null,"foc"]
[null,null,null,null,{"$f":"IF(D_Ver_jord_syst<>\"\",D_Ver_jord_syst,)","v":0},null,null,null,null,null,{"$f":"IF(D_Ver_thetaa_int<>\"\",D_Ver_thetaa_int,\"\")","v":""},null,null,{"$f":"IF(D_Ver_thetaw_int<>\"\",D_Ver_thetaw_int,\"\")","v":""},null,null,{"$f":"D_Ver_ntotal","v":""},null,null,{"$f":"D_ver_Volj","v":""},null,null,{"$f":"IF(D_ver_d_int<>\"\",D_ver_d_int,\"\")","v":""},null,null,{"$f":"D_Ver_rhob","v":""},null,null,{"$f":"IF(D_Ver_foc_int<>\"\",D_Ver_foc_int,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Ver_thetaa_syst<>\"\",D_Ver_thetaa_syst,\"\")","v":""},null,null,{"$f":"IF(D_Ver_thetaw_syst<>\"\",D_Ver_thetaw_syst,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_ver_d_syst<>\"\",D_ver_d_syst,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Ver_foc_syst<>\"\",D_Ver_foc_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Ver_My_VL),\"Tjek decimal\",IF(ISTEXT(Ver_My_VV),\"Tjek decimal\",IF(ISTEXT(Ver_My_d),\"Tjek decimal\",IF(ISTEXT(Ver_My_foc),\"Tjek decimal\",\"\"))))","v":""}]
[]
["Ved sprækketransport",null,null,null,null,null,null,"Indtast sprækkeegenskaber eller anvend standardforslag"]
[null,null,null,null,null,null,null,null,null,null,"Standardforslag",null,null,"Brugerdata"]
[]
[null,"Sprækkeafstand (2B) ",null,null,null,null,null,null,null,null,5,null,null,null,null,null,"m","Normalinterval er fra 1 m i oxideret ler (de øvre jordlag - brunt ler) og 5 m i reduceret ler (gråt ler) i større dyber"]
[]
[null,"Sprækkeapertur (2b)",null,null,null,null,"Beregnes",null,null,null,null,null,null,{"$f":"D_ver_2bapertur","v":{"$error":"#VALUE!"}},null,null,"m"]
[]
[null,"Bulk-hydraulisk ledningsevne (Kb)",null,null,null,null,null,null,null,null,6.2999999999999995E-8,null,null,null,null,null,"m/s","Normalinterval er fra 2,4 x10-6 m/s i oxideret ler (de øvre jordlag - brunt ler) og 6,3 x10-8 m/s i reduceret ler (gråt ler) i større dybder"]
[]
[]
["Forurening",null,null,null,null,null,null,"Data for porevandskoncentration er overført fra fugacitetsmodulet \nIndtast eventuelt andre testværdier eller en baggrundskoncentration "]
[]
[]
[]
["Stofnavn (fra enkeltstoffer)",null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
[]
["Porevandskoncentration",null,null,null,null,"CV",null,{"$f":"D_Enk_CV_endelig_1","v":""},null,null,null,null,null,{"$f":"D_Enk_CV_endelig_2","v":""},null,null,null,null,null,{"$f":"D_Enk_CV_endelig_3","v":""},null,null,null,null,null,{"$f":"D_Enk_CV_endelig_4","v":""},null,null,null,null,null,"mg/l",null,"Overføres fra enkeltstoffer"]
["Test af andre værdier",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l",null,{"$f":"IF(ISTEXT(Ver_CV_1),\"Tjek decimal\",IF(ISTEXT(Ver_CV_2),\"Tjek decimal\",IF(ISTEXT(Ver_CV_3),\"Tjek decimal\",IF(ISTEXT(Ver_CV_4),\"Tjek decimal\",\"\"))))","v":""}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Angiv nedbrydningsforhold"]
["Nedbrydningsforhold"]
[]
[]
[]
[{"$f":"CONCATENATE(\"Beregning: Stationær (ligevægt) koncentration efter vertikal transport  ned til grundvandsspejlet i \", Ver_z,\" m´s dybde (z)\")","v":"Beregning: Stationær (ligevægt) koncentration efter vertikal transport  ned til grundvandsspejlet i  m´s dybde (z)"}]
[]
["Kun for model A+C og model B DTU V1D model 1b"]
[]
[]
["C(z), Porevandskoncentration lige ",null,null,null,null,null,null,{"$f":"D_Ver_Cz_1","v":false},null,null,null,null,null,{"$f":"D_Ver_Cz_2","v":false},null,null,null,null,null,{"$f":"D_Ver_Cz_3","v":false},null,null,null,null,null,{"$f":"D_Ver_Cz_4","v":false}]
["over grundvandet (input til trin 1a)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l "]
[]
["Grundvandskriterium",null,null,null,null,null,null,{"$f":"D_Enk_GV_Krit_1","v":""},null,null,null,null,null,{"$f":"D_enk_GV_Krit_2","v":""},null,null,null,null,null,{"$f":"D_Enk_GV_Krit_3","v":""},null,null,null,null,null,{"$f":"D_Enk_GV_Krit_4","v":""},null,null,null,null,null,"mg/l"]
[]
["Overskridelse af kriteriet",null,null,null,null,null,null,{"$f":"D_Ver_GVKKover_1","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_Ver_GVKKover_2","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_Ver_GVKKover_3","v":"Intet kriterie"},null,null,null,null,null,{"$f":"D_Ver_GVKKover_4","v":"Intet kriterie"},null,null,null,null,null,"gange"]
[]
["Anvendt nedbrydningskonstant",null,null,null,null,null,null,{"$f":"D_Ver_lambda_1","v":""},null,null,null,null,null,{"$f":"D_Ver_lambda_2","v":""},null,null,null,null,null,{"$f":"D_Ver_lambda_3","v":""},null,null,null,null,null,{"$f":"D_Ver_lambda_4","v":""},null,null,null,null,null,"dage-1"]
[]
["Retardationskoefficient",null,null,null,null,"R",null,{"$f":"D_Ver_R_1","v":""},null,null,null,null,null,{"$f":"D_Ver_R_2","v":""},null,null,null,null,null,{"$f":"D_Ver_R_3","v":""},null,null,null,null,null,{"$f":"D_Ver_R_4","v":""}]
[]
["Total flux",null,null,null,null,"J",null,{"$f":"D_Ver_Flux_1","v":false},null,null,null,null,null,{"$f":"D_Ver_Flux_2","v":false},null,null,null,null,null,{"$f":"D_Ver_Flux_3","v":false},null,null,null,null,null,{"$f":"D_Ver_Flux_4","v":false},null,null,null,null,null,"g/år"]
[]
["Anvendt brugerdata",null,null,null,null,null,null,{"$f":"D_ver_brugerdata_1","v":""},null,null,null,null,null,{"$f":"D_ver_brugerdata_2","v":""},null,null,null,null,null,{"$f":"D_ver_brugerdata_3","v":""},null,null,null,null,null,{"$f":"D_ver_brugerdata_4","v":""}]
[]
[{"$f":"CONCATENATE(\"Beregning: Transient koncentration efter vertikal transport ned til grundvandsspejlet i \",Ver_z, \" m´s dybde (z) efter \", Ver_t,\" år (t)\")","v":"Beregning: Transient koncentration efter vertikal transport ned til grundvandsspejlet i  m´s dybde (z) efter  år (t)"}]
["Tid (t)",null,null,null,null,null,null,null,null,null,null,null,null,"Tid, år",null,null,null,null,null,{"$f":"D_Ver_t","v":0},null,null,null,null,null,"Tid, dage"]
[]
[null,null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[]
["C(z,t), transient porevandskonc.",null,null,null,null,null,null,{"$f":"D_Ver_czt_1","v":""},null,null,null,null,null,{"$f":"D_Ver_czt_2","v":""},null,null,null,null,null,{"$f":"D_Ver_czt_3","v":""},null,null,null,null,null,{"$f":"D_Ver_czt_4","v":""}]
["lige over grundvandet efter tid, t",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mg/l"]
[]
[]
[null,null,null,null,null,null,null,"Vælg stof for dataplot over transiente og stationære koncentrationer i dybden"]
[]
[]
[]
[null,null,null,null,null,null,null,"Fordeling af porevandskoncentrationer i dybden ned til grundvandet "]
[]
[]
[null,"Stof 1",null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC,$D$15,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 1",null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,$K$15,IF(D_vert_DTU_1b,$R$15,$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Se : A risk assessment tool for contaminated sites in low-permeability fractures media."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chambon, J., Bjerg, P.L. og Binning, P.J. Environmental Project No. 1786, 2015."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sprækkemodel"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM: (Equivalent Porous media) Kun 1-D advektion og dispersion "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diffusion: Kun diffusion i porevolumen"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. orden model (Kun for DTU V1D model 2 - en aftagende kilde)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stationær koncentration: kun for DTU V1D model 1b - en kontinuer kilde"]
[]
[]
[]
[]
[null,"Stof 2",null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC,$D$15,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 2",null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,$K$15,IF(D_vert_DTU_1b,$R$15,$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Se : A risk assessment tool for contaminated sites in low-permeability fractures media."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chambon, J., Bjerg, P.L. og Binning, P.J. Environmental Project No. 1786, 2015."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sprækkemodel"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM: (Equivalent Porous media) Kun 1-D advektion og dispersion "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diffusion: Kun diffusion i porevolumen"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. orden model (Kun for DTU V1D model 2 - en aftagende kilde)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stationær koncentration: kun for DTU V1D model 1b - en kontinuer kilde"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 3",null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC,$D$15,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 3",null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,$K$15,IF(D_vert_DTU_1b,$R$15,$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Se : A risk assessment tool for contaminated sites in low-permeability fractures media."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chambon, J., Bjerg, P.L. og Binning, P.J. Environmental Project No. 1786, 2015."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sprækkemodel"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM: (Equivalent Porous media) Kun 1-D advektion og dispersion "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diffusion: Kun diffusion i porevolumen"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. orden model (Kun for DTU V1D model 2 - en aftagende kilde)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stationær koncentration: kun for DTU V1D model 1b - en kontinuer kilde"]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 4",null,{"$f":"D_Enk_stofnavn_4","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC,$D$15,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Stof 4",null,{"$f":"D_Enk_stofnavn_4","v":""},null,null,null,null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,$K$15,IF(D_vert_DTU_1b,$R$15,$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Se : A risk assessment tool for contaminated sites in low-permeability fractures media."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chambon, J., Bjerg, P.L. og Binning, P.J. Environmental Project No. 1786, 2015."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sprækkemodel"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM: (Equivalent Porous media) Kun 1-D advektion og dispersion "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diffusion: Kun diffusion i porevolumen"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1. orden model (Kun for DTU V1D model 2 - en aftagende kilde)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stationær koncentration: kun for DTU V1D model 1b - en kontinuer kilde"]

{"sheet":"Dataark_Vertikal_Transport","index":28,"n_rows":297,"n_cols":25,"rows_kept":297,"cut":false,"hidden":true,"merged":[[191,2,192,3],[191,4,192,4],[191,5,192,5],[192,8,192,15],[60,11,60,13],[60,14,60,16],[60,17,60,19],[117,8,117,13],[193,8,193,9],[161,7,161,9],[196,7,196,9],[6,2,6,6],[79,2,79,6],[71,2,71,6],[60,2,60,6],[71,17,71,19],[60,8,60,10],[16,1,16,10],[46,8,46,10],[46,11,46,13],[46,14,46,16],[46,17,46,19],[18,2,18,10],[46,2,46,6],[71,8,71,10],[71,11,71,13],[71,14,71,16],[226,2,227,3],[226,4,227,4],[226,5,227,5],[227,8,227,15],[228,8,228,9],[231,7,231,9],[261,2,262,3],[261,4,262,4],[261,5,262,5],[262,8,262,15],[298,8,298,9],[263,8,263,9],[266,7,266,9],[296,2,297,3],[296,4,297,4],[296,5,297,5],[297,8,297,15]]}
[]
[null,null,"Vertikal transport igennem enten homogen vandmættet ler eller umættet ler og sand fra en overliggende kontinuert kilde","Model A + C",true]
[null,null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kilde, hvor varigheden af spildet er kendt","Model B\n DTU V1D Model 1a",false]
[null,null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kontinuert kilde","Model B\n DTU V1D Model 1b",false]
[null,null,"Vertikal transport igennem homogen vandmættet sprækket ler fra den aftagende kilde i lermatrix","Model B\n DTU V1D Model 2",false]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[null,null,"Beregnede koncentrationer"]
[null,null,"C(z), stationær porevandkoncentration","Cz","mg/l",{"$f":"IF(D_vert_AC,D$2,IF(D_vert_DTU_1a,D$3,IF(D_vert_DTU_1b,D$4,D$5)))","v":"Model A + C"},null,null,null,null,{"$f":"B_Ver_Cz_1","v":false},null,null,{"$f":"B_Ver_Cz_2","v":false},null,null,{"$f":"B_Ver_Cz_3","v":false},null,null,{"$f":"B_Ver_Cz_4","v":false},null,"D_Ver_cz_n","beregnes"]
[null,null,"C(z,t), transient porevandkoncentration","Czt","mg/l",{"$f":"IF(D_vert_AC,D$2,IF(D_vert_DTU_1a,D$3,IF(D_vert_DTU_1b,D$4,D$5)))","v":"Model A + C"},null,null,null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_1),B_Ver_Czt_1,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_2),B_Ver_Czt_2,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_3),B_Ver_Czt_3,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_4),B_Ver_Czt_4,\"\")","v":""},null,"D_Ver_czt_n","beregnes"]
[null,null,"Flux for stationær porevandkonc",null,"g/år",{"$f":"IF(D_vert_AC,D$2,IF(D_vert_DTU_1a,D$3,IF(D_vert_DTU_1b,D$4,D$5)))","v":"Model A + C"},null,null,null,null,{"$f":"B_Ver_Flux_1","v":false},null,null,{"$f":"B_Ver_Flux_2","v":false},null,null,{"$f":"B_Ver_Flux_3","v":false},null,null,{"$f":"B_Ver_Flux_4","v":false},null,"D_Ver_Flux_n","beregnes"]
[null,null,"Overskridelse af GV-krit for stationær porevandkonc.",null,"gange",{"$f":"IF(D_vert_AC,D$2,IF(D_vert_DTU_1a,D$3,IF(D_vert_DTU_1b,D$4,D$5)))","v":"Model A + C"},null,null,null,null,{"$f":"B_Ver_GVKKover_1","v":"Intet kriterie"},null,null,{"$f":"B_Ver_GVKKover_2","v":"Intet kriterie"},null,null,{"$f":"B_Ver_GVKKover_3","v":"Intet kriterie"},null,null,{"$f":"B_Ver_GVKKover_4","v":"Intet kriterie"},null,"D_Ver_GVKKover_n","beregnes"]
[]
[]
[]
[]
[]
[null,"Vertikal Transport (MODEL A+C, FINAL DOMENICO)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,null,"JAGG2"]
[null,null,null,"Forkortelse","Enhed","Oprindelsessted",null,"Interval","Default/Beregnet","Indtastet","Anvendt"]
[null,null,"Jordtype",null,null,null,null,null,null,{"$f":"Ver_My_jord","v":0},{"$f":"IF(ISTEXT(J21),J21,I21)","v":0},null,null,null,null,null,null,null,null,null,null,"D_Ver_jord","input"]
[null,null,"Porevandshastighed","Vw","m/dag","beregnes",null,null,{"$f":"B_Ver_Vw","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J22),J22,IF(I22<>0,I22,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"D_Ver_Vw","beregnes"]
[null,null,"Porevandhastighed","Vw","m/år","Enhed konverteres",null,null,null,null,{"$f":"IF(ISNUMBER(D_Ver_Vw),D_Ver_Vw*365,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,"D_ver_vw_year","beregnes i dataark"]
[null,null,"Darcy hastighed (vand)","qw","m/dag","input",null,null,{"$f":"D_Ver_infiltration","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J24),J24,IF(I24<>0,I24,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"D_Ver_qw","input"]
[null,null,"Vandindhold","qw","-","input",null,null,null,{"$f":"Ver_My_VV","v":0},{"$f":"IF(VALUE(J25),J25,IF(I25<>0,I25,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_Ver_thetaw","input"]
[null,null,"Luftindhold","qa","-","input",null,null,null,{"$f":"IF(ISNUMBER(Ver_My_VL),Ver_My_VL,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(J26),J26,IF(I26<>0,I26,0))","v":0},null,null,null,null,null,null,null,null,null,null,"D_Ver_thetaa","input"]
[null,null,"Total porøsitet (VL+VV)","n","-","input",null,null,{"$f":"SUM(D_Ver_thetaw+D_Ver_thetaa)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(I27),I27,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,"D_Ver_ntotal","beregnes i dataark"]
[null,null,"Volumen af jordskellet","Vj",null,null,null,null,{"$f":"1-D_Ver_ntotal","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(I28),I28,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,"D_ver_volj","beregnes i dataark"]
[null,null,"Kildens længde","Y","m","input",null,null,null,{"$f":"Ver_Y","v":0},{"$f":"IF(VALUE(J29),J29,IF(I29<>0,I29,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_Ver_Y","input"]
[null,null,"Kildens bredde","X","m","input",null,null,null,{"$f":"Ver_X","v":0},"",null,null,null,null,null,null,null,null,null,null,"D_Ver_X","input"]
[null,null,"Areal af kilden",null,null,null,null,null,null,null,{"$f":"D_Ver_Y*D_Ver_X","v":{"$error":"#VALUE!"}}]
[null,null,"Afstand fra kildens underkant til GV-spejl","Z","m","input",null,null,null,{"$f":"Ver_z","v":0},"",null,null,null,null,null,null,null,null,null,null,"D_Ver_Z","input"]
[null,null,"% Indhold organisk kulstof","foc (%)","-","input",null,null,null,{"$f":"Ver_My_foc","v":0},"",null,null,null,null,null,null,null,null,null,null,null,"input"]
[null,null,"Fraktion organisk indhold","foc",null,"beregnet",null,null,null,null,{"$f":"K33/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"D_Ver_foc","beregnes i dataark"]
[null,null,"Korn rumvægt","d","kg/l","input",null,null,null,{"$f":"Ver_My_d","v":0},{"$f":"IF(VALUE(J35),J35,IF(I35<>0,I35,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_ver_d","input"]
[null,null,"Bulkmassefylde= volumenvægt","(rho)r","kg/l","beregnet",null,null,{"$f":"(D_ver_d*D_ver_Volj)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(I36),I36,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,"D_Ver_rhob","beregnes i dataark"]
[null,null,"Nettoinfiltration= nettonedbør","N","m/dag","beregnes",null,null,{"$f":"B_Ver_infiltration","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_Ver_infiltration","beregnes"]
[null,null,"Kommune/Egn",null,null,null,null,null,null,{"$f":"Ver_My_Egn","v":0},{"$f":"IF(ISTEXT(J38),J38,I38)","v":0},null,null,null,null,null,null,null,null,null,null,"D_Ver_Egn","input"]
[null,null,"Nettoinfiltration= nettonedbør","N","mm/år","input",null,null,null,{"$f":"Ver_My_N","v":0},"",null,null,null,null,null,null,null,null,null,null,"D_Ver_infiltration_Temp","input"]
[null,null,"Long. dispersivitet (vand)","(alfa)L,w","m","Beregnes",null,null,6.5679999999999988E-2,{"$f":"Ver_alfaLw","v":0},{"$f":"IF(VALUE(J40),J40,IF(ISNUMBER(I40),I40,\"\"))","v":6.5679999999999988E-2},null,null,null,null,null,null,null,null,null,null,"D_Ver_alfaLw","input"]
[null,null,"Trans. dispersivitet (vand)","(alfa)T,w","m","beregnes",null,null,6.5679999999999992E-3,null,6.5679999999999992E-3,"ikke anvendes og udgør",null,null,null,null,null,null,null,null,null,"D_Ver_alfaTw","input"]
[null,null,"Aerobe nedbrydningsforhold",null,null,"input",null,null,null,true,{"$f":"D_Ver_an","v":true},null,null,null,null,null,null,null,null,null,null,"D_Ver_an","Styrende parameter"]
[null,null,"Anaerob nedbrydningsforhold",null,null,"input",null,null,null,false,{"$f":"D_Ver_anan","v":false},null,null,null,null,null,null,null,null,null,null,"D_Ver_anan","Styrende parameter"]
[null,null,"Transient løsning, tid","t","år","input",null,null,null,{"$f":"Ver_t","v":0}]
[null,null,"Transient løsning, tid (dage)","t","dage","Beregnes",null,null,null,null,{"$f":"B_Ver_t","v":0},null,null,null,null,null,null,null,null,null,null,"D_Ver_t","beregnes"]
[]
[null,null,"Stoffer",null,null,null,null,null,"Stof 1",null,null,"stof 2",null,null,"stof 3",null,null,"stof 4"]
[null,null,null,"Forkortelse","Enhed","Oprindelsessted",null,null,"Default/Ber./overført","Indtastet","Anvendt","Default/Beregnet","Indtastet","Anvendt","Default/Beregnet","Indtastet","Anvendt","Default/Beregnet","Indtastet","Anvendt"]
[null,null,"Forureningskomponent","stofnavn_n","-","input",null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,{"$f":"IF(ISTEXT(J49),J49,IF(I49<>0,I49,\"\"))","v":""},{"$f":"D_Enk_stofnavn_2","v":""},null,{"$f":"IF(ISTEXT(M49),M49,IF(L49<>0,L49,\"\"))","v":""},{"$f":"D_Enk_stofnavn_3","v":""},null,{"$f":"IF(ISTEXT(P49),P49,IF(O49<>0,O49,\"\"))","v":""},{"$f":"D_Enk_stofnavn_4","v":""},null,{"$f":"IF(ISTEXT(S49),S49,IF(R49<>0,R49,\"\"))","v":""},null,"D_Ver_stofnavn_n","Overført fra Enkeltstoffer"]
[null,null,"Kildekoncentration","C0_n","mg/L","input",null,null,{"$f":"D_Enk_CV_endelig_1","v":""},{"$f":"Ver_CV_1","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(J50),J50,IF(I50<>0,I50,\"\")),\"\")","v":""},{"$f":"D_Enk_CV_endelig_2","v":""},{"$f":"Ver_CV_2","v":0},{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(VALUE(M50),M50,IF(L50<>0,L50,\"\")),\"\")","v":""},{"$f":"D_Enk_CV_endelig_3","v":""},{"$f":"Ver_CV_3","v":0},{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(VALUE(P50),P50,IF(O50<>0,O50,\"\")),\"\")","v":""},{"$f":"D_Enk_CV_endelig_4","v":""},{"$f":"Ver_CV_4","v":0},{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(VALUE(S50),S50,IF(R50<>0,R50,\"\")),\"\")","v":""},null,"D_Ver_C0_n","Overført fra Enkeltstoffer"]
[null,null,"Nedbrydning (1. orden) aerobe forhold","(lambda)_ae_n","dag^-1","input",null,null,{"$f":"D_Enk_k1aerob_uz_syst_1","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_1),Enk_My_k1aerob_umættet_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(J51),J51,I51)","v":0},{"$f":"D_Enk_k1aerob_uz_syst_2","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_2),Enk_My_k1aerob_umættet_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(M51),M51,L51)","v":0},{"$f":"D_Enk_k1aerob_uz_syst_3","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_3),Enk_My_k1aerob_umættet_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(P51),P51,O51)","v":0},{"$f":"D_Enk_k1aerob_uz_syst_4","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1aerob_umættet_4),Enk_My_k1aerob_umættet_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(S51),S51,R51)","v":0},null,"D_Ver_lambda_aerobe_n","Overført fra Enkeltstoffer"]
[null,null,"Nedbrydning (1. orden) anaerobe forhold","(lambda)_an_n","dag^-1","input",null,null,{"$f":"D_Enk_k1anaerob_umættet_syst_1","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_1),Enk_My_k1anaerob_umættet_1,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(J52),J52,I52)","v":0},{"$f":"D_Enk_k1anaerob_umættet_syst_2","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_2),Enk_My_k1anaerob_umættet_2,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(M52),M52,L52)","v":0},{"$f":"D_Enk_k1anaerob_umættet_syst_3","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_3),Enk_My_k1anaerob_umættet_3,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(P52),P52,O52)","v":0},{"$f":"D_Enk_k1anaerob_umættet_syst_4","v":0},{"$f":"IF(ISNUMBER(Enk_My_k1anaerob_umættet_4),Enk_My_k1anaerob_umættet_4,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(S52),S52,R52)","v":0},null,"D_Ver_lambda_anaerobe_n","Overført fra Enkeltstoffer"]
[null,null,"Anvendt nedbrydningskonstant","(lambda)_n","dag^-1","beregnes",null,null,{"$f":"B_Ver_lambda_1","v":""},null,{"$f":"I53","v":""},{"$f":"B_Ver_lambda_2","v":""},null,{"$f":"L53","v":""},{"$f":"B_Ver_lambda_3","v":""},null,{"$f":"O53","v":""},{"$f":"B_Ver_lambda_4","v":""},null,{"$f":"R53","v":""},null,"D_Ver_lambda_n","beregnes"]
[null,null,"Diffusionskoefficient (luft)","Dd,a_n","m2/sek","Input",null,null,{"$f":"D_Enk_DL_syst_1","v":0},{"$f":"Enk_My_DL_1","v":0},{"$f":"IF(VALUE(J54),J54,IF(I54<>0,I54,\"\"))","v":""},{"$f":"D_Enk_DL_syst_2","v":0},{"$f":"Enk_My_DL_2","v":0},{"$f":"IF(VALUE(M54),M54,IF(L54<>0,L54,\"\"))","v":""},{"$f":"D_Enk_DL_syst_3","v":0},{"$f":"Enk_My_DL_3","v":0},{"$f":"IF(VALUE(P54),P54,IF(O54<>0,O54,\"\"))","v":""},{"$f":"D_Enk_DL_syst_4","v":0},{"$f":"Enk_My_DL_4","v":0},{"$f":"IF(VALUE(S54),S54,IF(R54<>0,R54,\"\"))","v":""},null,"D_Ver_DL_Temp_n","input"]
[null,null,"Diffusionskoefficient (luft)","Dd,a_n","m2/dag","beregnes",null,null,{"$f":"B_Ver_DL_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J55),J55,IF(I55<>0,I55,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_DL_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(M55),M55,IF(L55<>0,L55,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_DL_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(P55),P55,IF(O55<>0,O55,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_DL_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(S55),S55,IF(R55<>0,R55,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Ver_DL_n","Overført fra Enkeltstoffer"]
[null,null,"Effektiv diffusionskoefficient (luft)","D*a_n","m2/dag","beregnes",null,null,{"$f":"B_Ver_Da_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J56),J56,IF(I56<>0,I56,0))","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_Da_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(M56),M56,IF(L56<>0,L56,0))","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_Da_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(P56),P56,IF(O56<>0,O56,0))","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_Da_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(S56),S56,IF(R56<>0,R56,0))","v":{"$error":"#VALUE!"}},null,"D_Ver_Da_n","Overført fra Enkeltstoffer"]
[null,null,"Fordelingskoefficient ml. organisk kulstof og vand","Koc","l/kg","input",null,null,{"$f":"D_Enk_KOC_1","v":0},null,{"$f":"IF(VALUE(J57),J57,IF(I57<>0,I57,0))","v":0},{"$f":"D_Enk_KOC_2","v":0},null,{"$f":"IF(VALUE(M57),M57,IF(L57<>0,L57,0))","v":0},{"$f":"D_Enk_KOC_3","v":0},null,{"$f":"IF(VALUE(P57),P57,IF(O57<>0,O57,0))","v":0},{"$f":"IF(ISNUMBER(D_Enk_KOC_4),D_Enk_KOC_4,\"\")","v":0},null,{"$f":"IF(VALUE(S57),S57,IF(R57<>0,R57,0))","v":0},null,"D_Ver_KOC_n","Overført fra Enkeltstoffer"]
[null,null,"Grundvandskriteriet",null,"mg/l","input",null,null,null,null,{"$f":"D_Enk_GV_Krit_1","v":""},null,null,{"$f":"D_enk_GV_Krit_2","v":""},null,null,{"$f":"D_Enk_GV_Krit_3","v":""},null,null,{"$f":"D_Enk_GV_Krit_4","v":""},null,null,"Overført fra Enkeltstoffer"]
[null,null,"Henrys konstant","KH_n","-","input",null,null,{"$f":"D_Enk_KH_1","v":0},null,{"$f":"IF(VALUE(J59),J59,IF(I59<>0,I59,\"\"))","v":""},{"$f":"D_Enk_KH_2","v":0},null,{"$f":"IF(VALUE(M59),M59,IF(L59<>0,L59,\"\"))","v":""},{"$f":"D_Enk_KH_3","v":0},null,{"$f":"IF(VALUE(P59),P59,IF(O59<>0,O59,\"\"))","v":""},{"$f":"D_Enk_KH_4","v":0},null,{"$f":"IF(VALUE(S59),S59,IF(R59<>0,R59,\"\"))","v":""},null,"D_Ver_KH_n","Overført fra Enkeltstoffer"]
[null,null,null,null,null,null,null,null,null,null,"",null,null,"",null,null,"",null,null,""]
[null,null,"Vanddata",null,null,null,null,null,"Vanddata",null,null,"Vanddata",null,null,"Vanddata",null,null,"Vanddata"]
[null,null,"Hydrodynamisk long. disp (vand)","Dz","m2/dag","beregnes",null,null,{"$f":"B_Ver_Dz_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_Dz_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_Dz_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_Dz_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_Dz_n","beregnes"]
[null,null,"Hydrodynamisk trans. disp (vand)","Dy, Dx","m2/dag","beregnes",null,null,{"$f":"B_Ver_DyDx_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_DyDx_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_DyDx_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_DyDx_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_DyDx_n","beregnes"]
[null,null,"Retardationsfaktor","R","-","beregnes",null,null,{"$f":"B_Ver_R_1","v":""},null,{"$f":"IF(ISNUMBER(I64),I64,\"\")","v":""},{"$f":"B_Ver_R_2","v":""},null,{"$f":"IF(ISNUMBER(L64),L64,\"\")","v":""},{"$f":"B_Ver_R_3","v":""},null,{"$f":"IF(ISNUMBER(O64),O64,\"\")","v":""},{"$f":"B_Ver_R_4","v":""},null,{"$f":"IF(ISNUMBER(R64),R64,\"\")","v":""},null,"D_Ver_R_n","beregnes"]
[null,null,"Diffusionskoefficient (vand)","Dd,w","m2/s","input",null,null,{"$f":"D_Enk_Ddw_1","v":0},{"$f":"Enk_My_Ddw_1","v":0},{"$f":"IF(VALUE(J65),J65,IF(I65<>0,I65,\"\"))","v":""},{"$f":"D_Enk_Ddw_2","v":0},{"$f":"Enk_My_Ddw_2","v":0},"",{"$f":"D_Enk_Ddw_3","v":0},{"$f":"Enk_My_Ddw_3","v":0},"",{"$f":"D_Enk_Ddw_4","v":0},{"$f":"Enk_My_Ddw_4","v":0},"",null,"D_Ver_Ddw_n","Overført fra Enkeltstoffer"]
[null,null,"Diffusionskoefficient (vand)","Dd,w","m2/dag","beregnet",null,null,{"$f":"B_ver_Ddw_1","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J66),J66,IF(I66<>0,I66,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_ver_ddw_2","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(M66),M66,IF(L66<>0,L66,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_ver_Ddw_3","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(P66),P66,IF(O66<>0,O66,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"B_ver_Ddw_4","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(R66),R66,IF(#REF!<>0,#REF!,\"\"))","v":{"$error":"#VALUE!"}}]
[null,null,"Effektiv diffusionskoefficient (vand)","D*w","m2/dag","beregnes",null,null,{"$f":"B_Ver_Dw_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_Dw_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_Dw_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_Dw_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_Dw_n","beregnes"]
[]
[null,null,"Anvendt brugerdata",null,null,null,null,null,null,{"$f":"SUM($J25:$J26,$J33:$J35,$J39:$J41,J50:J54,J65)","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(J69>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM($J25:$J26,$J33:$J35,$J39:$J41,M50:M54,M65)","v":0},{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(M69>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM($J25:$J26,$J33:$J35,$J39:$J41,P50:P54,P65)","v":0},{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(P69>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""},null,{"$f":"SUM($J25:$J26,$J33:$J35,$J39:$J41,S50:S54,S65)","v":0},{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(S69>0,\"Ja, se bemærkning\",\"Nej\"),\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,"",null,null,"",null,null,"",null,null,""]
[null,null,null,null,null,null,null,null,null,null,"",null,null,"",null,null,"",null,null,""]
[null,null,"Hjælpekonstanter",null,null,null,null,null,"Hjælpekonstanter",null,null,"Hjælpekonstanter",null,null,"Hjælpekonstanter",null,null,"Hjælpekonstanter"]
[null,null,"u","u","m/dag","beregnes",null,null,{"$f":"B_Ver_u_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_u_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_u_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_u_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_u_n","beregnes"]
[null,null,"Arg1","Arg1","-","beregnes",null,null,{"$f":"B_Ver_Arg1_1","v":""},null,{"$f":"IF(ISNUMBER(I74),I74,\"\")","v":""},{"$f":"B_Ver_Arg1_2","v":""},null,{"$f":"IF(ISNUMBER(L74),L74,\"\")","v":""},{"$f":"B_Ver_Arg1_3","v":""},null,{"$f":"IF(ISNUMBER(O74),O74,\"\")","v":""},{"$f":"B_Ver_Arg1_3","v":""},null,{"$f":"IF(ISNUMBER(R74),R74,\"\")","v":""},null,"D_Ver_Arg1_n","beregnes"]
[null,null,"ArgX","ArgX","-","beregnes",null,null,{"$f":"B_Ver_ArgX_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgX_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgX_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgX_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_ArgX_n","beregnes"]
[null,null,"ArgY","ArgY","-","beregnes",null,null,{"$f":"B_Ver_ArgY_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgY_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgY_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgY_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_ArgY_n","beregnes"]
[null,null,"ArgZ (Rqw+KHqa)","Rqw+KHqa ","-","beregnes",null,null,{"$f":"B_Ver_ArgZ_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgZ_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgZ_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"B_Ver_ArgZ_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Ver_ArgZ_n","beregnes"]
[]
[]
[null,null,"Beregnede koncentrationer"]
[null,null,"C(z), stationær porevandkoncentration","Cz","mg/l",null,null,null,null,null,{"$f":"IF(ISNUMBER(B_ver_Cz_AC_1),B_ver_Cz_AC_1,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_CZ_AC_2),B_Ver_CZ_AC_2,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Cz_AC_3),B_Ver_Cz_AC_3,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_ver_Cz_AC_4),B_ver_Cz_AC_4,\"\")","v":""},null,"D_Ver_cz_n","beregnes"]
[null,null,"C(z,t), transient porevandkoncentration","Czt","mg/l",null,null,null,null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_AC_1),B_Ver_Czt_AC_1,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_AC_2),B_Ver_Czt_AC_2,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_AC_3),B_Ver_Czt_AC_3,\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(B_Ver_Czt_AC_4),B_Ver_Czt_AC_4,\"\")","v":""},null,"B_Ver_czt_n","beregnes"]
[]
[]
[]
[]
[null,null,"Jordtype:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_Enk_Kil_Com","Import . Bemærkningsfelt"]
[null,null,null,false]
[null,null,"Kilde data:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_Enk_Jord_Com","Import . Bemærkningsfelt"]
[null,null,null,false]
[null,null,"Forurening:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_Enk_For_Com","Import . Bemærkningsfelt"]
[null,null,null,false]
[null,null,"Beregning:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_Enk_Ber_Com","Import . Bemærkningsfelt"]
[null,null,null,false]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"SprækkeTransport - DTU-V1D-remtec"]
[]
[]
[null,null,"Model 1a og 1b og C"]
[]
[null,null,"Presence of fractures",null,"yes","For alle beregninger antages sprækker"]
[null,null,{"$f":"IF(E112=\"yes\",\"\",\"Advection in low-permeability media (yes/no)\")","v":""}]
[null,null,"If initially contaminated (yes/no)",null,{"$f":"IF(D_vert_DTU_2,\"yes\",\"no\")","v":"no"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_vert_DTU_2","input","true or false","true or false"]
[]
[]
[]
[null,null,"INPUT"]
[null,null,"BOX 1: General Input",null,null,null,null,null,"stof 1","Stof 2","Stof 3","Stof 4"]
[null,null,null,null,null,null,null,null,{"$f":"D_Ver_stofnavn_1","v":""},{"$f":"D_Ver_stofnavn_2","v":""},{"$f":"D_Ver_stofnavn_3","v":""},{"$f":"D_Ver_stofnavn_4","v":""}]
[null,null,"Input concentration","C0 (mg/l)",null,null,null,null,{"$f":"D_Ver_C0_1","v":""},{"$f":"D_Ver_C0_2","v":""},{"$f":"D_Ver_C0_3","v":""},{"$f":"D_Ver_C0_4","v":""},null,null,null,null,null,null,null,null,null,"D_Ver_C0_x","input"]
[null,null,"Matrix porosity","f",{"$f":"D_Ver_ntotal","v":""},{"$f":"D_Ver_jord","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_ntotal  ","input fra jordparametre"]
[null,null,"Diffusion coefficient in matrix","Dm (m2/year)",null,null,null,null,{"$f":"IF(ISNUMBER(B_ver_Ddwm_1),B_ver_Ddwm_1,\"\")","v":""},{"$f":"IF(ISNUMBER(B_ver_Ddwm_2),B_ver_Ddwm_2,\"\")","v":""},{"$f":"IF(ISNUMBER(B_ver_Ddwm_3),B_ver_Ddwm_3,\"\")","v":""},{"$f":"IF(ISNUMBER(B_ver_Ddwm_4),B_ver_Ddwm_4,\"\")","v":""},null,null,null,null,null,null,null,null,null,"D_Ver_Ddwm_x","beregnes i beregningsark"]
[null,null,"Degradation rate","l (dag-1)",null,{"$f":"IF(D_Ver_an,\"aerobe\",\"anaerobe\")","v":"aerobe"},null,null,{"$f":"D_Ver_lambda_1","v":""},{"$f":"D_Ver_lambda_2","v":""},{"$f":"D_Ver_lambda_3","v":""},{"$f":"D_Ver_lambda_4","v":""},null,null,null,null,null,null,null,null,null,"D_Ver_lambda_x","input"]
[null,null,"Degradation rate","l (year-1)",null,{"$f":"IF(D_Ver_an,\"aerobe\",\"anaerobe\")","v":"aerobe"},null,null,{"$f":"B_Ver_lambdayear_1","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_lambdayear_2","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_lambdayear_3","v":{"$error":"#VALUE!"}},{"$f":"B_Ver_lambdayear_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"D_Ver_lambdayear_x","beregnes i beregningsark"]
[null,null,"Retardation, fracture","Rf",null,"lige med Rm","jf. Chambon et al.J. of contaminant Hydrology 124 (2011),82-98",null,{"$f":"D_Ver_R_1","v":""},{"$f":"D_Ver_R_2","v":""},{"$f":"D_Ver_R_3","v":""},{"$f":"D_Ver_R_4","v":""},null,null,null,null,null,null,null,null,null,"D_Ver_R_x","beregnes i beregningsark"]
[null,null,"Retardation, matrix","Rm",null,"stof afhængig",null,null,{"$f":"D_Ver_R_1","v":""},{"$f":"D_Ver_R_2","v":""},{"$f":"D_Ver_R_3","v":""},{"$f":"D_Ver_R_4","v":""},null,null,null,null,null,null,null,null,null,"D_Ver_R_x","beregnes i beregningsark"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_ver_2bapertur","v":{"$error":"#VALUE!"}}]
[null,null,"Water velocity","vf (m/year)",{"$f":"B_ver_Vvel","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_Vvel","beregnes i beregningsark"]
[null,null,"Average velocity in EPM","vEPM (m/year)",{"$f":"B_Ver_EPM","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_EPM","beregnes i beregningsark"]
[null,null,"Longitudinal dispersivity","α (m)",{"$f":"D_Ver_alfaLw","v":6.5679999999999988E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_alfaLw","input"]
[null,null,"Spill time","a (year)",{"$f":"IF(D_vert_DTU_2, \"Aftagende\",IF(Ver_a>0,Ver_a,\"Vedvarende\"))","v":"Vedvarende"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_a","input"]
[]
[null,null,"BOX 2: Hydrogeological properties"]
[null,null,"calculated using from Box 3"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_ver_2B","v":""}]
[null,null,"Fracture aperture","2*b (m)",{"$f":"B_ver_2bapertur","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_2bapertur","beregnes i beregningsark"]
[null,null,"Bulk hydrualic conductivity","Kb (m/s)",{"$f":"D_ver_Kb","v":""}]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_Ver_infil","v":""}]
[null,null,"Vertical gradient","i (-)",{"$f":"B_ver_Vgrad","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_Vgrad","Beregens i beregningsark"]
[]
[null,null,"BOX 3: Specific Input depending on conceptual model",null,null,"Default/Ber./overført","Indtastet","Anvendt"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_ver_2B","v":""},{"$f":"Ver_2B","v":5},{"$f":"Ver_My_2B","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(G143),G143,IF(F143<>0,F143,\"\")),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_2B","input"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_ver_2bapertur","v":{"$error":"#VALUE!"}}]
[null,null,"Bulk hydraulic conductivity","Kb (m/s)",{"$f":"D_ver_Kb","v":""},{"$f":"Ver_Kb","v":6.2999999999999995E-8},{"$f":"Ver_My_Kb","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(G145),G145,IF(F145<>0,F145,\"\")),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_Kb","Input"]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_Ver_infiltration_Temp","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_infil","Input se oven D_Ver_infiltration_Temp"]
[null,null,"Vertical gradient","i (-)",{"$f":"D_Ver_Vgrad","v":{"$error":"#VALUE!"}}]
[]
[null,null,"BOX 4: Calculated Parameters-"]
[null,null,"A",null,null,null,null,null,{"$f":"B_ver_A_1","v":{"$error":"#VALUE!"}},{"$f":"B_ver_A_2","v":{"$error":"#VALUE!"}},{"$f":"B_ver_A_3","v":{"$error":"#VALUE!"}},{"$f":"B_ver_A_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"D_ver_A_X","Beregens i beregningsark"]
[null,null,"B ",null,null,null,null,null,{"$f":"B_ver_B_1","v":{"$error":"#VALUE!"}},{"$f":"B_ver_B_2","v":{"$error":"#VALUE!"}},{"$f":"B_ver_B_3","v":{"$error":"#VALUE!"}},{"$f":"B_ver_B_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"D_ver_B_X","Beregens i beregningsark"]
[null,null,"G",null,null,null,null,null,{"$f":"B_ver_G_1","v":{"$error":"#VALUE!"}},{"$f":"B_ver_G_2","v":{"$error":"#VALUE!"}},{"$f":"B_ver_G_3","v":{"$error":"#VALUE!"}},{"$f":"B_ver_G_4","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"D_ver_G_X","Beregens i beregningsark"]
[]
[null,null,"BOX 5: Calculation and graphic parameters"]
[null,null,"Time increment","(year)",{"$f":"B_ver_t_incre","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_t_incre","Beregens i beregningsark"]
[null,null,"Depth increment","(m)",{"$f":"B_ver_z_incr","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_z_incr","Beregens i beregningsark"]
[null,null,"Time plot",null,{"$f":"B_ver_timeplot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_ver_timeplot","Beregens i beregningsark"]
[null,null,"Time","t (year)",{"$f":"Ver_t","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver_t","input"]
[null,null,"Depth","z(m)",{"$f":"Ver_z","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver_z","input"]
[]
[]
[null,null,"Stof 1",{"$f":"D_Ver_stofnavn_1","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",Ver_z,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"B_Ver_Cz_DTU_1","v":0},"mg/l",{"$f":"IF(D_vert_AC,$D$2,IF(D_vert_DTU_1a,$D$3,IF(D_vert_DTU_1b,$D$4,$D$5)))","v":"Model A + C"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Koncentration i matrix i forskellige afstand (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstand (m) fra sprækken i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Koncentration i matrix  \ni forskellige afstand (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix  \ni forskellige afstand (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"B_ver_DTU_2_tmax_1","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[]
[]
[]
[]
[null,null,"Stof 2",{"$f":"D_Ver_stofnavn_2","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",Ver_z,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"B_ver_Cz_DTU_2","v":0},"mg/l",{"$f":"IF(D_vert_AC,$D$2,IF(D_vert_DTU_1a,$D$3,IF(D_vert_DTU_1b,$D$4,$D$5)))","v":"Model A + C"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Koncentration i matrix\n i forskellige afstand (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix\n i forskellige afstand (m) fra sprækken i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Koncentration i matrix i forskellige afstand (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstand (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"B_ver_DTU_2_tmax_2","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[]
[]
[]
[]
[null,null,"Stof 3",{"$f":"D_Ver_stofnavn_3","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",Ver_z,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"B_ver_Cz_DTU_3","v":0},"mg/l",{"$f":"IF(D_vert_AC,$D$2,IF(D_vert_DTU_1a,$D$3,IF(D_vert_DTU_1b,$D$4,$D$5)))","v":"Model A + C"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Koncentration i matrix i forskellige afstand (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstand (m) fra sprækken i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Koncentration i matrix i forskellige afstand (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstand (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"B_ver_DTU_2_tmax_3","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[]
[]
[]
[]
[null,null,"Stof 4",{"$f":"D_Ver_stofnavn_4","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",Ver_z,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"B_ver_Cz_DTU_3","v":0},"mg/l",{"$f":"IF(D_vert_AC,$D$2,IF(D_vert_DTU_1a,$D$3,IF(D_vert_DTU_1b,$D$4,$D$5)))","v":"Model A + C"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Koncentration i matrix i forskellige afstand (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstand (m) fra sprækken i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Koncentration i matrix i forskellige afstand (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstand (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"B_ver_DTU_2_tmax_3","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]

{"sheet":"Beregning_Vertikal_Transport","index":29,"n_rows":674,"n_cols":35,"rows_kept":674,"cut":false,"hidden":true,"merged":[[49,2,49,6],[6,2,6,6],[236,8,237,8],[14,1,14,16],[16,2,16,9],[25,2,25,6],[25,7,25,9],[25,10,25,12],[25,13,25,15],[25,16,25,18],[56,3,56,9],[162,8,162,13],[206,7,206,9],[234,2,235,3],[234,4,235,4],[234,5,235,5],[41,2,41,6],[41,7,41,9],[41,10,41,12],[41,13,41,15],[41,16,41,18],[33,2,33,6],[33,7,33,9],[33,10,33,12],[33,13,33,15],[33,16,33,18],[236,32,237,32],[236,31,237,31],[236,9,236,15],[236,16,236,22],[56,20,56,26],[105,3,105,9],[105,20,105,26],[235,8,235,15],[236,7,237,7],[236,6,237,6],[324,7,324,9],[351,23,354,23],[351,24,354,24],[354,16,354,22],[233,23,236,23],[233,24,236,24],[352,2,353,3],[352,4,353,4],[352,5,353,5],[353,8,353,15],[354,6,355,6],[354,7,355,7],[354,8,355,8],[354,9,354,15],[354,31,355,31],[354,32,355,32],[442,7,442,9],[469,23,472,23],[469,24,472,24],[472,16,472,22],[472,31,473,31],[472,32,473,32],[470,2,471,3],[470,4,471,4],[470,5,471,5],[471,8,471,15],[472,6,473,6],[472,7,473,7],[472,8,473,8],[472,9,472,15],[588,2,589,3],[588,4,589,4],[588,5,589,5],[589,8,589,15],[590,6,591,6],[590,7,591,7],[590,8,591,8],[590,9,590,15],[590,31,591,31],[590,32,591,32],[560,7,560,9],[587,23,590,23],[587,24,590,24],[590,16,590,22]]}
[]
[]
[null,null,"Vertikal transport igennem enten homogen vandmættet ler eller umættet ler og sand fra en overliggende kontinuert kilde","(Model A + C)",{"$f":"D_vert_AC","v":true}]
[null,null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kilde, hvor varigheden af spildet er kendt","(Model B DTU V1D Model 1a)",{"$f":"D_vert_DTU_1a","v":false}]
[null,null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kontinuert kilde","(Model B DTU V1D Model 1b)",{"$f":"D_vert_DTU_1b","v":false}]
[null,null,"Vertikal transport igennem homogen vandmættet sprækket ler fra den aftagende kilde i lermatrix","(Model B DTU V1D Model 2)",{"$f":"D_vert_DTU_2","v":false},null,null,null,null,{"$f":"D_Enk_stofnavn_1","v":""},null,null,{"$f":"D_Enk_stofnavn_2","v":""},null,null,{"$f":"D_Enk_stofnavn_3","v":""},null,null,{"$f":"D_Enk_stofnavn_4","v":""}]
[null,null,"Beregnede koncentrationer for den valgte model"]
[null,null,"C(z), stationær porevandkoncentration","Cz","mg/l",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"},null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_vert_AC,IF(ISNUMBER(B_ver_Cz_AC_1),B_ver_Cz_AC_1,\"\"),IF(D_vert_DTU_1b,IF(ISNUMBER(B_ver_Cz_1b_1),B_ver_Cz_1b_1,\"\"),IF(ISNUMBER(D_Ver_C0_1),\"Ikke stationær\",\"\"))))","v":false},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_vert_AC,IF(ISNUMBER(B_Ver_CZ_AC_2),B_Ver_CZ_AC_2,\"\"),IF(D_vert_DTU_1b,IF(ISNUMBER(B_ver_Cz_1b_2),B_ver_Cz_1b_2,\"\"),IF(ISNUMBER(D_Ver_C0_2),\"Ikke stationær\",\"\"))))","v":false},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_vert_AC,IF(ISNUMBER(B_Ver_Cz_AC_3),B_Ver_Cz_AC_3,\"\"),IF(D_vert_DTU_1b,IF(ISNUMBER(B_ver_Cz_1b_3),B_ver_Cz_1b_3,\"\"),IF(ISNUMBER(D_Ver_C0_3),\"Ikke stationær\",\"\"))))","v":false},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_vert_AC,IF(ISNUMBER(B_ver_Cz_AC_4),B_ver_Cz_AC_4,\"\"),IF(D_vert_DTU_1b,IF(ISNUMBER(B_ver_Cz_1b_4),B_ver_Cz_1b_4,\"\"),IF(ISNUMBER(D_Ver_C0_4),\"Ikke stationær\",\"\"))))","v":false},"B_Ver_cz_n"]
[null,null,"C(z,t), transient porevandkoncentration","Czt","mg/l",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"},null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(D_vert_AC,B_Ver_Czt_AC_1,B_ver_Czt_DTU_1),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(D_vert_AC,B_Ver_Czt_AC_2,B_ver_Czt_DTU_2),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(D_vert_AC,B_Ver_Czt_AC_3,B_ver_Czt_DTU_3),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(D_vert_AC,B_Ver_Czt_AC_4,B_ver_Czt_DTU_4),\"\")","v":""},"B_Ver_czt_n"]
[null,null,"Flux for stationær porevandkonc",null,"g/år",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"},null,null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(ISNUMBER(B_Ver_Cz_1),B_Ver_Cz_1*D_Ver_Y*D_Ver_X*B_Ver_infiltration*365,IF(ISTEXT(B_Ver_Cz_1),B_Ver_Cz_1,\"\")))","v":false},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(ISNUMBER(B_Ver_Cz_2),B_Ver_Cz_2*D_Ver_Y*D_Ver_X*B_Ver_infiltration*365,IF(ISTEXT(B_Ver_Cz_2),B_Ver_Cz_2,\"\")))","v":false},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(ISNUMBER(B_Ver_Cz_3),B_Ver_Cz_3*D_Ver_Y*D_Ver_X*B_Ver_infiltration*365,IF(ISTEXT(B_Ver_Cz_3),B_Ver_Cz_3,\"\")))","v":false},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(ISNUMBER(B_Ver_Cz_4),B_Ver_Cz_4*D_Ver_Y*D_Ver_X*B_Ver_infiltration*365,IF(ISTEXT(B_Ver_Cz_4),B_Ver_Cz_4,\"\")))","v":false},"B_Ver_Flux_n"]
[null,null,"Overskridelse af GV-krit for stationær porevandkonc.",null,"gange",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"},null,null,null,{"$f":"IF(D_Enk_GV_Krit_1=\"\",\"Intet kriterie\",IF(ISNUMBER(B_Ver_Cz_1),IF(B_Ver_Cz_1>D_Enk_GV_Krit_1,B_Ver_Cz_1/D_Enk_GV_Krit_1,\"nej\"),\"\"))","v":"Intet kriterie"},null,null,{"$f":"IF(D_enk_GV_Krit_2=\"\",\"Intet kriterie\",IF(ISNUMBER(B_Ver_Cz_2),IF(B_Ver_Cz_2>D_enk_GV_Krit_2,B_Ver_Cz_2/D_enk_GV_Krit_2,\"nej\"),\"\"))","v":"Intet kriterie"},null,null,{"$f":"IF(D_Enk_GV_Krit_3=\"\", \"Intet kriterie\",IF(ISNUMBER(B_Ver_Cz_3),IF(B_Ver_Cz_3>D_Enk_GV_Krit_3,B_Ver_Cz_3/D_Enk_GV_Krit_3,\"nej\"),\"\"))","v":"Intet kriterie"},null,null,{"$f":"IF(D_Enk_GV_Krit_4=\"\",\"Intet kriterie\",IF(ISNUMBER(B_Ver_Cz_4),IF(B_Ver_Cz_4>D_Enk_GV_Krit_4,B_Ver_Cz_4/D_Enk_GV_Krit_4,\"nej\"),\"\"))","v":"Intet kriterie"},"B_Ver_GVKKover_n"]
[]
[]
[]
[null,"Vertikal transport (MODEL A+C, FINAL DOMENICO)"]
[]
[null,null,"Lokalitetsspecifikke data/umættet zone"]
[null,"Bemærkninger",null,"Forkortelse","Enhed","Oprindelsessted","Note","Default/Beregnet","Indtastet","Anvendt"]
[null,null,"Jordtype",null,null,null,null,{"$f":"Ver_jord","v":0},{"$f":"Ver_My_jord","v":0},{"$f":"IF(ISTEXT(I19),I19,H19)","v":0},"B_Ver_jord"]
[null,null,"Porevandshastighed","Vw","m/dag","beregnes",null,{"$f":"D_Ver_infiltration/(D_Ver_thetaw)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I20),I20,IF(H20<>0,H20,\"\"))","v":{"$error":"#VALUE!"}},"B_Ver_Vw"]
[null,null,"Nettoinfiltration= nettonedbør","N","m/dag","Beregnes",null,{"$f":"(D_Ver_infiltration_Temp)/(1000*365)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I21),I21,IF(H21<>0,H21,\"\"))","v":{"$error":"#VALUE!"}},"B_Ver_infiltration"]
[null,null,"Long. dispersivitet (vand)","(alfa)L,w","m","Beregnes",null,{"$f":"(0.0000042*(POWER(D_Ver_Z,2))+(0.0036*D_Ver_Z)-0.008)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(H22<0,1E-36,H22)","v":{"$error":"#VALUE!"}},"B_Ver_alfaLw"]
[null,null,"Trans. dispersivitet (vand)","(alfa)T,w","m","beregnes",null,null,null,{"$f":"B_Ver_alfaLw*0.1","v":{"$error":"#VALUE!"}},"B_Ver_alfaTw"]
[null,null,"Transient løsning, tid","t","dage","beregnes",null,null,null,{"$f":"Ver_t*365","v":0},"B_Ver_t"]
[]
[null,null,"Stoffer",null,null,null,null,"Stof 1",null,null,"stof 2",null,null,"stof 3",null,null,"stof 4",null,null,"JAGG navn"]
[null,null,null,"Forkortelse","Enhed","Oprindelsessted","Note","Default/Ber./overført","Indtastet","Anvendt","Default/Beregnet","Indtastet","Anvendt","Default/Beregnet","Indtastet","Anvendt","Default/Beregnet","Indtastet","Anvendt"]
[null,null,"Forureningskomponent","stofnavn_n","-","input","stofafhængig",{"$f":"D_Enk_stofnavn_1","v":""},null,{"$f":"IF(ISTEXT(I28),I28,IF(H28<>0,H28,\"\"))","v":""},{"$f":"D_Enk_stofnavn_2","v":""},null,{"$f":"IF(ISTEXT(L28),L28,IF(K28<>0,K28,\"\"))","v":""},{"$f":"D_Enk_stofnavn_3","v":""},null,{"$f":"IF(ISTEXT(O28),O28,IF(N28<>0,N28,\"\"))","v":""},{"$f":"D_Enk_stofnavn_4","v":""},null,{"$f":"IF(ISTEXT(R28),R28,IF(Q28<>0,Q28,\"\"))","v":""},"B_Ver_stofnavn_n"]
[null,null,"Grundvandskriteriet",null,"mg/l",null,null,null,null,{"$f":"D_Enk_GV_Krit_1","v":""},null,null,{"$f":"D_enk_GV_Krit_2","v":""},null,null,{"$f":"D_Enk_GV_Krit_3","v":""},null,null,{"$f":"D_Enk_GV_Krit_4","v":""}]
[null,null,"Anvendt nedbrydningskonstant","(lambda)_n","dag^-1","Beregnes","stofafhængig",null,null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",(IF(D_Ver_aerobeforhold=TRUE,D_Ver_lambda_aerobe_1,D_Ver_lambda_anaerobe_1)),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",(IF(D_Ver_aerobeforhold=TRUE,D_Ver_lambda_aerobe_2,D_Ver_lambda_anaerobe_2)),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",(IF(D_Ver_aerobeforhold=TRUE,D_Ver_lambda_aerobe_3,D_Ver_lambda_anaerobe_3)),\"\")","v":""},null,null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",(IF(D_Ver_aerobeforhold=TRUE,D_Ver_lambda_aerobe_4,D_Ver_lambda_anaerobe_4)),\"\")","v":""},"B_Ver_lambda_n"]
[null,null,"Diffusionskoefficient (luft)","Dd,a_n","m2/dag","Beregnes","stofafhængig",{"$f":"D_Ver_DL_Temp_1*(24*60*60)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I31),I31,IF(H31<>0,H31,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_DL_Temp_2*(24*60*60)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L31),L31,IF(K31<>0,K31,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_DL_Temp_3*(24*60*60)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O31),O31,IF(N31<>0,N31,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_DL_Temp_4*(24*60*60)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(R31),R31,IF(Q31<>0,Q31,\"\"))","v":{"$error":"#VALUE!"}},"B_Ver_DL_n"]
[null,null,"Effektiv diffusionskoefficient (luft)","D*a_n","m2/dag","Beregnes","stofafhængig",{"$f":"D_Ver_DL_1*D_Ver_thetaa^2.5/D_Ver_ntotal","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I32),I32,IF(H32<>0,H32,0))","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_DL_2*D_Ver_thetaa^2.5/D_Ver_ntotal","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(L32),L32,IF(K32<>0,K32,0))","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_DL_3*D_Ver_thetaa^2.5/D_Ver_ntotal","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(O32),O32,IF(N32<>0,N32,0))","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_DL_4*D_Ver_thetaa^2.5/D_Ver_ntotal","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(R32),R32,IF(Q32<>0,Q32,0))","v":{"$error":"#VALUE!"}},"B_Ver_Da_n"]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(VALUE(I33),I33,IF(H33<>0,H33,\"\"))","v":""},null,null,{"$f":"IF(VALUE(L33),L33,IF(K33<>0,K33,\"\"))","v":""},null,null,{"$f":"IF(VALUE(O33),O33,IF(N33<>0,N33,\"\"))","v":""},null,null,{"$f":"IF(VALUE(R33),R33,IF(Q33<>0,Q33,\"\"))","v":""}]
[null,null,"Vanddata",null,null,null,null,"Vanddata",null,null,"Vanddata",null,null,"Vanddata",null,null,"Vanddata"]
[null,null,"Hydrodynamisk long. disp (vand)","Dz","m2/dag","beregnes","stofafhængig",{"$f":"(D_Ver_Vw*D_Ver_alfaLw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_1*D_Ver_KH_1+D_ver_Dw_1*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_Vw*D_Ver_alfaLw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_2*D_Ver_KH_2+D_Ver_Dw_2*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_Vw*D_Ver_alfaLw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_3*D_Ver_KH_3+D_Ver_Dw_3*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_Vw*D_Ver_alfaLw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_4*D_Ver_KH_4+D_Ver_Dw_4*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_Dz_n"]
[null,null,"Hydrodynamisk trans. disp (vand)","Dy, Dx","m2/dag","beregnes","stofafhængig",{"$f":"(D_Ver_Vw*D_Ver_alfaTw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_1*D_Ver_KH_1+D_ver_Dw_1*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_Vw*D_Ver_alfaTw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_2*D_Ver_KH_2+D_Ver_Dw_2*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_Vw*D_Ver_alfaTw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_3*D_Ver_KH_3+D_Ver_Dw_3*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_Vw*D_Ver_alfaTw*D_Ver_thetaw+D_Ver_thetaa*D_Ver_Da_4*D_Ver_KH_4+D_Ver_Dw_4*D_Ver_thetaw)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_DyDx_n"]
[null,null,"Retardationsfaktor","R","-","beregnes","stofafhængig",{"$f":"IF(D_Enk_stofnavn_1<>\"\",(1+D_Ver_KOC_1*D_Ver_foc*D_Ver_rhob/D_Ver_thetaw),\"\")","v":""},null,"",{"$f":"IF(D_Enk_stofnavn_2<>\"\",(1+D_Ver_KOC_2*D_Ver_foc*D_Ver_rhob/D_Ver_thetaw),\"\")","v":""},null,"",{"$f":"IF(D_Enk_stofnavn_3<>\"\",(1+D_Ver_KOC_3*D_Ver_foc*D_Ver_rhob/D_Ver_thetaw),\"\")","v":""},null,"",{"$f":"IF(D_Enk_stofnavn_4<>\"\",(1+D_Ver_KOC_4*D_Ver_foc*D_Ver_rhob/D_Ver_thetaw),\"\")","v":""},null,"","B_Ver_R_n"]
[null,null,"Diffusionskoefficient (vand)","D*w","m2/dage","Beregnes","stofafhængig",{"$f":"D_ver_Ddw_temp_1*(60*60*24)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I38),I38,IF(H38<>0,H38,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"D_ver_Ddw_temp_2*(60*60*24)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Ddw_temp_3*(60*60*24)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Ddw_temp_4*(60*60*24)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"}]
[null,null,"Effektiv diffusionskoefficient (vand)","D*w","m2/dag","beregnes","stofafhængig",{"$f":"1.1*D_Ver_thetaw*(D_Ver_thetaw-0.039*0.00312^0.52)*B_ver_Ddw_1","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1.1*D_Ver_thetaw*(D_Ver_thetaw-0.039*0.00312^0.52)*B_ver_ddw_2","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1.1*D_Ver_thetaw*(D_Ver_thetaw-0.039*0.00312^0.52)*B_ver_Ddw_3","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"1.1*D_Ver_thetaw*(D_Ver_thetaw-0.039*0.00312^0.52)*B_ver_Ddw_4","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_Dw_n"]
[null,null,null,null,null,null,null,null,null,"",null,null,"",null,null,"",null,null,""]
[null,null,null,null,null,null,null,null,null,"",null,null,"",null,null,"",null,null,""]
[null,null,"Hjælpekonstanter",null,null,null,null,"Hjælpekonstanter",null,null,"Hjælpekonstanter",null,null,"Hjælpekonstanter",null,null,"Hjælpekonstanter"]
[null,null,"u","u","m/dag","beregnes","stofafhængig",{"$f":"D_Ver_Vw*SQRT(1+4*D_Ver_lambda_1*D_Ver_Dz_1/D_Ver_Vw^2)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Vw*SQRT(1+4*D_Ver_lambda_2*D_Ver_Dz_2/D_Ver_Vw^2)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Vw*SQRT(1+4*D_Ver_lambda_3*D_Ver_Dz_3/D_Ver_Vw^2)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Vw*SQRT(1+4*D_Ver_lambda_4*D_Ver_Dz_4/D_Ver_Vw^2)","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_u_n"]
[null,null,"Arg1","Arg1","-","beregnes","stofafhængig",{"$f":"(D_Ver_Vw-D_Ver_u_1)/(2*D_Ver_Dz_1)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(H44),H44,\"\")","v":""},{"$f":"(D_Ver_Vw-D_Ver_u_2)/(2*D_Ver_Dz_2)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(K44),K44,\"\")","v":""},{"$f":"(D_Ver_Vw-D_Ver_u_3)/(2*D_Ver_Dz_3)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(N44),N44,\"\")","v":""},{"$f":"(D_Ver_Vw-D_Ver_u_4)/(2*D_Ver_Dz_4)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(ISNUMBER(Q44),Q44,\"\")","v":""},"B_Ver_Arg1_n"]
[null,null,"ArgX","ArgX","-","beregnes","stofafhængig",{"$f":"D_Ver_X/(4*SQRT(D_Ver_DyDx_1/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_X/(4*SQRT(D_Ver_DyDx_2/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_X/(4*SQRT(D_Ver_DyDx_3/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_X/(4*SQRT(D_Ver_DyDx_4/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_ArgX_n"]
[null,null,"ArgY","ArgY","-","beregnes","stofafhængig",{"$f":"D_Ver_Y/(4*SQRT(D_Ver_DyDx_1/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Y/(4*SQRT(D_Ver_DyDx_2/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Y/(4*SQRT(D_Ver_DyDx_3/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"D_Ver_Y/(4*SQRT(D_Ver_DyDx_4/D_Ver_Vw))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_ArgY_n"]
[null,null,"ArgZ (Rqw+KHqa)","Rqw+KHqa ","-","beregnes","stofafhængig",{"$f":"(D_Ver_R_1*D_Ver_thetaw+D_Ver_thetaa*D_Ver_KH_1)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_R_2*D_Ver_thetaw+D_Ver_thetaa*D_Ver_KH_2)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_R_3*D_Ver_thetaw+D_Ver_thetaa*D_Ver_KH_3)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$f":"(D_Ver_R_4*D_Ver_thetaw+D_Ver_thetaa*D_Ver_KH_4)/D_Ver_thetaw","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},"B_Ver_ArgZ_n"]
[]
[]
[null,null,"Beregnede koncentrationer"]
[null,null,"C(z), stationær porevandkoncentration","Cz","mg/l",null,null,null,null,{"$f":"B_ver_Cz_AC_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"B_Ver_CZ_AC_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"B_Ver_Cz_AC_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"B_ver_Cz_AC_4","v":{"$error":"#VALUE!"}},"B_Ver_cz_AC_n"]
[null,null,"C(z,t), transient porevandkoncentration","Czt","mg/l",null,null,null,null,{"$f":"B_Ver_Czt_AC_1","v":{"$error":"#VALUE!"}},null,null,{"$f":"B_Ver_Czt_AC_2","v":{"$error":"#VALUE!"}},null,null,{"$f":"B_Ver_Czt_AC_3","v":{"$error":"#VALUE!"}},null,null,{"$f":"B_Ver_Czt_AC_4","v":{"$error":"#VALUE!"}},"B_Ver_czt_AC_n"]
[]
[null,"STOF 1","Domenico - 1D (1987)","t =",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STOF 2","Domenico - 1D (1987)","t="]
[null,null,null,{"$f":"Ver_t","v":0},1,5,10,20,30,50,null,null,null,null,null,null,null,null,null,null,{"$f":"Ver_t","v":0},1,5,10,20,30,50]
[null,null,null,"år","år","år","år","år","år","år",null,null,null,null,null,null,null,null,null,null,"år","år","år","år","år","år","år"]
[null,"Vertical distance from source","Concentration 1D (centerline)","t (dage)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vertical distance from source","Concentration 1D (centerline)","t (dage)"]
[null,"[m]","Stationær",{"$f":"B_Ver_t","v":0},{"$f":"E55*365","v":365},1825,3650,7300,10950,18250,null,null,null,null,null,null,null,null,"[m]","Stationær",{"$f":"B_Ver_t","v":0},{"$f":"V55*365","v":365},1825,3650,7300,10950,18250]
[null,0,{"$f":"IF(D_vert_AC,D_Ver_C0_1*EXP((D_Ver_Vw-D_Ver_u_1)*B59/(2*D_Ver_Dz_1)),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B59/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B59*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,0,{"$f":"IF(D_vert_AC,D_Ver_C0_2*EXP((D_Ver_Vw-D_Ver_u_2)*S59/(2*D_Ver_Dz_2)),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S59/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S59*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"B61-D_Ver_Z/40","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B60/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B60*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"S61-D_Ver_Z/40","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S60/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S60*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B61/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B61*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S61/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S61*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B62/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B62*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S62/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S62*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B63/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B63*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S63/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S63*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B64/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B64*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S64/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S64*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B65/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B65*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S65/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S65*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B66/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B66*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S66/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S66*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B67/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B67*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S67/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S67*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B68/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B68*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S68/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S68*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B69/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B69*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S69/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S69*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B70/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B70*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S70/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S70*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B71/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B71*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S71/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S71*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B72/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B72*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S72/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S72*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B73/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B73*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S73/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S73*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B74/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B74*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S74/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S74*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B75/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B75*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S75/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S75*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B76/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B76*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S76/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S76*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B77/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B77*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S77/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S77*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B78/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B78*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S78/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S78*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B79/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B79*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S79/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S79*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B80/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B80*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S80/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S80*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B81/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B81*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S81/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S81*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B82/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B82*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S82/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S82*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B83/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B83*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S83/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S83*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B84/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B84*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S84/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S84*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B85/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B85*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S85/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S85*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B86/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B86*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S86/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S86*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B87/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B87*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S87/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S87*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B88/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B88*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S88/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S88*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B89/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B89*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S89/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S89*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B90/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B90*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S90/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S90*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B91/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B91*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S91/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S91*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B92/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B92*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S92/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S92*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B93/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B93*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S93/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S93*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B94/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B94*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S94/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S94*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B95/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B95*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S95/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S95*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B96/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B96*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S96/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S96*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B97/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B97*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S97/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S97*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B98/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B98*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S98/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S98*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"D_Ver_Z","v":""},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B99/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B99*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"D_Ver_Z","v":""},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S99/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S99*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,5,{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*D$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*D$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*E$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*E$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*F$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*F$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*G$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*G$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*H$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*H$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*I$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*I$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_1/2*(EXP((D_Ver_Vw-D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1-D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))>709,709,((D_Ver_Vw+D_Ver_u_1)*$B100/(2*D_Ver_Dz_1))))*(1-fejlfunkk(($B100*D_Ver_ArgZ_1+D_Ver_u_1*J$58)/(2*SQRT(D_Ver_Dz_1*D_Ver_ArgZ_1*J$58))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,5,{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*U$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*V$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*W$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*X$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*Y$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*Z$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_2/2*(EXP((D_Ver_Vw-D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2-D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))>709,709,((D_Ver_Vw+D_Ver_u_2)*$S100/(2*D_Ver_Dz_2))))*(1-fejlfunkk(($S100*D_Ver_ArgZ_2+D_Ver_u_2*AA$58)/(2*SQRT(D_Ver_Dz_2*D_Ver_ArgZ_2*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[]
[]
[null,"STOF 3","Domenico - 1D (1987)","t=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STOF 4","Domenico - 1D (1987)","t="]
[null,null,null,{"$f":"Ver_t","v":0},1,5,10,20,30,50,null,null,null,null,null,null,null,null,null,null,{"$f":"Ver_t","v":0},1,5,10,20,30,50]
[null,null,null,"år","år","år","år","år","år","år",null,null,null,null,null,null,null,null,null,null,"år","år","år","år","år","år","år"]
[null,"Vertical distance from source","Concentration 1D (centerline)","t (dage)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vertical distance from source","Concentration 1D (centerline)","t (dage)"]
[null,"[m]","Stationær",{"$f":"B_Ver_t","v":0},{"$f":"E104*365","v":365},1825,3650,7300,10950,18250,null,null,null,null,null,null,null,null,"[m]","Stationær",{"$f":"B_Ver_t","v":0},{"$f":"V104*365","v":365},1825,3650,7300,10950,18250]
[null,0,{"$f":"IF(D_vert_AC,D_Ver_C0_3*EXP((D_Ver_Vw-D_Ver_u_3)*B108/(2*D_Ver_Dz_3)),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B108/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B108*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,0,{"$f":"IF(D_vert_AC,D_Ver_C0_4*EXP((D_Ver_Vw-D_Ver_u_4)*S108/(2*D_Ver_Dz_4)),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S108/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S108*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"B110-D_Ver_Z/40","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B109/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B109*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"S110-D_Ver_Z/40","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S109/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S109*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B110/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B110*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S110/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S110*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B111/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B111*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S111/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S111*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B112/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B112*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S112/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S112*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B113/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B113*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S113/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S113*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B114/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B114*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S114/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S114*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B115/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B115*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S115/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S115*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B116/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B116*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S116/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S116*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B117/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B117*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S117/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S117*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B118/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B118*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S118/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S118*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B119/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B119*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S119/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S119*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B120/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B120*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S120/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S120*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B121/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B121*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S121/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S121*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B122/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B122*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S122/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S122*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B123/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B123*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S123/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S123*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B124/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B124*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S124/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S124*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B125/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B125*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S125/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S125*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B126/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B126*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S126/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S126*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B127/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B127*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S127/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S127*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B128/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B128*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S128/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S128*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B129/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B129*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S129/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S129*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B130/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B130*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S130/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S130*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B131/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B131*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S131/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S131*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B132/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B132*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S132/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S132*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B133/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B133*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S133/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S133*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B134/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B134*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S134/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S134*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B135/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B135*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S135/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S135*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B136/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B136*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S136/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S136*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B137/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B137*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S137/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S137*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B138/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B138*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S138/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S138*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B139/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B139*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S139/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S139*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B140/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B140*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S140/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S140*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B141/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B141*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S141/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S141*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B142/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B142*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S142/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S142*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B143/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B143*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S143/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S143*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B144/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B144*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S144/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S144*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B145/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B145*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S145/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S145*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B146/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B146*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S146/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S146*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B147/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B147*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S147/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S147*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,{"$f":"D_Ver_Z","v":""},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B148/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B148*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,{"$f":"D_Ver_Z","v":""},{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S148/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S148*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[null,5,{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*D$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*D$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*E$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*E$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*F$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*F$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*G$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*G$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*H$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*H$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*I$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*I$107))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_3/2*(EXP((D_Ver_Vw-D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3-D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))+EXP(IF(((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))>709,709,((D_Ver_Vw+D_Ver_u_3)*$B149/(2*D_Ver_Dz_3))))*(1-fejlfunkk(($B149*D_Ver_ArgZ_3+D_Ver_u_3*J$107)/(2*SQRT(D_Ver_Dz_3*D_Ver_ArgZ_3*J$107))))),0)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,5,{"$error":"#VALUE!"},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*U$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*U$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*V$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*V$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*W$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*W$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*X$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*X$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*Y$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Y$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*Z$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*Z$58))))),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_vert_AC,D_Ver_C0_4/2*(EXP((D_Ver_Vw-D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4-D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))+EXP(IF(((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))>709,709,((D_Ver_Vw+D_Ver_u_4)*$S149/(2*D_Ver_Dz_4))))*(1-fejlfunkk(($S149*D_Ver_ArgZ_4+D_Ver_u_4*AA$58)/(2*SQRT(D_Ver_Dz_4*D_Ver_ArgZ_4*AA$58))))),0)","v":{"$error":"#VALUE!"}}]
[]
[]
[null,null,"SprækkeTransport - DTU-V1D-remtec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JAGG navn","Oprindelse"]
[]
[]
[null,null,"DTU Model 1a og 1b og C"]
[]
[null,null,"Presence of fractures",null,"yes"]
[null,null,{"$f":"IF(E157=\"yes\",\"\",\"Advection in low-permeability media (yes/no)\")","v":""}]
[null,null,"If initially contaminated (yes/no)",null,{"$f":"IF(D_vert_DTU_2,\"yes\",\"no\")","v":"no"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_vert_DTU_2","imput","true or false"]
[]
[]
[]
[null,null,"INPUT"]
[null,null,"BOX 1: General Input",null,null,null,null,null,"stof 1","Stof 2","Stof 3","Stof 4"]
[null,null,null,null,null,null,null,null,{"$f":"D_Ver_stofnavn_1","v":""},{"$f":"D_Ver_stofnavn_2","v":""},{"$f":"D_Ver_stofnavn_3","v":""},{"$f":"D_Ver_stofnavn_4","v":""}]
[null,null,"Input concentration","C0 (mg/l)",null,null,null,null,{"$f":"D_Ver_C0_1","v":""},{"$f":"D_Ver_C0_2","v":""},{"$f":"D_Ver_C0_3","v":""},{"$f":"D_Ver_C0_4","v":""},null,null,null,null,null,null,null,"D_Ver_C0_x","Overført fra enkeltstoffer eller Vertical transport "]
[null,null,"Matrix porosity","f",{"$f":"D_Ver_ntotal","v":""},{"$f":"D_Ver_jord","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_ntotal  ","input  fra jordparametre og defineret i datark"]
[null,null,"Diffusion coefficient in matrix","Dm (m2/year)",null,null,null,null,{"$f":"D_ver_Ddw_temp_1*D_Ver_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_ver_Ddw_temp_2*D_Ver_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_Ddw_temp_3*D_Ver_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_Ddw_temp_4*D_Ver_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"B_Ver_Ddwm_x","Beregnes"]
[null,null,"Degradation rate","l (dag-1)",null,{"$f":"IF(D_Ver_an,\"aerobe\",\"anaerobe\")","v":"aerobe"},null,null,{"$f":"D_Ver_lambda_1","v":""},{"$f":"D_Ver_lambda_2","v":""},{"$f":"D_Ver_lambda_3","v":""},{"$f":"D_Ver_lambda_4","v":""},null,null,null,null,null,null,null,"D_Ver_lambda_x","input fra enkeltstoffer"]
[null,null,"Degradation rate","l (year-1)",null,{"$f":"IF(D_Ver_an,\"aerobe\",\"anaerobe\")","v":"aerobe"},null,null,{"$f":"D_Ver_lambda_1*365","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_lambda_2*365","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_lambda_3*365","v":{"$error":"#VALUE!"}},{"$f":"D_Ver_lambda_4*365","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"B_Ver_lambdayear_x","enhederne omregnes"]
[null,null,"Retardation, fracture","Rf",null,"lige med Rm","jf. Chambon et al.J. of contaminant Hydrology 124 (2011),82-98",null,{"$f":"D_Ver_R_1","v":""},{"$f":"D_Ver_R_2","v":""},{"$f":"D_Ver_R_3","v":""},{"$f":"D_Ver_R_4","v":""},null,null,null,null,null,null,null,"D_Ver_R_x","B_Ver_R beregnes ovenover i Domenico"]
[null,null,"Retardation, matrix","Rm",null,"stof afhængig beregnes",null,null,{"$f":"D_Ver_R_1","v":""},{"$f":"D_Ver_R_2","v":""},{"$f":"D_Ver_R_3","v":""},{"$f":"D_Ver_R_4","v":""},null,null,null,null,null,null,null,"D_Ver_R_x","B_Ver_R beregnes ovenover i Domenico"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_ver_2bapertur","v":{"$error":"#VALUE!"}}]
[null,null,"Water velocity","vf (m/year)",{"$f":"D_ver_2bapertur^2*1000*9.81/(12*0.0013)*D_Ver_Vgrad*3600*24*365","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_Vvel","Beregnes"]
[null,null,"Average velocity in EPM","vEPM (m/year)",{"$f":"D_ver_Kb*D_Ver_Vgrad*3600*24*365/D_Ver_ntotal","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_ver_EPM","Beregnes"]
[null,null,"Longitudinal dispersivity","α (m)",{"$f":"D_Ver_alfaLw","v":6.5679999999999988E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Ver_alfaLw","input"]
[null,null,"Spill time","a (year)",{"$f":"IF(Ver_a>0,Ver_a,\"constant\")","v":"constant"}]
[]
[null,null,"BOX 2: Hydrogeological properties"]
[null,null,"calculated using from Box 3"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_ver_2B","v":""}]
[null,null,"Fracture aperture","2*b (m)",{"$f":"(D_ver_Kb*12*0.0013*D_ver_2B/(1000*9.81))^(1/3)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_ver_2bapertur","Beregnes"]
[null,null,"Bulk hydrualic conductivity","Kb (m/s)",{"$f":"D_ver_Kb","v":""}]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_Ver_infil","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_inf","input"]
[null,null,"Vertical gradient","i (-)",{"$f":"D_Ver_infil/1000/3600/24/365/D_ver_Kb","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_ver_Vgrad","Beregnes"]
[]
[null,null,"BOX 3: Specific Input depending on conceptual model",null,null,"Default/Ber./overført","Indtastet","Anvendt"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_ver_2B","v":""},{"$f":"Ver_2B","v":5},{"$f":"Ver_My_2B","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(G188),G188,IF(F188<>0,F188,\"\")),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,"D_ver_2B","input"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_ver_2bapertur","v":{"$error":"#VALUE!"}}]
[null,null,"Bulk hydraulic conductivity","Kb (m/s)",{"$f":"D_ver_Kb","v":""},{"$f":"Ver_Kb","v":6.2999999999999995E-8},{"$f":"Ver_My_Kb","v":0},{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(VALUE(G190),G190,IF(F190<>0,F190,\"\")),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,"D_ver_Kb","Input"]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_Ver_infiltration_Temp","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_ver_infil","Input se oven D_Ver_infiltration_Temp"]
[null,null,"Vertical gradient","i (-)",{"$f":"D_Ver_Vgrad","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,"stof 1","Stof 2","Stof 3","Stof 4"]
[null,null,"BOX 4: Calculated Parameters-",null,null,null,null,null,{"$f":"D_Ver_stofnavn_1","v":""},{"$f":"D_Ver_stofnavn_2","v":""},{"$f":"D_Ver_stofnavn_3","v":""},{"$f":"D_Ver_stofnavn_4","v":""}]
[null,null,"A",null,null,null,null,null,{"$f":"D_ver_2bapertur/2*D_Ver_R_1/(D_Ver_ntotal*SQRT(D_Ver_R_1*D_ver_Ddwm_1))","v":{"$error":"#VALUE!"}},{"$f":"D_ver_2bapertur/2*D_Ver_R_2/(D_Ver_ntotal*SQRT(D_Ver_R_2*D_ver_Ddwm_2))","v":{"$error":"#VALUE!"}},{"$f":"D_ver_2bapertur/2*D_Ver_R_3/(D_Ver_ntotal*SQRT(D_Ver_R_3*D_ver_Ddwm_3))","v":{"$error":"#VALUE!"}},{"$f":"D_ver_2bapertur/2*D_Ver_R_4/(D_Ver_ntotal*SQRT(D_Ver_R_4*D_ver_Ddwm_4))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"B_ver_A_X","Beregnes"]
[null,null,"B ",null,null,null,null,null,{"$f":"SQRT(D_Ver_lambdayear_1/D_Ver_R_1)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_Ver_lambdayear_2/D_Ver_R_2)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_Ver_lambdayear_3/D_Ver_R_3)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_Ver_lambdayear_4/D_Ver_R_4)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"B_ver_B_X","Beregnes"]
[null,null,"G",null,null,null,null,null,{"$f":"SQRT(D_Ver_R_1/D_ver_Ddwm_1)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_Ver_R_2/D_ver_Ddwm_2)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_Ver_R_3/D_ver_Ddwm_3)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_Ver_R_4/D_ver_Ddwm_1)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,"B_ver_G_X","Beregnes"]
[]
[null,null,"BOX 5: Calculation and graphic parameters"]
[null,null,"Time increment","(year)",{"$f":"B_ver_timeplot/80","v":0}]
[null,null,"Depth increment","(m)",{"$f":"Ver_z/80","v":0}]
[null,null,"Time plot",null,{"$f":"IF(Ver_t>20,Ver_t,Ver_t*4)","v":0}]
[null,null,"Time","t (year)",{"$f":"Ver_t","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver_t","input"]
[null,null,"Depth","z(m)",{"$f":"Ver_z","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver_z","input"]
[]
[]
[null,null,"Stof 1",{"$f":"D_Ver_stofnavn_1","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",E204,\" m´s dybder\")","v":"Stationær konc. 0 m´s dybder"},null,null,{"$f":"IF(D_vert_DTU_1b,B_Ver_Cz_DTU_1,\"(ikke stationært)\")","v":"(ikke stationært)"},"mg/l",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Koncentration i matrix i forskellige afstande (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken i  m´s dybde"},null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_1,\": Koncentration i matrix i forskellige afstande (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kun DTU V1D-Model 2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Stationær konc.med tid i \",Ver_z,\" m´s dybde - Kun model 1b\")","v":"Stationær konc.med tid i  m´s dybde - Kun model 1b"},{"$f":"CONCATENATE(\"Stationær konc.i dybde ved tid \",Ver_t,\" år_ kun model 1b\")","v":"Stationær konc.i dybde ved tid  år_ kun model 1b"},null,null,null,null,null,null,null,null,"En aftagnende kilde"]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"IF(D_vert_DTU_2,(D_Ver_R_1*(D_ver_2B/2)^2)/D_ver_Ddwm_1,\"\")","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,"Sprækkemodel",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM model",null,null,null,"Diffusionsmodel",null,null,"1. ordens model"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in fracture with time at depth \",Ver_z,\" m\")","v":"Conc in fracture with time at depth  m"},{"$f":"CONCATENATE(\"Conc in fracture with depth at time \",Ver_t,\" years\")","v":"Conc in fracture with depth at time  years"},"Original Conc in fracture at depth and time",{"$f":"CONCATENATE(\"Conc in matrix with time at \",Ver_z, \" m depth at different distances x m from the fracture\")","v":"Conc in matrix with time at  m depth at different distances x m from the fracture"},null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in matrix with depth at \",Ver_t, \" years at different distances x m from the fracture\")","v":"Conc in matrix with depth at  years at different distances x m from the fracture"},null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EPM with time at depth \",Ver_z,\" m\")","v":"EPM with time at depth  m"},{"$f":"CONCATENATE(\"EPM in depth at time \",Ver_t,\" years\")","v":"EPM in depth at time  years"},null,"No fracture",{"$f":"CONCATENATE(\"Diffusion with time at depth \",Ver_z,\" m\")","v":"Diffusion with time at depth  m"},{"$f":"CONCATENATE(\"Diffusion in depth at time \",Ver_t,\" years\")","v":"Diffusion in depth at time  years"},{"$f":"CONCATENATE(\"1.order with time at depth \",Ver_z,\" m\")","v":"1.order with time at depth  m"},{"$f":"CONCATENATE(\"1.order in depth at time \",Ver_t,\" years\")","v":"1.order in depth at time  years"}]
[null,null,"z (depth)","t (time)","T'","T''",null,null,null,0.1,0.2,0.3,0.4,0.5,0.75,1,0.1,0.2,0.3,0.4,0.5,0.75,1,"Stationær konc.","Stationær konc.","u1",null,null,null,"u2","No advection"]
[null,null,{"$f":"Ver_z","v":0},{"$f":"Ver_t","v":0},{"$f":"IF((SQRT(D239-D_Ver_R_1/D_Ver_Vvel*$C239))>0,SQRT(D239-D_Ver_R_1/D_Ver_Vvel*$C239),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D239-(D_Ver_R_1/D_Ver_Vvel*$C239+D_ver_a)>0,SQRT(D239-(D_Ver_R_1/D_Ver_Vvel*$C239+D_ver_a)),0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E239)*SQRT(2))))),(IF(AND($E239>0,$F239=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E239)+D_ver_B_1*$E239)*SQRT(2)))*D_Ver_C0_1,IF($F239>0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E239)+D_ver_B_1*$E239)*SQRT(2)))-(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F239)-D_ver_B_1*$F239)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F239)+D_ver_B_1*$F239)*SQRT(2))))*D_Ver_C0_1,0)))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E$239)*SQRT(2))))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($F$239>0,0.5*EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP(D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1,0))))","v":0},{"$f":"IF(D_vert_AC,0,IF(AND($E239>0,$F239=0),0.5*EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP(D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E239)+D_ver_B_1*$E239)*SQRT(2)))*D_Ver_C0_1,IF($F239>0,0.5*EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP(D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$E239)+D_ver_B_1*$E239)*SQRT(2)))-(EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$F239)-D_ver_B_1*$F239)*SQRT(2))+EXP(D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/(2*D_ver_A_1*$F239)+D_ver_B_1*$F239)*SQRT(2))))*D_Ver_C0_1,0)))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D239/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E239)*SQRT(2)))),IF(AND($E239>0,$F239=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E239)+D_ver_B_1*$E239)*SQRT(2)))*D_Ver_C0_1,IF($E239=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E239)+D_ver_B_1*$E239)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F239)-D_ver_B_1*$F239)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F239)+D_ver_B_1*$F239)*SQRT(2))))*D_Ver_C0_1))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D239/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E239)*SQRT(2)))),IF(AND($E239>0,$F239=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E239)+D_ver_B_1*$E239)*SQRT(2)))*D_Ver_C0_1,IF($E239=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E239)-D_ver_B_1*$E239)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E239)+D_ver_B_1*$E239)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$F239)-D_ver_B_1*$F239)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$F239)+D_ver_B_1*$F239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C239/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*$C239/D_Ver_Vvel)*EXP(-D_Ver_R_1*$C239/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_1*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1)))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_1),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D239/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z-D_ver_EPM*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*Ver_z+D_ver_EPM*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z239*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))+EXP((D_ver_EPM+$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z239*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))),(IF($D239<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z239*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))+EXP((D_ver_EPM+$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z239*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z239*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))+EXP((D_ver_EPM+$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z239*$D239)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))-EXP((D_ver_EPM-$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z239*($D239-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D239-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z239)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z239*($D239-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D239-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C239-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C239/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*$C239+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$Z239*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$Z239*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$Z239*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$Z239*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$Z239*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$Z239*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$Z239*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z239)*$C239/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$Z239*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1))","v":0},{"$f":"IF( D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_1),0))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D239/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z)/2*SQRT((D_Ver_R_1*$D239))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_1/2*(EXP((-$AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD239*$D239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))+EXP(($AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD239*$D239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D239<=D_ver_a,\nD_Ver_C0_1/2*(EXP((-$AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD239*$D239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))+EXP(($AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD239*$D239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))),\nD_Ver_C0_1/2*(EXP((-$AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD239*$D239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))+EXP(($AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD239*$D239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D239)))*SQRT(2))-EXP((-$AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD239*($D239-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D239-D_ver_a))))*SQRT(2))-EXP(($AD239)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD239*($D239-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D239-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C239)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_1*$C239)/2*SQRT((D_Ver_R_1*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_1/2*(EXP((-$AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$AD239*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$AD239*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_1/2*(EXP((-$AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$AD239*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$AD239*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),\nD_Ver_C0_1/2*(EXP((-$AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$AD239*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$AD239*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((-$AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239-$AD239*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD239)*$C239/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C239+$AD239*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C239)+D_Ver_lambdayear_1)/D_Ver_R_1*$D239)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C239)+D_Ver_lambdayear_1)/D_Ver_R_1*Ver_t)),))","v":0}]
[null,null,0,{"$f":"0","v":0},{"$f":"IF((SQRT(D240-D_Ver_R_1/D_Ver_Vvel*$C240))>0,SQRT(D240-D_Ver_R_1/D_Ver_Vvel*$C240),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D240-(D_Ver_R_1/D_Ver_Vvel*$C240+D_ver_a)>0,SQRT(D240-(D_Ver_R_1/D_Ver_Vvel*$C240+D_ver_a)),0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D240/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E240^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E240)*SQRT(2))))),(IF(AND($E240>0,$F240=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E240)+D_ver_B_1*$E240)*SQRT(2)))*D_Ver_C0_1,IF($F240>0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E240)+D_ver_B_1*$E240)*SQRT(2)))-(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F240)-D_ver_B_1*$F240)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F240)+D_ver_B_1*$F240)*SQRT(2))))*D_Ver_C0_1,0)))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C240/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E$239)*SQRT(2))))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C240/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($F$239>0,0.5*EXP(-D_Ver_lambdayear_1*$C240/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP(D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1,0))))","v":0},{"$f":"IF(D_vert_AC,0,IF(AND($E240>0,$F240=0),0.5*EXP(-D_Ver_lambdayear_1*$C240/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP(D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E240)+D_ver_B_1*$E240)*SQRT(2)))*D_Ver_C0_1,IF($F240>0,0.5*EXP(-D_Ver_lambdayear_1*$C240/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP(D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$E240)+D_ver_B_1*$E240)*SQRT(2)))-(EXP(-D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$F240)-D_ver_B_1*$F240)*SQRT(2))+EXP(D_Ver_R_1*$C240/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C240/D_Ver_Vvel/(2*D_ver_A_1*$F240)+D_ver_B_1*$F240)*SQRT(2))))*D_Ver_C0_1,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D240/D_Ver_R_1))),IF(AND($E240>0,$F240=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E240)+D_ver_B_1*$E240)*SQRT(2)))*D_Ver_C0_1,IF($E240=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E240)+D_ver_B_1*$E240)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F240)-D_ver_B_1*$F240)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F240)+D_ver_B_1*$F240)*SQRT(2))))*D_Ver_C0_1))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D240/D_Ver_R_1))),IF(AND($E240>0,$F240=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E240)+D_ver_B_1*$E240)*SQRT(2)))*D_Ver_C0_1,IF($E240=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E240)-D_ver_B_1*$E240)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$E240)+D_ver_B_1*$E240)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$F240)-D_ver_B_1*$F240)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*K$238)/(2*$F240)+D_ver_B_1*$F240)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_1*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1)))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_1),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z240*$D240)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D240)))*SQRT(2))+EXP((D_ver_EPM+$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z240*$D240)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D240)))*SQRT(2))),(IF($D240<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z240*$D240)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D240)))*SQRT(2))+EXP((D_ver_EPM+$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z240*$D240)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D240)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z240*$D240)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D240)))*SQRT(2))+EXP((D_ver_EPM+$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z240*$D240)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D240)))*SQRT(2))-EXP((D_ver_EPM-$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z240*($D240-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D240-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z240)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z240*($D240-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D240-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240-$Z240*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240+$Z240*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240-$Z240*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240+$Z240*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240-$Z240*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240+$Z240*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240-$Z240*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z240)*$C240/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C240+$Z240*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_1),0))","v":0},0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_1)/D_Ver_R_1*$D240)),))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,IF(C240=0,D_Ver_C0_1,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C240)+D_Ver_lambdayear_1)/D_Ver_R_1*Ver_t))),))","v":0}]
[null,null,{"$f":"0+D_ver_z_incr","v":0},{"$f":"0+D_ver_t_incre","v":0},{"$f":"IF((SQRT(D241-D_Ver_R_1/D_Ver_Vvel*$C241))>0,SQRT(D241-D_Ver_R_1/D_Ver_Vvel*$C241),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D241-(D_Ver_R_1/D_Ver_Vvel*$C241+D_ver_a)>0,SQRT(D241-(D_Ver_R_1/D_Ver_Vvel*$C241+D_ver_a)),0)))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D241/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E241^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E241)*SQRT(2))))),(IF(AND($E241>0,$F241=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E241)-D_ver_B_1*$E241)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E241)+D_ver_B_1*$E241)*SQRT(2)))*D_Ver_C0_1,IF($F241>0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E241)-D_ver_B_1*$E241)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E241)+D_ver_B_1*$E241)*SQRT(2)))-(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F241)-D_ver_B_1*$F241)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F241)+D_ver_B_1*$F241)*SQRT(2))))*D_Ver_C0_1,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E241>0,$F241=0),0.5*EXP(-D_Ver_lambdayear_1*$C241/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C241/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C241/D_Ver_Vvel/(2*D_ver_A_1*$E241)-D_ver_B_1*$E241)*SQRT(2))+EXP(D_Ver_R_1*$C241/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C241/D_Ver_Vvel/(2*D_ver_A_1*$E241)+D_ver_B_1*$E241)*SQRT(2)))*D_Ver_C0_1,IF($F241>0,0.5*EXP(-D_Ver_lambdayear_1*$C241/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C241/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C241/D_Ver_Vvel/(2*D_ver_A_1*$E241)-D_ver_B_1*$E241)*SQRT(2))+EXP(D_Ver_R_1*$C241/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C241/D_Ver_Vvel/(2*D_ver_A_1*$E241)+D_ver_B_1*$E241)*SQRT(2)))-(EXP(-D_Ver_R_1*$C241/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C241/D_Ver_Vvel/(2*D_ver_A_1*$F241)-D_ver_B_1*$F241)*SQRT(2))+EXP(D_Ver_R_1*$C241/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C241/D_Ver_Vvel/(2*D_ver_A_1*$F241)+D_ver_B_1*$F241)*SQRT(2))))*D_Ver_C0_1,0)))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D241/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E241^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E241)*SQRT(2)))),IF(AND($E241>0,$F241=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E241)-D_ver_B_1*$E241)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E241)+D_ver_B_1*$E241)*SQRT(2)))*D_Ver_C0_1,IF($E241=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E241)-D_ver_B_1*$E241)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E241)+D_ver_B_1*$E241)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F241)-D_ver_B_1*$F241)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F241)+D_ver_B_1*$F241)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_1*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1)))","v":0},{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))),(IF($D241<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))-EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*($D241-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D241-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*($D241-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D241-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D241/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z-D_ver_EPM*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*Ver_z+D_ver_EPM*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))),(IF($D241<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z241*$D241)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))-EXP((D_ver_EPM-$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z241*($D241-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D241-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z241)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z241*($D241-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D241-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C241-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C241/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*$C241+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$Z241*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z241)*$C241/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$Z241*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1))","v":0},{"$f":"IF( D_vert_AC,0,IF($D241<=D_ver_a,D_Ver_C0_1/2*(EXP((-$AD241)*$C241/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$AD241*$D241)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP(($AD241)*$C241/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$AD241*$D241)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))),D_Ver_C0_1/2*(EXP((-$AD241)*$C241/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$AD241*$D241)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))+EXP(($AD241)*$C241/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$AD241*$D241)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D241)))*SQRT(2))-EXP((-$AD241)*$C241/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241-$AD241*($D241-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D241-D_ver_a))))*SQRT(2))-EXP(($AD241)*$C241/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C241+$AD241*($D241-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D241-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_1)/D_Ver_R_1*$D241)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C241)+D_Ver_lambdayear_1)/D_Ver_R_1*Ver_t)),))","v":0}]
[null,null,{"$f":"C241+D_ver_z_incr","v":0},{"$f":"D241+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D242/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E242^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E242)*SQRT(2))))),(IF(AND($E242>0,$F242=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E242)-D_ver_B_1*$E242)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E242)+D_ver_B_1*$E242)*SQRT(2)))*D_Ver_C0_1,IF($F242>0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E242)-D_ver_B_1*$E242)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E242)+D_ver_B_1*$E242)*SQRT(2)))-(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F242)-D_ver_B_1*$F242)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F242)+D_ver_B_1*$F242)*SQRT(2))))*D_Ver_C0_1,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E242>0,$F242=0),0.5*EXP(-D_Ver_lambdayear_1*$C242/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C242/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C242/D_Ver_Vvel/(2*D_ver_A_1*$E242)-D_ver_B_1*$E242)*SQRT(2))+EXP(D_Ver_R_1*$C242/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C242/D_Ver_Vvel/(2*D_ver_A_1*$E242)+D_ver_B_1*$E242)*SQRT(2)))*D_Ver_C0_1,IF($F242>0,0.5*EXP(-D_Ver_lambdayear_1*$C242/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C242/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C242/D_Ver_Vvel/(2*D_ver_A_1*$E242)-D_ver_B_1*$E242)*SQRT(2))+EXP(D_Ver_R_1*$C242/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C242/D_Ver_Vvel/(2*D_ver_A_1*$E242)+D_ver_B_1*$E242)*SQRT(2)))-(EXP(-D_Ver_R_1*$C242/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C242/D_Ver_Vvel/(2*D_ver_A_1*$F242)-D_ver_B_1*$F242)*SQRT(2))+EXP(D_Ver_R_1*$C242/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C242/D_Ver_Vvel/(2*D_ver_A_1*$F242)+D_ver_B_1*$F242)*SQRT(2))))*D_Ver_C0_1,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D242/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z-D_ver_EPM*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*Ver_z+D_ver_EPM*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z242*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242)))*SQRT(2))+EXP((D_ver_EPM+$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z242*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242)))*SQRT(2))),(IF($D242<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z242*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242)))*SQRT(2))+EXP((D_ver_EPM+$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z242*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z242*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242)))*SQRT(2))+EXP((D_ver_EPM+$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z242*$D242)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D242)))*SQRT(2))-EXP((D_ver_EPM-$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z242*($D242-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D242-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z242)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z242*($D242-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D242-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C242-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C242/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*$C242+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242-$Z242*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242+$Z242*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242-$Z242*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242+$Z242*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242-$Z242*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242+$Z242*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242-$Z242*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z242)*$C242/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C242+$Z242*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_1)/D_Ver_R_1*$D242)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C242)+D_Ver_lambdayear_1)/D_Ver_R_1*Ver_t)),))","v":0}]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C249/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C249/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C249/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C249/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D251/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E251^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E251)*SQRT(2)))),IF(AND($E251>0,$F251=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E251)-D_ver_B_1*$E251)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E251)+D_ver_B_1*$E251)*SQRT(2)))*D_Ver_C0_1,IF($E251=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E251)-D_ver_B_1*$E251)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E251)+D_ver_B_1*$E251)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F251)-D_ver_B_1*$F251)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F251)+D_ver_B_1*$F251)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C259/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C259/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C259/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C259/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D261/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E261^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E261)*SQRT(2)))),IF(AND($E261>0,$F261=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E261)-D_ver_B_1*$E261)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E261)+D_ver_B_1*$E261)*SQRT(2)))*D_Ver_C0_1,IF($E261=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E261)-D_ver_B_1*$E261)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E261)+D_ver_B_1*$E261)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F261)-D_ver_B_1*$F261)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F261)+D_ver_B_1*$F261)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C269/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C269/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C269/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C269/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C271/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$E$239)*SQRT(2))))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C271/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($F$239>0,0.5*EXP(-D_Ver_lambdayear_1*$C271/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP(D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C271/D_Ver_Vvel/(2*D_ver_A_1*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1,0))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D271/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E271^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E271)*SQRT(2)))),IF(AND($E271>0,$F271=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E271)-D_ver_B_1*$E271)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E271)+D_ver_B_1*$E271)*SQRT(2)))*D_Ver_C0_1,IF($E271=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E271)-D_ver_B_1*$E271)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E271)+D_ver_B_1*$E271)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F271)-D_ver_B_1*$F271)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F271)+D_ver_B_1*$F271)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*$C271/D_Ver_Vvel)*EXP(-D_Ver_R_1*$C271/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D271/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z)/2*SQRT((D_Ver_R_1*$D271))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_1/2*(EXP((-$AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD271*$D271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271)))*SQRT(2))+EXP(($AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD271*$D271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D271<=D_ver_a,\nD_Ver_C0_1/2*(EXP((-$AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD271*$D271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271)))*SQRT(2))+EXP(($AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD271*$D271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271)))*SQRT(2))),\nD_Ver_C0_1/2*(EXP((-$AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD271*$D271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271)))*SQRT(2))+EXP(($AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD271*$D271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D271)))*SQRT(2))-EXP((-$AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD271*($D271-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D271-D_ver_a))))*SQRT(2))-EXP(($AD271)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD271*($D271-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D271-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C271)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_1*$C271)/2*SQRT((D_Ver_R_1*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_1/2*(EXP((-$AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271-$AD271*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271+$AD271*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_1/2*(EXP((-$AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271-$AD271*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271+$AD271*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),\nD_Ver_C0_1/2*(EXP((-$AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271-$AD271*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271+$AD271*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((-$AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271-$AD271*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD271)*$C271/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C271+$AD271*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D273/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E273^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E273)*SQRT(2))))),(IF(AND($E273>0,$F273=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E273)-D_ver_B_1*$E273)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E273)+D_ver_B_1*$E273)*SQRT(2)))*D_Ver_C0_1,IF($F273>0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E273)-D_ver_B_1*$E273)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E273)+D_ver_B_1*$E273)*SQRT(2)))-(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F273)-D_ver_B_1*$F273)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F273)+D_ver_B_1*$F273)*SQRT(2))))*D_Ver_C0_1,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E273>0,$F273=0),0.5*EXP(-D_Ver_lambdayear_1*$C273/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C273/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C273/D_Ver_Vvel/(2*D_ver_A_1*$E273)-D_ver_B_1*$E273)*SQRT(2))+EXP(D_Ver_R_1*$C273/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C273/D_Ver_Vvel/(2*D_ver_A_1*$E273)+D_ver_B_1*$E273)*SQRT(2)))*D_Ver_C0_1,IF($F273>0,0.5*EXP(-D_Ver_lambdayear_1*$C273/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C273/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C273/D_Ver_Vvel/(2*D_ver_A_1*$E273)-D_ver_B_1*$E273)*SQRT(2))+EXP(D_Ver_R_1*$C273/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C273/D_Ver_Vvel/(2*D_ver_A_1*$E273)+D_ver_B_1*$E273)*SQRT(2)))-(EXP(-D_Ver_R_1*$C273/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C273/D_Ver_Vvel/(2*D_ver_A_1*$F273)-D_ver_B_1*$F273)*SQRT(2))+EXP(D_Ver_R_1*$C273/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C273/D_Ver_Vvel/(2*D_ver_A_1*$F273)+D_ver_B_1*$F273)*SQRT(2))))*D_Ver_C0_1,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_1*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1)))","v":0},{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))),(IF($D273<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))-EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*($D273-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D273-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*($D273-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D273-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D273/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z-D_ver_EPM*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*Ver_z+D_ver_EPM*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))),(IF($D273<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z273*$D273)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))-EXP((D_ver_EPM-$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z273*($D273-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D273-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z273)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z273*($D273-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D273-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C273-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C273/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*$C273+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$Z273*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z273)*$C273/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$Z273*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1))","v":0},{"$f":"IF( D_vert_AC,0,IF($D273<=D_ver_a,D_Ver_C0_1/2*(EXP((-$AD273)*$C273/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$AD273*$D273)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP(($AD273)*$C273/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$AD273*$D273)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))),D_Ver_C0_1/2*(EXP((-$AD273)*$C273/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$AD273*$D273)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))+EXP(($AD273)*$C273/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$AD273*$D273)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D273)))*SQRT(2))-EXP((-$AD273)*$C273/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273-$AD273*($D273-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D273-D_ver_a))))*SQRT(2))-EXP(($AD273)*$C273/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C273+$AD273*($D273-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D273-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_1)/D_Ver_R_1*$D273)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C273)+D_Ver_lambdayear_1)/D_Ver_R_1*Ver_t)),))","v":0}]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C279/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C279/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C279/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C279/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D281/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E281^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E281)*SQRT(2)))),IF(AND($E281>0,$F281=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E281)-D_ver_B_1*$E281)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E281)+D_ver_B_1*$E281)*SQRT(2)))*D_Ver_C0_1,IF($E281=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E281)-D_ver_B_1*$E281)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E281)+D_ver_B_1*$E281)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F281)-D_ver_B_1*$F281)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F281)+D_ver_B_1*$F281)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C289/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C289/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C289/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C289/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D291/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E291^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E291)*SQRT(2)))),IF(AND($E291>0,$F291=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E291)-D_ver_B_1*$E291)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E291)+D_ver_B_1*$E291)*SQRT(2)))*D_Ver_C0_1,IF($E291=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E291)-D_ver_B_1*$E291)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E291)+D_ver_B_1*$E291)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F291)-D_ver_B_1*$F291)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F291)+D_ver_B_1*$F291)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C299/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C299/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C299/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C299/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D301/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E301^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E301)*SQRT(2)))),IF(AND($E301>0,$F301=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E301)-D_ver_B_1*$E301)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E301)+D_ver_B_1*$E301)*SQRT(2)))*D_Ver_C0_1,IF($E301=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E301)-D_ver_B_1*$E301)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E301)+D_ver_B_1*$E301)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F301)-D_ver_B_1*$F301)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F301)+D_ver_B_1*$F301)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D303-D_Ver_R_1/D_Ver_Vvel*$C303))>0,SQRT(D303-D_Ver_R_1/D_Ver_Vvel*$C303),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D303-(D_Ver_R_1/D_Ver_Vvel*$C303+D_ver_a)>0,SQRT(D303-(D_Ver_R_1/D_Ver_Vvel*$C303+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C303/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$E$239)*SQRT(2))))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C303/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($F$239>0,0.5*EXP(-D_Ver_lambdayear_1*$C303/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP(D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP(D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C303/D_Ver_Vvel/(2*D_ver_A_1*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1,0))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_1*EXP(D_Ver_lambdayear_1*$C303/D_Ver_Vvel)*EXP(-D_Ver_R_1*$C303/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D303/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z)/2*SQRT((D_Ver_R_1*$D303))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_1/2*(EXP((-$AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD303*$D303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303)))*SQRT(2))+EXP(($AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD303*$D303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D303<=D_ver_a,\nD_Ver_C0_1/2*(EXP((-$AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD303*$D303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303)))*SQRT(2))+EXP(($AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD303*$D303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303)))*SQRT(2))),\nD_Ver_C0_1/2*(EXP((-$AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD303*$D303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303)))*SQRT(2))+EXP(($AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD303*$D303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D303)))*SQRT(2))-EXP((-$AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$AD303*($D303-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D303-D_ver_a))))*SQRT(2))-EXP(($AD303)*Ver_z/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$AD303*($D303-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D303-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C303)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_1*$C303)/2*SQRT((D_Ver_R_1*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_1/2*(EXP((-$AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303-$AD303*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303+$AD303*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_1/2*(EXP((-$AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303-$AD303*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303+$AD303*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),\nD_Ver_C0_1/2*(EXP((-$AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303-$AD303*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP(($AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303+$AD303*Ver_t)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((-$AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303-$AD303*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD303)*$C303/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C303+$AD303*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D305/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E305^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E305)*SQRT(2))))),(IF(AND($E305>0,$F305=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E305)-D_ver_B_1*$E305)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E305)+D_ver_B_1*$E305)*SQRT(2)))*D_Ver_C0_1,IF($F305>0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E305)-D_ver_B_1*$E305)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$E305)+D_ver_B_1*$E305)*SQRT(2)))-(EXP(-D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F305)-D_ver_B_1*$F305)*SQRT(2))+EXP(D_Ver_R_1*Ver_z/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/(2*D_ver_A_1*$F305)+D_ver_B_1*$F305)*SQRT(2))))*D_Ver_C0_1,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E305>0,$F305=0),0.5*EXP(-D_Ver_lambdayear_1*$C305/D_Ver_Vvel)*(EXP(-D_Ver_R_1*$C305/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C305/D_Ver_Vvel/(2*D_ver_A_1*$E305)-D_ver_B_1*$E305)*SQRT(2))+EXP(D_Ver_R_1*$C305/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C305/D_Ver_Vvel/(2*D_ver_A_1*$E305)+D_ver_B_1*$E305)*SQRT(2)))*D_Ver_C0_1,IF($F305>0,0.5*EXP(-D_Ver_lambdayear_1*$C305/D_Ver_Vvel)*((EXP(-D_Ver_R_1*$C305/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C305/D_Ver_Vvel/(2*D_ver_A_1*$E305)-D_ver_B_1*$E305)*SQRT(2))+EXP(D_Ver_R_1*$C305/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C305/D_Ver_Vvel/(2*D_ver_A_1*$E305)+D_ver_B_1*$E305)*SQRT(2)))-(EXP(-D_Ver_R_1*$C305/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C305/D_Ver_Vvel/(2*D_ver_A_1*$F305)-D_ver_B_1*$F305)*SQRT(2))+EXP(D_Ver_R_1*$C305/D_Ver_Vvel*D_ver_B_1/D_ver_A_1)*2*NORMSDIST(-(D_Ver_R_1*$C305/D_Ver_Vvel/(2*D_ver_A_1*$F305)+D_ver_B_1*$F305)*SQRT(2))))*D_Ver_C0_1,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_1*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1)))","v":0},{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))),(IF($D305<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))-EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*($D305-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D305-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*($D305-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D305-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*$D305/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*Ver_z-D_ver_EPM*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*Ver_z+D_ver_EPM*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))),(IF($D305<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z305*$D305)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))-EXP((D_ver_EPM-$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z-$Z305*($D305-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D305-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z305)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*Ver_z+$Z305*($D305-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*($D305-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)*(1-0.5*2*NORMSDIST(-(D_Ver_R_1*$C305-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C305/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-(D_Ver_R_1*$C305+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))),D_Ver_C0_1/2*(EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$Z305*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z305)*$C305/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$Z305*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_1)*D_Ver_R_1*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_1*D_ver_Ddwm_1))","v":0},{"$f":"IF( D_vert_AC,0,IF($D305<=D_ver_a,D_Ver_C0_1/2*(EXP((-$AD305)*$C305/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$AD305*$D305)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP(($AD305)*$C305/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$AD305*$D305)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))),D_Ver_C0_1/2*(EXP((-$AD305)*$C305/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$AD305*$D305)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))+EXP(($AD305)*$C305/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$AD305*$D305)/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*$D305)))*SQRT(2))-EXP((-$AD305)*$C305/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305-$AD305*($D305-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D305-D_ver_a))))*SQRT(2))-EXP(($AD305)*$C305/(2*(D_ver_Ddwm_1)))*2*NORMSDIST(-((D_Ver_R_1*$C305+$AD305*($D305-D_ver_a))/(2*SQRT((D_ver_Ddwm_1)*D_Ver_R_1*($D305-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_1)/D_Ver_R_1*$D305)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C305)+D_Ver_lambdayear_1)/D_Ver_R_1*Ver_t)),))","v":0}]
[null,null,{"$f":"C305+D_ver_z_incr","v":0},{"$f":"D305+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*Ver_t/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*$C309/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E$239^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)*SQRT(2)))),IF(AND($E$239>0,$F$239=0),0.5*EXP(-D_Ver_lambdayear_1*$C309/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))*D_Ver_C0_1,IF($E$239=0,0,0.5*EXP(-D_Ver_lambdayear_1*$C309/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)-D_ver_B_1*$E$239)*SQRT(2))+EXP((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$E$239)+D_ver_B_1*$E$239)*SQRT(2)))-(EXP(-(D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)-D_ver_B_1*$F$239)*SQRT(2))+EXP((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*$C309/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*Q$238)/(2*$F$239)+D_ver_B_1*$F$239)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_1*(EXP(-D_Ver_lambdayear_1*$D311/D_Ver_R_1)-EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_1*$E311^2/D_Ver_R_1)*2*NORMSDIST(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E311)*SQRT(2)))),IF(AND($E311>0,$F311=0),0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E311)-D_ver_B_1*$E311)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E311)+D_ver_B_1*$E311)*SQRT(2)))*D_Ver_C0_1,IF($E311=0,0,0.5*EXP(-D_Ver_lambdayear_1*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E311)-D_ver_B_1*$E311)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$E311)+D_ver_B_1*$E311)*SQRT(2)))-(EXP(-(D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F311)-D_ver_B_1*$F311)*SQRT(2))+EXP((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)*D_ver_B_1)*2*NORMSDIST(-((D_Ver_R_1*Ver_z/D_Ver_Vvel/D_ver_A_1+D_ver_G_1*J$238)/(2*$F311)+D_ver_B_1*$F311)*SQRT(2))))*D_Ver_C0_1))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,null,"Stof 2",{"$f":"D_Ver_stofnavn_2","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",E322,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"IF(D_vert_DTU_1b,B_ver_Cz_DTU_2,\"(ikke stationært)\")","v":"(ikke stationært)"},"mg/l",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Sammenligning af modeller \nKoncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller \nKoncentration efter  år"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Koncentration i matrix i forskellige afstande (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken i  m´s dybde"},null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_2,\": Koncentration i matrix i forskellige afstande (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kun DTU V1D-Model 2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Stationær konc.med tid i \",Ver_z,\" m´s dybde - Kun model 1b\")","v":"Stationær konc.med tid i  m´s dybde - Kun model 1b"},{"$f":"CONCATENATE(\"Stationær konc.i dybde ved tid \",Ver_t,\" år_ kun model 1b\")","v":"Stationær konc.i dybde ved tid  år_ kun model 1b"},null,null,null,null,null,null,null,null,"En aftagnende kilde"]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"IF(D_vert_DTU_2,(D_Ver_R_2*(D_ver_2B/2)^2)/D_ver_Ddwm_2,\"\")","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,"Sprækkemodel",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM model",null,null,null,"Diffusionsmodel",null,null,"1. ordens model"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in fracture with time at depth \",Ver_z,\" m\")","v":"Conc in fracture with time at depth  m"},{"$f":"CONCATENATE(\"Conc in fracture with depth at time \",Ver_t,\" years\")","v":"Conc in fracture with depth at time  years"},"Original Conc in fracture at depth and time",{"$f":"CONCATENATE(\"Conc in matrix with time at \",Ver_z, \" m depth at different distances x m from the fracture\")","v":"Conc in matrix with time at  m depth at different distances x m from the fracture"},null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in matrix with depth at \",Ver_t, \" years at different distances x m from the fracture\")","v":"Conc in matrix with depth at  years at different distances x m from the fracture"},null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EPM with time at depth \",Ver_z,\" m\")","v":"EPM with time at depth  m"},{"$f":"CONCATENATE(\"EPM in depth at time \",Ver_t,\" years\")","v":"EPM in depth at time  years"},null,"No fracture",{"$f":"CONCATENATE(\"Diffusion with time at depth \",Ver_z,\" m\")","v":"Diffusion with time at depth  m"},{"$f":"CONCATENATE(\"Diffusion in depth at time \",Ver_t,\" years\")","v":"Diffusion in depth at time  years"},{"$f":"CONCATENATE(\"1.order with time at depth \",Ver_z,\" m\")","v":"1.order with time at depth  m"},{"$f":"CONCATENATE(\"1.order in depth at time \",Ver_t,\" years\")","v":"1.order in depth at time  years"}]
[null,null,"z (depth)","t (time)","T'","T''",null,null,null,0.1,0.2,0.3,0.4,0.5,0.75,1,0.1,0.2,0.3,0.4,0.5,0.75,1,"Stationær konc.","Stationær konc.","u1",null,null,null,"u2","No advection"]
[null,null,{"$f":"Ver_z","v":0},{"$f":"Ver_t","v":0},{"$f":"IF((SQRT(D357-D_Ver_R_2/D_Ver_Vvel*$C357))>0,SQRT(D357-D_Ver_R_2/D_Ver_Vvel*$C357),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D357-(D_Ver_R_2/D_Ver_Vvel*$C357+D_ver_a)>0,SQRT(D357-(D_Ver_R_2/D_Ver_Vvel*$C357+D_ver_a)),0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E357)*SQRT(2))))),(IF(AND($E357>0,$F357=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E357)-D_ver_B_2*$E357)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E357)+D_ver_B_2*$E357)*SQRT(2)))*D_Ver_C0_2,IF($F357>0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E357)-D_ver_B_2*$E357)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E357)+D_ver_B_2*$E357)*SQRT(2)))-(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F357)-D_ver_B_2*$F357)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F357)+D_ver_B_2*$F357)*SQRT(2))))*D_Ver_C0_2,0)))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E$357)*SQRT(2))))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP(D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($F$357>0,0.5*EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP(D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP(D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2,0))))","v":0},{"$f":"IF(D_vert_AC,0,IF(AND($E357>0,$F357=0),0.5*EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E357)-D_ver_B_2*$E357)*SQRT(2))+EXP(D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E357)+D_ver_B_2*$E357)*SQRT(2)))*D_Ver_C0_2,IF($F357>0,0.5*EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E357)-D_ver_B_2*$E357)*SQRT(2))+EXP(D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$E357)+D_ver_B_2*$E357)*SQRT(2)))-(EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$F357)-D_ver_B_2*$F357)*SQRT(2))+EXP(D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/(2*D_ver_A_2*$F357)+D_ver_B_2*$F357)*SQRT(2))))*D_Ver_C0_2,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D357/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E357)*SQRT(2)))),IF(AND($E357>0,$F357=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E357)-D_ver_B_2*$E357)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E357)+D_ver_B_2*$E357)*SQRT(2)))*D_Ver_C0_2,IF($E357=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E357)-D_ver_B_2*$E357)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E357)+D_ver_B_2*$E357)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F357)-D_ver_B_2*$F357)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F357)+D_ver_B_2*$F357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C357/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_2*EXP(D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_2*EXP(D_Ver_lambdayear_2*$C357/D_Ver_Vvel)*EXP(-D_Ver_R_2*$C357/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2)))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_2),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D357/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z-D_ver_EPM*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*Ver_z+D_ver_EPM*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z357*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))+EXP((D_ver_EPM+$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z357*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))),(IF($D357<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z357*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))+EXP((D_ver_EPM+$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z357*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z357*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))+EXP((D_ver_EPM+$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z357*$D357)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))-EXP((D_ver_EPM-$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z357*($D357-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D357-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z357)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z357*($D357-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D357-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C357-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C357/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*$C357+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$Z357*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$Z357*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$Z357*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$Z357*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$Z357*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$Z357*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$Z357*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z357)*$C357/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$Z357*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2))","v":0},{"$f":"IF( D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_2),0))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D357/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z)/2*SQRT((D_Ver_R_2*$D357))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_2/2*(EXP((-$AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD357*$D357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))+EXP(($AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD357*$D357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D357<=D_ver_a,\nD_Ver_C0_2/2*(EXP((-$AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD357*$D357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))+EXP(($AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD357*$D357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))),\nD_Ver_C0_2/2*(EXP((-$AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD357*$D357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))+EXP(($AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD357*$D357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D357)))*SQRT(2))-EXP((-$AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD357*($D357-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D357-D_ver_a))))*SQRT(2))-EXP(($AD357)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD357*($D357-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D357-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C357)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_2*$C357)/2*SQRT((D_Ver_R_2*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_2/2*(EXP((-$AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$AD357*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$AD357*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_2/2*(EXP((-$AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$AD357*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$AD357*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),\nD_Ver_C0_2/2*(EXP((-$AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$AD357*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$AD357*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((-$AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357-$AD357*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD357)*$C357/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C357+$AD357*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C357)+D_Ver_lambdayear_2)/D_Ver_R_2*$D357)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C357)+D_Ver_lambdayear_2)/D_Ver_R_2*Ver_t)),))","v":0}]
[null,null,0,{"$f":"0","v":0},{"$error":"#VALUE!"},0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D358/D_Ver_R_2))),(IF(AND($E358>0,$F358=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E358)-D_ver_B_2*$E358)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E358)+D_ver_B_2*$E358)*SQRT(2)))*D_Ver_C0_2,IF($F358>0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E358)-D_ver_B_2*$E358)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E358)+D_ver_B_2*$E358)*SQRT(2)))-(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F358)-D_ver_B_2*$F358)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F358)+D_ver_B_2*$F358)*SQRT(2))))*D_Ver_C0_2,0)))))","v":0},0,{"$f":"IF(D_vert_AC,0,IF(AND($E358>0,$F358=0),0.5*EXP(-D_Ver_lambdayear_2*$C358/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C358/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C358/D_Ver_Vvel/(2*D_ver_A_2*$E358)-D_ver_B_2*$E358)*SQRT(2))+EXP(D_Ver_R_2*$C358/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C358/D_Ver_Vvel/(2*D_ver_A_2*$E358)+D_ver_B_2*$E358)*SQRT(2)))*D_Ver_C0_2,IF($F358>0,0.5*EXP(-D_Ver_lambdayear_2*$C358/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C358/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C358/D_Ver_Vvel/(2*D_ver_A_2*$E358)-D_ver_B_2*$E358)*SQRT(2))+EXP(D_Ver_R_2*$C358/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C358/D_Ver_Vvel/(2*D_ver_A_2*$E358)+D_ver_B_2*$E358)*SQRT(2)))-(EXP(-D_Ver_R_2*$C358/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C358/D_Ver_Vvel/(2*D_ver_A_2*$F358)-D_ver_B_2*$F358)*SQRT(2))+EXP(D_Ver_R_2*$C358/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C358/D_Ver_Vvel/(2*D_ver_A_2*$F358)+D_ver_B_2*$F358)*SQRT(2))))*D_Ver_C0_2,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D358/D_Ver_R_2))),IF(AND($E358>0,$F358=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E358)-D_ver_B_2*$E358)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E358)+D_ver_B_2*$E358)*SQRT(2)))*D_Ver_C0_2,IF($E358=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E358)-D_ver_B_2*$E358)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E358)+D_ver_B_2*$E358)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F358)-D_ver_B_2*$F358)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F358)+D_ver_B_2*$F358)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_2),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z358*$D358)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D358)))*SQRT(2))+EXP((D_ver_EPM+$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z358*$D358)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D358)))*SQRT(2))),(IF($D358<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z358*$D358)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D358)))*SQRT(2))+EXP((D_ver_EPM+$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z358*$D358)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D358)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z358*$D358)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D358)))*SQRT(2))+EXP((D_ver_EPM+$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z358*$D358)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D358)))*SQRT(2))-EXP((D_ver_EPM-$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z358*($D358-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D358-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z358)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z358*($D358-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D358-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358-$Z358*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358+$Z358*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358-$Z358*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358+$Z358*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358-$Z358*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358+$Z358*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358-$Z358*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z358)*$C358/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C358+$Z358*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_2),0))","v":0},0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_2)/D_Ver_R_2*$D358)),))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,IF(C358=0,D_Ver_C0_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C358)+D_Ver_lambdayear_2)/D_Ver_R_2*Ver_t))),))","v":0}]
[null,null,{"$f":"0+D_ver_z_incr","v":0},{"$f":"0+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D359/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E359^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E359)*SQRT(2))))),(IF(AND($E359>0,$F359=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E359)-D_ver_B_2*$E359)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E359)+D_ver_B_2*$E359)*SQRT(2)))*D_Ver_C0_2,IF($F359>0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E359)-D_ver_B_2*$E359)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E359)+D_ver_B_2*$E359)*SQRT(2)))-(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F359)-D_ver_B_2*$F359)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F359)+D_ver_B_2*$F359)*SQRT(2))))*D_Ver_C0_2,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E359>0,$F359=0),0.5*EXP(-D_Ver_lambdayear_2*$C359/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C359/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C359/D_Ver_Vvel/(2*D_ver_A_2*$E359)-D_ver_B_2*$E359)*SQRT(2))+EXP(D_Ver_R_2*$C359/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C359/D_Ver_Vvel/(2*D_ver_A_2*$E359)+D_ver_B_2*$E359)*SQRT(2)))*D_Ver_C0_2,IF($F359>0,0.5*EXP(-D_Ver_lambdayear_2*$C359/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C359/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C359/D_Ver_Vvel/(2*D_ver_A_2*$E359)-D_ver_B_2*$E359)*SQRT(2))+EXP(D_Ver_R_2*$C359/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C359/D_Ver_Vvel/(2*D_ver_A_2*$E359)+D_ver_B_2*$E359)*SQRT(2)))-(EXP(-D_Ver_R_2*$C359/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C359/D_Ver_Vvel/(2*D_ver_A_2*$F359)-D_ver_B_2*$F359)*SQRT(2))+EXP(D_Ver_R_2*$C359/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C359/D_Ver_Vvel/(2*D_ver_A_2*$F359)+D_ver_B_2*$F359)*SQRT(2))))*D_Ver_C0_2,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D359/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E359^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E359)*SQRT(2)))),IF(AND($E359>0,$F359=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E359)-D_ver_B_2*$E359)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E359)+D_ver_B_2*$E359)*SQRT(2)))*D_Ver_C0_2,IF($E359=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E359)-D_ver_B_2*$E359)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E359)+D_ver_B_2*$E359)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F359)-D_ver_B_2*$F359)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F359)+D_ver_B_2*$F359)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))),(IF($D359<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))-EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*($D359-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D359-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*($D359-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D359-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D359/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z-D_ver_EPM*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*Ver_z+D_ver_EPM*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))),(IF($D359<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z359*$D359)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))-EXP((D_ver_EPM-$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z359*($D359-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D359-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z359)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z359*($D359-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D359-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C359-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C359/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*$C359+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$Z359*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z359)*$C359/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$Z359*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2))","v":0},{"$f":"IF( D_vert_AC,0,IF($D359<=D_ver_a,D_Ver_C0_2/2*(EXP((-$AD359)*$C359/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$AD359*$D359)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP(($AD359)*$C359/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$AD359*$D359)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))),D_Ver_C0_2/2*(EXP((-$AD359)*$C359/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$AD359*$D359)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))+EXP(($AD359)*$C359/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$AD359*$D359)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D359)))*SQRT(2))-EXP((-$AD359)*$C359/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359-$AD359*($D359-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D359-D_ver_a))))*SQRT(2))-EXP(($AD359)*$C359/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C359+$AD359*($D359-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D359-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_2)/D_Ver_R_2*$D359)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C359)+D_Ver_lambdayear_2)/D_Ver_R_2*Ver_t)),))","v":0}]
[null,null,{"$f":"C359+D_ver_z_incr","v":0},{"$f":"D359+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C367/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C367/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C367/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C367/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D369/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E369^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E369)*SQRT(2)))),IF(AND($E369>0,$F369=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E369)-D_ver_B_2*$E369)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E369)+D_ver_B_2*$E369)*SQRT(2)))*D_Ver_C0_2,IF($E369=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E369)-D_ver_B_2*$E369)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E369)+D_ver_B_2*$E369)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F369)-D_ver_B_2*$F369)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F369)+D_ver_B_2*$F369)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C377/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C377/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C377/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C377/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D379/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E379^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E379)*SQRT(2)))),IF(AND($E379>0,$F379=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E379)-D_ver_B_2*$E379)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E379)+D_ver_B_2*$E379)*SQRT(2)))*D_Ver_C0_2,IF($E379=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E379)-D_ver_B_2*$E379)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E379)+D_ver_B_2*$E379)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F379)-D_ver_B_2*$F379)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F379)+D_ver_B_2*$F379)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C387/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C387/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C387/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C387/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D389-D_Ver_R_2/D_Ver_Vvel*$C389))>0,SQRT(D389-D_Ver_R_2/D_Ver_Vvel*$C389),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D389-(D_Ver_R_2/D_Ver_Vvel*$C389+D_ver_a)>0,SQRT(D389-(D_Ver_R_2/D_Ver_Vvel*$C389+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C389/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$E$357)*SQRT(2))))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C389/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP(D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($F$357>0,0.5*EXP(-D_Ver_lambdayear_2*$C389/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP(D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP(D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C389/D_Ver_Vvel/(2*D_ver_A_2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2,0))))","v":0},0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D389/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E389^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E389)*SQRT(2)))),IF(AND($E389>0,$F389=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E389)-D_ver_B_2*$E389)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E389)+D_ver_B_2*$E389)*SQRT(2)))*D_Ver_C0_2,IF($E389=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E389)-D_ver_B_2*$E389)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E389)+D_ver_B_2*$E389)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F389)-D_ver_B_2*$F389)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F389)+D_ver_B_2*$F389)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_2*EXP(D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_2*EXP(D_Ver_lambdayear_2*$C389/D_Ver_Vvel)*EXP(-D_Ver_R_2*$C389/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2)))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D389/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z)/2*SQRT((D_Ver_R_2*$D389))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_2/2*(EXP((-$AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD389*$D389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389)))*SQRT(2))+EXP(($AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD389*$D389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D389<=D_ver_a,\nD_Ver_C0_2/2*(EXP((-$AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD389*$D389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389)))*SQRT(2))+EXP(($AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD389*$D389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389)))*SQRT(2))),\nD_Ver_C0_2/2*(EXP((-$AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD389*$D389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389)))*SQRT(2))+EXP(($AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD389*$D389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D389)))*SQRT(2))-EXP((-$AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD389*($D389-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D389-D_ver_a))))*SQRT(2))-EXP(($AD389)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD389*($D389-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D389-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C389)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_2*$C389)/2*SQRT((D_Ver_R_2*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_2/2*(EXP((-$AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389-$AD389*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389+$AD389*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_2/2*(EXP((-$AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389-$AD389*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389+$AD389*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),\nD_Ver_C0_2/2*(EXP((-$AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389-$AD389*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389+$AD389*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((-$AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389-$AD389*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD389)*$C389/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C389+$AD389*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D391/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E391^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E391)*SQRT(2))))),(IF(AND($E391>0,$F391=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E391)-D_ver_B_2*$E391)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E391)+D_ver_B_2*$E391)*SQRT(2)))*D_Ver_C0_2,IF($F391>0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E391)-D_ver_B_2*$E391)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E391)+D_ver_B_2*$E391)*SQRT(2)))-(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F391)-D_ver_B_2*$F391)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F391)+D_ver_B_2*$F391)*SQRT(2))))*D_Ver_C0_2,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E391>0,$F391=0),0.5*EXP(-D_Ver_lambdayear_2*$C391/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C391/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C391/D_Ver_Vvel/(2*D_ver_A_2*$E391)-D_ver_B_2*$E391)*SQRT(2))+EXP(D_Ver_R_2*$C391/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C391/D_Ver_Vvel/(2*D_ver_A_2*$E391)+D_ver_B_2*$E391)*SQRT(2)))*D_Ver_C0_2,IF($F391>0,0.5*EXP(-D_Ver_lambdayear_2*$C391/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C391/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C391/D_Ver_Vvel/(2*D_ver_A_2*$E391)-D_ver_B_2*$E391)*SQRT(2))+EXP(D_Ver_R_2*$C391/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C391/D_Ver_Vvel/(2*D_ver_A_2*$E391)+D_ver_B_2*$E391)*SQRT(2)))-(EXP(-D_Ver_R_2*$C391/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C391/D_Ver_Vvel/(2*D_ver_A_2*$F391)-D_ver_B_2*$F391)*SQRT(2))+EXP(D_Ver_R_2*$C391/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C391/D_Ver_Vvel/(2*D_ver_A_2*$F391)+D_ver_B_2*$F391)*SQRT(2))))*D_Ver_C0_2,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))),(IF($D391<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))-EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*($D391-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D391-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*($D391-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D391-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D391/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z-D_ver_EPM*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*Ver_z+D_ver_EPM*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))),(IF($D391<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z391*$D391)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))-EXP((D_ver_EPM-$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z391*($D391-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D391-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z391)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z391*($D391-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D391-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C391-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C391/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*$C391+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$Z391*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z391)*$C391/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$Z391*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2))","v":0},{"$f":"IF( D_vert_AC,0,IF($D391<=D_ver_a,D_Ver_C0_2/2*(EXP((-$AD391)*$C391/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$AD391*$D391)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP(($AD391)*$C391/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$AD391*$D391)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))),D_Ver_C0_2/2*(EXP((-$AD391)*$C391/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$AD391*$D391)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))+EXP(($AD391)*$C391/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$AD391*$D391)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D391)))*SQRT(2))-EXP((-$AD391)*$C391/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391-$AD391*($D391-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D391-D_ver_a))))*SQRT(2))-EXP(($AD391)*$C391/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C391+$AD391*($D391-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D391-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_2)/D_Ver_R_2*$D391)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C391)+D_Ver_lambdayear_2)/D_Ver_R_2*Ver_t)),))","v":0}]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C397/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C397/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C397/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C397/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D399/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E399^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E399)*SQRT(2)))),IF(AND($E399>0,$F399=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E399)-D_ver_B_2*$E399)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E399)+D_ver_B_2*$E399)*SQRT(2)))*D_Ver_C0_2,IF($E399=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E399)-D_ver_B_2*$E399)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E399)+D_ver_B_2*$E399)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F399)-D_ver_B_2*$F399)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F399)+D_ver_B_2*$F399)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C407/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C407/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C407/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C407/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D409/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E409^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E409)*SQRT(2)))),IF(AND($E409>0,$F409=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E409)-D_ver_B_2*$E409)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E409)+D_ver_B_2*$E409)*SQRT(2)))*D_Ver_C0_2,IF($E409=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E409)-D_ver_B_2*$E409)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E409)+D_ver_B_2*$E409)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F409)-D_ver_B_2*$F409)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F409)+D_ver_B_2*$F409)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C417/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C417/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C417/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C417/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D419/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E419^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E419)*SQRT(2)))),IF(AND($E419>0,$F419=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E419)-D_ver_B_2*$E419)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E419)+D_ver_B_2*$E419)*SQRT(2)))*D_Ver_C0_2,IF($E419=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E419)-D_ver_B_2*$E419)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E419)+D_ver_B_2*$E419)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F419)-D_ver_B_2*$F419)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F419)+D_ver_B_2*$F419)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D421-D_Ver_R_2/D_Ver_Vvel*$C421))>0,SQRT(D421-D_Ver_R_2/D_Ver_Vvel*$C421),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D421-(D_Ver_R_2/D_Ver_Vvel*$C421+D_ver_a)>0,SQRT(D421-(D_Ver_R_2/D_Ver_Vvel*$C421+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C421/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$E$357)*SQRT(2))))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C421/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP(D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($F$357>0,0.5*EXP(-D_Ver_lambdayear_2*$C421/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP(D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP(D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C421/D_Ver_Vvel/(2*D_ver_A_2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2,0))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_2*EXP(D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_2*EXP(D_Ver_lambdayear_2*$C421/D_Ver_Vvel)*EXP(-D_Ver_R_2*$C421/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2)))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D421/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z)/2*SQRT((D_Ver_R_2*$D421))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_2/2*(EXP((-$AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD421*$D421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421)))*SQRT(2))+EXP(($AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD421*$D421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D421<=D_ver_a,\nD_Ver_C0_2/2*(EXP((-$AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD421*$D421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421)))*SQRT(2))+EXP(($AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD421*$D421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421)))*SQRT(2))),\nD_Ver_C0_2/2*(EXP((-$AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD421*$D421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421)))*SQRT(2))+EXP(($AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD421*$D421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D421)))*SQRT(2))-EXP((-$AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$AD421*($D421-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D421-D_ver_a))))*SQRT(2))-EXP(($AD421)*Ver_z/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$AD421*($D421-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D421-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C421)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_2*$C421)/2*SQRT((D_Ver_R_2*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_2/2*(EXP((-$AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421-$AD421*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421+$AD421*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_2/2*(EXP((-$AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421-$AD421*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421+$AD421*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),\nD_Ver_C0_2/2*(EXP((-$AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421-$AD421*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP(($AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421+$AD421*Ver_t)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((-$AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421-$AD421*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD421)*$C421/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C421+$AD421*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D423/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E423^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E423)*SQRT(2))))),(IF(AND($E423>0,$F423=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E423)-D_ver_B_2*$E423)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E423)+D_ver_B_2*$E423)*SQRT(2)))*D_Ver_C0_2,IF($F423>0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E423)-D_ver_B_2*$E423)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$E423)+D_ver_B_2*$E423)*SQRT(2)))-(EXP(-D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F423)-D_ver_B_2*$F423)*SQRT(2))+EXP(D_Ver_R_2*Ver_z/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/(2*D_ver_A_2*$F423)+D_ver_B_2*$F423)*SQRT(2))))*D_Ver_C0_2,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E423>0,$F423=0),0.5*EXP(-D_Ver_lambdayear_2*$C423/D_Ver_Vvel)*(EXP(-D_Ver_R_2*$C423/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C423/D_Ver_Vvel/(2*D_ver_A_2*$E423)-D_ver_B_2*$E423)*SQRT(2))+EXP(D_Ver_R_2*$C423/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C423/D_Ver_Vvel/(2*D_ver_A_2*$E423)+D_ver_B_2*$E423)*SQRT(2)))*D_Ver_C0_2,IF($F423>0,0.5*EXP(-D_Ver_lambdayear_2*$C423/D_Ver_Vvel)*((EXP(-D_Ver_R_2*$C423/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C423/D_Ver_Vvel/(2*D_ver_A_2*$E423)-D_ver_B_2*$E423)*SQRT(2))+EXP(D_Ver_R_2*$C423/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C423/D_Ver_Vvel/(2*D_ver_A_2*$E423)+D_ver_B_2*$E423)*SQRT(2)))-(EXP(-D_Ver_R_2*$C423/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C423/D_Ver_Vvel/(2*D_ver_A_2*$F423)-D_ver_B_2*$F423)*SQRT(2))+EXP(D_Ver_R_2*$C423/D_Ver_Vvel*D_ver_B_2/D_ver_A_2)*2*NORMSDIST(-(D_Ver_R_2*$C423/D_Ver_Vvel/(2*D_ver_A_2*$F423)+D_ver_B_2*$F423)*SQRT(2))))*D_Ver_C0_2,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))),(IF($D423<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))-EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*($D423-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D423-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*($D423-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D423-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*$D423/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*Ver_z-D_ver_EPM*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*Ver_z+D_ver_EPM*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))),(IF($D423<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z423*$D423)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))-EXP((D_ver_EPM-$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z-$Z423*($D423-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D423-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z423)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*Ver_z+$Z423*($D423-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*($D423-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)*(1-0.5*2*NORMSDIST(-(D_Ver_R_2*$C423-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C423/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-(D_Ver_R_2*$C423+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))),D_Ver_C0_2/2*(EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$Z423*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z423)*$C423/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$Z423*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_2)*D_Ver_R_2*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_2*D_ver_Ddwm_2))","v":0},{"$f":"IF( D_vert_AC,0,IF($D423<=D_ver_a,D_Ver_C0_2/2*(EXP((-$AD423)*$C423/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$AD423*$D423)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP(($AD423)*$C423/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$AD423*$D423)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))),D_Ver_C0_2/2*(EXP((-$AD423)*$C423/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$AD423*$D423)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))+EXP(($AD423)*$C423/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$AD423*$D423)/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*$D423)))*SQRT(2))-EXP((-$AD423)*$C423/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423-$AD423*($D423-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D423-D_ver_a))))*SQRT(2))-EXP(($AD423)*$C423/(2*(D_ver_Ddwm_2)))*2*NORMSDIST(-((D_Ver_R_2*$C423+$AD423*($D423-D_ver_a))/(2*SQRT((D_ver_Ddwm_2)*D_Ver_R_2*($D423-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_2)/D_Ver_R_2*$D423)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C423)+D_Ver_lambdayear_2)/D_Ver_R_2*Ver_t)),))","v":0}]
[null,null,{"$f":"C423+D_ver_z_incr","v":0},{"$f":"D423+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*Ver_t/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*$C427/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E$357^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)*SQRT(2)))),IF(AND($E$357>0,$F$357=0),0.5*EXP(-D_Ver_lambdayear_2*$C427/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))*D_Ver_C0_2,IF($E$357=0,0,0.5*EXP(-D_Ver_lambdayear_2*$C427/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)-D_ver_B_2*$E$357)*SQRT(2))+EXP((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$E$357)+D_ver_B_2*$E$357)*SQRT(2)))-(EXP(-(D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)-D_ver_B_2*$F$357)*SQRT(2))+EXP((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*$C427/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*Q$238)/(2*$F$357)+D_ver_B_2*$F$357)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_2*(EXP(-D_Ver_lambdayear_2*$D429/D_Ver_R_2)-EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_2*$E429^2/D_Ver_R_2)*2*NORMSDIST(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E429)*SQRT(2)))),IF(AND($E429>0,$F429=0),0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E429)-D_ver_B_2*$E429)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E429)+D_ver_B_2*$E429)*SQRT(2)))*D_Ver_C0_2,IF($E429=0,0,0.5*EXP(-D_Ver_lambdayear_2*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E429)-D_ver_B_2*$E429)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$E429)+D_ver_B_2*$E429)*SQRT(2)))-(EXP(-(D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F429)-D_ver_B_2*$F429)*SQRT(2))+EXP((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)*D_ver_B_2)*2*NORMSDIST(-((D_Ver_R_2*Ver_z/D_Ver_Vvel/D_ver_A_2+D_ver_G_2*J$356)/(2*$F429)+D_ver_B_2*$F429)*SQRT(2))))*D_Ver_C0_2))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,null,"Stof 3",{"$f":"D_Ver_stofnavn_3","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",E440,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"IF(D_vert_DTU_1b,B_ver_Cz_DTU_3,\"(ikke stationært)\")","v":"(ikke stationært)"},"mg/l",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Sammenligning af modeller\nKoncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\nKoncentration i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Koncentration i matrix i forskellige afstande (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken i  m´s dybde"},null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_3,\": Koncentration i matrix i forskellige afstande (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kun DTU V1D-Model 2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Stationær konc.med tid i \",Ver_z,\" m´s dybde - Kun model 1b\")","v":"Stationær konc.med tid i  m´s dybde - Kun model 1b"},{"$f":"CONCATENATE(\"Stationær konc.i dybde ved tid \",Ver_t,\" år_ kun model 1b\")","v":"Stationær konc.i dybde ved tid  år_ kun model 1b"},null,null,null,null,null,null,null,null,"En aftagnende kilde"]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"IF(D_vert_DTU_2,(D_Ver_R_3*(D_ver_2B/2)^2)/D_ver_Ddwm_3,\"\")","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,"Sprækkemodel",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM model",null,null,null,"Diffusionsmodel",null,null,"1. ordens model"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in fracture with time at depth \",Ver_z,\" m\")","v":"Conc in fracture with time at depth  m"},{"$f":"CONCATENATE(\"Conc in fracture with depth at time \",Ver_t,\" years\")","v":"Conc in fracture with depth at time  years"},"Original Conc in fracture at depth and time",{"$f":"CONCATENATE(\"Conc in matrix with time at \",Ver_z, \" m depth at different distances x m from the fracture\")","v":"Conc in matrix with time at  m depth at different distances x m from the fracture"},null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in matrix with depth at \",Ver_t, \" years at different distances x m from the fracture\")","v":"Conc in matrix with depth at  years at different distances x m from the fracture"},null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EPM with time at depth \",Ver_z,\" m\")","v":"EPM with time at depth  m"},{"$f":"CONCATENATE(\"EPM in depth at time \",Ver_t,\" years\")","v":"EPM in depth at time  years"},null,"No fracture",{"$f":"CONCATENATE(\"Diffusion with time at depth \",Ver_z,\" m\")","v":"Diffusion with time at depth  m"},{"$f":"CONCATENATE(\"Diffusion in depth at time \",Ver_t,\" years\")","v":"Diffusion in depth at time  years"},{"$f":"CONCATENATE(\"1.order with time at depth \",Ver_z,\" m\")","v":"1.order with time at depth  m"},{"$f":"CONCATENATE(\"1.order in depth at time \",Ver_t,\" years\")","v":"1.order in depth at time  years"}]
[null,null,"z (depth)","t (time)","T'","T''",null,null,null,0.1,0.2,0.3,0.4,0.5,0.75,1,0.1,0.2,0.3,0.4,0.5,0.75,1,"Stationær konc.","Stationær konc.","u1",null,null,null,"u2","No advection"]
[null,null,{"$f":"Ver_z","v":0},{"$f":"Ver_t","v":0},{"$f":"IF((SQRT(D475-D_Ver_R_3/D_Ver_Vvel*$C475))>0,SQRT(D475-D_Ver_R_3/D_Ver_Vvel*$C475),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D475-(D_Ver_R_3/D_Ver_Vvel*$C475+D_ver_a)>0,SQRT(D475-(D_Ver_R_3/D_Ver_Vvel*$C475+D_ver_a)),0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E475)*SQRT(2))))),(IF(AND($E475>0,$F475=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E475)-D_ver_B_3*$E475)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E475)+D_ver_B_3*$E475)*SQRT(2)))*D_Ver_C0_3,IF($F475>0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E475)-D_ver_B_3*$E475)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E475)+D_ver_B_3*$E475)*SQRT(2)))-(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F475)-D_ver_B_3*$F475)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F475)+D_ver_B_3*$F475)*SQRT(2))))*D_Ver_C0_3,0)))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E$475)*SQRT(2))))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP(D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($F$475>0,0.5*EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP(D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP(D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3,0))))","v":0},{"$f":"IF(D_vert_AC,0,IF(AND($E475>0,$F475=0),0.5*EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E475)-D_ver_B_3*$E475)*SQRT(2))+EXP(D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E475)+D_ver_B_3*$E475)*SQRT(2)))*D_Ver_C0_3,IF($F475>0,0.5*EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E475)-D_ver_B_3*$E475)*SQRT(2))+EXP(D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$E475)+D_ver_B_3*$E475)*SQRT(2)))-(EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$F475)-D_ver_B_3*$F475)*SQRT(2))+EXP(D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/(2*D_ver_A_3*$F475)+D_ver_B_3*$F475)*SQRT(2))))*D_Ver_C0_3,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D475/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E475)*SQRT(2)))),IF(AND($E475>0,$F475=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E475)-D_ver_B_3*$E475)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E475)+D_ver_B_3*$E475)*SQRT(2)))*D_Ver_C0_3,IF($E475=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E475)-D_ver_B_3*$E475)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E475)+D_ver_B_3*$E475)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F475)-D_ver_B_3*$F475)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F475)+D_ver_B_3*$F475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C475/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_3*EXP(D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_3*EXP(D_Ver_lambdayear_3*$C475/D_Ver_Vvel)*EXP(-D_Ver_R_3*$C475/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_3*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3)))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_3),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D475/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z-D_ver_EPM*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*Ver_z+D_ver_EPM*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z475*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))+EXP((D_ver_EPM+$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z475*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))),(IF($D475<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z475*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))+EXP((D_ver_EPM+$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z475*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z475*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))+EXP((D_ver_EPM+$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z475*$D475)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))-EXP((D_ver_EPM-$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z475*($D475-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D475-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z475)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z475*($D475-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D475-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C475-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C475/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*$C475+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$Z475*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$Z475*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$Z475*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$Z475*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$Z475*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$Z475*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$Z475*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z475)*$C475/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$Z475*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3))","v":0},{"$f":"IF( D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_3),0))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D475/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z)/2*SQRT((D_Ver_R_3*$D475))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_3/2*(EXP((-$AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD475*$D475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))+EXP(($AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD475*$D475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D475<=D_ver_a,\nD_Ver_C0_3/2*(EXP((-$AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD475*$D475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))+EXP(($AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD475*$D475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))),\nD_Ver_C0_3/2*(EXP((-$AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD475*$D475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))+EXP(($AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD475*$D475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D475)))*SQRT(2))-EXP((-$AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD475*($D475-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D475-D_ver_a))))*SQRT(2))-EXP(($AD475)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD475*($D475-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D475-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C475)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_3*$C475)/2*SQRT((D_Ver_R_3*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_3/2*(EXP((-$AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$AD475*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$AD475*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_3/2*(EXP((-$AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$AD475*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$AD475*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),\nD_Ver_C0_3/2*(EXP((-$AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$AD475*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$AD475*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((-$AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475-$AD475*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD475)*$C475/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C475+$AD475*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C475)+D_Ver_lambdayear_3)/D_Ver_R_3*$D475)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C475)+D_Ver_lambdayear_3)/D_Ver_R_3*Ver_t)),))","v":0}]
[null,null,0,{"$f":"0","v":0},{"$error":"#VALUE!"},0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D476/D_Ver_R_3))),(IF(AND($E476>0,$F476=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E476)-D_ver_B_3*$E476)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E476)+D_ver_B_3*$E476)*SQRT(2)))*D_Ver_C0_3,IF($F476>0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E476)-D_ver_B_3*$E476)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E476)+D_ver_B_3*$E476)*SQRT(2)))-(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F476)-D_ver_B_3*$F476)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F476)+D_ver_B_3*$F476)*SQRT(2))))*D_Ver_C0_3,0)))))","v":0},0,{"$f":"IF(D_vert_AC,0,IF(AND($E476>0,$F476=0),0.5*EXP(-D_Ver_lambdayear_3*$C476/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C476/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C476/D_Ver_Vvel/(2*D_ver_A_3*$E476)-D_ver_B_3*$E476)*SQRT(2))+EXP(D_Ver_R_3*$C476/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C476/D_Ver_Vvel/(2*D_ver_A_3*$E476)+D_ver_B_3*$E476)*SQRT(2)))*D_Ver_C0_3,IF($F476>0,0.5*EXP(-D_Ver_lambdayear_3*$C476/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C476/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C476/D_Ver_Vvel/(2*D_ver_A_3*$E476)-D_ver_B_3*$E476)*SQRT(2))+EXP(D_Ver_R_3*$C476/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C476/D_Ver_Vvel/(2*D_ver_A_3*$E476)+D_ver_B_3*$E476)*SQRT(2)))-(EXP(-D_Ver_R_3*$C476/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C476/D_Ver_Vvel/(2*D_ver_A_3*$F476)-D_ver_B_3*$F476)*SQRT(2))+EXP(D_Ver_R_3*$C476/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C476/D_Ver_Vvel/(2*D_ver_A_3*$F476)+D_ver_B_3*$F476)*SQRT(2))))*D_Ver_C0_3,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D476/D_Ver_R_3))),IF(AND($E476>0,$F476=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E476)-D_ver_B_3*$E476)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E476)+D_ver_B_3*$E476)*SQRT(2)))*D_Ver_C0_3,IF($E476=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E476)-D_ver_B_3*$E476)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E476)+D_ver_B_3*$E476)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F476)-D_ver_B_3*$F476)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F476)+D_ver_B_3*$F476)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_3*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3)))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_3),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z476*$D476)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D476)))*SQRT(2))+EXP((D_ver_EPM+$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z476*$D476)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D476)))*SQRT(2))),(IF($D476<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z476*$D476)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D476)))*SQRT(2))+EXP((D_ver_EPM+$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z476*$D476)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D476)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z476*$D476)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D476)))*SQRT(2))+EXP((D_ver_EPM+$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z476*$D476)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D476)))*SQRT(2))-EXP((D_ver_EPM-$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z476*($D476-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D476-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z476)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z476*($D476-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D476-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476-$Z476*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476+$Z476*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476-$Z476*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476+$Z476*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476-$Z476*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476+$Z476*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476-$Z476*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z476)*$C476/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C476+$Z476*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_3),0))","v":0},0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_3)/D_Ver_R_3*$D476)),))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,IF(C476=0,D_Ver_C0_3,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C476)+D_Ver_lambdayear_3)/D_Ver_R_3*Ver_t))),))","v":0}]
[null,null,{"$f":"0+D_ver_z_incr","v":0},{"$f":"0+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D477/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E477^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E477)*SQRT(2))))),(IF(AND($E477>0,$F477=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E477)-D_ver_B_3*$E477)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E477)+D_ver_B_3*$E477)*SQRT(2)))*D_Ver_C0_3,IF($F477>0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E477)-D_ver_B_3*$E477)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E477)+D_ver_B_3*$E477)*SQRT(2)))-(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F477)-D_ver_B_3*$F477)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F477)+D_ver_B_3*$F477)*SQRT(2))))*D_Ver_C0_3,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E477>0,$F477=0),0.5*EXP(-D_Ver_lambdayear_3*$C477/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C477/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C477/D_Ver_Vvel/(2*D_ver_A_3*$E477)-D_ver_B_3*$E477)*SQRT(2))+EXP(D_Ver_R_3*$C477/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C477/D_Ver_Vvel/(2*D_ver_A_3*$E477)+D_ver_B_3*$E477)*SQRT(2)))*D_Ver_C0_3,IF($F477>0,0.5*EXP(-D_Ver_lambdayear_3*$C477/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C477/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C477/D_Ver_Vvel/(2*D_ver_A_3*$E477)-D_ver_B_3*$E477)*SQRT(2))+EXP(D_Ver_R_3*$C477/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C477/D_Ver_Vvel/(2*D_ver_A_3*$E477)+D_ver_B_3*$E477)*SQRT(2)))-(EXP(-D_Ver_R_3*$C477/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C477/D_Ver_Vvel/(2*D_ver_A_3*$F477)-D_ver_B_3*$F477)*SQRT(2))+EXP(D_Ver_R_3*$C477/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C477/D_Ver_Vvel/(2*D_ver_A_3*$F477)+D_ver_B_3*$F477)*SQRT(2))))*D_Ver_C0_3,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D477/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E477^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E477)*SQRT(2)))),IF(AND($E477>0,$F477=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E477)-D_ver_B_3*$E477)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E477)+D_ver_B_3*$E477)*SQRT(2)))*D_Ver_C0_3,IF($E477=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E477)-D_ver_B_3*$E477)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E477)+D_ver_B_3*$E477)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F477)-D_ver_B_3*$F477)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F477)+D_ver_B_3*$F477)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))),(IF($D477<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))-EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*($D477-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D477-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*($D477-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D477-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D477/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z-D_ver_EPM*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*Ver_z+D_ver_EPM*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))),(IF($D477<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z477*$D477)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))-EXP((D_ver_EPM-$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z477*($D477-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D477-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z477)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z477*($D477-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D477-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C477-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C477/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*$C477+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$Z477*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z477)*$C477/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$Z477*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3))","v":0},{"$f":"IF( D_vert_AC,0,IF($D477<=D_ver_a,D_Ver_C0_3/2*(EXP((-$AD477)*$C477/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$AD477*$D477)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP(($AD477)*$C477/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$AD477*$D477)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))),D_Ver_C0_3/2*(EXP((-$AD477)*$C477/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$AD477*$D477)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))+EXP(($AD477)*$C477/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$AD477*$D477)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D477)))*SQRT(2))-EXP((-$AD477)*$C477/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477-$AD477*($D477-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D477-D_ver_a))))*SQRT(2))-EXP(($AD477)*$C477/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C477+$AD477*($D477-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D477-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_3)/D_Ver_R_3*$D477)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C477)+D_Ver_lambdayear_3)/D_Ver_R_3*Ver_t)),))","v":0}]
[null,null,{"$f":"C477+D_ver_z_incr","v":0},{"$f":"D477+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C485/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C485/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C485/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C485/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D487/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E487^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E487)*SQRT(2)))),IF(AND($E487>0,$F487=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E487)-D_ver_B_3*$E487)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E487)+D_ver_B_3*$E487)*SQRT(2)))*D_Ver_C0_3,IF($E487=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E487)-D_ver_B_3*$E487)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E487)+D_ver_B_3*$E487)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F487)-D_ver_B_3*$F487)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F487)+D_ver_B_3*$F487)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C495/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C495/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C495/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C495/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D497/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E497^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E497)*SQRT(2)))),IF(AND($E497>0,$F497=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E497)-D_ver_B_3*$E497)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E497)+D_ver_B_3*$E497)*SQRT(2)))*D_Ver_C0_3,IF($E497=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E497)-D_ver_B_3*$E497)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E497)+D_ver_B_3*$E497)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F497)-D_ver_B_3*$F497)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F497)+D_ver_B_3*$F497)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C505/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C505/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C505/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C505/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D507-D_Ver_R_3/D_Ver_Vvel*$C507))>0,SQRT(D507-D_Ver_R_3/D_Ver_Vvel*$C507),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D507-(D_Ver_R_3/D_Ver_Vvel*$C507+D_ver_a)>0,SQRT(D507-(D_Ver_R_3/D_Ver_Vvel*$C507+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C507/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$E$475)*SQRT(2))))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C507/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP(D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($F$475>0,0.5*EXP(-D_Ver_lambdayear_3*$C507/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP(D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP(D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C507/D_Ver_Vvel/(2*D_ver_A_3*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3,0))))","v":0},0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D507/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E507^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E507)*SQRT(2)))),IF(AND($E507>0,$F507=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E507)-D_ver_B_3*$E507)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E507)+D_ver_B_3*$E507)*SQRT(2)))*D_Ver_C0_3,IF($E507=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E507)-D_ver_B_3*$E507)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E507)+D_ver_B_3*$E507)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F507)-D_ver_B_3*$F507)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F507)+D_ver_B_3*$F507)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_3*EXP(D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_3*EXP(D_Ver_lambdayear_3*$C507/D_Ver_Vvel)*EXP(-D_Ver_R_3*$C507/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_3*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3)))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D507/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z)/2*SQRT((D_Ver_R_3*$D507))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_3/2*(EXP((-$AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD507*$D507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507)))*SQRT(2))+EXP(($AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD507*$D507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D507<=D_ver_a,\nD_Ver_C0_3/2*(EXP((-$AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD507*$D507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507)))*SQRT(2))+EXP(($AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD507*$D507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507)))*SQRT(2))),\nD_Ver_C0_3/2*(EXP((-$AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD507*$D507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507)))*SQRT(2))+EXP(($AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD507*$D507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D507)))*SQRT(2))-EXP((-$AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD507*($D507-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D507-D_ver_a))))*SQRT(2))-EXP(($AD507)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD507*($D507-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D507-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C507)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_3*$C507)/2*SQRT((D_Ver_R_3*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_3/2*(EXP((-$AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507-$AD507*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507+$AD507*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_3/2*(EXP((-$AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507-$AD507*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507+$AD507*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),\nD_Ver_C0_3/2*(EXP((-$AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507-$AD507*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507+$AD507*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((-$AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507-$AD507*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD507)*$C507/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C507+$AD507*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D509/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E509^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E509)*SQRT(2))))),(IF(AND($E509>0,$F509=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E509)-D_ver_B_3*$E509)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E509)+D_ver_B_3*$E509)*SQRT(2)))*D_Ver_C0_3,IF($F509>0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E509)-D_ver_B_3*$E509)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E509)+D_ver_B_3*$E509)*SQRT(2)))-(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F509)-D_ver_B_3*$F509)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F509)+D_ver_B_3*$F509)*SQRT(2))))*D_Ver_C0_3,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E509>0,$F509=0),0.5*EXP(-D_Ver_lambdayear_3*$C509/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C509/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C509/D_Ver_Vvel/(2*D_ver_A_3*$E509)-D_ver_B_3*$E509)*SQRT(2))+EXP(D_Ver_R_3*$C509/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C509/D_Ver_Vvel/(2*D_ver_A_3*$E509)+D_ver_B_3*$E509)*SQRT(2)))*D_Ver_C0_3,IF($F509>0,0.5*EXP(-D_Ver_lambdayear_3*$C509/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C509/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C509/D_Ver_Vvel/(2*D_ver_A_3*$E509)-D_ver_B_3*$E509)*SQRT(2))+EXP(D_Ver_R_3*$C509/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C509/D_Ver_Vvel/(2*D_ver_A_3*$E509)+D_ver_B_3*$E509)*SQRT(2)))-(EXP(-D_Ver_R_3*$C509/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C509/D_Ver_Vvel/(2*D_ver_A_3*$F509)-D_ver_B_3*$F509)*SQRT(2))+EXP(D_Ver_R_3*$C509/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C509/D_Ver_Vvel/(2*D_ver_A_3*$F509)+D_ver_B_3*$F509)*SQRT(2))))*D_Ver_C0_3,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))),(IF($D509<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))-EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*($D509-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D509-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*($D509-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D509-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D509/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z-D_ver_EPM*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*Ver_z+D_ver_EPM*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))),(IF($D509<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z509*$D509)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))-EXP((D_ver_EPM-$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z509*($D509-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D509-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z509)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z509*($D509-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D509-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C509-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C509/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*$C509+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$Z509*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z509)*$C509/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$Z509*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3))","v":0},{"$f":"IF( D_vert_AC,0,IF($D509<=D_ver_a,D_Ver_C0_3/2*(EXP((-$AD509)*$C509/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$AD509*$D509)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP(($AD509)*$C509/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$AD509*$D509)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))),D_Ver_C0_3/2*(EXP((-$AD509)*$C509/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$AD509*$D509)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))+EXP(($AD509)*$C509/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$AD509*$D509)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D509)))*SQRT(2))-EXP((-$AD509)*$C509/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509-$AD509*($D509-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D509-D_ver_a))))*SQRT(2))-EXP(($AD509)*$C509/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C509+$AD509*($D509-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D509-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_3)/D_Ver_R_3*$D509)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C509)+D_Ver_lambdayear_3)/D_Ver_R_3*Ver_t)),))","v":0}]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C515/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C515/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C515/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C515/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D517/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E517^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E517)*SQRT(2)))),IF(AND($E517>0,$F517=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E517)-D_ver_B_3*$E517)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E517)+D_ver_B_3*$E517)*SQRT(2)))*D_Ver_C0_3,IF($E517=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E517)-D_ver_B_3*$E517)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E517)+D_ver_B_3*$E517)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F517)-D_ver_B_3*$F517)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F517)+D_ver_B_3*$F517)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C525/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C525/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C525/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C525/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D527/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E527^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E527)*SQRT(2)))),IF(AND($E527>0,$F527=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E527)-D_ver_B_3*$E527)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E527)+D_ver_B_3*$E527)*SQRT(2)))*D_Ver_C0_3,IF($E527=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E527)-D_ver_B_3*$E527)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E527)+D_ver_B_3*$E527)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F527)-D_ver_B_3*$F527)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F527)+D_ver_B_3*$F527)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C535/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C535/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C535/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C535/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D537/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E537^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E537)*SQRT(2)))),IF(AND($E537>0,$F537=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E537)-D_ver_B_3*$E537)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E537)+D_ver_B_3*$E537)*SQRT(2)))*D_Ver_C0_3,IF($E537=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E537)-D_ver_B_3*$E537)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E537)+D_ver_B_3*$E537)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F537)-D_ver_B_3*$F537)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F537)+D_ver_B_3*$F537)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D539-D_Ver_R_3/D_Ver_Vvel*$C539))>0,SQRT(D539-D_Ver_R_3/D_Ver_Vvel*$C539),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D539-(D_Ver_R_3/D_Ver_Vvel*$C539+D_ver_a)>0,SQRT(D539-(D_Ver_R_3/D_Ver_Vvel*$C539+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C539/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$E$475)*SQRT(2))))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C539/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP(D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($F$475>0,0.5*EXP(-D_Ver_lambdayear_3*$C539/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP(D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP(D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C539/D_Ver_Vvel/(2*D_ver_A_3*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3,0))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_3*EXP(D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_3*EXP(D_Ver_lambdayear_3*$C539/D_Ver_Vvel)*EXP(-D_Ver_R_3*$C539/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_3*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3)))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D539/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z)/2*SQRT((D_Ver_R_3*$D539))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_3/2*(EXP((-$AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD539*$D539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539)))*SQRT(2))+EXP(($AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD539*$D539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D539<=D_ver_a,\nD_Ver_C0_3/2*(EXP((-$AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD539*$D539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539)))*SQRT(2))+EXP(($AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD539*$D539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539)))*SQRT(2))),\nD_Ver_C0_3/2*(EXP((-$AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD539*$D539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539)))*SQRT(2))+EXP(($AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD539*$D539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D539)))*SQRT(2))-EXP((-$AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$AD539*($D539-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D539-D_ver_a))))*SQRT(2))-EXP(($AD539)*Ver_z/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$AD539*($D539-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D539-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C539)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_3*$C539)/2*SQRT((D_Ver_R_3*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_3/2*(EXP((-$AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539-$AD539*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539+$AD539*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_3/2*(EXP((-$AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539-$AD539*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539+$AD539*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),\nD_Ver_C0_3/2*(EXP((-$AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539-$AD539*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP(($AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539+$AD539*Ver_t)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((-$AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539-$AD539*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD539)*$C539/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C539+$AD539*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D541/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E541^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E541)*SQRT(2))))),(IF(AND($E541>0,$F541=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E541)-D_ver_B_3*$E541)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E541)+D_ver_B_3*$E541)*SQRT(2)))*D_Ver_C0_3,IF($F541>0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E541)-D_ver_B_3*$E541)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$E541)+D_ver_B_3*$E541)*SQRT(2)))-(EXP(-D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F541)-D_ver_B_3*$F541)*SQRT(2))+EXP(D_Ver_R_3*Ver_z/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/(2*D_ver_A_3*$F541)+D_ver_B_3*$F541)*SQRT(2))))*D_Ver_C0_3,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E541>0,$F541=0),0.5*EXP(-D_Ver_lambdayear_3*$C541/D_Ver_Vvel)*(EXP(-D_Ver_R_3*$C541/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C541/D_Ver_Vvel/(2*D_ver_A_3*$E541)-D_ver_B_3*$E541)*SQRT(2))+EXP(D_Ver_R_3*$C541/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C541/D_Ver_Vvel/(2*D_ver_A_3*$E541)+D_ver_B_3*$E541)*SQRT(2)))*D_Ver_C0_3,IF($F541>0,0.5*EXP(-D_Ver_lambdayear_3*$C541/D_Ver_Vvel)*((EXP(-D_Ver_R_3*$C541/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C541/D_Ver_Vvel/(2*D_ver_A_3*$E541)-D_ver_B_3*$E541)*SQRT(2))+EXP(D_Ver_R_3*$C541/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C541/D_Ver_Vvel/(2*D_ver_A_3*$E541)+D_ver_B_3*$E541)*SQRT(2)))-(EXP(-D_Ver_R_3*$C541/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C541/D_Ver_Vvel/(2*D_ver_A_3*$F541)-D_ver_B_3*$F541)*SQRT(2))+EXP(D_Ver_R_3*$C541/D_Ver_Vvel*D_ver_B_3/D_ver_A_3)*2*NORMSDIST(-(D_Ver_R_3*$C541/D_Ver_Vvel/(2*D_ver_A_3*$F541)+D_ver_B_3*$F541)*SQRT(2))))*D_Ver_C0_3,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))),(IF($D541<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))-EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*($D541-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D541-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*($D541-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D541-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*$D541/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*Ver_z-D_ver_EPM*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*Ver_z+D_ver_EPM*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))),(IF($D541<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z541*$D541)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))-EXP((D_ver_EPM-$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z-$Z541*($D541-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D541-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z541)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*Ver_z+$Z541*($D541-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*($D541-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)*(1-0.5*2*NORMSDIST(-(D_Ver_R_3*$C541-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C541/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-(D_Ver_R_3*$C541+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))),D_Ver_C0_3/2*(EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$Z541*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z541)*$C541/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$Z541*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_3)*D_Ver_R_3*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_3*D_ver_Ddwm_3))","v":0},{"$f":"IF( D_vert_AC,0,IF($D541<=D_ver_a,D_Ver_C0_3/2*(EXP((-$AD541)*$C541/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$AD541*$D541)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP(($AD541)*$C541/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$AD541*$D541)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))),D_Ver_C0_3/2*(EXP((-$AD541)*$C541/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$AD541*$D541)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))+EXP(($AD541)*$C541/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$AD541*$D541)/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*$D541)))*SQRT(2))-EXP((-$AD541)*$C541/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541-$AD541*($D541-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D541-D_ver_a))))*SQRT(2))-EXP(($AD541)*$C541/(2*(D_ver_Ddwm_3)))*2*NORMSDIST(-((D_Ver_R_3*$C541+$AD541*($D541-D_ver_a))/(2*SQRT((D_ver_Ddwm_3)*D_Ver_R_3*($D541-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_3)/D_Ver_R_3*$D541)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C541)+D_Ver_lambdayear_3)/D_Ver_R_3*Ver_t)),))","v":0}]
[null,null,{"$f":"C541+D_ver_z_incr","v":0},{"$f":"D541+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*Ver_t/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*$C545/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E$475^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)*SQRT(2)))),IF(AND($E$475>0,$F$475=0),0.5*EXP(-D_Ver_lambdayear_3*$C545/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))*D_Ver_C0_3,IF($E$475=0,0,0.5*EXP(-D_Ver_lambdayear_3*$C545/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)-D_ver_B_3*$E$475)*SQRT(2))+EXP((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$E$475)+D_ver_B_3*$E$475)*SQRT(2)))-(EXP(-(D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)-D_ver_B_3*$F$475)*SQRT(2))+EXP((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*$C545/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*Q$474)/(2*$F$475)+D_ver_B_3*$F$475)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_3*(EXP(-D_Ver_lambdayear_3*$D547/D_Ver_R_3)-EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_3*$E547^2/D_Ver_R_3)*2*NORMSDIST(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E547)*SQRT(2)))),IF(AND($E547>0,$F547=0),0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E547)-D_ver_B_3*$E547)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E547)+D_ver_B_3*$E547)*SQRT(2)))*D_Ver_C0_3,IF($E547=0,0,0.5*EXP(-D_Ver_lambdayear_3*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E547)-D_ver_B_3*$E547)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$E547)+D_ver_B_3*$E547)*SQRT(2)))-(EXP(-(D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F547)-D_ver_B_3*$F547)*SQRT(2))+EXP((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)*D_ver_B_3)*2*NORMSDIST(-((D_Ver_R_3*Ver_z/D_Ver_Vvel/D_ver_A_3+D_ver_G_3*J$474)/(2*$F547)+D_ver_B_3*$F547)*SQRT(2))))*D_Ver_C0_3))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,null,"Stof 4",{"$f":"D_Ver_stofnavn_4","v":""},null,null,null,{"$f":"CONCATENATE(\"Stationær konc. \",E558,\" m´s dybder\")","v":"Stationær konc.  m´s dybder"},null,null,{"$f":"IF(D_vert_DTU_1b,B_ver_Cz_DTU_4,\"(ikke stationært)\")","v":"(ikke stationært)"},"mg/l",{"$f":"IF(D_vert_AC,$D$3,IF(D_vert_DTU_1a,$D$4,IF(D_vert_DTU_1b,$D$5,$D$6)))","v":"(Model A + C)"}]
[null,null,null,null,null,null,"Comparison of models",null,null,null,null,null,null,null,null,"Fracture model - Concentration in matrix"]
[]
[null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Sammenligning af modeller\n Koncentration i \",Ver_z,\" m´s dybde\")","v":": Sammenligning af modeller\n Koncentration i  m´s dybde"},null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Sammenligning af modeller\n Koncentration efter \",Ver_t,\" år\")","v":": Sammenligning af modeller\n Koncentration efter  år"},null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Koncentration i matrix i forskellige afstande (m) fra sprækken i \",Ver_z,\" m´s dybde\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken i  m´s dybde"},null,null,null,null,null,{"$f":"CONCATENATE(D_Ver_stofnavn_4,\": Koncentration i matrix i forskellige afstande (m) fra sprækken efter \",Ver_t,\" år\")","v":": Koncentration i matrix i forskellige afstande (m) fra sprækken efter  år"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kun DTU V1D-Model 2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Stationær konc.med tid i \",Ver_z,\" m´s dybde - Kun model 1b\")","v":"Stationær konc.med tid i  m´s dybde - Kun model 1b"},{"$f":"CONCATENATE(\"Stationær konc.i dybde ved tid \",Ver_t,\" år_ kun model 1b\")","v":"Stationær konc.i dybde ved tid  år_ kun model 1b"},null,null,null,null,null,null,null,null,"En aftagnende kilde"]
[null,null,{"$f":"IF( D_vert_DTU_2,\"Ved DTU model 2 skal der ses bort fra de beregnede koncentrationer for udvaskning fra matrix til sprækker ved tider større end\",\"\")","v":""},null,{"$f":"IF(D_vert_DTU_2,(D_Ver_R_4*(D_ver_2B/2)^2)/D_ver_Ddwm_4,\"\")","v":""},{"$f":"IF( D_vert_DTU_2,\"år\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,"Sprækkemodel",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPM model",null,null,null,"Diffusionsmodel",null,null,"1. ordens model"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in fracture with time at depth \",Ver_z,\" m\")","v":"Conc in fracture with time at depth  m"},{"$f":"CONCATENATE(\"Conc in fracture with depth at time \",Ver_t,\" years\")","v":"Conc in fracture with depth at time  years"},"Original Conc in fracture at depth and time",{"$f":"CONCATENATE(\"Conc in matrix with time at \",Ver_z, \" m depth at different distances x m from the fracture\")","v":"Conc in matrix with time at  m depth at different distances x m from the fracture"},null,null,null,null,null,null,{"$f":"CONCATENATE(\"Conc in matrix with depth at \",Ver_t, \" years at different distances x m from the fracture\")","v":"Conc in matrix with depth at  years at different distances x m from the fracture"},null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"EPM with time at depth \",Ver_z,\" m\")","v":"EPM with time at depth  m"},{"$f":"CONCATENATE(\"EPM in depth at time \",Ver_t,\" years\")","v":"EPM in depth at time  years"},null,"No fracture",{"$f":"CONCATENATE(\"Diffusion with time at depth \",Ver_z,\" m\")","v":"Diffusion with time at depth  m"},{"$f":"CONCATENATE(\"Diffusion in depth at time \",Ver_t,\" years\")","v":"Diffusion in depth at time  years"},{"$f":"CONCATENATE(\"1.order with time at depth \",Ver_z,\" m\")","v":"1.order with time at depth  m"},{"$f":"CONCATENATE(\"1.order in depth at time \",Ver_t,\" years\")","v":"1.order in depth at time  years"}]
[null,null,"z (depth)","t (time)","T'","T''",null,null,null,0.1,0.2,0.3,0.4,0.5,0.75,1,0.1,0.2,0.3,0.4,0.5,0.75,1,"Stationær konc.","Stationær konc.","u1",null,null,null,"u2","No advection"]
[null,null,{"$f":"Ver_z","v":0},{"$f":"Ver_t","v":0},{"$f":"IF((SQRT(D593-D_Ver_R_4/D_Ver_Vvel*$C593))>0,SQRT(D593-D_Ver_R_4/D_Ver_Vvel*$C593),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D593-(D_Ver_R_4/D_Ver_Vvel*$C593+D_ver_a)>0,SQRT(D593-(D_Ver_R_4/D_Ver_Vvel*$C593+D_ver_a)),0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E593)*SQRT(2))))),(IF(AND($E593>0,$F593=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E593)-D_ver_B_4*$E593)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E593)+D_ver_B_4*$E593)*SQRT(2)))*D_Ver_C0_4,IF($F593>0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E593)-D_ver_B_4*$E593)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E593)+D_ver_B_4*$E593)*SQRT(2)))-(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F593)-D_ver_B_4*$F593)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F593)+D_ver_B_4*$F593)*SQRT(2))))*D_Ver_C0_4,0)))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E$593)*SQRT(2))))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP(D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($F$593>0,0.5*EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP(D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP(D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4,0))))","v":0},{"$f":"IF(D_vert_AC,0,IF(AND($E593>0,$F593=0),0.5*EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E593)-D_ver_B_4*$E593)*SQRT(2))+EXP(D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E593)+D_ver_B_4*$E593)*SQRT(2)))*D_Ver_C0_4,IF($F593>0,0.5*EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E593)-D_ver_B_4*$E593)*SQRT(2))+EXP(D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$E593)+D_ver_B_4*$E593)*SQRT(2)))-(EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$F593)-D_ver_B_4*$F593)*SQRT(2))+EXP(D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/(2*D_ver_A_4*$F593)+D_ver_B_4*$F593)*SQRT(2))))*D_Ver_C0_4,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D593/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E593)*SQRT(2)))),IF(AND($E593>0,$F593=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E593)-D_ver_B_4*$E593)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E593)+D_ver_B_4*$E593)*SQRT(2)))*D_Ver_C0_4,IF($E593=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E593)-D_ver_B_4*$E593)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E593)+D_ver_B_4*$E593)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F593)-D_ver_B_4*$F593)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F593)+D_ver_B_4*$F593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C593/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_4*EXP(D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_4*EXP(D_Ver_lambdayear_4*$C593/D_Ver_Vvel)*EXP(-D_Ver_R_4*$C593/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_4*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4)))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_4),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D593/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z-D_ver_EPM*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*Ver_z+D_ver_EPM*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z593*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))+EXP((D_ver_EPM+$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z593*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))),(IF($D593<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z593*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))+EXP((D_ver_EPM+$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z593*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z593*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))+EXP((D_ver_EPM+$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z593*$D593)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))-EXP((D_ver_EPM-$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z593*($D593-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D593-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z593)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z593*($D593-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D593-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C593-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C593/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*$C593+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$Z593*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$Z593*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$Z593*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$Z593*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$Z593*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$Z593*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$Z593*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z593)*$C593/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$Z593*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4))","v":0},{"$f":"IF( D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_4),0))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D593/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z)/2*SQRT((D_Ver_R_4*$D593))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_4/2*(EXP((-$AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD593*$D593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))+EXP(($AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD593*$D593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D593<=D_ver_a,\nD_Ver_C0_4/2*(EXP((-$AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD593*$D593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))+EXP(($AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD593*$D593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))),\nD_Ver_C0_4/2*(EXP((-$AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD593*$D593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))+EXP(($AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD593*$D593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D593)))*SQRT(2))-EXP((-$AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD593*($D593-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D593-D_ver_a))))*SQRT(2))-EXP(($AD593)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD593*($D593-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D593-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C593)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_4*$C593)/2*SQRT((D_Ver_R_4*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_4/2*(EXP((-$AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$AD593*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$AD593*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_4/2*(EXP((-$AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$AD593*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$AD593*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),\nD_Ver_C0_4/2*(EXP((-$AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$AD593*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$AD593*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((-$AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593-$AD593*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD593)*$C593/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C593+$AD593*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C593)+D_Ver_lambdayear_4)/D_Ver_R_4*$D593)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C593)+D_Ver_lambdayear_4)/D_Ver_R_4*Ver_t)),))","v":0}]
[null,null,0,{"$f":"0","v":0},{"$error":"#VALUE!"},0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D594/D_Ver_R_4))),(IF(AND($E594>0,$F594=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E594)-D_ver_B_4*$E594)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E594)+D_ver_B_4*$E594)*SQRT(2)))*D_Ver_C0_4,IF($F594>0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E594)-D_ver_B_4*$E594)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E594)+D_ver_B_4*$E594)*SQRT(2)))-(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F594)-D_ver_B_4*$F594)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F594)+D_ver_B_4*$F594)*SQRT(2))))*D_Ver_C0_4,0)))))","v":0},0,{"$f":"IF(D_vert_AC,0,IF(AND($E594>0,$F594=0),0.5*EXP(-D_Ver_lambdayear_4*$C594/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C594/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C594/D_Ver_Vvel/(2*D_ver_A_4*$E594)-D_ver_B_4*$E594)*SQRT(2))+EXP(D_Ver_R_4*$C594/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C594/D_Ver_Vvel/(2*D_ver_A_4*$E594)+D_ver_B_4*$E594)*SQRT(2)))*D_Ver_C0_4,IF($F594>0,0.5*EXP(-D_Ver_lambdayear_4*$C594/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C594/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C594/D_Ver_Vvel/(2*D_ver_A_4*$E594)-D_ver_B_4*$E594)*SQRT(2))+EXP(D_Ver_R_4*$C594/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C594/D_Ver_Vvel/(2*D_ver_A_4*$E594)+D_ver_B_4*$E594)*SQRT(2)))-(EXP(-D_Ver_R_4*$C594/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C594/D_Ver_Vvel/(2*D_ver_A_4*$F594)-D_ver_B_4*$F594)*SQRT(2))+EXP(D_Ver_R_4*$C594/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C594/D_Ver_Vvel/(2*D_ver_A_4*$F594)+D_ver_B_4*$F594)*SQRT(2))))*D_Ver_C0_4,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D594/D_Ver_R_4))),IF(AND($E594>0,$F594=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E594)-D_ver_B_4*$E594)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E594)+D_ver_B_4*$E594)*SQRT(2)))*D_Ver_C0_4,IF($E594=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E594)-D_ver_B_4*$E594)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E594)+D_ver_B_4*$E594)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F594)-D_ver_B_4*$F594)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F594)+D_ver_B_4*$F594)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_4),0))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z594*$D594)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D594)))*SQRT(2))+EXP((D_ver_EPM+$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z594*$D594)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D594)))*SQRT(2))),(IF($D594<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z594*$D594)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D594)))*SQRT(2))+EXP((D_ver_EPM+$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z594*$D594)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D594)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z594*$D594)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D594)))*SQRT(2))+EXP((D_ver_EPM+$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z594*$D594)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D594)))*SQRT(2))-EXP((D_ver_EPM-$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z594*($D594-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D594-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z594)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z594*($D594-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D594-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594-$Z594*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594+$Z594*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594-$Z594*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594+$Z594*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594-$Z594*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594+$Z594*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594-$Z594*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z594)*$C594/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C594+$Z594*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_AC,0,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4))","v":0},{"$f":"IF(D_vert_AC,0,IF(Ver_z=0,IF(Ver_t>D_ver_a,0,D_Ver_C0_4),0))","v":0},0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_4)/D_Ver_R_4*$D594)),))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,IF(C594=0,D_Ver_C0_4,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C594)+D_Ver_lambdayear_4)/D_Ver_R_4*Ver_t))),))","v":0}]
[null,null,{"$f":"0+D_ver_z_incr","v":0},{"$f":"0+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D595/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E595^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E595)*SQRT(2))))),(IF(AND($E595>0,$F595=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E595)-D_ver_B_4*$E595)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E595)+D_ver_B_4*$E595)*SQRT(2)))*D_Ver_C0_4,IF($F595>0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E595)-D_ver_B_4*$E595)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E595)+D_ver_B_4*$E595)*SQRT(2)))-(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F595)-D_ver_B_4*$F595)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F595)+D_ver_B_4*$F595)*SQRT(2))))*D_Ver_C0_4,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E595>0,$F595=0),0.5*EXP(-D_Ver_lambdayear_4*$C595/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C595/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C595/D_Ver_Vvel/(2*D_ver_A_4*$E595)-D_ver_B_4*$E595)*SQRT(2))+EXP(D_Ver_R_4*$C595/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C595/D_Ver_Vvel/(2*D_ver_A_4*$E595)+D_ver_B_4*$E595)*SQRT(2)))*D_Ver_C0_4,IF($F595>0,0.5*EXP(-D_Ver_lambdayear_4*$C595/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C595/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C595/D_Ver_Vvel/(2*D_ver_A_4*$E595)-D_ver_B_4*$E595)*SQRT(2))+EXP(D_Ver_R_4*$C595/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C595/D_Ver_Vvel/(2*D_ver_A_4*$E595)+D_ver_B_4*$E595)*SQRT(2)))-(EXP(-D_Ver_R_4*$C595/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C595/D_Ver_Vvel/(2*D_ver_A_4*$F595)-D_ver_B_4*$F595)*SQRT(2))+EXP(D_Ver_R_4*$C595/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C595/D_Ver_Vvel/(2*D_ver_A_4*$F595)+D_ver_B_4*$F595)*SQRT(2))))*D_Ver_C0_4,0)))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D595/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E595^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E595)*SQRT(2)))),IF(AND($E595>0,$F595=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E595)-D_ver_B_4*$E595)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E595)+D_ver_B_4*$E595)*SQRT(2)))*D_Ver_C0_4,IF($E595=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E595)-D_ver_B_4*$E595)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E595)+D_ver_B_4*$E595)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F595)-D_ver_B_4*$F595)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F595)+D_ver_B_4*$F595)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))),(IF($D595<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))-EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*($D595-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D595-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*($D595-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D595-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D595/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z-D_ver_EPM*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*Ver_z+D_ver_EPM*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))),(IF($D595<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z595*$D595)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))-EXP((D_ver_EPM-$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z595*($D595-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D595-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z595)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z595*($D595-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D595-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C595-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C595/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*$C595+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$Z595*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z595)*$C595/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$Z595*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4))","v":0},{"$f":"IF( D_vert_AC,0,IF($D595<=D_ver_a,D_Ver_C0_4/2*(EXP((-$AD595)*$C595/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$AD595*$D595)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP(($AD595)*$C595/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$AD595*$D595)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))),D_Ver_C0_4/2*(EXP((-$AD595)*$C595/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$AD595*$D595)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))+EXP(($AD595)*$C595/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$AD595*$D595)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D595)))*SQRT(2))-EXP((-$AD595)*$C595/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595-$AD595*($D595-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D595-D_ver_a))))*SQRT(2))-EXP(($AD595)*$C595/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C595+$AD595*($D595-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D595-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_4)/D_Ver_R_4*$D595)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C595)+D_Ver_lambdayear_4)/D_Ver_R_4*Ver_t)),))","v":0}]
[null,null,{"$f":"C595+D_ver_z_incr","v":0},{"$f":"D595+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C603/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C603/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C603/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C603/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D605/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E605^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E605)*SQRT(2)))),IF(AND($E605>0,$F605=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E605)-D_ver_B_4*$E605)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E605)+D_ver_B_4*$E605)*SQRT(2)))*D_Ver_C0_4,IF($E605=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E605)-D_ver_B_4*$E605)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E605)+D_ver_B_4*$E605)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F605)-D_ver_B_4*$F605)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F605)+D_ver_B_4*$F605)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C613/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C613/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C613/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C613/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D615/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E615^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E615)*SQRT(2)))),IF(AND($E615>0,$F615=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E615)-D_ver_B_4*$E615)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E615)+D_ver_B_4*$E615)*SQRT(2)))*D_Ver_C0_4,IF($E615=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E615)-D_ver_B_4*$E615)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E615)+D_ver_B_4*$E615)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F615)-D_ver_B_4*$F615)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F615)+D_ver_B_4*$F615)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C623/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C623/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C623/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C623/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D625-D_Ver_R_4/D_Ver_Vvel*$C625))>0,SQRT(D625-D_Ver_R_4/D_Ver_Vvel*$C625),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D625-(D_Ver_R_4/D_Ver_Vvel*$C625+D_ver_a)>0,SQRT(D625-(D_Ver_R_4/D_Ver_Vvel*$C625+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C625/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$E$593)*SQRT(2))))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C625/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP(D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($F$593>0,0.5*EXP(-D_Ver_lambdayear_4*$C625/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP(D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP(D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C625/D_Ver_Vvel/(2*D_ver_A_4*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4,0))))","v":0},0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D625/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E625^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E625)*SQRT(2)))),IF(AND($E625>0,$F625=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E625)-D_ver_B_4*$E625)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E625)+D_ver_B_4*$E625)*SQRT(2)))*D_Ver_C0_4,IF($E625=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E625)-D_ver_B_4*$E625)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E625)+D_ver_B_4*$E625)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F625)-D_ver_B_4*$F625)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F625)+D_ver_B_4*$F625)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_4*EXP(D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_4*EXP(D_Ver_lambdayear_4*$C625/D_Ver_Vvel)*EXP(-D_Ver_R_4*$C625/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_4*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4)))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D625/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z)/2*SQRT((D_Ver_R_4*$D625))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_4/2*(EXP((-$AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD625*$D625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625)))*SQRT(2))+EXP(($AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD625*$D625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D625<=D_ver_a,\nD_Ver_C0_4/2*(EXP((-$AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD625*$D625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625)))*SQRT(2))+EXP(($AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD625*$D625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625)))*SQRT(2))),\nD_Ver_C0_4/2*(EXP((-$AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD625*$D625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625)))*SQRT(2))+EXP(($AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD625*$D625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D625)))*SQRT(2))-EXP((-$AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD625*($D625-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D625-D_ver_a))))*SQRT(2))-EXP(($AD625)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD625*($D625-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D625-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C625)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_4*$C625)/2*SQRT((D_Ver_R_4*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_4/2*(EXP((-$AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625-$AD625*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625+$AD625*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_4/2*(EXP((-$AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625-$AD625*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625+$AD625*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),\nD_Ver_C0_4/2*(EXP((-$AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625-$AD625*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625+$AD625*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((-$AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625-$AD625*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD625)*$C625/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C625+$AD625*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D627/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E627^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E627)*SQRT(2))))),(IF(AND($E627>0,$F627=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E627)-D_ver_B_4*$E627)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E627)+D_ver_B_4*$E627)*SQRT(2)))*D_Ver_C0_4,IF($F627>0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E627)-D_ver_B_4*$E627)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E627)+D_ver_B_4*$E627)*SQRT(2)))-(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F627)-D_ver_B_4*$F627)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F627)+D_ver_B_4*$F627)*SQRT(2))))*D_Ver_C0_4,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E627>0,$F627=0),0.5*EXP(-D_Ver_lambdayear_4*$C627/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C627/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C627/D_Ver_Vvel/(2*D_ver_A_4*$E627)-D_ver_B_4*$E627)*SQRT(2))+EXP(D_Ver_R_4*$C627/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C627/D_Ver_Vvel/(2*D_ver_A_4*$E627)+D_ver_B_4*$E627)*SQRT(2)))*D_Ver_C0_4,IF($F627>0,0.5*EXP(-D_Ver_lambdayear_4*$C627/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C627/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C627/D_Ver_Vvel/(2*D_ver_A_4*$E627)-D_ver_B_4*$E627)*SQRT(2))+EXP(D_Ver_R_4*$C627/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C627/D_Ver_Vvel/(2*D_ver_A_4*$E627)+D_ver_B_4*$E627)*SQRT(2)))-(EXP(-D_Ver_R_4*$C627/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C627/D_Ver_Vvel/(2*D_ver_A_4*$F627)-D_ver_B_4*$F627)*SQRT(2))+EXP(D_Ver_R_4*$C627/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C627/D_Ver_Vvel/(2*D_ver_A_4*$F627)+D_ver_B_4*$F627)*SQRT(2))))*D_Ver_C0_4,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))),(IF($D627<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))-EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*($D627-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D627-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*($D627-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D627-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D627/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z-D_ver_EPM*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*Ver_z+D_ver_EPM*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))),(IF($D627<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z627*$D627)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))-EXP((D_ver_EPM-$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z627*($D627-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D627-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z627)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z627*($D627-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D627-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C627-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C627/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*$C627+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$Z627*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z627)*$C627/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$Z627*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4))","v":0},{"$f":"IF( D_vert_AC,0,IF($D627<=D_ver_a,D_Ver_C0_4/2*(EXP((-$AD627)*$C627/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$AD627*$D627)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP(($AD627)*$C627/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$AD627*$D627)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))),D_Ver_C0_4/2*(EXP((-$AD627)*$C627/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$AD627*$D627)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))+EXP(($AD627)*$C627/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$AD627*$D627)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D627)))*SQRT(2))-EXP((-$AD627)*$C627/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627-$AD627*($D627-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D627-D_ver_a))))*SQRT(2))-EXP(($AD627)*$C627/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C627+$AD627*($D627-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D627-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_4)/D_Ver_R_4*$D627)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C627)+D_Ver_lambdayear_4)/D_Ver_R_4*Ver_t)),))","v":0}]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C633/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C633/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C633/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C633/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D635/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E635^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E635)*SQRT(2)))),IF(AND($E635>0,$F635=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E635)-D_ver_B_4*$E635)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E635)+D_ver_B_4*$E635)*SQRT(2)))*D_Ver_C0_4,IF($E635=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E635)-D_ver_B_4*$E635)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E635)+D_ver_B_4*$E635)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F635)-D_ver_B_4*$F635)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F635)+D_ver_B_4*$F635)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C643/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C643/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C643/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C643/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D645/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E645^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E645)*SQRT(2)))),IF(AND($E645>0,$F645=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E645)-D_ver_B_4*$E645)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E645)+D_ver_B_4*$E645)*SQRT(2)))*D_Ver_C0_4,IF($E645=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E645)-D_ver_B_4*$E645)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E645)+D_ver_B_4*$E645)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F645)-D_ver_B_4*$F645)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F645)+D_ver_B_4*$F645)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C653/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C653/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C653/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C653/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D655/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E655^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E655)*SQRT(2)))),IF(AND($E655>0,$F655=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E655)-D_ver_B_4*$E655)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E655)+D_ver_B_4*$E655)*SQRT(2)))*D_Ver_C0_4,IF($E655=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E655)-D_ver_B_4*$E655)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E655)+D_ver_B_4*$E655)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F655)-D_ver_B_4*$F655)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F655)+D_ver_B_4*$F655)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$f":"IF((SQRT(D657-D_Ver_R_4/D_Ver_Vvel*$C657))>0,SQRT(D657-D_Ver_R_4/D_Ver_Vvel*$C657),0)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_ver_a),0,(IF(D657-(D_Ver_R_4/D_Ver_Vvel*$C657+D_ver_a)>0,SQRT(D657-(D_Ver_R_4/D_Ver_Vvel*$C657+D_ver_a)),0)))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C657/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$E$593)*SQRT(2))))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C657/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP(D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($F$593>0,0.5*EXP(-D_Ver_lambdayear_4*$C657/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP(D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP(D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C657/D_Ver_Vvel/(2*D_ver_A_4*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4,0))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_4*EXP(D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,0,IF(D_vert_DTU_1a,0,(D_Ver_C0_4*EXP(D_Ver_lambdayear_4*$C657/D_Ver_Vvel)*EXP(-D_Ver_R_4*$C657/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)))))","v":0},{"$f":"IF(D_vert_AC,0,IF(D_ver_EPM>0,D_ver_EPM*(1+4*D_Ver_lambdayear_4*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)/D_ver_EPM^2)^0.5,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4)))","v":0},0,0,0,0,0,{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D657/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z)/2*SQRT((D_Ver_R_4*$D657))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_4/2*(EXP((-$AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD657*$D657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657)))*SQRT(2))+EXP(($AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD657*$D657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF($D657<=D_ver_a,\nD_Ver_C0_4/2*(EXP((-$AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD657*$D657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657)))*SQRT(2))+EXP(($AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD657*$D657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657)))*SQRT(2))),\nD_Ver_C0_4/2*(EXP((-$AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD657*$D657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657)))*SQRT(2))+EXP(($AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD657*$D657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D657)))*SQRT(2))-EXP((-$AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$AD657*($D657-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D657-D_ver_a))))*SQRT(2))-EXP(($AD657)*Ver_z/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$AD657*($D657-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D657-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF(D_vert_DTU_2,\nD_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C657)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-(0.5*2*NORMSDIST(-(D_Ver_R_4*$C657)/2*SQRT((D_Ver_R_4*Ver_t))*SQRT(2)))),\nIF(D_vert_DTU_1b,\nD_Ver_C0_4/2*(EXP((-$AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657-$AD657*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657+$AD657*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),\nIF(D_vert_AC,0,\nIF(Ver_t<=D_ver_a,\nD_Ver_C0_4/2*(EXP((-$AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657-$AD657*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657+$AD657*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),\nD_Ver_C0_4/2*(EXP((-$AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657-$AD657*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP(($AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657+$AD657*Ver_t)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((-$AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657-$AD657*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP(($AD657)*$C657/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C657+$AD657*(Ver_t-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))","v":0},0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D659/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E659^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E659)*SQRT(2))))),(IF(AND($E659>0,$F659=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E659)-D_ver_B_4*$E659)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E659)+D_ver_B_4*$E659)*SQRT(2)))*D_Ver_C0_4,IF($F659>0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E659)-D_ver_B_4*$E659)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$E659)+D_ver_B_4*$E659)*SQRT(2)))-(EXP(-D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F659)-D_ver_B_4*$F659)*SQRT(2))+EXP(D_Ver_R_4*Ver_z/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/(2*D_ver_A_4*$F659)+D_ver_B_4*$F659)*SQRT(2))))*D_Ver_C0_4,0)))))","v":0},0,{"$f":"IF( D_vert_AC,0,IF(AND($E659>0,$F659=0),0.5*EXP(-D_Ver_lambdayear_4*$C659/D_Ver_Vvel)*(EXP(-D_Ver_R_4*$C659/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C659/D_Ver_Vvel/(2*D_ver_A_4*$E659)-D_ver_B_4*$E659)*SQRT(2))+EXP(D_Ver_R_4*$C659/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C659/D_Ver_Vvel/(2*D_ver_A_4*$E659)+D_ver_B_4*$E659)*SQRT(2)))*D_Ver_C0_4,IF($F659>0,0.5*EXP(-D_Ver_lambdayear_4*$C659/D_Ver_Vvel)*((EXP(-D_Ver_R_4*$C659/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C659/D_Ver_Vvel/(2*D_ver_A_4*$E659)-D_ver_B_4*$E659)*SQRT(2))+EXP(D_Ver_R_4*$C659/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C659/D_Ver_Vvel/(2*D_ver_A_4*$E659)+D_ver_B_4*$E659)*SQRT(2)))-(EXP(-D_Ver_R_4*$C659/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C659/D_Ver_Vvel/(2*D_ver_A_4*$F659)-D_ver_B_4*$F659)*SQRT(2))+EXP(D_Ver_R_4*$C659/D_Ver_Vvel*D_ver_B_4/D_ver_A_4)*2*NORMSDIST(-(D_Ver_R_4*$C659/D_Ver_Vvel/(2*D_ver_A_4*$F659)+D_ver_B_4*$F659)*SQRT(2))))*D_Ver_C0_4,0)))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF( D_vert_AC,0,IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))),(IF($D659<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))-EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*($D659-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D659-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*($D659-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D659-D_ver_a))))*SQRT(2)))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*$D659/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*Ver_z-D_ver_EPM*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659))*SQRT(2))-0.5*EXP(D_ver_EPM*Ver_z/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*Ver_z+D_ver_EPM*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))),(IF($D659<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z659*$D659)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))-EXP((D_ver_EPM-$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z-$Z659*($D659-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D659-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z659)*Ver_z/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*Ver_z+$Z659*($D659-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*($D659-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)*(1-0.5*2*NORMSDIST(-(D_Ver_R_4*$C659-D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2))-0.5*EXP(D_ver_EPM*$C659/((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-(D_Ver_R_4*$C659+D_ver_EPM*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t))*SQRT(2)))),IF(ISBLANK(D_ver_a),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),(IF(Ver_t<=D_ver_a,D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))),D_Ver_C0_4/2*(EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))+EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*Ver_t)/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*Ver_t)))*SQRT(2))-EXP((D_ver_EPM-$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$Z659*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2))-EXP((D_ver_EPM+$Z659)*$C659/(2*(D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$Z659*(Ver_t-D_ver_a))/(2*SQRT((D_Ver_alfaLw*D_ver_EPM+D_ver_Ddwm_4)*D_Ver_R_4*(Ver_t-D_ver_a))))*SQRT(2)))))))))","v":0},{"$f":"IF( D_vert_AC,0,SQRT(4*D_Ver_lambdayear_4*D_ver_Ddwm_4))","v":0},{"$f":"IF( D_vert_AC,0,IF($D659<=D_ver_a,D_Ver_C0_4/2*(EXP((-$AD659)*$C659/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$AD659*$D659)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP(($AD659)*$C659/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$AD659*$D659)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))),D_Ver_C0_4/2*(EXP((-$AD659)*$C659/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$AD659*$D659)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))+EXP(($AD659)*$C659/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$AD659*$D659)/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*$D659)))*SQRT(2))-EXP((-$AD659)*$C659/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659-$AD659*($D659-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D659-D_ver_a))))*SQRT(2))-EXP(($AD659)*$C659/(2*(D_ver_Ddwm_4)))*2*NORMSDIST(-((D_Ver_R_4*$C659+$AD659*($D659-D_ver_a))/(2*SQRT((D_ver_Ddwm_4)*D_Ver_R_4*($D659-D_ver_a))))*SQRT(2)))))","v":0},0,0,{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*Ver_z)+D_Ver_lambdayear_4)/D_Ver_R_4*$D659)),))","v":0},{"$f":"IF( D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*EXP(-(D_Ver_infil/1000/(D_Ver_ntotal*$C659)+D_Ver_lambdayear_4)/D_Ver_R_4*Ver_t)),))","v":0}]
[null,null,{"$f":"C659+D_ver_z_incr","v":0},{"$f":"D659+D_ver_t_incre","v":0},{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*Ver_t/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*$C663/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E$593^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)*SQRT(2)))),IF(AND($E$593>0,$F$593=0),0.5*EXP(-D_Ver_lambdayear_4*$C663/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))*D_Ver_C0_4,IF($E$593=0,0,0.5*EXP(-D_Ver_lambdayear_4*$C663/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)-D_ver_B_4*$E$593)*SQRT(2))+EXP((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$E$593)+D_ver_B_4*$E$593)*SQRT(2)))-(EXP(-(D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)-D_ver_B_4*$F$593)*SQRT(2))+EXP((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*$C663/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*Q$592)/(2*$F$593)+D_ver_B_4*$F$593)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,{"$f":"IF(D_vert_AC,0,IF(D_vert_DTU_2,(D_Ver_C0_4*(EXP(-D_Ver_lambdayear_4*$D665/D_Ver_R_4)-EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*EXP(-D_Ver_lambdayear_4*$E665^2/D_Ver_R_4)*2*NORMSDIST(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E665)*SQRT(2)))),IF(AND($E665>0,$F665=0),0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E665)-D_ver_B_4*$E665)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E665)+D_ver_B_4*$E665)*SQRT(2)))*D_Ver_C0_4,IF($E665=0,0,0.5*EXP(-D_Ver_lambdayear_4*Ver_z/D_Ver_Vvel)*((EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E665)-D_ver_B_4*$E665)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$E665)+D_ver_B_4*$E665)*SQRT(2)))-(EXP(-(D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F665)-D_ver_B_4*$F665)*SQRT(2))+EXP((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)*D_ver_B_4)*2*NORMSDIST(-((D_Ver_R_4*Ver_z/D_Ver_Vvel/D_ver_A_4+D_ver_G_4*J$592)/(2*$F665)+D_ver_B_4*$F665)*SQRT(2))))*D_Ver_C0_4))))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,{"$error":"#VALUE!"},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"Udskrift_Vertikal_Transport","index":30,"n_rows":332,"n_cols":12,"rows_kept":332,"cut":false,"hidden":true,"merged":[[57,2,57,3],[57,4,57,5],[57,6,57,7],[57,8,57,9],[5,1,5,10],[55,2,56,3],[55,4,56,5],[55,6,56,7],[55,8,56,9],[40,2,40,3],[40,4,40,5],[40,6,40,7],[40,8,40,9],[42,2,42,3],[42,4,42,5],[42,6,42,7],[2,1,2,5],[3,1,3,5],[2,8,2,10],[3,8,3,10],[4,8,4,10],[4,1,4,5],[129,1,140,9],[67,2,67,3],[67,4,67,5],[67,6,67,7],[67,8,67,9],[102,1,114,9],[116,1,127,9],[76,1,87,9],[89,1,100,9],[65,2,66,3],[65,4,66,5],[65,6,66,7],[59,8,59,9],[59,2,59,3],[59,4,59,5],[59,6,59,7],[65,8,66,9],[63,2,63,3],[42,8,42,9],[41,2,41,3],[41,4,41,5],[41,6,41,7],[41,8,41,9],[35,6,35,7],[35,8,35,9],[39,2,39,3],[39,4,39,5],[39,6,39,7],[39,8,39,9],[35,4,35,5],[38,2,38,3],[38,4,38,5],[38,6,38,7],[38,8,38,9],[36,2,37,3],[36,4,37,5],[36,6,37,7],[36,8,37,9],[35,2,35,3],[26,2,26,3],[26,4,26,5],[27,2,27,3],[27,4,27,5],[32,0,32,1],[31,2,31,3],[31,4,31,5],[28,2,28,3],[28,4,28,5],[29,2,29,3],[29,4,29,5],[30,2,30,3],[30,4,30,5],[7,0,7,1],[9,2,9,3],[10,2,10,3],[13,2,13,3],[13,4,13,5],[55,10,56,10],[65,10,66,10],[14,2,14,3],[14,4,14,5],[16,2,16,3],[17,2,17,3],[18,2,18,3],[24,2,24,3],[24,4,24,5],[23,2,23,3],[23,4,23,5],[17,4,17,5],[18,4,18,5],[22,2,22,5],[25,2,25,3],[25,4,25,5]]}
["Vertikal transport"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr./by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nummer.",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
[]
["Kildeområde"]
["Kommentar",{"$f":"IF( D_Ver_Enk_Kil_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Længde af kildeområde","Y",{"$f":"IF(D_Ver_Y<>\"\",D_Ver_Y,\"\")","v":""},null,"m"]
["Bredde af kildeområde","x",{"$f":"IF(D_Ver_X<>\"\",D_Ver_X,\"\")","v":""},null,"m"]
[]
[null,null,"Standard data",null,"Indtastede data (angives med fed)"]
["Nettonedbør","N",{"$f":"IF(D_Ver_infiltration_syst<>\"\",D_Ver_infiltration_syst,\"\")","v":""},null,{"$f":"IF(Ver_My_N<>\"\",Ver_My_N,\"\")","v":""},null,"mm/år"]
["Kommune/Egn",null,{"$f":"IF(D_Ver_Egn_syst<>\"\",D_Ver_Egn_syst,\"\")","v":""},null,{"$f":"IF(Ver_My_Egn<>\"\",Ver_My_Egn,\"\")","v":""}]
[]
["Afstand til grundvandsspejl","Z",{"$f":"IF(D_Ver_Z<>\"\",D_Ver_Z,\"\")","v":""},null,"m",null,"Beregnet porevandshastighed",null,null,null,{"$f":"Ver_Vw","v":""},"m/år"]
["Longitudinal dispersivitet","αL,W",{"$f":"IF(D_Ver_alfaLw_beregn<>\"\",D_Ver_alfaLw_beregn,\"\")","v":6.5679999999999988E-2},null,{"$f":"IF(Ver_alfaLw<>\"\",Ver_alfaLw,\"\")","v":""}]
["Varighed af spild","a",null,null,{"$f":"IF(Ver_a >0,Ver_a_tjek,D_ver_a)","v":"Vedvarende"},null,null,"Kun for DTU V1D model 1a"]
[]
["Jordparametre"]
["Kommentar",{"$f":"IF( D_Ver_Enk_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Standard data",null,"Indtastede data (angives med fed)"]
["Jordtype",null,{"$f":"IF(D_Ver_jord<>\"\",D_Ver_jord,\"\")","v":0}]
["Vandindhold","qw",{"$f":"IF(D_Ver_thetaw_syst<>\"\",D_Ver_thetaw_syst,\"\")","v":""},null,{"$f":"IF(Ver_My_VV<>\"\",Ver_My_VV,\"\")","v":""}]
["Luftindhold","qa",{"$f":"IF(D_Ver_thetaa_syst<>\"\",D_Ver_thetaa_syst,\"\")","v":""},null,{"$f":"IF(Ver_My_VL<>\"\",Ver_My_VL,\"\")","v":""}]
["Total porøsitet (VL+VV)","n",{"$f":"D_Ver_ntotal","v":""}]
["% organisk indhold","foc",{"$f":"IF(D_Ver_foc_syst<>\"\",D_Ver_foc_syst,\"\")","v":""},null,{"$f":"IF(Ver_My_foc<>\"\",Ver_My_foc,\"\")","v":""}]
["Bulkmassefylde","r",{"$f":"IF(D_Ver_rhob<>\"\",D_Ver_rhob,\"\")","v":""},null,null,null,"kg/l"]
["Sprækkeafstand (2B) ","2B",{"$f":"IF(Ver_2B<>\"\",Ver_2B,\"\")","v":5},null,{"$f":"IF(Ver_My_2B<>\"\",Ver_My_2B,\"\")","v":""},null,"m","Kun hvis sprækketransport"]
["Sprækkeapertur (2b)","2b",{"$f":"IF(D_ver_2bapertur<>\"\",D_ver_2bapertur,\"\")","v":{"$error":"#VALUE!"}},null,null,null,"m","Kun hvis sprækketransport"]
["Bulk-hydraulisk ledningsevne (Kb)","Kb",{"$f":"IF(Ver_Kb<>\"\",Ver_Kb,\"\")","v":6.2999999999999995E-8},null,{"$f":"IF(Ver_My_Kb<>\"\",Ver_My_Kb,\"\")","v":""},null,"m/s","Kun hvis sprækketransport"]
[]
["Nedbrydningsforhold:",null,{"$f":"IF(D_Ver_an,\"Aerobe forhold\",\"Anaerobe forhold\")","v":"Aerobe forhold"}]
[]
["Stoffer og stofegenskaber"]
["Kommentar",{"$f":"IF( D_Ver_Enk_For_ComUds,\"ja\",\"nej\")","v":"nej"},"Stof 1",null,"Stof 2",null,"Stof 3",null,"Stof 4"]
["Forureningskomponent",null,{"$f":"IF(D_Ver_stofnavn_1<>\"\",D_Ver_stofnavn_1,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_2<>\"\",D_Ver_stofnavn_2,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_3<>\"\",D_Ver_stofnavn_3,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_4<>\"\",D_Ver_stofnavn_4,\"\")","v":""}]
[]
["Målepunkt",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_MP_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_MP_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_MP_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_MP_4,\"\")","v":""}]
["Dato",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",D_Enk_dato_1,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",D_Enk_dato_2,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",D_Enk_dato_3,\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",D_Enk_dato_4,\"\")","v":""}]
["Kildekoncentration",null,{"$f":"IF(ISNUMBER(D_Ver_C0_1), (ROUND(D_Ver_C0_1,3-(INT(LOG(D_Ver_C0_1))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ver_C0_2), (ROUND(D_Ver_C0_2,3-(INT(LOG(D_Ver_C0_2))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ver_C0_3), (ROUND(D_Ver_C0_3,3-(INT(LOG(D_Ver_C0_3))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ver_C0_4), (ROUND(D_Ver_C0_4,3-(INT(LOG(D_Ver_C0_4))+1))),\"\")","v":""},null,"mg/l"]
["Beregnet værdi anvendt",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",(IF(C43=\"ja\",\"Nej\",(IF(ISNUMBER(Enk_My_CV_1),\"Nej\",\"Ja\")))),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",(IF(E43=\"ja\",\"Nej\",(IF(ISNUMBER(Enk_My_CV_2),\"Nej\",\"Ja\")))),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",(IF(G43=\"ja\",\"nej\",(IF(ISNUMBER(Enk_My_CV_3),\"Nej\",\"Ja\")))),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",(IF(I43=\"ja\",\"Nej\",(IF(ISNUMBER(Enk_My_CV_4),\"Nej\",\"Ja\")))),\"\")","v":""}]
["Testværdi anvendt",null,{"$f":"IF(D_Enk_stofnavn_1<>\"\",IF(ISNUMBER(Ver_CV_1),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_2<>\"\",IF(ISNUMBER(Ver_CV_2),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_3<>\"\",IF(ISNUMBER(Ver_CV_3),\"Ja\",\"Nej\"),\"\")","v":""},null,{"$f":"IF(D_Enk_stofnavn_4<>\"\",IF(ISNUMBER(Ver_CV_4),\"Ja\",\"Nej\"),\"\")","v":""}]
["1. ordens nedbrydn.konst., aerob",null,{"$f":"IF(D_Enk_k1aerob_uz_syst_1<>\"\",D_Enk_k1aerob_uz_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_k1aerob_umættet_1<>\"\",Enk_My_k1aerob_umættet_1,\"\")","v":""},{"$f":"IF(D_Enk_k1aerob_uz_syst_2<>\"\",D_Enk_k1aerob_uz_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_k1aerob_umættet_2<>\"\",Enk_My_k1aerob_umættet_2,\"\")","v":""},{"$f":"IF(D_Enk_k1aerob_uz_syst_3<>\"\",D_Enk_k1aerob_uz_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_k1aerob_umættet_3<>\"\",Enk_My_k1aerob_umættet_3,\"\")","v":""},{"$f":"IF(D_Enk_k1aerob_uz_syst_4<>\"\",D_Enk_k1aerob_uz_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_k1aerob_umættet_4<>\"\",Enk_My_k1aerob_umættet_4,\"\")","v":""},"dag-1"]
["1. ordens nedbrydn.konst., anaerob",null,{"$f":"IF(D_Enk_k1anaerob_umættet_syst_1<>\"\",D_Enk_k1anaerob_umættet_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_k1anaerob_umættet_1<>\"\",Enk_My_k1anaerob_umættet_1,\"\")","v":""},{"$f":"IF(D_Enk_k1anaerob_umættet_syst_2<>\"\",D_Enk_k1anaerob_umættet_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_k1anaerob_umættet_2<>\"\",Enk_My_k1anaerob_umættet_2,\"\")","v":""},{"$f":"IF(D_Enk_k1anaerob_umættet_syst_3<>\"\",D_Enk_k1anaerob_umættet_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_k1anaerob_umættet_3<>\"\",Enk_My_k1anaerob_umættet_3,\"\")","v":""},{"$f":"IF(D_Enk_k1anaerob_umættet_syst_4<>\"\",D_Enk_k1anaerob_umættet_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_k1anaerob_umættet_4<>\"\",Enk_My_k1anaerob_umættet_4,\"\")","v":""},"dag-1"]
["Diffusionskoefficient (luft)","Dda",{"$f":"IF(D_Enk_DL_syst_1<>\"\",D_Enk_DL_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_DL_1<>\"\",Enk_My_DL_1,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_2<>\"\",D_Enk_DL_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_DL_2<>\"\",Enk_My_DL_2,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_3<>\"\",D_Enk_DL_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_DL_3<>\"\",Enk_My_DL_3,\"\")","v":""},{"$f":"IF(D_Enk_DL_syst_4<>\"\",D_Enk_DL_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_DL_4<>\"\",Enk_My_DL_4,\"\")","v":""},"m2/s"]
["Diffusionskoefficient (vand)","Ddw",{"$f":"IF(D_Enk_Ddw_syst_1<>\"\",D_Enk_Ddw_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_Ddw_1<>\"\",Enk_My_Ddw_1,\"\")","v":""},{"$f":"IF(D_Enk_Ddw_syst_2<>\"\",D_Enk_Ddw_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_Ddw_2<>\"\",Enk_My_Ddw_2,\"\")","v":""},{"$f":"IF(D_Enk_Ddw_syst_3<>\"\",D_Enk_Ddw_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_Ddw_3<>\"\",Enk_My_Ddw_3,\"\")","v":""},{"$f":"IF(D_Enk_Ddw_syst_4<>\"\",D_Enk_Ddw_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_Ddw_4<>\"\",Enk_My_Ddw_4,\"\")","v":""},"m2/s"]
["Diffusionskoefficient (matrix)","Dm",{"$f":"IF(D_Ver_stofnavn_1<>\"\",D_ver_Ddwm_1,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_2<>\"\",D_ver_Ddwm_2,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_3<>\"\",D_ver_Ddwm_3,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_4<>\"\",D_ver_Ddwm_4,\"\")","v":""},null,"m2/år"]
["KOC","KOC",{"$f":"IF(D_Enk_KOC_syst_1<>\"\",D_Enk_KOC_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_KOC_1<>\"\",Enk_My_KOC_1,\"\")","v":""},{"$f":"IF(D_Enk_KOC_syst_2<>\"\",D_Enk_KOC_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_KOC_2<>\"\",Enk_My_KOC_2,\"\")","v":""},{"$f":"IF(D_Enk_KOC_syst_3<>\"\",D_Enk_KOC_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_KOC_3<>\"\",Enk_My_KOC_3,\"\")","v":""},{"$f":"IF(D_Enk_KOC_syst_4<>\"\",D_Enk_KOC_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_KOC_4<>\"\",Enk_My_KOC_4,\"\")","v":""},"mg/l"]
["Henrys konstant","KH",{"$f":"IF(D_Enk_KH_syst_1<>\"\",D_Enk_KH_syst_1,\"\")","v":""},{"$f":"IF(Enk_My_KH_1<>\"\",Enk_My_KH_1,\"\")","v":""},{"$f":"IF(D_Enk_KH_syst_2<>\"\",D_Enk_KH_syst_2,\"\")","v":""},{"$f":"IF(Enk_My_KH_2<>\"\",Enk_My_KH_2,\"\")","v":""},{"$f":"IF(D_Enk_KH_syst_3<>\"\",D_Enk_KH_syst_3,\"\")","v":""},{"$f":"IF(Enk_My_KH_3<>\"\",Enk_My_KH_3,\"\")","v":""},{"$f":"IF(D_Enk_KH_syst_4<>\"\",D_Enk_KH_syst_4,\"\")","v":""},{"$f":"IF(Enk_My_KH_4<>\"\",Enk_My_KH_4,\"\")","v":""}]
["Retardation","R",{"$f":"IF(D_Ver_stofnavn_1<>\"\",D_Ver_R_1,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_2<>\"\",D_Ver_R_2,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_3<>\"\",D_Ver_R_3,\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_4<>\"\",D_Ver_R_4,\"\")","v":""}]
[]
["Beregning: Vertikal transport"]
["Kommentar",{"$f":"IF( D_Ver_Enk_Ber_ComUds,\"ja\",\"nej\")","v":"nej"},{"$f":"CONCATENATE(\"Anvendt model: \",D_ver_model)","v":"Anvendt model: Model A + C"},null,null,null,null,null,"Angiv signifikant ciffer",null,3]
[{"$f":"CONCATENATE(\"Stationær (ligevægts) koncentration efter nedsivning til grundvandet i \", Ver_z, \" m´s dybde (z)\")","v":"Stationær (ligevægts) koncentration efter nedsivning til grundvandet i  m´s dybde (z)"}]
["C(z), Porevandskoncentration lige ",null,{"$f":"IF(ISNUMBER(D_Ver_Cz_1),(ROUND(D_Ver_Cz_1,Ver_ciffer-(INT(LOG(D_Ver_Cz_1))+1))),D_Ver_Cz_1)","v":false},null,{"$f":"IF(ISNUMBER(D_Ver_Cz_2),(ROUND(D_Ver_Cz_2,Ver_ciffer-(INT(LOG(D_Ver_Cz_2))+1))),D_Ver_Cz_2)","v":false},null,{"$f":"IF(ISNUMBER(D_Ver_Cz_3),(ROUND(D_Ver_Cz_3,Ver_ciffer-(INT(LOG(D_Ver_Cz_3))+1))),(D_Ver_Cz_3))","v":false},null,{"$f":"IF(ISNUMBER(D_Ver_Cz_4),(ROUND(D_Ver_Cz_4,Ver_ciffer-(INT(LOG(D_Ver_Cz_4))+1))),D_Ver_Cz_4)","v":false},null,"mg/l"]
["over grundvandet (input til trin 1a)"]
["Total flux",null,{"$f":"IF(D_Ver_stofnavn_1<>\"\",IF(ISNUMBER(D_Ver_Flux_1),ROUND(D_Ver_Flux_1,Ver_ciffer-(INT(LOG(D_Ver_Flux_1))+1)),(D_Ver_Flux_1)),\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_2<>\"\",IF(ISNUMBER(D_Ver_Flux_2),ROUND(D_Ver_Flux_2,Ver_ciffer-(INT(LOG(D_Ver_Flux_2))+1)),(D_Ver_Flux_2)),\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_3<>\"\",IF(ISNUMBER(D_Ver_Flux_3),ROUND(D_Ver_Flux_3,Ver_ciffer-(INT(LOG(D_Ver_Flux_3))+1)),(D_Ver_Flux_3)),\"\")","v":""},null,{"$f":"IF(D_Ver_stofnavn_4<>\"\",IF(ISNUMBER(D_Ver_Flux_4),ROUND(D_Ver_Flux_4,Ver_ciffer-(INT(LOG(D_Ver_Flux_4))+1)),(D_Ver_Flux_4)),\"\")","v":""},null,"g/år"]
["Grundvandskriterium",null,{"$f":"IF(D_Enk_GV_krit_syst_1<>\"\",D_Enk_GV_krit_syst_1/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_1<>\"\",Enk_My_GV_krit_1/1000,\"\")","v":""},{"$f":"IF(D_Enk_GV_krit_syst_2<>\"\",D_Enk_GV_krit_syst_2/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_2<>\"\",Enk_My_GV_krit_2/1000,\"\")","v":""},{"$f":"IF(D_Enk_GV_krit_syst_3<>\"\",D_Enk_GV_krit_syst_3/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_3<>\"\",Enk_My_GV_krit_3/1000,\"\")","v":""},{"$f":"IF(D_Enk_GV_krit_syst_4<>\"\",D_Enk_GV_krit_syst_4/1000,\"\")","v":""},{"$f":"IF(Enk_My_GV_krit_4<>\"\",Enk_My_GV_krit_4/1000,\"\")","v":""},"mg/l"]
["Overskridelse af kriteriet",null,{"$f":"IF(D_Ver_GVKKover_1<>\"\",IF(ISNUMBER(D_Ver_GVKKover_1),(ROUND(D_Ver_GVKKover_1,Ver_ciffer-(INT(LOG(D_Ver_GVKKover_1))+1))),D_Ver_GVKKover_1),\"\")","v":"Intet kriterie"},null,{"$f":"IF(D_Ver_GVKKover_2<>\"\",IF(ISNUMBER(D_Ver_GVKKover_2),(ROUND(D_Ver_GVKKover_2,Ver_ciffer-(INT(LOG(D_Ver_GVKKover_2))+1))),D_Ver_GVKKover_2),\"\")","v":"Intet kriterie"},null,{"$f":"IF(D_Ver_GVKKover_3<>\"\",IF(ISNUMBER(D_Ver_GVKKover_3),(ROUND(D_Ver_GVKKover_3,Ver_ciffer-(INT(LOG(D_Ver_GVKKover_3))+1))),D_Ver_GVKKover_3),\"\")","v":"Intet kriterie"},null,{"$f":"IF(D_Ver_GVKKover_4<>\"\",IF(ISNUMBER(D_Ver_GVKKover_4),(ROUND(D_Ver_GVKKover_4,Ver_ciffer-(INT(LOG(D_Ver_GVKKover_4))+1))),D_Ver_GVKKover_4),\"\")","v":"Intet kriterie"},null,"gange"]
[]
[{"$f":"CONCATENATE(\"Transient koncentration efter nedsivning igennem \", Ver_z,\" m til grundvandet efter \",Ver_t,\" år \")","v":"Transient koncentration efter nedsivning igennem  m til grundvandet efter  år "}]
[]
["Tid (t), år",null,{"$f":"Ver_t","v":0}]
[]
["C(z,t), transient porevandskonc.",null,{"$f":"IF(ISNUMBER(D_Ver_czt_1),IF(D_Ver_czt_1=0,D_Ver_czt_1,ROUND(D_Ver_czt_1,Ver_ciffer-(INT(LOG(D_Ver_czt_1))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ver_czt_2),IF(D_Ver_czt_2=0,D_Ver_czt_2,ROUND(D_Ver_czt_2,Ver_ciffer-(INT(LOG(D_Ver_czt_2))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ver_czt_3),IF(D_Ver_czt_3=0,D_Ver_czt_3,ROUND(D_Ver_czt_3,Ver_ciffer-(INT(LOG(D_Ver_czt_3))+1))),\"\")","v":""},null,{"$f":"IF(ISNUMBER(D_Ver_czt_4),IF(D_Ver_czt_4=0,D_Ver_czt_4,ROUND(D_Ver_czt_4,Ver_ciffer-(INT(LOG(D_Ver_czt_4))+1))),\"\")","v":""},null,"mg/l"]
["lige over grundvandet efter tid, t"]
["Anvendt brugerdata?",null,{"$f":"D_ver_brugerdata_1","v":""},null,{"$f":"D_ver_brugerdata_2","v":""},null,{"$f":"D_ver_brugerdata_3","v":""},null,{"$f":"D_ver_brugerdata_4","v":""}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"IF(Lok_firma<>\"\",Lok_firma,\"\")","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler."]
[]
["Bemærkninger",{"$f":"IF(D_Ver_Enk_Kil_Com <> \"\", D_Ver_Enk_Kil_Com, \"\")","v":""}]
["om kildeområde"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ver_Enk_Jord_Com <> \"\", D_Ver_Enk_Jord_Com, \"\")","v":""}]
["om jordparametre"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ver_Enk_For_Com <> \"\", D_Ver_Enk_For_Com, \"\")","v":""}]
["om forurening"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Ver_Enk_Ber_Com <> \"\", D_Ver_Enk_Ber_Com, \"\")","v":""}]
["om beregning"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Enk_Kem_Com<>\"\",D_Enk_Kem_Com,\"\")","v":""}]
["om kemiske stoffer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Fordeling af porevandskoncentrationer i dybden ned til grundvandet "]
[]
["Stof 1",{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,{"$f":"IF(D_vert_AC,Domenico_model_A_C,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 1",{"$f":"D_Enk_stofnavn_1","v":""},null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,'Vertikal Transport'!$K$15,IF(D_vert_DTU_1b,'Vertikal Transport'!$R$15,'Vertikal Transport'!$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 2",{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,{"$f":"IF(D_vert_AC,Domenico_model_A_C,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 2",{"$f":"D_Enk_stofnavn_2","v":""},null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,'Vertikal Transport'!$K$15,IF(D_vert_DTU_1b,'Vertikal Transport'!$R$15,'Vertikal Transport'!$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 3",{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,{"$f":"IF(D_vert_AC,Domenico_model_A_C,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 3",{"$f":"D_Enk_stofnavn_3","v":""},null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,'Vertikal Transport'!$K$15,IF(D_vert_DTU_1b,'Vertikal Transport'!$R$15,'Vertikal Transport'!$Z$15)))","v":"DTU V1D modeller ikke valgt"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 4",{"$f":"D_Enk_stofnavn_4","v":""},null,null,null,{"$f":"IF(D_vert_AC,Domenico_model_A_C,CONCATENATE(\"Model A+C ikke valgt\"))","v":"Model A+C*"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Stof 4",{"$f":"D_Enk_stofnavn_4","v":""},null,null,null,{"$f":"IF(D_vert_AC, \"DTU V1D modeller ikke valgt\",IF(D_vert_DTU_1a,'Vertikal Transport'!$K$15,IF(D_vert_DTU_1b,'Vertikal Transport'!$R$15,'Vertikal Transport'!$Z$15)))","v":"DTU V1D modeller ikke valgt"}]

{"sheet":"Vejledning_Vertikal_Transport","index":31,"n_rows":149,"n_cols":2,"rows_kept":149,"cut":false,"hidden":true,"merged":[[1,1,1,15],[2,1,5,15],[6,1,6,15],[38,1,38,15],[61,1,61,15],[40,1,59,15],[62,1,67,15],[68,1,68,15],[69,1,69,15],[70,1,72,15],[73,1,73,15],[74,1,74,15],[75,1,89,15],[90,1,90,15],[91,1,91,15],[92,1,94,14],[131,1,131,15],[95,1,95,15],[97,1,102,15],[103,1,103,15],[104,1,104,15],[105,1,106,15],[107,1,107,15],[108,1,116,15],[117,1,117,15],[118,1,118,15],[119,1,129,15],[130,1,130,15],[146,1,146,15],[147,1,147,15],[148,1,149,15],[132,1,133,15],[134,1,134,15],[135,1,135,15],[136,1,138,15],[140,1,140,15],[141,1,145,15]]}
[null,"Vejledning - Vertikal transport "]
[null,"Formål"]
[null,"I dette regneark kan der foretages en beregning af vertikal transport og evt. nedbrydning igennem enten et homogent jordlag eller sprækker i moræneler og ned til det førstkommende betydende grundvandsmagasin. Vertikal transport i et homogent jordlag er baseret på beregninger for konceptuel model A og C, beskrevet i Miljøprojektet om vertikal transport ned til det førstkommende betydende magasin. Beregninger af vertikal transport i vandmættet sprækket ler – konceptuel model B - er baseret på DTU V1D model. DTU Miljø. Manual. DTU V1D – DTU Vertical 1D Transport Model. A spreadsheet for risk assessment in low-permeability media. http://www.sara.env.dtu.dk/Modelvaerktoejer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEREGNINGER"]
[null,"Valg af model:"]
[null,"Der kan vælges imellem 4 forskellige beregningsmodeller for vertikal transport af organiske stoffer igennem et jordlag og ned til førstkommende grundvandsmagasin.\n\nFor model A eller C er der tale om en kontinuer kilde, som nedsives igennem et homogent vandmættet ler eller et umættet sand- eller lerlag. Da kildekoncentrationen er kontinuert (ikke aftager) vil der med tiden opnås stationære forhold, og koncentrationen lige over grundvandet vil være lig kildekoncentrationen, med mindre der sker nedbrydning under transport.\n \nFor DTUV1D model 1a er der en kendt spildperiode, hvorefter kildekoncentrationen aftager og  koncentrationen lige over grundvandsspejlet ligeledes vil aftage med tiden. Der skal kun indtastes varighed af spild, såfremt der vælges Model B- DTU V1D model1a.\n\nFor DTUV1D model 1b er der tale om en kontinuert kilde, som nedsives igennem en sprækket vandmættet ler. Da kildekoncentrationen er kontinuert (ikke aftager) vil der med tiden opnås stationære forhold og koncentrationen lige over grundvandet vil være lig kildekoncentrationen, med mindre der sker nedbrydning under transport.\n\nFor DTUV1D model 2 er der tale om en aftagende kilde, idet der antages, at forureningskilden er ophørt, og nedsivningen styres af diffusion fra matrix til sprækker og herefter igennem den sprækkede vandmættede ler."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Kildeområde:"]
[null,"Længden x og bredden y af kilden, hvorfra nedsivning sker, skal angives.\nz er afstanden fra bunden af kilden til grundvandsspejlet dvs. svarende til tykkelsen af det homogene jordlag (enten mættet ler eller umættet sand og ler). \nDer skal enten vælges nedbørsdata fra standardlisten ved at vælge det geografiske område, som forureningen er beliggende i, eller indtastes nye værdier. Det er også muligt at anvende og oprette egne nedbørsdata ved at klikke på knappen \"Egen liste\"."]
[]
[]
[]
[]
[]
[]
[null,"Jordtype:"]
[null,"Jordtypen i den umættede zone skal enten vælges som standardjordtyper fra listen (klik på \"Jordtype\") eller indtaste egne værdier. Egne jordtyper kan oprettes svarende til for nedbørsdata. OBS: For mættede forhold bør VV sættes til maks. porøsitet og VL til nul."]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata for porevand overføres fra \"Enkeltstoffer\". Hvis der i dette ark er indtastet en målt grundvandskoncentration, indtastes denne, ellers overføres vandkoncentrationen beregnet ud fra en jordkoncentration eller alternativt en indtastet poreluftkoncentration. Der kan også indtastes værdier direkte i de hvide felter. Af udskriften vil det så fremgå, at der ikke er anvendt målte værdier. \n\nHerudover skal der vælges nedbrydningsforhold (aerobe eller anaerobe). Nedbrydningskonstanter for nedbrydning i den umættede zone hentes fra kemiske data i \"Enkeltstoffer\", hvor det er muligt at indsætte andre værdier, såfremt standardværdier fra databasen ikke ønskes anvendt. Standardværdier er af Miljøstyrelsen defineret som nul, dvs. at der i standardberegninger ikke antages at foregå nedbrydning under den vertikale transport.  Beregninger uden nedbrydning viser dermed at koncentrationen i det første betydende magasin under stationære forhold vil være lig porevandskoncentrationen.\n\nDer kan indsættes en tid, t (år) og beregne de transiente porevandskoncentrationer lige over grundvandspejl efter tid, t. Desuden vises udvikling i de transiente porevandkoncentrationer i forskellige dybder under transport igennem jordlaget med tiden på en figur."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GENERELT"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under olie & benzin modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under olie & benzin modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTE VÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Oliestoffer","index":32,"n_rows":98,"n_cols":41,"rows_kept":98,"cut":false,"hidden":true,"merged":[[79,34,79,35],[61,40,61,41],[58,25,58,26],[58,28,58,29],[61,34,61,35],[78,34,78,35],[75,22,75,23],[78,22,78,23],[62,40,62,41],[66,40,66,41],[68,40,68,41],[58,22,58,23],[61,25,61,26],[66,25,66,26],[78,25,78,26],[61,22,61,23],[72,34,72,35],[72,22,72,23],[64,25,64,26],[70,25,70,26],[72,25,72,26],[68,25,68,26],[62,25,62,26],[70,34,70,35],[64,34,64,35],[68,28,68,29],[62,34,62,35],[66,34,66,35],[68,34,68,35],[91,37,91,38],[47,40,47,41],[79,40,79,41],[78,40,78,41],[72,40,72,41],[70,40,70,41],[64,40,64,41],[58,40,58,41],[79,37,79,38],[81,37,81,38],[83,37,83,38],[62,28,62,29],[70,28,70,29],[64,28,64,29],[48,28,48,29],[50,28,50,29],[52,28,52,29],[54,28,54,29],[55,40,55,41],[61,37,61,38],[66,37,66,38],[68,37,68,38],[62,37,62,38],[70,37,70,38],[64,37,64,38],[72,37,72,38],[78,37,78,38],[56,37,56,38],[58,37,58,38],[44,28,44,29],[37,22,37,23],[41,22,41,23],[39,13,39,14],[40,13,40,14],[39,22,39,23],[40,22,40,23],[37,28,37,29],[40,16,40,17],[39,28,39,29],[40,28,40,29],[41,28,41,29],[37,25,37,26],[39,25,39,26],[40,25,40,26],[41,25,41,26],[44,25,44,26],[28,22,28,29],[29,22,29,29],[29,7,29,17],[30,37,32,39],[30,21,32,24],[30,15,32,18],[34,7,34,8],[34,10,34,11],[34,13,34,14],[33,37,33,38],[34,22,34,23],[34,28,34,29],[29,34,29,41],[30,33,32,36],[33,34,33,35],[34,40,34,41],[34,34,34,35],[33,7,33,8],[33,10,33,11],[33,13,33,14],[33,16,33,17],[33,22,33,23],[33,25,33,26],[33,28,33,29],[40,37,40,38],[41,37,41,38],[44,40,44,41],[44,34,44,35],[40,40,40,41],[37,40,37,41],[33,40,33,41],[36,40,36,41],[36,34,36,35],[36,37,36,38],[34,37,34,38],[40,34,40,35],[44,37,44,38],[36,10,36,11],[36,13,36,14],[36,16,36,17],[36,22,36,23],[47,7,47,8],[47,10,47,11],[47,13,47,14],[47,16,47,17],[41,7,41,8],[39,7,39,8],[44,22,44,23],[47,22,47,23],[39,10,39,11],[55,22,55,23],[56,25,56,26],[56,22,56,23],[91,28,91,29],[72,28,72,29],[75,28,75,29],[78,28,78,29],[79,28,79,29],[81,28,81,29],[83,28,83,29],[87,28,87,29],[87,22,87,23],[89,22,89,23],[89,28,89,29],[47,25,47,26],[75,25,75,26],[79,22,79,23],[79,25,79,26],[95,7,95,11],[97,7,97,11],[41,10,41,11],[89,7,89,8],[89,10,89,11],[91,16,91,17],[79,7,79,8],[79,10,79,11],[41,13,41,14],[79,16,79,17],[81,16,81,17],[83,16,83,17],[85,16,85,17],[44,7,44,8],[44,10,44,11],[74,13,74,14],[61,16,61,17],[91,7,91,8],[78,16,78,17],[64,16,64,17],[74,16,74,17],[66,16,66,17],[68,16,68,17],[62,16,62,17],[91,10,91,11],[91,40,91,41],[91,34,91,35],[85,7,85,8],[85,10,85,11],[85,40,85,41],[85,34,85,35],[87,7,87,8],[87,10,87,11],[87,40,87,41],[87,34,87,35],[85,13,85,14],[87,13,87,14],[89,13,89,14],[91,13,91,14],[91,22,91,23],[87,25,87,26],[89,25,89,26],[91,25,91,26],[85,28,85,29],[89,16,89,17],[89,40,89,41],[89,34,89,35],[81,25,81,26],[83,25,83,26],[85,25,85,26],[83,22,83,23],[85,22,85,23],[85,37,85,38],[87,37,87,38],[89,37,89,38],[81,40,81,41],[81,34,81,35],[83,40,83,41],[83,34,83,35],[81,22,81,23],[72,13,72,14],[72,16,72,17],[70,22,70,23],[64,22,64,23],[87,16,87,17],[81,7,81,8],[81,10,81,11],[83,7,83,8],[83,10,83,11],[83,13,83,14],[79,13,79,14],[81,13,81,14],[78,7,78,8],[78,10,78,11],[78,13,78,14],[75,10,75,11],[75,13,75,14],[75,16,75,17],[72,7,72,8],[72,10,72,11],[74,7,74,8],[74,10,74,11],[70,7,70,8],[70,10,70,11],[70,16,70,17],[61,28,61,29],[66,28,66,29],[62,7,62,8],[62,10,62,11],[66,7,66,8],[66,10,66,11],[68,7,68,8],[68,10,68,11],[66,13,66,14],[68,13,68,14],[62,13,62,14],[66,22,66,23],[68,22,68,23],[62,22,62,23],[61,7,61,8],[61,10,61,11],[61,13,61,14],[64,7,64,8],[64,10,64,11],[70,13,70,14],[64,13,64,14],[58,7,58,8],[58,10,58,11],[58,34,58,35],[37,7,37,8],[37,10,37,11],[37,34,37,35],[58,13,58,14],[37,13,37,14],[55,7,55,8],[55,10,55,11],[50,22,50,23],[48,7,48,8],[48,10,48,11],[55,28,55,29],[44,13,44,14],[58,16,58,17],[44,16,44,17],[48,16,48,17],[50,16,50,17],[52,16,52,17],[54,16,54,17],[55,16,55,17],[56,16,56,17],[55,34,55,35],[56,7,56,8],[56,10,56,11],[56,40,56,41],[56,34,56,35],[52,7,52,8],[52,10,52,11],[52,40,52,41],[52,34,52,35],[54,7,54,8],[54,10,54,11],[54,40,54,41],[54,34,54,35],[52,13,52,14],[54,13,54,14],[55,13,55,14],[56,13,56,14],[56,28,56,29],[52,37,52,38],[54,37,54,38],[55,37,55,38],[54,25,54,26],[55,25,55,26],[52,22,52,23],[54,22,54,23],[48,40,48,41],[48,34,48,35],[50,7,50,8],[50,10,50,11],[50,40,50,41],[50,34,50,35],[48,25,48,26],[50,25,50,26],[52,25,52,26],[48,37,48,38],[50,37,50,38],[30,40,32,42],[47,37,47,38],[30,28,32,30],[30,25,32,27],[47,28,47,29],[15,16,15,17],[15,19,15,20],[15,22,15,23],[15,25,15,26],[15,28,15,29],[16,25,18,26],[16,28,16,29],[19,27,19,28],[20,24,20,26],[34,25,34,26],[36,25,36,26],[36,28,36,29],[47,34,47,35],[41,40,41,41],[41,34,41,35],[39,40,39,41],[39,34,39,35],[37,37,37,38],[39,37,39,38],[18,28,18,29],[99,7,99,8],[16,4,17,8],[16,10,16,11],[16,13,16,14],[16,16,18,17],[16,19,18,20],[16,22,16,23],[18,4,18,8],[23,7,23,11],[24,7,24,11],[48,13,48,14],[50,13,50,14],[30,6,32,8],[30,9,32,12],[30,13,32,14],[48,22,48,23],[41,16,41,17],[34,16,34,17],[37,16,37,17],[39,16,39,17],[36,7,36,8],[40,7,40,8],[40,10,40,11],[23,16,25,31],[15,10,15,11],[15,13,15,14],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[12,10,14,11],[12,13,14,14],[12,16,14,17],[12,19,14,20],[12,22,14,23],[9,4,9,29],[12,25,14,26],[12,28,14,29],[14,4,14,8],[17,10,17,11],[17,13,17,14],[17,22,17,23],[17,28,17,29],[18,10,18,11],[18,13,18,14],[18,22,18,23]]}
["Kemiske data og fugacitet for oliekomponenter"]
["Lokaliteten"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[]
["Jordtype",null,null,null,null,null,"Vælg jordart for fugacitetsberegning eller indtast egen jordartsdata"]
[]
[null,null,null,null,null,null,null,null,null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,null,"Volumen\naf jordskellet",null,null,"Korn-rumvægt\n(kg/l)",null,null,"Volumen-vægt\n(kg/l)",null,null,"% Indhold af organisk kulstof"]
[]
[null,null,null,null,"Jordtype"]
[null,null,null,null,null,null,null,null,null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ",null,null,"d",null,null,"r",null,null,"foc"]
[null,null,null,null,{"$f":"IF(D_Olie_jordtype_sys<>\"\",D_Olie_jordtype_sys,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Olie_VL_int_sys<>\"\",D_Olie_VL_int_sys,\"\")","v":""},null,null,{"$f":"IF(D_Olie_VV_int_sys<>\"\",D_Olie_VV_int_sys,\"\")","v":""},null,null,{"$f":"D_Olie_e","v":0},null,null,{"$f":"D_Olie_VJ","v":1},null,null,{"$f":"IF(D_Olie_d_int_sys<>\"\",D_Olie_d_int_sys,\"\")","v":""},null,null,{"$f":"D_Olie_p","v":0},null,null,{"$f":"IF(D_Olie_foc_int_sys<>\"\",D_Olie_foc_int_sys,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Olie_VL_sys<>\"\",D_Olie_VL_sys,\"\")","v":""},null,null,{"$f":"IF(D_Olie_VV_sys<>\"\",D_Olie_VV_sys,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_Olie_d_sys<>\"\",D_Olie_d_sys,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_Olie_foc_sys<>\"\",D_Olie_foc_sys,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_Olie_e>0.45,\"Er det korrekt at den samlede porøsitet er >0,45? - tjek VL og VV\",\"\")","v":""}]
[]
[]
["Kemiske data",null,null,null,null,null,null,"Indtast målepunkt og evt prøvetagningsdato samt den målte værdi. Der kan kun indtastes oplysninger for et medie"]
[]
["Målepunkt",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"De 2 profiler omhandler dels et profil for tung olie svarende til fyringsolie eller diesel, dels et profil for en blanding af benzin og diesel."]
["Dato"]
[]
[null,null,null,null,null,null,null,"Vælg profil for oliekomponent"]
[]
[]
[null,null,null,null,null,null,null,"Jordkoncentration Ct",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Porevandskoncentration Cv",null,null,null,null,null,null,null,null,null,null,null,"Poreluftskoncentration Cl"]
[null,null,null,null,null,null,"Indtastede\nværdier",null,null,"Beregnet ud fra olieprofil ",null,null,null,"Jord-kvalitets-kriterium",null,"Overskridelse af kriteriet",null,null,null,null,null,"fugacitets-beregning ud fra jordprøve",null,null,null,"Grundvands-kvalitets-kriterium",null,null,"Overskridelse af kriteriet",null,null,null,null,"fugacitets-beregning ud fra jordprøve",null,null,null,"Afdampnings-kriterium",null,null,"Overskridelse af kriteriet"]
[]
[]
[null,null,null,null,null,null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"gange",null,null,null,null,null,"µg/l",null,null,"µg/l",null,null,"gange",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,"gange"]
[null,"Sum af kulbrinter C6-C35",null,null,null,null,null,null,null,null,{"$f":"D_Olie_1a","v":0},null,null,{"$f":"D_Olie_1_jkk","v":100},null,null,{"$f":"D_Olie_1_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_1_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_1_gkk","v":9},null,null,{"$f":"D_Olie_1_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_1_cl","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_1_ak","v":0.1},null,null,{"$f":"D_Olie_1_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
["Kulbrintefraktioner"]
[null,"C6-C10",null,null,null,null,null,null,null,null,{"$f":"D_Olie_510a","v":0},null,null,{"$f":"D_Olie_510_jkk","v":25},null,null,{"$f":"D_Olie_510_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_510_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_510_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"C10-C15",null,null,null,null,null,null,null,null,{"$f":"D_Olie_1015a","v":0},null,null,{"$f":"D_Olie_1015_jkk","v":40},null,null,{"$f":"D_Olie_1015_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_1015_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_1015_cl","v":{"$error":"#DIV/0!"}}]
[null,"C15-C20",null,null,null,null,null,null,null,null,{"$f":"D_Olie_1520a","v":0},null,null,{"$f":"D_Olie_1520_jkk","v":55},null,null,{"$f":"D_Olie_1520_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_1520_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_1520_cl","v":{"$error":"#DIV/0!"}}]
[null,"C20-C35",null,null,null,null,null,null,null,null,{"$f":"D_Olie_2040a","v":0},null,null,{"$f":"D_Olie_2040_jkk","v":100},null,null,{"$f":"D_Olie_2040_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_2040_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_2040_cl","v":{"$error":"#DIV/0!"}}]
[]
["Aromatiske kulbrinter "]
[null,"C9-C10 aromatiske kulbrinter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_olie_910_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_olie_910_gkk","v":1},null,null,{"$f":"D_olie_910_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_910_cl","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_60_ak","v":0.03},null,null,{"$f":"D_Olie_60_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
[]
["BTEX'er",null,null,null,null,null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"gange",null,null,null,null,null,"µg/l",null,null,"µg/l",null,null,"gange",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,"gange"]
[null,"Benzen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_52a","v":0},null,null,{"$f":"D_Olie_52_jkk","v":1.5},null,null,{"$f":"D_Olie_52_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_52_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_52_gkk","v":1},null,null,{"$f":"D_Olie_52_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},null,null,{"$f":"D_Olie_52_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
[null,"Toluen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_54a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_54_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_54_gkk","v":5},null,null,{"$f":"D_Olie_54_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_54_ak","v":0.4},null,null,{"$f":"D_Olie_54_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
[null,"Ethylbenzen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_58a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_58_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,null,"o-Xylen",null,null,null,null,null,null,null,{"$f":"D_Olie_571a","v":0}]
[null,null,"m+p-Xylen",null,null,null,null,null,null,null,{"$f":"D_Olie_572a","v":0}]
[null,"Sum Xylener",null,null,null,null,null,null,null,null,{"$f":"D_Olie_57a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_57_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_57_gkk","v":5},null,null,{"$f":"D_Olie_57_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_57_ak","v":0.1},null,null,{"$f":"D_Olie_57_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
[null,"Naphtalen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_103a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_103_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_103_gkk","v":1},null,null,{"$f":"D_Olie_103_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_103_ak","v":0.04},null,null,{"$f":"D_Olie_103_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
[]
["Polyaromatiske Kulbrinter (PAH)",null,null,null,null,null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"gange",null,null,null,null,null,"µg/l",null,null,"µg/l",null,null,"gange",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,"gange"]
[null,"Benzo(ghi)perylen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_258a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_258_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Fluoranthen",null,null,null,null,"J",null,null,null,{"$f":"D_Olie_156a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_156_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_156_gkk","v":0.1},null,null,{"$f":"D_Olie_156_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Benzo(a)pyren",null,null,null,null,"J",null,null,null,{"$f":"D_Olie_256a","v":0},null,null,{"$f":"D_Olie_256_jkk","v":0.3},null,null,{"$f":"D_Olie_256_jkk_overskr","v":"Nej"},null,null,null,null,null,{"$f":"D_Olie_256_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_256_gkk","v":0.01},null,null,{"$f":"D_Olie_256_gkk_overskr","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Benzo(b+j+k)fluoranthen",null,null,null,null,"J",null,null,null,{"$f":"D_Olie_255a","v":0},null,null,null,null,null,null,null,null,null,null,"V",{"$f":"D_Olie_255_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dibenz(a,h)anthracen",null,null,null,null,"J",null,null,null,{"$f":"D_Olie_257a","v":0},null,null,{"$f":"D_Olie_257_jkk","v":0.3},null,null,{"$f":"D_Olie_257_jkk_overskr","v":"Nej"},null,null,null,null,"V",{"$f":"D_Olie_257_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Indeno(1,2,3-cd)pyren",null,null,null,null,"J",null,null,null,{"$f":"D_Olie_352a","v":0},null,null,null,null,null,null,null,null,null,null,"V",{"$f":"D_Olie_352_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af 7 PAH'er jord",null,null,null,null,"J",null,null,null,{"$f":"D_Olie_20a","v":0},null,null,{"$f":"D_Olie_20_jkk","v":4},null,null,{"$f":"D_Olie_20_jkk_overskr","v":"Nej"}]
[null,"Sum af 4 PAH'er vand",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V",{"$f":"D_Olie_21_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_21_gkk","v":0.1},null,null,{"$f":"D_Olie_21_gkk_overskr","v":{"$error":"#DIV/0!"}}]
[]
[]
["NSO-forbindelser",null,null,null,null,null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"mg/kg TS",null,null,"gange",null,null,null,null,null,"µg/l",null,null,"µg/l",null,null,"gange",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,"gange"]
[null,"Benzo(b)thiophen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_10a","v":0.02},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_10_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dibenzofuran",null,null,null,null,null,null,null,null,{"$f":"D_Olie_11a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_11_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dibenzothiophen",null,null,null,null,null,null,null,null,{"$f":"D_Olie_12a","v":5.0000000000000001E-3},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_12_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Acridin",null,null,null,null,null,null,null,null,{"$f":"D_Olie_13a","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_13_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Carbazol",null,null,null,null,null,null,null,null,{"$f":"D_Olie_14a","v":0.01},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_14_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Anilin",null,null,null,null,null,null,null,null,{"$f":"D_Olie_15a","v":1E-4},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_15_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dimethyldisulfid",null,null,null,null,null,null,null,null,{"$f":"D_Olie_16a","v":5.0000000000000001E-3},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_16_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}}]
[]
[]
[]
["Fri fase?",null,null,null,null,null,null,{"$f":"D_Olie_FF","v":"Nej"}]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"D_Olie_bruger","v":"Nej"}]

{"sheet":"Dataark_Oliestoffer","index":33,"n_rows":119,"n_cols":21,"rows_kept":119,"cut":false,"hidden":true,"merged":[[1,1,1,17],[3,1,3,9],[8,1,8,9],[22,2,22,17],[29,15,29,17],[115,8,115,9],[5,6,5,7],[6,6,6,7],[29,6,29,11],[29,12,29,14],[113,1,113,9]]}
[]
[null,"Dataark Oliestoffer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Stamdata"]
[]
[null,null,"Målepunkt",null,null,null,{"$f":"IF(ISBLANK(Olie_målepunkt),\"\",Olie_målepunkt)","v":""}]
[null,null,"Dato",null,null,null,{"$f":"IF(ISBLANK(Olie_dato),\"\",Olie_dato)","v":""}]
[]
[null,"Jord"]
[]
[null,null,"Navn",null,"Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes"]
[null,null,"Jordtype",null,null,null,null,null,{"$f":"Olie_My_jordtype","v":0},{"$f":"IF(ISTEXT(I12),I12,H12)","v":0},null,null,null,null,null,null,null,null,null,"D_Olie_jordtype","input"]
[null,null,"Poreluftvolumen",null,"VL",null,null,null,{"$f":"IF(ISNUMBER(Olie_My_VL),Olie_My_VL,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(I13),I13,H13)","v":0},null,null,null,null,null,null,null,null,null,"D_Olie_VL","input"]
[null,null,"Vand-indhold",null,"VV",null,null,null,{"$f":"IF(ISNUMBER(Olie_My_VV),Olie_My_VV,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(I14),I14,H14)","v":0},null,null,null,null,null,null,null,null,null,"D_Olie_VV","input"]
[null,null,"Samlet\nporøsitet",null,"e=VT=VL+VV",null,null,null,null,{"$f":"B_Olie_e","v":0},null,null,null,null,null,null,null,null,null,"D_Olie_e","beregnes"]
[null,null,"Volumen af jordskellet",null,"VJ",null,null,null,null,{"$f":"B_Olie_VJ","v":1},null,null,null,null,null,null,null,null,null,"D_Olie_VJ","beregnes"]
[null,null,"Kornrumvægt",null,"d","kg/l",null,null,{"$f":"Olie_My_d","v":0},{"$f":"IF(VALUE(I17),I17,H17)","v":0},null,null,null,null,null,null,null,null,null,"D_Olie_d","input"]
[null,null,"Volumenvægt",null,"r","kg/l",null,null,null,{"$f":"B_Olie_p","v":0},null,null,null,null,null,null,null,null,null,"D_Olie_p","beregnes"]
[null,null,"Indhold af organisk kulstof",null,"foc",null,null,null,{"$f":"Olie_My_foc","v":0},0,null,null,null,null,null,null,null,null,null,"D_Olie_foc","input"]
[null,null,"Anvendt brugerdata",null,null,null,null,null,{"$f":"SUM(I13:I19)","v":0},{"$f":"IF(I20>0,\"Ja\",\"Nej\")","v":"Nej"},null,null,null,null,null,null,null,null,null,"D_Olie_bruger","beregnes i dataark"]
[]
[]
[null,null,"Oliekomponent"]
[]
[null,null,null,null,null,null,"Olie/benzin","Tung olie","Modificeret","Anvendes"]
[null,null,"Valgt olieprofil",null,null,null,true,false,null,{"$f":"IF(D_Olie_olieprofil=TRUE,1,IF(D_Olie_tungolieprofil=TRUE,2,IF(D_Olie_modificeretprofil=TRUE,3,0)))","v":1}]
[]
[null,null,null,null,null,"Systemnavn","D_Olie_x","D_Olie_xv","D_Olie_xa","D_Olie_x_jkk","D_Olie_x_jkk_overskr",null,"D_Olie_x_cv","D_Olie_x_gkk","D_Olie_x_gkk_overskr","D_Olie_x_cl","D_Olie_x_ak","D_Olie_x_ak_overskr"]
[]
[null,null,"Koncentration af oliekomponent",null,null,null,"I jord",null,null,null,null,null,"I porevand",null,null,"I poreluft"]
[null,null,null,null,null,null,"Indtastet","Værdi","Anvendt konc Ct","Jord \nkvalitets-kriterium","Overskridelse af kriterium","Afskæringskriterium","Beregnet konc Cv","Grundv. \nkvalitets-kriterium","Overskridelse af kriterium","Beregnet konc Cl","Afdamp-nings-kriterium","Overskridelse af kriterium"]
[null,50,"C5-C6",null,null,null,null,null,{"$f":"B_Olie_50_ct","v":0},null,null,null,{"$f":"B_Olie_50_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_50_cl","v":{"$error":"#DIV/0!"}}]
[null,51,">5 - 6, alifater","2-methylbutan",null,null,null,null,{"$f":"B_Olie_51_ct","v":0},null,null,null,{"$f":"B_Olie_51_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_51_cl","v":{"$error":"#DIV/0!"}}]
[null,511,null,"Pentan",null,null,null,null,{"$f":"B_Olie_511_ct","v":0},null,null,null,{"$f":"B_Olie_511_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_511_cl","v":{"$error":"#DIV/0!"}}]
[null,512,null,"2-methylpentan",null,null,null,null,{"$f":"B_Olie_512_ct","v":0},null,null,null,{"$f":"B_Olie_512_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_512_cl","v":{"$error":"#DIV/0!"}}]
[null,513,null,"3-methylpentan (C6)",null,null,null,null,{"$f":"B_Olie_513_ct","v":0},null,null,null,{"$f":"B_Olie_513_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_513_cl","v":{"$error":"#DIV/0!"}}]
[null,510,"C6-C10",null,null,null,{"$f":"Olie_510","v":0},{"$f":"IF(Olie_510<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_510_ct","v":0},25,{"$f":"B_Olie_510_jkk_overskr","v":"Nej"},null,{"$f":"B_Olie_510_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_510_cl","v":{"$error":"#DIV/0!"}}]
[null,52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"Olie_52","v":0},{"$f":"IF(Olie_52<>\"\", TRUE,FALSE)","v":false},{"$f":"B_Olie_52_ct","v":0},1.5,{"$f":"B_Olie_52_jkk_overskr","v":"Nej"},null,{"$f":"B_Olie_52_cv","v":{"$error":"#DIV/0!"}},1,{"$f":"B_Olie_52_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_52_cl","v":{"$error":"#DIV/0!"}},1.2999999999999999E-4,{"$f":"B_Olie_52_ak_overskr","v":{"$error":"#DIV/0!"}}]
[null,53,">6 - 8, alifater",">6 - 8, alifater",null,null,null,null,{"$f":"B_Olie_53_ct","v":0},null,null,null,{"$f":"B_Olie_53_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_53_cl","v":{"$error":"#DIV/0!"}}]
[null,54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"Olie_54","v":0},{"$f":"IF(Olie_54<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_54_ct","v":0},null,{"$f":"B_Olie_54_jkk_overskr","v":"Nej"},null,{"$f":"B_Olie_54_cv","v":{"$error":"#DIV/0!"}},5,{"$f":"B_Olie_54_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_54_cl","v":{"$error":"#DIV/0!"}},0.4,{"$f":"B_Olie_54_ak_overskr","v":{"$error":"#DIV/0!"}}]
[null,"55A",">8 - 10, alifater",">8 - 10, alifater, Tung olie",null,null,null,null,{"$f":"B_Olie_55A_ct","v":0},null,null,null,{"$f":"B_Olie_55A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_55A_cl","v":{"$error":"#DIV/0!"}}]
[null,"55B",null,">8 - 10, alifater, Olieblandinger",null,null,null,null,{"$f":"B_Olie_55B_ct","v":0},null,null,null,{"$f":"B_Olie_55B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_55B_cl","v":{"$error":"#DIV/0!"}}]
[null,56,">8 -10, aromater","Sum >8-10, aromater",null,null,null,null,{"$f":"B_Olie_56_ct","v":0}]
[null,571,null,"o-Xylen",null,null,{"$f":"Olie_571","v":0},{"$f":"IF(Olie_571<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_571_ct","v":0}]
[null,572,null,"m+p-Xylen",null,null,{"$f":"Olie_572","v":0},{"$f":"IF(Olie_572<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_572_ct","v":0}]
[null,57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"Olie_57","v":0},{"$f":"IF(Olie_57<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_57_ct","v":0},null,{"$f":"B_Olie_57_jkk_overskr","v":"Nej"},null,{"$f":"B_Olie_57_cv","v":{"$error":"#DIV/0!"}},5,{"$f":"B_Olie_57_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_57_cl","v":{"$error":"#DIV/0!"}},0.1,{"$f":"B_Olie_57_ak_overskr","v":{"$error":"#DIV/0!"}}]
[null,58,null,"Ethylbenzen (C8)",null,null,{"$f":"Olie_58","v":0},{"$f":"IF(Olie_58<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_58_ct","v":0},null,null,null,{"$f":"B_Olie_58_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_58_cl","v":{"$error":"#DIV/0!"}}]
[null,59,null,"1,3,5-trimethylbenzen (C9)",null,null,null,null,{"$f":"B_Olie_59_ct","v":0},null,null,null,{"$f":"B_Olie_59_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_59_cl","v":{"$error":"#DIV/0!"}}]
[null,"60A",null,">8-10, aromater, øvrige, Tung olie",null,null,null,null,{"$f":"B_Olie_60A_ct","v":0},null,null,null,{"$f":"B_Olie_60A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_60A_cl","v":{"$error":"#DIV/0!"}}]
[null,"60B",null,">8 -10, aromater,øvrige, Olieblanding",null,null,null,null,{"$f":"B_Olie_60B_ct","v":0},null,null,null,{"$f":"B_Olie_60B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_60B_cl","v":{"$error":"#DIV/0!"}}]
[null,60,null,">8 -10, aromater,øvrige, Samlet",null,null,null,null,null,null,null,null,{"$f":"MAX(M49:M50)","v":{"$error":"#DIV/0!"}},1,{"$f":"B_Olie_60_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"MAX(P49:P50)","v":{"$error":"#DIV/0!"}}]
[null,910,null,null,null,null,null,null,null,null,null,"C9-C10 aromatiske kulbrinter",{"$f":"SUM(D_olie_60_cv,D_Olie_59_cv)","v":{"$error":"#DIV/0!"}},1,{"$f":"B_olie_910_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_60_cl+D_Olie_59_cl","v":{"$error":"#DIV/0!"}},0.03,{"$f":"B_Olie_60_ak_overskr","v":{"$error":"#DIV/0!"}}]
[null,1015,"C11-C15",null,null,null,{"$f":"Olie_1015","v":0},{"$f":"IF(Olie_1015<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_1015_ct","v":0},40,{"$f":"B_Olie_1015_jkk_overskr","v":"Nej"},{"$error":"#N/A"},{"$f":"B_Olie_1015_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_1015_cl","v":{"$error":"#DIV/0!"}}]
[null,101,">10 - 12, alifater","Dodecan(C12)",null,null,null,null,{"$f":"B_Olie_101_ct","v":0},null,null,null,{"$f":"B_Olie_101_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_101_cl","v":{"$error":"#DIV/0!"}}]
[null,102,">10 - 12, aromater","Sum >10 - 12 aromater",null,null,null,null,{"$f":"B_Olie_102_ct","v":0}]
[null,103,null,"Naphthalen (C10)",null,null,{"$f":"Olie_103","v":0},{"$f":"IF(Olie_103<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_103_ct","v":0},null,null,{"$error":"#N/A"},{"$f":"B_Olie_103_cv","v":{"$error":"#DIV/0!"}},1,{"$f":"B_Olie_103_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_103_cl","v":{"$error":"#DIV/0!"}},0.04,{"$f":"B_Olie_103_ak_overskr","v":{"$error":"#DIV/0!"}}]
[null,"104A",null,">10 - 12, aromater, øvrige, Tung Olie",null,null,null,null,{"$f":"B_Olie_104A_ct","v":0},null,null,null,{"$f":"B_Olie_104A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_104A_cl","v":{"$error":"#DIV/0!"}}]
[null,"104B",null,">10 - 12, aromater, øvrige, Olieblanding",null,null,null,null,{"$f":"B_Olie_104B_ct","v":0},null,null,null,{"$f":"B_Olie_104B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_104B_cl","v":{"$error":"#DIV/0!"}}]
[null,"105A",">12 - 16, alifater",">12 - 16, alifater, Tung Olie",null,null,null,null,{"$f":"B_Olie_105A_ct","v":0},null,null,null,{"$f":"B_Olie_105A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_105A_cl","v":{"$error":"#DIV/0!"}}]
[null,"105B",null,">12 - 16, alifater, Olieblandinger",null,null,null,null,{"$f":"B_Olie_105B_ct","v":0},null,null,null,{"$f":"B_Olie_105B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_105B_cl","v":{"$error":"#DIV/0!"}}]
[null,106,">12 - 16, aromater","Sum >10 - 12 aromater",null,null,null,null,{"$f":"B_Olie_106_ct","v":0}]
[null,107,null,"Acenaphthylen (C12)",null,null,null,null,{"$f":"B_Olie_107_ct","v":0},null,null,null,{"$f":"B_Olie_107_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_107_cl","v":{"$error":"#DIV/0!"}}]
[null,108,null,"Acenaphthen (C12)",null,null,null,null,{"$f":"B_Olie_108_ct","v":0},null,null,null,{"$f":"B_Olie_108_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_108_cl","v":{"$error":"#DIV/0!"}}]
[null,"109A",null,">12 - 16, aromater,øvrige, Tung Olie",null,null,null,null,{"$f":"B_Olie_109A_ct","v":0},null,null,null,{"$f":"B_Olie_109A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_109A_cl","v":{"$error":"#DIV/0!"}}]
[null,"109B",null,">12 - 16, aromater,øvrige, Olieblandinger",null,null,null,null,{"$f":"B_Olie_109B_ct","v":0},null,null,null,{"$f":"B_Olie_109B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_109B_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,1520,"C16-C20",null,null,null,{"$f":"Olie_1520","v":0},{"$f":"IF(Olie_1520<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_1520_ct","v":0},55,{"$f":"B_Olie_1520_jkk_overskr","v":"Nej"},{"$error":"#N/A"},{"$f":"B_Olie_1520_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_1520_cl","v":{"$error":"#DIV/0!"}}]
[null,"151A",">16 - 21, alifater",">16 - 21, alifater, Tung Olie",null,null,null,null,{"$f":"B_Olie_151A_ct","v":0},null,null,null,{"$f":"B_Olie_151A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_151A_cl","v":{"$error":"#DIV/0!"}}]
[null,"151B",null,">16 - 21, alifater, Olieblandinger",null,null,null,null,{"$f":"B_Olie_151B_ct","v":0},null,null,null,{"$f":"B_Olie_151B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_151B_cl","v":{"$error":"#DIV/0!"}}]
[null,152,">16 - 21, aromater","Sum >16 - 21 aromater",null,null,null,null,{"$f":"B_Olie_152_ct","v":0}]
[null,153,null,"Fluoren (C13)",null,null,null,null,{"$f":"B_Olie_153_ct","v":0},null,null,null,{"$f":"B_Olie_153_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_153_cl","v":{"$error":"#DIV/0!"}}]
[null,154,null,"Phenanthren (C14)",null,null,null,null,{"$f":"B_Olie_154_ct","v":0},null,null,null,{"$f":"B_Olie_154_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_154_cl","v":{"$error":"#DIV/0!"}}]
[null,155,null,"Anthracen (C14)",null,null,null,null,{"$f":"B_Olie_155_ct","v":0},null,null,null,{"$f":"B_Olie_155_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_155_cl","v":{"$error":"#DIV/0!"}}]
[null,156,null,"Fluoranthen (C16)",null,null,{"$f":"Olie_156","v":0},{"$f":"IF(Olie_156<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_156_ct","v":0},null,null,null,{"$f":"B_Olie_156_cv","v":{"$error":"#DIV/0!"}},0.1,{"$f":"B_Olie_156_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_156_cl","v":{"$error":"#DIV/0!"}}]
[null,157,null,"Pyren (C16)",null,null,null,null,{"$f":"B_Olie_157_ct","v":0},null,null,null,{"$f":"B_Olie_157_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_157_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,2025,"C21-C25",null,null,null,null,false,{"$f":"B_Olie_2025_ct","v":0},null,null,null,{"$f":"B_Olie_2025_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_2025_cl","v":{"$error":"#DIV/0!"}}]
[null,"201A",">21 - 25, alifater",">21 - 25, alifater, Tung olie",null,null,null,null,{"$f":"B_Olie_201A_ct","v":0},null,null,null,{"$f":"B_Olie_201A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_201A_cl","v":{"$error":"#DIV/0!"}}]
[null,"201B",null,">21 - 25, alifater, Olieblandinger",null,null,null,null,{"$f":"B_Olie_201B_ct","v":0},null,null,null,{"$f":"B_Olie_201B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_201B_cl","v":{"$error":"#DIV/0!"}}]
[null,202,">21 - 25, aromater","Ingen repræsentanter",null,null,null,null,{"$f":"B_Olie_202_ct","v":0}]
[null,2535,"C25-C35",null,null,null,{"$f":"Olie_2535","v":{"$error":"#NAME?"}},{"$f":"IF(Olie_2535<>\"\",TRUE,FALSE)","v":{"$error":"#NAME?"}},{"$f":"B_Olie_2535_ct","v":0},null,null,null,{"$f":"B_Olie_2535_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_2535_cl","v":{"$error":"#DIV/0!"}}]
[null,"251A",">25 - 35, alifater",">25 - 35, alifater, Tung olie",null,null,null,null,{"$f":"B_Olie_251A_ct","v":0},null,null,null,{"$f":"B_Olie_251A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_251A_cl","v":{"$error":"#DIV/0!"}}]
[null,"251B",null,">25 - 35, alifater, Olieblandinger",null,null,null,null,{"$f":"B_Olie_251B_ct","v":0},null,null,null,{"$f":"B_Olie_251B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_251B_cl","v":{"$error":"#DIV/0!"}}]
[null,252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,{"$f":"B_Olie_252_ct","v":0}]
[null,253,null,"Benzo(a)anthracen (C18)",null,null,null,null,{"$f":"B_Olie_253_ct","v":0},null,null,null,{"$f":"B_Olie_253_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_253_cl","v":{"$error":"#DIV/0!"}}]
[null,254,null,"Chrysen (C18)",null,null,null,null,{"$f":"B_Olie_254_ct","v":0},null,null,null,{"$f":"B_Olie_254_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_254_cl","v":{"$error":"#DIV/0!"}}]
[null,255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"Olie_255","v":0},{"$f":"IF(Olie_255<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_255_ct","v":0},null,null,null,{"$f":"B_Olie_255_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_255_cl","v":{"$error":"#DIV/0!"}}]
[null,256,null,"Benzo(a)pyren",null,null,{"$f":"Olie_256","v":0},{"$f":"IF(Olie_256<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_256_ct","v":0},0.3,{"$f":"B_Olie_256_jkk_overskr","v":"Nej"},3,{"$f":"B_Olie_256_cv","v":{"$error":"#DIV/0!"}},0.01,{"$f":"B_Olie_256_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_256_cl","v":{"$error":"#DIV/0!"}}]
[null,257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"Olie_257","v":0},{"$f":"IF(Olie_257<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_257_ct","v":0},0.3,{"$f":"B_Olie_257_jkk_overskr","v":"Nej"},3,{"$f":"B_Olie_257_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_257_cl","v":{"$error":"#DIV/0!"}}]
[null,258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"Olie_258","v":0},{"$f":"IF(Olie_258<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_258_ct","v":0},null,null,null,{"$f":"B_Olie_258_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_258_cl","v":{"$error":"#DIV/0!"}}]
[null,"259A",null,">25 - 35, aromater, øvrige, Tung olie",null,null,null,null,{"$f":"B_Olie_259A_ct","v":0},null,null,null,{"$f":"B_Olie_259A_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_259A_cl","v":{"$error":"#DIV/0!"}}]
[null,"259B",null,">25 - 35, aromater, øvrige, Olieblandinger",null,null,null,null,{"$f":"B_Olie_259B_ct","v":0},null,null,null,{"$f":"B_Olie_259B_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_259B_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,3540,">C35",null,null,null,null,false,{"$f":"B_Olie_3540_ct","v":0},null,null,null,{"$f":"B_Olie_3540_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_3540_cl","v":{"$error":"#DIV/0!"}}]
[null,351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,null,null,{"$f":"B_Olie_351_ct","v":0},null,null,null,{"$f":"B_Olie_351_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_351_cl","v":{"$error":"#DIV/0!"}}]
[null,352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"Olie_352","v":0},{"$f":"IF(Olie_352<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_352_ct","v":0},null,null,null,{"$f":"B_Olie_352_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_352_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,2040,"C21-C35",null,null,null,{"$f":"Olie_2040","v":0},{"$f":"IF(Olie_2040<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_2040_ct","v":0},100,{"$f":"B_Olie_2040_jkk_overskr","v":"Nej"},{"$error":"#N/A"},{"$f":"B_Olie_2040_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_2040_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,20,"Sum af 7 PAH'er jord",null,null,null,null,null,{"$f":"B_Olie_20_ct","v":0},4,{"$f":"B_Olie_20_jkk_overskr","v":"Nej"},40]
[null,21,"Sum af 4 PAH'er vand",null,null,null,null,null,null,null,null,null,{"$f":"B_Olie_21_cv","v":{"$error":"#DIV/0!"}},0.1,{"$f":"B_Olie_21_gkk_overskr","v":{"$error":"#DIV/0!"}}]
[]
[null,null,"NSO-forbindelser"]
[null,10,null,"Benzo(b)thiophen",null,null,{"$f":"Olie_10","v":0},{"$f":"IF(Olie_10<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_10_ct","v":0.02},null,null,null,{"$f":"B_Olie_10_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_10_cl","v":{"$error":"#DIV/0!"}}]
[null,11,null,"Dibenzofuran",null,null,{"$f":"Olie_11","v":0},{"$f":"IF(Olie_11<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_11_ct","v":0},null,null,null,{"$f":"B_Olie_11_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_11_cl","v":{"$error":"#DIV/0!"}}]
[null,12,null,"Dibenzothiophen",null,null,{"$f":"Olie_12","v":0},{"$f":"IF(Olie_12<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_12_ct","v":5.0000000000000001E-3},null,null,null,{"$f":"B_Olie_12_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_12_cl","v":{"$error":"#DIV/0!"}}]
[null,13,null,"Acridin",null,null,{"$f":"Olie_13","v":0},{"$f":"IF(Olie_13<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_13_ct","v":0},null,null,null,{"$f":"B_Olie_13_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_13_cl","v":{"$error":"#DIV/0!"}}]
[null,14,null,"Carbazol",null,null,{"$f":"Olie_14","v":0},{"$f":"IF(Olie_14<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_14_ct","v":0.01},null,null,null,{"$f":"B_Olie_14_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_14_cl","v":{"$error":"#DIV/0!"}}]
[null,15,null,"Anilin",null,null,{"$f":"Olie_15","v":0},{"$f":"IF(Olie_15<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_15_ct","v":1E-4},null,null,null,{"$f":"B_Olie_15_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_15_cl","v":{"$error":"#DIV/0!"}}]
[null,16,null,"Dimethyldisulfid",null,null,{"$f":"Olie_16","v":0},{"$f":"IF(Olie_16<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_16_ct","v":5.0000000000000001E-3},null,null,null,{"$f":"B_Olie_16_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Olie_16_cl","v":{"$error":"#DIV/0!"}}]
[]
[null,1,"Sum af kulbrinter C6-C35",null,null,null,{"$f":"Olie_1","v":0},{"$f":"IF(Olie_1<>\"\",TRUE,FALSE)","v":false},{"$f":"B_Olie_1_ct","v":0},100,{"$f":"B_Olie_1_jkk_overskr","v":"Nej"},{"$error":"#N/A"},{"$f":"B_Olie_1_cv","v":{"$error":"#DIV/0!"}},9,{"$f":"B_Olie_1_gkk_overskr","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_1_cl","v":{"$error":"#DIV/0!"}},0.1,{"$f":"B_Olie_1_ak_overskr","v":{"$error":"#DIV/0!"}}]
[]
[null,"Bemærkninger"]
[]
[null,null,"Det forurenede område:","D_Olie_Jord_ComUds",null,null,null,"Mulighed for fri fase?",{"$f":"B_Olie_FF","v":"Nej"}]
[null,null,null,false]
[null,null,"Kemisk analyse","D_Olie_Kem_ComUds"]
[null,null,null,false]

{"sheet":"Beregning_Oliestoffer","index":34,"n_rows":195,"n_cols":49,"rows_kept":195,"cut":false,"hidden":true,"merged":[[14,47,17,47],[14,38,14,41],[14,36,17,36],[14,37,17,37],[15,32,16,32],[14,29,14,34],[14,23,14,25],[14,15,14,22],[14,26,14,28],[14,42,14,44],[14,46,17,46],[116,10,116,11],[14,4,14,14],[116,4,116,5],[116,6,116,7],[116,8,116,9]]}
[null,null,null,"Beregningsark Oliestoffer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PAH'er",null,"((1-B_Olie_e)*10^(0,989*V19-0,346)*B_Olie_foc*B_Olie_d)/(U19)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NSO'er",null,"((1-B_Olie_e)*10^(1,04*V19-0,84)*B_Olie_foc*B_Olie_d)/(U19)"]
[null,null,null,"Jordparametre"]
[null,null,null,"Navn","Forkortelse","Enhed","Overført fra","Værdi","Beregnet",null,null,null,null,null,null,null,null,null,null,null,null,"Alifater",null,"((1-B_Olie_e)*10^(0,45*C19+0,43)*B_Olie_foc*B_Olie_d)/(U19)",null,null,null,null,null,{"$f":"AD27/AD5","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,{"$f":"AM27/AM5","v":{"$error":"#DIV/0!"}}]
[null,null,null,"Jordtype",null,null,"Oliestoffer",{"$f":"D_Olie_jordtype","v":0},null,"B_Olie_jordtype",null,null,null,null,null,null,null,null,null,null,null,"aromater",null,"((1-B_Olie_e)*10^(0,10*C19+2,3)*B_Olie_foc*B_Olie_d)/(U19)",null,null,null,null,null,1.26,null,null,null,null,null,null,null,null,0.30099999999999999]
[null,null,null,"Poreluftvolumen","VL",null,"Oliestoffer",{"$f":"D_Olie_VL","v":0},null,"B_Olie_VL",null,null,null,null,null,null,null,null,null,null,null,null,null,"((1-B_Olie_e)*10^(0,72*V19+0,49)*B_Olie_foc*B_Olie_d)/(U19)",null,null,null,null,null,{"$f":"AD29/AD7","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,{"$f":"AM29/AM7","v":{"$error":"#DIV/0!"}}]
[null,null,null,"Vandindhold","VV",null,"Oliestoffer",{"$f":"D_Olie_VV","v":0},null,"B_Olie_VV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.83,null,null,null,null,null,null,null,null,0.23899999999999999]
[null,"EC=4,12+0,02*R19+(0,000065*R19*R19)",null,"Samlet\nporøsitet","e=VT=VL+VV",null,null,{"$f":"I8","v":0},{"$f":"B_Olie_VL+B_Olie_VV","v":0},"B_Olie_e",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AM31/AM9","v":{"$error":"#DIV/0!"}}]
[null,null,null,"Volumen af jordskellet","VJ",null,"Oliestoffer",{"$f":"I9","v":1},{"$f":"1-B_Olie_e","v":1},"B_Olie_VJ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,3.3459575960034537E-3,null,null,null,null,null,null,null,null,5108]
[null,null,null,"Kornrumvægt","d","kg/l","Oliestoffer",{"$f":"D_Olie_d","v":0},null,"B_Olie_d",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5,8.6157036027822934E-3]
[null,null,null,"Volumenvægt","r","kg/l","Oliestoffer",{"$f":"I11","v":0},{"$f":"B_Olie_d*B_Olie_VJ","v":0},"B_Olie_p",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,8.5334275511565211E-3]
[null,null,null,"Indhold af organisk kulstof","foc",null,"Oliestoffer",{"$f":"D_Olie_foc/100","v":0},null,"B_Olie_foc",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"O37*$J111","v":0}]
[]
["Beregning af stoffordeling af kulbrinter i jord, vand og poreluft i den umættede zone",null,null,null,null,null,null,null,null,"B_Olie_x_ct",null,"B_Olie_x_jkk_overskr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B_Olie_x_cv",null,null,null,null,"B_Olie_x_gkk_overskr",null,null,null,null,null,null,null,"B_Olie_x_cl",null,"B_Olie_x_ak_overskr"]
[null,null,null,null,"Jordprøve",null,null,null,null,null,null,null,null,null,null,"Fysiskkemiske data",null,null,null,null,null,null,null,"Stofandel",null,null,"Fordeling i umættet jordzone",null,null,"Cv",null,null,null,null,null,null,"Grundvands-kriterie","Overskridelse af kriterium","CL (Jord til poreluft)",null,null,null,"CL (Vand til poreluft)",null,null,"CL","Afdampnings-kriterie","Overskridelse af kriterium"]
[null,"Interval","EC nummer","Modelstof","Olieprofil","Profil mellem-regning","Korrigeret\nprofil","Beregnet\nkoncentration","Analyseret koncentration","Anvændt mængde","Jordkvalitets-kriterium","Overskridelse af kriterium","Fordeling af tot. Konc.",null,"Molbrøk","Molvægt","Tryk v. 25 C","Koge-punkt","Tryk v. 10 C","Vand-opløselig-hed","Henrys konstant","Okt./vand-forhold","Diffusionskoef.","på jord","i porevand","i poreluft","Jord %","Vand %","Luft %","teori","max","Risiko for fri fase","Porevands-konc.\nCv",null,"Ai, vand","Molbrøk",null,null,"teori","max","Poreluft-koncentration","Uden C5 fraktion","teori fra vand","max fra vand","Poreluft-konc., fra vand","Maks. Poreluft-koncentration"]
[null,null,null,null,null,null,null,"Ct-b","Ct-a","Ct",null,null,"v","Ai"," m.b.","m","p, 25 C","k.p.","p, 10 C","S","H","log Kow","DL","Mj,max","Mv,max","ML,max"]
[null,null,null,null,null,null,null,"(mg/kg)","(mg/kg)","(mg/kg)",null,null,"(%)",null,null,"(g/mol)","(kPa)","( C)","(kPa)","(mg/l)","(KPam3/mol)"," ","(m2/s)"," "," "," "," "," "," ","µg/l","µg/l",null,"µg/l","%",null,null,null,null,"(mg/m³)","(mg/m³)","(mg/m³)","(mg/m³)","mg/m3","mg/m3","mg/m3","(mg/m³)"]
[50,">C5 - C6",null,null,{"$f":"B_Olie_50_anv","v":1.8479560556049979E-2},{"$f":"IF(ISNUMBER(I19),0,E19)","v":1.8479560556049979E-2},{"$f":"E19","v":1.8479560556049979E-2},{"$f":"(H$109*G19)","v":0},null,{"$f":"H19","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum C5",null,{"$f":"SUM(AG20:AG23)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI20:AI23)","v":{"$error":"#DIV/0!"}},null,null,null,null,"Sum C5",{"$f":"SUM(AO20:AO23)","v":{"$error":"#DIV/0!"}},null,null,"Sum C5",{"$f":"SUM(AS20:AS23)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT20:AT23)","v":{"$error":"#DIV/0!"}}]
[51,">5 - 6, alifater",{"$f":"4.12+0.02*R20+(0.000065*R20*R20)","v":4.7262345999999997},"2-methylbutan",{"$f":"B_Olie_51_anv","v":3.2999999999999995E-2},{"$f":"IF(ISNUMBER(I20),0,E20)","v":3.2999999999999995E-2},{"$f":"F20/F$26","v":3.3094017094017082E-2},{"$f":"(H$19*G20)","v":0},null,{"$f":"IF(I20>0,I20,H20)","v":0},null,null,{"$f":"J20*100/J$111","v":0},{"$f":"M20/P20","v":0},{"$f":"N20/N$111","v":0},72.150000000000006,91.64,27.8,{"$f":"Q20*EXP(((LN(Q20/101.325))/(0.00336-(1/(273+R20))))*0.000178)","v":55.399952757516715},48,141.86000000000001,2.72,{"$f":"0.0000084*((78.1/P20)^0.5)","v":8.7395009776804372E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C20+0.43)*B_Olie_foc*B_Olie_d)/(U20)","v":0},{"$f":"B_Olie_VV/U20","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X20/SUM(X20:Z20)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y20/SUM(X20:Z20)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z20/SUM(X20:Z20)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O20*$J111*(0.01*$AB20)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T20*O20","v":0},{"$f":"IF(AD20>AE20,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD20:AE20)","v":{"$error":"#DIV/0!"}},{"$f":"AG20*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH20/$P20","v":{"$error":"#DIV/0!"}},{"$f":"AI20/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O20*$J111*(0.01*$AC20)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O20*1000000*$S20*$P20/2353","v":0},{"$f":"MINA(AM20:AN20)","v":{"$error":"#DIV/0!"}},null,{"$f":"AJ20*$AG$111*(0.01*$AC20)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ20*1000000*$S20*$P20/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ20:AR20)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS20,AO20)","v":{"$error":"#DIV/0!"}}]
[511,null,{"$f":"4.12+0.02*R21+(0.000065*R21*R21)","v":4.9242400000000002},"Pentan",{"$f":"B_Olie_511_anv","v":1.1818181818181816E-2},{"$f":"IF(ISNUMBER(I21),0,E21)","v":1.1818181818181816E-2},{"$f":"F21/F$26","v":1.1851851851851848E-2},{"$f":"(H$19*G21)","v":0},null,{"$f":"IF(I21>0,I21,H21)","v":0},null,null,{"$f":"J21*100/J$111","v":0},{"$f":"M21/P21","v":0},{"$f":"N21/N$111","v":0},72.2,68.527697368421059,36,39.044867150968891,38,126.66,3.39,9.6725251295755997E-6,{"$f":"((1-B_Olie_e)*10^(0.45*C21+0.43)*B_Olie_foc*B_Olie_d)/(U21)","v":0},{"$f":"B_Olie_VV/U21","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X21/SUM(X21:Z21)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y21/SUM(X21:Z21)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z21/SUM(X21:Z21)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O21*$J111*(0.01*$AB21)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T21*O21","v":0},{"$f":"IF(AD21>AE21,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD21:AE21)","v":{"$error":"#DIV/0!"}},{"$f":"AG21*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH21/$P21","v":{"$error":"#DIV/0!"}},{"$f":"AI21/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O21*$J111*(0.01*$AC21)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O21*1000000*$S21*$P21/2353","v":0},{"$f":"MINA(AM21:AN21)","v":{"$error":"#DIV/0!"}},null,{"$f":"AJ21*$AG$111*(0.01*$AC21)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ21*1000000*$S21*$P21/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ21:AR21)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS21,AO21)","v":{"$error":"#DIV/0!"}}]
[512,null,{"$f":"4.12+0.02*R22+(0.000065*R22*R22)","v":5.5595625999999996},"2-methylpentan",{"$f":"B_Olie_512_anv","v":0.58409090909090899},{"$f":"IF(ISNUMBER(I22),0,E22)","v":0.58409090909090899},{"$f":"F22/F$26","v":0.58575498575498552},{"$f":"(H$19*G22)","v":0},null,{"$f":"IF(I22>0,I22,H22)","v":0},null,null,{"$f":"J22*100/J$111","v":0},{"$f":"M22/P22","v":0},{"$f":"N22/N$111","v":0},86.18,28.06,60.2,14.840503418797068,14,173.27,3.21,{"$f":"0.0000084*((78.1/P22)^0.5)","v":7.996529764863221E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C22+0.43)*B_Olie_foc*B_Olie_d)/(U22)","v":0},{"$f":"B_Olie_VV/U22","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X22/SUM(X22:Z22)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y22/SUM(X22:Z22)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z22/SUM(X22:Z22)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O22*$J111*(0.01*$AB22)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T22*O22","v":0},{"$f":"IF(AD22>AE22,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD22:AE22)","v":{"$error":"#DIV/0!"}},{"$f":"AG22*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH22/$P22","v":{"$error":"#DIV/0!"}},{"$f":"AI22/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O22*$J111*(0.01*$AC22)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O22*1000000*$S22*$P22/2353","v":0},{"$f":"MINA(AM22:AN22)","v":{"$error":"#DIV/0!"}},null,{"$f":"AJ22*$AG$111*(0.01*$AC22)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ22*1000000*$S22*$P22/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ22:AR22)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS22,AO22)","v":{"$error":"#DIV/0!"}}]
[513,null,{"$f":"4.12+0.02*R23+(0.000065*R23*R23)","v":5.6436256},"3-methylpentan (C6)",{"$f":"B_Olie_513_anv","v":0.37045454545454543},{"$f":"IF(ISNUMBER(I23),0,E23)","v":0.37045454545454543},{"$f":"F23/F$26","v":0.37150997150997145},{"$f":"(H$19*G23)","v":0},null,{"$f":"IF(I23>0,I23,H23)","v":0},null,null,{"$f":"J23*100/J$111","v":0},{"$f":"M23/P23","v":0},{"$f":"N23/N$111","v":0},86.18,25.27,63.2,13.310169612935836,17.899999999999999,170.226,3.6,{"$f":"0.0000084*((78.1/P23)^0.5)","v":7.996529764863221E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C23+0.43)*B_Olie_foc*B_Olie_d)/(U23)","v":0},{"$f":"B_Olie_VV/U23","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X23/SUM(X23:Z23)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y23/SUM(X23:Z23)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z23/SUM(X23:Z23)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O23*$J111*(0.01*$AB23)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T23*O23","v":0},{"$f":"IF(AD23>AE23,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD23:AE23)","v":{"$error":"#DIV/0!"}},{"$f":"AG23*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH23/$P23","v":{"$error":"#DIV/0!"}},{"$f":"AI23/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O23*$J111*(0.01*$AC23)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O23*1000000*$S23*$P23/2353","v":0},{"$f":"MINA(AM23:AN23)","v":{"$error":"#DIV/0!"}},null,{"$f":"AJ23*$AG$111*(0.01*$AC23)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ23*1000000*$S23*$P23/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ23:AR23)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS23,AO23)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,0,null,null,0]
[510,">C6 - C10",null,null,{"$f":"B_Olie_510_anv","v":0.47520582560016161},{"$f":"IF(D_Olie_510v=TRUE,0,E25)","v":0.47520582560016161},{"$f":"F25/F$110","v":0.47520582560016161},{"$f":"(I$110*G25)","v":0},{"$f":"D_Olie_510","v":0},{"$f":"IF(D_Olie_510v=TRUE,I25,H25)","v":0},{"$f":"D_Olie_510_jkk","v":25},{"$f":"IF(ISNUMBER(K25),IF(J25>K25,J25/K25,\"Nej\"),\" \")","v":"Nej"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum","C6-C10",null,{"$f":"SUM(AG27:AG39)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI27:AI39)","v":{"$error":"#DIV/0!"}},null,null,null,"Sum","C6-C10",{"$f":"SUM(AO27:AO39)","v":{"$error":"#DIV/0!"}},{"$f":"AO25*$AO$110","v":{"$error":"#DIV/0!"}},"Sum","C6-C10",{"$f":"SUM(AS27:AS39)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT27:AT39)","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel",null,null,null,{"$f":"SUM(F27:F39)","v":0.99715909090909105},null,null,{"$f":"IF(J$25-SUM(I27:I39)-H37<0,0,J$25-SUM(I27:I39))","v":0}]
[52,">5 - 7, aromater",6.5,"Benzen (C6) (>5-7, aromater)",{"$f":"B_Olie_52_anv","v":9.469696969696971E-5},{"$f":"IF((D_Olie_52v=TRUE),0,E27)","v":9.469696969696971E-5},{"$f":"F27/F$26","v":9.4966761633428294E-5},{"$f":"(I$26*G27)","v":0},{"$f":"D_Olie_52","v":0},{"$f":"IF(D_Olie_52v=TRUE,I27,H27)","v":0},{"$f":"D_Olie_52_jkk","v":1.5},{"$f":"IF(ISNUMBER(K27),IF(J27>K27,J27/K27,\"Nej\"),\" \")","v":"Nej"},{"$f":"J27*100/J$111","v":0},{"$f":"M27/P27","v":0},{"$f":"N27/N$111","v":0},78.099999999999994,12.63896052631579,80.09,6.2642876603127293,1790,0.56240000000000001,2.13,9.3000000000000007E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C27+2.3)*B_Olie_foc*B_Olie_d)/(U27)","v":0},{"$f":"B_Olie_VV/U27","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X27/SUM(X27:Z27)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y27/SUM(X27:Z27)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z27/SUM(X27:Z27)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O27*$J111*(0.01*$AB27)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T27*O27","v":0},{"$f":"IF(AD27>AE27,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD27:AE27)","v":{"$error":"#DIV/0!"}},{"$f":"AG27*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH27/$P27","v":{"$error":"#DIV/0!"}},{"$f":"AI27/$AI$111","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_52_gkk","v":1},{"$f":"IF(ISNUMBER(AK27),IF(AG27>AK27,AG27/AK27,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O27*$J111*(0.01*$AC27)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O27*1000000*$S27*$P27/2353","v":0},{"$f":"MINA(AM27:AN27)","v":{"$error":"#DIV/0!"}},{"$f":"AO27*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ27*$AG$111*(0.01*$AC27)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ27*1000000*$S27*$P27/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ27:AR27)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS27,AO27)","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},{"$f":"IF(ISNUMBER(AU27),IF(AT27>AU27,AT27/AU27,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[53,">6 - 8, alifater",{"$f":"4.12+0.02*R28+(0.000065*R28*R28)","v":6.8429145999999994},">6 - 8, alifater",{"$f":"B_Olie_53_anv","v":0.44100378787878791},{"$f":"IF(ISNUMBER(I28),0,E28)","v":0.44100378787878791},{"$f":"F28/F$26","v":0.44226020892687556},{"$f":"(I$26*G28)","v":0},null,{"$f":"IF(I28>0,I28,H28)","v":0},null,null,{"$f":"J28*100/J$111","v":0},{"$f":"M28/P28","v":0},{"$f":"N28/N$111","v":0},109.3,6.8029999999999999,102.2,3.4053933559010843,3.01,308.16000000000003,4.29,{"$f":"0.0000084*((78.1/P28)^0.5)","v":7.1005946686005421E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C28+0.43)*B_Olie_foc*B_Olie_d)/(U28)","v":0},{"$f":"B_Olie_VV/U28","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X28/SUM(X28:Z28)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y28/SUM(X28:Z28)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z28/SUM(X28:Z28)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O28*$J111*(0.01*$AB28)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T28*O28","v":0},{"$f":"IF(AD28>AE28,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD28:AE28)","v":{"$error":"#DIV/0!"}},{"$f":"AG28*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH28/$P28","v":{"$error":"#DIV/0!"}},{"$f":"AI28/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O28*$J111*(0.01*$AC28)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O28*1000000*$S28*$P28/2353","v":0},{"$f":"MINA(AM28:AN28)","v":{"$error":"#DIV/0!"}},{"$f":"AO28*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ28*$AG$111*(0.01*$AC28)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ28*1000000*$S28*$P28/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ28:AR28)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS28,AO28)","v":{"$error":"#DIV/0!"}}]
[54,">7 - 8, aromater",7.58,"Toluen (C7)(>7-8, aromater",{"$f":"B_Olie_54_anv","v":9.469696969696971E-5},{"$f":"IF(D_Olie_54v=TRUE,0,E29)","v":9.469696969696971E-5},{"$f":"F29/F$26","v":9.4966761633428294E-5},{"$f":"(I$26*G29)","v":0},{"$f":"D_Olie_54","v":0},{"$f":"IF(D_Olie_54v=TRUE,I29,H29)","v":0},{"$f":"D_Olie_54_jkk","v":0},{"$f":"IF(ISNUMBER(K29),IF(J29>K29,J29/K29,\"Nej\"),\" \")","v":"Nej"},{"$f":"J29*100/J$111","v":0},{"$f":"M29/P29","v":0},{"$f":"N29/N$111","v":0},92.1,3.7863552631578945,110.6,1.7411320859431541,530,0.67379999999999995,2.73,8.5640392765120893E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C29+2.3)*B_Olie_foc*B_Olie_d)/(U29)","v":0},{"$f":"B_Olie_VV/U29","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X29/SUM(X29:Z29)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y29/SUM(X29:Z29)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z29/SUM(X29:Z29)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O29*$J111*(0.01*$AB29)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T29*O29","v":0},{"$f":"IF(AD29>AE29,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD29:AE29)","v":{"$error":"#DIV/0!"}},{"$f":"AG29*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH29/$P29","v":{"$error":"#DIV/0!"}},{"$f":"AI29/$AI$111","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_54_gkk","v":5},{"$f":"IF(ISNUMBER(AK29),IF(AG29>AK29,AG29/AK29,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O29*$J111*(0.01*$AC29)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O29*1000000*$S29*$P29/2353","v":0},{"$f":"MINA(AM29:AN29)","v":{"$error":"#DIV/0!"}},{"$f":"AO29*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ29*$AG$111*(0.01*$AC29)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ29*1000000*$S29*$P29/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ29:AR29)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS29,AO29)","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_54_ak","v":0.4},{"$f":"IF(ISNUMBER(AU29),IF(AT29>AU29,AT29/AU29,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["55A",">8 - 10, alifater",{"$f":"4.12+0.02*R30+(0.000065*R30*R30)","v":9.1937706500000012},">8 - 10, alifater, Tung olie",{"$f":"B_Olie_55A_anv","v":0},{"$f":"IF(ISNUMBER(I30),0,E30)","v":0},{"$f":"F30/F$26","v":0},{"$f":"(I$26*G30)","v":0},null,{"$f":"IF(I30>0,I30,H30)","v":0},null,null,{"$f":"J30*100/J$111","v":0},{"$f":"M30/P30","v":0},{"$f":"N30/N$111","v":0},134.22,0.4521,165.1,0.18506622486420399,0.379,497.55,5.08,5.5030901075876E-6,{"$f":"((1-B_Olie_e)*10^(0.45*C30+0.43)*B_Olie_foc*B_Olie_d)/(U30)","v":0},{"$f":"B_Olie_VV/U30","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X30/SUM(X30:Z30)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y30/SUM(X30:Z30)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z30/SUM(X30:Z30)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O30*$J111*(0.01*$AB30)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T30*O30","v":0},{"$f":"IF(AD30>AE30,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD30:AE30)","v":{"$error":"#DIV/0!"}},{"$f":"AG30*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH30/$P30","v":{"$error":"#DIV/0!"}},{"$f":"AI30/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O30*$J111*(0.01*$AC30)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O30*1000000*$S30*$P30/2353","v":0},{"$f":"MINA(AM30:AN30)","v":{"$error":"#DIV/0!"}},{"$f":"AO30*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ30*$AG$111*(0.01*$AC30)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ30*1000000*$S30*$P30/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ30:AR30)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS30,AO30)","v":{"$error":"#DIV/0!"}}]
["55B",null,{"$f":"4.12+0.02*R31+(0.000065*R31*R31)","v":9.3296308240000005},">8 - 10, alifater, Olieblandinger",{"$f":"B_Olie_55B_anv","v":0.1631628787878788},{"$f":"IF(ISNUMBER(I31),0,E31)","v":0.1631628787878788},{"$f":"F31/F$26","v":0.16362773029439695},{"$f":"(I$26*G31)","v":0},null,{"$f":"IF(I31>0,I31,H31)","v":0},null,null,{"$f":"J31*100/J$111","v":0},{"$f":"M31/P31","v":0},{"$f":"N31/N$111","v":0},142.29,0.2404,168.36,8.9944621562165095E-2,0.747,534.27,5.15,{"$f":"0.0000084*((78.1/P31)^0.5)","v":6.2232552378840063E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C31+0.43)*B_Olie_foc*B_Olie_d)/(U31)","v":0},{"$f":"B_Olie_VV/U31","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X31/SUM(X31:Z31)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y31/SUM(X31:Z31)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z31/SUM(X31:Z31)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O31*$J111*(0.01*$AB31)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T31*O31","v":0},{"$f":"IF(AD31>AE31,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD31:AE31)","v":{"$error":"#DIV/0!"}},{"$f":"AG31*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH31/$P31","v":{"$error":"#DIV/0!"}},{"$f":"AI31/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O31*$J111*(0.01*$AC31)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O31*1000000*$S31*$P31/2353","v":0},{"$f":"MINA(AM31:AN31)","v":{"$error":"#DIV/0!"}},{"$f":"AO31*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ31*$AG$111*(0.01*$AC31)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ31*1000000*$S31*$P31/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ31:AR31)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS31,AO31)","v":{"$error":"#DIV/0!"}}]
[56,">8 -10, aromater",null,"Sum >8-10, aromater",null,null,null,null,null,{"$f":"SUM(J35:J39)","v":0}]
[571,null,null,"o-Xylen",null,null,null,null,{"$f":"D_Olie_571","v":0},{"$f":"IF(D_Olie_571v=TRUE,I33,H33)","v":0}]
[572,null,null,"m+p-Xylen",null,null,null,null,{"$f":"D_Olie_572","v":0},{"$f":"IF(D_Olie_572v=TRUE,I34,H34)","v":0}]
[57,null,8.6,"Sum Xylener regnes som m-Xylen (C8)",{"$f":"B_Olie_57_anv","v":9.469696969696971E-5},{"$f":"IF(OR(D_Olie_571v=TRUE,D_Olie_572v=TRUE,D_Olie_57v=TRUE),0,E35)","v":9.469696969696971E-5},{"$f":"F35/F$26","v":9.4966761633428294E-5},{"$f":"IF(OR(D_Olie_571v=TRUE,D_Olie_572v=TRUE),(I33+I34),(I$26*G35))","v":0},{"$f":"D_Olie_57","v":0},{"$f":"IF(D_Olie_57v=TRUE,I35,H35)","v":0},{"$f":"D_Olie_57_jkk","v":0},{"$f":"IF(ISNUMBER(K35),IF((J35+J36)>K35,(J35+J36)/K35,\"Nej\"),\" \")","v":"Nej"},{"$f":"J35*100/J$111","v":0},{"$f":"M35/P35","v":0},{"$f":"N35/N$111","v":0},106.2,1.1052424342105263,139.1,{"$f":"Q35*EXP(((LN(Q35/101.325))/(0.00336-(1/(273+R35))))*0.000178)","v":0.46693373684719081},161,0.72750000000000004,3.2,7.9752849160092975E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C35+2.3)*B_Olie_foc*B_Olie_d)/(U35)","v":0},{"$f":"B_Olie_VV/U35","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X35/SUM(X35:Z35)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y35/SUM(X35:Z35)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z35/SUM(X35:Z35)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O35*$J111*(0.01*$AB35)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T35*O35","v":0},{"$f":"IF(AD35>AE35,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD35:AE35)","v":{"$error":"#DIV/0!"}},{"$f":"AG35*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH35/$P35","v":{"$error":"#DIV/0!"}},{"$f":"AI35/$AI$111","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_57_gkk","v":5},{"$f":"IF(ISNUMBER(AK35),IF((AG35+B_Olie_58_cv)>AK35,(AG35+B_Olie_58_cv)/AK35,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O35*$J111*(0.01*$AC35)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O35*1000000*$S35*$P35/2353","v":0},{"$f":"MINA(AM35:AN35)","v":{"$error":"#DIV/0!"}},{"$f":"AO35*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ35*$AG$111*(0.01*$AC35)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ35*1000000*$S35*$P35/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ35:AR35)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS35,AO35)","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_57_ak","v":0.1},{"$f":"IF(ISNUMBER(AU35),IF((AT35+AT36)>AU35,(AT35+AT36)/AU35,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[58,null,8.5,"Ethylbenzen (C8)",{"$f":"B_Olie_58_anv","v":9.469696969696971E-5},{"$f":"IF(D_Olie_58v=TRUE,0,E36)","v":9.469696969696971E-5},{"$f":"F36/F$26","v":9.4966761633428294E-5},{"$f":"(I$26*G36)","v":0},{"$f":"D_Olie_58","v":0},{"$f":"IF(D_Olie_58v=TRUE,I36,H36)","v":0},null,null,{"$f":"J36*100/J$111","v":0},{"$f":"M36/P36","v":0},{"$f":"N36/N$111","v":0},106.2,1.2798947368421052,136.1,{"$f":"Q36*EXP(((LN(Q36/101.325))/(0.00336-(1/(273+R36))))*0.000178)","v":0.54712472087591502},169,0.7984,3.15,7.9752849160092975E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C36+2.3)*B_Olie_foc*B_Olie_d)/(U36)","v":0},{"$f":"B_Olie_VV/U36","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X36/SUM(X36:Z36)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y36/SUM(X36:Z36)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z36/SUM(X36:Z36)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O36*$J111*(0.01*$AB36)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T36*O36","v":0},{"$f":"IF(AD36>AE36,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD36:AE36)","v":{"$error":"#DIV/0!"}},{"$f":"AG36*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH36/$P36","v":{"$error":"#DIV/0!"}},{"$f":"AI36/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O36*$J111*(0.01*$AC36)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O36*1000000*$S36*$P36/2353","v":0},{"$f":"MINA(AM36:AN36)","v":{"$error":"#DIV/0!"}},{"$f":"AO36*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ36*$AG$111*(0.01*$AC36)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ36*1000000*$S36*$P36/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ36:AR36)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS36,AO36)","v":{"$error":"#DIV/0!"}}]
[59,null,9.6199999999999992,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"MAX(G38:G39)","v":0.3937321937321937},{"$f":"B_Olie_59_fastdel_anv","v":0.3},null,{"$f":"IF(H37>B_Olie_510_ct*G37,B_Olie_510_ct*G37,H37)","v":0},null,null,{"$f":"J37*100/J$111","v":0},{"$f":"M37/P37","v":0},{"$f":"N37/N$111","v":0},120.2,0.33063947368421054,164.7,{"$f":"Q37*EXP(((LN(Q37/101.325))/(0.00336-(1/(273+R37))))*0.000178)","v":0.12816983345801572},48.2,0.89,3.42,7.4964600630922756E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C37+2.3)*B_Olie_foc*B_Olie_d)/(U37)","v":0},{"$f":"B_Olie_VV/U37","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X37/SUM(X37:Z37)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y37/SUM(X37:Z37)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z37/SUM(X37:Z37)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O37*$J111*(0.01*$AB37)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T37*O37","v":0},{"$f":"IF(AD37>AE37,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD37:AE37)","v":{"$error":"#DIV/0!"}},{"$f":"AG37*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH37/$P37","v":{"$error":"#DIV/0!"}},{"$f":"AI37/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O37*$J111*(0.01*$AC37)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O37*1000000*$S37*$P37/2353","v":0},{"$f":"MINA(AM37:AN37)","v":{"$error":"#DIV/0!"}},{"$f":"AO37*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ37*$AG$111*(0.01*$AC37)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ37*1000000*$S37*$P37/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ37:AR37)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS37,AO37)","v":{"$error":"#DIV/0!"}}]
["60A",null,{"$f":"4.12+0.02*R38+(0.000065*R38*R38)","v":9.7387215866122876},">8-10, aromater, øvrige, Tung olie",{"$f":"B_Olie_60A_anv","v":0},{"$f":"IF(ISNUMBER(I38),0,E38)","v":0},{"$f":"F38/F$26","v":0},{"$f":"IF((I$26*G38)-$H$37>0,(I$26*G38)-$H$37,0)","v":0},null,{"$f":"IF(I38>0,I38,H38)","v":0},null,null,{"$f":"J38*100/J$111","v":0},{"$f":"M38/P38","v":0},{"$f":"N38/N$111","v":0},134.22,0.2028789189189189,177.98288288288288,{"$f":"Q38*EXP(((LN(Q38/101.325))/(0.00336-(1/(273+R38))))*0.000178)","v":7.7065824454518192E-2},36.534034034034029,0.77438988988988977,4.5,5.8479979979979979E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C38+2.3)*B_Olie_foc*B_Olie_d)/(U38)","v":0},{"$f":"B_Olie_VV/U38","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X38/SUM(X38:Z38)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y38/SUM(X38:Z38)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z38/SUM(X38:Z38)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O38*$J111*(0.01*$AB38)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T38*O38","v":0},{"$f":"IF(AD38>AE38,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD38:AE38)","v":{"$error":"#DIV/0!"}},{"$f":"AG38*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH38/$P38","v":{"$error":"#DIV/0!"}},{"$f":"AI38/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O38*$J111*(0.01*$AC38)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O38*1000000*$S38*$P38/2353","v":0},{"$f":"MINA(AM38:AN38)","v":{"$error":"#DIV/0!"}},{"$f":"AO38*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ38*$AG$111*(0.01*$AC38)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ38*1000000*$S38*$P38/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ38:AR38)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS38,AO38)","v":{"$error":"#DIV/0!"}}]
["60B",null,{"$f":"4.12+0.02*R39+(0.000065*R39*R39)","v":9.956785},">8 -10, aromater,øvrige, Olieblanding",{"$f":"B_Olie_60B_anv","v":0.39261363636363639},{"$f":"IF(ISNUMBER(I39),0,E39)","v":0.39261363636363639},{"$f":"F39/F$26","v":0.3937321937321937},{"$f":"IF((I$26*G39)-$H$37>0,(I$26*G39)-$H$37,0)","v":0},null,{"$f":"IF(I39>0,I39,H39)","v":0},null,null,{"$f":"J39*100/J$111","v":0},{"$f":"M39/P39","v":0},{"$f":"N39/N$111","v":0},132.94999999999999,0.16070000000000001,183,{"$f":"Q39*EXP(((LN(Q39/101.325))/(0.00336-(1/(273+R39))))*0.000178)","v":6.0115984637894748E-2},25.09,0.88,4.43,{"$f":"0.0000084*((78.1/P39)^0.5)","v":6.4381431991356133E-6},{"$f":"((1-B_Olie_e)*10^(0.1*C39+2.3)*B_Olie_foc*B_Olie_d)/(U39)","v":0},{"$f":"B_Olie_VV/U39","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X39/SUM(X39:Z39)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y39/SUM(X39:Z39)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z39/SUM(X39:Z39)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O39*$J111*(0.01*$AB39)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T39*O39","v":0},{"$f":"IF(AD39>AE39,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD39:AE39)","v":{"$error":"#DIV/0!"}},{"$f":"AG39*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH39/$P39","v":{"$error":"#DIV/0!"}},{"$f":"AI39/$AI$111","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_60_gkk","v":1},{"$f":"IF(ISNUMBER(AK39),IF(SUM(AG37:AG39)>AK39,SUM(AG37:AG39)/AK39,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O39*$J111*(0.01*$AC39)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O39*1000000*$S39*$P39/2353","v":0},{"$f":"MINA(AM39:AN39)","v":{"$error":"#DIV/0!"}},{"$f":"AO39*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ39*$AG$111*(0.01*$AC39)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ39*1000000*$S39*$P39/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ39:AR39)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS39,AO39)","v":{"$error":"#DIV/0!"}}]
[910,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(B_Olie_60B_cv+B_Olie_59_cv)","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Olie_60_gkk","v":1},{"$f":"IF(ISNUMBER(AK40),IF(AG40>AK40,AG40/AK40,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,{"$f":"B_Olie_60B_cl+B_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_60_ak","v":0.03},{"$f":"IF(ISNUMBER(AU40),IF(SUM(AT37:AT39)>AU40,SUM(AT37:AT39)/AU40,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},"SumC9-C10"]
[1015,">C10 - C15",null,null,{"$f":"B_Olie_1015_anv","v":0.3587034419191179},{"$f":"IF(D_Olie_1015v = TRUE,0,E41)","v":0.3587034419191179},{"$f":"F41/F$110","v":0.3587034419191179},{"$f":"(I$110*G41)","v":0},{"$f":"D_Olie_1015","v":0},{"$f":"IF(D_Olie_1015v=TRUE,I41,H41)","v":0},{"$f":"D_Olie_1015_jkk","v":40},{"$f":"IF(ISNUMBER(K41),IF(J41>K41,J41/K41,\"Nej\"),\" \")","v":"Nej"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum","C15-C20",null,{"$f":"SUM(AG43:AG54)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI43:AI54)","v":{"$error":"#DIV/0!"}},null,null,null,"Sum","C15-C20",{"$f":"SUM(AO43:AO54)","v":{"$error":"#DIV/0!"}},{"$f":"AO41*$AO$110","v":{"$error":"#DIV/0!"}},"Sum","C15-C20",{"$f":"SUM(AS43:AS54)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT43:AT54)","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel",null," ",null,{"$f":"SUM(F43:F54)","v":1},null,null,{"$f":"IF(J41-SUM(I43:I54)<0,0,J41-SUM(I43:I54))","v":0}]
[101,">10 - 12, alifater",12,"Dodecan(C12)",{"$f":"B_Olie_101_anv","v":9.3861460484325143E-2},{"$f":"IF(ISNUMBER(I43),0,E43)","v":9.3861460484325143E-2},{"$f":"F43/F$42","v":9.3861460484325143E-2},{"$f":"G43*I$42","v":0},null,{"$f":"IF(I43>0,I43,H43)","v":0},null,null,{"$f":"J43*100/J$111","v":0},{"$f":"M43/P43","v":0},{"$f":"N43/N$111","v":0},170.34,1.7954999999999999E-2,216.3,{"$f":"Q43*EXP((1*(LN(Q43/101.324))/(0.00336-(1/(273+R43))))*0.000178)","v":5.5829254527894386E-3},3.7000000000000002E-3,828.83849999999995,6.1,{"$f":"0.0000084*((78.1/P43)^0.5)","v":5.6878283496407569E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C43+0.43)*B_Olie_foc*B_Olie_d)/(U43)","v":0},{"$f":"B_Olie_VV/U43","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X43/SUM(X43:Z43)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y43/SUM(X43:Z43)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z43/SUM(X43:Z43)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O43*$J111*(0.01*$AB43)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T43*O43","v":0},{"$f":"IF(AD43>AE43,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD43:AE43)","v":{"$error":"#DIV/0!"}},{"$f":"AG43*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH43/$P43","v":{"$error":"#DIV/0!"}},{"$f":"AI43/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O43*$J111*(0.01*$AC43)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O43*1000000*$S43*$P43/2353","v":0},{"$f":"MINA(AM43:AN43)","v":{"$error":"#DIV/0!"}},{"$f":"AO43*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ43*$AG$111*(0.01*$AC43)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ43*1000000*$S43*$P43/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ43:AR43)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS43,AO43)","v":{"$error":"#DIV/0!"}}]
[102,">10 - 12, aromater",null,"Sum >10 - 12 aromater",null,null,null,null,null,{"$f":"SUM(J45:J47)","v":0}]
[103,null,11.69,"Naphthalen (C10)",{"$f":"B_Olie_103_anv","v":2.9499316152216473E-3},{"$f":"IF(D_Olie_103v = TRUE,0,E45)","v":2.9499316152216473E-3},{"$f":"F45/F$42","v":2.9499316152216473E-3},{"$f":"G45*I$42","v":0},{"$f":"D_Olie_103","v":0},{"$f":"IF(D_Olie_103v=TRUE,I45,H45)","v":0},{"$f":"D_Olie_103_jkk","v":0},{"$f":"IF(ISNUMBER(K45),IF(J45>K45,J45/K45,\"Nej\"),\" \")","v":"Nej"},{"$f":"J45*100/J$111","v":0},{"$f":"M45/P45","v":0},{"$f":"N45/N$111","v":0},128.19999999999999,1.1332401315789473E-2,217.9,{"$f":"Q45*EXP(((LN(Q45/101.325))/(0.00336-(1/(273+R45))))*0.000178)","v":3.3316592097730469E-3},31,4.4582999999999998E-2,3.3,7.2587936878955403E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C45+2.3)*B_Olie_foc*B_Olie_d)/(U45)","v":0},{"$f":"B_Olie_VV/U45","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X45/SUM(X45:Z45)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y45/SUM(X45:Z45)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z45/SUM(X45:Z45)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O45*$J111*(0.01*$AB45)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T45*O45","v":0},{"$f":"IF(AD45>AE45,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD45:AE45)","v":{"$error":"#DIV/0!"}},{"$f":"AG45*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH45/$P45","v":{"$error":"#DIV/0!"}},{"$f":"AI45/$AI$111","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_103_gkk","v":1},{"$f":"IF(ISNUMBER(AK45),IF(AG45>AK45,AG45/AK45,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O45*$J111*(0.01*$AC45)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O45*1000000*$S45*$P45/2353","v":0},{"$f":"MINA(AM45:AN45)","v":{"$error":"#DIV/0!"}},{"$f":"AO45*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ45*$AG$111*(0.01*$AC45)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ45*1000000*$S45*$P45/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ45:AR45)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS45,AO45)","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_103_ak","v":0.04},{"$f":"IF(ISNUMBER(AU45),IF(AT45>AU45,AT45/AU45,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["104A",null,{"$f":"4.12+0.02*R46+(0.000065*R46*R46)","v":10.83554069290965},">10 - 12, aromater, øvrige, Tung Olie",{"$f":"B_Olie_104A_anv","v":0},{"$f":"IF(ISNUMBER(I46),0,E46)","v":0},{"$f":"F46/F$42","v":0},{"$f":"G46*I$42","v":0},null,{"$f":"IF(I46>0,I46,H46)","v":0},null,null,{"$f":"J46*100/J$111","v":0},{"$f":"M46/P46","v":0},{"$f":"N46/N$111","v":0},188.93421942668863,5.9823081927853656E-4,202.50290215568668,1.8547169361600978E-4,1.9651746667441627,8.8234259184450572E-3,5.1654035688753765,5.9633499312903359E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C46+2.3)*B_Olie_foc*B_Olie_d)/(U46)","v":0},{"$f":"B_Olie_VV/U46","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X46/SUM(X46:Z46)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y46/SUM(X46:Z46)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z46/SUM(X46:Z46)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O46*$J111*(0.01*$AB46)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T46*O46","v":0},{"$f":"IF(AD46>AE46,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD46:AE46)","v":{"$error":"#DIV/0!"}},{"$f":"AG46*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH46/$P46","v":{"$error":"#DIV/0!"}},{"$f":"AI46/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O46*$J111*(0.01*$AC46)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O46*1000000*$S46*$P46/2353","v":0},{"$f":"MINA(AM46:AN46)","v":{"$error":"#DIV/0!"}},{"$f":"AO46*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ46*$AG$111*(0.01*$AC46)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ46*1000000*$S46*$P46/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ46:AR46)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS46,AO46)","v":{"$error":"#DIV/0!"}}]
["104B",null,{"$f":"4.12+0.02*R47+(0.000065*R47*R47)","v":10.674064999999999},">10 - 12, aromater, øvrige, Olieblanding",{"$f":"B_Olie_104B_anv","v":0.5870363914291078},0.5870363914291078,{"$f":"F47/F$42","v":0.5870363914291078},{"$f":"G47*I$42","v":0},null,{"$f":"IF(I47>0,I47,H47)","v":0},null,null,{"$f":"J47*100/J$111","v":0},{"$f":"M47/P47","v":0},{"$f":"N47/N$111","v":0},180.46,1.32E-2,199,{"$f":"Q47*EXP(((LN(Q47/101.325))/(0.00336-(1/(273+R47))))*0.000178)","v":3.6599668137628893E-3},5.7949999999999999,0.16700000000000001,4.7300000000000004,5.5260438461528997E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C47+2.3)*B_Olie_foc*B_Olie_d)/(U47)","v":0},{"$f":"B_Olie_VV/U47","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X47/SUM(X47:Z47)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y47/SUM(X47:Z47)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z47/SUM(X47:Z47)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O47*$J111*(0.01*$AB47)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T47*O47","v":0},{"$f":"IF(AD47>AE47,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD47:AE47)","v":{"$error":"#DIV/0!"}},{"$f":"AG47*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH47/$P47","v":{"$error":"#DIV/0!"}},{"$f":"AI47/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O47*$J111*(0.01*$AC47)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O47*1000000*$S47*$P47/2353","v":0},{"$f":"MINA(AM47:AN47)","v":{"$error":"#DIV/0!"}},{"$f":"AO47*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ47*$AG$111*(0.01*$AC47)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ47*1000000*$S47*$P47/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ47:AR47)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS47,AO47)","v":{"$error":"#DIV/0!"}}]
["105A",">12 - 16, alifater",{"$f":"4.12+0.02*R48+(0.000065*R48*R48)","v":14.475124411301071},">12 - 16, alifater, Tung Olie",{"$f":"B_Olie_105A_anv","v":0},0,{"$f":"F48/F$42","v":0},{"$f":"G48*I$42","v":0},null,{"$f":"IF(I48>0,I48,H48)","v":0},null,null,{"$f":"J48*100/J$111","v":0},{"$f":"M48/P48","v":0},{"$f":"N48/N$111","v":0},215.47820551830094,5.9432816606045671E-4,273.91341107433186,{"$f":"Q48*EXP(((LN(Q48/101.325))/(0.00336-(1/(273+R48))))*0.000178)","v":1.4655171700946601E-4},9.5985985184114566E-4,633.14956118085502,7.8347832873878831,4.3460519456567218E-6,{"$f":"((1-B_Olie_e)*10^(0.45*C48+0.43)*B_Olie_foc*B_Olie_d)/(U48)","v":0},{"$f":"B_Olie_VV/U48","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X48/SUM(X48:Z48)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y48/SUM(X48:Z48)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z48/SUM(X48:Z48)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O48*$J111*(0.01*$AB48)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T48*O48","v":0},{"$f":"IF(AD48>AE48,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD48:AE48)","v":{"$error":"#DIV/0!"}},{"$f":"AG48*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH48/$P48","v":{"$error":"#DIV/0!"}},{"$f":"AI48/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O48*$J111*(0.01*$AC48)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O48*1000000*$S48*$P48/2353","v":0},{"$f":"MINA(AM48:AN48)","v":{"$error":"#DIV/0!"}},{"$f":"AO48*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ48*$AG$111*(0.01*$AC48)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ48*1000000*$S48*$P48/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ48:AR48)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS48,AO48)","v":{"$error":"#DIV/0!"}}]
["105B",null,{"$f":"4.12+0.02*R49+(0.000065*R49*R49)","v":11.059263850000001},">12 - 16, alifater, Olieblandinger",{"$f":"B_Olie_105B_anv","v":0.2949931615221647},0.2949931615221647,{"$f":"F49/F$42","v":0.2949931615221647},{"$f":"G49*I$42","v":0},null,{"$f":"IF(I49>0,I49,H49)","v":0},null,null,{"$f":"J49*100/J$111","v":0},{"$f":"M49/P49","v":0},{"$f":"N49/N$111","v":0},212.42,7.4339999999999996E-4,207.3,{"$f":"Q49*EXP(((LN(Q49/101.325))/(0.00336-(1/(273+R49))))*0.000178)","v":1.4324241674757866E-4},1.1077999999999999E-3,726.05,7.72,{"$f":"0.0000084*((78.1/P49)^0.5)","v":5.0933919872504982E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C49+0.43)*B_Olie_foc*B_Olie_d)/(U49)","v":0},{"$f":"B_Olie_VV/U49","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X49/SUM(X49:Z49)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y49/SUM(X49:Z49)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z49/SUM(X49:Z49)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O49*$J111*(0.01*$AB49)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T49*O49","v":0},{"$f":"IF(AD49>AE49,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD49:AE49)","v":{"$error":"#DIV/0!"}},{"$f":"AG49*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH49/$P49","v":{"$error":"#DIV/0!"}},{"$f":"AI49/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O49*$J111*(0.01*$AC49)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O49*1000000*$S49*$P49/2353","v":0},{"$f":"MINA(AM49:AN49)","v":{"$error":"#DIV/0!"}},{"$f":"AO49*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ49*$AG$111*(0.01*$AC49)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ49*1000000*$S49*$P49/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ49:AR49)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS49,AO49)","v":{"$error":"#DIV/0!"}}]
[106,">12 - 16, aromater",null,"Sum >10 - 12 aromater",null,null,null,null,null,{"$f":"SUM(J51:J54)","v":0}]
[107,null,15.06,"Acenaphthylen (C12)",{"$f":"B_Olie_107_anv","v":8.045268041513582E-4},8.045268041513582E-4,{"$f":"F51/F$42","v":8.045268041513582E-4},{"$f":"G51*I$42","v":0},null,{"$f":"IF(I51>0,I51,H51)","v":0},null,null,{"$f":"J51*100/J$111","v":0},{"$f":"M51/P51","v":0},{"$f":"N51/N$111","v":0},152.19999999999999,8.9059342105263163E-4,280,{"$f":"Q51*EXP(((LN(Q51/101.325))/(0.00336-(1/(273+R51))))*0.000178)","v":2.3425021423060055E-4},16.100000000000001,0.11550000000000001,4.07,6.6619464783515415E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V51-0.346)*B_Olie_foc*B_Olie_d)/(U51)","v":0},{"$f":"B_Olie_VV/U51","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X51/SUM(X51:Z51)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y51/SUM(X51:Z51)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z51/SUM(X51:Z51)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O51*$J111*(0.01*$AB51)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T51*O51","v":0},{"$f":"IF(AD51>AE51,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD51:AE51)","v":{"$error":"#DIV/0!"}},{"$f":"AG51*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH51/$P51","v":{"$error":"#DIV/0!"}},{"$f":"AI51/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O51*$J111*(0.01*$AC51)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O51*1000000*$S51*$P51/2353","v":0},{"$f":"MINA(AM51:AN51)","v":{"$error":"#DIV/0!"}},{"$f":"AO51*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ51*$AG$111*(0.01*$AC51)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ51*1000000*$S51*$P51/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ51:AR51)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS51,AO51)","v":{"$error":"#DIV/0!"}}]
[108,null,15.5,"Acenaphthen (C12)",{"$f":"B_Olie_108_anv","v":2.4135804124540751E-4},2.4135804124540751E-4,{"$f":"F52/F$42","v":2.4135804124540751E-4},{"$f":"G52*I$42","v":0},null,{"$f":"IF(I52>0,I52,H52)","v":0},null,null,{"$f":"J52*100/J$111","v":0},{"$f":"M52/P52","v":0},{"$f":"N52/N$111","v":0},154.19999999999999,2.8664309210526319E-4,279,{"$f":"Q52*EXP(((LN(Q52/101.325))/(0.00336-(1/(273+R52))))*0.000178)","v":6.5995940955220012E-5},3.9,0.18643799999999999,3.92,6.6186021894078394E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V52-0.346)*B_Olie_foc*B_Olie_d)/(U52)","v":0},{"$f":"B_Olie_VV/U52","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X52/SUM(X52:Z52)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y52/SUM(X52:Z52)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z52/SUM(X52:Z52)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O52*$J111*(0.01*$AB52)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T52*O52","v":0},{"$f":"IF(AD52>AE52,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD52:AE52)","v":{"$error":"#DIV/0!"}},{"$f":"AG52*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH52/$P52","v":{"$error":"#DIV/0!"}},{"$f":"AI52/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O52*$J111*(0.01*$AC52)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O52*1000000*$S52*$P52/2353","v":0},{"$f":"MINA(AM52:AN52)","v":{"$error":"#DIV/0!"}},{"$f":"AO52*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ52*$AG$111*(0.01*$AC52)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ52*1000000*$S52*$P52/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ52:AR52)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS52,AO52)","v":{"$error":"#DIV/0!"}}]
["109A",null,{"$f":"4.12+0.02*R53+(0.000065*R53*R53)","v":15.008004640601659},">12 - 16, aromater,øvrige, Tung Olie",{"$f":"B_Olie_109A_anv","v":0},0,{"$f":"F53/F$42","v":0},{"$f":"G53*I$42","v":0},null,{"$f":"IF(I53>0,I53,H53)","v":0},null,null,{"$f":"J53*100/J$111","v":0},{"$f":"M53/P53","v":0},{"$f":"N53/N$111","v":0},169.31945491974597,4.7032765747787345E-4,283.39108468096248,{"$f":"Q53*EXP(((LN(Q53/101.325))/(0.00336-(1/(273+R53))))*0.000178)","v":1.1612028500595566E-4},5.1369110482731557,0.6724,4.7555981176612647,5.5027929670196982E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C53+2.3)*B_Olie_foc*B_Olie_d)/(U53)","v":0},{"$f":"B_Olie_VV/U53","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X53/SUM(X53:Z53)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y53/SUM(X53:Z53)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z53/SUM(X53:Z53)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O53*$J111*(0.01*$AB53)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T53*O53","v":0},{"$f":"IF(AD53>AE53,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD53:AE53)","v":{"$error":"#DIV/0!"}},{"$f":"AG53*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH53/$P53","v":{"$error":"#DIV/0!"}},{"$f":"AI53/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O53*$J111*(0.01*$AC53)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O53*1000000*$S53*$P53/2353","v":0},{"$f":"MINA(AM53:AN53)","v":{"$error":"#DIV/0!"}},{"$f":"AO53*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ53*$AG$111*(0.01*$AC53)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ53*1000000*$S53*$P53/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ53:AR53)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS53,AO53)","v":{"$error":"#DIV/0!"}}]
["109B",null,{"$f":"4.12+0.02*R54+(0.000065*R54*R54)","v":13.775416474},">12 - 16, aromater,øvrige, Olieblandinger",{"$f":"B_Olie_109B_anv","v":2.0113170103783957E-2},2.0113170103783957E-2,{"$f":"F54/F$42","v":2.0113170103783957E-2},{"$f":"G54*I$42","v":0},null,{"$f":"IF(I54>0,I54,H54)","v":0},null,null,{"$f":"J54*100/J$111","v":0},{"$f":"M54/P54","v":0},{"$f":"N54/N$111","v":0},155.65,2.358597E-3,261.14,1.3317165564636099E-3,11.44,7.8600000000000003E-2,4.4000000000000004,5.9000000000000003E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C54+2.3)*B_Olie_foc*B_Olie_d)/(U54)","v":0},{"$f":"B_Olie_VV/U54","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X54/SUM(X54:Z54)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y54/SUM(X54:Z54)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z54/SUM(X54:Z54)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O54*$J111*(0.01*$AB54)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T54*O54","v":0},{"$f":"IF(AD54>AE54,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD54:AE54)","v":{"$error":"#DIV/0!"}},{"$f":"AG54*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH54/$P54","v":{"$error":"#DIV/0!"}},{"$f":"AI54/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O54*$J111*(0.01*$AC54)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O54*1000000*$S54*$P54/2353","v":0},{"$f":"MINA(AM54:AN54)","v":{"$error":"#DIV/0!"}},{"$f":"AO54*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ54*$AG$111*(0.01*$AC54)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ54*1000000*$S54*$P54/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ54:AR54)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS54,AO54)","v":{"$error":"#DIV/0!"}}]
[]
[1520,">C15 - C20",null,null,{"$f":"B_Olie_1520_anv","v":0.10312639784102291},{"$f":"IF(D_Olie_1520v = TRUE,0,E56)","v":0.10312639784102291},{"$f":"F56/F$110","v":0.10312639784102291},{"$f":"(I$110*G56)","v":0},{"$f":"D_Olie_1520","v":0},{"$f":"IF(D_Olie_1520v=TRUE,I56,H56)","v":0},{"$f":"D_Olie_1520_jkk","v":55},{"$f":"IF(ISNUMBER(K56),IF(J56>K56,J56/K56,\"Nej\"),\" \")","v":"Nej"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum","C15-C20",null,{"$f":"SUM(AG58:AG65)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI58:AI65)","v":{"$error":"#DIV/0!"}},null,null,null,"Sum","C15-C20",{"$f":"SUM(AO58:AO65)","v":{"$error":"#DIV/0!"}},{"$f":"AO56*$AO$110","v":{"$error":"#DIV/0!"}},"Sum","C15-C20",{"$f":"SUM(AS58:AS65)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT58:AT65)","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel",null," ",null,{"$f":"SUM(F58:F65)","v":1.0000000000000002},null,null,{"$f":"IF(J56-SUM(I58:I65)<0,0,J56-SUM(I58:I65))","v":0}]
["151A",">16 - 21, alifater",{"$f":"4.12+0.02*R58+(0.000065*R58*R58)","v":17.605848706218453},">16 - 21, alifater, Tung Olie",{"$f":"B_Olie_151A_anv","v":0},{"$f":"IF(ISNUMBER(I58),0,E58)","v":0},{"$f":"F58/F$57","v":0},{"$f":"G58*I$57","v":0},null,{"$f":"IF(I58>0,I58,H58)","v":0},null,null,{"$f":"J58*100/J$111","v":0},{"$f":"M58/P58","v":0},{"$f":"N58/N$111","v":0},274.64803638303852,1.6411826136987585E-4,326.92742543367547,4.2140875071855743E-5,2.0940088232287682E-3,8194.6857666854648,9.8096024587856352,3.7468864349159863E-6,{"$f":"((1-B_Olie_e)*10^(0.45*C58+0.43)*B_Olie_foc*B_Olie_d)/(U58)","v":0},{"$f":"B_Olie_VV/U58","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X58/SUM(X58:Z58)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y58/SUM(X58:Z58)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z58/SUM(X58:Z58)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O58*$J111*(0.01*$AB58)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T58*O58","v":0},{"$f":"IF(AD58>AE58,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD58:AE58)","v":{"$error":"#DIV/0!"}},{"$f":"AG58*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH58/$P58","v":{"$error":"#DIV/0!"}},{"$f":"AI58/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O58*$J111*(0.01*$AC58)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O58*1000000*$S58*$P58/2353","v":0},{"$f":"MINA(AM58:AN58)","v":{"$error":"#DIV/0!"}},{"$f":"AO58*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ58*$AG$111*(0.01*$AC58)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ58*1000000*$S58*$P58/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ58:AR58)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS58,AO58)","v":{"$error":"#DIV/0!"}}]
["151B",null,{"$f":"4.12+0.02*R59+(0.000065*R59*R59)","v":17.671707226000002},">16 - 21, alifater, Olieblandinger",{"$f":"B_Olie_151B_anv","v":0.97943192948090119},{"$f":"IF(ISNUMBER(I59),0,E59)","v":0.97943192948090119},{"$f":"F59/F$57","v":0.97943192948090096},{"$f":"G59*I$57","v":0},null,{"$f":"IF(I59>0,I59,H59)","v":0},null,null,{"$f":"J59*100/J$111","v":0},{"$f":"M59/P59","v":0},{"$f":"N59/N$111","v":0},275.54000000000002,2.6216100000000001E-4,327.98,{"$f":"Q59*EXP(((LN(Q59/101.325))/(0.00336-(1/(273+R59))))*0.000178)","v":6.7951446668690167E-5},1.9900000000000001E-4,8341.59,9.84,{"$f":"0.0000084*((78.1/P59)^0.5)","v":4.4721099862171762E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C59+0.43)*B_Olie_foc*B_Olie_d)/(U59)","v":0},{"$f":"B_Olie_VV/U59","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X59/SUM(X59:Z59)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y59/SUM(X59:Z59)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z59/SUM(X59:Z59)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O59*$J111*(0.01*$AB59)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T59*O59","v":0},{"$f":"IF(AD59>AE59,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD59:AE59)","v":{"$error":"#DIV/0!"}},{"$f":"AG59*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH59/$P59","v":{"$error":"#DIV/0!"}},{"$f":"AI59/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O59*$J111*(0.01*$AC59)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O59*1000000*$S59*$P59/2353","v":0},{"$f":"MINA(AM59:AN59)","v":{"$error":"#DIV/0!"}},{"$f":"AO59*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ59*$AG$111*(0.01*$AC59)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ59*1000000*$S59*$P59/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ59:AR59)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS59,AO59)","v":{"$error":"#DIV/0!"}}]
[152,">16 - 21, aromater",null,"Sum >16 - 21 aromater",null,null,null,null,null,{"$f":"SUM(J61:J65)","v":0}]
[153,null,16.55,"Fluoren (C13)",{"$f":"B_Olie_153_anv","v":2.938295788442704E-3},{"$f":"IF(ISNUMBER(I61),0,E61)","v":2.938295788442704E-3},{"$f":"F61/F$57","v":2.9382957884427031E-3},{"$f":"G61*I$57","v":0},null,{"$f":"IF(I61>0,I61,H61)","v":0},null,null,{"$f":"J61*100/J$111","v":0},{"$f":"M61/P61","v":0},{"$f":"N61/N$111","v":0},166.2,7.9993421052631581E-5,295,{"$f":"Q61*EXP(((LN(Q61/101.325))/(0.00336-(1/(273+R61))))*0.000178)","v":1.6745339000281659E-5},1.69,9.7474650000000003E-3,4.18,6.3751874043382609E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V61-0.346)*B_Olie_foc*B_Olie_d)/(U61)","v":0},{"$f":"B_Olie_VV/U61","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X61/SUM(X61:Z61)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y61/SUM(X61:Z61)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z61/SUM(X61:Z61)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O61*$J111*(0.01*$AB61)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T61*O61","v":0},"Ikke medtaget",{"$f":"MINA(AD61:AE61)","v":{"$error":"#DIV/0!"}},{"$f":"AG61*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH61/$P61","v":{"$error":"#DIV/0!"}},{"$f":"AI61/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O61*$J111*(0.01*$AC61)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O61*1000000*$S61*$P61/2353","v":0},{"$f":"MINA(AM61:AN61)","v":{"$error":"#DIV/0!"}},{"$f":"AO61*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ61*$AG$111*(0.01*$AC61)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ61*1000000*$S61*$P61/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ61:AR61)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS61,AO61)","v":{"$error":"#DIV/0!"}}]
[154,null,19.36,"Phenanthren (C14)",{"$f":"B_Olie_154_anv","v":4.8971596474045058E-3},{"$f":"IF(ISNUMBER(I62),0,E62)","v":4.8971596474045058E-3},{"$f":"F62/F$57","v":4.8971596474045049E-3},{"$f":"G62*I$57","v":0},null,0,null,null,{"$f":"J62*100/J$111","v":0},{"$f":"M62/P62","v":0},{"$f":"N62/N$111","v":0},178.2,1.6132006578947369E-5,340,{"$f":"Q62*EXP(((LN(Q62/101.325))/(0.00336-(1/(273+R62))))*0.000178)","v":3.2188700264955089E-6},1.1499999999999999,4.2860475E-3,4.46,6.1567938987033759E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V62-0.346)*B_Olie_foc*B_Olie_d)/(U62)","v":0},{"$f":"B_Olie_VV/U62","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X62/SUM(X62:Z62)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y62/SUM(X62:Z62)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z62/SUM(X62:Z62)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O62*$J111*(0.01*$AB62)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T62*O62","v":0},"Ikke medtaget",{"$f":"MINA(AD62:AE62)","v":{"$error":"#DIV/0!"}},{"$f":"AG62*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH62/$P62","v":{"$error":"#DIV/0!"}},{"$f":"AI62/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O62*$J111*(0.01*$AC62)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O62*1000000*$S62*$P62/2353","v":0},{"$f":"MINA(AM62:AN62)","v":{"$error":"#DIV/0!"}},{"$f":"AO62*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ62*$AG$111*(0.01*$AC62)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ62*1000000*$S62*$P62/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ62:AR62)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS62,AO62)","v":{"$error":"#DIV/0!"}}]
[155,null,19.43,"Anthracen (C14)",{"$f":"B_Olie_155_anv","v":2.938295788442704E-3},{"$f":"IF(ISNUMBER(I63),0,E63)","v":2.938295788442704E-3},{"$f":"F63/F$57","v":2.9382957884427031E-3},{"$f":"G63*I$57","v":0},null,0,null,null,{"$f":"J63*100/J$111","v":0},{"$f":"M63/P63","v":0},{"$f":"N63/N$111","v":0},178.2,1.3999999999999999E-6,339.9,{"$f":"Q63*EXP(((LN(Q63/101.325))/(0.00336-(1/(273+R63))))*0.000178)","v":2.1712550537918424E-7},4.3400000000000001E-2,5.6336700000000003E-3,4.45,6.1567938987033759E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V63-0.346)*B_Olie_foc*B_Olie_d)/(U63)","v":0},{"$f":"B_Olie_VV/U63","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X63/SUM(X63:Z63)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y63/SUM(X63:Z63)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z63/SUM(X63:Z63)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O63*$J111*(0.01*$AB63)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T63*O63","v":0},"Ikke medtaget",{"$f":"MINA(AD63:AE63)","v":{"$error":"#DIV/0!"}},{"$f":"AG63*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH63/$P63","v":{"$error":"#DIV/0!"}},{"$f":"AI63/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O63*$J111*(0.01*$AC63)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O63*1000000*$S63*$P63/2353","v":0},{"$f":"MINA(AM63:AN63)","v":{"$error":"#DIV/0!"}},{"$f":"AO63*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ63*$AG$111*(0.01*$AC63)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ63*1000000*$S63*$P63/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ63:AR63)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS63,AO63)","v":{"$error":"#DIV/0!"}}]
[156,null,21.85,"Fluoranthen (C16)",{"$f":"B_Olie_156_anv","v":4.8971596474045058E-3},{"$f":"IF(D_Olie_156v = TRUE,0,E64)","v":4.8971596474045058E-3},{"$f":"F64/F$57","v":4.8971596474045049E-3},{"$f":"G64*I$57","v":0},{"$f":"D_Olie_156","v":0},{"$f":"IF(D_Olie_156v=TRUE,I64,H64)","v":0},null,null,{"$f":"J64*100/J$111","v":0},{"$f":"M64/P64","v":0},{"$f":"N64/N$111","v":0},202.3,1.2999999999999998E-6,384,{"$f":"Q64*EXP(((LN(Q64/101.325))/(0.00336-(1/(273+R64))))*0.000178)","v":2.2368673073819918E-7},0.26,8.977395E-4,5.16,5.7784388814859601E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V64-0.346)*B_Olie_foc*B_Olie_d)/(U64)","v":0},{"$f":"B_Olie_VV/U64","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X64/SUM(X64:Z64)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y64/SUM(X64:Z64)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z64/SUM(X64:Z64)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O64*$J111*(0.01*$AB64)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T64*O64","v":0},"Ikke medtaget",{"$f":"MINA(AD64:AE64)","v":{"$error":"#DIV/0!"}},{"$f":"AG64*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH64/$P64","v":{"$error":"#DIV/0!"}},{"$f":"AI64/$AI$111","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_156_gkk","v":0.1},{"$f":"IF(ISNUMBER(AK64),IF(AG64>AK64,AG64/AK64,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O64*$J111*(0.01*$AC64)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O64*1000000*$S64*$P64/2353","v":0},{"$f":"MINA(AM64:AN64)","v":{"$error":"#DIV/0!"}},{"$f":"AO64*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ64*$AG$111*(0.01*$AC64)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ64*1000000*$S64*$P64/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ64:AR64)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS64,AO64)","v":{"$error":"#DIV/0!"}}]
[157,null,20.8,"Pyren (C16)",{"$f":"B_Olie_157_anv","v":4.8971596474045058E-3},{"$f":"IF(ISNUMBER(I65),0,E65)","v":4.8971596474045058E-3},{"$f":"F65/F$57","v":4.8971596474045049E-3},{"$f":"G65*I$57","v":0},null,0,null,null,{"$f":"J65*100/J$111","v":0},{"$f":"M65/P65","v":0},{"$f":"N65/N$111","v":0},202.3,6.0999999999999998E-7,404,{"$f":"Q65*EXP(((LN(Q65/101.325))/(0.00336-(1/(273+R65))))*0.000178)","v":1.019091894718149E-7},0.13500000000000001,1.2057674999999999E-3,4.88,5.7784388814859601E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V65-0.346)*B_Olie_foc*B_Olie_d)/(U65)","v":0},{"$f":"B_Olie_VV/U65","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X65/SUM(X65:Z65)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y65/SUM(X65:Z65)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z65/SUM(X65:Z65)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O65*$J111*(0.01*$AB65)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T65*O65","v":0},"Ikke medtaget",{"$f":"MINA(AD65:AE65)","v":{"$error":"#DIV/0!"}},{"$f":"AG65*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH65/$P65","v":{"$error":"#DIV/0!"}},{"$f":"AI65/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O65*$J111*(0.01*$AC65)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O65*1000000*$S65*$P65/2353","v":0},{"$f":"MINA(AM65:AN65)","v":{"$error":"#DIV/0!"}},{"$f":"AO65*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ65*$AG$111*(0.01*$AC65)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ65*1000000*$S65*$P65/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ65:AR65)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS65,AO65)","v":{"$error":"#DIV/0!"}}]
[]
[2025,">C20 - C25",null,null,{"$f":"B_Olie_2025_anv","v":1.9239102251018689E-2},{"$f":"IF(I67>0,0,E67)","v":1.9239102251018689E-2},{"$f":"F67/F$110","v":1.9239102251018689E-2},{"$f":"(I$110*G67)","v":0},{"$f":"IF(H93>0,H93,0)","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum","C20-C35",null,{"$f":"SUM(AG69:AG70)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI69:AI76)","v":{"$error":"#DIV/0!"}},null,null,null,"Sum","C20-C25",{"$f":"SUM(AO69:AO70)","v":{"$error":"#DIV/0!"}},{"$f":"AO67*$AO$110","v":{"$error":"#DIV/0!"}},"Sum","C20-C25",{"$f":"SUM(AS69:AS70)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT69:AT76)","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel",null," ",null,{"$f":"SUM(F69:F70)","v":1},null,null,{"$f":"IF(J67-SUM(I69:I71)<0,0,J67-SUM(I69:I71))","v":0}]
["201A",">21 - 25, alifater",25,">21 - 25, alifater, Tung olie",{"$f":"B_Olie_201A_anv","v":0},{"$f":"IF(ISNUMBER(I69),0,E69)","v":0},{"$f":"F69/F$68","v":0},{"$f":"G69*I$68","v":0},null,{"$f":"IF(I69>0,I69,H69)","v":0},null,null,{"$f":"J69*100/J$111","v":0},{"$f":"M69/P69","v":0},{"$f":"N69/N$111","v":0},408.8,2.23042E-8,440.1,{"$f":"Q69*EXP(((LN(Q69/101.325))/(0.00336-(1/(273+R69))))*0.000178)","v":2.953252151639657E-9},4.2499999999999998E-4,757252.5,14.58,{"$f":"0.0000084*((78.1/P69)^0.5)","v":3.6715492605442101E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C69+0.43)*B_Olie_foc*B_Olie_d)/(U69)","v":0},{"$f":"B_Olie_VV/U69","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X69/SUM(X69:Z69)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y69/SUM(X69:Z69)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z69/SUM(X69:Z69)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O69*$J111*(0.01*$AB69)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T69*O69","v":0},{"$f":"IF(AD69>AE69,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD69:AE69)","v":{"$error":"#DIV/0!"}},{"$f":"AG69*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH69/$P69","v":{"$error":"#DIV/0!"}},{"$f":"AI69/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O69*$J111*(0.01*$AC69)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O69*1000000*$S69*$P69/2353","v":0},{"$f":"MINA(AM69:AN69)","v":{"$error":"#DIV/0!"}},{"$f":"AO69*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ69*$AG$111*(0.01*$AC69)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ69*1000000*$S69*$P69/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ69:AR69)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS69,AO69)","v":{"$error":"#DIV/0!"}}]
["201B",null,{"$f":"4.12+0.02*R70+(0.000065*R70*R70)","v":22.65703465},">21 - 25, alifater, Olieblandinger",{"$f":"B_Olie_201B_anv","v":1},{"$f":"IF(ISNUMBER(I70),0,E70)","v":1},{"$f":"F70/F$68","v":1},{"$f":"G70*I$68","v":0},null,{"$f":"IF(I70>0,I70,H70)","v":0},null,null,{"$f":"J70*100/J$111","v":0},{"$f":"M70/P70","v":0},{"$f":"N70/N$111","v":0},352.69,2.0083000000000001E-7,401.9,{"$f":"Q70*EXP(((LN(Q70/101.325))/(0.00336-(1/(273+R70))))*0.000178)","v":3.0066683752352857E-8},2.9000000000000002E-8,37693,12.62,{"$f":"0.0000084*((78.1/P70)^0.5)","v":3.9528308464137552E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C70+0.43)*B_Olie_foc*B_Olie_d)/(U70)","v":0},{"$f":"B_Olie_VV/U70","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X70/SUM(X70:Z70)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y70/SUM(X70:Z70)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z70/SUM(X70:Z70)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O70*$J111*(0.01*$AB70)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T70*O70","v":0},{"$f":"IF(AD70>AE70,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD70:AE70)","v":{"$error":"#DIV/0!"}},{"$f":"AG70*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH70/$P70","v":{"$error":"#DIV/0!"}},{"$f":"AI70/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O70*$J111*(0.01*$AC70)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O70*1000000*$S70*$P70/2353","v":0},{"$f":"MINA(AM70:AN70)","v":{"$error":"#DIV/0!"}},{"$f":"AO70*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ70*$AG$111*(0.01*$AC70)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ70*1000000*$S70*$P70/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ70:AR70)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS70,AO70)","v":{"$error":"#DIV/0!"}}]
[202,">21 - 25, aromater",null,"Ingen repræsentanter",null,null,null,0,null,{"$f":"IF(I71>0,I71,H71)","v":0}]
[]
[2535,">C25 - C35",null,null,{"$f":"B_Olie_2535_anv","v":4.3725232388678842E-2},{"$f":"IF(I73>0,0,E73)","v":4.3725232388678842E-2},{"$f":"F73/F$110","v":4.3725232388678842E-2},{"$f":"I$110*G73","v":0},{"$f":"IF(H94>0,H94,0)","v":0},{"$f":"IF(I73>0,I73,H73)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum","C25-C35",null,{"$f":"SUM(AG75:AG85)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI75:AI85)","v":{"$error":"#DIV/0!"}},null,null,null,"Sum","C25-C35",{"$f":"SUM(AO75:AO85)","v":{"$error":"#DIV/0!"}},{"$f":"AO73*$AO$110","v":{"$error":"#DIV/0!"}},"Sum","C25-C35",{"$f":"SUM(AS75:AS85)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT75:AT85)","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel",null," ",null,{"$f":"SUM(F75:F85)","v":1},null,null,{"$f":"IF(J$73-SUM(I75:I85)<0,0,J$73-SUM(I75:I85))","v":0}]
["251A",">25 - 35, alifater",{"$f":"4.12+0.02*R75+(0.000065*R75*R75)","v":25.444852213948739},">25 - 35, alifater, Tung olie",{"$f":"B_Olie_251A_anv","v":0},{"$f":"IF(ISNUMBER(I75),0,E75)","v":0},{"$f":"F75/F$74","v":0},{"$f":"IF(E75=0,0,G75*$I$74)","v":0},null,{"$f":"IF(H75<0,0,H75)","v":0},null,null,{"$f":"J75*100/J$111","v":0},{"$f":"M75/P75","v":0},{"$f":"N75/N$111","v":0},407.40647650551284,2.2166069970774379E-8,439.2333420889355,3.0650884499592387E-9,4.3468322206145456E-4,707619.73693936015,14.533637648509041,3.0055777156880082E-6,{"$f":"((1-B_Olie_e)*10^(0.45*C75+0.43)*B_Olie_foc*B_Olie_d)/(U75)","v":0},{"$f":"B_Olie_VV/U75","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X75/SUM(X75:Z75)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y75/SUM(X75:Z75)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z75/SUM(X75:Z75)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O75*$J111*(0.01*$AB75)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T75*O75","v":0},{"$f":"IF(AD75>AE75,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD75:AE75)","v":{"$error":"#DIV/0!"}},{"$f":"AG75*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH75/$P75","v":{"$error":"#DIV/0!"}},{"$f":"AI75/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O75*$J111*(0.01*$AC75)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O75*1000000*$S75*$P75/2353","v":0},{"$f":"MINA(AM75:AN75)","v":{"$error":"#DIV/0!"}},{"$f":"AO75*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"1000*S75*B_Olie_1*(0.01*$AC75)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$AJ75*1000000*$S75*$P75/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ75:AR75)","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AR75:AS75)","v":{"$error":"#DIV/0!"}}]
["251B",null,{"$f":"4.12+0.02*R76+(0.000065*R76*R76)","v":25.511720650000001},">25 - 35, alifater, Olieblandinger",{"$f":"B_Olie_251B_anv","v":0.9},{"$f":"IF(ISNUMBER(I76),0,E76)","v":0.9},{"$f":"F76/F$74","v":0.9},{"$f":"IF(E76=0,0,G76*$I$74)","v":0},null,{"$f":"IF(H76<0,0,H76)","v":0},null,null,{"$f":"J76*100/J$111","v":0},{"$f":"M76/P76","v":0},{"$f":"N76/N$111","v":0},408.8,2.23042E-8,440.1,{"$f":"Q76*EXP(((LN(Q76/101.325))/(0.00336-(1/(273+R76))))*0.000178)","v":2.953252151639657E-9},4.2499999999999998E-4,757252,14.58,{"$f":"0.0000084*((78.1/P76)^0.5)","v":3.6715492605442101E-6},{"$f":"((1-B_Olie_e)*10^(0.45*C76+0.43)*B_Olie_foc*B_Olie_d)/(U76)","v":0},{"$f":"B_Olie_VV/U76","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X76/SUM(X76:Z76)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y76/SUM(X76:Z76)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z76/SUM(X76:Z76)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O76*$J111*(0.01*$AB76)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T76*O76","v":0},{"$f":"IF(AD76>AE76,\"Ja\",\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AD76:AE76)","v":{"$error":"#DIV/0!"}},{"$f":"AG76*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH76/$P76","v":{"$error":"#DIV/0!"}},{"$f":"AI76/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O76*$J111*(0.01*$AC76)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O76*1000000*$S76*$P76/2353","v":0},{"$f":"MINA(AM76:AN76)","v":{"$error":"#DIV/0!"}},{"$f":"AO76*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"1000*S76*B_Olie_1*(0.01*$AC76)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$AJ76*1000000*$S76*$P76/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ76:AR76)","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AR76:AS76)","v":{"$error":"#DIV/0!"}}]
[252,">25 - 35, aromater",null,"Sum >25 - 35 aromater",null,null,{"$f":"MAX(G84:G85)","v":0.1},{"$f":"SUM(H78:H83)","v":0.8600000000000001},null,{"$f":"SUM(J78:J85)","v":0}]
[253,null,26.37,"Benzo(a)anthracen (C18)",null,null,{"$f":"B_Olie_253_fastdel_anv","v":0.1},{"$f":"IF(I78>0,0,G78)","v":0.1},null,{"$f":"IF(I78>0,I78,IF($H$77>($G$77*$I$74),H78*($G$77*$I$74)/$H$77,H78))","v":0},null,null,{"$f":"J78*100/J$111","v":0},{"$f":"M78/P78","v":0},{"$f":"N78/N$111","v":0},228.3,2.7E-8,437.6,{"$f":"Q78*EXP(((LN(Q78/101.325))/(0.00336-(1/(273+R78))))*0.000178)","v":3.6192855741595076E-9},9.4000000000000004E-3,1.2159E-3,5.76,5.4394565218975376E-6,{"$f":"((1-B_Olie_e)*10^(0.989*V78-0.346)*B_Olie_foc*B_Olie_d)/(U78)","v":0},{"$f":"B_Olie_VV/U78","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X78/SUM(X78:Z78)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y78/SUM(X78:Z78)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z78/SUM(X78:Z78)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O78*$J111*(0.01*$AB78)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T78*O78","v":0},"Ikke medtaget",{"$f":"MINA(AD78:AE78)","v":{"$error":"#DIV/0!"}},{"$f":"AG78*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH78/$P78","v":{"$error":"#DIV/0!"}},{"$f":"AI78/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O78*$J111*(0.01*$AC78)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O78*1000000*$S78*$P78/2353","v":0},{"$f":"MINA(AM78:AN78)","v":{"$error":"#DIV/0!"}},{"$f":"AO78*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ78*$AG$111*(0.01*$AC78)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ78*1000000*$S78*$P78/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ78:AR78)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS78,AO78)","v":{"$error":"#DIV/0!"}}]
[254,null,27.41,"Chrysen (C18)",null,null,{"$f":"B_Olie_254_fastdel_anv","v":0.15},{"$f":"IF(I79>0,0,G79)","v":0.15},null,0,null,null,0,0,0,228.3,8.3999999999999999E-10,448,8.4053110291696773E-11,2.0999999999999999E-3,5.2992974999999999E-4,5.81,5.4394565218975376E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O79*$J111*(0.01*$AB79)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O79*$J111*(0.01*$AC79)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[255,null,30.14,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"B_Olie_255_fastdel_anv","v":0.3},{"$f":"IF(D_Olie_255v=TRUE,0,G80)","v":0.3},{"$f":"D_Olie_255","v":0},0,null,null,0,0,0,252.3,4.9999999999999993E-10,357,3.6613242749387275E-11,1.5E-3,6.6570524999999997E-5,5.78,5.1742789740511641E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O80*$J111*(0.01*$AB80)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O80*$J111*(0.01*$AC80)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[256,null,31.34,"Benzo(a)pyren",null,null,{"$f":"B_Olie_256_fastdel_anv","v":0.15},{"$f":"IF(D_Olie_256v=TRUE,0,G81)","v":0.15},{"$f":"D_Olie_256","v":0},0,{"$f":"D_Olie_256_jkk","v":0.3},{"$f":"IF(ISNUMBER(K81),IF(J81>K81,J81/K81,\"Nej\"),\" \")","v":"Nej"},0,0,0,252.3,7.2999999999999996E-10,495,7.9352171631410997E-11,1.6199999999999999E-3,4.6305525000000001E-5,6.13,5.1742789740511641E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O81*$J111*(0.01*$AB81)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_Olie_256_gkk","v":0.01},{"$f":"IF(ISNUMBER(AK81),IF(AG81>AK81,AG81/AK81,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},{"$f":"1000*O81*$J111*(0.01*$AC81)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[257,null,33.92,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"B_Olie_257_fastdel_anv","v":0.01},{"$f":"IF(D_Olie_257v=TRUE,0,G82)","v":0.01},{"$f":"D_Olie_257","v":0},0,{"$f":"D_Olie_257_jkk","v":0.3},{"$f":"IF(ISNUMBER(K82),IF(J82>K82,J82/K82,\"Nej\"),\" \")","v":"Nej"},0,0,0,278.39999999999998,3.7000000000000004E-13,524,2.2260156805741643E-14,2.49E-3,1.4286825E-5,6.75,4.9257668316019948E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O82*$J111*(0.01*$AB82)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O82*$J111*(0.01*$AC82)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[258,null,34.01,"Benzo(g,h,i)perylen (C22)",null,null,{"$f":"B_Olie_258_fastdel_anv","v":0.15},{"$f":"IF(D_Olie_258v=TRUE,0,G83)","v":0.15},{"$f":"D_Olie_258","v":0},0,null,null,0,0,0,276.3,1.3E-11,520,1.0487543252634132E-12,2.5999999999999998E-4,3.3538575000000003E-5,6.63,4.9444503816447828E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O83*$J111*(0.01*$AB83)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O83*$J111*(0.01*$AC83)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["259A",null,{"$f":"4.12+0.02*R84+(0.000065*R84*R84)","v":27.404624817544899},">25 - 35, aromater, øvrige, Tung olie",{"$f":"B_Olie_259A_anv","v":0},{"$f":"IF(ISNUMBER(I84),0,E84)","v":0},{"$f":"F84/F$74","v":0},{"$f":"IF(E84=0,0,(($I$74*G84)-SUM($J$78:$J$83)))","v":0},null,{"$f":"IF(H84<0,0,H84)","v":0},null,null,0,0,0,250.05356087955366,2.7101747876509737E-9,464.12927952175352,2.8704398283342149E-10,3.9685392369703372E-2,1.8382187846013197E-5,6.0585189187866568,5.5943064295556175E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C84+2.3)*B_Olie_foc*B_Olie_d)/(U84)","v":0},0,0,{"$f":"100*X84/SUM(X84:Z84)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y84/SUM(X84:Z84)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"1000*O84*$J111*(0.01*$AB84)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O84*$J111*(0.01*$AC84)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["259B",null,{"$f":"4.12+0.02*R85+(0.000065*R85*R85)","v":32.008465000000001},">25 - 35, aromater, øvrige, Olieblandinger",{"$f":"B_Olie_259B_anv","v":0.1},{"$f":"IF(ISNUMBER(I85),0,E85)","v":0.1},{"$f":"F85/F$74","v":0.1},{"$f":"IF(E85=0,0,($I$74*G85-SUM($J$78:$J$83)))","v":0},null,{"$f":"IF(H85<0,0,H85)","v":0},null,null,0,0,0,278.36,4.9608999999999999E-10,519,5.4411372337535734E-11,4.3099999999999996E-3,4.95479E-5,7.11,{"$f":"0.0000084*((78.1/P85)^0.5)","v":4.4493993711079091E-6},{"$f":"((1-B_Olie_e)*10^(0.1*C85+2.3)*B_Olie_foc*B_Olie_d)/(U85)","v":0},0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O85*$J111*(0.01*$AB85)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O85*$J111*(0.01*$AC85)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[3540,">C35",null,null,{"$f":"B_Olie_3540_anv","v":2.0999500631874973E-2},{"$f":"IF(I87>0,0,E87)","v":2.0999500631874973E-2},{"$f":"F87","v":2.0999500631874973E-2},{"$f":"I$109*G87","v":0},null,{"$f":"IF(I87>0,I87,H87)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum",">C35",null,{"$f":"SUM(AG89:AG90)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI89:AI90)","v":{"$error":"#DIV/0!"}},null,null,null,"Sum",">C35",{"$f":"SUM(AO89:AO90)","v":{"$error":"#DIV/0!"}},{"$f":"AO87*$AO$110","v":{"$error":"#DIV/0!"}},"Sum",">C35",{"$f":"SUM(AS89:AS90)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT89:AT90)","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel",null,null,null,{"$f":"SUM(F89:F90)","v":1},null,null,{"$f":"IF(J$87-SUM(I89:I90)<0,0,J$87-SUM(I89:I90))","v":0}]
[351,">35 - 44, alifater",35,"Pentatriacontan (C35)",{"$f":"B_Olie_351_anv","v":0.84},{"$f":"IF(ISNUMBER(I89),0,E89)","v":0.84},{"$f":"F89/F$88","v":0.84},{"$f":"(I$88*G89)","v":0},null,{"$f":"IF(I89>0,I89,H89)","v":0},null,null,{"$f":"J89*100/J$111","v":0},{"$f":"M89/P89","v":0},{"$f":"N89/N$111","v":0},492.9538,7.1860756578947365E-13,490,{"$f":"Q89*EXP((1*(LN(Q89/101.324))/(0.00336-(1/(273+R89))))*0.000178)","v":4.2418572078348355E-14},2.4700000000000001E-13,640374,17.53,3.7017352631160009E-6,{"$f":"((1-B_Olie_e)*10^(0.45*C89+0.43)*B_Olie_foc*B_Olie_d)/(U89)","v":0},{"$f":"B_Olie_VV/U89","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X89/SUM(X89:Z89)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y89/SUM(X89:Z89)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z89/SUM(X89:Z89)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O89*$J111*(0.01*$AB89)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T89*O89","v":0},"Ikke medtaget",{"$f":"MINA(AD89:AE89)","v":{"$error":"#DIV/0!"}},{"$f":"AG89*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH89/$P89","v":{"$error":"#DIV/0!"}},{"$f":"AI89/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O89*$J111*(0.01*$AC89)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O89*1000000*$S89*$P89/2353","v":0},{"$f":"MINA(AM89:AN89)","v":{"$error":"#DIV/0!"}},{"$f":"AO89*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ89*$AG$111*(0.01*$AC89)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ89*1000000*$S89*$P89/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ89:AR89)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS89,AO89)","v":{"$error":"#DIV/0!"}}]
[352,">35 - 44, aromater",35.01,"Indeno(1,2,3-cd)pyren (C22)",{"$f":"B_Olie_352_anv","v":0.16},{"$f":"IF(D_Olie_352v=TRUE,0,E90)","v":0.16},{"$f":"F90/F$88","v":0.16},{"$f":"(I$88*G90)","v":0},{"$f":"D_Olie_352","v":0},{"$f":"IF(D_Olie_352v=TRUE,I90,H90)","v":0},null,null,{"$f":"J90*100/J$111","v":0},{"$f":"M90/P90","v":0},{"$f":"N90/N$111","v":0},276.33679999999998,1.6665296052631578E-11,536,{"$f":"Q90*EXP(((LN(Q90/101.325))/(0.00336-(1/(273+R90))))*0.000178)","v":1.4139093320994384E-12},1.9000000000000001E-4,3.52611E-5,6.7,4.9441211424116288E-6,{"$f":"((1-B_Olie_e)*10^(0.1*C90+2.3)*B_Olie_foc*B_Olie_d)/(U90)","v":0},{"$f":"B_Olie_VV/U90","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X90/SUM(X90:Z90)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y90/SUM(X90:Z90)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z90/SUM(X90:Z90)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O90*$J111*(0.01*$AB90)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T90*O90","v":0},"Ikke medtaget",{"$f":"MINA(AD90:AE90)","v":{"$error":"#DIV/0!"}},{"$f":"AG90*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH90/$P90","v":{"$error":"#DIV/0!"}},{"$f":"AI90/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O90*$J111*(0.01*$AC90)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O90*1000000*$S90*$P90/2353","v":0},{"$f":"MINA(AM90:AN90)","v":{"$error":"#DIV/0!"}},{"$f":"AO90*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ90*$AG$111*(0.01*$AC90)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ90*1000000*$S90*$P90/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ90:AR90)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS90,AO90)","v":{"$error":"#DIV/0!"}}]
[]
[2040,">C20 - C35",null,null,{"$f":"SUM(E93:E94)","v":6.2964334639697528E-2},null,null,{"$f":"B_Olie_2025_ct+B_Olie_2535_ct","v":0},{"$f":"D_Olie_2040","v":0},{"$f":"IF(I92>0,I92,H92)","v":0},{"$f":"D_Olie_2040_jkk","v":100},{"$f":"IF(ISNUMBER(K92),IF(J92>K92,J92/K92,\"Nej\"),\" \")","v":"Nej"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum","C20-C35",null,{"$f":"B_Olie_2535_cv+B_Olie_201B_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"AI87+AI73+AI70","v":{"$error":"#DIV/0!"}},null,null,null,"Sum","C20-C35",{"$f":"B_Olie_2535_cl+B_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"AO92*$AO$110","v":{"$error":"#DIV/0!"}},"Sum","C20-C35",{"$f":"B_Olie_2535_cl+B_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_Olie_3540_cl+B_Olie_2535_cl+B_Olie_201B_cl","v":{"$error":"#DIV/0!"}}]
[null,null,null,"C20-C25",{"$f":"E67","v":1.9239102251018689E-2},null,{"$f":"E93/E$92","v":0.30555555555555558},{"$f":"G93*I$92","v":0}]
[null,null,null,"C25-C35",{"$f":"E73","v":4.3725232388678842E-2},null,{"$f":"E94/E$92","v":0.69444444444444453},{"$f":"G94*I$92","v":0}]
[null,null,null,"C35-C40",{"$f":"E87","v":2.0999500631874973E-2},null,{"$f":"E95/E$92","v":0.3335142148653038},{"$f":"G95*I$92","v":0}]
[]
[20,"Sum af 7 PAH'er jord",null,null,null,null,null,null,null,{"$f":"J81+J80+J82+J64+B_Olie_352_ct","v":0},{"$f":"D_Olie_20_jkk","v":4},{"$f":"IF(ISNUMBER(K97),IF(J97>K97,J97/K97,\"Nej\"),\" \")","v":"Nej"}]
[21,"Sum af 4 PAH'er vand",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_Olie_352_cv+B_Olie_258_cv+B_Olie_255_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"AI83+AI81+AI80","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_21_gkk","v":0.1},{"$f":"IF(ISNUMBER(AK98),IF(AG98>AK98,AG98/AK98,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[]
[null,"NSO-forbindelser"]
[10,null,11.7,"Benzo(b)thiophen",null,null,null,{"$f":"B_Olie_10_fastandel_anv","v":0.02},0,{"$f":"IF(D_Olie_10v=TRUE,I101,H101)","v":0.02},null,null,{"$f":"J101*100/J$111","v":49.875311720698249},{"$f":"M101/P101","v":0.37166185816129499},{"$f":"N101/N$111","v":0.51367754815257893},134.19540000000001,3.1654000000000002E-2,221,{"$f":"Q101*EXP((1*(LN(Q101/101.324))/(0.00336-(1/(273+R101))))*0.000178)","v":1.0797055721932987E-2},130,3.267666769230769E-2,3.12,7.9048861340223873E-6,{"$f":"((1-B_Olie_e)*10^(1.04*V101-0.84)*B_Olie_foc*B_Olie_d)/(U101)","v":0},{"$f":"B_Olie_VV/U101","v":0},{"$f":"B_Olie_VL*1000/(8.314*283)","v":0},{"$f":"100*X101/SUM(X101:Z101)","v":{"$error":"#DIV/0!"}},{"$f":"100*Y101/SUM(X101:Z101)","v":{"$error":"#DIV/0!"}},{"$f":"100*Z101/SUM(X101:Z101)","v":{"$error":"#DIV/0!"}},{"$f":"1000*O101*$J111*(0.01*$AB101)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},{"$f":"1000*T101*O101","v":66778.081259835264},"Ikke medtaget",{"$f":"MINA(AD101:AE101)","v":{"$error":"#DIV/0!"}},{"$f":"AG101*100/$AG$111","v":{"$error":"#DIV/0!"}},{"$f":"AH101/$P101","v":{"$error":"#DIV/0!"}},{"$f":"AI101/$AI$111","v":{"$error":"#DIV/0!"}},null,null,{"$f":"1000*O101*$J111*(0.01*$AC101)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},{"$f":"$O101*1000000*$S101*$P101/2353","v":316.30905792045945},{"$f":"MINA(AM101:AN101)","v":{"$error":"#DIV/0!"}},{"$f":"AO101*$AO$110","v":{"$error":"#DIV/0!"}},{"$f":"AJ101*$AG$111*(0.01*$AC101)*$H$11/$H$6","v":{"$error":"#DIV/0!"}},{"$f":"$AJ101*1000000*$S101*$P101/2353","v":{"$error":"#DIV/0!"}},{"$f":"MINA(AQ101:AR101)","v":{"$error":"#DIV/0!"}},{"$f":"MAXA(AS101,AO101)","v":{"$error":"#DIV/0!"}}]
[11,null,15.21,"Dibenzofuran",null,null,null,{"$f":"B_Olie_11_fastandel_anv","v":0},{"$f":"D_olie_11","v":0},{"$f":"IF(D_Olie_11v=TRUE,I102,H102)","v":0},null,null,0,0,0,168.19460000000001,3.5063782894736843E-4,287,8.4608815838286969E-5,3.1,1.7893245806451612E-2,4.12,6.3372733653665426E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O102*$J111*(0.01*$AB102)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O102*$J111*(0.01*$AC102)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[12,null,17.96,"Dibenzothiophen",null,null,null,{"$f":"B_Olie_12_fastandel_anv","v":5.0000000000000001E-3},{"$f":"D_olie_12","v":0},{"$f":"IF(D_Olie_12v=TRUE,I103,H103)","v":5.0000000000000001E-3},null,null,12.468827930174562,6.7671511741185936E-2,9.3529468972048821E-2,184.2552,2.7265000000000001E-5,332.5,5.6375202907530211E-6,1.47,3.4173988095238094E-3,4.38,6.0547830833864374E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O103*$J111*(0.01*$AB103)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},137.48831938891178,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O103*$J111*(0.01*$AC103)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},4.1289004569856909E-2,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,null,18.82,"Acridin",null,null,null,{"$f":"B_Olie_13_fastandel_anv","v":0},{"$f":"D_olie_13","v":0},{"$f":"IF(D_Olie_13v=TRUE,I104,H104)","v":0},null,null,0,0,0,179.2208,1.7999999999999997E-5,346,3.6854293678220715E-6,38.4,8.4009375000000007E-5,3.4,6.1392350270271861E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O104*$J111*(0.01*$AB104)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},0,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O104*$J111*(0.01*$AC104)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[14,null,19.39,"Carbazol",null,null,null,{"$f":"B_Olie_14_fastandel_anv","v":0.01},{"$f":"D_olie_14","v":0},{"$f":"IF(D_Olie_14v=TRUE,I105,H105)","v":0.01},null,null,24.937655860349125,0.14913991799732507,0.20612776298205787,167.2098,9.9750000000000003E-8,354.7,1.2346563991810438E-8,1.8,9.2662208333333337E-6,2.36,1.2376252771055592E-5,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O105*$J111*(0.01*$AB105)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},371.02997336770414,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O105*$J111*(0.01*$AC105)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},1.8085161943135085E-4,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,null,{"$f":"4.12+0.02*R106+(0.000065*R106*R106)","v":10.005032649999999},"Anilin",null,null,null,{"$f":"B_Olie_15_fastandel_anv","v":1E-4},{"$f":"D_olie_15","v":0},{"$f":"IF(D_Olie_15v=TRUE,I106,H106)","v":1E-4},null,null,0.24937655860349126,2.6777828215304878E-3,3.7009902524135921E-3,93.128,6.5327960526315787E-2,184.1,2.1411141018130252E-2,36000,1.6859116944444445E-4,0.9,8.5166407345416544E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O106*$J111*(0.01*$AB106)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},133235.64908688932,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O106*$J111*(0.01*$AC106)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},3.1362891971971809,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[16,null,{"$f":"4.12+0.02*R107+(0.000065*R107*R107)","v":7.099642600000001},"Dimethyldisulfid",null,null,null,{"$f":"B_Olie_16_fastandel_anv","v":5.0000000000000001E-3},{"$f":"D_olie_16","v":0},{"$f":"IF(D_Olie_16v=TRUE,I107,H107)","v":5.0000000000000001E-3},null,null,12.468827930174562,0.13238037327103222,0.18296422964090067,94.189400000000006,3.8170999999999999,109.8,1.7487294403378397,3000,0.11932,1.77,8.468518688960739E-6,0,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"1000*O107*$J111*(0.01*$AB107)*B_Olie_p/(B_Olie_VV)","v":{"$error":"#DIV/0!"}},548892.68892270199,"Ikke medtaget",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"1000*O107*$J111*(0.01*$AC107)*B_Olie_p/(B_Olie_VL)","v":{"$error":"#DIV/0!"}},12807.634230955107,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[1,"SUM af kulbrinter C6 - C35",null,null,null,null,null,{"$f":"I73+I67+I56+I41+I25","v":0},{"$f":"D_olie_1","v":0},{"$f":"IF(D_Olie_1v=TRUE,I109,H109)","v":0},{"$f":"D_Olie_1_jkk","v":100},{"$f":"IF(ISNUMBER(K109),IF(J109>K109,J109/K109,\"Nej\"),\" \")","v":"Nej"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUM af kulbrinter C6 - C35",null,null,{"$f":"AG73+AG67+AG56+AG41+AG25","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Olie_1_gkk","v":9},{"$f":"IF(ISNUMBER(AK109),IF(AG109>AK109,AG109/AK109,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}},"SUM af kulbrinter C6 - C35",null,{"$f":"AO73+AO67+AO56+AO41+AO25","v":{"$error":"#DIV/0!"}},null,"SUM af kulbrinter C6 - C35",null,{"$f":"SUM(AS101:AS107)+AS87+AS73+AS67+AS56+AS41+AS25+AS19","v":{"$error":"#DIV/0!"}},{"$f":"AT73+AT67+AT56+AT41+AT25","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"IF(ISNUMBER(AU109),IF(AT109>AU109,AT109/AU109,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[null,"Beregnet andel af fraktioner",null,null,null,{"$f":"F73+F67+F56+F41+F25","v":1},null,null,{"$f":"IF(J$109-H109<0,0,J$109-H109)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"1-AO19/AO111","v":{"$error":"#DIV/0!"}}]
[null,"SUM af Alle kulbrinter C5 - C40 og NSO",null,null,null,null,null,null,{"$f":"I87+I73+I67+I56+I41+I25+I19+SUM(I101:I107)","v":0},{"$f":"J87+J73+J67+J56+J41+J25+J19+SUM(J101:J107)","v":4.0100000000000004E-2},null,null,{"$f":"SUM(M27:M107)","v":99.999999999999972},{"$f":"SUM(N27:N107)","v":0.72353144399236879},{"$f":"SUM(O27:O107)","v":0.99999999999999989},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sum alle kulbrinter",null,null,{"$f":"SUM(AG101:AG107)+AG87+AG73+AG67+AG56+AG41+AG25+AG19","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(AI101:AI107)+AI87+AI73+AI67+AI56+AI41+AI25+AI19","v":{"$error":"#DIV/0!"}},null,null,null,"Sum alle kulbrinter",null,{"$f":"SUM(AO101:AO107)+AO87+AO73+AO67+AO56+AO41+AO25+AO19","v":{"$error":"#DIV/0!"}},null,"Sum alle kulbrinter",null,{"$f":"SUM(AS101:AS107)+AS87+AS73+AS67+AS56+AS41+AS25+AS19","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AT101:AT107)+AT87+AT73+AT67+AT56+AT41+AT25+AT19","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fri fase ?",null,{"$f":"IF(COUNTIF(AF20:AF107,\"JA\")>3,\"Risiko for frifase\",\"Nej\")","v":"Nej"}]
["OLIEPROFILER"]
[]
[null,"Valgte profil",{"$f":"D_Olie_profil","v":1}]
[null,null,null,null,1,null,2,null,3]
[null,"Interval","EC nummer","Modelstof","Olie/benzinblanding",null,"Tung olie",null,"Egen profil",null,"ANVENDES"]
[null,null,null,null,"% andel","Fast andel","% andel","Fast andel","% andel","Fast andel","% andel","Fast andel"]
[null,null,null,null,null,null,null,null,null,null,"B_Olie_profil_n","B_Olie_pro_fast_n","Cellenavn"]
[50,">C5-C6",null,null,{"$f":"4.4/238.1009","v":1.8479560556049979E-2},null,0,null,null,null,{"$f":"CHOOSE(C$115,E120,G120,I120)","v":1.8479560556049979E-2},null,"B_Olie_50_anv"]
[51,">5 - 6, alifater",null,"2-methylbutan",{"$f":"0.1452/4.4","v":3.2999999999999995E-2},null,0,null,null,null,{"$f":"CHOOSE(C$115,E121,G121,I121)","v":3.2999999999999995E-2},null,"B_Olie_51_anv"]
[511,null,null,"Pentan",{"$f":"0.052/4.4","v":1.1818181818181816E-2},null,0,null,null,null,{"$f":"CHOOSE(C$115,E122,G122,I122)","v":1.1818181818181816E-2},null,"B_Olie_511_anv"]
[512,null,null,"2-methylpentan",{"$f":"2.57/4.4","v":0.58409090909090899},null,0,null,null,null,{"$f":"CHOOSE(C$115,E123,G123,I123)","v":0.58409090909090899},null,"B_Olie_512_anv"]
[513,null,null,"3-methylpentan (C6)",{"$f":"1.63/4.4","v":0.37045454545454543},null,0,null,null,null,{"$f":"CHOOSE(C$115,E124,G124,I124)","v":0.37045454545454543},null,"B_Olie_513_anv"]
[]
[510,">C6 - C10",null,null,{"$f":"(113.08-4.4)/228.7009","v":0.47520582560016161},null,{"$f":"8/223","v":3.5874439461883408E-2},null,null,null,{"$f":"CHOOSE($C$115,E126,G126,I126)","v":0.47520582560016161},null,"B_Olie_510_anv"]
[52,">5 - 7, aromater",6.5,"Benzen (C6) (>5-7, aromater)",{"$f":"0.01/105.6","v":9.469696969696971E-5},null,{"$f":"0.6*0.00025","v":1.4999999999999999E-4},null,null,null,{"$f":"CHOOSE(C$115,E127,G127,I127)","v":9.469696969696971E-5},null,"B_Olie_52_anv"]
[53,">6 - 8, alifater",null,">6 - 8, alifater",{"$f":"46.57/105.6","v":0.44100378787878791},null,0,null,null,null,{"$f":"CHOOSE(C$115,E128,G128,I128)","v":0.44100378787878791},null,"B_Olie_53_anv"]
[54,">7 - 8, aromater",7.58,"Toluen (C7)(>7-8, aromater",{"$f":"0.01/105.6","v":9.469696969696971E-5},null,{"$f":"0.6*0.00025","v":1.4999999999999999E-4},null,null,null,{"$f":"CHOOSE(C$115,E129,G129,I129)","v":9.469696969696971E-5},null,"B_Olie_54_anv"]
["55A",">8 - 10, alifater",null,">8 - 10, alifater, Tung Olie",null,null,0.4,null,null,null,{"$f":"CHOOSE(C$115,E130,G130,I130)","v":0},null,"B_Olie_55A_anv"]
["55B",null,null,">8 - 10, alifater, Olieblamdinger",{"$f":"17.23/105.6","v":0.1631628787878788},null,null,null,null,null,{"$f":"CHOOSE(C$115,E131,G131,I131)","v":0.1631628787878788},null,"B_Olie_55B_anv"]
[56,">8 -10, aromater",null,"Sum >8-10, aromater"]
[571,null,null,"o-Xylen"]
[572,null,null,"m+p-Xylen"]
[57,null,8.6,"Sum Xylener regnes som m-Xylen (C8)",{"$f":"0.01/105.6","v":9.469696969696971E-5},null,{"$f":"0.6*0.00025","v":1.4999999999999999E-4},null,null,null,{"$f":"CHOOSE(C$115,E135,G135,I135)","v":9.469696969696971E-5},null,"B_Olie_57_anv"]
[58,null,8.5,"Ethylbenzen (C8)",{"$f":"0.01/105.6","v":9.469696969696971E-5},null,{"$f":"0.6*0.00025","v":1.4999999999999999E-4},null,null,null,{"$f":"CHOOSE(C$115,E136,G136,I136)","v":9.469696969696971E-5},null,"B_Olie_58_anv"]
[59,null,9.6199999999999992,"1,3,5-trimethylbenzen (C9)",null,0.3,null,3.0000000000000001E-3,null,3.0000000000000001E-3,null,{"$f":"CHOOSE(C$115,F137,H137,J137)","v":0.3},"B_Olie_59_fastdel_anv"]
["60A",null,null,">8 -10, aromater,øvrige, Tung olie",0,null,0.59940000000000004,null,null,null,{"$f":"CHOOSE(C$115,E138,G138,I138)","v":0},null,"B_Olie_60A_anv"]
["60B",null,null,">8 -10, aromater,øvrige, Olieblandinger",{"$f":"41.46/105.6","v":0.39261363636363639},null,0,null,null,null,{"$f":"CHOOSE(C$115,E139,G139,I139)","v":0.39261363636363639},null,"B_Olie_60B_anv"]
[]
[1015,">C10 - C15",null,null,{"$f":"110*0.74578/228.7009","v":0.3587034419191179},null,{"$f":"48.2426/223","v":0.21633452914798207},null,null,null,{"$f":"CHOOSE(C$115,E141,G141,I141)","v":0.3587034419191179},null,"B_Olie_1015_anv"]
[101,">10 - 12, alifater",12,"Dodecan(C12)",9.3861460484325143E-2,null,{"$f":"14.45/48.2426","v":0.29952780322785255},null,null,null,{"$f":"CHOOSE(C$115,E142,G142,I142)","v":9.3861460484325143E-2},null,"B_Olie_101_anv"]
[102,">10 - 12, aromater",null,"Sum >10 - 12 aromater"]
[103,null,11.69,"Naphthalen (C10)",2.9499316152216473E-3,null,{"$f":"0.0009/48.2426","v":1.8655710927686316E-5},null,null,null,{"$f":"CHOOSE(C$115,E144,G144,I144)","v":2.9499316152216473E-3},null,"B_Olie_103_anv"]
["104A",null,null,">10 - 12, aromater, øvrige, Tung Olie",0,null,{"$f":"9.35/48.2426","v":0.1938121079709634},null,null,null,{"$f":"CHOOSE(C$115,E145,G145,I145)","v":0},null,"B_Olie_104A_anv"]
["104B",null,null,">10 - 12, aromater, øvrige, Olieblanding",0.5870363914291078,null,0,null,null,null,{"$f":"CHOOSE(C$115,E146,G146,I146)","v":0.5870363914291078},null,"B_Olie_104B_anv"]
["105A",">12 - 16, alifater",null,">12 - 16, alifater, Tung Olie",0,null,{"$f":"21.25/48.2426","v":0.4404820635703714},null,null,null,{"$f":"CHOOSE(C$115,E147,G147,I147)","v":0},null,"B_Olie_105A_anv"]
["105B",null,null,">12 - 16, alifater, Olieblandinger",0.2949931615221647,null,0,null,null,null,{"$f":"CHOOSE(C$115,E148,G148,I148)","v":0.2949931615221647},null,"B_Olie_105B_anv",null,null,14.4549,17.001799999999999,{"$f":"P$166*Q148/100","v":14.45153},{"$f":"R148/R$155","v":0.29955951793642965}]
[106,">12 - 16, aromater",null,"Sum >10 - 12 aromater",null,null,null,null,null,null,null,null,null,null,null,8.9999999999999998E-4,1E-3,8.5000000000000006E-4,1.7619282542814861E-5]
[107,null,15.06,"Acenaphthylen (C12)",8.045268041513582E-4,null,{"$f":"0.0102/48.2426","v":2.1143139051377829E-4},null,null,null,{"$f":"CHOOSE(C$115,E150,G150,I150)","v":8.045268041513582E-4},null,"B_Olie_107_anv",null,null,9.35,11,9.35,0.19381210797096343]
[108,null,15.5,"Acenaphthen (C12)",2.4135804124540751E-4,null,{"$f":"0.00102/48.2426","v":2.1143139051377828E-5},null,null,null,{"$f":"CHOOSE(C$115,E151,G151,I151)","v":2.4135804124540751E-4},null,"B_Olie_108_anv",null,null,21.25,25,21.25,0.44048206357037145]
["109A",null,null,">12 - 16, aromater,øvrige",0,null,{"$f":"3.18/48.2426","v":6.5916845277824987E-2},null,null,null,{"$f":"CHOOSE(C$115,E152,G152,I152)","v":0},null,"B_Olie_109A_anv",null,null,1.0200000000000001E-2,1.2E-2,1.0200000000000001E-2,2.1143139051377831E-4]
["109B",null,null,">12 - 16, aromater,øvrige",2.0113170103783957E-2,null,0,null,null,null,{"$f":"CHOOSE(C$115,E153,G153,I153)","v":2.0113170103783957E-2},null,"B_Olie_109B_anv",null,null,1.0200000000000001E-3,1.1999999999999999E-3,1.0199999999999999E-3,2.1143139051377828E-5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.18,3.74,3.1790000000000003,6.5896116710127572E-2]
[1520,">C15 - C20",null,null,{"$f":"110*0.21441/228.7009","v":0.10312639784102291},null,{"$f":"33.3574/223","v":0.14958475336322868},null,null,null,{"$f":"CHOOSE(C$115,E155,G155,I155)","v":0.10312639784102291},null,"B_Olie_1520_anv",null,null,{"$f":"SUM(P148:P154)","v":48.247019999999992},{"$f":"SUM(Q148:Q154)","v":56.756},{"$f":"SUM(R148:R154)","v":48.242599999999996},1]
["151A",">16 - 21, alifater",null,">16 - 21, alifater, Tung Olie",0,null,{"$f":"33.15/33.3574","v":0.993782489042911},null,null,null,{"$f":"CHOOSE(C$115,E156,G156,I156)","v":0},null,"B_Olie_151A_anv"]
["151B",null,null,">16 - 21, alifater, Olieblandinger",0.97943192948090119,null,0,null,null,null,{"$f":"CHOOSE(C$115,E157,G157,I157)","v":0.97943192948090119},null,"B_Olie_151B_anv",null,null,33.15,39,{"$f":"P$166*Q157/100","v":33.15},{"$f":"R157/R$164","v":0.993782489042911}]
[152,">16 - 21, aromater",null,"Sum >16 - 21 aromater",null,null,null,null,null,null,null,null,null,null,null,3.3999999999999998E-3,4.0000000000000001E-3,3.4000000000000002E-3,1.0192640913260627E-4]
[153,null,16.55,"Fluoren (C13)",2.938295788442704E-3,null,{"$f":"0.0034/33.3574","v":1.0192640913260625E-4},null,null,null,{"$f":"CHOOSE(C$115,E159,G159,I159)","v":2.938295788442704E-3},null,"B_Olie_153_anv",null,null,6.8000000000000005E-2,0.08,6.8000000000000005E-2,2.0385281826521256E-3]
[154,null,19.36,"Phenanthren (C14)",4.8971596474045058E-3,null,{"$f":"0.068/33.3574","v":2.0385281826521256E-3},null,null,null,{"$f":"CHOOSE(C$115,E160,G160,I160)","v":4.8971596474045058E-3},null,"B_Olie_154_anv",null,null,6.8000000000000005E-2,0.08,6.8000000000000005E-2,2.0385281826521256E-3]
[155,null,19.43,"Anthracen (C14)",2.938295788442704E-3,null,{"$f":"0.068/33.3574","v":2.0385281826521256E-3},null,null,null,{"$f":"CHOOSE(C$115,E161,G161,I161)","v":2.938295788442704E-3},null,"B_Olie_155_anv",null,null,1.7000000000000001E-2,0.02,1.7000000000000001E-2,5.096320456630314E-4]
[156,null,21.85,"Fluoranthen (C16)",4.8971596474045058E-3,null,{"$f":"0.017/33.3574","v":5.096320456630314E-4},null,null,null,{"$f":"CHOOSE(C$115,E162,G162,I162)","v":4.8971596474045058E-3},null,"B_Olie_156_anv",null,null,5.0999999999999997E-2,0.06,5.0999999999999997E-2,1.5288961369890938E-3]
[157,null,20.8,"Pyren (C16)",4.8971596474045058E-3,null,{"$f":"0.051/33.3574","v":1.5288961369890938E-3},null,null,null,{"$f":"CHOOSE(C$115,E163,G163,I163)","v":4.8971596474045058E-3},null,"B_Olie_157_anv",null,null,3.4,4,3.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(P157:P162)","v":33.357399999999998},{"$f":"SUM(Q157:Q163)","v":43.244},{"$f":"SUM(R157:R162)","v":33.357399999999998},{"$f":"R164/R$164","v":1}]
[2025,">C20 - C25",null,null,{"$f":"110*0.04/228.7009","v":1.9239102251018689E-2},null,{"$f":"3.4/223","v":1.5246636771300448E-2},null,null,null,{"$f":"CHOOSE(C$115,E165,G165,I165)","v":1.9239102251018689E-2},null,"B_Olie_2025_anv",null,null,{"$f":"P155+P164","v":81.60441999999999},{"$f":"Q155+Q164","v":100},{"$f":"R155+R164","v":81.599999999999994}]
["201A",">21 - 25, alifater",25,">21 - 25, alifater, Tung olie",0,null,1,null,null,null,{"$f":"CHOOSE(C$115,E166,G166,I166)","v":0},null,"B_Olie_201A_anv",null,null,85,null,85]
["201B",null,25,">21 - 25, alifater, Olieblandinger",1,null,0,null,null,null,{"$f":"CHOOSE(C$115,E167,G167,I167)","v":1},null,"B_Olie_201B_anv"]
[202,">21 - 25, aromater",null,"Ingen repræsentanter"]
[]
[2535,">C25 - C35",null,null,{"$f":"10/228.7009","v":4.3725232388678842E-2},null,{"$f":"130/223","v":0.5829596412556054},null,null,null,{"$f":"CHOOSE($C$115,E170,G170,I170)","v":4.3725232388678842E-2},null,"B_Olie_2535_anv"]
["251A",">25 - 35, alifater",null,">25 - 35, alifater, Tung olie",null,null,{"$f":"117/195","v":0.6},null,null,null,{"$f":"CHOOSE(C$115,E171,G171,I171)","v":0},null,"B_Olie_251A_anv",null,null,76,null,null,{"$f":"P171/P179","v":0.58461538461538465}]
["251B",null,null,">25 - 35, alifater, Olieblandinger",0.9,null,null,null,null,null,{"$f":"CHOOSE(C$115,E172,G172,I172)","v":0.9},null,"B_Olie_251B_anv",null,null,0.15]
[252,">25 - 35, aromater",null,"Sum >25 - 35 aromater",null,null,null,null,null,null,null,null,null,null,null,0.4]
[253,null,26.37,"Benzo(a)anthracen (C18)",null,0.1,null,0.15,null,0.1,null,{"$f":"CHOOSE(C$115,F174,H174,J174)","v":0.1},"B_Olie_253_fastdel_anv",null,null,0.5]
[254,null,27.41,"Chrysen (C18)",null,0.15,null,0.4,null,0.15,null,0.15,"B_Olie_254_fastdel_anv",null,null,0.5]
[255,null,30.14,"Benzo(b)fluoranthen (C20)",null,0.3,null,0.5,null,0.3,null,0.3,"B_Olie_255_fastdel_anv",null,null,0.05]
[256,null,31.34,"Benzo(a)pyren",null,0.15,null,0.5,null,0.15,null,0.15,"B_Olie_256_fastdel_anv",null,null,0.4]
[257,null,33.92,"Dibenz(a,h)anthracen (C22)",null,0.01,null,0.05,null,0.01,null,0.01,"B_Olie_257_fastdel_anv",null,null,52,null,null,{"$f":"P178/P179","v":0.4}]
[258,null,34.01,"Benzo(ghi)perylen (C22)",null,0.15,null,0.4,null,0.15,null,0.15,"B_Olie_258_fastdel_anv",null,null,{"$f":"SUM(P171:P178)","v":130}]
["259A",null,null,">25 - 35, aromater, øvrige, Tung olie",null,null,0.4,null,null,null,{"$f":"CHOOSE(C$115,E180,G180,I180)","v":0},null,"B_Olie_259A_anv"]
["259B",null,null,">25 - 35, aromater, øvrige, Olieblandinger",0.1,null,null,null,null,null,{"$f":"CHOOSE(C$115,E181,G181,I181)","v":0.1},null,"B_Olie_259B_anv"]
[]
[3540,">C35",null,null,{"$f":"5/238.1009","v":2.0999500631874973E-2},null,{"$f":"65/223","v":0.2914798206278027},null,null,null,{"$f":"CHOOSE($C$115,E183,G183,I183)","v":2.0999500631874973E-2},null,"B_Olie_350_anv"]
[351,">35 - 44, alifater",35,"Pentatriacontan (C35)",0.84,null,0.84,null,null,null,{"$f":"CHOOSE(C$115,E184,G184,I184)","v":0.84},null,"B_Olie_351_anv"]
[352,">35 - 44, aromater",35.01,"Indeno(1,2,3-cd)pyren (C22)",0.16,null,0.16,null,null,null,{"$f":"CHOOSE(C$115,E185,G185,I185)","v":0.16},null,"B_Olie_352_anv"]
[]
[null,"NSO-forbindelser"]
[10,null,11.7,"Benzo(b)thiophen",null,0.02,null,0.02,null,0.02,null,{"$f":"CHOOSE(C$115,F188,H188,J188)","v":0.02},"B_Olie_10_fastandel_anv"]
[11,null,15.21,"Dibenzofuran",null,0,null,0.04,null,0.04,null,0,"B_Olie_11_fastandel_anv"]
[12,null,17.96,"Dibenzothiophen",null,5.0000000000000001E-3,null,5.0000000000000001E-3,null,5.0000000000000001E-3,null,5.0000000000000001E-3,"B_Olie_12_fastandel_anv"]
[13,null,18.82,"Acridin",null,0,null,0.02,null,0.02,null,0,"B_Olie_13_fastandel_anv"]
[14,null,19.39,"Carbazol",null,0.01,null,0.01,null,0.01,null,0.01,"B_Olie_14_fastandel_anv"]
[15,null,null,"Anilin",null,1E-4,null,1E-4,null,1E-4,null,1E-4,"B_Olie_15_fastandel_anv"]
[16,null,null,"Dimethyldisulfid",null,5.0000000000000001E-3,null,5.0000000000000001E-3,null,5.0000000000000001E-3,null,5.0000000000000001E-3,"B_Olie_16_fastandel_anv"]
[null,null,null,null,{"$f":"E170+E165+E155+E141+E126","v":1},null,{"$f":"G170+G165+G155+G141+G126","v":1.0000000000000002}]

{"sheet":"Udskrift_Oliestoffer","index":35,"n_rows":81,"n_cols":11,"rows_kept":81,"cut":false,"hidden":true,"merged":[[5,1,5,10],[57,7,57,9],[58,7,58,9],[58,1,58,4],[57,1,57,4],[10,2,10,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[2,8,2,10],[3,8,3,10],[4,8,4,10],[2,1,2,5],[3,1,3,5],[4,1,4,5],[25,13,25,15],[19,8,19,10],[20,8,20,10],[14,2,14,3],[14,4,14,5],[15,2,15,3],[15,4,15,5],[16,2,16,3],[16,4,16,5],[64,1,77,9],[79,1,92,9],[9,2,9,5],[10,4,10,5],[11,2,11,3],[11,4,11,5],[12,2,12,3],[19,2,19,3],[19,4,19,5],[19,6,19,7],[20,2,20,3],[20,4,20,5],[20,6,20,7],[22,1,22,4],[22,5,22,7],[22,8,22,10]]}
["Oliestoffer - fugacitetsberegninger"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
[]
["Jord"]
["Kommentar",{"$f":"IF(D_Olie_Jord_ComUds,\"Ja\",\"Nej\")","v":"Nej"},"Standard data",null,"Indtastede data (angives med fed)"]
["Jordtype",null,{"$f":"IF(D_Olie_jordtype=0,\"\",D_Olie_jordtype)","v":""}]
["Poreluftvolumen","VL",{"$f":"IF(ISNUMBER(D_Olie_VL_sys),D_Olie_VL_sys,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Olie_My_VL),Olie_My_VL,\"\")","v":""}]
["Vand-indhold","VV",{"$f":"IF(ISNUMBER(D_Olie_VV_sys),D_Olie_VV_sys,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Olie_My_VV),Olie_My_VV,\"\")","v":""}]
["Samlet porøsitet","e=VL+VV",{"$f":"IF(ISNUMBER(B_Olie_e),B_Olie_e,\"\")","v":0}]
["Volumen af jordskellet","VJ",{"$f":"D_Olie_VJ","v":1}]
["Kornrumvægt","d",{"$f":"IF(ISNUMBER(D_Olie_d_sys),D_Olie_d_sys,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Olie_My_d),Olie_My_d,\"\")","v":""}]
["Volumenvægt","r",{"$f":"IF(ISNUMBER(D_Olie_p),D_Olie_p,\"\")","v":0}]
["Indhold af organisk kulstof","foc",{"$f":"IF(ISNUMBER(D_Olie_foc_sys),D_Olie_foc_sys,\"\")","v":""},null,{"$f":"IF(ISNUMBER(Olie_My_foc),Olie_My_foc,\"\")","v":""}]
[]
["Beregning: Fugacitet"]
["Kommentar",{"$f":"IF(D_Olie_Kem_ComUds,\"Ja\",\"Nej\")","v":"Nej"},"Målepunkt",null,"Dato",null,"Fri fase?",null,"Anvendt brugerdata"]
[null,null,{"$f":"D_olie_målepunkt","v":""},null,{"$f":"D_olie_dato","v":""},null,{"$f":"Olie_frifase","v":"Nej"},null,{"$f":"D_Olie_bruger","v":"Nej"}]
["Angiv signifikant ciffer",2]
[null,"Jordkoncentrationer",null,null,null,"Vandkoncentrationer",null,null,"Poreluft konc."]
[null,"Indtastede værdier","Beregnet ud fra profil","Jordkvalitets-kriterium","Overskridelse \naf kriteriet","Beregnet ud fra fugacitet","Grundvands-\nkriteriet","Overskridelse \naf kriteriet","Beregnet ud fra fugacitet","Afdampnings-kriteriet","Overskridelse \naf kriteriet"]
[null,"mg/kg","mg/kg","mg/kg","gange","µg/l","µg/l","gange","mg/m³","mg/m³","gange"]
["BTEX'er"]
["Benzen",{"$f":"IF(Olie_52=\"\",\"\",Olie_52)","v":""},{"$f":"D_Olie_52a","v":0},{"$f":"IF(D_Olie_52_jkk=\"\",\"\",D_Olie_52_jkk)","v":1.5},{"$f":"IF(ISNUMBER(D_Olie_52_jkk_overskr),(ROUND(D_Olie_52_jkk_overskr,3-(INT(LOG(D_Olie_52_jkk_overskr))+1))),D_Olie_52_jkk_overskr)","v":"Nej"},{"$f":"IF(D_Olie_52_cv=0,0,(IF(ISNUMBER(D_Olie_52_cv),(ROUND(D_Olie_52_cv,olie_ciffer-(INT(LOG(D_Olie_52_cv))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_52_gkk","v":1},{"$f":"IF(ISNUMBER(D_Olie_52_gkk_overskr),(ROUND(D_Olie_52_gkk_overskr,3-(INT(LOG(D_Olie_52_gkk_overskr))+1))),D_Olie_52_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_52_cl=0,0,(IF(ISNUMBER(D_Olie_52_cl),(ROUND(D_Olie_52_cl,olie_ciffer-(INT(LOG(D_Olie_52_cl))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_52_ak),(ROUND(D_Olie_52_ak,3-(INT(LOG(D_Olie_52_ak))+1))),\"\")","v":1.2999999999999999E-4},{"$f":"IF(ISNUMBER(D_Olie_52_ak_overskr),(ROUND(D_Olie_52_ak_overskr,3-(INT(LOG(D_Olie_52_ak_overskr))+1))),D_Olie_52_ak_overskr)","v":{"$error":"#DIV/0!"}}]
["Toluen",{"$f":"IF(Olie_54=\"\",\"\",Olie_54)","v":""},{"$f":"D_Olie_54a","v":0},null,null,{"$f":"IF(D_Olie_54_cv=0,0,(IF(ISNUMBER(D_Olie_54_cv),(ROUND(D_Olie_54_cv,olie_ciffer-(INT(LOG(D_Olie_54_cv))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_57_gkk","v":5},{"$f":"IF(ISNUMBER(D_Olie_54_gkk_overskr),(ROUND(D_Olie_54_gkk_overskr,3-(INT(LOG(D_Olie_54_gkk_overskr))+1))),D_Olie_54_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_54_cl=0,0,(IF(ISNUMBER(D_Olie_54_cl),(ROUND(D_Olie_54_cl,olie_ciffer-(INT(LOG(D_Olie_54_cl))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_54_ak),(ROUND(D_Olie_54_ak,3-(INT(LOG(D_Olie_54_ak))+1))),\"\")","v":0.4},{"$f":"IF(ISNUMBER(D_Olie_54_ak_overskr),(ROUND(D_Olie_54_ak_overskr,3-(INT(LOG(D_Olie_54_ak_overskr))+1))),D_Olie_54_ak_overskr)","v":{"$error":"#DIV/0!"}}]
["Ethylbenzen",{"$f":"IF(Olie_58=\"\",\"\",Olie_58)","v":""},{"$f":"D_Olie_58a","v":0},null,null,{"$f":"IF(D_Olie_58_cv=0,0,(IF(ISNUMBER(D_Olie_58_cv),(ROUND(D_Olie_58_cv,olie_ciffer-(INT(LOG(D_Olie_58_cv))+1))),\"\")))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IF(D_Olie_58_cl=0,0,(IF(ISNUMBER(D_Olie_58_cl),(ROUND(D_Olie_58_cl,olie_ciffer-(INT(LOG(D_Olie_58_cl))+1))),\"\")))","v":{"$error":"#DIV/0!"}}]
["Sum Xylener",{"$f":"IF(Olie_57=\"\",IF(Olie_571+Olie_572>0,Olie_571+Olie_572,\"\"),Olie_57)","v":""},{"$f":"D_Olie_57a","v":0},null,null,{"$f":"IF(D_Olie_57_cv=0,0,(IF(ISNUMBER(D_Olie_57_cv),(ROUND(D_Olie_57_cv,olie_ciffer-(INT(LOG(D_Olie_57_cv))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_57_gkk","v":5},{"$f":"IF(ISNUMBER(D_Olie_57_gkk_overskr),(ROUND(D_Olie_57_gkk_overskr,3-(INT(LOG(D_Olie_57_gkk_overskr))+1))),D_Olie_57_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_57_cl=0,0,(IF(ISNUMBER(D_Olie_57_cl),(ROUND(D_Olie_57_cl,olie_ciffer-(INT(LOG(D_Olie_57_cl))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_57_ak),(ROUND(D_Olie_57_ak,3-(INT(LOG(D_Olie_57_ak))+1))),\"\")","v":0.1},{"$f":"IF(ISNUMBER(D_Olie_57_ak_overskr),(ROUND(D_Olie_57_ak_overskr,3-(INT(LOG(D_Olie_57_ak_overskr))+1))),D_Olie_57_ak_overskr)","v":{"$error":"#DIV/0!"}}]
["Naphtalen",{"$f":"IF(Olie_103=\"\",\"\",Olie_103)","v":""},{"$f":"D_Olie_103a","v":0},null,null,{"$f":"IF(D_Olie_103_cv=0,0,(IF(ISNUMBER(D_Olie_103_cv),(ROUND(D_Olie_103_cv,olie_ciffer-(INT(LOG(D_Olie_103_cv))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_103_gkk","v":1},{"$f":"IF(ISNUMBER(D_Olie_103_gkk_overskr),(ROUND(D_Olie_103_gkk_overskr,3-(INT(LOG(D_Olie_103_gkk_overskr))+1))),D_Olie_103_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_103_cl=0,0,(IF(ISNUMBER(D_Olie_103_cl),(ROUND(D_Olie_103_cl,olie_ciffer-(INT(LOG(D_Olie_103_cl))+1))),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_103_ak),(ROUND(D_Olie_103_ak,3-(INT(LOG(D_Olie_103_ak))+1))),\"\")","v":0.04},{"$f":"IF(ISNUMBER(D_Olie_103_ak_overskr),(ROUND(D_Olie_103_ak_overskr,3-(INT(LOG(D_Olie_103_ak_overskr))+1))),D_Olie_103_ak_overskr)","v":{"$error":"#DIV/0!"}}]
[]
["Kulbrintefraktioner"]
["C6-C10 ",{"$f":"IF(Olie_510=\"\",\"\",Olie_510)","v":""},{"$f":"D_Olie_510a","v":0},{"$f":"IF(D_Olie_510_jkk=\"\",\"\",D_Olie_510_jkk)","v":25},{"$f":"IF(ISNUMBER(D_Olie_510_jkk_overskr),(ROUND(D_Olie_510_jkk_overskr,3-(INT(LOG(D_Olie_510_jkk_overskr))+1))),D_Olie_510_jkk_overskr)","v":"Nej"},{"$f":"IF(ISNUMBER(D_Olie_510_cv),(ROUND(D_Olie_510_cv,olie_ciffer-(INT(LOG(D_Olie_510_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_510_cl),(ROUND(D_Olie_510_cl,olie_ciffer-(INT(LOG(D_Olie_510_cl))+1))),\"\")","v":""}]
["C10-C15 ",{"$f":"IF(Olie_1015=\"\",\"\",Olie_1015)","v":""},{"$f":"D_Olie_1015a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_1015_cv),(ROUND(D_Olie_1015_cv,olie_ciffer-(INT(LOG(D_Olie_1015_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_1015_cl),(ROUND(D_Olie_1015_cl,olie_ciffer-(INT(LOG(D_Olie_1015_cl))+1))),\"\")","v":""}]
["C15-C20 ",{"$f":"IF(Olie_1520=\"\",\"\",Olie_1520)","v":""},{"$f":"D_Olie_1520a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_1520_cv),(ROUND(D_Olie_1520_cv,olie_ciffer-(INT(LOG(D_Olie_1520_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_1520_cl),(ROUND(D_Olie_1520_cl,olie_ciffer-(INT(LOG(D_Olie_1520_cl))+1))),\"\")","v":""}]
["C20-C35",{"$f":"IF(Olie_2040=\"\",\"\",Olie_2040)","v":""},{"$f":"D_Olie_2040a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_2040_cv),(ROUND(D_Olie_2040_cv,olie_ciffer-(INT(LOG(D_Olie_2040_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_2040_cl),(ROUND(D_Olie_2040_cl,olie_ciffer-(INT(LOG(D_Olie_2040_cl))+1))),\"\")","v":""}]
["Sum af kulbrinter",{"$f":"IF(Olie_1=\"\",\"\",Olie_1)","v":""},{"$f":"D_Olie_1a","v":0},{"$f":"IF(D_Olie_1_jkk=\"\",\"\",D_Olie_1_jkk)","v":100},{"$f":"IF(ISNUMBER(D_Olie_1_jkk_overskr),(ROUND(D_Olie_1_jkk_overskr,3-(INT(LOG(D_Olie_1_jkk_overskr))+1))),D_Olie_1_jkk_overskr)","v":"Nej"},{"$f":"IF(ISNUMBER(D_Olie_1_cv),(ROUND(D_Olie_1_cv,olie_ciffer-(INT(LOG(D_Olie_1_cv))+1))),\"\")","v":""},{"$f":"D_Olie_1_gkk","v":9},{"$f":"IF(ISNUMBER(D_Olie_1_gkk_overskr),(ROUND(D_Olie_1_gkk_overskr,3-(INT(LOG(D_Olie_1_gkk_overskr))+1))),D_Olie_1_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_1_cl),(ROUND(D_Olie_1_cl,olie_ciffer-(INT(LOG(D_Olie_1_cl))+1))),\"\")","v":""},{"$f":"IF(ISNUMBER(D_Olie_1_ak),(ROUND(D_Olie_1_ak,3-(INT(LOG(D_Olie_1_ak))+1))),\"\")","v":0.1},{"$f":"IF(ISNUMBER(D_Olie_1_ak_overskr),(ROUND(D_Olie_1_ak_overskr,3-(INT(LOG(D_Olie_1_ak_overskr))+1))),D_Olie_1_ak_overskr)","v":{"$error":"#DIV/0!"}}]
[]
["Alkylbenzener"]
["C9-C10 aromatiske kulbrinter",null,null,null,null,{"$f":"IF(ISNUMBER(D_olie_910_cv),(ROUND(D_olie_910_cv,olie_ciffer-(INT(LOG(D_olie_910_cv))+1))),\"\")","v":""},{"$f":"D_Olie_60_gkk","v":1},{"$f":"IF(ISNUMBER(D_Olie_60_gkk_overskr),(ROUND(D_Olie_60_gkk_overskr,3-(INT(LOG(D_Olie_60_gkk_overskr))+1))),D_Olie_60_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_910_cl),(ROUND(D_Olie_910_cl,olie_ciffer-(INT(LOG(D_Olie_910_cl))+1))),\"\")","v":""},{"$f":"IF(ISNUMBER(D_Olie_60_ak),(ROUND(D_Olie_60_ak,3-(INT(LOG(D_Olie_60_ak))+1))),\"\")","v":0.03},{"$f":"IF(ISNUMBER(D_Olie_60_ak_overskr),(ROUND(D_Olie_60_ak_overskr,3-(INT(LOG(D_Olie_60_ak_overskr))+1))),D_Olie_60_ak_overskr)","v":{"$error":"#DIV/0!"}}]
[]
["Polyaromatiske Kulbrinter (PAH)"]
["Benzo(a)pyren",{"$f":"IF(Olie_256=\"\",\"\",Olie_256)","v":""},{"$f":"D_Olie_256a","v":0},{"$f":"IF(D_Olie_256_jkk=\"\",\"\",D_Olie_256_jkk)","v":0.3},{"$f":"IF(ISNUMBER(D_Olie_256_jkk_overskr),(ROUND(D_Olie_256_jkk_overskr,3-(INT(LOG(D_Olie_256_jkk_overskr))+1))),D_Olie_256_jkk_overskr)","v":"Nej"},{"$f":"IF(ISNUMBER(D_Olie_256_cv),(ROUND(D_Olie_256_cv,olie_ciffer-(INT(LOG(D_Olie_256_cv))+1))),\"\")","v":""},{"$f":"D_Olie_256_gkk","v":0.01},{"$f":"IF(ISNUMBER(D_Olie_256_gkk_overskr),(ROUND(D_Olie_256_gkk_overskr,3-(INT(LOG(D_Olie_256_gkk_overskr))+1))),D_Olie_256_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_256_cl),(ROUND(D_Olie_256_cl,olie_ciffer-(INT(LOG(D_Olie_256_cl))+1))),\"\")","v":""}]
["benzo(b+j+k)fluoranthen",{"$f":"IF(Olie_255=\"\",\"\",Olie_255)","v":""},{"$f":"D_Olie_255a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_255_cv),(ROUND(D_Olie_255_cv,olie_ciffer-(INT(LOG(D_Olie_255_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_255_cl),(ROUND(D_Olie_255_cl,olie_ciffer-(INT(LOG(D_Olie_255_cl))+1))),\"\")","v":""}]
["benzo(ghi)perylen",{"$f":"IF(Olie_258=\"\",\"\",Olie_258)","v":""},{"$f":"D_Olie_258a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_258_cv),(ROUND(D_Olie_258_cv,olie_ciffer-(INT(LOG(D_Olie_258_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_258_cl),(ROUND(D_Olie_258_cl,olie_ciffer-(INT(LOG(D_Olie_258_cl))+1))),\"\")","v":""}]
["Dibenz(a,h)anthracen",{"$f":"IF(Olie_257=\"\",\"\",Olie_257)","v":""},{"$f":"D_Olie_257a","v":0},{"$f":"IF(D_Olie_257_jkk=\"\",\"\",D_Olie_257_jkk)","v":0.3},{"$f":"IF(ISNUMBER(D_Olie_257_jkk_overskr),(ROUND(D_Olie_257_jkk_overskr,3-(INT(LOG(D_Olie_257_jkk_overskr))+1))),D_Olie_257_jkk_overskr)","v":"Nej"},{"$f":"IF(ISNUMBER(D_Olie_257_cv),(ROUND(D_Olie_257_cv,olie_ciffer-(INT(LOG(D_Olie_257_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_257_cl),(ROUND(D_Olie_257_cl,olie_ciffer-(INT(LOG(D_Olie_257_cl))+1))),\"\")","v":""}]
["Fluoranthen",{"$f":"IF(Olie_156=\"\",\"\",Olie_156)","v":""},{"$f":"D_Olie_156a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_156_cv),(ROUND(D_Olie_156_cv,olie_ciffer-(INT(LOG(D_Olie_156_cv))+1))),\"\")","v":""},{"$f":"D_Olie_156_gkk","v":0.1},{"$f":"IF(ISNUMBER(D_Olie_156_gkk_overskr),(ROUND(D_Olie_156_gkk_overskr,3-(INT(LOG(D_Olie_156_gkk_overskr))+1))),D_Olie_156_gkk_overskr)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Olie_156_cl),(ROUND(D_Olie_156_cl,olie_ciffer-(INT(LOG(D_Olie_156_cl))+1))),\"\")","v":""}]
["indeno(1,2,3-cd)pyren",{"$f":"IF(Olie_352=\"\",\"\",Olie_352)","v":""},{"$f":"D_Olie_352a","v":0},null,null,{"$f":"IF(ISNUMBER(D_Olie_352_cv),(ROUND(D_Olie_352_cv,olie_ciffer-(INT(LOG(D_Olie_352_cv))+1))),\"\")","v":""},null,null,{"$f":"IF(ISNUMBER(D_Olie_352_cl),(ROUND(D_Olie_352_cl,olie_ciffer-(INT(LOG(D_Olie_352_cl))+1))),\"\")","v":""}]
["Sum af 7 PAH'er jord",null,{"$f":"D_Olie_20a","v":0},{"$f":"IF(D_Olie_20_jkk=\"\",\"\",D_Olie_20_jkk)","v":4},{"$f":"IF(ISNUMBER(D_Olie_20_jkk_overskr),(ROUND(D_Olie_20_jkk_overskr,3-(INT(LOG(D_Olie_20_jkk_overskr))+1))),D_Olie_20_jkk_overskr)","v":"Nej"}]
["Sum af 4 PAH`er",null,null,null,null,{"$f":"IF(ISNUMBER(D_Olie_21_cv),(ROUND(D_Olie_21_cv,olie_ciffer-(INT(LOG(D_Olie_21_cv))+1))),\"\")","v":""},{"$f":"D_Olie_21_gkk","v":0.1},{"$f":"IF(ISNUMBER(D_Olie_21_gkk_overskr),(ROUND(D_Olie_21_gkk_overskr,3-(INT(LOG(D_Olie_21_gkk_overskr))+1))),D_Olie_21_gkk_overskr)","v":{"$error":"#DIV/0!"}}]
[]
["NSO-forbindelser"]
["Sum af NSO-forbindelser",{"$f":"D_olie_10+D_olie_11+D_olie_12+D_olie_13+D_olie_14+D_olie_15+D_olie_16","v":0},{"$f":"D_Olie_10a+D_Olie_11a+D_Olie_12a+D_Olie_13a+D_Olie_14a+D_Olie_15a+D_Olie_16a","v":4.0100000000000004E-2},null,null,{"$f":"D_Olie_10_cv+D_Olie_11_cv+D_Olie_12_cv+D_Olie_13_cv+D_Olie_14_cv+D_Olie_15_cv+D_Olie_16_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Olie_10_cl+D_Olie_11_cl+D_Olie_12_cl+D_Olie_13_cl+D_Olie_14_cl+D_Olie_15_cl+D_Olie_16_cl","v":{"$error":"#DIV/0!"}}]
[]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_Olie_Jord_Com <> \"\", D_Olie_Jord_Com, \"\")","v":""}]
["om jordtypen"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Olie_Kem_Com <> \"\", D_Olie_Kem_Com, \"\")","v":""}]
["kemisk analyse"]

{"sheet":"Vejledning_Oliestoffer","index":36,"n_rows":113,"n_cols":5,"rows_kept":113,"cut":false,"hidden":true,"merged":[[10,1,15,2],[2,1,7,2],[18,1,20,2],[44,4,52,8],[54,4,55,8],[38,4,43,8],[34,4,37,8],[97,1,97,8],[98,1,98,8],[99,1,99,8],[22,1,27,8],[30,1,33,8],[57,4,59,8],[76,1,83,8],[84,1,84,8],[85,1,85,8],[86,1,95,8],[96,1,96,8],[61,1,63,7],[73,1,74,8],[75,1,75,8],[71,1,71,8],[66,1,70,8],[110,1,110,8],[111,1,111,8],[112,1,112,8],[113,1,113,8],[100,1,100,8],[101,1,102,8],[103,1,103,8],[104,1,104,8],[105,1,109,8]]}
[null,"Vejledning  -Oliestoffer"]
[null,"Formål"]
[null,"Der er to formål med arket oliestoffer. \nDet primære formål, er at foretage fugacitetsberegninger på olieblandinger. Arket beregner desuden de stofkoncentrationer, som risikoberegningerne (indeklima, grundvand m.v.) skal gennemføres med, "]
[]
[]
[]
[]
[]
[]
[null,"Fugacitetsberegninger"]
[null,"Modulet \"Oliestoffer\" adskiller sig på en række punkter sig fra modulet \"Enkeltstoffer\", dog mest markant ved, at fugacitetsberegningerne kun kan foretages med udgangspunkt i kendte jordkoncen-trationer, og ikke med udgangspunkt i grundvands- eller poreluftprøver."]
[]
[]
[]
[]
[]
[]
[null,"Jordtype:"]
[null,"For at fasefordelingen i jorden, porevandet og poreluften kan beregnes, skal der indtastes data om jordarten.\n"]
[]
[]
[]
[null,"Jordtypen kan vælges ved at klikke på knappen \"Jordtype\" og vælge en standardjordtype fra listen, hverved indlæses automatisk en række standardværdier for jordtypen. \n\nSåfremt man i beregningen ønsker at anvende andre værdier end standardværdierne kan de ønskede værdier indtastes i de hvide felter. Det er også muligt at anvende og oprette egne \"jordtyper\" ved at klikke på knappen \"Egen liste\". Se iøvrigt bemærkninger om anvendelse af valglister under afsnittet Generelt"]
[]
[]
[]
[]
[]
[]
[null,"Kemiske data:"]
[null,"De kemiske data er opdelt efter to olieprofiler, et profil for benzin/olieblandinger og et profil for tung olie. Hvert profil angiver en default procentvis fordeling af kulbrintefraktionerne. Hver kulbrintefraktion fordeles herudover på flere modelstoffer afhængig af olieprofilet. Enkelte af modelstofferne (BTEX'er og PAH'er) fremgår af brugergrænsefladen, men hovedparten af modelstofferne vil være gemt i de bagvedliggende data og beregningsark."]
[]
[]
[]
[null,null,null,null,"Fugacitetsberegningerne og de efterfølgende risikoberegninger foretages  for alle modelstofferne. Herefter summeres resultaterne i nye kulbrintefraktioner afhængigt af mediet og gældende grænseværdier."]
[]
[]
[]
[null,null,null,null,"Der er mulighed for at indtaste koncentrationer for de enkelte kulbrinte fraktioner. Indtastning af koncentrationer for en kulbrintefraktion vil påvirke den beregnede koncentration af de øvrige fraktioner, men ikke det totale kulbrinteindhold uanset om summen af de enkelte kulbrintefraktioner er større eller mindre end den indtastede værdi for total indholdet af kulbrinter."]
[]
[]
[]
[]
[]
[null,null,null,null,"For nogle af modelstofferne (BTEX'er og PAH'er) er det muligt at indtaste koncentrationer. Indtastning af koncentrationer for et modelstof vil påvirke den beregnede koncentration af de øvrige modelstoffer under den samme kulbrintefraktion, men ikke koncentrationen af modelstoffer for de øvrige kulbrintefraktioner.  Indtastning af koncentrationer for et modelstof vil heller ikke påvirke koncentrationen af kulbrintefraktionen uanset om summen af de enkelte modelstoffer er større eller mindre end værdien for kulbrintefraktionen."]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Kemidata overføres til de øvrige beregningsmoduler"]
[null,null,null,null,"Ved at klikke på de respektive knapper øverst til højre i skærmbilledet er det muligt at navigere til det ønskede beregningsmodul."]
[]
[]
[null,null,null,null,"Til hvert beregningsmodul overføres de koncentrationerne af modelstofferne, som udfra fugacitetsprincippet er beregnet for det aktuelle medie."]
[]
[]
[null,"Generelt"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under olie & benzin modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under olie & benzin modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikkke på den ønskede værdi\n· At vælge en forekomst ved at skreve dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiskestoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet.Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lysseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[null,"Sletning af enkeltværdier:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne incl. resultat af mellemberegninger"]

{"sheet":"Grundvand-Olie","index":37,"n_rows":115,"n_cols":37,"rows_kept":115,"cut":false,"hidden":true,"merged":[[67,16,67,17],[70,16,70,17],[72,16,72,17],[74,16,74,17],[53,10,54,12],[93,25,93,26],[57,25,57,26],[59,25,59,26],[61,25,61,26],[63,25,63,26],[65,25,65,26],[67,25,67,26],[70,25,70,26],[72,25,72,26],[74,25,74,26],[76,25,76,26],[78,25,78,26],[83,25,83,26],[87,25,87,26],[89,25,89,26],[91,25,91,26],[89,16,89,17],[87,16,87,17],[76,16,76,17],[78,16,78,17],[67,10,67,11],[89,7,89,8],[89,13,89,14],[89,19,89,20],[89,22,89,23],[63,13,63,14],[63,22,63,23],[65,19,65,20],[65,22,65,23],[78,7,78,8],[63,7,63,8],[63,19,63,20],[76,7,76,8],[76,13,76,14],[76,19,76,20],[76,22,76,23],[70,7,70,8],[70,13,70,14],[70,19,70,20],[70,22,70,23],[67,7,67,8],[65,16,65,17],[89,10,89,11],[63,16,63,17],[61,7,61,8],[61,13,61,14],[61,19,61,20],[61,22,61,23],[14,10,14,11],[19,13,19,14],[20,13,20,14],[19,7,19,11],[20,7,20,11],[27,10,27,11],[27,13,27,15],[27,16,27,18],[27,19,27,20],[17,13,17,14],[21,13,21,14],[16,7,16,11],[29,7,30,11],[29,16,29,17],[29,19,29,20],[29,22,29,23],[57,10,57,11],[59,10,59,11],[59,16,59,17],[61,16,61,17],[59,7,59,8],[59,13,59,14],[59,19,59,20],[59,22,59,23],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[10,7,10,29],[11,6,11,17],[11,20,11,29],[12,10,12,11],[29,25,29,26],[29,28,29,29],[39,7,39,8],[43,7,44,32],[46,7,46,11],[47,7,47,11],[33,28,33,29],[33,31,33,32],[57,16,57,17],[31,13,31,14],[31,31,31,32],[27,31,27,32],[27,34,27,35],[28,13,28,14],[28,16,28,17],[28,19,28,20],[28,22,28,23],[28,25,28,26],[28,28,28,29],[28,31,28,32],[28,34,28,35],[27,22,27,23],[27,25,27,26],[27,28,27,29],[32,34,32,35],[29,34,31,35],[30,16,30,17],[30,19,30,20],[30,22,30,23],[30,25,30,26],[30,28,30,29],[31,28,31,29],[35,0,36,4],[36,7,36,8],[31,7,31,11],[31,16,31,17],[31,19,31,20],[31,22,31,23],[31,25,31,26],[32,19,32,20],[32,22,32,23],[32,25,32,26],[32,28,32,29],[32,31,32,32],[33,7,33,8],[33,19,33,20],[33,22,33,23],[33,25,33,26],[38,0,40,2],[46,14,47,19],[57,7,57,8],[57,13,57,14],[57,19,57,20],[57,22,57,23],[49,14,51,19],[49,20,51,22],[49,23,51,24],[53,19,54,20],[56,19,56,20],[53,22,54,23],[55,10,55,11],[53,24,54,27],[49,7,49,11],[51,7,51,11],[53,7,54,8],[53,13,54,14],[55,7,55,8],[55,13,55,14],[55,19,55,20],[55,22,55,23],[56,7,56,8],[56,13,56,14],[33,34,33,35],[34,19,34,20],[34,22,34,23],[34,25,34,26],[34,28,34,29],[34,31,34,32],[34,34,34,35],[53,15,54,18],[55,15,55,18],[46,20,47,22],[46,23,47,24],[55,24,55,27],[36,20,36,22],[65,7,65,8],[65,13,65,14],[74,7,74,8],[74,13,74,14],[74,19,74,20],[74,22,74,23],[81,13,81,14],[81,19,81,20],[81,22,81,23],[78,13,78,14],[78,19,78,20],[78,22,78,23],[79,13,79,14],[79,19,79,20],[79,22,79,23],[72,7,72,8],[72,13,72,14],[67,22,67,23],[78,10,78,11],[67,19,67,20],[72,19,72,20],[72,22,72,23],[67,13,67,14],[65,10,65,11],[85,19,85,20],[85,22,85,23],[87,7,87,8],[87,13,87,14],[87,19,87,20],[87,22,87,23],[83,7,83,8],[83,13,83,14],[83,19,83,20],[83,22,83,23],[83,10,83,11],[87,10,87,11],[83,16,83,17],[85,13,85,14],[93,7,93,8],[93,13,93,14],[93,19,93,20],[93,22,93,23],[95,7,95,8],[95,13,95,14],[95,19,95,20],[95,22,95,23],[91,13,91,14],[91,19,91,20],[91,22,91,23],[91,7,91,8],[91,16,91,17],[93,16,93,17],[95,16,95,17],[104,16,104,17],[95,25,95,26],[97,7,97,8],[97,13,97,14],[97,19,97,20],[97,22,97,23],[100,7,100,8],[100,13,100,14],[100,19,100,20],[100,22,100,23],[97,10,97,11],[100,16,100,17],[97,16,97,17],[97,25,97,26],[100,25,100,26],[112,16,112,17],[102,25,102,26],[104,25,104,26],[108,7,108,8],[108,13,108,14],[108,19,108,20],[108,22,108,23],[106,13,106,14],[106,19,106,20],[106,22,106,23],[106,7,106,8],[106,16,106,17],[108,16,108,17],[106,25,106,26],[108,25,108,26],[102,7,102,8],[102,13,102,14],[102,19,102,20],[102,22,102,23],[104,7,104,8],[104,13,104,14],[104,19,104,20],[104,22,104,23],[102,16,102,17],[14,26,14,28],[9,7,9,15],[117,20,117,22],[110,25,110,26],[112,25,112,26],[116,23,116,25],[114,7,114,8],[114,13,114,14],[114,19,114,20],[114,22,114,23],[116,10,116,11],[116,13,116,14],[116,16,116,17],[114,16,114,17],[114,25,114,26],[110,7,110,8],[110,13,110,14],[110,19,110,20],[110,22,110,23],[112,7,112,8],[112,13,112,14],[112,19,112,20],[112,22,112,23],[110,16,110,17]]}
["Grundvandskoncentrationen i det først betydende magasin - oliestoffer"]
["Lokaliteten"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[]
["Det forurenede område"]
[]
["Længde af kildeområde",null,null,null,null,"Y",null,null,null,null,null,null,"m"]
[]
["Bredde af kildeområde",null,null,null,null,"X",null,null,null,null,null,null,"m",null,{"$f":"IF(ISTEXT(GruOlie_X),\"Tjek decimal\",\"\")","v":""},null,null,null,null,"Areal af det forurenede område ",null,null,null,null,null,null,{"$f":"D_GruOlie_A","v":""},null,null,"m2"]
[]
[null,null,null,null,null,null,null,"Kommune/Egn",null,null,null,null,null,"Nettonedbør"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"N"]
[]
[null,null,null,null,null,null,null,{"$f":"IF(D_GruOlie_Kommune_syst<>\"\",D_GruOlie_Kommune_syst,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_GruOlie_N_syst<>\"\",D_GruOlie_N_syst,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"mm/år"]
[]
[]
[]
["Det først betydende magasin",null,null,null,null,null,null,null,"Indtaste data for den første betydende magasin, hvori risiko skal beregnes"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Hydraulisk gradient\n(m/m)",null,null,"Hydraulisk lednings-\nevne",null,null,"Effektiv porøsitet",null,null,"Vand-mættede porøsitet",null,null,"Bulkmasse-fylde\n(kg/l)",null,null,"% Indhold organisk kulstof",null,null,"Tykkelse af magasin\n(m)",null,null,"Opblandings-dybde\n(m)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"i",null,null,"k",null,null,"eff.",null,null,"ew",null,null,"r",null,null,"foc",null,null,"maxdm",null,null,"dm"]
[null,null,null,null,null,null,null,{"$f":"IF(D_GruOlie_Aqui_syst<>\"\",D_GruOlie_Aqui_syst,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_GruOlie_trin1a_k_int<>\"\",D_GruOlie_trin1a_k_int,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_trin2a_eeff_int<>\"\",D_GruOlie_trin2a_eeff_int,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_trin3_eW_int<>\"\",D_GruOlie_trin3_eW_int,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_rhob_int<>\"\",D_GruOlie_rhob_int,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_foc_int<>\"\",D_GruOlie_foc_int,\"\")","v":""},null,null,null,null,null,{"$f":"D_GruOlie_trin2a_dm_2a","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_GruOlie_trin1a_k_syst<>\"\",D_GruOlie_trin1a_k_syst,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_trin2a_eeff_syst<>\"\",D_GruOlie_trin2a_eeff_syst,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_trin3_eW_syst<>\"\",D_GruOlie_trin3_eW_syst,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_rhob_syst<>\"\",D_GruOlie_rhob_syst,\"\")","v":""},null,null,{"$f":"IF(D_GruOlie_foc_syst<>\"\",D_GruOlie_foc_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(GruOlie_i),\"Tjek decimal\",IF(ISTEXT(GruOlie_my_k),\"Tjek decimal\",IF(ISTEXT(GruOlie_My_eff),\"Tjek decimal\",IF(ISTEXT(GruOlie_My_ew),\"Tjek decimal\",IF(ISTEXT(GruOlie_My_p),\"Tjek decimal\",IF(ISTEXT(GruOlie_My_foc),\"Tjek decimal\",IF(ISTEXT(GruOlie_Maxdm),\"Tjek decimal\",\"\")))))))","v":""}]
[]
["Gns. porevandhastighed",null,null,null,null,"Vp",null,{"$f":"D_GruOlie_trin2a_VP","v":{"$error":"#VALUE!"}},null,null,"m/år"]
[]
["Afstand til teoretisk beregningspunkt"]
[null,null,null,null,null,"L",null,{"$f":"D_GruOlie_trin1b_LL","v":{"$error":"#VALUE!"}},null,null,"m",null,null,"Brugerens beregningpunkt",null,null,null,null,null,null,null,null,null,null,"m"]
[]
["Transporttid til  \nberegningspktunkt"]
[null,null,null,null,null,"ttid",null,{"$f":"D_GruOlie_trin2a_t","v":{"$error":"#VALUE!"}},null,null,"år"]
[]
[]
[]
["Beregning: Grundvand",null,null,null,null,null,null,"Data for forurening er overført fra fugacitetsmodulet for oliestoffer "]
[]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"IF(Olie_målepunkt<>\"\",D_olie_målepunkt,\"\")","v":""},null,null,null,null,null,null,"Standard nedbrydningskonstant",null,null,null,null,null,0,null,null,"dage-1"]
["Dato",null,null,null,null,null,null,{"$f":"IF(Olie_dato<>\"\",D_olie_dato,\"\")","v":""}]
[]
["Fri fase?",null,null,null,null,null,null,{"$f":"D_Olie_FF","v":"Nej"},null,null,null,null,null,null,"Brugervalgt nedbrydnings\nkonstant (alle stoffer)",null,null,null,null,null,null,null,null,"dage-1"]
[]
["Anvendt Brugerdata?",null,null,null,null,null,null,{"$f":"D_gruolie_bruger","v":"Nej"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Gruolie_My_ned),\"Tjek decimal\",\"\")","v":""}]
[]
[null,null,null,null,null,null,null,"Porevands-konc\nkonc.",null,null,"Grundvands-\nkriteriet",null,null,"Trin 1\n C1",null,"Overskridelse \naf kriteriet",null,null,null,"Trin 2\n C2",null,null,"Trin 3\n C3",null,"Overskridelse \naf kriteriet"]
[]
[null,null,null,null,null,null,null,"µg/l",null,null,"µg/l",null,null,"µg/l",null,"Gange",null,null,null,"µg/l",null,null,"µg/l",null,"Gange"]
["BTEX'er"]
[null,"Benzen",null,null,null,null,null,{"$f":"D_Gruolie_cv_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_GVK_52","v":1},null,null,{"$f":"D_Gruolie_c1_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_overskr1_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c2_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_overskr_52","v":{"$error":"#DIV/0!"}}]
[]
[null,"Toluen",null,null,null,null,null,{"$f":"D_gruolie_cv_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_gvk_54","v":5},null,null,{"$f":"D_gruolie_c1_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr1_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c2_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr_54","v":{"$error":"#DIV/0!"}}]
[]
[null,"Ethylbenzen",null,null,null,null,null,{"$f":"D_gruolie_cv_58","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_58","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_58","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum Xylener",null,null,null,null,null,{"$f":"D_gruolie_cv_57","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_57","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_57","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_57","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum Xylener + ethylbenzen",null,null,null,null,null,{"$f":"D_GruOlie_cv_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_gvk_57","v":5},null,null,{"$f":"D_Gruolie_c1_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr1_57","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_c2_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_C3_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr_57","v":{"$error":"#DIV/0!"}}]
[]
[null,"Naphthalen",null,null,null,null,null,{"$f":"D_gruolie_cv_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_gvk_103","v":1},null,null,{"$f":"D_gruolie_c1_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr1_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c2_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr_103","v":{"$error":"#DIV/0!"}}]
[]
["Kulbrintefraktioner"]
[null,"C6-C10",null,null,null,null,null,{"$f":"D_gruolie_cv_510","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_510","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_510","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_510","v":{"$error":"#DIV/0!"}}]
[]
[null,"C10-C15",null,null,null,null,null,{"$f":"D_gruolie_cv_1015","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_1015","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_1015","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_1015","v":{"$error":"#DIV/0!"}}]
[]
[null,"C15-C20",null,null,null,null,null,{"$f":"D_gruolie_cv_1520","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_1520","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_1520","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_1520","v":{"$error":"#DIV/0!"}}]
[]
[null,"C20-C35",null,null,null,null,null,{"$f":"D_gruolie_cv_2040","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_2040","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_2040","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_2040","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af kulbrinter",null,null,null,null,null,{"$f":"D_Gruolie_cv_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_gvk_1","v":9},null,null,{"$f":"D_Gruolie_c1_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_overskr1_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c2_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_overskr_1","v":{"$error":"#DIV/0!"}}]
[]
[]
["Alkylbenzener, aromatiske kulbrinter "]
[]
[null,"C9-C10 aromatiske kulbrinter",null,null,null,null,null,{"$f":"D_Gruolie_cv_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_gvk_60","v":1},null,null,{"$f":"D_GruOlie_C1_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_overskr1_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_C2_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_C3_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_overskr_910","v":{"$error":"#DIV/0!"}}]
[]
["Polyaromatiske Kulbrinter (PAH)"]
[]
[null,"Fluoranthen",null,null,null,null,null,{"$f":"D_GruOlie_cv_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_gvk_156","v":0.1},null,null,{"$f":"D_GruOlie_C1_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_overskr1_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_C2_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_C3_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_GruOlie_overskr_156","v":{"$error":"#DIV/0!"}}]
[]
[null,"Benzo(a)pyren",null,null,null,null,null,{"$f":"D_gruolie_cv_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_gvk_256","v":0.01},null,null,{"$f":"D_gruolie_c1_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr1_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c2_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr_256","v":{"$error":"#DIV/0!"}}]
[]
[null,"Benzo(b+k)fluoranthen",null,null,null,null,null,{"$f":"D_gruolie_cv_255","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_255","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_255","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_255","v":{"$error":"#DIV/0!"}}]
[]
[null,"Benzo(ghi)perylen",null,null,null,null,null,{"$f":"D_gruolie_cv_258","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_258","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_258","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_258","v":{"$error":"#DIV/0!"}}]
[]
[null,"Indeno(1,2,3-cd)pyren",null,null,null,null,null,{"$f":"D_gruolie_cv_352","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c1_352","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_gruolie_c2_352","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_352","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af 4 PAH`er",null,null,null,null,null,{"$f":"D_gruolie_cv_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_gvk_21","v":0.1},null,null,{"$f":"D_gruolie_c1_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr1_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c2_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_c3_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_gruolie_overskr_21","v":{"$error":"#DIV/0!"}}]
[]
["NSO-forbindelser"]
[null,"Benzo(b)thiophen",null,null,null,null,null,{"$f":"D_Gruolie_cv_10","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_10","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_10","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_10","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dibenzofuran",null,null,null,null,null,{"$f":"D_Gruolie_cv_11","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_11","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_11","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gruolie_c3_11","v":{"$error":"#VALUE!"}}]
[]
[null,"Dibenzothiophen",null,null,null,null,null,{"$f":"D_Gruolie_cv_12","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_12","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_12","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_12","v":{"$error":"#DIV/0!"}}]
[]
[null,"Acridin",null,null,null,null,null,{"$f":"D_Gruolie_cv_13","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_13","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_13","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Gruolie_c3_13","v":{"$error":"#VALUE!"}}]
[]
[null,"Carbazol",null,null,null,null,null,{"$f":"D_Gruolie_cv_14","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_14","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_14","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_14","v":{"$error":"#DIV/0!"}}]
[]
[null,"Anilin",null,null,null,null,null,{"$f":"D_Gruolie_cv_15","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_15","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_15","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_15","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dimethyldisulfid",null,null,null,null,null,{"$f":"D_Gruolie_cv_16","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_16","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_16","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_16","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af NSO-forbindelser",null,null,null,null,null,{"$f":"D_Gruolie_cv_nso","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c1_nso","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_Gruolie_c2_nso","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Gruolie_c3_nso","v":{"$error":"#DIV/0!"}}]

{"sheet":"Dataark_Grundvand-Olie","index":38,"n_rows":125,"n_cols":20,"rows_kept":125,"cut":false,"hidden":true,"merged":[[1,1,1,16]]}
[]
[null,"Dataark-Grundvand-Olie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Vanddata"]
[null,"Parameter","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes"]
[null,"Hydraulisk ledningsevne (m/s)","k","m/s",null,null,{"$f":"GruOlie_my_k","v":0},{"$f":"IF(VALUE(G6),G6,IF(F6<>0,F6,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1a_k","input, jorddata-hydraulik"]
[null,"Hydraulisk ledningsevne (m/år)","kår","m/år",null,{"$f":"B_GruOlie_trin1a_kår","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1a_kår","beregnes"]
[null,"Hydraulisk gradient","i","-",null,null,{"$f":"GruOlie_i","v":0},"",null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1a_i","input"]
[null,"Baggrundskoncentration upstrøms",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,"D_GruOlie_Cg","input"]
[null,"Vandflux","Q0","m3/år",null,{"$f":"B_GruOlie_trin1a_Q0","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1a_Q0","beregnes"]
[null,"Darcy hastighed (vand)","VD","m/år",null,{"$f":"B_GruOlie_trin1a_VD","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1a_VD","beregnes"]
[null,"Grundvandsflux","Qg","m3/år",null,{"$f":"B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1a_Qg","beregnes"]
[null,"Gns. porevandshastighed","VP","m/år",null,{"$f":"B_GruOlie_trin2a_VP","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_VP","beregnes"]
[null,"Grundvandsflux","Qg_2a","m3/år",null,{"$f":"B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_Qg_2a","beregnes"]
[]
[null,"Lokalitetsspecifikke data"]
[null,"Parameter","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes"]
[null,"Areal af forurenet område","A","m2",null,null,{"$f":"GruOlie_Y*GruOlie_X","v":0},{"$f":"IF(VALUE(G18),G18,IF(F18<>0,F18,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_A","input"]
[null,"Længde af kildeområde","Y",null,null,null,{"$f":"GruOlie_Y","v":0}]
[null,"Bredde af kildeområde","X","m",null,null,{"$f":"GruOlie_X","v":0},{"$f":"IF(VALUE(G20),G20,IF(F20<>0,F20,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_B","input"]
[null,"Nettoinfiltration","N","mm/år",null,null,{"$f":"GruOlie_My_Nedbør","v":0},{"$f":"IF(VALUE(G21),G21,IF(F21<>0,F21,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_N","nedbørsdata"]
[null,"Egnsnavn",null,null,null,null,{"$f":"GruOlie_My_Kommune","v":0},{"$f":"IF(ISTEXT(G22),G22,IF(F22<>0,F22,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_Kommune","Egnsnavn"]
[null,"Aquifermaterial",null,null,null,null,{"$f":"GruOlie_My_Aqui","v":0},{"$f":"IF(ISTEXT(G23),G23,IF(F23<>0,F23,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_Aqui_syst","input"]
[null,"Opblandingstykkelse_trin1a","dm_1a","m",null,0.25,null,{"$f":"IF(VALUE(G24),G24,IF(F24<>0,F24,\"\"))","v":0.25},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_dm_1a","default=0,25, (input)"]
[null,"Porøsitet, vandmættet ","eW","-",null,null,{"$f":"GruOlie_My_ew","v":0},{"$f":"IF(VALUE(G25),G25,IF(F25<>0,F25,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin3_eW","fra trin1a"]
[null,"Bulkmassefylde","(rho)b","kg/l",null,null,{"$f":"GruOlie_My_p","v":0},{"$f":"IF(VALUE(G26),G26,IF(F26<>0,F26,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_rhob","input"]
[null,"% Indhold organisk kulstof","foc (%)","-",null,null,{"$f":"GruOlie_My_foc","v":0},{"$f":"IF(VALUE(G27),G27,IF(F27<>0,F27,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_foc_syst","input"]
[null,"Fraktion organisk indhold","foc",null,null,{"$f":"F27/100","v":0},{"$f":"G27/100","v":0},{"$f":"H27/100","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_foc","beregnes i dataark"]
[null,"Effiktiv porøsitet","eeff","-",null,null,{"$f":"GruOlie_My_eff","v":0},{"$f":"IF(VALUE(G29),G29,IF(F29<>0,F29,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_eeff","jorddata"]
[null,"Tykkelse af grundvandsmagasin","dm_max","m",null,null,{"$f":"GruOlie_Maxdm","v":0},"",null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_dm_max","input"]
[null,"Langsgående dispersivitet","(alfa)L","m",null,{"$f":"B_GruOlie_trin2a_aL","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_aL","beregnes"]
[null,"Transporttid","t","år",null,{"$f":"B_GruOlie_trin2a_t","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_t","beregnes"]
[null,"Opblandingstykkelse_trin2a","dm_2a","m",null,{"$f":"B_GruOlie_trin2a_dm_2a","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin2a_dm_2a","beregnes"]
[null,"Afstand til teoretisk beregningspunkt","L","m",null,{"$f":"GruOlie_beregnet_teoretisk_afstand","v":{"$error":"#VALUE!"}},{"$f":"GruOlie_my_Beregnpunkt","v":0},{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"D_GruOlie_trin1b_LL","beregnes"]
[null,"Nedbrydningskonstant",null,"dage-1",null,0,{"$f":"Gruolie_My_ned","v":0},{"$f":"IF(ISNUMBER(G35),G35,IF(F35<>0,F35,\"\"))","v":0},null,null,null,null,null,null,null,null,null,null,"D_Gruolie_ned","input"]
[null,"Anvendt brugerdata",null,null,null,null,{"$f":"SUM(G6+G21+G25+G26+G27+G29+G35)","v":0}]
[null,"Anvendt brugerdata i oliefugacitetsmodul",null,null,null,{"$f":"Olie_bruger","v":"Nej"},{"$f":"IF(F37=\"Nej\",0,10)","v":0}]
[null,"Samlet brugerdata",null,null,null,null,{"$f":"SUM(G36:G37)","v":0},{"$f":"IF(G38>0,\"Ja\",\"Nej\")","v":"Nej"}]
[]
[null,null,null,null,null,null,null,null,"Trin 1a",null,"Trin2a","Trin 3 uden nedbrydning"]
[null,null,null,null,null,"Beregnet konc Cv","Log Kow","Grundvands\nkriteriet","Forurenings\nkonc._C1","Overskridelse","Forurenings\nkonc._C2","Forurenings\nkonc._C3","Overskridelse","Nedbrydnings\nkonstant","log KD","R","stofhastighed m. sorption","Transporttid med sorption\ntil teoretisk beregn.pkt."]
[null,null,null,null,null,"µg/l",null,"µg/l","µg/l","gange","µg/l","µg/l","gange","dage-1",null,null,"m/år","dage"]
[50,"C5-C6"]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_51","v":2.72},null,null,null,null,null,null,{"$f":"D_gruolie_ned","v":0},{"$f":"B_Gruolie_logKD_51","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_51","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_51","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_51","v":{"$error":"#VALUE!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_511","v":3.39},null,null,null,null,null,null,0,{"$f":"B_Gruolie_logKD_511","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_511","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_511","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_511","v":{"$error":"#VALUE!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_512","v":3.21},null,null,null,null,null,null,0,{"$f":"B_Gruolie_logKD_512","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_512","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_512","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_512","v":{"$error":"#VALUE!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_513","v":3.6},null,null,null,null,null,null,0,{"$f":"B_Gruolie_logKD_513","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_513","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_513","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_513","v":{"$error":"#VALUE!"}}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Gruolie_C1_510","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_510","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_510","v":{"$error":"#DIV/0!"}},null,0]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_52","v":2.13},{"$f":"D_Olie_52_gkk","v":1},{"$f":"B_Gruolie_C1_52","v":{"$error":"#DIV/0!"}},{"$f":"IF(I50/H50>1,I50/H50,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_52","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_52","v":{"$error":"#DIV/0!"}},{"$f":"IF(L50/H50>1,L50/H50,\"Nej\")","v":{"$error":"#DIV/0!"}},0,{"$f":"B_Gruolie_logKD_52","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_52","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_52","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_52","v":{"$error":"#VALUE!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_53","v":4.29},null,{"$f":"B_Gruolie_C1_53","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_53","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_53","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_53","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_53","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_53","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_53","v":{"$error":"#VALUE!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_54","v":2.73},{"$f":"D_Olie_54_gkk","v":5},{"$f":"B_Gruolie_C1_54","v":{"$error":"#DIV/0!"}},{"$f":"IF(I52/H52>1,I52/H52,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_54","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_54","v":{"$error":"#DIV/0!"}},{"$f":"IF(L52/H52>1,L52/H52,\"Nej\")","v":{"$error":"#DIV/0!"}},0,{"$f":"B_Gruolie_logKD_54","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_54","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_54","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_54","v":{"$error":"#VALUE!"}}]
[55,">8 - 10, alifater",">8 - 10, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_55B_cv,D_Olie_55A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_55b,B_olie_kow_55a)","v":5.15},null,{"$f":"B_Gruolie_C1_55","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_55","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_55","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_55","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_55","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_55","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_55","v":{"$error":"#VALUE!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater",null,null,null,null,null,null,null,null,null,null,0]
[571,null,"o-Xylen",null,null,null,null,null,null,null,null,null,null,0]
[572,null,"m+p-Xylen",null,null,null,null,null,null,null,null,null,null,0]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_57","v":3.2},null,{"$f":"B_GruOlie_C1_57","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_57","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_57","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_57","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_57","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_57","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_57","v":{"$error":"#VALUE!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_58","v":3.15},null,{"$f":"B_GruOlie_C1_58","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_58","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_58","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_58","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_58","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_58","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_58","v":{"$error":"#VALUE!"}}]
[null,null,"Sum af xylener og ethylbenzen",null,null,{"$f":"SUM(F57:F58)","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_57_gkk","v":5},{"$f":"SUM(I57:I58)","v":{"$error":"#DIV/0!"}},{"$f":"IF(I59/H59>1,I59/H59,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"SUM(K57:K58)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L57:L58)","v":{"$error":"#DIV/0!"}},{"$f":"IF(L59/H59>1,L59/H59,\"Nej\")","v":{"$error":"#DIV/0!"}}]
[59,null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},null,{"$f":"B_GruOlie_C1_59","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_59","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_59","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_59","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_59","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_59","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_59","v":{"$error":"#VALUE!"}}]
[60,null,">8 -10, aromater,øvrige",null,null,{"$f":"D_olie_60_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"D_Olie_60_gkk","v":1},{"$f":"B_GruOlie_C1_60","v":{"$error":"#DIV/0!"}},{"$f":"IF(I61/H61>1,I61/H61,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_60","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_60","v":{"$error":"#DIV/0!"}},{"$f":"IF(L61/H61>1,L61/H61,\"Nej\")","v":{"$error":"#DIV/0!"}},0]
[910,null,null,null,null,{"$f":"D_olie_910_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"D_Olie_60_gkk","v":1},{"$f":"B_GruOlie_C1_910","v":{"$error":"#DIV/0!"}},{"$f":"IF(I62/H62>1,I62/H62,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_GruOlie_C2_910","v":{"$error":"#DIV/0!"}},{"$f":"B_GruOlie_C3_910","v":{"$error":"#DIV/0!"}},{"$f":"IF(L62/H62>1,L62/H62,\"Nej\")","v":{"$error":"#DIV/0!"}},0,{"$f":"B_GruOlie_logKD_910","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_R_910","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_VP_910","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_T_910","v":{"$error":"#VALUE!"}}]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_GruOlie_C1_1015","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_1015","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_1015","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_101","v":6.1},null,{"$f":"B_GruOlie_C1_101","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_101","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_101","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_101","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_101","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_101","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_101","v":{"$error":"#VALUE!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater",null,null,null,null,null,null,null,null,null,null,0]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_103","v":3.3},{"$f":"D_Olie_103_gkk","v":1},{"$f":"B_GruOlie_C1_103","v":{"$error":"#DIV/0!"}},{"$f":"IF(I66/H66>1,I66/H66,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_103","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_103","v":{"$error":"#DIV/0!"}},{"$f":"IF(L66/H66>1,L66/H66,\"Nej\")","v":{"$error":"#DIV/0!"}},0,{"$f":"B_Gruolie_logKD_103","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_103","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_103","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_103","v":{"$error":"#VALUE!"}}]
[104,null,">10 - 12, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_104B_cv,D_Olie_104A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_104b,B_olie_kow_104a)","v":4.7300000000000004},null,{"$f":"B_GruOlie_C1_104","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_104","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_104","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_104","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_104","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_104","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_104","v":{"$error":"#VALUE!"}}]
[105,">12 - 16, alifater",">12 - 16, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_105B_cv,D_Olie_105A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_105b,B_olie_kow_105a)","v":7.72},null,{"$f":"B_GruOlie_C1_105","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_105","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_105","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_105","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_105","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_105","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_105","v":{"$error":"#VALUE!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater",null,null,null,null,null,null,null,null,null,null,0]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_107","v":4.07},null,{"$f":"B_GruOlie_C1_107","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_107","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_107","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_107","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_107","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_107","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_107","v":{"$error":"#VALUE!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_108","v":3.92},null,{"$f":"B_GruOlie_C1_108","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_108","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_108","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_108","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_108","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_108","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_108","v":{"$error":"#VALUE!"}}]
[109,null,">12 - 16, aromater,øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_109B_cv,D_Olie_109A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_109b,B_olie_kow_109a)","v":4.4000000000000004},null,{"$f":"B_GruOlie_C1_109","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_109","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_109","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_109","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_109","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_109","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_109","v":{"$error":"#VALUE!"}}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_GruOlie_C1_1520","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_1520","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_1520","v":{"$error":"#DIV/0!"}},null,0]
[151,">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_151B_cv,D_Olie_151A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_151b,B_olie_kow_151a)","v":9.84},null,{"$f":"B_GruOlie_C1_151","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_151","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_151","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_151","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_151","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_151","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_151","v":{"$error":"#VALUE!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater",null,null,null,null,null,null,null,null,null,null,0]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_153","v":4.18},null,{"$f":"B_GruOlie_C1_153","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_153","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_153","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_153","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_153","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_153","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_153","v":{"$error":"#VALUE!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_154","v":4.46},null,{"$f":"B_GruOlie_C1_154","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_154","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_154","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_154","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_154","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_154","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_154","v":{"$error":"#VALUE!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_155","v":4.45},null,{"$f":"B_GruOlie_C1_155","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_155","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_155","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_155","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_155","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_155","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_155","v":{"$error":"#VALUE!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_156","v":5.16},{"$f":"D_Olie_156_gkk","v":0.1},{"$f":"B_GruOlie_C1_156","v":{"$error":"#DIV/0!"}},{"$f":"IF(I80/H80>1,I80/H80,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_156","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_156","v":{"$error":"#DIV/0!"}},{"$f":"IF(L80/H80>1,L80/H80,\"Nej\")","v":{"$error":"#DIV/0!"}},0,{"$f":"B_Gruolie_logKD_156","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_156","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_156","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_156","v":{"$error":"#VALUE!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_157","v":4.88},null,{"$f":"B_GruOlie_C1_157","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_157","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_157","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_157","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_157","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_157","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_157","v":{"$error":"#VALUE!"}}]
[]
[2025,"C21-C25",null,null,null,null,null,null,null,null,null,null,null,0]
[201,">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_201B_cv,D_Olie_201A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_201b,B_olie_kow_201a)","v":12.62},null,{"$f":"B_GruOlie_C1_201","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_201","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_201","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_201","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_201","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_201","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_201","v":{"$error":"#VALUE!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter",null,null,null,null,null,null,null,null,null,null,0]
[]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_GruOlie_C1_2535","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_2535","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_2535","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0}]
[251,">25 - 35, alifater",">25 - 35, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_251B_cv,D_Olie_251A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_251b,B_olie_kow_251a)","v":14.58},null,{"$f":"B_GruOlie_C1_251","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_251","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_251","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_251","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_251","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_251","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_251","v":{"$error":"#VALUE!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,null,null,null,null,null,null,0]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_253","v":5.76},null,{"$f":"B_GruOlie_C1_253","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_253","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_253","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_253","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_253","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_253","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_253","v":{"$error":"#VALUE!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_254","v":5.81},null,{"$f":"B_GruOlie_C1_254","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_254","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_254","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_254","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_254","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_254","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_254","v":{"$error":"#VALUE!"}}]
[255,null,"Benzo(b+k)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_255","v":5.78},null,{"$f":"B_GruOlie_C1_255","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_255","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_255","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_255","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_255","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_255","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_255","v":{"$error":"#VALUE!"}}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_256","v":6.13},{"$f":"D_Olie_256_gkk","v":0.01},{"$f":"B_GruOlie_C1_256","v":{"$error":"#DIV/0!"}},{"$f":"IF(I93/H93>1,I93/H93,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_256","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_256","v":{"$error":"#DIV/0!"}},{"$f":"IF(L93/H93>1,L93/H93,\"Nej\")","v":{"$error":"#DIV/0!"}},0,{"$f":"B_Gruolie_logKD_256","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_256","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_256","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_256","v":{"$error":"#VALUE!"}}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_257","v":6.75},null,{"$f":"B_GruOlie_C1_257","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_257","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_257","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_257","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_257","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_257","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_257","v":{"$error":"#VALUE!"}}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_258","v":6.63},null,{"$f":"B_GruOlie_C1_258","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_258","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_258","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_258","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_258","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_258","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_258","v":{"$error":"#VALUE!"}}]
[259,null,">25 - 35, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_259B_cv,D_Olie_259A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_259b,B_olie_kow_259a)","v":7.11},null,{"$f":"B_GruOlie_C1_259","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_259","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_259","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_259","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_259","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_259","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_259","v":{"$error":"#VALUE!"}}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_GruOlie_C1_3540","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_3540","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_3540","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_351","v":17.53},null,{"$f":"B_GruOlie_C1_351","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_351","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_351","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0},{"$f":"B_Gruolie_logKD_351","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_351","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_351","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_351","v":{"$error":"#VALUE!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_352","v":6.7},null,{"$f":"B_GruOlie_C1_352","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_352","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_352","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0},{"$f":"B_Gruolie_logKD_352","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_352","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_352","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_352","v":{"$error":"#VALUE!"}}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_GruOlie_C1_2040","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_2040","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_2040","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0}]
[]
[20,"Sum af 7 PAH'er jord",null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_gruolie_ned","v":0}]
[21,"Sum af 4 PAH'er vand",null,null,null,{"$f":"SUM(F92+F95+F100)","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_21_gkk","v":0.1},{"$f":"B_GruOlie_C1_21","v":{"$error":"#DIV/0!"}},{"$f":"IF(I105/H105>1,I105/H105,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_21","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_21","v":{"$error":"#DIV/0!"}},{"$f":"IF(L105/H105>1,L105/H105,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_ned","v":0}]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_10","v":3.12},null,{"$f":"B_GruOlie_C1_10","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_10","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_10","v":{"$error":"#DIV/0!"}},null,{"$f":"D_gruolie_ned","v":0},{"$f":"B_Gruolie_logKD_10","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_10","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_10","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_10","v":{"$error":"#VALUE!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_11","v":4.12},null,{"$f":"B_GruOlie_C1_11","v":{"$error":"#VALUE!"}},null,{"$f":"B_Gruolie_C2_11","v":{"$error":"#VALUE!"}},{"$f":"B_Gruolie_C3_11","v":{"$error":"#VALUE!"}},null,0,{"$f":"B_Gruolie_logKD_11","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_11","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_11","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_11","v":{"$error":"#VALUE!"}}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_12","v":4.38},null,{"$f":"B_GruOlie_C1_12","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_12","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_12","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_12","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_12","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_12","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_12","v":{"$error":"#VALUE!"}}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_13","v":3.4},null,{"$f":"B_GruOlie_C1_13","v":{"$error":"#VALUE!"}},null,{"$f":"B_Gruolie_C2_13","v":{"$error":"#VALUE!"}},{"$f":"B_Gruolie_C3_13","v":{"$error":"#VALUE!"}},null,0,{"$f":"B_Gruolie_logKD_13","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_13","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_13","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_13","v":{"$error":"#VALUE!"}}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_14","v":2.36},null,{"$f":"B_GruOlie_C1_14","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_14","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_14","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_14","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_14","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_14","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_14","v":{"$error":"#VALUE!"}}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_15","v":0.9},null,{"$f":"B_GruOlie_C1_15","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_15","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_15","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_15","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_15","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_15","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_15","v":{"$error":"#VALUE!"}}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_16","v":1.77},null,{"$f":"B_GruOlie_C1_16","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_16","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_16","v":{"$error":"#DIV/0!"}},null,0,{"$f":"B_Gruolie_logKD_16","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_R_16","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_VP_16","v":{"$error":"#VALUE!"}},{"$f":"B_gruolie_T_16","v":{"$error":"#VALUE!"}}]
[null,null,"sum af NSO",null,null,{"$f":"SUM(F108:F114)","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_GruOlie_C1_nso","v":{"$error":"#DIV/0!"}},null,{"$f":"B_Gruolie_C2_nso","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_nso","v":{"$error":"#DIV/0!"}},null,0]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_1_gkk","v":9},{"$f":"B_GruOlie_C1_1","v":{"$error":"#DIV/0!"}},{"$f":"IF(I117/H117>1,I117/H117,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C2_1","v":{"$error":"#DIV/0!"}},{"$f":"B_Gruolie_C3_1","v":{"$error":"#DIV/0!"}},{"$f":"IF(L117/H117>1,L117/H117,\"Nej\")","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_ned","v":0}]
[]
[null,"Bagrundskonc, Cg, er defineret som 0"]
[]
[null,"Bemærkninger"]
[null,"Det forurenede område:","D_GruOlie_DFO_ComUds"]
[null,null,false]
[null,"Magasin:","D_GruOlie_Mag_ComUds"]
[null,null,false]

{"sheet":"Beregning_Grundvand-Olie","index":39,"n_rows":97,"n_cols":19,"rows_kept":97,"cut":false,"hidden":true,"merged":[[1,1,1,15]]}
[]
[null,"Beregningslag Grundvand-Olie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Vanddata"]
[null,"Stoffer","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Hydraulisk ledningsevne (m/år)","kår","m/år",{"$f":"D_GruOlie_trin1a_k*(60*60*24*365.25)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F6),F6,IF(E6<>0,E6,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin1a_kår","beregnes"]
[null,"Vandflux","Q0","m3/år",{"$f":"(D_GruOlie_N*D_GruOlie_A)/1000","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin1a_Q0","beregnes"]
[null,"Darcy hastighed (vand)","VD","m/år",{"$f":"D_GruOlie_trin1a_kår*D_GruOlie_trin1a_i","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin1a_VD","beregnes"]
[null,"Grundvandsflux","Qg","m3/år",{"$f":"D_GruOlie_B*D_GruOlie_dm_1a*D_GruOlie_trin1a_VD","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin1a_Qg","beregnes"]
[null,"Gns. porevandshastighed","VP","m/år",{"$f":"D_GruOlie_trin1a_VD/D_GruOlie_trin2a_eeff","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin2a_VP","beregnes"]
[null,"Grundvandsflux","Qg_2a","m3/år",{"$f":"D_GruOlie_B*D_GruOlie_trin2a_dm_2a*D_GruOlie_trin1a_VD","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin2a_Qg_2a","beregnes"]
[]
[null,"Lokalitetsspecifikke data"]
[null,"Stoffer","Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Langsgående dispersivitet","(alfa)L","m",{"$f":"0.0000042*POWER(D_GruOlie_trin1b_LL,2)+0.0036*D_GruOlie_trin1b_LL-0.008","v":{"$error":"#VALUE!"}},null,{"$f":"IF(E15<0,1E-36,E15)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin2a_aL","beregnes"]
[null,"Transporttid","t","år",{"$f":"D_GruOlie_trin1b_LL/D_GruOlie_trin2a_VP","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F16),F16,IF(E16<>0,E16,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin2a_t","beregnes"]
[null,"Opblandingstykkelse_trin2a","dm_2a","m",{"$f":"MAX(D_GruOlie_dm_1a,MIN(IF(D_GruOlie_trin2a_dm_max>0,D_GruOlie_trin2a_dm_max,1E+36),SQRT((72/900)*D_GruOlie_trin2a_aL*D_GruOlie_trin2a_VP*D_GruOlie_trin2a_t)))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(F17),F17,IF(E17<>0,E17,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin2a_dm_2a","beregnes"]
[null,"Afstand til teoretisk beregningspunkt","L","m",{"$f":"MIN(D_GruOlie_trin2a_VP,100)","v":{"$error":"#VALUE!"}},{"$f":"GruOlie_my_Beregnpunkt","v":0},{"$f":"IF(VALUE(F18),F18,IF(E18<>0,E18,\"\"))","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,"B_GruOlie_trin1b_LL","beregnes"]
[]
[null,null,null,null,null,null,null,null,"Trin 1a",null,"Trin 2a",null,"Trin 3 "]
[null,null,null,null,null,"Beregnet konc Cv","Log Kow","Stofflux","Naturlig grundvandsflux","Forurenings\nkonc._C1","Naturlig grundvandsflux","Forurenings\nkonc._C2","Forurenings\nkonc._C3","Nedbrydnings\nkonstant","log KD","KD","R","stofhastighed m. sorption","Transporttid med sorption\ntil teoretisk beregn.pkt."]
[null,null,null,null,null,"µg/L",null,"µg/år","µg/år","µg/l","µg/år","µg/l","µg/l","dage-1",null,null,null,"m/år","dage"]
[50,"C5-C6",null,null,null,{"$f":"SUM(F24:F27)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(H24:H27)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(J24:J27)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(L24:L27)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(M24:M27)","v":{"$error":"#DIV/0!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_51","v":2.72},{"$f":"F24*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"(H24+I24)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin1a_Qg)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"(H24+K24)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#DIV/0!"}},{"$f":"L24*EXP(-N24*S24)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_51","v":0},{"$f":"1.04*G24+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$f":"POWER(10,O24)","v":{"$error":"#VALUE!"}},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P24","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q24","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R24*365.25","v":{"$error":"#VALUE!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_511","v":3.39},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_511","v":0},{"$error":"#VALUE!"},{"$f":"POWER(10,O25)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_512","v":3.21},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_512","v":0},{"$error":"#VALUE!"},{"$f":"POWER(10,O26)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_513","v":3.6},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_513","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(H30:H40)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_52","v":2.13},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_52","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_53","v":4.29},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_53","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_54","v":2.73},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_54","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[55,">8 - 10, alifater",">8 - 10, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_55B_cv,D_Olie_55A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_55b,B_olie_kow_55a)","v":5.15},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_55","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_57","v":3.2},{"$f":"F37*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"L37*EXP(-N37*S37)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_57","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_58","v":3.15},{"$f":"F38*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_58","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[59,null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"F39*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_59","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[60,null,">8 -10, aromater,øvrige",null,null,{"$f":"D_olie_60_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"F40*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_nedkonst_60","v":0},{"$f":"1.04*G40+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$f":"POWER(10,O40)","v":{"$error":"#VALUE!"}},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P40","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q40","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R40*365.25","v":{"$error":"#VALUE!"}}]
[910,null,null,null,null,{"$f":"D_olie_910_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"F41*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"(H41+K41)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#DIV/0!"}},{"$f":"L41*EXP(-N41*S41)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_nedkonst_60","v":0},{"$f":"1.04*G41+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$f":"POWER(10,O41)","v":{"$error":"#VALUE!"}},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P41","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q41","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R41*365.25","v":{"$error":"#VALUE!"}}]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(H43:H51)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_101","v":6.1},{"$f":"F43*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_101","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_103","v":3.3},{"$f":"F45*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_103","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[104,null,">10 - 12, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_104B_cv,D_Olie_104A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_104b,B_olie_kow_104a)","v":4.7300000000000004},{"$f":"F46*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_104","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[105,">12 - 16, alifater",">12 - 16, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_105B_cv,D_Olie_105A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_105b,B_olie_kow_105a)","v":7.72},{"$f":"F47*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_105","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_107","v":4.07},{"$f":"F49*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_107","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_108","v":3.92},{"$f":"F50*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_108","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[109,null,">12 - 16, aromater,øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_109B_cv,D_Olie_109A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_109b,B_olie_kow_109a)","v":4.4000000000000004},{"$f":"F51*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_109","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(H54:H60)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[151,">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_151B_cv,D_Olie_151A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_151b,B_olie_kow_151a)","v":9.84},{"$f":"F54*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_151","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_153","v":4.18},{"$f":"F56*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_153","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_154","v":4.46},{"$f":"F57*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"(H57+I57)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin1a_Qg)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"(H57+K57)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_154","v":0},{"$f":"1.04*G57+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P57","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q57","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R57*365.25","v":{"$error":"#VALUE!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_155","v":4.45},{"$f":"F58*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_155","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_156","v":5.16},{"$f":"F59*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_156","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_157","v":4.88},{"$f":"F60*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_157","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[2025,"C21-C25"]
[201,">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_201B_cv,D_Olie_201A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_201b,B_olie_kow_201a)","v":12.62},{"$f":"F63*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_201","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[202,">21 - 25, aromater","Ingen repræsentanter"]
[]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(H67:H75)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[251,">25 - 35, alifater",">25 - 35, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_251B_cv,D_Olie_251A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_251b,B_olie_kow_251a)","v":14.58},{"$f":"F67*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_251","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater"]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_253","v":5.76},{"$f":"F69*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_253","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_254","v":5.81},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_254","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[255,null,"Benzo(b+k)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_255","v":5.78},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_255","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_256","v":6.13},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_256","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_257","v":6.75},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_257","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_258","v":6.63},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_258","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[259,null,">25 - 35, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_259B_cv,D_Olie_259A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_259b,B_olie_kow_259a)","v":7.11},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_259","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(H78:H79)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_351","v":17.53},{"$f":"F78*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_351","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_352","v":6.7},{"$f":"F79*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_352","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"F81*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"SUM(B_GruOlie_C1_2535+B_GruOlie_C1_201)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"SUM(B_Gruolie_C2_2535+B_Gruolie_C2_201)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_Gruolie_C3_2535+B_Gruolie_C3_201)","v":{"$error":"#DIV/0!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand",null,null,null,{"$f":"SUM(F71+F74+F79)","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(B_GruOlie_C1_352+B_GruOlie_C1_255+B_GruOlie_C1_258)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"SUM(B_Gruolie_C2_352+B_Gruolie_C2_255+B_Gruolie_C2_258)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_Gruolie_C3_352+B_Gruolie_C3_255+B_Gruolie_C3_258)","v":{"$error":"#DIV/0!"}}]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_10","v":3.12},{"$f":"F87*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_10","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_11","v":4.12},null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"D_gruolie_nedkonst_11","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_12","v":4.38},{"$f":"F89*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_12","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_13","v":3.4},null,null,{"$f":"(H90+I90)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin1a_Qg)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"(H90+K90)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"D_gruolie_nedkonst_13","v":0},{"$f":"1.04*G90+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P90","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q90","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R90*365.25","v":{"$error":"#VALUE!"}}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_14","v":2.36},{"$f":"F91*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"(H91+I91)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin1a_Qg)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$f":"(H91+K91)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"D_gruolie_nedkonst_14","v":0},{"$f":"1.04*G91+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P91","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q91","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R91*365.25","v":{"$error":"#VALUE!"}}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_15","v":0.9},{"$f":"F92*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"(H92+I92)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin1a_Qg)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$f":"(H92+K92)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#DIV/0!"}},{"$f":"L92*EXP(-N92*S92)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_15","v":0},{"$f":"1.04*G92+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$f":"POWER(10,O92)","v":{"$error":"#VALUE!"}},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P92","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q92","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R92*365.25","v":{"$error":"#VALUE!"}}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_16","v":1.77},{"$f":"F93*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"(H93+I93)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin1a_Qg)","v":{"$error":"#DIV/0!"}},{"$error":"#VALUE!"},{"$f":"(H93+K93)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#DIV/0!"}},{"$f":"L93*EXP(-N93*S93)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_16","v":0},{"$f":"1.04*G93+LOG(D_GruOlie_foc)-0.84","v":{"$error":"#VALUE!"}},{"$f":"POWER(10,O93)","v":{"$error":"#VALUE!"}},{"$f":"1+D_GruOlie_rhob/D_GruOlie_trin3_eW*P93","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin2a_VP/Q93","v":{"$error":"#VALUE!"}},{"$f":"B_GruOlie_trin1b_LL/R93*365.25","v":{"$error":"#VALUE!"}}]
[null,"Sum af NSO-forbindelser ",null,null,null,{"$f":"SUM(F87:F93)","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J87:J93)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(L87:L93)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(M87:M93)","v":{"$error":"#DIV/0!"}}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cv","v":{"$error":"#DIV/0!"}},null,{"$f":"F96*B_GruOlie_trin1a_Q0","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin1a_Qg","v":{"$error":"#VALUE!"}},{"$f":"SUM(B_Gruolie_C1_510+B_GruOlie_C1_1015+B_GruOlie_C1_1520+B_GruOlie_C1_201+B_GruOlie_C1_2535+B_GruOlie_C1_3540)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"SUM(B_Gruolie_C2_510+B_Gruolie_C2_1015+B_Gruolie_C2_1520+B_Gruolie_C2_201+B_Gruolie_C2_2535+B_Gruolie_C2_3540)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_Gruolie_C3_510+B_Gruolie_C3_1015+B_Gruolie_C3_1520+B_Gruolie_C3_201+B_Gruolie_C3_2535+B_Gruolie_C3_3540)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J23+B_Gruolie_C1_510+B_GruOlie_C1_1015+B_GruOlie_C1_1520+B_GruOlie_C1_201+B_GruOlie_C1_2535+B_GruOlie_C1_3540+B_GruOlie_C1_nso)","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(L23+B_Gruolie_C2_510+B_Gruolie_C2_1015+B_Gruolie_C2_1520+B_Gruolie_C2_201+B_Gruolie_C2_2535+B_Gruolie_C2_3540+B_Gruolie_C2_nso)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(M23+B_Gruolie_C3_510+B_Gruolie_C3_1015+B_Gruolie_C3_1520+B_Gruolie_C3_201+B_Gruolie_C3_2535+B_Gruolie_C3_3540+B_Gruolie_C3_nso)","v":{"$error":"#DIV/0!"}}]

{"sheet":"Udskrift_Grundvand-Olie","index":40,"n_rows":84,"n_cols":10,"rows_kept":84,"cut":false,"hidden":true,"merged":[[9,5,9,7],[10,5,10,7],[9,2,9,4],[10,2,10,4],[16,2,16,4],[16,5,16,7],[12,2,12,4],[12,5,12,7],[13,2,13,4],[13,5,13,7],[5,1,5,10],[2,8,2,10],[3,8,3,10],[4,8,4,10],[2,1,2,5],[3,1,3,5],[4,1,4,5],[21,5,21,7],[22,5,22,7],[21,2,21,4],[17,2,17,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[17,5,17,7],[18,5,18,7],[19,5,19,7],[20,5,20,7],[23,5,23,7],[22,2,22,4],[24,2,24,4],[25,2,25,4],[28,8,28,9],[23,2,23,4],[25,5,25,7],[67,1,80,9],[82,1,95,9],[28,2,28,3],[28,4,28,5],[28,6,28,7],[33,13,33,15],[29,2,29,3],[29,4,29,5],[29,6,29,7],[29,8,29,9]]}
["Grundvand-Olie"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
[]
["Det forurenede område",null,null,null,null,null,null,null,"Kommentar",{"$f":"IF(D_GruOlie_DFO_ComUds,\"ja\",\"nej\")","v":"nej"}]
[null,null,"Standard data",null,null,"Indtastede data (angives med fed)"]
["Areal: forurenede område","A",null,null,null,{"$f":"IF(GruOlie_Y<>\"\",D_GruOlie_A,\"\")","v":""},null,null,"m²"]
["Bredde: forurenede område","B",null,null,null,{"$f":"IF(GruOlie_X<>\"\",GruOlie_X,\"\")","v":""},null,null,"m"]
[]
["Nettonedbør","N",{"$f":"IF(D_GruOlie_N_syst<>\"\",D_GruOlie_N_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_My_Nedbør<>\"\",GruOlie_My_Nedbør,\"\")","v":""},null,null,"mm/år"]
["Kommune/Egn",null,{"$f":"IF(D_GruOlie_Kommune_syst<>\"\",D_GruOlie_Kommune_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_My_Kommune<>\"\",GruOlie_My_Kommune,\"\")","v":""}]
[]
["Det først betydende magasin",null,null,null,null,null,null,null,"Kommentar",{"$f":"IF(D_GruOlie_Mag_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Aguifer",null,{"$f":"IF(D_GruOlie_Aqui_syst<>\"\",D_GruOlie_Aqui_syst,\"\")","v":""},null,null,{"$f":"IF(AND(D_GruOlie_Aqui<>\"\",D_GruOlie_Aqui<>D_GruOlie_Aqui_syst),D_GruOlie_Aqui,\"\")","v":""}]
["Effektiv porøsitet","eeff",{"$f":"IF(D_GruOlie_trin2a_eeff_syst<>\"\",D_GruOlie_trin2a_eeff_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_My_eff<>\"\",GruOlie_My_eff,\"\")","v":""}]
["Porøsitet, vandmættet ","eW",{"$f":"IF(D_GruOlie_trin3_eW_syst<>\"\",D_GruOlie_trin3_eW_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_My_ew<>\"\",GruOlie_My_ew,\"\")","v":""}]
["Bulkmassefylde","(rho)b",{"$f":"IF(D_GruOlie_rhob_syst<>\"\",D_GruOlie_rhob_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_My_p<>\"\",GruOlie_My_p,\"\")","v":""},null,null,"kg/l"]
["% organisk indhold","foc",{"$f":"IF(D_GruOlie_foc_syst<>\"\",D_GruOlie_foc_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_My_foc<>\"\",GruOlie_My_foc,\"\")","v":""}]
["Tykkelse af GV-magasin","dm_max",null,null,null,{"$f":"IF(GruOlie_Maxdm<>\"\",GruOlie_Maxdm,\"\")","v":""},null,null,"m"]
["Hydraulisk ledningsevne","k",{"$f":"IF(D_GruOlie_trin1a_k_syst<>\"\",D_GruOlie_trin1a_k_syst,\"\")","v":""},null,null,{"$f":"IF(GruOlie_my_k<>\"\",GruOlie_my_k,\"\")","v":""},null,null,"m/s"]
["Hydraulisk gradient","i",null,null,null,{"$f":"D_GruOlie_trin1a_i","v":""},null,null,"m/m"]
["Gvs. porevandshastighed","Vp",{"$f":"D_GruOlie_trin2a_VP","v":{"$error":"#VALUE!"}},null,null,null,null,null,"m/år"]
["Beregningspunkt","L",{"$f":"GruOlie_beregnet_teoretisk_afstand","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(GruOlie_my_Beregnpunkt <>0,GruOlie_my_Beregnpunkt,\"\")","v":""},null,null,"m"]
[]
["Beregning: Grundvand"]
[null,null,"Målepunkt",null,"Dato",null,"Fri fase?",null,"Anvendt brugerdata"]
["Angiv signifikant ciffer",2,{"$f":"IF(Olie_målepunkt<>\"\",D_olie_målepunkt,\"\")","v":""},null,{"$f":"IF(Olie_dato<>\"\",D_olie_dato,\"\")","v":""},null,{"$f":"Olie_frifase","v":"Nej"},null,{"$f":"D_gruolie_bruger","v":"Nej"}]
[]
[null,null,"Pore-\nvands\nkonc.","Nedbryd-nings\nkonstant","Grund\nvands-\nkrite-rium","Trin 1\n C1","Over-\nskridelse \naf kriteriet","Trin 2\n C2","Trin 3\n C3","Over-\nskridelse \naf kriteriet"]
[null,null,"µg/l","dage-1","µg/l","µg/l","gange","µg/l","µg/l","gange"]
["BTEX'er",null,"Nedbrydningskonstant i trin 3 er sat til",null,null,null,null,{"$f":"Gruolie_My_ned","v":0},"dage-1"]
["Benzen",null,{"$f":"IF(D_Gruolie_cv_52>0,ROUND(D_Gruolie_cv_52,3-(INT(LOG(D_Gruolie_cv_52))+1)),D_Gruolie_cv_52)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_52","v":0},{"$f":"D_gruolie_GVK_52","v":1},{"$f":"IF(D_Gruolie_c1_52>0,ROUND(D_Gruolie_c1_52,Gruolie_ciffer-(INT(LOG(D_Gruolie_c1_52))+1)),D_Gruolie_c1_52)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Gruolie_overskr1_52),ROUND(D_Gruolie_overskr1_52,Gruolie_ciffer-(INT(LOG(D_Gruolie_overskr1_52))+1)),D_Gruolie_overskr1_52)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Gruolie_c2_52>0,ROUND(D_Gruolie_c2_52,Gruolie_ciffer-(INT(LOG(D_Gruolie_c2_52))+1)),D_Gruolie_c2_52)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Gruolie_c3_52>0,ROUND(D_Gruolie_c3_52,Gruolie_ciffer-(INT(LOG(D_Gruolie_c3_52))+1)),D_Gruolie_c3_52)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Gruolie_overskr_52),ROUND(D_Gruolie_overskr_52,Gruolie_ciffer-(INT(LOG(D_Gruolie_overskr_52))+1)),D_Gruolie_overskr_52)","v":{"$error":"#DIV/0!"}}]
["Toluen",null,{"$f":"IF(D_gruolie_cv_54>0,ROUND(D_gruolie_cv_54,3-(INT(LOG(D_gruolie_cv_54))+1)),D_gruolie_cv_54)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_54","v":0},{"$f":"D_gruolie_gvk_54","v":5},{"$f":"IF(D_gruolie_c1_54>0,ROUND(D_gruolie_c1_54,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_54))+1)),D_gruolie_c1_54)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr1_54),ROUND(D_gruolie_overskr1_54,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr1_54))+1)),\"\")","v":""},{"$f":"IF(D_gruolie_c2_54>0,ROUND(D_gruolie_c2_54,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_54))+1)),D_gruolie_c2_54)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_54>0,ROUND(D_gruolie_c3_54,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_54))+1)),D_gruolie_c3_54)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr_54),ROUND(D_gruolie_overskr_54,3-(INT(LOG(D_gruolie_overskr_54))+1)),\"\")","v":""}]
["Ethylbenzen",null,{"$f":"IF(D_gruolie_cv_58>0,ROUND(D_gruolie_cv_58,3-(INT(LOG(D_gruolie_cv_58))+1)),D_gruolie_cv_58)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_58","v":0},null,{"$f":"IF(D_gruolie_c1_58>0,ROUND(D_gruolie_c1_58,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_58))+1)),D_gruolie_c1_58)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_gruolie_c2_58>0,ROUND(D_gruolie_c2_58,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_58))+1)),D_gruolie_c2_58)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_58>0,ROUND(D_gruolie_c3_58,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_58))+1)),D_gruolie_c3_58)","v":{"$error":"#DIV/0!"}}]
["Sum Xylener",null,{"$f":"IF(D_gruolie_cv_57>0,ROUND(D_gruolie_cv_57,3-(INT(LOG(D_gruolie_cv_57))+1)),D_gruolie_cv_57)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_57","v":0},null,{"$f":"IF(D_gruolie_c1_57>0,ROUND(D_gruolie_c1_57,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_57))+1)),D_gruolie_c1_57)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_gruolie_c1_57>0,ROUND(D_gruolie_c1_57,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_57))+1)),D_gruolie_c1_57)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_57>0,ROUND(D_gruolie_c3_57,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_57))+1)),D_gruolie_c3_57)","v":{"$error":"#DIV/0!"}}]
["Sum af xylener+ethylbenzen",null,{"$f":"IF(D_GruOlie_cv_57_58>0,ROUND(D_GruOlie_cv_57_58,3-(INT(LOG(D_GruOlie_cv_57_58))+1)),D_GruOlie_cv_57_58)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_57","v":0},{"$f":"D_gruolie_gvk_57","v":5},{"$f":"IF(D_Gruolie_c1_57_58>0,ROUND(D_Gruolie_c1_57_58,Gruolie_ciffer-(INT(LOG(D_Gruolie_c1_57_58))+1)),D_Gruolie_c1_57_58)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Gruolie_overskr1_57_58),ROUND(D_Gruolie_overskr1_57_58,Gruolie_ciffer-(INT(LOG(D_Gruolie_overskr1_57_58))+1)),\"\")","v":""},{"$f":"IF(D_GruOlie_c2_57_58>0,ROUND(D_GruOlie_c2_57_58,Gruolie_ciffer-(INT(LOG(D_GruOlie_c2_57_58))+1)),D_GruOlie_c2_57_58)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_GruOlie_C3_57_58>0,ROUND(D_GruOlie_C3_57_58,Gruolie_ciffer-(INT(LOG(D_GruOlie_C3_57_58))+1)),D_GruOlie_C3_57_58)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Gruolie_overskr_57_58),ROUND(D_Gruolie_overskr_57_58,3-(INT(LOG(D_Gruolie_overskr_57_58))+1)),\"\")","v":""}]
["Naphthalen",null,{"$f":"IF(D_gruolie_cv_103>0,ROUND(D_gruolie_cv_103,3-(INT(LOG(D_gruolie_cv_103))+1)),D_gruolie_cv_103)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_103","v":0},{"$f":"D_gruolie_gvk_103","v":1},{"$f":"IF(D_gruolie_c1_103>0,ROUND(D_gruolie_c1_103,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_103))+1)),D_gruolie_c1_103)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr1_103),ROUND(D_gruolie_overskr1_103,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr1_103))+1)),\"\")","v":""},{"$f":"IF(D_gruolie_c2_103>0,ROUND(D_gruolie_c2_103,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_103))+1)),D_gruolie_c2_103)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_103>0,ROUND(D_gruolie_c3_103,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_103))+1)),D_gruolie_c3_103)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr_103),ROUND(D_gruolie_overskr_103,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr_103))+1)),\"\")","v":""}]
[]
["Kulbrintefraktioner"]
["C6-C10",null,{"$f":"IF(D_gruolie_cv_510>0,ROUND(D_gruolie_cv_510,3-(INT(LOG(D_gruolie_cv_510))+1)),D_gruolie_cv_510)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_510","v":0},null,{"$f":"IF(D_gruolie_c1_510>0,ROUND(D_gruolie_c1_510,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_510))+1)),D_gruolie_c1_510)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_gruolie_c2_510>0,ROUND(D_gruolie_c2_510,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_510))+1)),D_gruolie_c2_510)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_510>0,ROUND(D_gruolie_c3_510,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_510))+1)),D_gruolie_c3_510)","v":{"$error":"#DIV/0!"}}]
["C10-C15",null,{"$f":"IF(D_gruolie_cv_1015>0,ROUND(D_gruolie_cv_1015,3-(INT(LOG(D_gruolie_cv_1015))+1)),D_gruolie_cv_1015)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_1015","v":0},null,{"$f":"IF(D_gruolie_c1_1015>0,ROUND(D_gruolie_c1_1015,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_1015))+1)),D_gruolie_c1_1015)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_gruolie_c2_1015>0,ROUND(D_gruolie_c2_1015,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_1015))+1)),D_gruolie_c2_1015)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_1015>0,ROUND(D_gruolie_c3_1015,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_1015))+1)),D_gruolie_c3_1015)","v":{"$error":"#DIV/0!"}}]
["C15-C20 ",null,{"$f":"IF(D_gruolie_cv_1520>0,ROUND(D_gruolie_cv_1520,3-(INT(LOG(D_gruolie_cv_1520))+1)),D_gruolie_cv_1520)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_1520","v":0},null,{"$f":"IF(D_gruolie_c1_1520>0,ROUND(D_gruolie_c1_1520,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_1520))+1)),D_gruolie_c1_1520)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_gruolie_c2_1520>0,ROUND(D_gruolie_c2_1520,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_1520))+1)),D_gruolie_c2_1520)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_1520>0,ROUND(D_gruolie_c3_1520,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_1520))+1)),D_gruolie_c3_1520)","v":{"$error":"#DIV/0!"}}]
["C20-C35",null,{"$f":"IF(D_gruolie_cv_2040>0,ROUND(D_gruolie_cv_2040,3-(INT(LOG(D_gruolie_cv_2040))+1)),D_gruolie_cv_2040)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_2040","v":0},null,{"$f":"IF(D_gruolie_c1_2040>0,ROUND(D_gruolie_c1_2040,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_2040))+1)),D_gruolie_c1_2040)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_gruolie_c2_2040>0,ROUND(D_gruolie_c2_2040,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_2040))+1)),D_gruolie_c2_2040)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_2040>0,ROUND(D_gruolie_c3_2040,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_2040))+1)),D_gruolie_c3_2040)","v":{"$error":"#DIV/0!"}}]
["Sum af kulbrinter",null,{"$f":"IF(D_Gruolie_cv_1>0,ROUND(D_Gruolie_cv_1,3-(INT(LOG(D_Gruolie_cv_1))+1)),D_Gruolie_cv_1)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_1","v":0},{"$f":"D_Gruolie_gvk_1","v":9},{"$f":"IF(D_Gruolie_c1_1>0,ROUND(D_Gruolie_c1_1,Gruolie_ciffer-(INT(LOG(D_Gruolie_c1_1))+1)),D_Gruolie_c1_1)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Gruolie_overskr1_1),ROUND(D_Gruolie_overskr1_1,Gruolie_ciffer-(INT(LOG(D_Gruolie_overskr1_1))+1)),D_Gruolie_overskr1_1)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Gruolie_c2_1>0,ROUND(D_Gruolie_c2_1,Gruolie_ciffer-(INT(LOG(D_Gruolie_c2_1))+1)),D_Gruolie_c2_1)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Gruolie_c3_1>0,ROUND(D_Gruolie_c3_1,Gruolie_ciffer-(INT(LOG(D_Gruolie_c3_1))+1)),D_Gruolie_c3_1)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_Gruolie_overskr_1),ROUND(D_Gruolie_overskr_1,Gruolie_ciffer-(INT(LOG(D_Gruolie_overskr_1))+1)),D_Gruolie_overskr_1)","v":{"$error":"#DIV/0!"}}]
[]
["Alkylbenzener"]
["C9-C10 aromatiske kulbrinter",null,{"$f":"IF(D_Gruolie_cv_910>0,ROUND(D_Gruolie_cv_910,3-(INT(LOG(D_Gruolie_cv_910))+1)),D_Gruolie_cv_910)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_1","v":0},{"$f":"D_GruOlie_gvk_910","v":1},{"$f":"IF(D_GruOlie_C1_910>0,ROUND(D_GruOlie_C1_910,Gruolie_ciffer-(INT(LOG(D_GruOlie_C1_910))+1)),D_GruOlie_C1_910)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_GruOlie_overskr1_910),ROUND(D_GruOlie_overskr1_910,Gruolie_ciffer-(INT(LOG(D_GruOlie_overskr1_910))+1)),D_GruOlie_overskr1_910)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_GruOlie_C2_910>0,ROUND(D_GruOlie_C2_910,Gruolie_ciffer-(INT(LOG(D_GruOlie_C2_910))+1)),D_GruOlie_C2_910)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_GruOlie_C3_910>0,ROUND(D_GruOlie_C3_910,Gruolie_ciffer-(INT(LOG(D_GruOlie_C3_910))+1)),D_GruOlie_C3_910)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_GruOlie_overskr_910),ROUND(D_GruOlie_overskr_910,Gruolie_ciffer-(INT(LOG(D_GruOlie_overskr_910))+1)),D_GruOlie_overskr_910)","v":{"$error":"#DIV/0!"}}]
[]
["Polyaromatiske Kulbrinter (PAH)"]
["Fluoranthen",null,{"$f":"IF(D_GruOlie_cv_156>0,ROUND(D_GruOlie_cv_156,3-(INT(LOG(D_GruOlie_cv_156))+1)),D_GruOlie_cv_156)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_156","v":0},{"$f":"D_GruOlie_gvk_156","v":0.1},{"$f":"IF(D_GruOlie_C1_156>0,ROUND(D_GruOlie_C1_156,Gruolie_ciffer-(INT(LOG(D_GruOlie_C1_156))+1)),D_GruOlie_C1_156)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_GruOlie_overskr1_156),ROUND(D_GruOlie_overskr1_156,Gruolie_ciffer-(INT(LOG(D_GruOlie_overskr1_156))+1)),D_GruOlie_overskr1_156)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_GruOlie_C2_156>0,ROUND(D_GruOlie_C2_156,Gruolie_ciffer-(INT(LOG(D_GruOlie_C2_156))+1)),D_GruOlie_C2_156)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_GruOlie_C3_156>0,ROUND(D_GruOlie_C3_156,Gruolie_ciffer-(INT(LOG(D_GruOlie_C3_156))+1)),D_GruOlie_C3_156)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_GruOlie_overskr_156),ROUND(D_GruOlie_overskr_156,Gruolie_ciffer-(INT(LOG(D_GruOlie_overskr_156))+1)),D_GruOlie_overskr_156)","v":{"$error":"#DIV/0!"}}]
["Benzo(a)pyren",null,{"$f":"IF(D_gruolie_cv_256>0,ROUND(D_gruolie_cv_256,3-(INT(LOG(D_gruolie_cv_256))+1)),D_gruolie_cv_256)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_1","v":0},{"$f":"D_gruolie_gvk_256","v":0.01},{"$f":"IF(D_gruolie_c1_256>0,ROUND(D_gruolie_c1_256,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_256))+1)),D_gruolie_c1_256)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr1_256),ROUND(D_gruolie_overskr1_256,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr1_256))+1)),D_gruolie_overskr1_256)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c2_256>0,ROUND(D_gruolie_c2_256,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_256))+1)),D_gruolie_c2_256)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_256>0,ROUND(D_gruolie_c3_256,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_256))+1)),D_gruolie_c3_256)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr_256),ROUND(D_gruolie_overskr_256,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr_256))+1)),D_gruolie_overskr_256)","v":{"$error":"#DIV/0!"}}]
["Sum af 4 PAH`er",null,{"$f":"IF(D_gruolie_cv_21>0,ROUND(D_gruolie_cv_21,3-(INT(LOG(D_gruolie_cv_21))+1)),D_gruolie_cv_21)","v":{"$error":"#DIV/0!"}},{"$f":"D_gruolie_nedkonst_21","v":0},{"$f":"D_gruolie_gvk_21","v":0.1},{"$f":"IF(D_gruolie_c1_21>0,ROUND(D_gruolie_c1_21,Gruolie_ciffer-(INT(LOG(D_gruolie_c1_21))+1)),D_gruolie_c1_21)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr1_21),ROUND(D_gruolie_overskr1_21,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr1_21))+1)),D_gruolie_overskr1_21)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c2_21>0,ROUND(D_gruolie_c2_21,Gruolie_ciffer-(INT(LOG(D_gruolie_c2_21))+1)),D_gruolie_c2_21)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_gruolie_c3_21>0,ROUND(D_gruolie_c3_21,Gruolie_ciffer-(INT(LOG(D_gruolie_c3_21))+1)),D_gruolie_c3_21)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISNUMBER(D_gruolie_overskr_21),ROUND(D_gruolie_overskr_21,Gruolie_ciffer-(INT(LOG(D_gruolie_overskr_21))+1)),D_gruolie_overskr_21)","v":{"$error":"#DIV/0!"}}]
[]
["NSO-forbindelser"]
["Sum af NSO-forbindelser",null,{"$f":"IF(D_Gruolie_cv_nso>0,ROUND(D_Gruolie_cv_nso,3-(INT(LOG(D_Gruolie_cv_nso))+1)),D_Gruolie_cv_nso)","v":{"$error":"#DIV/0!"}},{"$f":"D_Gruolie_nedkonst_NSO","v":0},null,{"$f":"IF(D_Gruolie_c1_nso>0,ROUND(D_Gruolie_c1_nso,Gruolie_ciffer-(INT(LOG(D_Gruolie_c1_nso))+1)),D_Gruolie_c1_nso)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_Gruolie_c2_nso>0,ROUND(D_Gruolie_c2_nso,Gruolie_ciffer-(INT(LOG(D_Gruolie_c2_nso))+1)),D_Gruolie_c2_nso)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Gruolie_c3_nso>0,ROUND(D_Gruolie_c3_nso,Gruolie_ciffer-(INT(LOG(D_Gruolie_c3_nso))+1)),D_Gruolie_c3_nso)","v":{"$error":"#DIV/0!"}}]
[]
["Beregningerne udført af",null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_GruOlie_DFO_Com <> \"\", D_GruOlie_DFO_Com, \"\")","v":""}]
["om det forurenede område"]
["(herunder nettonedbør)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_GruOlie_Mag_Com <> \"\", D_GruOlie_Mag_Com, \"\")","v":""}]
["om magasinparametre"]

{"sheet":"Vejledning_Grundvand-Olie","index":41,"n_rows":86,"n_cols":2,"rows_kept":86,"cut":false,"hidden":true,"merged":[[10,1,11,15],[1,1,1,15],[2,1,6,15],[7,1,7,15],[8,1,8,15],[9,1,9,15],[16,1,16,15],[17,1,17,15],[18,1,20,15],[12,1,12,15],[13,1,13,15],[14,1,15,15],[44,1,44,15],[21,1,21,15],[22,1,22,15],[27,1,27,15],[28,1,28,15],[29,1,31,14],[32,1,32,15],[34,1,39,15],[40,1,40,15],[41,1,41,15],[42,1,43,15],[83,1,83,15],[84,1,84,15],[85,1,86,15],[23,1,26,15],[69,1,70,15],[71,1,71,15],[72,1,72,15],[73,1,75,15],[77,1,77,15],[78,1,82,15],[45,1,53,15],[54,1,54,15],[55,1,55,15],[56,1,66,15],[67,1,67,15],[68,1,68,15]]}
[null,"Vejledning - Grundvand Oliestoffer"]
[null,"Formål"]
[null,"I dette regneark kan der foretages en beregning af konsekvenser for grundvand, jf. appendiks 5.6 i MST´s Oprydningsvejledning fra 1998, baseret på teoretiske porevands-koncentrationer for forurening med benzin- eller olie-blandinger. \n\nDer kan kun udføres beregninger baseret på kildestyrkekoncentrationen, dvs. trin 1A -beregning"]
[]
[]
[]
[]
[]
[null,"BEREGNINGER"]
[null,"Det forurenede areal - trin 1A:"]
[null,"Arealet og bredden af det forurenede område skal indtastes og der vælges enten nedbørs-data fra standardlisten, \"Egen liste\" eller indtastes egenværdier.\nDet er også muligt at anvende og oprette egne nedbørsdata."]
[]
[]
[null,"Det første betydende magasin:"]
[null,"Vælg aquifermateriale og indtast de hydrauliske parametre for det første betydende magasin, hvori risikoen skal beregnes."]
[]
[]
[null,"Forureningsdata - trin 1A:"]
[null,"Forureningsdata, dvs. de teoretiske porevandskoncentrationer for forurening med benzin- eller olieblandinger, er overført til grundvand-olie modulet og kan ikke ændres. Kun ved ændringer af jordkoncentrationer i \"Oliestoffer \"vil der også ske ændringer i de anvendte forureningsdata."]
[]
[]
[]
[null,"Nedbrydning i trin 3 :"]
[null,"Da der ikke foreligger nedbrydningsdata for de fleste af de repræsentative kulbrinte-fraktioner og modelstoffer, er nedbrydningskonstanterne sat til nul og de beregnede grundvandskoncentrationer i trin 3 er lig koncentrationerne i trin 2. I dataarket kan der dog aflæses en række parametre såsom retardations-koefficient, R, og gennemsnits-stofhastighed med sorption."]
[]
[]
[]
[]
[null,"GENERELT"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under Enkeltstof-modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under Enkeltstof-modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTVÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Indeklima-Olie","index":42,"n_rows":129,"n_cols":35,"rows_kept":129,"cut":false,"hidden":true,"merged":[[106,25,106,26],[112,25,112,26],[114,25,114,26],[125,25,125,26],[128,25,128,26],[102,28,102,29],[104,28,104,29],[106,28,106,29],[112,28,112,29],[114,28,114,29],[125,28,125,29],[128,28,128,29],[119,16,119,17],[121,16,121,17],[123,16,123,17],[110,22,110,23],[112,22,112,23],[114,22,114,23],[117,22,117,23],[119,22,119,23],[121,22,121,23],[123,22,123,23],[106,16,106,17],[108,16,108,17],[106,22,106,23],[108,22,108,23],[125,7,125,8],[128,7,128,8],[128,10,128,11],[125,16,125,17],[128,16,128,17],[125,22,125,23],[128,22,128,23],[123,7,123,8],[123,10,123,11],[114,13,114,14],[117,13,117,14],[119,13,119,14],[121,13,121,14],[123,13,123,14],[125,13,125,14],[128,13,128,14],[110,16,110,17],[112,16,112,17],[114,16,114,17],[117,16,117,17],[121,7,121,8],[121,10,121,11],[117,7,117,8],[117,10,117,11],[119,7,119,8],[119,10,119,11],[110,7,110,8],[112,7,112,8],[114,7,114,8],[114,10,114,11],[110,13,110,14],[112,13,112,14],[96,7,96,11],[101,7,101,8],[101,10,101,11],[103,10,103,11],[102,7,102,8],[104,7,104,8],[104,10,104,11],[104,13,104,14],[102,13,102,14],[98,6,100,9],[98,10,100,11],[101,13,101,14],[98,12,100,14],[106,7,106,8],[106,10,106,11],[108,7,108,8],[108,10,108,11],[106,13,106,14],[108,13,108,14],[102,16,102,17],[104,16,104,17],[102,22,102,23],[104,22,104,23],[84,10,84,11],[84,25,84,26],[84,28,84,29],[86,7,86,8],[86,10,86,11],[88,7,89,32],[91,7,91,11],[92,7,92,11],[94,7,94,11],[98,15,100,17],[101,16,101,17],[101,22,101,23],[98,22,100,23],[98,24,100,27],[98,28,100,29],[102,25,102,26],[104,25,104,26],[66,7,66,8],[66,10,66,11],[66,25,66,26],[66,28,66,29],[68,7,68,8],[68,10,68,11],[72,25,74,33],[76,7,76,11],[86,25,86,26],[78,10,78,11],[78,25,78,26],[78,28,78,29],[80,7,80,8],[80,10,80,11],[80,25,80,26],[80,28,80,29],[82,10,82,11],[82,25,82,26],[82,28,82,29],[61,25,61,26],[62,7,62,8],[62,10,62,11],[62,25,62,26],[62,28,62,29],[64,7,64,8],[64,10,64,11],[64,25,64,26],[64,28,64,29],[54,6,54,11],[56,7,56,8],[56,10,56,11],[58,7,58,8],[58,10,58,11],[58,25,58,26],[58,28,58,29],[59,25,59,26],[60,7,60,8],[60,10,60,11],[60,25,60,26],[60,28,60,29],[43,16,43,17],[44,16,44,17],[44,31,44,32],[49,7,51,31],[53,6,53,11],[40,25,42,26],[40,28,42,29],[40,31,42,32],[41,19,41,20],[40,5,41,8],[40,10,41,11],[40,13,41,14],[40,16,41,17],[40,19,40,20],[40,22,40,23],[41,22,41,23],[42,5,42,8],[42,10,42,11],[42,13,42,14],[42,16,42,17],[42,19,42,20],[42,22,42,23],[36,5,37,8],[36,10,37,11],[36,13,37,14],[36,16,37,17],[36,19,36,20],[36,22,36,23],[36,25,38,26],[36,28,38,29],[36,31,38,32],[37,19,37,20],[37,22,37,23],[38,5,38,8],[38,10,38,11],[38,13,38,14],[38,16,38,17],[38,19,38,20],[38,22,38,23],[32,5,33,8],[32,10,33,11],[32,13,33,14],[32,16,33,17],[32,19,32,20],[32,22,32,23],[32,25,34,26],[32,28,34,29],[32,31,34,32],[33,19,33,20],[33,22,33,23],[34,5,34,8],[34,10,34,11],[34,13,34,14],[34,16,34,17],[34,19,34,20],[34,22,34,23],[28,28,30,29],[28,31,30,32],[29,19,29,20],[29,22,29,23],[30,5,30,8],[30,10,30,11],[30,13,30,14],[30,16,30,17],[30,19,30,20],[28,25,30,26],[28,5,29,8],[28,10,29,11],[28,13,29,14],[28,16,29,17],[28,19,28,20],[28,22,28,23],[30,22,30,23],[22,28,24,29],[22,31,24,32],[23,19,23,20],[23,22,23,23],[24,5,24,8],[24,16,24,17],[18,5,19,8],[18,16,19,17],[18,18,19,19],[18,31,18,32],[19,31,19,32],[24,19,24,20],[24,22,24,23],[20,5,20,8],[20,16,20,17],[20,31,20,32],[22,5,23,8],[22,19,22,20],[22,22,22,23],[22,25,24,26],[131,7,131,29],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[12,8,14,32],[17,16,17,17],[17,19,17,20],[17,22,17,23],[17,25,17,26],[17,28,17,29],[15,10,16,11],[15,13,16,14],[15,16,16,17],[15,19,16,20],[15,22,16,23],[16,5,16,8],[15,27,16,30],[15,31,16,32],[15,25,16,26],[17,10,17,11],[17,13,17,14],[11,5,11,32]]}
["Beregning af indeklimakoncentration"]
["i bygning med terrændæk"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,"For krybekælder: benyt knap til højre"]
[]
[]
["Influenszone og membran",null,null,null,null,null,null,null,"Indtast data for evt. membran og kapilarbrydende lag og for jordlag mellem prøvetagningspunktet og bygningen. "]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Jordlag Dybde fra",null,null,"Jordlag Dybde til",null,null,"Lag-tykkelse",null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,"Volumen\naf jordskellet",null,null,null,"Materiale-konstant"]
[null,null,null,null,null,"Jordtype/Membran"]
[null,null,null,null,null,null,null,null,null,null,"m u.gulv",null,null,"m u.gulv",null,null,"(m)",null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ"]
[null,null,null,null,null,{"$f":"D_IndOlie_navnb_1_syst","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_Xb_1_syst","v":0},null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_Nb_1_int","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_Nb_1_syst","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOLie_b_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"D_IndOlie_navnb_2_syst","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_VLb_2_int","v":0},null,null,{"$f":"D_IndOlie_VVb_2_int","v":0},null,null,{"$f":"D_IndOlie_eb_2","v":0},null,null,{"$f":"D_IndOlie_VJb_2","v":1},null,null,{"$f":"D_IndOlie_Nb_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_VLb_2_syst","v":0},null,null,{"$f":"D_IndOlie_VVb_2_syst","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOLie_b_mangeljt_2","v":""}]
[]
["Jordparametre"]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlie_jordtype_1_syst<>\"\",D_IndOlie_jordtype_1_syst,\"\")","v":""},null,null,null,null,{"$f":"D_IndOlie_Xb_tot","v":0},null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_1_int<>\"\",D_IndOlie_VL_1_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_1_int<>\"\",D_IndOlie_VV_1_int,\"\")","v":""},null,null,{"$f":"D_IndOlie_e_1","v":0},null,null,{"$f":"D_IndOlie_VJ_1","v":1},null,null,{"$f":"D_IndOlie_N_1","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_1_syst<>\"\",D_IndOlie_VL_1_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_1_syst<>\"\",D_IndOlie_VV_1_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_X_1","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlie_jordtype_2_syst<>\"\",D_IndOlie_jordtype_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_2_int<>\"\",D_IndOlie_VL_2_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_2_int<>\"\",D_IndOlie_VV_2_int,\"\")","v":""},null,null,{"$f":"D_IndOlie_e_2","v":0},null,null,{"$f":"D_IndOlie_VJ_2","v":1},null,null,{"$f":"D_IndOlie_N_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_2_syst<>\"\",D_IndOlie_VL_2_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_2_syst<>\"\",D_IndOlie_VV_2_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_lagfra_2","v":0},null,null,null,null,null,{"$f":"D_IndOlie_X_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_mangeljt_2","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlie_jordtype_3_syst<>\"\",D_IndOlie_jordtype_3_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_3_int<>\"\",D_IndOlie_VL_3_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_3_int<>\"\",D_IndOlie_VV_3_int,\"\")","v":""},null,null,{"$f":"D_IndOlie_e_3","v":0},null,null,{"$f":"D_IndOlie_VJ_3","v":1},null,null,{"$f":"D_IndOlie_N_3","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_3_syst<>\"\",D_IndOlie_VL_3_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_3_syst<>\"\",D_IndOlie_VV_3_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_lagfra_3","v":0},null,null,null,null,null,{"$f":"D_IndOlie_X_3","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_mangeljt_3","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlie_jordtype_4_syst<>\"\",D_IndOlie_jordtype_4_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_4_int<>\"\",D_IndOlie_VL_4_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_4_int<>\"\",D_IndOlie_VV_4_int,\"\")","v":""},null,null,{"$f":"D_IndOlie_e_4","v":0},null,null,{"$f":"D_IndOlie_VJ_4","v":1},null,null,{"$f":"D_IndOlie_N_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlie_VL_4_syst<>\"\",D_IndOlie_VL_4_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlie_VV_4_syst<>\"\",D_IndOlie_VV_4_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_lagfra_4","v":0},null,null,null,null,null,{"$f":"D_IndOlie_X_4","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_mangeljt_4","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_negativ_X_tot","v":" "}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Samlede lagtykkelse",null,{"$f":"D_IndOlie_X_tot","v":0},null,"m for jordlag",null,null,null,null,null,null,null,null,null,null,"Samlet materialekonstant KW",null,{"$f":"D_IndOlie_N_tot","v":{"$error":"#DIV/0!"}}]
[]
["Bygningsdata"]
[]
[]
["Terrændæk",null,null,null,null,null,null,"Vælg type af terrændæk, eller indtast egen data"]
[]
[]
[]
["Type af terrændæk",null,null,null,null,null,{"$f":"IF(D_IndOlie_Inddæk_syst<>\"\",D_IndOlie_Inddæk_syst,\"\")","v":""}]
[]
[]
["Betontværsnit",null,null,null,null,"hb",null,{"$f":"IF(D_IndOlie_hb_syst<>\"\",D_IndOlie_hb_syst,\"\")","v":""},null,null,null,null,null,"mm"]
[]
["Relativ luftfugtighed",null,null,null,null,"RF",null,{"$f":"IF(D_IndOlie_RF_syst<>\"\",D_IndOlie_RF_syst,\"\")","v":""},null,null,null,null,null,"%",null,null,"Armeringsdiameter",null,null,null,null,null,null,"da",null,{"$f":"IF(D_IndOlie_daCh<>\"\",D_IndOlie_daCh,\"\")","v":""},null,null,null,null,null,"mm",null,"Ind_da"]
[]
["Vand/cement-tallet",null,null,null,null,"v/c",null,{"$f":"IF(D_IndOlie_wc_syst<>\"\",D_IndOlie_wc_syst,\"\")","v":""},null,null,null,null,null,null,null,null,"Armeringskonstant",null,null,null,null,null,null,"k",null,{"$f":"IF(D_IndOlie_k_syst<>\"\",D_IndOlie_k_syst,\"\")","v":""}]
[]
["Cementindhold",null,null,null,null,"CM",null,{"$f":"IF(D_IndOlie_CM_syst<>\"\",D_IndOlie_CM_syst,\"\")","v":""},null,null,null,null,null,"kg/m3",null,null,"Afstand mellem armeringsjern",null,null,null,null,null,null,"Db",null,{"$f":"IF(D_IndOlie_Db_syst<>\"\",D_IndOlie_Db_syst,\"\")","v":""},null,null,null,null,null,"mm"]
[]
["Svindtid",null,null,null,null,"ts",null,{"$f":"IF(D_IndOlie_ts_syst<>\"\",D_IndOlie_ts_syst,\"\")","v":""},null,null,null,null,null,"døgn",null,null,"Dynamisk viskositet af luft",null,null,null,null,null,null,"m",null,{"$f":"D_IndOlie_my_syst","v":1.8E-5},null,null,null,null,null,"kg/(m * s)"]
[]
["Elasticitetskoeff. Beton",null,null,null,null,"Eb",null,{"$f":"D_IndOlie_Eb_syst","v":20000},null,null,null,null,null,"MPa",null,null,"Elasticitetskoeff. Stål",null,null,null,null,null,null,"Es",null,{"$f":"D_IndOlie_Es_syst","v":210000},null,null,null,null,null,"MPa"]
[]
["Materialekonst. for beton",null,null,null,null,"Nb",null,{"$f":"IF(D_IndOlie_Nb_syst<>\"\",D_IndOlie_Nb_syst,\"\")","v":""}]
[]
[]
[]
["Bygningsdata",null,null,null,null,null,null,"Indtast bygnings data",null,null,null,null,null,null,null,null,"Beregnede bygningsdata",null,null,null,null,null,null,null,null,"Anvend beregnede bygningsdata,\neller indtast målte data"]
[]
[]
[]
["Rumtype/anvendelse"]
[]
["Loftshøjde",null,null,null,null,"Lh",null,null,null,null,null,null,null,"m",null,null,"Revnevidde",null,null,null,null,null,null,"w",null,{"$f":"D_IndOlie_w","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mm"]
[]
["Luftskifte",null,null,null,null,"Ls",null,{"$f":"D_IndOlie_Ls_Sys","v":8.2999999999999998E-5},null,null,null,null,null,"s-1",null,null,"Gnmsn. revneafstand",null,null,null,null,null,null,"lw",null,{"$f":"D_IndOlie_lw","v":{"$error":"#VALUE!"}},null,null,null,null,null,"mm"]
[]
["Gulvbredde",null,null,null,null,"lb",null,null,null,null,null,null,null,"m",null,null,"Total revnelængde",null,null,null,null,null,null,"ltot",null,{"$f":"D_IndOlie_ltot_ber","v":0},null,null,null,null,null,"m"]
[]
["Gulvlængde",null,null,null,null,"ll",null,null,null,null,null,null,null,"m",null,null,"Vol. strøm gennem beton",null,null,null,null,null,null,"qb",null,{"$f":"D_IndOlie_q","v":{"$error":"#VALUE!"}},null,null,null,null,null,"m³/(s · m²)"]
[]
["Trykforskel over betondæk",null,null,null,null,"DP",null,{"$f":"D_IndOlie_DP_Sys","v":5},null,null,null,null,null,"Pa",null,null,"Vol. strøm gennem beton pr. m²",null,null,null,null,null,null,"Qb",null,{"$f":"D_IndOlie_q/(IndOlie_My_Lb*IndOlie_My_Ll)","v":{"$error":"#VALUE!"}},null,null,null,null,null,"m³/(s · m²)"]
[]
["Beregning: indeluft",null,null,null,null,null,null,"Data for olieforureningen er overført fra fugacitetsmodulet \n"]
[]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"D_olie_målepunkt","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"D_olie_dato","v":""}]
[]
["Fri fase?",null,null,null,null,null,null,{"$f":"D_Olie_FF","v":"Nej"}]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"D_Udeolie_bruger","v":"Nej"}]
[]
[null,null,null,null,null,null,"Porelufts-\nkonc.",null,null,null,null,null,"Porelufts-\nkonc. under gulv",null,null,"Diffusivt bidrag til indeluft",null,null,null,null,null,null,"Totalt bidrag til indeluft",null,"Afdampnings-kriterium",null,null,null,"Overskri-delse af kriteriet"]
[]
[]
[null,null,null,null,null,null,null,"CL",null,null,null,null,null,"Cp",null,null,"Cdi",null,null,null,null,null,"Ci"]
[null,null,null,null,null,null,null,"mg/m³",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,"Gange"]
["BTEX'er"]
[null,"Benzen",null,null,null,null,null,{"$f":"D_IndOlie_52_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_52_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_52_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_52_ci","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_IndOlie_52_ak","v":1.2999999999999999E-4},null,null,{"$f":"D_IndOlie_omkr_52","v":{"$error":"#DIV/0!"}}]
[]
[null,"Toluen",null,null,null,null,null,{"$f":"D_IndOlie_54_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_54_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_54_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_54_ci","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_IndOlie_54_ak","v":0.4},null,null,{"$f":"D_IndOlie_omkr_54","v":{"$error":"#DIV/0!"}}]
[]
[null,"Ethylbenzen",null,null,null,null,null,{"$f":"D_IndOlie_58_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_58_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_58_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_58_ci","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum Xylener",null,null,null,null,null,{"$f":"D_IndOlie_57_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_57_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_57_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_57_ci","v":{"$error":"#DIV/0!"}}]
[]
[null,"∑Xylener+Ethylbenzen",null,null,null,null,null,{"$f":"D_IndOlie_59_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_59_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_59_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_59_ci","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_IndOlie_59_ak","v":0.1},null,null,{"$f":"D_IndOlie_omkr_59","v":{"$error":"#DIV/0!"}}]
[]
[null,"Naphtalen",null,null,null,null,null,{"$f":"D_IndOlie_103_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_103_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_103_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_103_ci","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_IndOlie_103_ak","v":0.04},null,null,{"$f":"D_IndOlie_omkr_103","v":{"$error":"#DIV/0!"}}]
[]
["Kulbrintefraktioner"]
[null,"C6-C10",null,null,null,null,null,{"$f":"D_IndOlie_510_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_510_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_510_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_510_ci","v":{"$error":"#DIV/0!"}}]
[]
[null,"C10-C15",null,null,null,null,null,{"$f":"D_IndOlie_1015_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_1015_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_1015_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_1015_ci","v":{"$error":"#DIV/0!"}}]
[]
[null,"C15-C20",null,null,null,null,null,{"$f":"D_IndOlie_1520_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_1520_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_1520_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_1520_ci","v":{"$error":"#DIV/0!"}}]
[]
[null,"C20-C35",null,null,null,null,null,{"$f":"D_IndOlie_2040_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_2040_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_2040_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_2040_ci","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af kulbrinter",null,null,null,null,null,{"$f":"D_IndOlie_1_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_1_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_1_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_1_ci","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_IndOlie_1_ak","v":0.1},null,null,{"$f":"D_IndOlie_omkr_1","v":{"$error":"#DIV/0!"}}]
[]
["Aromatiske kulbrinter "]
[null,"C9-C10 aromatiske kulbr.",null,null,null,null,null,{"$f":"D_IndOlie_910_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlie_910_cp","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_910_cdi","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlie_910_ci","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_IndOlie_910_ak","v":0.03},null,null,{"$f":"D_IndOlie_omkr_910","v":{"$error":"#DIV/0!"}}]

{"sheet":"Indeklima-Olie_Krybekælder","index":43,"n_rows":121,"n_cols":35,"rows_kept":121,"cut":false,"hidden":true,"merged":[[120,22,120,23],[120,25,120,26],[120,7,120,8],[120,10,120,11],[120,13,120,14],[117,7,117,8],[117,13,117,14],[120,19,120,20],[115,19,115,20],[117,19,117,20],[117,22,117,23],[117,25,117,26],[128,7,128,11],[128,13,128,17],[128,19,128,23],[128,25,128,29],[124,28,124,29],[126,7,126,11],[126,13,126,17],[126,19,126,23],[126,25,126,29],[124,7,124,26],[113,7,113,8],[113,10,113,11],[113,13,113,14],[113,19,113,20],[115,7,115,8],[115,10,115,11],[115,13,115,14],[104,7,104,8],[104,13,104,14],[104,19,104,20],[111,7,111,8],[111,10,111,11],[111,13,111,14],[111,19,111,20],[106,13,106,14],[106,19,106,20],[106,7,106,8],[106,10,106,11],[106,22,106,23],[106,25,106,26],[109,7,109,8],[109,10,109,11],[109,13,109,14],[109,19,109,20],[95,10,95,11],[80,7,81,32],[83,7,83,11],[84,7,84,11],[86,7,86,11],[88,7,88,11],[90,6,92,9],[90,10,92,11],[90,12,92,14],[90,19,92,20],[90,21,92,24],[90,25,92,26],[93,7,93,8],[93,13,93,14],[93,19,93,20],[94,7,94,8],[94,13,94,14],[94,19,94,20],[70,7,70,8],[94,22,94,23],[94,25,94,26],[93,10,93,11],[70,10,70,11],[72,7,72,8],[72,10,72,11],[74,7,74,8],[75,7,75,8],[75,10,75,11],[75,14,75,32],[77,14,77,33],[77,7,77,8],[44,31,44,32],[55,10,55,11],[57,10,57,11],[62,7,62,11],[66,10,66,11],[68,10,68,11],[64,7,64,8],[64,10,64,11],[68,7,68,8],[49,7,49,11],[51,10,51,11],[53,7,53,8],[53,10,53,11],[44,16,44,17],[32,28,34,29],[36,25,38,26],[36,28,38,29],[40,31,42,32],[41,19,41,20],[41,22,41,23],[42,5,42,8],[42,10,42,11],[42,13,42,14],[42,16,42,17],[42,19,42,20],[40,10,41,11],[40,13,41,14],[40,16,41,17],[40,19,40,20],[40,22,40,23],[42,22,42,23],[40,5,41,8],[40,25,42,26],[40,28,42,29],[38,22,38,23],[36,31,38,32],[37,19,37,20],[37,22,37,23],[38,5,38,8],[38,10,38,11],[38,13,38,14],[38,16,38,17],[38,19,38,20],[36,5,37,8],[36,10,37,11],[36,13,37,14],[36,16,37,17],[36,19,36,20],[36,22,36,23],[28,16,29,17],[28,19,28,20],[28,22,28,23],[30,22,30,23],[28,25,30,26],[33,22,33,23],[34,5,34,8],[34,10,34,11],[34,13,34,14],[34,16,34,17],[32,25,34,26],[32,31,34,32],[33,19,33,20],[25,31,25,32],[26,5,26,8],[26,16,26,17],[26,31,26,32],[20,5,21,8],[20,16,21,17],[20,31,21,32],[22,5,22,8],[22,16,22,17],[22,31,22,32],[28,28,30,29],[28,31,30,32],[29,19,29,20],[29,22,29,23],[30,5,30,8],[30,10,30,11],[30,13,30,14],[30,16,30,17],[30,19,30,20],[28,5,29,8],[28,10,29,11],[28,13,29,14],[18,25,18,26],[18,28,18,29],[16,10,17,11],[16,13,17,14],[16,16,17,17],[16,19,17,20],[16,22,17,23],[16,25,17,26],[24,31,24,32],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[24,5,25,8],[24,16,25,17],[34,19,34,20],[32,5,33,8],[32,10,33,11],[32,13,33,14],[32,16,33,17],[32,19,32,20],[32,22,32,23],[34,22,34,23],[11,5,11,32],[16,27,17,30],[16,31,17,32],[17,5,17,8],[18,10,18,11],[18,13,18,14],[18,16,18,17],[18,19,18,20],[18,22,18,23],[96,22,96,23],[96,25,96,26],[98,7,98,8],[98,10,98,11],[98,13,98,14],[98,19,98,20],[98,22,98,23],[98,25,98,26],[104,22,104,23],[104,25,104,26],[100,7,100,8],[100,10,100,11],[100,13,100,14],[100,19,100,20],[102,7,102,8],[102,13,102,14],[102,19,102,20],[96,7,96,8],[96,10,96,11],[96,13,96,14],[96,19,96,20]]}
["Beregning af indeklimakoncentration"]
["i bygning med krybekælder"]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,"Vælg terrændæk/kælder eller krybekælder"]
[]
[]
["Ventilleret krybekælder"]
[]
["Jordparametre og gulv i krybekælderen",null,null,null,null,null,null,null,null,null,null,null,"Indtast data om krybekælderens gulv og om jordlag"]
[]
[null,null,null,null,null,null,null,null,null,null,"Jordlag Dybde fra",null,null,"Jordlag Dybde til",null,null,"Lag-tykkelse",null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,"Volumen\naf jordskellet",null,null,null,"Materiale-konstant"]
[null,null,null,null,null,"Jordtype/Membran"]
[null,null,null,null,null,null,null,null,null,null,"m u.gulv",null,null,"m u.gulv",null,null,"(m)",null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ"]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlieK_navnb_1_syst<>\"\",D_IndOlieK_navnb_1_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_Xb_1_syst<>\"\",D_IndOlieK_Xb_1_syst,\"\")","v":""},null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_Nb_1_syst<>\"\",D_IndOlieK_Nb_1_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOLieK_b_mangeljt_1","v":""}]
[]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlieK_navnb_2_syst<>\"\",D_IndOlieK_navnb_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_Xb_2_syst<>\"\",D_IndOlieK_Xb_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_Nb_2_int<>\"\",D_IndOlieK_Nb_2_int,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_Nb_2_syst<>\"\",D_IndOlieK_Nb_2_syst,\"\")","v":""},null,null,{"$f":"D_IndOLieK_b_mangeljt_2","v":""}]
[]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlieK_jordtype_1_syst<>\"\",D_IndOlieK_jordtype_1_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_1_int<>\"\",D_IndOlieK_VL_1_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_1_int<>\"\",D_IndOlieK_VV_1_int,\"\")","v":""},null,null,{"$f":"D_IndOlieK_e_1","v":0},null,null,{"$f":"D_IndOlieK_VJ_1","v":1},null,null,{"$f":"D_IndOlieK_N_1","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_1_syst<>\"\",D_IndOlieK_VL_1_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_1_syst<>\"\",D_IndOlieK_VV_1_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlie_mangeljt_1","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_lagfra_1","v":0},null,null,null,null,null,{"$f":"D_IndOlieK_X_1","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_mangeljt_1","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlieK_jordtype_2_syst<>\"\",D_IndOlieK_jordtype_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_2_int<>\"\",D_IndOlieK_VL_2_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_2_int<>\"\",D_IndOlieK_VV_2_int,\"\")","v":""},null,null,{"$f":"D_IndOlieK_e_2","v":0},null,null,{"$f":"D_IndOlieK_VJ_2","v":1},null,null,{"$f":"D_IndOlieK_N_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_2_syst<>\"\",D_IndOlieK_VL_2_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_2_syst<>\"\",D_IndOlieK_VV_2_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_mangeljt_2","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_lagfra_2","v":0},null,null,null,null,null,{"$f":"D_IndOlieK_X_2","v":0}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlieK_jordtype_3_syst<>\"\",D_IndOlieK_jordtype_3_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_3_int<>\"\",D_IndOlieK_VL_3_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_3_int<>\"\",D_IndOlieK_VV_3_int,\"\")","v":""},null,null,{"$f":"D_IndOlieK_e_3","v":0},null,null,{"$f":"D_IndOlieK_VJ_3","v":1},null,null,{"$f":"D_IndOlieK_N_3","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_3_syst<>\"\",D_IndOlieK_VL_3_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_3_syst<>\"\",D_IndOlieK_VV_3_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_mangeljt_3","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_lagfra_3","v":0},null,null,null,null,null,{"$f":"D_IndOlieK_X_3","v":0}]
[]
[null,null,null,null,null,{"$f":"IF(D_IndOlieK_jordtype_4_syst<>\"\",D_IndOlieK_jordtype_4_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_4_int<>\"\",D_IndOlieK_VL_4_int,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_4_int<>\"\",D_IndOlieK_VV_4_int,\"\")","v":""},null,null,{"$f":"D_IndOlieK_e_4","v":0},null,null,{"$f":"D_IndOlieK_VJ_4","v":1},null,null,{"$f":"D_IndOlieK_N_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieK_VL_4_syst<>\"\",D_IndOlieK_VL_4_syst,\"\")","v":""},null,null,{"$f":"IF(D_IndOlieK_VV_4_syst<>\"\",D_IndOlieK_VV_4_syst,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_mangeljt_4","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_lagfra_4","v":0},null,null,null,null,null,{"$f":"D_IndOlieK_X_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_IndOlieK_negativ_X_tot","v":" "}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Samlede lagtykkelse",null,{"$f":"D_IndOlieK_X_tot","v":0},null,"m for jordlag",null,null,null,null,null,null,null,null,null,null,"Samlet materialekonstant KW",null,{"$f":"D_IndOlieK_N_tot","v":{"$error":"#DIV/0!"}}]
[]
[]
["Bygningsdata",null,null,null,null,null,null,"Alternativt Indtast bygningsdata"]
[]
["Rumtype/anvendelse"]
[]
["Loftshøjde",null,null,null,null,"Lh",null,null,null,null,null,null,"m"]
[]
["Luftskifte",null,null,null,null,"Ls",null,{"$f":"D_IndOlieK_Ls_syst","v":8.2999999999999998E-5},null,null,null,null,"s-1"]
[]
["Gulvbredde",null,null,null,null,"lb",null,null,null,null,null,null,"m"]
[]
["Gulvlængde",null,null,null,null,"ll",null,null,null,null,null,null,"m"]
[]
[]
["Data for krybekælder",null,null,null,null,null,null,"Indtast data om krybekælderen"]
[]
[null,null,null,null,null,null,null,{"$f":"IF(D_IndOlieKk_syst<>\"\",D_IndOlieKk_syst,\"\")","v":""}]
[]
["Reduktionsfaktoren",null,null,null,null,null,"Rkr",{"$f":"IF(ISNUMBER(D_IndOlieKk_Rkr_syst),D_IndOlieKk_Rkr_syst,\"\")","v":""}]
[]
["Loftshøjde",null,null,null,null,null,"Lh",null,null,null,null,null,"m"]
[]
["Gulvbredde",null,null,null,null,null,"lb",{"$f":"D_IndOlieK_Lb","v":0},null,null,null,null,"m"]
[]
["Gulvlængde",null,null,null,null,null,"ll",{"$f":"D_IndOlieK_Ll","v":0},null,null,null,null,"m"]
[]
["Luftskifte",null,null,null,null,null,"Ls",{"$f":"D_IndOlieKk_Ls_berg","v":{"$error":"#DIV/0!"}},null,null,null,null,"s-1"]
[]
["Vol. strøm gennem loft i"]
["krybekælderen",null,null,null,null,null,"qgv",{"$f":"D_IndOlieK_qgv_beregn","v":{"$error":"#DIV/0!"}},null,null,null,null,"m³/s",null,{"$f":"D_IndOlieK_q_check","v":{"$error":"#DIV/0!"}}]
[]
["Reduktionsfaktor beregn.",null,null,null,null,null,"Rkr",{"$f":"D_IndOlieKk_Rkr_bereg","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_IndOlieK_Rkr_check","v":{"$error":"#DIV/0!"}}]
[]
[]
["Beregning: indeluft",null,null,null,null,null,null,"Data for olieforureningen er overført fra fugacitetsmodulet \n"]
[]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"D_olie_målepunkt","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"D_olie_dato","v":""}]
[]
["Fri fase?",null,null,null,null,null,null,{"$f":"D_Olie_FF","v":"Nej"}]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"D_Udeolie_bruger","v":"Nej"}]
[]
[null,null,null,null,null,null,"Porelufts-\nkonc.",null,null,null,null,null,"Luftskonc. i krybe-kælderen",null,null,null,null,null,null,"Totalt bidrag til indeluft",null,"Afdampnings-kriterium",null,null,null,"Overskri-delse af kriteriet"]
[]
[]
[null,null,null,null,null,null,null,"CL",null,null,null,null,null,"Ckr",null,null,null,null,null,"Ci"]
[null,null,null,null,null,null,null,"mg/m³",null,null,null,null,null,"mg/m³",null,null,null,null,null,"mg/m³",null,null,"mg/m³",null,null,"Gange"]
["BTEX'er"]
[null,"Benzen",null,null,null,null,null,{"$f":"D_IndOlie_52_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_52_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_52_ci","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_52_ak","v":1.2999999999999999E-4},null,null,{"$f":"D_IndOlieK_omkr_52","v":{"$error":"#VALUE!"}}]
[]
[null,"Toluen",null,null,null,null,null,{"$f":"D_IndOlie_54_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_54_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_54_ci","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_54_ak","v":0.4},null,null,{"$f":"D_IndOlieK_omkr_54","v":{"$error":"#VALUE!"}}]
[]
[null,"Ethylbenzen",null,null,null,null,null,{"$f":"D_IndOlie_58_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_58_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_58_ci","v":{"$error":"#VALUE!"}}]
[]
[null,"Sum Xylener",null,null,null,null,null,{"$f":"D_IndOlie_57_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_57_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_57_ci","v":{"$error":"#VALUE!"}}]
[]
[null,"∑Xylener+Ethylbenzen",null,null,null,null,null,{"$f":"D_IndOlie_59_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_59_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_59_ci","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_59_ak","v":0.1},null,null,{"$f":"D_IndOlieK_omkr_59","v":{"$error":"#VALUE!"}}]
[]
[null,"Naphtalen",null,null,null,null,null,{"$f":"D_IndOlie_103_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_103_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_103_ci","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_103_ak","v":0.04},null,null,{"$f":"D_IndOlieK_omkr_103","v":{"$error":"#VALUE!"}}]
[]
["Kulbrintefraktioner"]
[null,"C6-C10",null,null,null,null,null,{"$f":"D_IndOlie_510_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_510_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_510_ci","v":{"$error":"#VALUE!"}}]
[]
[null,"C10-C15",null,null,null,null,null,{"$f":"D_IndOlie_1015_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_1015_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_1015_ci","v":{"$error":"#VALUE!"}}]
[]
[null,"C15-C20",null,null,null,null,null,{"$f":"D_IndOlie_1520_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_1520_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_1520_ci","v":{"$error":"#VALUE!"}}]
[]
[null,"C20-C35",null,null,null,null,null,{"$f":"D_IndOlie_2040_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_2040_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_2040_ci","v":{"$error":"#VALUE!"}}]
[]
[null,"Sum af kulbrinter",null,null,null,null,null,{"$f":"D_IndOlie_1_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_1_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_1_ci","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_1_ak","v":0.1},null,null,{"$f":"D_IndOlieK_omkr_1","v":{"$error":"#VALUE!"}}]
[]
["Aromatiske kulbrinter "]
[null,"C9-C10 aromatiske kulbr.",null,null,null,null,null,{"$f":"D_IndOlie_910_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"D_IndOlieK_910_ckr","v":{"$error":"#VALUE!"}},null,null,null,null,null,{"$f":"D_IndOlieK_910_ci","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_IndOlie_910_ak","v":0.03},null,null,{"$f":"D_IndOlieK_omkr_910","v":{"$error":"#VALUE!"}}]

{"sheet":"Dataark_Indeklima-Olie","index":44,"n_rows":325,"n_cols":27,"rows_kept":325,"cut":false,"hidden":true,"merged":[[47,10,47,11],[48,10,48,11],[1,1,1,23],[39,1,39,23],[41,1,41,23],[45,10,45,11],[46,10,46,11],[6,1,6,23],[8,4,8,7],[8,8,8,11],[21,1,21,23],[23,4,23,7],[23,8,23,11],[23,12,23,15],[23,16,23,19],[82,1,82,16],[49,10,49,11],[50,10,50,11],[59,1,59,23],[69,1,69,23],[238,1,238,16],[206,1,206,23],[216,1,216,23],[181,1,181,23],[183,1,183,23],[185,4,185,7],[185,8,185,11],[192,4,192,7],[192,8,192,11],[192,12,192,15],[192,16,192,19]]}
[]
[null,"Dataark - Indeklima-Olie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Terrændæk, kælder",true]
[null,"Krybekælder",false]
[]
[null,"Influenszone og membran"]
[]
[null,null,null,null,"Membran (1)",null,null,null,"Kapilarbrydende lag (2)"]
[null,null,"Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Navn",null,null,null,null,{"$f":"IndOlie_My_Memb","v":0},{"$f":"IF(ISTEXT(G11),G11,F11)","v":0},null,null,{"$f":"IndOlie_My_Kab_2","v":0},{"$f":"IF(ISTEXT(K11),K11,J11)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_navnb_n","Indput"]
[null,"Tykkelse af lag","Xb","m",null,null,{"$f":"IndOlie_My_Xb_1","v":0},{"$f":"IF(VALUE(G12),G12,F12)","v":0},null,null,{"$f":"IndOlie_My_Xb_2","v":0},{"$f":"K12","v":0},{"$f":"B_IndOlie_Xb_tot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Xb_n","Input/beregnes"]
[null,"Poreluftvolumen","VL",null,null,null,null,null,null,null,{"$f":"IndOlie_My_Kab_VL_2","v":0},{"$f":"IF(VALUE(K13),K13,J13)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_VLb_n","Indput"]
[null,"Vand-indhold","VV",null,null,null,null,null,null,null,{"$f":"IndOlie_My_Kab_VV_2","v":0},{"$f":"IF(VALUE(K14),K14,J14)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_VVb_n","Indput"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,null,null,null,null,null,{"$f":"B_IndOlie_eb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_eb_n","Indput"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,null,null,null,null,{"$f":"B_IndOlie_VJb_2","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_VJb_n","Indput"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,null,null,{"$f":"IndOlie_My_Nb_n","v":0},{"$f":"IF(VALUE(G17),G17,F17)","v":0},null,null,null,{"$f":"B_IndOlie_Nb_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Nb_n","Beregnes"]
[null,"Korigeret materialekonstant","N-kor",null,null,null,null,{"$f":"B_IndOlie_Nb_kor_1","v":1},null,null,null,{"$f":"B_IndOlie_Nb_kor_2","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Nb_kor_n","Beregnes"]
[null,"Check af manglende navn",null,null,null,null,null,{"$f":"IF(AND(D_IndOlie_Xb_1>0,D_IndOlie_navnb_1=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlie_Xb_2>0,D_IndOlie_navnb_2=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOLie_b_mangeljt_n","Beregnet i datalag"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,null,null,null,{"$f":"B_IndOlie_Nb_mel_1","v":0},null,null,null,{"$f":"B_IndOlie_Nb_mel_2","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Nb_mel_n","Beregnes"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,null,{"$f":"IndOlie_My_Jord1","v":0},{"$f":"IF(ISTEXT(G26),G26,F26)","v":0},null,null,{"$f":"IndOlie_My_Jord2","v":0},{"$f":"IF(ISTEXT(K26),K26,J26)","v":0},null,null,{"$f":"IndOlie_My_Jord3","v":0},{"$f":"IF(ISTEXT(O26),O26,N26)","v":0},null,null,{"$f":"IndOlie_My_Jord4","v":0},{"$f":"IF(ISTEXT(S26),S26,R26)","v":0},null,null,null,null,null,"D_IndOlie_jordtype_n","Indput"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,{"$f":"D_IndOlie_Xb_tot","v":0},{"$f":"IndOlie_Jord_df","v":0},{"$f":"IF(VALUE(G27),G27,F27)","v":0},null,{"$f":"D_IndOlie_lagtil_1","v":0},null,{"$f":"J27","v":0},null,{"$f":"D_IndOlie_lagtil_2","v":0},null,{"$f":"N27","v":0},null,{"$f":"D_IndOlie_lagtil_3","v":0},null,{"$f":"R27","v":0},null,null,null,null,null,"D_IndOlie_lagfra_n","Indput"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"IndOlie_Jord_dt1","v":0},{"$f":"G28","v":0},null,null,{"$f":"IndOlie_Jord_dt2","v":0},{"$f":"K28","v":0},null,null,{"$f":"IndOlie_Jord_dt3","v":0},{"$f":"O28","v":0},null,null,{"$f":"IndOlie_Jord_dt4","v":0},{"$f":"IF(VALUE(S28),S28,R28)","v":0},null,null,null,null,null,"D_IndOlie_lagtil_n","Indput"]
[null,"Tykkelse af jordlag","X","m",null,null,null,{"$f":"B_IndOlie_X_1","v":0},null,null,null,{"$f":"B_IndOlie_X_2","v":0},null,null,null,{"$f":"B_IndOlie_X_3","v":0},null,null,null,{"$f":"B_IndOlie_X_4","v":0},{"$f":"B_IndOlie_X_tot","v":0},null,null,null,null,"D_IndOlie_X_n","Beregnes"]
[null,"Check af negativ højde",null,null,null,null,null,{"$f":"B_IndOlie_negativ_X_1","v":0},null,null,null,{"$f":"B_IndOlie_negativ_X_2","v":0},null,null,null,{"$f":"B_IndOlie_negativ_X_3","v":0},null,null,null,{"$f":"B_IndOlie_negativ_X_4","v":0},{"$f":"B_IndOlie_negativ_X_tot","v":" "},null,null,null,null,"D_IndOlie_negativ_X_n","Input/beregnes"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"IndOlie_My_VL1","v":0},{"$f":"IF(VALUE(G31),G31,F31)","v":0},null,null,{"$f":"IndOlie_My_VL2","v":0},{"$f":"IF(VALUE(K31),K31,J31)","v":0},null,null,{"$f":"IndOlie_My_VL3","v":0},{"$f":"IF(VALUE(O31),O31,N31)","v":0},null,null,{"$f":"IndOlie_My_VL4","v":0},{"$f":"IF(VALUE(S31),S31,R31)","v":0},null,null,null,null,null,"D_IndOlie_VL_n","Indput"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"IndOlie_My_VV1","v":0},{"$f":"IF(VALUE(G32),G32,F32)","v":0},null,null,{"$f":"IndOlie_My_VV2","v":0},{"$f":"IF(VALUE(K32),K32,J32)","v":0},null,null,{"$f":"IndOlie_My_VV3","v":0},{"$f":"IF(VALUE(O32),O32,N32)","v":0},null,null,{"$f":"IndOlie_My_VV4","v":0},{"$f":"IF(VALUE(S32),S32,R32)","v":0},null,null,null,null,null,"D_IndOlie_VV_n","Indput"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,null,{"$f":"B_IndOlie_e_1","v":0},null,null,null,{"$f":"B_IndOlie_e_2","v":0},null,null,null,{"$f":"B_IndOlie_e_3","v":0},null,null,null,{"$f":"B_IndOlie_e_4","v":0},null,null,null,null,null,"D_IndOlie_e_n","Indput"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,{"$f":"B_IndOlie_VJ_1","v":1},null,null,null,{"$f":"B_IndOlie_VJ_2","v":1},null,null,null,{"$f":"B_IndOlie_VJ_3","v":1},null,null,null,{"$f":"B_IndOlie_VJ_4","v":1},null,null,null,null,null,"D_IndOlie_VJ_n","Indput"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,null,null,null,{"$f":"B_IndOlie_N_1","v":0},null,null,null,{"$f":"B_IndOlie_N_2","v":0},null,null,null,{"$f":"B_IndOlie_N_3","v":0},null,null,null,{"$f":"B_IndOlie_N_4","v":0},null,null,null,null,null,"D_IndOlie_N_n","Beregnes"]
[null,"Korigeret materialekonstant","N-kor",null,null,null,null,{"$f":"B_IndOlie_N_kor_1","v":1},null,null,null,{"$f":"B_IndOlie_N_kor_2","v":1},null,null,null,{"$f":"B_IndOlie_N_kor_3","v":1},null,null,null,{"$f":"B_IndOlie_N_kor_4","v":1},null,null,null,null,null,"D_IndOlie_N_kor_n","Beregnes"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,null,null,null,{"$f":"B_IndOlie_N_mel_1","v":0},null,null,null,{"$f":"B_IndOlie_N_mel_2","v":0},null,null,null,{"$f":"B_IndOlie_N_mel_3","v":0},null,null,null,{"$f":"B_IndOlie_N_mel_4","v":0},null,null,null,null,null,"D_IndOlie_N_mel_n","Beregnes"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,{"$f":"IF(AND(D_IndOlie_lagtil_1>0,D_IndOlie_jordtype_1=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlie_lagtil_2>0,D_IndOlie_jordtype_2=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlie_lagtil_3>0,D_IndOlie_jordtype_3=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlie_lagtil_4>0,D_IndOlie_jordtype_4=0),\"FEJL! Jordtype mangler\",\"\")","v":""},{"$f":"B_IndOlie_N_tot","v":{"$error":"#DIV/0!"}},null,null,null,null,"D_IndOlie_N_tot","Beregnes"]
[]
[null,"Bygningsdata"]
[]
[null,"Terrændæk"]
[]
[null,null,"Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Type af terrændæk",null,null,null,{"$f":"IndOlie_My_Inddæk","v":0},{"$f":"IF(ISTEXT(F45),F45,E45)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Inddæk","Indput"]
[null,"Betontværsnit","hb","mm",null,{"$f":"IndOlie_My_hb","v":0},{"$f":"IF(VALUE(F46),F46,E46)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_hb","Indput"]
[null,"Relativ luftfugtighed","RF","%",null,{"$f":"IndOlie_My_RF","v":0},{"$f":"IF(VALUE(F47),F47,E47)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_RF","Indput"]
[null,"Vand/cement-tallet","v/c",null,null,{"$f":"IndOlie_My_wc","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_wc","Indput"]
[null,"Cementindhold","CM","kg/m3",null,{"$f":"IndOlie_My_CM","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_CM","Indput"]
[null,"Svindtid","ts","døgn",null,{"$f":"IndOlie_My_ts","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_ts","Indput"]
[null,"Materialekonst. for beton","Nb",null,null,{"$f":"IndOlie_My_Nb","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Nb","Indput"]
[null,"Armeringsdiameter","da","mm",null,{"$f":"IndOlie_My_da","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_da","Indput"]
[null,"Armeringskonstant","k",null,null,{"$f":"IndOlie_My_k","v":0},0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_k","Indput"]
[null,"Afstand mellem armeringsjern","Db","mm",null,{"$f":"IF(VALUE(IndOlie_My_Db),IndOlie_My_Db,\"\")","v":""},{"$f":"IF(ISNUMBER(F54),F54,IF(ISNUMBER(E54),E54,\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Db","Indput"]
[null,"Dynamisk viskositet af luft","m","kg/(m * s)",1.8E-5,{"$f":"IndOlie_My_my","v":0},1.8E-5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_my","Indput"]
[null,"Elasticitetskoeff. Stål","Es","MPa",210000,{"$f":"IndOlie_My_Es","v":0},210000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Es","Indput"]
[null,"Elasticitetskoeff. Beton","Eb","MPa",20000,{"$f":"IndOlie_My_Eb","v":0},20000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Eb","Indput"]
[null,"Samlet materialekonstant for terrændæk og \ninfluenszone & membran (app. 5.3 lign 68B)","KN","m³/(m²·s)",null,null,{"$f":"B_IndOlie_Kn","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Kn","Beregnes"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Rumtype/anvendelse",null,null,null,{"$f":"IndOlie_My_anv","v":0},{"$f":"IF(ISTEXT(F63),F63,E63)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_anv","Indput"]
[null,"Loftshøjde","Lh","m",null,{"$f":"IndOlie_My_Lh","v":0},{"$f":"IF(VALUE(F64),F64,E64)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Lh","Indput"]
[null,"Luftskifte","Ls","s-1",8.2999999999999998E-5,{"$f":"IndOlie_My_Ls","v":0},{"$f":"IF(VALUE(F65),F65,E65)","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Ls","Indput"]
[null,"Gulvbredde","lb","m",null,{"$f":"IndOlie_My_Lb","v":0},{"$f":"IF(VALUE(F66),F66,E66)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Lb","Indput"]
[null,"Gulvlængde","ll","m",null,{"$f":"IndOlie_My_Ll","v":0},{"$f":"IF(VALUE(F67),F67,E67)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Ll","Indput"]
[null,"Trykforskel over betondæk","DP","Pa",5,{"$f":"IndOlie_My_DP","v":0},{"$f":"IF(VALUE(F68),F68,E68)","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_DP","Indput"]
[]
[null,"Beregnede bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Beregnet værdi","Indtastet","Anvendes"]
[null,"Revnevidde \n(app 5.3 lign. 73 eller MST nr. 7 1998 - lign 40)","w","mm",{"$f":"B_IndOlie_w_Ber","v":{"$error":"#VALUE!"}},{"$f":"IndOlie_My_w","v":0},{"$f":"IF(VALUE(F73),F73,E73)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_w","Input/beregnes"]
[null,"Basissvindet (MST nr. 7 1998 - lign 31)","ec","%",{"$f":"B_IndOlie_ec_Ber","v":5.3293413173652694E-2},null,{"$f":"D_IndOlie_ec_ber","v":5.3293413173652694E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_ec","Beregnes"]
[null,"Beton-sammensætningskoefficient \n(MST nr. 7 1998 - lign 32)","kb",null,{"$f":"B_IndOlie_Kb_Ber","v":0},null,{"$f":"D_IndOlie_Kb_ber","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Kb","Beregnes"]
[null,"Gnmsn. Revneafstand\n(MST nr. 7 1998 - lign 41+42)","lw","mm",{"$f":"B_IndOlie_lw_Ber","v":{"$error":"#VALUE!"}},{"$f":"IndOlie_My_Lw","v":0},{"$f":"IF(VALUE(F76),F76,E76)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_lw","Input/beregnes"]
[null,"Total revnelængde\n(app 5.3 lign. 72 eller MST nr. 7 1998 - lign 43)","ltot","m",{"$f":"B_IndOlie_ltot_Ber","v":0},{"$f":"IndOlie_My_ltot","v":0},{"$f":"IF(VALUE(F77),F77,E77)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_ltot","Input/beregnes"]
[null,"Vol. strøm gennem beton\n(app 5.3 lign. 70 eller MST nr. 7 1998 - lign 44)","qb","m³/(s )",{"$f":"B_IndOlie_q_Ber","v":{"$error":"#VALUE!"}},{"$f":"IndOlie_My_q","v":0},{"$f":"IF(VALUE(F78),F78,E78)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_q","Input/beregnes"]
[null,"Vol. strøm i bygningen","qbyg","m³/(s )",{"$f":"B_indOlie_qbyg_ber","v":0},null,{"$f":"D_IndOlie_qbyg_ber","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_qbyg","Beregnes"]
[null,"CHECK af volumenstrøm gennem beton","q_check","%",{"$f":"B_indOlie_qcheck_ber","v":{"$error":"#VALUE!"}},null,{"$f":"D_IndOlie_qcheck_ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_qcheck","Beregnes"]
[null,"Den frie svindtøjning\nMST nr. 7 1998 - lign 30 til lign36","eg","%",{"$f":"B_IndOlie_eg_Ber","v":{"$error":"#VALUE!"}},null,{"$f":"D_IndOlie_eg_ber","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_eg","Beregnes"]
[]
[null,"Oliestoffer"]
[]
[null,null,null,null,null,"Beregnet CL fra fugacitets\nmodul","Diffusionkoef. Luft","Totalt bidrag til indeluft (app. 53 ligning 77)","Poreluftkonc. under gulv (app. 53 ligning 78)","Diffusivt bidrag til indeluft  (app. 53 ligning 67A)","Afdamp-nings-kriterium","Overskridelse af kriteriet"]
[null,null,null,null,null,"CL","DL","Ci","Cp","Cdi"]
[null,null,null,null,null,"mg/m3","m2/s","mg/m³","mg/m³","mg/m³","mg/m³"]
[50,"C5-C6",null,null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!K90","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L90","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M90","v":{"$error":"#VALUE!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},{"$f":"'Beregning_Indeklima-Olie'!K91","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L91","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M91","v":{"$error":"#VALUE!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},{"$f":"'Beregning_Indeklima-Olie'!K92","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L92","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M92","v":{"$error":"#VALUE!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},{"$f":"'Beregning_Indeklima-Olie'!K93","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L93","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M93","v":{"$error":"#VALUE!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},{"$f":"'Beregning_Indeklima-Olie'!K94","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L94","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M94","v":{"$error":"#VALUE!"}}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K96","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L96","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M96","v":{"$error":"#VALUE!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},{"$f":"D_Ind_DL_1","v":0},{"$f":"'Beregning_Indeklima-Olie'!K97","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L97","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M97","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},{"$f":"IF(ISNUMBER(K95),IF(H95>K95,H95/K95,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},{"$f":"'Beregning_Indeklima-Olie'!K98","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L98","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M98","v":{"$error":"#VALUE!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},{"$f":"'Beregning_Indeklima-Olie'!K99","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L99","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M99","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_54_ak","v":0.4},{"$f":"IF(ISNUMBER(K97),IF(H97>K97,H97/K97,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["55A",">8 - 10, alifater",">8 - 10, alifater, Tung olie",null,null,{"$f":"D_Olie_55A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55A","v":5.5030901075876E-6},{"$f":"'Beregning_Indeklima-Olie'!K100","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L100","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M100","v":{"$error":"#VALUE!"}}]
["55B",null,">8 - 10, alifater, Olieblandinger",null,null,{"$f":"D_Olie_55B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55B","v":6.2232552378840063E-6},{"$f":"'Beregning_Indeklima-Olie'!K101","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L101","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M101","v":{"$error":"#VALUE!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},{"$f":"'Beregning_Indeklima-Olie'!K105","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L105","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M105","v":{"$error":"#VALUE!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},{"$f":"'Beregning_Indeklima-Olie'!K106","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L106","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M106","v":{"$error":"#VALUE!"}}]
[59,null,"Sum af xylener +ethylbenzen",null,null,{"$f":"D_Olie_57_cl+D_Olie_58_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K107","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L107","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M107","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_57_ak","v":0.1},{"$f":"IF(ISNUMBER(K105),IF(H105>K105,H105/K105,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["60A",null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"'Beregning_Indeklima-Olie'!K108","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L108","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M108","v":{"$error":"#VALUE!"}}]
["60B",null,">8 -10, aromater,øvrige",null,null,{"$f":"D_Olie_60_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_60B","v":6.4381431991356133E-6},{"$f":"'Beregning_Indeklima-Olie'!K109","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L109","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M109","v":{"$error":"#VALUE!"}}]
[910,"Sum C9-C10 aromater",null,null,null,{"$f":"D_Olie_60_cl+D_Olie_59_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K110","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L110","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M110","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_60_ak","v":0.03},{"$f":"IF(ISNUMBER(K108),IF(H108>K108,H108/K108,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K112","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L112","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M112","v":{"$error":"#VALUE!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},{"$f":"'Beregning_Indeklima-Olie'!K113","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L113","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M113","v":{"$error":"#VALUE!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},{"$f":"'Beregning_Indeklima-Olie'!K115","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L115","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M115","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_103_ak","v":0.04},{"$f":"IF(ISNUMBER(K113),IF(H113>K113,H113/K113,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["104A",null,">10 - 12, aromater, øvrige, Tung Olie",null,null,{"$f":"D_Olie_104A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104A","v":5.9633499312903359E-6},{"$f":"'Beregning_Indeklima-Olie'!K116","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L116","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M116","v":{"$error":"#VALUE!"}}]
["104B",null,">10 - 12, aromater, øvrige, Olieblanding",null,null,{"$f":"D_Olie_104B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104B","v":5.5260438461528997E-6},{"$f":"'Beregning_Indeklima-Olie'!K117","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L117","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M117","v":{"$error":"#VALUE!"}}]
["105A",null,">12 - 16, alifater, Tung Olie",null,null,{"$f":"D_Olie_105a_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105A","v":4.3460519456567218E-6},{"$f":"'Beregning_Indeklima-Olie'!K118","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L118","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M118","v":{"$error":"#VALUE!"}}]
["105B",">12 - 16, alifater",">12 - 16, alifater, Olieblandinger",null,null,{"$f":"D_Olie_105B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105B","v":5.0933919872504982E-6},{"$f":"'Beregning_Indeklima-Olie'!K119","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L119","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M119","v":{"$error":"#VALUE!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},{"$f":"'Beregning_Indeklima-Olie'!K121","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L121","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M121","v":{"$error":"#VALUE!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},{"$f":"'Beregning_Indeklima-Olie'!K122","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L122","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M122","v":{"$error":"#VALUE!"}}]
["109A",null,">12 - 16, aromater,øvrige, Tung Olie",null,null,{"$f":"D_Olie_109A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109A","v":5.5027929670196982E-6},{"$f":"'Beregning_Indeklima-Olie'!K123","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L123","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M123","v":{"$error":"#VALUE!"}}]
["109B",null,">12 - 16, aromater,øvrige, Olieblandinger",null,null,{"$f":"D_Olie_109B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109B","v":5.9000000000000003E-6},{"$f":"'Beregning_Indeklima-Olie'!K124","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L124","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M124","v":{"$error":"#VALUE!"}}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K126","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L126","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M126","v":{"$error":"#VALUE!"}}]
["151A",">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"D_Olie_151A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151A","v":3.7468864349159863E-6},{"$f":"'Beregning_Indeklima-Olie'!K127","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L127","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M127","v":{"$error":"#VALUE!"}}]
["151B",null,">16 - 21, alifater",null,null,{"$f":"D_Olie_151B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151B","v":4.4721099862171762E-6},{"$f":"'Beregning_Indeklima-Olie'!K128","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L128","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M128","v":{"$error":"#VALUE!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},{"$f":"'Beregning_Indeklima-Olie'!K130","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L130","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M130","v":{"$error":"#VALUE!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},{"$f":"'Beregning_Indeklima-Olie'!K131","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L131","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M131","v":{"$error":"#VALUE!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},{"$f":"'Beregning_Indeklima-Olie'!K132","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L132","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M132","v":{"$error":"#VALUE!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},{"$f":"'Beregning_Indeklima-Olie'!K133","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L133","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M133","v":{"$error":"#VALUE!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},{"$f":"'Beregning_Indeklima-Olie'!K134","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L134","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M134","v":{"$error":"#VALUE!"}}]
[]
[2025,"C21-C25",null,null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!K136","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L136","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M136","v":{"$error":"#VALUE!"}}]
["201A",">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"D_Olie_201A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201A","v":3.6715492605442101E-6},{"$f":"'Beregning_Indeklima-Olie'!K137","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L137","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M137","v":{"$error":"#VALUE!"}}]
["201B",null,">21 - 25, alifater",null,null,{"$f":"D_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201B","v":3.9528308464137552E-6},{"$f":"'Beregning_Indeklima-Olie'!K138","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L138","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M138","v":{"$error":"#VALUE!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter",null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!K139","v":0},{"$f":"'Beregning_Indeklima-Olie'!L139","v":0},{"$f":"'Beregning_Indeklima-Olie'!M139","v":0}]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K140","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L140","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M140","v":{"$error":"#VALUE!"}}]
["251A",">25 - 35, alifater",">25 - 35, alifater, Tung olie",null,null,{"$f":"D_Olie_251A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251A","v":3.0055777156880082E-6},{"$f":"'Beregning_Indeklima-Olie'!K141","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L141","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M141","v":{"$error":"#VALUE!"}}]
["251B",null,">25 - 35, alifater, Olieblandinger",null,null,{"$f":"D_Olie_251B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251B","v":3.6715492605442101E-6},{"$f":"'Beregning_Indeklima-Olie'!K142","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L142","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M142","v":{"$error":"#VALUE!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!K143","v":0},{"$f":"'Beregning_Indeklima-Olie'!L143","v":0},{"$f":"'Beregning_Indeklima-Olie'!M143","v":0}]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},{"$f":"'Beregning_Indeklima-Olie'!K144","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L144","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M144","v":{"$error":"#VALUE!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},{"$f":"'Beregning_Indeklima-Olie'!K145","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L145","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M145","v":{"$error":"#VALUE!"}}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},{"$f":"'Beregning_Indeklima-Olie'!K146","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L146","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M146","v":{"$error":"#VALUE!"}}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},{"$f":"'Beregning_Indeklima-Olie'!K147","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L147","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M147","v":{"$error":"#VALUE!"}}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},{"$f":"'Beregning_Indeklima-Olie'!K148","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L148","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M148","v":{"$error":"#VALUE!"}}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},{"$f":"'Beregning_Indeklima-Olie'!K149","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L149","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M149","v":{"$error":"#VALUE!"}}]
["259A",null,">25 - 35, aromater, øvrige, Tung olie",null,null,{"$f":"D_Olie_259A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259A","v":5.5943064295556175E-6},{"$f":"'Beregning_Indeklima-Olie'!K150","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L150","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M150","v":{"$error":"#VALUE!"}}]
["259B",null,">25 - 35, aromater, øvrige, Olieblandinger",null,null,{"$f":"D_Olie_259B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259B","v":4.4493993711079091E-6},{"$f":"'Beregning_Indeklima-Olie'!K151","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L151","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M151","v":{"$error":"#VALUE!"}}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K153","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L153","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M153","v":{"$error":"#VALUE!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},{"$f":"'Beregning_Indeklima-Olie'!K154","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L154","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M154","v":{"$error":"#VALUE!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},{"$f":"'Beregning_Indeklima-Olie'!K155","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L155","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M155","v":{"$error":"#VALUE!"}}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K157","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L157","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M157","v":{"$error":"#VALUE!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand"]
[]
[null,"NSO-forbindelser",null,null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!K162","v":0},{"$f":"'Beregning_Indeklima-Olie'!L162","v":0},{"$f":"'Beregning_Indeklima-Olie'!M162","v":0}]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},{"$f":"'Beregning_Indeklima-Olie'!K163","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L163","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M163","v":{"$error":"#VALUE!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},{"$f":"'Beregning_Indeklima-Olie'!K164","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L164","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M164","v":{"$error":"#VALUE!"}}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},{"$f":"'Beregning_Indeklima-Olie'!K165","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L165","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M165","v":{"$error":"#VALUE!"}}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},{"$f":"'Beregning_Indeklima-Olie'!K166","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L166","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M166","v":{"$error":"#VALUE!"}}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},{"$f":"'Beregning_Indeklima-Olie'!K167","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L167","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M167","v":{"$error":"#VALUE!"}}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},{"$f":"'Beregning_Indeklima-Olie'!K168","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L168","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M168","v":{"$error":"#VALUE!"}}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},{"$f":"'Beregning_Indeklima-Olie'!K169","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L169","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M169","v":{"$error":"#VALUE!"}}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!K171","v":{"$error":"#DIV/0!"}},{"$f":"'Beregning_Indeklima-Olie'!L171","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!M171","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"IF(ISNUMBER(K169),IF(H169>K169,H169/K169,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[]
[]
[]
[null,"Jordparametre:","D_IndOlie_Jord_Com"]
[null,null,{"$f":"IF(ISBLANK(D_IndOlie_Jord_Com),\"FALSE\",\"TRUE\")","v":"FALSE"}]
[null,"Influenszone og membran:","D_IndOlie_Inf_Com"]
[null,null,{"$f":"IF(ISBLANK(D_IndOlie_Inf_Com),\"FALSE\",\"TRUE\")","v":"FALSE"}]
[null,"Terrændæk:","D_IndOlie_Ter_Com"]
[null,null,{"$f":"IF(ISBLANK(D_IndOlie_Ter_Com),\"FALSE\",\"TRUE\")","v":"FALSE"}]
[null,"Bygningsdata:","D_IndOlie_Ind_Com"]
[null,null,{"$f":"IF(ISBLANK(D_IndOlie_Ind_Com),\"FALSE\",\"TRUE\")","v":"FALSE"}]
[]
[null," Indeklima-Olie Krybekælder"]
[]
[null,"Betongulv, membran og jord"]
[]
[null,null,null,null,"Betongulv (1)",null,null,null,"Membran (2)"]
[null,null,"Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Navn",null,null,null,null,{"$f":"IndOlieK_My_Gulv","v":0},{"$f":"IF(ISTEXT(G188),G188,F188)","v":0},null,null,{"$f":"IndOlieK_My_Memb","v":0},{"$f":"IF(ISTEXT(K188),K188,J188)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_navnb_n","Indput"]
[null,"Tykkelse af lag","Xb","m",null,null,{"$f":"IndOlieK_My_Xb_1","v":0},{"$f":"IF(VALUE(G189),G189,F189)","v":0},null,null,{"$f":"IndOlieK_My_Xb_2","v":0},{"$f":"IF(VALUE(K189),K189,J189)","v":0},{"$f":"B_IndOlieK_Xb_tot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Xb_n","Indput"]
[null,"Check af manglende navn",null,null,null,null,null,{"$f":"IF(AND(D_IndOlieK_Xb_1>0,D_IndOlieK_navnb_1=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlieK_Xb_2>0,D_IndOlieK_navnb_2=0),\"Fejl! Typeangivelse mangler\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOLieK_b_mangeljt_n","Beregnes i dataark"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,null,null,{"$f":"IndOlieK_My_Nb_1","v":0},{"$f":"IF(VALUE(G191),G191,F191)","v":0},null,null,{"$f":"IndOlieK_My_Nb_2","v":0},{"$f":"IF(VALUE(K191),K191,J191)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Nb_n","Indput"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,null,{"$f":"IndOlieK_My_Jord1","v":0},{"$f":"IF(ISTEXT(G195),G195,F195)","v":0},null,null,{"$f":"IndOlieK_My_Jord2","v":0},{"$f":"IF(ISTEXT(K195),K195,J195)","v":0},null,null,{"$f":"IndOlieK_My_Jord3","v":0},{"$f":"IF(ISTEXT(O195),O195,N195)","v":0},null,null,{"$f":"IndOlieK_My_Jord4","v":0},{"$f":"IF(ISTEXT(S195),S195,R195)","v":0},null,null,null,null,null,"D_IndOlieK_jordtype_n","Indput"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,{"$f":"B_IndOlieK_lagfra_1","v":0},null,{"$f":"IF(VALUE(G196),G196,F196)","v":0},null,{"$f":"B_IndOlieK_lagfra_2","v":0},null,{"$f":"J196","v":0},null,{"$f":"D_IndOlieK_lagtil_2","v":0},null,{"$f":"N196","v":0},null,{"$f":"D_IndOlieK_lagtil_3","v":0},null,{"$f":"R196","v":0},null,null,null,null,null,"D_IndOlieK_lagfra_n","beregnes"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"IndOlieK_Jord_dt1","v":0},{"$f":"G197","v":0},null,null,{"$f":"IndOlieK_Jord_dt2","v":0},{"$f":"K197","v":0},null,null,{"$f":"IndOlieK_Jord_dt3","v":0},{"$f":"O197","v":0},null,null,{"$f":"IndOlieK_Jord_dt4","v":0},{"$f":"IF(VALUE(S197),S197,R197)","v":0},null,null,null,null,null,"D_IndOlieK_lagtil_n","Indput"]
[null,"Tykkelse af jordlag","X","m",null,null,null,{"$f":"B_IndOlieK_X_1","v":0},null,null,null,{"$f":"B_IndOlieK_X_2","v":0},null,null,null,{"$f":"B_IndOlieK_X_3","v":0},null,null,null,{"$f":"B_IndOlieK_X_4","v":0},{"$f":"B_IndOlieK_X_tot","v":0},null,null,null,null,"D_IndOlieK_X_n","beregnes"]
[null,"Check af negativ højde",null,null,null,null,null,{"$f":"B_IndOlieK_negativ_X_1","v":0},null,null,null,{"$f":"B_IndOlieK_negativ_X_2","v":0},null,null,null,{"$f":"B_IndOlieK_negativ_X_3","v":0},null,null,null,{"$f":"B_IndOlieK_negativ_X_4","v":0},{"$f":"B_IndOlieK_negativ_X_tot","v":" "},null,null,null,null,"D_IndOlieK_negativ_X_n","beregnes"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"IndOlieK_My_VL1","v":0},{"$f":"IF(VALUE(G200),G200,F200)","v":0},null,null,{"$f":"IndOlieK_My_VL2","v":0},{"$f":"IF(VALUE(K200),K200,J200)","v":0},null,null,{"$f":"IndOlieK_My_VL3","v":0},{"$f":"IF(VALUE(O200),O200,N200)","v":0},null,null,{"$f":"IndOlieK_My_VL4","v":0},{"$f":"IF(VALUE(S200),S200,R200)","v":0},null,null,null,null,null,"D_IndOlieK_VL_n","Indput"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"IndOlieK_My_VV1","v":0},{"$f":"IF(VALUE(G201),G201,F201)","v":0},null,null,{"$f":"IndOlieK_My_VV2","v":0},{"$f":"IF(VALUE(K201),K201,J201)","v":0},null,null,{"$f":"IndOlieK_My_VV3","v":0},{"$f":"IF(VALUE(O201),O201,N201)","v":0},null,null,{"$f":"IndOlieK_My_VV4","v":0},{"$f":"IF(VALUE(S201),S201,R201)","v":0},null,null,null,null,null,"D_IndOlieK_VV_n","Indput"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,null,{"$f":"B_IndOlieK_e_1","v":0},null,null,null,{"$f":"B_IndOlieK_e_2","v":0},null,null,null,{"$f":"B_IndOlieK_e_3","v":0},null,null,null,{"$f":"B_IndOlieK_e_4","v":0},null,null,null,null,null,"D_IndOlieK_e_n","beregnes"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,{"$f":"B_IndOlieK_VJ_1","v":1},null,null,null,{"$f":"B_IndOlieK_VJ_2","v":1},null,null,null,{"$f":"B_IndOlieK_VJ_3","v":1},null,null,null,{"$f":"B_IndOlieK_VJ_4","v":1},null,null,null,null,null,"D_IndOlieK_VJ_n","beregnes"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,null,null,null,{"$f":"B_IndOlieK_N_1","v":0},null,null,null,{"$f":"B_IndOlieK_N_2","v":0},null,null,null,{"$f":"B_IndOlieK_N_3","v":0},null,null,null,{"$f":"B_IndOlieK_N_4","v":0},null,null,null,null,null,"D_IndOlieK_N_n","beregnes"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,{"$f":"IF(AND(D_IndOlieK_lagtil_1>0,D_IndOlieK_jordtype_1=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlieK_lagtil_2>0,D_IndOlieK_jordtype_2=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlieK_lagtil_3>0,D_IndOlieK_jordtype_3=0),\"FEJL! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_IndOlieK_lagtil_4>0,D_IndOlieK_jordtype_4=0),\"FEJL! Jordtype mangler\",\"\")","v":""},{"$f":"B_IndOlieK_N_tot","v":{"$error":"#DIV/0!"}},null,null,null,null,"D_IndOlieK_N_tot","Beregnes i dataark"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Systemværdi","Indtastet","Anvendes"]
[null,"Rumtype/anvendelse",null,null,null,{"$f":"IndOlieK_anv","v":0},{"$f":"IF(ISTEXT(F210),F210,E210)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_anv","Indput"]
[null,"Loftshøjde","Lh","m",null,{"$f":"IndOlieK_Lh","v":0},{"$f":"IF(VALUE(F211),F211,E211)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Lh","Indput"]
[null,"Luftskifte","Ls","s-1",8.2999999999999998E-5,{"$f":"IndOlieK_Ls","v":0},{"$f":"IF(VALUE(F212),F212,E212)","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Ls","Systemværdi"]
[null,"Gulvbredde","lb","m",null,{"$f":"IndOlieK_Lb","v":0},{"$f":"IF(VALUE(F213),F213,E213)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Lb","Indput"]
[null,"Gulvlængde","ll","m",null,{"$f":"IndOlieK_Ll","v":0},{"$f":"IF(VALUE(F214),F214,E214)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Ll","Indput"]
[null,"Volumenstrøm i beboelse","Qbeboelse","m³/s",{"$f":"B_IndOlieK_qbb","v":0},null,{"$f":"E215","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"beregnes"]
[]
[null,"Krybekælder"]
[]
[null,null,"Forkortelse","Enhed","Beregnet værdi","Indtastet","Anvendes"]
[null,"Etageadskillelse",null,null,null,null,{"$f":"IF(ISTEXT(F220),F220,E220)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_anv","Indput"]
[null,"Reduktionsfaktoren","Rkr",null,null,{"$f":"IndOlieKk_Rkr","v":0},{"$f":"IF(VALUE(F221),F221,E221)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_Rkr","Indput"]
[null,"Loftshøjde","Lh","m",null,{"$f":"IndOlieKk_Lh","v":0},{"$f":"F222","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_Lh","Indput"]
[null,"Gulvbredde","lb","m",{"$f":"D_IndOlieK_Lb","v":0},{"$f":"IndOlieKk_Lb","v":0},{"$f":"IF(VALUE(F223),F223,E223)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_Lb","Indput"]
[null,"Gulvlængde","ll","m",{"$f":"D_IndOlieK_Ll","v":0},{"$f":"IndOlieKk_Ll","v":0},{"$f":"IF(VALUE(F224),F224,E224)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_Ll","Indput"]
[null,"Luftskifte","Ls","m",{"$f":"B_IndOlieKk_Ls_berg","v":{"$error":"#DIV/0!"}},{"$f":"IndOlieKk_Ls","v":0},{"$f":"IF(VALUE(F225),F225,E225)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_Ls","beregnes"]
[null,"Vol. strøm gennem Krybekældergulv","qgv","m³/(s )",{"$f":"B_IndOlieK_qgv_berg","v":{"$error":"#DIV/0!"}},{"$f":"IndOlieK_qgv","v":0},{"$f":"IF(VALUE(F226),F226,E226)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_qgv","beregnes"]
[null,"Vol. strøm i krybekælderen","qbyg","m³/(s )",null,null,{"$f":"B_IndOlieKk_qbyg_berg","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_qbyg","beregnes"]
[null,"Check af volumenstrøm",null,null,null,null,{"$f":"B_IndOlieK_q_check","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_q_check","beregnes"]
[null,"Beregnet reduktionsfaktor","Rkr, beregnet",null,null,null,{"$f":"B_IndOlieKk_Rkr_bereg","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieKk_Rkr_bereg","beregnes"]
[null,"Check af reduktionsfaktor",null,null,null,null,{"$f":"B_IndOlieK_Rkr_check","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlieK_Rkr_check","beregnes"]
[]
[null,"Jordparametre:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Ven_Jord_Com","Input. Bemærkninger"]
[null,null,false]
[null,"Bygningsdata:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Ven_Byg_Com","Input. Bemærkninger"]
[null,null,false]
[null,"Krybekælderdata",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_IndOlie_Ven_Kryb_Com","Input. Bemærkninger"]
[null,null,false]
[]
[null,"Oliestoffer"]
[]
[null,null,null,null,null,"Beregnet CL fra fugacitets\nmodul","Diffusionkoef. Luft","Luftkoncen-trationen i krybekælder","Totalt bidrag til indeluft ","Afdamp-nings-kriterium","Overskridelse af kriteriet"]
[null,null,null,null,null,"CL","DL","Ckr","Ci"]
[null,null,null,null,null,"mg/m3","m2/s","mg/m³","mg/m³","mg/m³"]
[50,"C5-C6",null,null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!I232","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J232","v":{"$error":"#VALUE!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},{"$f":"'Beregning_Indeklima-Olie'!I233","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J233","v":{"$error":"#VALUE!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},{"$f":"'Beregning_Indeklima-Olie'!I234","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J234","v":{"$error":"#VALUE!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},{"$f":"'Beregning_Indeklima-Olie'!I235","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J235","v":{"$error":"#VALUE!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},{"$f":"'Beregning_Indeklima-Olie'!I236","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J236","v":{"$error":"#VALUE!"}}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I238","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J238","v":{"$error":"#VALUE!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},{"$f":"D_Ind_DL_1","v":0},{"$f":"'Beregning_Indeklima-Olie'!I239","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J239","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},{"$f":"IF(ISNUMBER(J251),IF(I251>J251,I251/J251,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},{"$f":"'Beregning_Indeklima-Olie'!I240","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J240","v":{"$error":"#VALUE!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},{"$f":"'Beregning_Indeklima-Olie'!I241","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J241","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_54_ak","v":0.4},{"$f":"IF(ISNUMBER(J253),IF(I253>J253,I253/J253,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
["55A",">8 - 10, alifater",">8 - 10, alifater, Tung olie",null,null,{"$f":"D_Olie_55A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55A","v":5.5030901075876E-6},{"$f":"'Beregning_Indeklima-Olie'!I242","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J242","v":{"$error":"#VALUE!"}}]
["55B",null,">8 - 10, alifater, Olieblandinger",null,null,{"$f":"D_Olie_55B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55B","v":6.2232552378840063E-6},{"$f":"'Beregning_Indeklima-Olie'!I243","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J243","v":{"$error":"#VALUE!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},{"$f":"'Beregning_Indeklima-Olie'!I247","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J247","v":{"$error":"#VALUE!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},{"$f":"'Beregning_Indeklima-Olie'!I248","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J248","v":{"$error":"#VALUE!"}}]
[59,null,"Sum af xylener +ethylbenzen",null,null,{"$f":"D_Olie_57_cl+D_Olie_58_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I249","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J249","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_57_ak","v":0.1},{"$f":"IF(ISNUMBER(J261),IF(I261>J261,I261/J261,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
["60A",null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"'Beregning_Indeklima-Olie'!I250","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J250","v":{"$error":"#VALUE!"}}]
["60B",null,">8 -10, aromater,øvrige",null,null,{"$f":"D_Olie_60_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_60B","v":6.4381431991356133E-6},{"$f":"'Beregning_Indeklima-Olie'!I251","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J251","v":{"$error":"#VALUE!"}}]
[910,"Sum C9-C10 aromater",null,null,null,{"$f":"D_Olie_60_cl+D_Olie_59_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I252","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J252","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_60_ak","v":0.03},{"$f":"IF(ISNUMBER(J264),IF(I264>J264,I264/J264,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
[]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I254","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J254","v":{"$error":"#VALUE!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},{"$f":"'Beregning_Indeklima-Olie'!I255","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J255","v":{"$error":"#VALUE!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},{"$f":"'Beregning_Indeklima-Olie'!I257","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J257","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_103_ak","v":0.04},{"$f":"IF(ISNUMBER(J269),IF(I269>J269,I269/J269,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
["104A",null,">10 - 12, aromater, øvrige, Tung Olie",null,null,{"$f":"D_Olie_104A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104A","v":5.9633499312903359E-6},{"$f":"'Beregning_Indeklima-Olie'!I258","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J258","v":{"$error":"#VALUE!"}}]
["104B",null,">10 - 12, aromater, øvrige, Olieblanding",null,null,{"$f":"D_Olie_104B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104B","v":5.5260438461528997E-6},{"$f":"'Beregning_Indeklima-Olie'!I259","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J259","v":{"$error":"#VALUE!"}}]
["105A",null,">12 - 16, alifater, Tung Olie",null,null,{"$f":"D_Olie_105a_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105A","v":4.3460519456567218E-6},{"$f":"'Beregning_Indeklima-Olie'!I260","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J260","v":{"$error":"#VALUE!"}}]
["105B",">12 - 16, alifater",">12 - 16, alifater, Olieblandinger",null,null,{"$f":"D_Olie_105B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105B","v":5.0933919872504982E-6},{"$f":"'Beregning_Indeklima-Olie'!I261","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J261","v":{"$error":"#VALUE!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},{"$f":"'Beregning_Indeklima-Olie'!I263","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J263","v":{"$error":"#VALUE!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},{"$f":"'Beregning_Indeklima-Olie'!I264","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J264","v":{"$error":"#VALUE!"}}]
["109A",null,">12 - 16, aromater,øvrige, Tung Olie",null,null,{"$f":"D_Olie_109A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109A","v":5.5027929670196982E-6},{"$f":"'Beregning_Indeklima-Olie'!I265","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J265","v":{"$error":"#VALUE!"}}]
["109B",null,">12 - 16, aromater,øvrige, Olieblandinger",null,null,{"$f":"D_Olie_109B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109B","v":5.9000000000000003E-6},{"$f":"'Beregning_Indeklima-Olie'!I266","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J266","v":{"$error":"#VALUE!"}}]
[]
[1520,"C16-C20","Reflab4",null,null,{"$f":"D_Olie_1520_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I268","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J268","v":{"$error":"#VALUE!"}}]
["151A",">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"D_Olie_151A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151A","v":3.7468864349159863E-6},{"$f":"'Beregning_Indeklima-Olie'!I269","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J269","v":{"$error":"#VALUE!"}}]
["151B",null,">16 - 21, alifater",null,null,{"$f":"D_Olie_151B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151B","v":4.4721099862171762E-6},{"$f":"'Beregning_Indeklima-Olie'!I270","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J270","v":{"$error":"#VALUE!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},{"$f":"'Beregning_Indeklima-Olie'!I272","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J272","v":{"$error":"#VALUE!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},{"$f":"'Beregning_Indeklima-Olie'!I273","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J273","v":{"$error":"#VALUE!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},{"$f":"'Beregning_Indeklima-Olie'!I274","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J274","v":{"$error":"#VALUE!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},{"$f":"'Beregning_Indeklima-Olie'!I275","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J275","v":{"$error":"#VALUE!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},{"$f":"'Beregning_Indeklima-Olie'!I276","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J276","v":{"$error":"#VALUE!"}}]
[]
[2025,"C21-C25",null,null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!I278","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J278","v":{"$error":"#VALUE!"}}]
["201A",">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"D_Olie_201A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201A","v":3.6715492605442101E-6},{"$f":"'Beregning_Indeklima-Olie'!I279","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J279","v":{"$error":"#VALUE!"}}]
["201B",null,">21 - 25, alifater",null,null,{"$f":"D_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201B","v":3.9528308464137552E-6},{"$f":"'Beregning_Indeklima-Olie'!I280","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J280","v":{"$error":"#VALUE!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter",null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!I281","v":0},{"$f":"'Beregning_Indeklima-Olie'!J281","v":0}]
[2535,"C25-C35","VKI",null,null,{"$f":"D_Olie_2535_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I282","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J282","v":{"$error":"#VALUE!"}}]
["251A",">25 - 35, alifater",">25 - 35, alifater, Tung olie",null,null,{"$f":"D_Olie_251A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251A","v":3.0055777156880082E-6},{"$f":"'Beregning_Indeklima-Olie'!I283","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J283","v":{"$error":"#VALUE!"}}]
["251B",null,">25 - 35, alifater, Olieblandinger",null,null,{"$f":"D_Olie_251B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251B","v":3.6715492605442101E-6},{"$f":"'Beregning_Indeklima-Olie'!I284","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J284","v":{"$error":"#VALUE!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,{"$f":"'Beregning_Indeklima-Olie'!I285","v":0},{"$f":"'Beregning_Indeklima-Olie'!J285","v":0}]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},{"$f":"'Beregning_Indeklima-Olie'!I286","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J286","v":{"$error":"#VALUE!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},{"$f":"'Beregning_Indeklima-Olie'!I287","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J287","v":{"$error":"#VALUE!"}}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},{"$f":"'Beregning_Indeklima-Olie'!I288","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J288","v":{"$error":"#VALUE!"}}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},{"$f":"'Beregning_Indeklima-Olie'!I289","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J289","v":{"$error":"#VALUE!"}}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},{"$f":"'Beregning_Indeklima-Olie'!I290","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J290","v":{"$error":"#VALUE!"}}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},{"$f":"'Beregning_Indeklima-Olie'!I291","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J291","v":{"$error":"#VALUE!"}}]
["259A",null,">25 - 35, aromater, øvrige, Tung olie",null,null,{"$f":"D_Olie_259A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259A","v":5.5943064295556175E-6},{"$f":"'Beregning_Indeklima-Olie'!I292","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J292","v":{"$error":"#VALUE!"}}]
["259B",null,">25 - 35, aromater, øvrige, Olieblandinger",null,null,{"$f":"D_Olie_259B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259B","v":4.4493993711079091E-6},{"$f":"'Beregning_Indeklima-Olie'!I293","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J293","v":{"$error":"#VALUE!"}}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I295","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J295","v":{"$error":"#VALUE!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},{"$f":"'Beregning_Indeklima-Olie'!I296","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J296","v":{"$error":"#VALUE!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},{"$f":"'Beregning_Indeklima-Olie'!I297","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J297","v":{"$error":"#VALUE!"}}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I299","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J299","v":{"$error":"#VALUE!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand"]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},{"$f":"'Beregning_Indeklima-Olie'!I305","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J305","v":{"$error":"#VALUE!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},{"$f":"'Beregning_Indeklima-Olie'!I306","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J306","v":{"$error":"#VALUE!"}}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},{"$f":"'Beregning_Indeklima-Olie'!I307","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J307","v":{"$error":"#VALUE!"}}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},{"$f":"'Beregning_Indeklima-Olie'!I308","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J308","v":{"$error":"#VALUE!"}}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},{"$f":"'Beregning_Indeklima-Olie'!I309","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J309","v":{"$error":"#VALUE!"}}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},{"$f":"'Beregning_Indeklima-Olie'!I310","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J310","v":{"$error":"#VALUE!"}}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},{"$f":"'Beregning_Indeklima-Olie'!I311","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J311","v":{"$error":"#VALUE!"}}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"'Beregning_Indeklima-Olie'!I313","v":{"$error":"#VALUE!"}},{"$f":"'Beregning_Indeklima-Olie'!J313","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"'Beregning_Indeklima-Olie'!L313","v":{"$error":"#VALUE!"}}]

{"sheet":"Beregning_Indeklima-Olie","index":45,"n_rows":313,"n_cols":18,"rows_kept":313,"cut":false,"hidden":true,"merged":[[226,1,226,16],[211,1,211,15],[185,4,185,5],[185,6,185,7],[185,8,185,9],[185,10,185,11],[201,1,201,15],[172,1,172,23],[173,1,173,15],[175,4,175,5],[175,6,175,7],[183,1,183,15],[1,1,1,15],[3,1,3,15],[5,4,5,5],[5,6,5,7],[17,1,17,15],[44,11,44,12],[19,4,19,5],[19,6,19,7],[19,8,19,9],[19,10,19,11],[35,1,35,15],[37,1,37,15],[41,11,41,12],[42,11,42,12],[43,11,43,12],[84,1,84,16],[45,11,45,12],[46,11,46,12],[56,1,56,15],[66,1,66,15]]}
[]
[null,"Beregning - Indeklima-Olie",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn"]
[]
[null,"Influenszone og membran"]
[]
[null,null,null,null,"Membran (1)",null,"Kapilarbrydende lag (2)"]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Navn",null,null,{"$f":"D_IndOlie_navnb_1","v":0},null,{"$f":"D_IndOlie_navnb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_IndOlie_navnb_n"]
[null,"Tykkelse af lag","Xb","m",{"$f":"D_IndOlie_Xb_1","v":0},{"$f":"E9/1000","v":0},{"$f":"D_IndOlie_Xb_2","v":0},null,{"$f":"B_IndOlie_Xb_1+B_IndOlie_Xb_2","v":0},null,null,null,null,null,null,null,null,"B_IndOlie_Xb_n"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"D_IndOlie_VLb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_IndOlie_VLb_n"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"D_IndOlie_VVb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_IndOlie_VVb_n"]
[null,"Samlet porøsitet","e=VL+VV",null,null,null,{"$f":"H12","v":0},{"$f":"B_IndOlie_VLb_2+B_IndOlie_VVb_2","v":0},null,null,null,null,null,null,null,null,null,"B_IndOlie_eb_n"]
[null,"Volumen af jordskellet","VJ",null,null,null,{"$f":"H13","v":1},{"$f":"1-B_IndOlie_eb_2","v":1},null,null,null,null,null,null,null,null,null,"B_IndOlie_VJb_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,{"$f":"D_IndOlie_Nb_1","v":0},null,{"$f":"H14","v":0},{"$f":"IF((B_IndOlie_eb_2)=0,0,((B_IndOlie_VLb_2)^2.5)/(B_IndOlie_eb_2))","v":0},null,null,null,null,null,null,null,null,null,"B_IndOlie_Nb_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F15","v":1},{"$f":"IF((B_IndOlie_Nb_1)=0,1,(B_IndOlie_Nb_1))","v":1},{"$f":"H15","v":1},{"$f":"IF((B_IndOlie_Nb_2)=0,1,(B_IndOlie_Nb_2))","v":1},null,null,null,null,null,null,null,null,null,"B_IndOlie_Nb_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F16","v":0},{"$f":"B_IndOlie_Xb_1*B_IndOlie_N_kor_1*B_IndOlie_N_kor_2*B_IndOlie_N_kor_3*B_IndOlie_N_kor_4*B_IndOlie_Nb_kor_2","v":0},{"$f":"H16","v":0},{"$f":"B_IndOlie_Xb_2*B_IndOlie_N_kor_1*B_IndOlie_N_kor_2*B_IndOlie_N_kor_3*B_IndOlie_N_kor_4*B_IndOlie_Nb_kor_1","v":0},null,null,null,null,null,null,null,null,null,"B_IndOlie_Nb_mel_n"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Jordtype",null,null,{"$f":"D_IndOlie_jordtype_1","v":0},null,{"$f":"D_IndOlie_jordtype_2","v":0},null,{"$f":"D_IndOlie_jordtype_3","v":0},null,{"$f":"D_IndOlie_jordtype_4","v":0},null,null,null,null,null,null,"B_IndOlie_jordtype_n"]
[null,"Jordlag, Dybde fra","x1","m u.t.",{"$f":"D_IndOlie_lagfra_1","v":0},null,{"$f":"D_IndOlie_lagfra_2","v":0},null,{"$f":"D_IndOlie_lagfra_3","v":0},null,{"$f":"D_IndOlie_lagfra_4","v":0},null,null,null,null,null,null,"B_IndOlie_lagfra_n"]
[null,"Jordlag, Dybde til","x2","m u.t.",{"$f":"D_IndOlie_lagtil_1","v":0},null,{"$f":"D_IndOlie_lagtil_2","v":0},null,{"$f":"D_IndOlie_lagtil_3","v":0},null,{"$f":"D_IndOlie_lagtil_4","v":0},null,null,null,null,null,null,"B_IndOlie_lagtil_n"]
[null,"Tykkelse af jordlag","X","m",{"$f":"F25","v":0},{"$f":"IF(ISNUMBER(IndOlie_Jord_dt1),B_IndOlie_lagtil_1-B_IndOlie_lagfra_1,0)","v":0},{"$f":"H25","v":0},{"$f":"IF(ISNUMBER(IndOlie_Jord_dt2),B_IndOlie_lagtil_2-B_IndOlie_lagfra_2,0)","v":0},{"$f":"J25","v":0},{"$f":"IF(ISNUMBER(IndOlie_Jord_dt3),B_IndOlie_lagtil_3-B_IndOlie_lagfra_3,0)","v":0},{"$f":"L25","v":0},{"$f":"IF(ISNUMBER(IndOlie_Jord_dt4),B_IndOlie_lagtil_4-B_IndOlie_lagfra_4,0)","v":0},{"$f":"B_IndOlie_X_1+B_IndOlie_X_2+B_IndOlie_X_3+B_IndOlie_X_4+B_IndOlie_Xb_tot","v":0},null,null,null,null,"B_IndOlie_X_n"]
[null,"Check af negativ højde",null,null,{"$f":"F26","v":0},{"$f":"IF(B_IndOlie_X_1<0,1,0)","v":0},{"$f":"H26","v":0},{"$f":"IF(B_IndOlie_X_2<0,1,0)","v":0},{"$f":"J26","v":0},{"$f":"IF(B_IndOlie_X_2<0,1,0)","v":0},{"$f":"L26","v":0},{"$f":"IF(B_IndOlie_X_2<0,1,0)","v":0},{"$f":"IF(B_IndOlie_negativ_X_1+B_IndOlie_negativ_X_2+B_IndOlie_negativ_X_3+B_IndOlie_negativ_X_4>0,\"FEJL!! Der er jordlag med negativ højde\",\" \")","v":" "},null,null,null,null,"B_IndOlie_negativ_X_n"]
[null,"Poreluftvolumen","VL",null,{"$f":"D_IndOlie_VL_1","v":0},null,{"$f":"D_IndOlie_VL_2","v":0},null,{"$f":"D_IndOlie_VL_3","v":0},null,{"$f":"D_IndOlie_VL_4","v":0},null,null,null,null,null,null,"B_IndOlie_VL_n"]
[null,"Vand-indhold","VV",null,{"$f":"D_IndOlie_VV_1","v":0},null,{"$f":"D_IndOlie_VV_2","v":0},null,{"$f":"D_IndOlie_VV_3","v":0},null,{"$f":"D_IndOlie_VV_4","v":0},null,null,null,null,null,null,"B_IndOlie_VV_n"]
[null,"Samlet porøsitet","e=VL+VV",null,{"$f":"F29","v":0},{"$f":"B_IndOlie_VL_1+B_IndOlie_VV_1","v":0},{"$f":"H29","v":0},{"$f":"B_IndOlie_VL_2+B_IndOlie_VV_2","v":0},{"$f":"J29","v":0},{"$f":"B_IndOlie_VL_3+B_IndOlie_VV_3","v":0},{"$f":"L29","v":0},{"$f":"B_IndOlie_VL_1+B_IndOlie_VV_1","v":0},null,null,null,null,null,"B_IndOlie_e_n"]
[null,"Volumen af jordskellet","VJ",null,{"$f":"F30","v":1},{"$f":"1-B_IndOlie_e_1","v":1},{"$f":"H30","v":1},{"$f":"1-B_IndOlie_e_2","v":1},{"$f":"J30","v":1},{"$f":"1-B_IndOlie_e_3","v":1},{"$f":"L30","v":1},{"$f":"1-B_IndOlie_e_4","v":1},null,null,null,null,null,"B_IndOlie_VJ_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,{"$f":"F31","v":0},{"$f":"IF((B_IndOlie_e_1)=0,0,((B_IndOlie_VL_1)^2.5)/(B_IndOlie_e_1))","v":0},{"$f":"H31","v":0},{"$f":"IF((B_IndOlie_e_2)=0,0,((B_IndOlie_VL_2)^2.5)/(B_IndOlie_e_2))","v":0},{"$f":"J31","v":0},{"$f":"IF((B_IndOlie_e_3)=0,0,((B_IndOlie_VL_3)^2.5)/(B_IndOlie_e_3))","v":0},{"$f":"L31","v":0},{"$f":"IF((B_IndOlie_e_4)=0,0,((B_IndOlie_VL_4)^2.5)/(B_IndOlie_e_4))","v":0},null,null,null,null,null,"B_IndOlie_N_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F32","v":1},{"$f":"IF((B_IndOlie_N_1)=0,1,(B_IndOlie_N_1))","v":1},{"$f":"H32","v":1},{"$f":"IF((B_IndOlie_N_2)=0,1,(B_IndOlie_N_2))","v":1},{"$f":"J32","v":1},{"$f":"IF((B_IndOlie_N_3)=0,1,(B_IndOlie_N_3))","v":1},{"$f":"L32","v":1},{"$f":"IF((B_IndOlie_N_4)=0,1,(B_IndOlie_N_4))","v":1},null,null,null,null,null,"B_IndOlie_N_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F33","v":0},{"$f":"B_IndOlie_X_1*B_IndOlie_N_kor_2*B_IndOlie_N_kor_3*B_IndOlie_N_kor_4*B_IndOlie_Nb_kor_1*B_IndOlie_Nb_kor_2","v":0},{"$f":"H33","v":0},{"$f":"B_IndOlie_X_2*B_IndOlie_N_kor_1*B_IndOlie_N_kor_3*B_IndOlie_N_kor_4*B_IndOlie_Nb_kor_1*B_IndOlie_Nb_kor_2","v":0},{"$f":"J33","v":0},{"$f":"B_IndOlie_X_3*B_IndOlie_N_kor_1*B_IndOlie_N_kor_2*B_IndOlie_N_kor_4*B_IndOlie_Nb_kor_1*B_IndOlie_Nb_kor_2","v":0},{"$f":"L33","v":0},{"$f":"B_IndOlie_X_4*B_IndOlie_N_kor_1*B_IndOlie_N_kor_2*B_IndOlie_N_kor_3*B_IndOlie_Nb_kor_1*B_IndOlie_Nb_kor_2","v":0},null,null,null,null,null,"B_IndOlie_N_mel_n"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,null,null,null,null,null,{"$f":"(B_IndOlie_N_kor_1*B_IndOlie_N_kor_2*B_IndOlie_N_kor_3*B_IndOlie_N_kor_4*B_IndOlie_Nb_kor_1*B_IndOlie_Nb_kor_2)/(B_IndOlie_N_mel_1+B_IndOlie_N_mel_2+B_IndOlie_N_mel_3+B_IndOlie_N_mel_4+B_IndOlie_Nb_mel_1+B_IndOlie_Nb_mel_2)","v":{"$error":"#DIV/0!"}},null,null,null,null,"B_IndOlie_N_tot"]
[]
[null,"Bygningsdata"]
[]
[null,"Terrændæk"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet"]
[null,"Type af terrændæk",null,null,{"$f":"D_IndOlie_Inddæk","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Inddæk"]
[null,"Betontværsnit","hb","mm",{"$f":"D_IndOlie_hb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_hb"]
[null,"Relativ luftfugtighed","RF","%",{"$f":"D_IndOlie_RF","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_RF"]
[null,"Vand/cement-tallet","v/c",null,{"$f":"D_IndOlie_wc","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_wc"]
[null,"Cementindhold","CM","kg/m3",{"$f":"D_IndOlie_CM","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_CM"]
[null,"Svindtid","ts","døgn",{"$f":"D_IndOlie_ts","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_ts"]
[null,"Materialekonst. for beton","Nb",null,{"$f":"D_IndOlie_Nb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Nb"]
[null,"Armeringsdiameter","da","mm",{"$f":"D_IndOlie_da","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_da"]
[null,"Armeringskonstant","k",null,{"$f":"D_IndOlie_k","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_k"]
[null,"Afstand mellem armeringsjern","Db","mm",{"$f":"D_IndOlie_Db","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Db"]
[null,"Dynamisk viskositet af luft","m","kg/(m * s)",{"$f":"D_IndOlie_my","v":1.8E-5},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_my"]
[null,"Elasticitetskoeff. Stål","Es","MPa",{"$f":"D_IndOlie_Es","v":210000},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Es"]
[null,"Elasticitetskoeff. Beton","Eb","MPa",{"$f":"D_IndOlie_Eb","v":20000},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Eb"]
[]
[null,"Samlet materialekonstant for terrændæk og \ninfluenszone & membran (app. 5.3 lign 68B)","KN","m³/(m²·s)","Beregnet værdi",{"$f":"G55","v":{"$error":"#DIV/0!"}},{"$f":"B_IndOlie_Nb/(B_IndOlie_hb/1000)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Kn"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet",null,null,null,null,"MST nr. 7 1998 - lign 25","aw=Acef/Sdw"]
[null,"Rumtype/anvendelse",null,null,{"$f":"D_IndOlie_anv","v":0},null,null,null,null,null,"MST nr. 7 1998 - lign 26","Acef=hb·ll",null,null,null,null,null,"B_IndOlie_anv"]
[null,"Loftshøjde (hb)","Lh","m",{"$f":"D_IndOlie_Lh","v":0},null,null,null,null,null,"MST nr. 7 1998 - lign 27","dw=k·da",null,null,null,null,null,"B_IndOlie_Lh"]
[null,"Luftskifte (Lb)","Ls","s-1",{"$f":"D_IndOlie_Ls","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Ls"]
[null,"Gulvbredde","lb","m",{"$f":"D_IndOlie_Lb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Lb"]
[null,"Gulvlængde","ll","m",{"$f":"D_IndOlie_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Ll"]
[null,"Trykforskel over betondæk","DP","Pa",{"$f":"D_IndOlie_DP","v":5},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlie_DP"]
[]
[null,"Beregnede bygningsdata"]
[null,null,null,null,null,null,null,"Begge betontyper"]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet",null,"Uarmeret betondæk",null,"Armeret betondæk",null,null,"Ligning 29+27","aw=(hb·Db)/(k·da)"]
[null,"Revnevidde \n(app 5.3 lign. 73 eller MST nr. 7 1998 - lign 40)","w","mm",{"$f":"D_IndOlie_w","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(B_IndOlie_Db),IndLigning40(B_IndOlie_hb,B_IndOlie_Db,B_IndOlie_k,B_IndOlie_da,B_IndOlie_Es, B_IndOlie_Eb,B_IndOlie_eg),IndLigning73(B_IndOlie_eg,B_IndOlie_Lb,B_IndOlie_Ll, B_IndOlie_ltot))","v":{"$error":"#VALUE!"}},null,"app 5.3 lign. 73","w=eg·lb·ll/ltot","Ligning 40","w=5·10-5·ss·(aw)½",null,"Ligning 39+28","ss=(Es·eg)/[(1+(Es/Eb)·j)·100]",null,null,null,"B_IndOlie_w"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ligning 37","j=(p·da2)/(4·hb·Db)"]
[null,"Basissvindet (MST nr. 7 1998 - lign 31)","ec","%",{"$f":"D_IndOlie_ec","v":5.3293413173652694E-2},{"$f":"0.089*(100-B_IndOlie_RF)/(167-B_IndOlie_RF)","v":5.3293413173652694E-2},null,"Ligning 31","ec=[0,089·(100-RF)]/[167-RF]",null,null,null,null,null,null,null,null,"B_IndOlie_ec"]
[null,"Beton-sammensætningskoefficient \n(MST nr. 7 1998 - lign 32)","kb",null,{"$f":"D_IndOlie_Kb","v":0},{"$f":"IndLigning32(B_IndOlie_CM,B_IndOlie_wc)","v":0},null,"Ligning 32","kb=0,007·CM·(v/c+0,333)·v/c",null,null,null,null,null,null,null,null,"B_IndOlie_Kb"]
[null,"Gnmsn. Revneafstand\n(MST nr. 7 1998 - lign 41+42)","lw","mm",{"$f":"D_IndOlie_lw","v":{"$error":"#VALUE!"}},{"$f":"IndLigning41_42(B_IndOlie_hb,B_IndOlie_Db,B_IndOlie_k,B_IndOlie_da)","v":{"$error":"#VALUE!"}},null,null,null,"Ligning 41+42","lw=1,5 ·aw/p",null,null,null,null,null,null,"B_IndOlie_lw"]
[null,"Total revnelængde\n(app 5.3 lign. 72 eller MST nr. 7 1998 - lign 43)","ltot","m",{"$f":"D_IndOlie_ltot","v":0},{"$f":"IF(ISNUMBER(B_IndOlie_Db),IndLigning43(B_IndOlie_Lb,B_IndOlie_lw,B_IndOlie_Ll),IndLigning72(B_IndOlie_Lb,B_IndOlie_Ll))","v":0},null,"app 5.3 lign. 72","ltot=2·(lb+ll)","Ligning 43","ltot=[(lb·1000)/(lw)-1]·ll+[(ll·1000)/(lw)-1]·lb",null,null,null,null,null,null,"B_IndOlie_ltot"]
[null,"Vol. strøm gennem beton\n(app 5.3 lign. 70 eller MST nr. 7 1998 - lign 44)","qb","m³/(s )",{"$f":"D_IndOlie_q","v":{"$error":"#VALUE!"}},{"$f":"IndLigning44_70(B_IndOlie_ltot,B_IndOlie_w,B_IndOlie_DP,B_IndOlie_my,B_IndOlie_hb)","v":{"$error":"#VALUE!"}},null,"Lingning 44 / 70","qb=(ltot·w3·DP·10-6)/(12·m·hb)",null,null,null,null,null,null,null,null,"B_IndOlie_q"]
[null,"Vol. strøm i bygningen","qbyg","m³/(s )",{"$f":"D_IndOlie_qbyg","v":0},{"$f":"B_IndOlie_Ls*B_IndOlie_Lh*B_IndOlie_Lb*B_IndOlie_Ll","v":0},null,null,"qbyg=Ls*Lh*lb*ll",null,null,null,null,null,null,null,null,"B_IndOlie_qbyg"]
[null,"CHECK af volumenstrøm gennem beton","q_check","%",{"$f":"D_IndOlie_qcheck","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_q/B_IndOlie_qbyg","v":{"$error":"#VALUE!"}},null,null,"q_check=qc/qbyg",null,null,null,null,null,null,null,null,"B_IndOlie_qcheck"]
[null,"Vol. strøm gennem beton pr. kvadratmeter gulv \n(MST nr. 7 1998 - lign 45)","Qb","m³/(s· m²)",null,{"$f":"B_IndOlie_q/(B_IndOlie_Lb*B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},null,"Ligning 30+34+33","eg=ec·kb·kd·kt=ec·kb·[0,25·(852+2·hb)/(132+2·hb)]·kt"]
[null,"Den frie svindtøjning\nMST nr. 7 1998 - lign 30 til lign36","eg","%",{"$f":"D_IndOlie_eg","v":{"$error":"#VALUE!"}},{"$f":"IndLigning30_33_34(B_IndOlie_ec,B_IndOlie_Kb,B_IndOlie_hb,B_IndOlie_ts)","v":{"$error":"#VALUE!"}},null,"Ligning 35","kt=tsa/(tsa+t0)",null,null,null,null,null,null,null,null,"B_IndOlie_eg"]
[null,null,null,null,null,null,null,"Ligning 36","a=0,75+0,125·b"]
[null,null,null,null,null,null,null,null,"b=(ln(0,025·2·hb))/ln2"]
[null,null,null,null,null,null,null,null,"t0=9·((10)½)ab"]
[]
[null,"Oliestoffer"]
[null,null,null,null,null,null,null,null,null,null,"B_IndOlie_Ci_n"]
[null,"Gruppe","Forureningskomponent",null,null,"Poreluftskoncentration ","Diffusionskoefficient luft","Flux gennem jorden (app. 5.3 ligning 63)","Kjord (app. 53 ligning 75)","Stofspecifik materialekonstant","Totalt bidrag til indeluft (app. 53 ligning 77)","Poreluftkonc. under gulv (app. 53 ligning 78)","Diffusivt bidrag til indeluft  (app. 53 ligning 67A)","Afdamp-nings-kriterium","Overskridelse af kriteriet"]
[null,null,null,null,null,"CL","DL","Jz","Kjord","KN","Ci","Cp","Cdi"]
[null,null,null,null,null,"mg/m³","m²/s","mg/(m² s)","m³/(m²·s)",null,"mg/m³","mg/m³","mg/m³","mg/m³"]
[50,"C5-C6",null,null,null,null,null,null,null,null,{"$f":"SUM(K91:K94)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L91:L94)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M91:M94)","v":{"$error":"#VALUE!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},{"$f":"IndLigning63(F91,B_IndOlie_X_tot,B_IndOlie_N_tot,G91,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H91/F91","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G91","v":{"$error":"#DIV/0!"}},{"$f":"IF(F91=0,0,IndLigning77(J91,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F91,I91,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K91,B_IndOlie_Lh,B_IndOlie_Ls,J91,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J91, L91, K91, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},{"$f":"IndLigning63(F92,B_IndOlie_X_tot,B_IndOlie_N_tot,G92,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H92/F92","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G92","v":{"$error":"#DIV/0!"}},{"$f":"IF(F92=0,0,IndLigning77(J92,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F92,I92,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K92,B_IndOlie_Lh,B_IndOlie_Ls,J92,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J92, L92, K92, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},{"$f":"IndLigning63(F93,B_IndOlie_X_tot,B_IndOlie_N_tot,G93,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G93","v":{"$error":"#DIV/0!"}},{"$f":"IF(F93=0,0,IndLigning77(J93,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F93,I93,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K93,B_IndOlie_Lh,B_IndOlie_Ls,J93,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J93, L93, K93, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},{"$f":"IndLigning63(F94,B_IndOlie_X_tot,B_IndOlie_N_tot,G94,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G94","v":{"$error":"#DIV/0!"}},{"$f":"IF(F94=0,0,IndLigning77(J94,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F94,I94,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K94,B_IndOlie_Lh,B_IndOlie_Ls,J94,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J94, L94, K94, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[]
[510,"C6-C10",null,null,null,null,null,null,null,null,{"$f":"SUM(K97:K101)+SUM(K107:K109)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L97:L101)+SUM(L107:L109)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M97:M101)+SUM(M107:M109)","v":{"$error":"#VALUE!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_52","v":9.3000000000000007E-6},{"$f":"IndLigning63(F97,B_IndOlie_X_tot,B_IndOlie_N_tot,G97,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G97","v":{"$error":"#DIV/0!"}},{"$f":"IF(F97=0,0,IndLigning77(J97,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F97,I97,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K97,B_IndOlie_Lh,B_IndOlie_Ls,J97,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J97, L97, K97, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},{"$f":"IF(ISNUMBER(N97),IF(K97>N97,K97/N97,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},{"$f":"IndLigning63(F98,B_IndOlie_X_tot,B_IndOlie_N_tot,G98,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G98","v":{"$error":"#DIV/0!"}},{"$f":"IF(F98=0,0,IndLigning77(J98,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F98,I98,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K98,B_IndOlie_Lh,B_IndOlie_Ls,J98,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J98, L98, K98, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},{"$f":"IndLigning63(F99,B_IndOlie_X_tot,B_IndOlie_N_tot,G99,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G99","v":{"$error":"#DIV/0!"}},{"$f":"IF(F99=0,0,IndLigning77(J99,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F99,I99,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K99,B_IndOlie_Lh,B_IndOlie_Ls,J99,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J99, L99, K99, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_54_ak","v":0.4},{"$f":"IF(ISNUMBER(N99),IF(K99>N99,K99/N99,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["55A",">8 - 10, alifater",">8 - 10, alifater, Tung olie",null,null,{"$f":"D_Olie_55A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55A","v":5.5030901075876E-6},{"$f":"IndLigning63(F100,B_IndOlie_X_tot,B_IndOlie_N_tot,G100,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G100","v":{"$error":"#DIV/0!"}},{"$f":"IF(F100=0,0,IndLigning77(J100,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F100,I100,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K100,B_IndOlie_Lh,B_IndOlie_Ls,J100,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J100, L100, K100, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["55B",null,">8 - 10, alifater, Olieblandinger",null,null,{"$f":"D_Olie_55B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55B","v":6.2232552378840063E-6},{"$f":"IndLigning63(F101,B_IndOlie_X_tot,B_IndOlie_N_tot,G101,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H101/F101","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G101","v":{"$error":"#DIV/0!"}},{"$f":"IF(F101=0,0,IndLigning77(J101,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F101,I101,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K101,B_IndOlie_Lh,B_IndOlie_Ls,J101,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J101, L101, K101, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},{"$f":"IndLigning63(F105,B_IndOlie_X_tot,B_IndOlie_N_tot,G105,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G105","v":{"$error":"#DIV/0!"}},{"$f":"IF(F105=0,0,IndLigning77(J105,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F105,I105,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K105,B_IndOlie_Lh,B_IndOlie_Ls,J105,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J105, L105, K105, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},{"$f":"IndLigning63(F106,B_IndOlie_X_tot,B_IndOlie_N_tot,G106,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G106","v":{"$error":"#DIV/0!"}},{"$f":"IF(F106=0,0,IndLigning77(J106,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F106,I106,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K106,B_IndOlie_Lh,B_IndOlie_Ls,J106,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J106, L106, K106, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[59,null,"Sum af xylener +ethylbenzen",null,null,null,null,null,null,null,{"$f":"K106+K105","v":{"$error":"#DIV/0!"}},{"$f":"L106+L105","v":{"$error":"#VALUE!"}},{"$f":"M106+M105","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_57_ak","v":0.1},{"$f":"IF(ISNUMBER(N107),IF(K107>N107,K107/N107,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["60A",null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"IndLigning63(F108,B_IndOlie_X_tot,B_IndOlie_N_tot,G108,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G108","v":{"$error":"#DIV/0!"}},{"$f":"IF(F108=0,0,IndLigning77(J108,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F108,I108,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K108,B_IndOlie_Lh,B_IndOlie_Ls,J108,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J108, L108, K108, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["60B",null,">8 -10, aromater,øvrige",null,null,{"$f":"D_Olie_60_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_60B","v":6.4381431991356133E-6},{"$f":"IndLigning63(F109,B_IndOlie_X_tot,B_IndOlie_N_tot,G109,1E-20)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"B_IndOlie_Kn*G109","v":{"$error":"#DIV/0!"}},{"$f":"IF(F109=0,0,IndLigning77(J109,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F109,I109,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K109,B_IndOlie_Lh,B_IndOlie_Ls,J109,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J109, L109, K109, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[910,"C9-C10 aromater",null,null,null,null,null,null,null,null,{"$f":"SUM(K108:K109)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L108:L109)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M108:M109)","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_60_ak","v":0.03},{"$f":"IF(ISNUMBER(N110),IF(K110>N110,K110/N110,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[]
[1015,"C11-C15",null,null,null,null,null,null,null,null,{"$f":"SUM(K113:K124)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L113:L124)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M113:M124)","v":{"$error":"#VALUE!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},{"$f":"IndLigning63(F113,B_IndOlie_X_tot,B_IndOlie_N_tot,G113,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H113/F113","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G113","v":{"$error":"#DIV/0!"}},{"$f":"IF(F113=0,0,IndLigning77(J113,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F113,I113,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K113,B_IndOlie_Lh,B_IndOlie_Ls,J113,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J113, L113, K113, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},{"$f":"IndLigning63(F115,B_IndOlie_X_tot,B_IndOlie_N_tot,G115,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H115/F115","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G115","v":{"$error":"#DIV/0!"}},{"$f":"IF(F115=0,0,IndLigning77(J115,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F115,I115,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K115,B_IndOlie_Lh,B_IndOlie_Ls,J115,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J115, L115, K115, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_103_ak","v":0.04},{"$f":"IF(ISNUMBER(N115),IF(K115>N115,K115/N115,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
["104A",null,">10 - 12, aromater, øvrige, Tung Olie",null,null,{"$f":"D_Olie_104A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104A","v":5.9633499312903359E-6},{"$f":"IndLigning63(F116,B_IndOlie_X_tot,B_IndOlie_N_tot,G116,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H116/F116","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G116","v":{"$error":"#DIV/0!"}},{"$f":"IF(F116=0,0,IndLigning77(J116,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F116,I116,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K116,B_IndOlie_Lh,B_IndOlie_Ls,J116,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J116, L116, K116, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["104B",null,">10 - 12, aromater, øvrige, Olieblanding",null,null,{"$f":"D_Olie_104B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104B","v":5.5260438461528997E-6},{"$f":"IndLigning63(F117,B_IndOlie_X_tot,B_IndOlie_N_tot,G117,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H117/F117","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G117","v":{"$error":"#DIV/0!"}},{"$f":"IF(F117=0,0,IndLigning77(J117,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F117,I117,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K117,B_IndOlie_Lh,B_IndOlie_Ls,J117,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J117, L117, K117, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["105A",null,">12 - 16, alifater, Tung Olie",null,null,{"$f":"D_Olie_105a_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105A","v":4.3460519456567218E-6},{"$f":"IndLigning63(F118,B_IndOlie_X_tot,B_IndOlie_N_tot,G118,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H118/F118","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G118","v":{"$error":"#DIV/0!"}},{"$f":"IF(F118=0,0,IndLigning77(J118,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F118,I118,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K118,B_IndOlie_Lh,B_IndOlie_Ls,J118,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J118, L118, K118, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["105B",">12 - 16, alifater",">12 - 16, alifater, Olieblandinger",null,null,{"$f":"D_Olie_105B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105B","v":5.0933919872504982E-6},{"$f":"IndLigning63(F119,B_IndOlie_X_tot,B_IndOlie_N_tot,G119,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H119/F119","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G119","v":{"$error":"#DIV/0!"}},{"$f":"IF(F119=0,0,IndLigning77(J119,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F119,I119,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K119,B_IndOlie_Lh,B_IndOlie_Ls,J119,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J119, L119, K119, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},{"$f":"IndLigning63(F121,B_IndOlie_X_tot,B_IndOlie_N_tot,G121,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H121/F121","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G121","v":{"$error":"#DIV/0!"}},{"$f":"IF(F121=0,0,IndLigning77(J121,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F121,I121,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K121,B_IndOlie_Lh,B_IndOlie_Ls,J121,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J121, L121, K121, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},{"$f":"IndLigning63(F122,B_IndOlie_X_tot,B_IndOlie_N_tot,G122,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H122/F122","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G122","v":{"$error":"#DIV/0!"}},{"$f":"IF(F122=0,0,IndLigning77(J122,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F122,I122,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K122,B_IndOlie_Lh,B_IndOlie_Ls,J122,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J122, L122, K122, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["109A",null,">12 - 16, aromater,øvrige, Tung Olie",null,null,{"$f":"D_Olie_109A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109A","v":5.5027929670196982E-6},{"$f":"IndLigning63(F123,B_IndOlie_X_tot,B_IndOlie_N_tot,G123,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H123/F123","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G123","v":{"$error":"#DIV/0!"}},{"$f":"IF(F123=0,0,IndLigning77(J123,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F123,I123,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K123,B_IndOlie_Lh,B_IndOlie_Ls,J123,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J123, L123, K123, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["109B",null,">12 - 16, aromater,øvrige, Olieblandinger",null,null,{"$f":"D_Olie_109B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109B","v":5.9000000000000003E-6},{"$f":"IndLigning63(F124,B_IndOlie_X_tot,B_IndOlie_N_tot,G124,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H124/F124","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G124","v":{"$error":"#DIV/0!"}},{"$f":"IF(F124=0,0,IndLigning77(J124,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F124,I124,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K124,B_IndOlie_Lh,B_IndOlie_Ls,J124,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J124, L124, K124, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[]
[1520,"C16-C20",null,null,null,null,null,null,null,null,{"$f":"SUM(K128:K134)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L128:L134)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M128:M134)","v":{"$error":"#VALUE!"}}]
["151A",">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"D_Olie_151A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151A","v":3.7468864349159863E-6},{"$f":"IndLigning63(F127,B_IndOlie_X_tot,B_IndOlie_N_tot,G127,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H127/F127","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G127","v":{"$error":"#DIV/0!"}},{"$f":"IF(F127=0,0,IndLigning77(J127,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F127,I127,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K127,B_IndOlie_Lh,B_IndOlie_Ls,J127,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J127, L127, K127, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["151B",null,">16 - 21, alifater",null,null,{"$f":"D_Olie_151B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151B","v":4.4721099862171762E-6},{"$f":"IndLigning63(F128,B_IndOlie_X_tot,B_IndOlie_N_tot,G128,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H128/F128","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G128","v":{"$error":"#DIV/0!"}},{"$f":"IF(F128=0,0,IndLigning77(J128,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F128,I128,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K128,B_IndOlie_Lh,B_IndOlie_Ls,J128,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J128, L128, K128, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},{"$f":"IndLigning63(F130,B_IndOlie_X_tot,B_IndOlie_N_tot,G130,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H130/F130","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G130","v":{"$error":"#DIV/0!"}},{"$f":"IF(F130=0,0,IndLigning77(J130,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F130,I130,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K130,B_IndOlie_Lh,B_IndOlie_Ls,J130,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J130, L130, K130, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},{"$f":"IndLigning63(F131,B_IndOlie_X_tot,B_IndOlie_N_tot,G131,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H131/F131","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G131","v":{"$error":"#DIV/0!"}},{"$f":"IF(F131=0,0,IndLigning77(J131,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F131,I131,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K131,B_IndOlie_Lh,B_IndOlie_Ls,J131,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J131, L131, K131, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},{"$f":"IndLigning63(F132,B_IndOlie_X_tot,B_IndOlie_N_tot,G132,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H132/F132","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G132","v":{"$error":"#DIV/0!"}},{"$f":"IF(F132=0,0,IndLigning77(J132,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F132,I132,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K132,B_IndOlie_Lh,B_IndOlie_Ls,J132,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J132, L132, K132, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},{"$f":"IndLigning63(F133,B_IndOlie_X_tot,B_IndOlie_N_tot,G133,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H133/F133","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G133","v":{"$error":"#DIV/0!"}},{"$f":"IF(F133=0,0,IndLigning77(J133,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F133,I133,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K133,B_IndOlie_Lh,B_IndOlie_Ls,J133,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J133, L133, K133, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},{"$f":"IndLigning63(F134,B_IndOlie_X_tot,B_IndOlie_N_tot,G134,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H134/F134","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G134","v":{"$error":"#DIV/0!"}},{"$f":"IF(F134=0,0,IndLigning77(J134,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F134,I134,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K134,B_IndOlie_Lh,B_IndOlie_Ls,J134,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J134, L134, K134, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[]
[2025,"C21-C25",null,null,null,null,null,null,null,null,{"$f":"SUM(K138:K139)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L138:L139)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M138:M139)","v":{"$error":"#VALUE!"}}]
["201A",">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"D_Olie_201A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201A","v":3.6715492605442101E-6},{"$f":"IndLigning63(F137,B_IndOlie_X_tot,B_IndOlie_N_tot,G137,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H137/F137","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G137","v":{"$error":"#DIV/0!"}},{"$f":"IF(F137=0,0,IndLigning77(J137,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F137,I137,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K137,B_IndOlie_Lh,B_IndOlie_Ls,J137,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J137, L137, K137, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["201B",null,">21 - 25, alifater",null,null,{"$f":"D_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201B","v":3.9528308464137552E-6},{"$f":"IndLigning63(F138,B_IndOlie_X_tot,B_IndOlie_N_tot,G138,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H138/F138","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G138","v":{"$error":"#DIV/0!"}},{"$f":"IF(F138=0,0,IndLigning77(J138,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F138,I138,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K138,B_IndOlie_Lh,B_IndOlie_Ls,J138,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J138, L138, K138, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter"]
[2535,"C25-C35","VKI",null,null,null,null,null,null,null,{"$f":"SUM(K142:K151)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L142:L151)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M142:M151)","v":{"$error":"#VALUE!"}}]
["251A",">25 - 35, alifater",">25 - 35, alifater, Tung olie",null,null,{"$f":"D_Olie_251A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251A","v":3.0055777156880082E-6},{"$f":"IndLigning63(F141,B_IndOlie_X_tot,B_IndOlie_N_tot,G141,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H141/F141","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G141","v":{"$error":"#DIV/0!"}},{"$f":"IF(F141=0,0,IndLigning77(J141,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F141,I141,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K141,B_IndOlie_Lh,B_IndOlie_Ls,J141,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J141, L141, K141, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
["251B",null,">25 - 35, alifater, Olieblandinger",null,null,{"$f":"D_Olie_251B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251B","v":3.6715492605442101E-6},{"$f":"IndLigning63(F142,B_IndOlie_X_tot,B_IndOlie_N_tot,G142,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H142/F142","v":{"$error":"#VALUE!"}},{"$f":"B_IndOlie_Kn*G142","v":{"$error":"#DIV/0!"}},{"$f":"IF(F142=0,0,IndLigning77(J142,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F142,I142,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K142,B_IndOlie_Lh,B_IndOlie_Ls,J142,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J142, L142, K142, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater"]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},0.1,{"$f":"H144/F144","v":{"$error":"#DIV/0!"}},{"$f":"B_IndOlie_Kn*G144","v":{"$error":"#DIV/0!"}},{"$f":"IF(F144=0,0,IndLigning77(J144,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F144,I144,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K144,B_IndOlie_Lh,B_IndOlie_Ls,J144,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J144, L144, K144, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},0.1,{"$f":"H145/F145","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["259A",null,">25 - 35, aromater, øvrige, Tung olie",null,null,{"$f":"D_Olie_259A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259A","v":5.5943064295556175E-6},0.1,{"$f":"H150/F150","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["259B",null,">25 - 35, aromater, øvrige, Olieblandinger",null,null,{"$f":"D_Olie_259B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259B","v":4.4493993711079091E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[3540,">C35",null,null,null,null,null,null,null,null,{"$f":"SUM(K154:K155)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L154:L155)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M154:M155)","v":{"$error":"#VALUE!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},0.1,{"$f":"H154/F154","v":{"$error":"#DIV/0!"}},{"$f":"B_IndOlie_Kn*G154","v":{"$error":"#DIV/0!"}},{"$f":"IF(F154=0,0,IndLigning77(J154,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F154,I154,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K154,B_IndOlie_Lh,B_IndOlie_Ls,J154,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J154, L154, K154, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},0.1,{"$f":"H155/F155","v":{"$error":"#DIV/0!"}},{"$f":"B_IndOlie_Kn*G155","v":{"$error":"#DIV/0!"}},{"$f":"IF(F155=0,0,IndLigning77(J155,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F155,I155,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K155,B_IndOlie_Lh,B_IndOlie_Ls,J155,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J155, L155, K155, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[]
[2040,"C21-C35",null,null,null,null,null,null,null,null,{"$f":"K140+K136","v":{"$error":"#DIV/0!"}},{"$f":"L140+L136","v":{"$error":"#VALUE!"}},{"$f":"M140+M136","v":{"$error":"#VALUE!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand"]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},0.1,{"$f":"H163/F163","v":{"$error":"#DIV/0!"}},{"$f":"B_IndOlie_Kn*G163","v":{"$error":"#DIV/0!"}},{"$f":"IF(F163=0,0,IndLigning77(J163,B_IndOlie_Lb,B_IndOlie_Ll,B_IndOlie_Ls,F163,I163,B_IndOlie_q,B_IndOlie_Lh))","v":{"$error":"#DIV/0!"}},{"$f":"IndLigning78(K163,B_IndOlie_Lh,B_IndOlie_Ls,J163,B_IndOlie_q,B_IndOlie_Lb,B_IndOlie_Ll)","v":{"$error":"#VALUE!"}},{"$f":"IndLigning67A(J163, L163, K163, B_IndOlie_Lh, B_IndOlie_Ls)","v":{"$error":"#VALUE!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[1,"Sum af kulbrinter",null,null,null,null,null,null,null,null,{"$f":"K153+K140+K136+K126+K112+K96","v":{"$error":"#DIV/0!"}},{"$f":"L153+L140+L136+L126+L112+L96","v":{"$error":"#VALUE!"}},{"$f":"M153+M140+M136+M126+M112+M96","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"IF(ISNUMBER(N171),IF(K171>N171,K171/N171,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(K162:K169)+K153+K140+K136+K126+K112+K96","v":{"$error":"#DIV/0!"}},{"$f":"SUM(L162:L169)+L153+L140+L136+L126+L112+L96","v":{"$error":"#VALUE!"}},{"$f":"SUM(M162:M169)+M153+M140+M136+M126+M112+M96","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"IF(ISNUMBER(N172),IF(K172>N172,K172/N172,\"Nej\"),\" \")","v":{"$error":"#DIV/0!"}}]
[null,"Krybekælder"]
[null,"Betongulv, membran og jord"]
[]
[null,null,null,null,"Betongulv (1)",null,"Membran (2)"]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Navn",null,null,{"$f":"D_IndOlieK_navnb_1","v":0},null,{"$f":"D_IndOlieK_navnb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_navnb_n"]
[null,"Tykkelse af lag","Xb","m",{"$f":"D_IndOlieK_Xb_1","v":0},{"$f":"E179/1000","v":0},{"$f":"D_IndOlieK_Xb_2","v":0},{"$f":"G179/1000","v":0},{"$f":"B_IndOlieK_Xb_1+B_IndOlieK_Xb_2","v":0},null,null,null,null,null,null,null,null,"B_IndOlieK_Xb_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","tb",null,{"$f":"D_IndOlieK_Nb_1","v":0},null,{"$f":"D_IndOlieK_Nb_2","v":0},null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_Nb_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F181","v":1},{"$f":"IF((B_IndOlieK_Nb_1)=0,1,(B_IndOlieK_Nb_1))","v":1},{"$f":"H181","v":1},{"$f":"IF((B_IndOlieK_Nb_2)=0,1,(B_IndOlieK_Nb_2))","v":1},null,null,null,null,null,null,null,null,null,"B_IndOlieK_Nb_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F182","v":0},{"$f":"(B_IndOlieK_Xb_1)*B_IndOlieK_N_kor_1*B_IndOlieK_N_kor_2*B_IndOlieK_N_kor_3*B_IndOlieK_N_kor_4*B_IndOlieK_Nb_kor_2","v":0},{"$f":"H182","v":0},{"$f":"(B_IndOlieK_Xb_2)*B_IndOlieK_N_kor_1*B_IndOlieK_N_kor_2*B_IndOlieK_N_kor_3*B_IndOlieK_N_kor_4*B_IndOlieK_Nb_kor_1","v":0},null,null,null,null,null,null,null,null,null,"B_IndOlieK_Nb_mel_n"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","Værdi","Beregnet","SAMLET"]
[null,"Jordtype",null,null,{"$f":"D_IndOlieK_jordtype_1","v":0},null,{"$f":"D_IndOlieK_jordtype_2","v":0},null,{"$f":"D_IndOlieK_jordtype_3","v":0},null,{"$f":"D_IndOlieK_jordtype_4","v":0}]
[null,"Jordlag, Dybde fra","x1","m u.t.",{"$f":"F189","v":0},{"$f":"I179","v":0},{"$f":"B_IndOlieK_lagtil_1","v":0},null,{"$f":"B_IndOlieK_lagtil_2","v":0},null,{"$f":"B_IndOlieK_lagtil_3","v":0},null,null,null,null,null,null,"B_IndOlieK_lagfra_n"]
[null,"Jordlag, Dybde til","x2","m u.t.",{"$f":"D_IndOlieK_lagtil_1","v":0},null,{"$f":"D_IndOlieK_lagtil_2","v":0},null,{"$f":"D_IndOlieK_lagtil_3","v":0},null,{"$f":"D_IndOlieK_lagtil_4","v":0},null,null,null,null,null,null,"B_IndOlieK_lagtil_n"]
[null,"Tykkelse af jordlag","X","m",{"$f":"F191","v":0},{"$f":"IF(ISNUMBER(IndOlieK_Jord_dt1),B_IndOlieK_lagtil_1-B_IndOlieK_lagfra_1,0)","v":0},{"$f":"H191","v":0},{"$f":"IF(ISNUMBER(IndOlieK_Jord_dt2),B_IndOlieK_lagtil_2-B_IndOlieK_lagfra_2,0)","v":0},{"$f":"J191","v":0},{"$f":"IF(ISNUMBER(IndOlieK_Jord_dt3),B_IndOlieK_lagtil_3-B_IndOlieK_lagfra_3,0)","v":0},{"$f":"L191","v":0},{"$f":"IF(ISNUMBER(IndOlieK_Jord_dt4),B_IndOlieK_lagtil_4-B_IndOlieK_lagfra_4,0)","v":0},{"$f":"B_IndOlieK_X_1+B_IndOlieK_X_2+B_IndOlieK_X_3+B_IndOlieK_X_4+I179","v":0},null,null,null,null,"B_IndOlieK_X_n"]
[null,"Check af negativ højde",null,null,{"$f":"F192","v":0},{"$f":"IF(B_IndOlieK_X_1<0,1,0)","v":0},{"$f":"H192","v":0},{"$f":"IF(B_IndOlieK_X_2<0,1,0)","v":0},{"$f":"J192","v":0},{"$f":"IF(B_IndOlieK_X_3<0,1,0)","v":0},{"$f":"L192","v":0},{"$f":"IF(B_IndOlieK_X_4<0,1,0)","v":0},{"$f":"IF(B_IndOlieK_negativ_X_1+B_IndOlieK_negativ_X_2+B_IndOlieK_negativ_X_3+B_IndOlieK_negativ_X_4>0,\"FEJL!! Der er jordlag med negativ højde\",\" \")","v":" "},null,null,null,null,"B_IndOlieK_negativ_X_n"]
[null,"Poreluftvolumen","VL",null,{"$f":"D_IndOlieK_VL_1","v":0},null,{"$f":"D_IndOlieK_VL_2","v":0},null,{"$f":"D_IndOlieK_VL_3","v":0},null,{"$f":"D_IndOlieK_VL_4","v":0},null,null,null,null,null,null,"B_IndOlieK_VL_n"]
[null,"Vand-indhold","VV",null,{"$f":"D_IndOlieK_VV_1","v":0},null,{"$f":"D_IndOlieK_VV_2","v":0},null,{"$f":"D_IndOlieK_VV_3","v":0},null,{"$f":"D_IndOlieK_VV_4","v":0},null,null,null,null,null,null,"B_IndOlieK_VV_n"]
[null,"Samlet porøsitet","e=VL+VV",null,{"$f":"F195","v":0},{"$f":"B_IndOlieK_VL_1+B_IndOlieK_VV_1","v":0},{"$f":"H195","v":0},{"$f":"B_IndOlieK_VL_2+B_IndOlieK_VV_2","v":0},{"$f":"J195","v":0},{"$f":"B_IndOlieK_VL_3+B_IndOlieK_VV_3","v":0},{"$f":"L195","v":0},{"$f":"B_IndOlieK_VL_4+B_IndOlieK_VV_4","v":0},null,null,null,null,null,"B_IndOlieK_e_n"]
[null,"Volumen af jordskellet","VJ",null,{"$f":"F196","v":1},{"$f":"1-B_IndOlieK_e_1","v":1},{"$f":"H196","v":1},{"$f":"1-B_IndOlieK_e_2","v":1},{"$f":"J196","v":1},{"$f":"1-B_IndOlieK_e_3","v":1},{"$f":"L196","v":1},{"$f":"1-B_IndOlieK_e_4","v":1},null,null,null,null,null,"B_IndOlieK_VJ_n"]
[null,"Materialekonstant (app 5.3 - lign 64)","t",null,{"$f":"F197","v":0},{"$f":"IF((B_IndOlieK_e_1)=0,0,((B_IndOlieK_VL_1)^2.5)/(B_IndOlieK_e_1))","v":0},{"$f":"H197","v":0},{"$f":"IF((B_IndOlieK_e_2)=0,0,((B_IndOlieK_VL_2)^2.5)/(B_IndOlieK_e_2))","v":0},{"$f":"J197","v":0},{"$f":"IF((B_IndOlieK_e_3)=0,0,((B_IndOlieK_VL_3)^2.5)/(B_IndOlieK_e_3))","v":0},{"$f":"L197","v":0},{"$f":"IF((B_IndOlieK_e_4)=0,0,((B_IndOlieK_VL_4)^2.5)/(B_IndOlieK_e_4))","v":0},null,null,null,null,null,"B_IndOlieK_N_n"]
[null,"Korigeret materialekonstant","N-kor",null,{"$f":"F198","v":1},{"$f":"IF((B_IndOlieK_N_1)=0,1,(B_IndOlieK_N_1))","v":1},{"$f":"H198","v":1},{"$f":"IF((B_IndOlieK_N_2)=0,1,(B_IndOlieK_N_2))","v":1},{"$f":"J198","v":1},{"$f":"IF((B_IndOlieK_N_3)=0,1,(B_IndOlieK_N_3))","v":1},{"$f":"L198","v":1},{"$f":"IF((B_IndOlieK_N_4)=0,1,(B_IndOlieK_N_4))","v":1},null,null,null,null,null,"B_IndOlieK_N_kor_n"]
[null,"Mellemregning (app. 5.3 - Lign 80)",null,null,{"$f":"F199","v":0},{"$f":"(B_IndOlieK_X_1)*B_IndOlieK_N_kor_2*B_IndOlieK_N_kor_3*B_IndOlieK_N_kor_4*B_IndOlieK_Nb_kor_1*B_IndOlieK_Nb_kor_2","v":0},{"$f":"H199","v":0},{"$f":"(B_IndOlieK_X_2)*B_IndOlieK_N_kor_1*B_IndOlieK_N_kor_3*B_IndOlieK_N_kor_4*B_IndOlieK_Nb_kor_1*B_IndOlieK_Nb_kor_2","v":0},{"$f":"J199","v":0},{"$f":"(B_IndOlieK_X_3)*B_IndOlieK_N_kor_1*B_IndOlieK_N_kor_2*B_IndOlieK_N_kor_4*B_IndOlieK_Nb_kor_1*B_IndOlieK_Nb_kor_2","v":0},{"$f":"L199","v":0},{"$f":"(B_IndOlieK_X_4)*B_IndOlieK_N_kor_1*B_IndOlieK_N_kor_2*B_IndOlieK_N_kor_3*B_IndOlieK_Nb_kor_1*B_IndOlieK_Nb_kor_2","v":0},null,null,null,null,null,"B_IndOlieK_N_mel_n"]
[null,"Samlet materiale konstant (app 5.3 - lign. 80)","t*",null,null,null,null,null,null,null,null,null,{"$f":"(B_IndOlieK_N_kor_1*B_IndOlieK_N_kor_2*B_IndOlieK_N_kor_3*B_IndOlieK_N_kor_4*B_IndOlieK_Nb_kor_1*B_IndOlieK_Nb_kor_2)/(B_IndOlieK_N_mel_1+B_IndOlieK_N_mel_2+B_IndOlieK_N_mel_3+B_IndOlieK_N_mel_4+B_IndOlieK_Nb_mel_1+B_IndOlieK_Nb_mel_2)","v":{"$error":"#DIV/0!"}},null,null,null,null,"B_IndOlieK_N_tot"]
[]
[null,"Bygningsdata"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet"]
[null,"Rumtype/anvendelse",null,null,{"$f":"D_IndOlieK_anv","v":0}]
[null,"Loftshøjde","Lh","m",{"$f":"D_IndOlieK_Lh","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_Lh"]
[null,"Luftskifte","Ls","s-1",{"$f":"D_IndOlieK_Ls","v":8.2999999999999998E-5},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_Ls"]
[null,"Gulvbredde","lb","m",{"$f":"IndOlieK_Lb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_Lb"]
[null,"Gulvlængde","ll","m",{"$f":"IndOlieK_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_Ll"]
[null,"Volumenstrøm i beboelse","Qbeboelse","m³/s",{"$f":"B_IndOlieK_Ls*B_IndOlieK_Lh*B_IndOlieK_Lb*B_IndOlieK_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_qbb"]
[]
[null,"Krybekælder"]
[]
[null,null,"Forkortelse","Enhed","Værdi","Beregnet"]
[null,"Etageadskillelse",null,null,{"$f":"D_IndOlieKk_anv","v":0}]
[null,"Reduktionsfaktoren","Rkr",null,{"$f":"D_IndOlieKk_Rkr","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieKk_Rkr"]
[null,"Loftshøjde","Lh,kr","m",{"$f":"D_IndOlieKk_Lh","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieKk_Lh"]
[null,"Gulvbredde","lb,kr","m",{"$f":"D_IndOlieKk_Lb","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieKk_Lb"]
[null,"Gulvlængde","ll,kr","m",{"$f":"D_IndOlieKk_Ll","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieKk_Ll"]
[null,"Luftskifte","Ls,kr","s-1",{"$f":"D_IndOlieKk_Ls","v":{"$error":"#DIV/0!"}},{"$f":"(B_IndOlieK_qbb)/(B_IndOlieKk_Lh*(B_IndOlieKk_Lb*B_IndOlieKk_Ll))","v":{"$error":"#DIV/0!"}},null,null,null,"Ls,kr=(Lh·Ls·lb·ll)/(Lh,kr·Ls,kr·lb,kr·ll,kr)  idet Rkr=1",null,null,null,null,null,null,null,"B_IndOlieKk_Ls"]
[null,"Vol. strøm i krybekælder","Qbygn","m³/(s )",{"$f":"B_IndOlieKk_qbyg_berg","v":{"$error":"#DIV/0!"}},{"$f":"B_IndOlieKk_Ls*B_IndOlieKk_Ll*B_IndOlieKk_Lb*B_IndOlieKk_Lh","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieKk_qbyg"]
[null,"Vol. strøm mellem krybekælder og stueetage","q,gv","m³/(s·m² )",{"$f":"D_IndOlieK_qgv","v":{"$error":"#DIV/0!"}},{"$f":"IF(B_IndOlieKk_qbyg>B_IndOlieK_qbb/B_IndOlieKk_Rkr,B_IndOlieK_qbb/(B_IndOlieKk_Rkr*(B_IndOlieKk_Lb*B_IndOlieKk_Ll)),B_IndOlieKk_qbyg/(B_IndOlieKk_Lb*B_IndOlieKk_Ll))","v":{"$error":"#DIV/0!"}},null,null,null,"qgv=(Lh,kr·Ls,kr·lb,kr·ll,kr)/Rkr",null,null,null,null,null,null,null,"B_IndOlieK_qgv"]
[null,"Check af volumenstrøm",null,null,null,{"$f":"IF(B_IndOlieK_qgv*B_IndOlieKk_Lh>B_IndOlieKk_qbyg,\"FEJL: Luftstrømmen igennem etageadskillelsen er større end luftskiftet i krybekælderen\",\"\")","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_q_check"]
[null,"Beregnet reduktionsfaktor","R,kr",null,null,{"$f":"B_IndOlieK_qbb/(B_IndOlieK_qgv*B_IndOlieKk_Lb*B_IndOlieKk_Ll)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieKk_Rkr_bereg"]
[null,"Check af reduktionsfaktor",null,null,null,{"$f":"IF(B_IndOlieKk_Rkr_bereg<1,\"FEJL: Luftstrømmen igennem etageadskillelsen er større end luftudskiftet i beboelsen\",\"\")","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,"B_IndOlieK_Rkr_check"]
[]
[null,"Oliestoffer"]
[null,null,null,null,null,null,null,null,null,"B_IndOlie_Ci_n"]
[null,"Gruppe","Forureningskomponent",null,null,"Poreluftskoncentration ","Diffusionskoefficient luft","Flux gennem jorden (app. 5.3 ligning 80)","Luftkoncen-trationen i krybekælder\n(app. 5.3 ligning 81)","Totalt bidrag til indeluft","Afdamp-nings-kriterium","Overskridelse af kriteriet"]
[null,null,null,null,null,"CL","DL","Jz","Ckr","Ci"]
[null,null,null,null,null,"mg/m³","m²/s","mg/(m² s)","mg/m³","mg/m³","mg/m³"]
[50,"C5-C6",null,null,null,null,null,null,{"$f":"SUM(I233:I236)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J233:J236)","v":{"$error":"#VALUE!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},{"$f":"IndLigning80(F233,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G233,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H233/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I233*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},{"$f":"IndLigning80(F234,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G234,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H234/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I234*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},{"$f":"IndLigning80(F235,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G235,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H235/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I235*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},{"$f":"IndLigning80(F236,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G236,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H236/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I236*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[]
[510,"C6-C10",null,null,null,null,null,null,{"$f":"SUM(I239:I243)+SUM(I249:I251)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J239:J243)+SUM(J249:J251)","v":{"$error":"#VALUE!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_52","v":9.3000000000000007E-6},{"$f":"IndLigning80(F239,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G239,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H239/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I239*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},{"$f":"IF(ISNUMBER(K239),IF(J239>K239,J239/K239,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},{"$f":"IndLigning80(F240,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G240,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H240/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I240*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},{"$f":"IndLigning80(F241,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G241,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H241/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I241*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_54_ak","v":0.4},{"$f":"IF(ISNUMBER(K241),IF(J241>K241,J241/K241,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
["55A",">8 - 10, alifater",">8 - 10, alifater, Tung olie",null,null,{"$f":"D_Olie_55A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55A","v":5.5030901075876E-6},{"$f":"IndLigning80(F242,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G242,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H242/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I242*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["55B",null,">8 - 10, alifater, Olieblandinger",null,null,{"$f":"D_Olie_55B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55B","v":6.2232552378840063E-6},{"$f":"IndLigning80(F243,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G243,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H243/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I243*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},{"$f":"IndLigning80(F247,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G247,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H247/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I247*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},{"$f":"IndLigning80(F248,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G248,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H248/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I248*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[59,null,"Sum af xylener +ethylbenzen",null,null,null,null,null,{"$f":"I248+I247","v":{"$error":"#VALUE!"}},{"$f":"J248+J247","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_57_ak","v":0.1},{"$f":"IF(ISNUMBER(K249),IF(J249>K249,J249/K249,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
["60A",null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"IndLigning80(F250,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G250,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H250/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I250*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["60B",null,">8 -10, aromater,øvrige",null,null,{"$f":"D_Olie_60_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_60B","v":6.4381431991356133E-6},{"$f":"IndLigning80(F251,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G251,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H251/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I251*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[910,"C9-C10 aromater",null,null,null,null,null,null,{"$f":"SUM(I250:I251)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J250:J251)","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_60_ak","v":0.03},{"$f":"IF(ISNUMBER(K252),IF(J252>K252,J252/K252,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
[]
[1015,"C11-C15",null,null,null,null,null,null,{"$f":"SUM(I255:I266)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J255:J266)","v":{"$error":"#VALUE!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},{"$f":"IndLigning80(F255,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G255,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H255/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I255*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},{"$f":"IndLigning80(F257,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G257,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H257/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I257*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_103_ak","v":0.04},{"$f":"IF(ISNUMBER(K257),IF(J257>K257,J257/K257,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]
["104A",null,">10 - 12, aromater, øvrige, Tung Olie",null,null,{"$f":"D_Olie_104A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104A","v":5.9633499312903359E-6},{"$f":"IndLigning80(F258,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G258,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H258/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I258*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["104B",null,">10 - 12, aromater, øvrige, Olieblanding",null,null,{"$f":"D_Olie_104B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104B","v":5.5260438461528997E-6},{"$f":"IndLigning80(F259,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G259,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H259/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I259*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["105A",null,">12 - 16, alifater, Tung Olie",null,null,{"$f":"D_Olie_105a_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105A","v":4.3460519456567218E-6},{"$f":"IndLigning80(F260,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G260,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H260/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I260*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["105B",">12 - 16, alifater",">12 - 16, alifater, Olieblandinger",null,null,{"$f":"D_Olie_105B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105B","v":5.0933919872504982E-6},{"$f":"IndLigning80(F261,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G261,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H261/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I261*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},{"$f":"IndLigning80(F263,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G263,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H263/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I263*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},{"$f":"IndLigning80(F264,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G264,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H264/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I264*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["109A",null,">12 - 16, aromater,øvrige, Tung Olie",null,null,{"$f":"D_Olie_109A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109A","v":5.5027929670196982E-6},{"$f":"IndLigning80(F265,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G265,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H265/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I265*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["109B",null,">12 - 16, aromater,øvrige, Olieblandinger",null,null,{"$f":"D_Olie_109B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109B","v":5.9000000000000003E-6},{"$f":"IndLigning80(F266,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G266,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H266/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I266*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[]
[1520,"C16-C20",null,null,null,null,null,null,{"$f":"SUM(I270:I276)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J270:J276)","v":{"$error":"#VALUE!"}}]
["151A",">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"D_Olie_151A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151A","v":3.7468864349159863E-6},{"$f":"IndLigning80(F269,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G269,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H269/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I269*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["151B",null,">16 - 21, alifater",null,null,{"$f":"D_Olie_151B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151B","v":4.4721099862171762E-6},{"$f":"IndLigning80(F270,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G270,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H270/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I270*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},{"$f":"IndLigning80(F272,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G272,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H272/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I272*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},{"$f":"IndLigning80(F273,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G273,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H273/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I273*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},{"$f":"IndLigning80(F274,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G274,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H274/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I274*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},{"$f":"IndLigning80(F275,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G275,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H275/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I275*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},{"$f":"IndLigning80(F276,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G276,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H276/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I276*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[]
[2025,"C21-C25",null,null,null,null,null,null,{"$f":"SUM(I280:I281)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J280:J281)","v":{"$error":"#VALUE!"}}]
["201A",">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"D_Olie_201A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201A","v":3.6715492605442101E-6},{"$f":"IndLigning80(F279,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G279,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H279/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I279*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["201B",null,">21 - 25, alifater",null,null,{"$f":"D_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201B","v":3.9528308464137552E-6},{"$f":"IndLigning80(F280,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G280,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H280/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I280*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter"]
[2535,"C25-C35",null,null,null,null,null,null,{"$f":"SUM(I284:I293)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J284:J293)","v":{"$error":"#VALUE!"}}]
["251A",">25 - 35, alifater",">25 - 35, alifater, Tung olie",null,null,{"$f":"D_Olie_251A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251A","v":3.0055777156880082E-6},{"$f":"IndLigning80(F283,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G283,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H283/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I283*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
["251B",null,">25 - 35, alifater, Olieblandinger",null,null,{"$f":"D_Olie_251B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251B","v":3.6715492605442101E-6},{"$f":"IndLigning80(F284,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G284,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H284/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I284*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater"]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},{"$f":"IndLigning80(F286,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G286,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H286/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I286*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["259A",null,">25 - 35, aromater, øvrige, Tung olie",null,null,{"$f":"D_Olie_259A_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259A","v":5.5943064295556175E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["259B",null,">25 - 35, aromater, øvrige, Olieblandinger",null,null,{"$f":"D_Olie_259B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259B","v":4.4493993711079091E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[3540,">C35",null,null,null,null,null,null,{"$f":"SUM(I296:I297)","v":{"$error":"#VALUE!"}},{"$f":"SUM(J296:J297)","v":{"$error":"#VALUE!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},{"$f":"IndLigning80(F296,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G296,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H296/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I296*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},{"$f":"IndLigning80(F297,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G297,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H297/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I297*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[]
[2040,"C21-C35","Reflab4",null,null,null,null,null,{"$f":"I282+I278","v":{"$error":"#VALUE!"}},{"$f":"J282+J278","v":{"$error":"#VALUE!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand"]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},{"$f":"IndLigning80(F305,B_IndOlieK_X_tot,B_IndOlieK_N_tot,G305,1E-20)","v":{"$error":"#VALUE!"}},{"$f":"H305/(B_IndOlieKk_Lh*B_IndOlieKk_Ls)","v":{"$error":"#VALUE!"}},{"$f":"I305*B_IndOlieKk_Rkr_bereg","v":{"$error":"#VALUE!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[1,"Sum af kulbrinter",null,null,null,null,null,null,{"$f":"SUM(I304:I311)+I295+I282+I278+I268+I254+I238","v":{"$error":"#VALUE!"}},{"$f":"SUM(J304:J311)+J295+J282+J278+J268+J254+J238","v":{"$error":"#VALUE!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"IF(ISNUMBER(K313),IF(J313>K313,J313/K313,\"Nej\"),\" \")","v":{"$error":"#VALUE!"}}]

{"sheet":"Udskrift_Indeklima-Olie","index":46,"n_rows":137,"n_cols":11,"rows_kept":137,"cut":false,"hidden":true,"merged":[[31,2,31,3],[31,4,31,5],[31,6,31,7],[31,8,31,10],[33,6,33,7],[33,8,33,9],[33,10,33,11],[1,1,1,5],[1,8,1,11],[2,8,2,11],[2,1,2,5],[3,1,3,5],[4,1,4,11],[3,8,3,11],[29,0,29,1],[30,2,30,3],[30,4,30,5],[11,2,11,3],[11,4,11,5],[11,6,11,7],[11,8,11,9],[14,2,14,3],[14,4,14,5],[17,6,17,7],[17,8,17,9],[18,2,18,9],[19,8,19,9],[30,6,30,7],[37,6,37,7],[37,8,37,9],[37,10,37,11],[33,4,33,5],[37,12,37,14],[34,2,34,3],[34,6,34,7],[34,8,34,9],[34,10,34,11],[35,2,35,3],[35,6,35,7],[35,8,35,9],[35,10,35,11],[34,4,34,5],[35,4,35,5],[36,4,36,5],[37,4,37,5],[36,2,36,3],[36,6,36,7],[36,8,36,9],[36,10,36,11],[36,12,36,14],[37,2,37,3],[33,2,33,3],[40,12,40,14],[41,12,41,14],[38,2,38,3],[38,6,38,7],[38,8,38,9],[38,10,38,11],[38,12,38,14],[39,2,39,3],[39,6,39,7],[39,8,39,9],[39,10,39,11],[39,12,39,14],[38,4,38,5],[39,4,39,5],[42,2,42,3],[42,6,42,7],[42,8,42,9],[42,10,42,11],[43,2,43,3],[43,6,43,7],[43,8,43,9],[43,10,43,11],[40,2,40,3],[40,6,40,7],[40,8,40,9],[40,10,40,11],[40,4,40,5],[42,4,42,5],[43,4,43,5],[44,2,44,3],[44,6,44,7],[44,8,44,9],[44,10,44,11],[45,2,45,3],[45,6,45,7],[45,8,45,9],[45,10,45,11],[44,4,44,5],[45,4,45,5],[58,1,67,9],[69,1,78,9],[80,1,89,9],[46,2,46,3],[46,6,46,7],[46,8,46,9],[46,10,46,11],[48,2,48,3],[48,6,48,7],[48,8,48,9],[48,10,48,11],[46,4,46,5],[48,4,48,5],[51,8,51,11],[52,8,52,11],[51,1,51,5],[52,1,52,5],[27,15,27,18],[22,8,23,9],[6,2,6,3],[6,7,6,10],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[13,2,13,3],[13,4,13,5],[13,6,13,7],[13,8,13,9],[9,2,9,3],[9,8,9,9],[7,2,7,3],[7,8,7,9],[8,2,8,3],[8,8,8,9],[22,2,23,3],[17,2,17,3],[19,2,19,3],[14,6,14,7],[14,8,14,9],[17,4,17,5],[102,1,111,9],[91,1,100,9],[114,0,115,0],[114,3,115,4],[114,5,115,6],[116,3,116,4],[116,5,116,6],[117,3,117,4],[117,5,117,6],[118,5,118,6],[119,3,119,4],[119,5,119,6],[120,3,120,4],[120,5,120,6],[121,3,121,4],[121,5,121,6],[122,3,122,4],[122,5,122,6],[135,3,135,4],[135,5,135,6],[136,3,136,6],[70,0,71,0],[131,0,131,1],[131,3,131,4],[131,5,131,6],[132,3,132,4],[132,5,132,6],[133,3,133,4],[133,5,133,6],[134,3,134,4],[134,5,134,6],[123,3,123,4],[123,5,123,6],[124,3,124,4],[124,5,124,6],[125,3,125,4],[125,5,125,6],[126,3,126,4],[126,5,126,6],[129,3,130,4],[129,5,130,6],[118,3,118,4]]}
["Indeklima-Olie"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jordparametre",null,"Indtastede data angives med fed"]
["Kommentar",{"$f":"IF(D_IndOlie_Inf_ComUds,\"ja\",\"nej\")","v":"nej"},"Membran",null,null,null,null,"Kapilarbrydende lag"]
["Membran type",null,{"$f":"IF(AND(D_IndOlie_navnb_1_syst=\"\",IndOlie_My_Memb=\"\"),\"\",D_IndOlie_navnb_1)","v":""},null,null,"Jord type",null,null,{"$f":"IF(AND(D_IndOlie_navnb_2_syst=\"\",IndOlie_My_Kab_2=\"\"),\"\",D_IndOlie_navnb_2)","v":""}]
["Tykkelse",null,{"$f":"IF(D_IndOlie_Xb_1<>0,D_IndOlie_Xb_1,\"\")","v":""},null,"mm","Tykkelse",null,null,{"$f":"IF(D_IndOlie_Xb_2<>0,D_IndOlie_Xb_2,\"\")","v":""},null,"m"]
["Materialekonstant",null,{"$f":"IF(B_IndOlie_Nb_1<>0,D_IndOlie_Nb_1,\"\")","v":""},null,null,"Materialekonstant",null,null,{"$f":"IF(B_IndOlie_Nb_2<>0,D_IndOlie_Nb_2,\"\")","v":""}]
[]
["Kommentar",{"$f":"IF(D_IndOlie_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
["Jordtype",null,{"$f":"IF(AND(D_IndOlie_jordtype_1_syst=\"\",IndOlie_My_Jord1=\"\"),\"\",D_IndOlie_jordtype_1)","v":""},null,{"$f":"IF(AND(D_IndOlie_jordtype_2_syst=\"\",IndOlie_My_Jord2=\"\"),\"\",D_IndOlie_jordtype_2)","v":""},null,{"$f":"IF(AND(D_IndOlie_jordtype_3_syst=\"\",IndOlie_My_Jord3=\"\"),\"\",D_IndOlie_jordtype_3)","v":""},null,{"$f":"IF(AND(D_IndOlie_jordtype_4_syst=\"\",IndOlie_My_Jord4=\"\"),\"\",D_IndOlie_jordtype_4)","v":""}]
["Jordlag, Dybde fra",null,{"$f":"IF(D_IndOlie_lagtil_1<>0,D_IndOlie_lagfra_1,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_2<>0,D_IndOlie_lagfra_2,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_3<>0,D_IndOlie_lagfra_3,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_4<>0,D_IndOlie_lagfra_4,\"\")","v":""},null,"m u.t."]
["Jordlag, Dybde til",null,{"$f":"IF(D_IndOlie_lagtil_1<>0,D_IndOlie_lagtil_1,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_2<>0,D_IndOlie_lagtil_2,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_3<>0,D_IndOlie_lagtil_3,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_4<>0,D_IndOlie_lagtil_4,\"\")","v":""},null,"m u.t."]
["Poreluftvolumen","VL",{"$f":"IF(D_IndOlie_VL_1_syst<>\"\",D_IndOlie_VL_1_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VL1<>\"\",IndOlie_My_VL1,\"\")","v":""},{"$f":"IF(D_IndOlie_VL_2_syst<>\"\",D_IndOlie_VL_2_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VL2<>\"\",IndOlie_My_VL2,\"\")","v":""},{"$f":"IF(D_IndOlie_VL_3_syst<>\"\",D_IndOlie_VL_3_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VL3<>\"\",IndOlie_My_VL3,\"\")","v":""},{"$f":"IF(D_IndOlie_VL_4_syst<>\"\",D_IndOlie_VL_4_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VL4<>\"\",IndOlie_My_VL4,\"\")","v":""}]
["Vand-indhold","VV",{"$f":"IF(D_IndOlie_VV_1_syst<>\"\",D_IndOlie_VV_1_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VV1<>\"\",IndOlie_My_VV1,\"\")","v":""},{"$f":"IF(D_IndOlie_VV_2_syst<>\"\",D_IndOlie_VV_2_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VV2<>\"\",IndOlie_My_VV2,\"\")","v":""},{"$f":"IF(D_IndOlie_VV_3_syst<>\"\",D_IndOlie_VV_3_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VV3<>\"\",IndOlie_My_VV3,\"\")","v":""},{"$f":"IF(D_IndOlie_VV_4_syst<>\"\",D_IndOlie_VV_4_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_VV4<>\"\",IndOlie_My_VV4,\"\")","v":""}]
["Materialekonstant",null,{"$f":"IF(D_IndOlie_lagtil_1<>0,D_IndOlie_N_1,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_2<>0,D_IndOlie_N_2,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_3<>0,D_IndOlie_N_3,\"\")","v":""},null,{"$f":"IF(D_IndOlie_lagtil_4<>0,D_IndOlie_N_4,\"\")","v":""}]
[null,null,{"$f":"D_IndOlie_negativ_X_tot","v":" "}]
["Samlet materialekonstant"," KW",{"$f":"B_IndOlie_N_tot","v":{"$error":"#DIV/0!"}},null,null,"Samlet tykkelse af jordlag",null,null,{"$f":"D_IndOlie_X_tot","v":0},null,"m"]
[]
["Terrændæk",null,null,null,null,"Bygningsdata"]
["Kommentar",{"$f":"IF(D_IndOlie_Ter_ComUds,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(AND(D_IndOlie_Inddæk_syst=\"\",IndOlie_My_Inddæk=\"\"),\"\",D_IndOlie_Inddæk)","v":""},null,null,"Kommentar",null,{"$f":"IF(D_IndOlie_Ind_ComUds,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(IndOlie_My_anv=\"\",\"\",IndOlie_My_anv)","v":""}]
["Type af terrændæk",null,null,null,null,"Rumtype/anvendelse"]
["Betontværsnit (mm)","hb",{"$f":"IF(D_IndOlie_hb_syst<>\"\",D_IndOlie_hb_syst,\"\")","v":""},{"$f":"IF(IndOlie_My_hb<>\"\",D_IndOlie_hb,\"\")","v":""},null,"Loftshøjde (m)",null,"Lh",null,{"$f":"IF(D_IndOlie_Lh<>\"\",D_IndOlie_Lh,\"\")","v":0}]
[null,null,null,null,null,"Gulvbredde (m)",null,"lb",null,{"$f":"IF(D_IndOlie_Lb<>\"\",D_IndOlie_Lb,\"\")","v":0}]
["Trykforskel over \nbetondæk  (Pa)","DP",{"$f":"D_IndOlie_DP_Sys","v":5},{"$f":"IF(IndOlie_My_DP<>\"\",D_IndOlie_DP,\"\")","v":""},null,"Gulvlængde (m)",null,"ll",null,{"$f":"IF(D_IndOlie_Ll<>\"\",D_IndOlie_Ll,\"\")","v":0}]
["Øvrige detaljer se side 3",null,null,null,null,"Luftskifte (s-1)",null,"Ls",{"$f":"D_IndOlie_Ls_Sys","v":8.2999999999999998E-5},{"$f":"IF(IndOlie_My_Ls<>\"\",D_IndOlie_Ls,\"\")","v":""}]
[]
["Beregning: Indeklima"]
["Kommentar",{"$f":"IF(D_Olie_Kem_ComUds,\"ja\",\"nej\")","v":"nej"},"Målepunkt",null,"Dato",null,"Fri fase?",null,"Anvendt brugerdata"]
["Angiv signifikant ciffer",3,{"$f":"D_olie_målepunkt","v":""},null,{"$f":"D_olie_dato","v":""},null,{"$f":"D_Olie_FF","v":"Nej"},null,{"$f":"D_Udeolie_bruger","v":"Nej"}]
[]
[null,null,"Poreluftkonc.",null,"Poreluftkonc.\nunder gulv",null,"Total bidrag til indeluft",null,"Afdampnings\nkriteriet",null,"Over\nskridelse"]
["BTEX'er",null,"mg/m3",null,"mg/m3",null,"mg/m3",null,"mg/m3",null,"gange"]
["Benzen",null,{"$f":"IF(D_IndOlie_52_cl=0,0,(ROUND(D_IndOlie_52_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_52_cl))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_IndOlie_52_cp=0,0,(ROUND(D_IndOlie_52_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_52_cp))+1))))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D_IndOlie_52_ci=0,0,(ROUND(D_IndOlie_52_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_52_ci))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},null,{"$f":"D_IndOlie_omkr_52","v":{"$error":"#DIV/0!"}}]
["Toluen",null,{"$f":"IF(D_IndOlie_54_cl=0,0,(ROUND(D_IndOlie_54_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_54_cl))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_IndOlie_54_cp=0,0,(ROUND(D_IndOlie_54_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_54_cp))+1))))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D_IndOlie_54_ci=0,0,(ROUND(D_IndOlie_54_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_54_ci))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_54_ak","v":0.4},null,{"$f":"D_IndOlie_omkr_54","v":{"$error":"#DIV/0!"}}]
["Ethylbenzen",null,{"$f":"IF(D_IndOlie_58_cl=0,0,(ROUND(D_IndOlie_58_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_58_cl))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_IndOlie_58_cp=0,0,(ROUND(D_IndOlie_58_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_58_cp))+1))))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D_IndOlie_58_ci=0,0,(ROUND(D_IndOlie_58_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_58_ci))+1))))","v":{"$error":"#DIV/0!"}}]
["Sum Xylener",null,{"$f":"IF(D_IndOlie_57_cl=0,0,(ROUND(D_IndOlie_57_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_57_cl))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_IndOlie_57_cp=0,0,(ROUND(D_IndOlie_57_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_57_cp))+1))))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D_IndOlie_57_ci=0,0,(ROUND(D_IndOlie_57_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_57_ci))+1))))","v":{"$error":"#DIV/0!"}}]
["∑Xylener+Ethylbenzen",null,{"$f":"IF(D_IndOlie_59_cl=0,0,(ROUND(D_IndOlie_59_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_59_cl))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_IndOlie_59_cp=0,0,(ROUND(D_IndOlie_59_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_59_cp))+1))))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D_IndOlie_59_ci=0,0,(ROUND(D_IndOlie_59_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_59_ci))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_57_ak","v":0.1},null,{"$f":"D_IndOlie_omkr_59","v":{"$error":"#DIV/0!"}}]
["Naphtalen",null,{"$f":"IF(D_IndOlie_103_cl=0,0,(ROUND(D_IndOlie_103_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_103_cl))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_IndOlie_103_cp=0,0,(ROUND(D_IndOlie_103_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_103_cp))+1))))","v":{"$error":"#VALUE!"}},null,{"$f":"IF(D_IndOlie_103_ci=0,0,(ROUND(D_IndOlie_103_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_103_ci))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_103_ak","v":0.04},null,{"$f":"D_IndOlie_omkr_103","v":{"$error":"#DIV/0!"}}]
["Kulbrintefraktioner"]
["C6-C10",null,{"$f":"ROUND(D_IndOlie_510_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_510_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlie_510_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_510_cp))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlie_510_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_510_ci))+1))","v":{"$error":"#DIV/0!"}}]
["C10-C15",null,{"$f":"ROUND(D_IndOlie_1015_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_1015_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlie_1015_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_1015_cp))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlie_1015_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_1015_ci))+1))","v":{"$error":"#DIV/0!"}}]
["C15-C20",null,{"$f":"ROUND(D_IndOlie_1520_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_1520_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlie_1520_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_1520_cp))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlie_1520_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_1520_ci))+1))","v":{"$error":"#DIV/0!"}}]
["C20-C35",null,{"$f":"ROUND(D_IndOlie_2040_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_2040_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlie_2040_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_2040_cp))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlie_2040_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_2040_ci))+1))","v":{"$error":"#DIV/0!"}}]
["Sum af kulbrinter",null,{"$f":"ROUND(D_IndOlie_1_cl,indeolie_ciffer-(INT(LOG(D_IndOlie_1_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlie_1_cp,indeolie_ciffer-(INT(LOG(D_IndOlie_1_cp))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlie_1_ci,indeolie_ciffer-(INT(LOG(D_IndOlie_1_ci))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_1_ak","v":0.1},null,{"$f":"D_IndOlie_omkr_1","v":{"$error":"#DIV/0!"}}]
["Aromatiske kulbrinter "]
["C9-C10 aromatiske kulbrinter",null,{"$f":"D_IndOlie_910_cl","v":{"$error":"#DIV/0!"}},null,{"$f":"D_IndOlie_910_cp","v":{"$error":"#VALUE!"}},null,{"$f":"D_IndOlie_910_ci","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_60_ak","v":0.03},null,{"$f":"D_IndOlie_omkr_910","v":{"$error":"#DIV/0!"}}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_IndOlie_Jord_Com<>\"\",D_IndOlie_Jord_Com,\"\")","v":""}]
["om jordlag"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger om",{"$f":"IF(D_IndOlie_Inf_Com<>\"\",D_IndOlie_Inf_Com,\"\")","v":""}]
["Influenszone og membran"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Olie_Kem_Com<>\"\",D_Olie_Kem_Com,\"\")","v":""}]
["om forurening"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_IndOlie_Ter_Com<>\"\",D_IndOlie_Ter_Com,\"\")","v":""}]
["om terrændæk"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_IndOlie_Ind_Com<>\"\",D_IndOlie_Ind_Com,\"\")","v":""}]
["om bygningsdata"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Detailoplysninger om terrændæk"]
["Type af terrændæk",null,null,{"$f":"IF(D_IndOlie_Inddæk_syst<>0,D_IndOlie_Inddæk_syst,\"\")","v":""},null,{"$f":"IF(D_IndOlie_Inddæk<>0,D_IndOlie_Inddæk,\"\")","v":""}]
[]
["Relativ luftfugtighed",null,"RF",{"$f":"IF(D_IndOlie_RF_syst<>0,D_IndOlie_RF_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_RF<>\"\",D_IndOlie_RF,\"\")","v":""},null,"%"]
["Vand/cement-tallet",null,"v/c",{"$f":"IF(D_IndOlie_wc_syst<>0,D_IndOlie_wc_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_wc<>\"\",D_IndOlie_wc,\"\")","v":""}]
["Cementindhold",null,"CM",{"$f":"IF(D_IndOlie_CM_syst<>0,D_IndOlie_CM_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_CM<>\"\",D_IndOlie_CM,\"\")","v":""},null,"kg/m³"]
["Svindtid",null,"ts",{"$f":"IF(D_IndOlie_ts_syst<>0,D_IndOlie_ts_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_ts<>\"\",D_IndOlie_ts,\"\")","v":""},null,"døgn"]
["Materialekonst. for beton",null,"Nb",{"$f":"IF(D_IndOlie_Nb_syst<>0,D_IndOlie_Nb_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_Nb<>\"\",D_IndOlie_Nb,\"\")","v":""}]
["Armeringsdiameter",null,"da",{"$f":"IF(D_IndOlie_daCh<>0,D_IndOlie_daCh,\"\")","v":""},null,{"$f":"IF(Ind_My_da<>\"\",D_IndOlie_da,\"\")","v":""},null,"mm"]
["Armeringskonstant",null,"k",{"$f":"IF(D_IndOlie_k_syst<>0,D_IndOlie_k_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_k<>\"\",D_IndOlie_k,\"\")","v":""}]
["Afstand mellem \narmeringsjern",null,"Db",{"$f":"IF(D_IndOlie_Db_syst<>0,D_IndOlie_Db_syst,\"\")","v":""},null,{"$f":"IF(Ind_My_Db<>\"\",D_IndOlie_Db,\"\")","v":""},null,"mm"]
["Dynamisk viskositet af luft",null,"m",{"$f":"IF(D_IndOlie_my_syst<>0,D_IndOlie_my_syst,\"\")","v":1.8E-5},null,{"$f":"IF(Ind_My_my<>\"\",D_IndOlie_my,\"\")","v":""},null,"kg/m·s"]
["Elasticitetskoeff. Beton",null,"Eb",{"$f":"IF(D_IndOlie_Eb_syst<>0,D_IndOlie_Eb_syst,\"\")","v":20000},null,{"$f":"IF(Ind_My_Eb<>\"\",D_IndOlie_Eb,\"\")","v":""},null,"MPa"]
["Elasticitetskoeff. Stål (MPa)",null,"Es",{"$f":"IF(D_IndOlie_Es_syst<>0,D_IndOlie_Es_syst,\"\")","v":210000},null,{"$f":"IF(Ind_My_Es<>\"\",D_IndOlie_Es,\"\")","v":""},null,"MPa"]
[]
["Beregnede data om terrændæk"]
[null,null,null,"Beregnede værdier",null,"Indtastede (målte) værdier"]
[]
["Materialekonstant for terrændæk",null,"KN",{"$f":"D_IndOlie_Kn","v":{"$error":"#DIV/0!"}}]
["Revnevidde ",null,"w",{"$f":"IF(D_IndOlie_w_ber,D_IndOlie_w_ber,\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Ind_My_w<>\"\",D_IndOlie_w,\"\")","v":""},null,"mm"]
["Gnmsn. Revneafstand",null,"lw",{"$f":"IF(D_IndOlie_lw_ber,D_IndOlie_lw_ber,\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Ind_My_Lw<>\"\",D_IndOlie_lw,\"\")","v":""},null,"mm"]
["Total revnelængde",null,"ltot",{"$f":"IF(D_IndOlie_ltot_ber,D_IndOlie_ltot_ber,\"\")","v":""},null,{"$f":"IF(Ind_My_ltot<>\"\",D_IndOlie_ltot,\"\")","v":""},null,"mm"]
["Vol. strøm gennem beton",null,"qb",{"$f":"IF(D_IndOlie_q_ber,D_IndOlie_q_ber,\"\")","v":{"$error":"#VALUE!"}},null,{"$f":"IF(Ind_My_q<>\"\",D_IndOlie_q,\"\")","v":""},null,"m³/s"]
["Vol. strøm i bygningen",null,"qbyg",{"$f":"D_IndOlie_qbyg","v":0},null,null,null,"m³/s"]

{"sheet":"Udskrift_Indeklima_KK-Olie","index":47,"n_rows":92,"n_cols":11,"rows_kept":92,"cut":false,"hidden":true,"merged":[[1,8,1,11],[2,8,2,11],[1,1,1,5],[3,1,3,5],[3,8,3,11],[4,1,4,11],[2,1,2,5],[50,1,50,4],[51,1,51,4],[6,7,6,10],[7,2,7,3],[7,8,7,9],[11,2,11,3],[11,4,11,5],[11,6,11,7],[11,8,11,9],[32,10,32,11],[35,10,35,11],[38,10,38,11],[47,10,47,11],[45,10,45,11],[44,10,44,11],[42,2,42,3],[42,4,42,5],[90,1,99,9],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[13,2,13,3],[13,4,13,5],[13,6,13,7],[13,8,13,9],[18,2,18,3],[18,8,18,9],[21,2,22,3],[32,6,32,7],[32,8,32,9],[28,0,28,1],[29,2,29,3],[29,4,29,5],[29,6,29,7],[30,2,30,3],[30,4,30,5],[30,6,30,7],[30,8,30,10],[32,2,32,3],[32,4,32,5],[26,15,26,18],[21,8,21,9],[23,8,23,9],[24,8,24,9],[25,8,25,9],[14,2,14,3],[14,4,14,5],[14,6,14,7],[14,8,14,9],[17,2,17,3],[17,4,17,5],[17,6,17,7],[17,8,17,9],[23,2,23,3],[24,2,24,3],[25,2,25,3],[35,12,35,14],[33,2,33,3],[33,4,33,5],[33,6,33,7],[33,8,33,9],[33,10,33,11],[34,2,34,3],[34,4,34,5],[34,6,34,7],[34,8,34,9],[34,10,34,11],[35,2,35,3],[35,4,35,5],[35,6,35,7],[35,8,35,9],[38,12,38,14],[37,2,37,3],[37,4,37,5],[37,6,37,7],[37,8,37,9],[37,10,37,11],[37,12,37,14],[36,2,36,3],[36,4,36,5],[36,6,36,7],[36,8,36,9],[36,10,36,11],[36,12,36,14],[38,2,38,3],[38,4,38,5],[38,6,38,7],[38,8,38,9],[40,12,40,14],[41,2,41,3],[41,4,41,5],[41,6,41,7],[41,8,41,9],[41,10,41,11],[39,2,39,3],[39,4,39,5],[39,6,39,7],[39,8,39,9],[39,10,39,11],[39,12,39,14],[42,6,42,7],[42,8,42,9],[42,10,42,11],[43,2,43,3],[43,4,43,5],[43,6,43,7],[43,8,43,9],[43,10,43,11],[68,1,77,9],[79,1,88,9],[47,2,47,3],[47,4,47,5],[47,6,47,7],[47,8,47,9],[44,2,44,3],[44,4,44,5],[44,6,44,7],[44,8,44,9],[57,1,66,9],[45,2,45,3],[45,4,45,5],[45,6,45,7],[45,8,45,9]]}
["Indeklima-Olie"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jordparametre",null,"Indtastede data angives med fed"]
["Kommentar",{"$f":"IF( D_IndOlie_Ven_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Gulv i kr. kælder",null,null,null,null,"Membran"]
["Gulv type",null,{"$f":"IF(AND(D_IndOlieK_navnb_1_syst=\"\",IndOlieK_My_Memb=\"\"),\"\",D_IndOlieK_navnb_1)","v":""},null,null,"Membran type",null,null,{"$f":"IF(AND(D_IndOlieK_navnb_2_syst=\"\",IndOlieK_My_Memb=\"\"),\"\",D_IndOlieK_navnb_2)","v":""}]
["Tykkelse","mm",{"$f":"IF(D_IndOlieK_Xb_1_syst<>0,D_IndOlieK_Xb_1_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_Xb_1<>0,IndOlieK_My_Xb_1,\"\")","v":""},null,"Tykkelse",null,"mm",{"$f":"IF(D_IndOlieK_Xb_2_syst<>0,D_IndOlieK_Xb_2_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_Xb_2<>0,IndOlieK_My_Xb_2,\"\")","v":""}]
["Materialekonstant",null,{"$f":"IF(D_IndOlieK_Nb_1_syst<>0,D_IndOlieK_Nb_1_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_Nb_1<>0,IndOlieK_My_Nb_1,\"\")","v":""},null,"Materialekonstant",null,null,{"$f":"IF(D_IndOlieK_Nb_2_syst<>0,D_IndOlieK_Nb_2_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_Nb_2<>0,IndOlieK_My_Nb_2,\"\")","v":""}]
[]
[null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
["Jordtype",null,{"$f":"IF(AND(D_IndOlieK_jordtype_1_syst=\"\",IndOlieK_My_Jord1=\"\"),\"\",D_IndOlieK_jordtype_1)","v":""},null,{"$f":"IF(AND(D_IndOlieK_jordtype_2_syst=\"\",IndOlieK_My_Jord2=\"\"),\"\",D_IndOlieK_jordtype_2)","v":""},null,{"$f":"IF(AND(D_IndOlieK_jordtype_3_syst=\"\",IndOlieK_My_Jord3=\"\"),\"\",D_IndOlieK_jordtype_3)","v":""},null,{"$f":"IF(AND(D_IndOlieK_jordtype_4_syst=\"\",IndOlieK_My_Jord4=\"\"),\"\",D_IndOlieK_jordtype_4)","v":""}]
["Jordlag, Dybde fra",null,{"$f":"IF(D_IndOlieK_lagtil_1<>0,D_IndOlieK_lagfra_1,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_2<>0,D_IndOlieK_lagfra_2,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_3<>0,D_IndOlieK_lagfra_3,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_4<>0,D_IndOlieK_lagfra_4,\"\")","v":""},null,"m u.t."]
["Jordlag, Dybde til",null,{"$f":"IF(D_IndOlieK_lagtil_1<>0,D_IndOlieK_lagtil_1,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_2<>0,D_IndOlieK_lagtil_2,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_3<>0,D_IndOlieK_lagtil_3,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_4<>0,D_IndOlieK_lagtil_4,\"\")","v":""},null,"m u.t."]
["Poreluftvolumen","VL",{"$f":"IF(D_IndOlieK_VL_1_syst<>\"\",D_IndOlieK_VL_1_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VL1<>\"\",IndOlieK_My_VL1,\"\")","v":""},{"$f":"IF(D_IndOlieK_VL_2_syst<>\"\",D_IndOlieK_VL_2_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VL2<>\"\",IndOlieK_My_VL2,\"\")","v":""},{"$f":"IF(D_IndOlieK_VL_3_syst<>\"\",D_IndOlieK_VL_3_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VL3<>\"\",IndOlieK_My_VL3,\"\")","v":""},{"$f":"IF(D_IndOlieK_VL_4_syst<>\"\",D_IndOlieK_VL_4_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VL4<>\"\",IndOlieK_My_VL4,\"\")","v":""}]
["Vand-indhold","VV",{"$f":"IF(D_IndOlieK_VV_1_syst<>\"\",D_IndOlieK_VV_1_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VV1<>\"\",IndOlieK_My_VV1,\"\")","v":""},{"$f":"IF(D_IndOlieK_VV_2_syst<>\"\",D_IndOlieK_VV_2_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VV2<>\"\",IndOlieK_My_VV2,\"\")","v":""},{"$f":"IF(D_IndOlieK_VV_3_syst<>\"\",D_IndOlieK_VV_3_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VV3<>\"\",IndOlieK_My_VV3,\"\")","v":""},{"$f":"IF(D_IndOlieK_VV_4_syst<>\"\",D_IndOlieK_VV_4_syst,\"\")","v":""},{"$f":"IF(IndOlieK_My_VV4<>\"\",IndOlieK_My_VV4,\"\")","v":""}]
["Materialekonstant",null,{"$f":"IF(D_IndOlieK_lagtil_1<>0,D_IndOlieK_N_1,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_2<>0,D_IndOlieK_N_2,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_3<>0,D_IndOlieK_N_3,\"\")","v":""},null,{"$f":"IF(D_IndOlieK_lagtil_4<>0,D_IndOlieK_N_4,\"\")","v":""}]
["Samlet materialekonstant"," KW",{"$f":"B_IndOlieK_N_tot","v":{"$error":"#DIV/0!"}},null,null,null,null,"Samlet tykkelse af jordlag",{"$f":"D_IndOlieK_X_tot","v":0},null,"m"]
[]
["Bygningsdata",null,"Stueetage",null,null,null,"Kommentar",null,"Krybekælder"]
["Kommentar",{"$f":"IF( D_IndOlie_Ven_Byg_ComUds,\"ja\",\"nej\")","v":"nej"},{"$f":"IF(D_IndOlieK_anv<>0,D_IndOlieK_anv,\"\")","v":""},null,null,null,"Etageadskillelse",null,{"$f":"IF(D_IndOlieKk_anv<>0,D_IndOlieKk_anv,\"\")","v":""}]
["Rumtype/anvendelse",null,null,null,null,null,"Reduktionsfaktor","Rkr",{"$f":"IF(D_IndOlieKk_Rkr<>0,D_IndOlieKk_Rkr,\"\")","v":""},{"$f":"IF(IndOlieKk_Rkr<>\"\",IndOlieKk_Rkr,\"\")","v":""}]
["Loftshøjde","Lh",{"$f":"IF(D_IndOlieK_Lh<>0,D_IndOlieK_Lh,\"\")","v":""},null,"m",null,"Loftshøjde","Lh",{"$f":"IF(D_IndOlieKk_Lh<>0,D_IndOlieKk_Lh,\"\")","v":""},null,"m"]
["Gulvbredde","lb",{"$f":"IF(D_IndOlieK_Lb<>0,D_IndOlieK_Lb,\"\")","v":""},null,"m",null,"Gulvbredde","lb",{"$f":"IF(D_IndOlieKk_Lb<>0,D_IndOlieKk_Lb,\"\")","v":""},null,"m"]
["Gulvlængde","ll",{"$f":"IF(D_IndOlieK_Ll<>0,D_IndOlieK_Ll,\"\")","v":""},null,"m",null,"Gulvlængde","ll",{"$f":"IF(D_IndOlieKk_Ll<>0,D_IndOlieKk_Ll,\"\")","v":""},null,"m"]
["Luftskifte","Ls",{"$f":"D_IndOlieK_Ls_syst","v":8.2999999999999998E-5},{"$f":"IF(IndK_Ls<>\"\",D_IndOlieK_Ls,\"\")","v":""},"m³/s",null,"Luftskifte","Ls",{"$f":"D_IndOlieKk_Ls_berg","v":{"$error":"#DIV/0!"}},{"$f":"IF(IndOlieKk_Ls<>\"\",D_IndOlieKk_Ls,\"\")","v":""},"m³/s"]
[null,null,null,null,null,null,"Volumenstrøm gennem etageadskillelsen","qgv",{"$f":"IF(D_IndOlieK_qgv_beregn<>0,D_IndOlieK_qgv_beregn,\"\")","v":{"$error":"#DIV/0!"}},{"$f":"IF(IndOlieK_qgv<>0,IndOlieK_qgv,\"\")","v":""},"m³/s"]
["Beregning: Indeklima"]
["Kommentar",{"$f":"IF( D_Olie_Kem_ComUds,\"ja\",\"nej\")","v":"nej"},"Målepunkt",null,"Dato",null,"Fri fase?",null,"Anvendt brugerdata"]
["Angiv signifikant ciffer",2,{"$f":"D_olie_målepunkt","v":""},null,{"$f":"D_olie_dato","v":""},null,{"$f":"D_Olie_FF","v":"Nej"},null,{"$f":"D_Udeolie_bruger","v":"Nej"}]
[]
[null,null,"Poreluftkonc.",null,"Luftkonc. i krybekælder\nunder gulv",null,"Total bidrag til udeluft",null,"Afdampnings\nkriteriet",null,"Over\nskridelse"]
["BTEX'er",null,"mg/m3",null,"mg/m3",null,"mg/m3",null,"mg/m3",null,"gange"]
["Benzen",null,{"$f":"ROUND(D_IndOlie_52_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_52_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_52_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_52_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_52_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_52_ci))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},null,{"$f":"D_IndOlieK_omkr_52","v":{"$error":"#VALUE!"}}]
["Toluen",null,{"$f":"ROUND(D_IndOlie_54_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_54_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_54_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_54_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_54_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_54_ci))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"D_Olie_54_ak","v":0.4},null,{"$f":"D_IndOlieK_omkr_54","v":{"$error":"#VALUE!"}}]
["Ethylbenzen",null,{"$f":"ROUND(D_IndOlie_58_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_58_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_58_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_58_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_58_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_58_ci))+1))","v":{"$error":"#VALUE!"}}]
["Sum Xylener",null,{"$f":"ROUND(D_IndOlie_57_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_57_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_57_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_57_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_57_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_57_ci))+1))","v":{"$error":"#VALUE!"}}]
["∑Xylener+Ethylbenzen",null,{"$f":"ROUND(D_IndOlie_59_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_59_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_59_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_59_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_59_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_59_ci))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"D_Olie_57_ak","v":0.1},null,{"$f":"D_IndOlieK_omkr_59","v":{"$error":"#VALUE!"}}]
["Naphtalen",null,{"$f":"ROUND(D_IndOlie_103_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_103_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_103_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_103_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_103_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_103_ci))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"D_Olie_103_ak","v":0.04},null,{"$f":"D_IndOlieK_omkr_103","v":{"$error":"#VALUE!"}}]
["Kulbrintefraktioner"]
["C6-C10",null,{"$f":"ROUND(D_IndOlie_510_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_510_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_510_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_510_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_510_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_510_ci))+1))","v":{"$error":"#VALUE!"}}]
["C10-C15",null,{"$f":"ROUND(D_IndOlie_1015_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_1015_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_1015_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_1015_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_1015_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_1015_ci))+1))","v":{"$error":"#VALUE!"}}]
["C15-C20",null,{"$f":"ROUND(D_IndOlie_1520_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_1520_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_1520_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_1520_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_1520_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_1520_ci))+1))","v":{"$error":"#VALUE!"}}]
["C20-C35",null,{"$f":"ROUND(D_IndOlie_2040_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_2040_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_2040_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_2040_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_2040_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_2040_ci))+1))","v":{"$error":"#VALUE!"}}]
["Sum af kulbrinter",null,{"$f":"ROUND(D_IndOlie_1_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_1_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_1_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_1_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_1_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_1_ci))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"D_Olie_1_ak","v":0.1},null,{"$f":"D_IndOlieK_omkr_1","v":{"$error":"#VALUE!"}}]
["Aromatiske kulbrinter "]
["C9-C10 aromatiske kulbrinter",null,{"$f":"ROUND(D_IndOlie_910_cl,indeolieK_ciffer-(INT(LOG(D_IndOlie_910_cl))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_IndOlieK_910_ckr,indeolieK_ciffer-(INT(LOG(D_IndOlieK_910_ckr))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"ROUND(D_IndOlieK_910_ci,indeolieK_ciffer-(INT(LOG(D_IndOlieK_910_ci))+1))","v":{"$error":"#VALUE!"}},null,{"$f":"D_Olie_60_ak","v":0.03},null,{"$f":"D_IndOlieK_omkr_910","v":{"$error":"#VALUE!"}}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_IndOlie_Ven_Jord_Com<>\"\",D_IndOlie_Ven_Jord_Com,\"\")","v":""}]
["om jordlag"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_IndOlie_Ven_Byg_Com<>\"\",D_IndOlie_Ven_Byg_Com,\"\")","v":""}]
["om stueetage"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_IndOlie_Ven_Kryb_Com<>\"\",D_IndOlie_Ven_Kryb_Com,\"\")","v":""}]
["om krybekælder"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Olie_Kem_Com<>\"\",D_Olie_Kem_Com,\"\")","v":""}]
["om forurening"]

{"sheet":"Vejledning_Indeklima-Olie","index":48,"n_rows":154,"n_cols":2,"rows_kept":154,"cut":false,"hidden":true,"merged":[[138,1,139,11],[142,1,143,11],[146,1,150,11],[153,1,153,10],[99,1,101,10],[104,1,109,11],[112,1,113,11],[115,1,123,11],[126,1,136,11],[55,1,56,11],[95,1,96,11],[79,1,81,5],[83,1,83,10],[84,1,87,5],[89,1,89,10],[90,1,92,10],[94,1,94,11],[60,1,62,5],[64,1,67,5],[69,1,74,5],[76,1,77,5],[58,1,58,11],[59,1,59,5],[47,1,47,11],[49,1,49,10],[50,1,52,11],[54,1,54,11],[1,1,1,11],[2,1,4,11],[5,1,5,11],[6,1,7,11],[9,1,9,11],[11,1,11,5],[12,1,23,5],[24,1,25,5],[27,1,40,5],[42,1,42,10],[43,1,45,11]]}
[null,"Vejledning  - Indeklima"]
[null,"Formål"]
[null,"I dette ark kan der foretages beregning af bidraget til indeklimaet fra en forurening der afdamper gennem den umættet zone, og trænger ind i en bygning. Beregningerne kan foretages for bygninger med et betondæk (enten kælderdæk eller terrændæk) eller for bygninger med krybekælder.\n\nNærmere detaljer om beregningerne er beskrevet i Miljørapport. \"Opgradering af JAGG. Indeklimamodul 2010\". Miljøstyrelsen."]
[]
[]
[]
[null,"Nærmere detaljer om beregningerne er beskrevet i Miljørapport. \"Opgradering af JAGG. Indeklimamodul 2010\". Miljøstyrelsen."]
[]
[]
[null,"Beregninger for betondæk"]
[]
[null,"Umættet zone:"]
[null,"Den umættede zone som forureningen skal afdampe gennem skal indledningsvis beskrives. Den umættede zone medtager både de jordlag som findes mellem forureningen og betondækket, et eventuelt kapillarbrydende lag og en eventuel membran. De ønskede lag kan vælges som standardtyper ved at klikke på knappen \"Jordtype\", \"Membran\" eller \"Kapillarbrydende lag\". Alternativt kan der vælges lag fra \"Egen Liste\", eller der kan manuelt indtastes værdier i de hvide felter. Se iøvrigt bemærkninger om anvendelse af valglister under afsnittet generelt.\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Når det ønskede lag er valgt, angives lagets tykkelse, porøsitet og/eller materialekonstant"]
[]
[]
[null,"NB! I beregningerne af gastransport i den umættede zone kan der medtages nedbrydning, hvis der under fanebladet enkeltstodffer indtastes en nedbrydnings-konstant for det pågældende stof. Der må kun anven-des lokalitetsspecifikke nedbrydningskonstanter i beregningen. Såfremt der ikke haves en lokalitets-specifik nedbrydningskonstant sættes nedbrydningen til \"0\". \nDet skal porienteres, at nedbrydningskonstanter fra de andre moduler (grundvand og vertikal transport) ikke kan anvendes i indeklimamodulets beregninger, da nedbrydningen i beregnes i forhold til poreluftkoncen-trationen og ikke som i de andre i moduler forhold til porevandskoncentrationen"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Terrændæk:"]
[null,"Det ønskede betondæk kan vælges som standardtyper ved at klikke på knappen \"Terrændæk\". Alternativt kan der vælges dæktyper fra \"Egen Liste\", eller der kan manuelt indtastes værdier i de hvide felter. Tykkelsen af dækket indtastes."]
[]
[]
[]
[null,"Såfremt man ønsker at se eller rette de detaljerede data om terrændækket klikkes på knappen \"vis detailoplysninger\"\n"]
[]
[null,"Bygningsdata:"]
[null,"Oplysninger om det/de rum som der ønskes risikovurderet i forhold til indtastes. Såfremt der beregnes på et ikke armeret betongulv, skal størrelsen af betondækket indtastes. Betondækkets størrelse er ikke nødvendigvis det samme som husets fodaftryk. Bygningen vil oftest bestå af flere mindre betondæk, opdelt af fundamentet."]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata for poreluft overføres som modelstoffer fra arket \"Oliestoffer\". Beregningerne foretages på modelstofferne og omregnes herefter til kulbrintefraktionen"]
[]
[]
[null,"Beregninger for krybekælder"]
[null,"Umættet zone:"]
[null,"Som beskrevet under afsnittet \"Beregninger for betondæk\" skal den umættede zone indledningsvis beskrives.\n"]
[]
[]
[]
[null,"Ved beregninger med krybekælder medtager den umættede zone både de jordlag som findes mellem forureningen og betondækket, en eventuel membran, samt et eventuelt gulv i krybekælderen."]
[]
[]
[]
[]
[null,"De ønskede lag kan vælges som standardtyper ved at klikke på knappen \"Jordtype\", \"Membran\" eller \"Beton type\". Alternativt kan der vælges lag fra \"Egen Liste\", eller der kan manuelt indtastes værdier i de hvide felter. Se iøvrigt bemærkninger om anvendelse af valglister under afsnittet generelt.\n"]
[]
[]
[]
[]
[]
[]
[null,"Når det ønskede lag er valgt, angives lagets tykkelse, porøsitet og/eller materialekonstant"]
[]
[]
[null,"NB! I beregningerne af gastransport i den umættede zone kan der medtages nedbrydning. Se nærmere herom under afsnittet \"Beregninger for betondæk\"."]
[]
[]
[]
[null,"Bygningsdata:"]
[null,"Oplysninger om etagen over krybekælderen indtastes. Hvis forureningens fordeling i krybekælderen  ikke er kendt, tages der udgangspunkt i at hele stueetagen påvirkes."]
[]
[]
[]
[]
[null,"Krybekælder:"]
[null,"Oplysninger om krybekælderen indtastes. Hvis forureningens fordeling i krybekælderen  ikke er kendt, tages der udgangspunkt i at hele krybekælderen påvirkes. Etageadskildelsen mellem krybekælder og stueetage vælges fra standardvalglisten"]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata for poreluft overføres som modelstoffer fra arket \"Oliestoffer\". Beregningerne foretages på modelstofferne og omregnes herefter til kulbrintefraktionen"]
[]
[]
[null,"Generelt"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under Enkeltstof-modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under Enkeltstof-modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikkke på den ønskede værdi\n· At vælge en forekomst ved at skreve dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiskestoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet.Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lysseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"Sletning af enkeltværdier:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne incl. resultat af mellemberegninger"]

{"sheet":"Udeluft-Olie","index":49,"n_rows":85,"n_cols":35,"rows_kept":85,"cut":false,"hidden":true,"merged":[[60,40,60,41],[62,40,62,41],[59,40,59,41],[55,13,56,17],[55,23,57,25],[70,40,70,41],[73,40,73,41],[66,40,66,41],[66,23,66,25],[64,19,64,20],[64,23,64,25],[68,23,68,25],[66,14,66,16],[64,40,64,41],[86,40,86,41],[84,40,84,41],[80,40,80,41],[77,40,77,41],[78,40,78,41],[74,40,74,41],[76,40,76,41],[79,19,79,20],[79,23,79,25],[62,7,62,8],[66,19,66,20],[62,14,62,16],[70,14,70,16],[62,19,62,20],[68,7,68,8],[77,19,77,20],[77,23,77,25],[64,14,64,16],[70,23,70,25],[73,23,73,25],[70,7,70,8],[70,10,70,11],[70,19,70,20],[75,7,75,8],[75,10,75,11],[75,19,75,20],[66,7,66,8],[64,10,64,11],[64,7,64,8],[62,10,62,11],[68,14,68,16],[68,19,68,20],[62,23,62,25],[84,7,84,8],[75,23,75,25],[73,7,73,8],[73,10,73,11],[84,10,84,11],[84,19,84,20],[81,7,81,8],[81,14,81,16],[81,19,81,20],[81,23,81,25],[77,7,77,8],[77,10,77,11],[79,14,79,16],[73,14,73,16],[75,14,75,16],[77,14,77,16],[73,19,73,20],[79,7,79,8],[84,23,84,25],[84,14,84,16],[79,10,79,11],[37,0,38,4],[38,19,38,20],[38,22,38,23],[28,25,30,26],[28,28,30,29],[28,31,30,32],[29,19,29,20],[28,6,29,8],[29,22,29,23],[28,22,28,23],[28,19,28,20],[30,6,30,8],[30,19,30,20],[30,22,30,23],[37,19,37,20],[37,22,37,23],[38,25,38,26],[32,31,32,32],[28,10,30,11],[28,16,30,17],[30,13,30,14],[15,31,15,32],[16,6,17,8],[20,25,22,26],[20,28,22,29],[20,31,22,32],[21,19,21,20],[21,22,21,23],[22,19,22,20],[20,22,20,23],[22,22,22,23],[22,6,22,8],[15,10,15,11],[15,13,15,14],[15,16,15,17],[15,19,15,20],[15,22,15,23],[18,6,18,8],[15,25,15,26],[15,28,15,29],[18,19,18,20],[18,22,18,23],[16,19,16,20],[16,22,16,23],[16,25,18,26],[10,7,12,31],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[13,10,14,11],[13,13,14,14],[13,16,14,17],[13,19,14,20],[13,22,14,23],[13,25,14,26],[13,27,14,30],[13,31,14,32],[14,6,14,8],[9,7,9,23],[20,6,21,8],[26,22,26,23],[24,22,24,23],[24,19,24,20],[20,10,22,11],[24,10,26,11],[24,16,26,17],[18,10,18,11],[18,13,18,14],[22,13,22,14],[26,13,26,14],[16,16,18,17],[20,16,22,17],[26,6,26,8],[20,19,20,20],[24,6,25,8],[59,10,59,11],[55,18,56,21],[58,14,58,16],[60,14,60,16],[58,23,58,25],[16,28,18,29],[16,31,18,32],[17,19,17,20],[17,22,17,23],[25,22,25,23],[26,19,26,20],[24,25,26,26],[24,28,26,29],[88,7,88,25],[24,31,26,32],[25,19,25,20],[40,19,40,20],[40,25,40,26],[42,25,42,26],[45,7,46,32],[48,7,48,11],[32,16,32,17],[40,22,40,23],[42,19,42,20],[42,22,42,23],[60,7,60,8],[60,10,60,11],[60,19,60,20],[60,23,60,25],[49,7,49,11],[51,7,51,11],[53,7,53,11],[55,6,56,9],[55,10,56,11],[58,7,58,8],[58,19,58,20],[57,10,57,11]]}
["Beregning af udeluftkoncentrationen - Oliestoffer"]
[]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[]
["Jordparametre",null,null,null,null,null,null,"Indtast data om jordlag mellem prøvetagningspunktet og jordoverfladen"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Jordlag Dybde fra",null,null,"Jordlag Dybde til",null,null,"Lag-tykkelse",null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,"Volumen\naf jordskellet",null,null,null,"Materiale-konstant"]
[null,null,null,null,null,null,"Jordtype"]
[null,null,null,null,null,null,null,null,null,null,"m u.t",null,null,"m u.t",null,null,"(m)",null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ",null,null,"N"]
[null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_jordtype_syst1<>\"\",D_UdeOlie_jordtype_syst1,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"D_UdeOlie_X_1","v":0},null,null,{"$f":"IF(D_UdeOlie_VL_int1<>\"\",D_UdeOlie_VL_int1,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_int1<>\"\",D_UdeOlie_VV_int1,\"\")","v":""},null,null,{"$f":"D_UdeOlie_porositet_1","v":0},null,null,{"$f":"D_UdeOlie_VJ_1","v":0},null,null,{"$f":"D_UdeOlie_N_1","v":0}]
["",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_VL_syst1<>\"\",D_UdeOlie_VL_syst1,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_syst1<>\"\",D_UdeOlie_VV_syst1,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_udeolie_mangeljt_1","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(UdeOlie_jord_dt1),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VL1),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VV1),\"Tjek decimal\",\"\")))","v":""}]
[]
[null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_jordtype_syst2<>\"\",D_UdeOlie_jordtype_syst2,\"\")","v":""},null,null,null,{"$f":"D_UdeOlie_lagfra_2","v":0},null,null,null,null,null,{"$f":"D_UdeOlie_X_2","v":0},null,null,{"$f":"IF(D_UdeOlie_VL_int2<>\"\",D_UdeOlie_VL_int2,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_int2<>\"\",D_UdeOlie_VV_int2,\"\")","v":""},null,null,{"$f":"D_UdeOlie_porositet_2","v":0},null,null,{"$f":"D_UdeOlie_VJ_2","v":0},null,null,{"$f":"D_UdeOlie_N_2","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_VL_syst2<>\"\",D_UdeOlie_VL_syst2,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_syst2<>\"\",D_UdeOlie_VV_syst2,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_udeolie_mangeljt_2","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(UdeOlie_jord_dt2),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VL2),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VV2),\"Tjek decimal\",\"\")))","v":""}]
[]
[null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_jordtype_syst3<>\"\",D_UdeOlie_jordtype_syst3,\"\")","v":""},null,null,null,{"$f":"D_UdeOlie_lagfra_3","v":0},null,null,null,null,null,{"$f":"D_UdeOlie_X_3","v":0},null,null,{"$f":"IF(D_UdeOlie_VL_int3<>\"\",D_UdeOlie_VL_int3,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_int3<>\"\",D_UdeOlie_VV_int3,\"\")","v":""},null,null,{"$f":"D_UdeOlie_porositet_3","v":0},null,null,{"$f":"D_UdeOlie_VJ_3","v":0},null,null,{"$f":"D_UdeOlie_N_3","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_VL_syst3<>\"\",D_UdeOlie_VL_syst3,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_syst3<>\"\",D_UdeOlie_VV_syst3,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_udeolie_mangeljt_3","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(UdeOlie_jord_dt3),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VL3),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VV3),\"Tjek decimal\",\"\")))","v":""}]
[]
[null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_jordtype_syst4<>\"\",D_UdeOlie_jordtype_syst4,\"\")","v":""},null,null,null,{"$f":"D_UdeOlie_lagfra_4","v":0},null,null,null,null,null,{"$f":"D_UdeOlie_X_4","v":0},null,null,{"$f":"IF(D_UdeOlie_VL_int4<>\"\",D_UdeOlie_VL_int4,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_syst4<>\"\",D_UdeOlie_VV_int4,\"\")","v":""},null,null,{"$f":"D_UdeOlie_porositet_4","v":0},null,null,{"$f":"D_UdeOlie_VJ_4","v":0},null,null,{"$f":"D_UdeOlie_N_4","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_UdeOlie_VL_syst4<>\"\",D_UdeOlie_VL_syst4,\"\")","v":""},null,null,{"$f":"IF(D_UdeOlie_VV_syst4<>\"\",D_UdeOlie_VV_syst4,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_udeolie_mangeljt_4","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(UdeOlie_jord_dt4),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VL4),\"Tjek decimal\",IF(ISTEXT(UdeOlie_My_VV4),\"Tjek decimal\",\"\")))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_udeOlie_negativ_x","v":" "}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Samlede lagtykkelse",null,{"$f":"D_UdeOlie_X_tot","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Samlede ækvivalente jordtykkelse",null,{"$f":"D_UdeOlie_N_tot","v":{"$error":"#DIV/0!"}}]
[]
[]
["Det forurenede område",null,null,null,null,null,null,"Indtast data om det forurenede område, eller anvend standardværdier"]
[]
["Længde af det \nforurenede område",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Standard ",null,null,"Brugerdata",null,null,"Anvendt i beregning"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"l",null,{"$f":"D_UdeOlie_l_syst","v":100},null,null,null,null,null,{"$f":"D_UdeOlie_l","v":100},null,null,"m"]
[]
["Opblandingshøjde ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"h",null,{"$f":"D_UdeOlie_h_syst","v":8},null,null,null,null,null,{"$f":"D_UdeOlie_h","v":8},null,null,"m"]
[]
["Opblandingshøjde/længde",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"h/l",null,{"$f":"D_UdeOlie_hl_syst","v":0.08},null,null,{"$f":"D_UdeOlie_hl","v":0.08},null,null,{"$f":"D_UdeOlie_hl","v":0.08}]
[]
[]
["Beregning: Udeluft",null,null,null,null,null,null,"Data for olieforureningen er overført fra fugacitetsmodulet \n"]
[]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"IF(Olie_målepunkt<>\"\",D_olie_målepunkt,\"\")","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"IF(Olie_dato<>\"\",D_olie_dato,\"\")","v":""}]
[]
["Fri fase?",null,null,null,null,null,null,{"$f":"D_Olie_FF","v":"Nej"}]
[]
["Anvendt Brugerdata?",null,null,null,null,null,null,{"$f":"D_Udeolie_bruger","v":"Nej"}]
[]
[null,null,null,null,null,null,"Porelufts-\nkonc.",null,null,null,null,null,null,"Totalt bidrag \ntil udeluft",null,null,null,null,"Afdampnings-\nkriterie",null,null,null,null,"Over\nskridelse \naf kriteriet"]
[]
[]
[null,null,null,null,null,null,null,"mg/m³",null,null,null,null,null,null,"mg/m³",null,null,null,null,"mg/m³",null,null,null,"gange"]
["BTEX'er"]
[null,"Benzen",null,null,null,null,null,{"$f":"D_Udeolie_CF_52","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_Udeolie_CL_52","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},null,null,null,{"$f":"D_udeolie_overskr_52","v":{"$error":"#DIV/0!"}}]
[]
[null,"Toluen",null,null,null,null,null,{"$f":"D_Udeolie_CF_54","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_CL_54","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Olie_54_ak","v":0.4},null,null,null,{"$f":"D_udeolie_overskr_54","v":{"$error":"#DIV/0!"}}]
[]
[null,"Ethylbenzen",null,null,null,null,null,{"$f":"D_udeolie_cf_58","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_CL_58","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum Xylener",null,null,null,null,null,{"$f":"D_Udeolie_Cf_57","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_CL_57","v":{"$error":"#DIV/0!"}}]
[]
[null,"∑Xylener+Ethylbenzen",null,null,null,null,null,{"$f":"D_udeolie_cf_57a","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_cl_57a","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Olie_57_ak","v":0.1},null,null,null,{"$f":"D_udeolie_overskr_57a","v":{"$error":"#DIV/0!"}}]
[]
[null,"Naphthalen",null,null,null,null,null,{"$f":"D_Udeolie_Cf_103","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_CL_103","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Olie_103_ak","v":0.04},null,null,null,{"$f":"D_udeolie_overskr_103","v":{"$error":"#DIV/0!"}}]
[]
["Kulbrintefraktioner"]
[null,"C6-C10",null,null,null,null,null,{"$f":"D_Olie_510_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_cf_510","v":{"$error":"#DIV/0!"}}]
[]
[null,"C10-C15",null,null,null,null,null,{"$f":"D_Olie_1015_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_cf_1015","v":{"$error":"#DIV/0!"}}]
[]
[null,"C15-C20",null,null,null,null,null,{"$f":"D_Olie_1520_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_Udeolie_cf_1520","v":{"$error":"#DIV/0!"}}]
[]
[null,"C20-C35",null,null,null,null,null,{"$f":"D_udeolie_cl_2040","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_cf_2040","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af kulbrinter",null,null,null,null,null,{"$f":"D_Olie_1_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_Udeolie_cf_1","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Olie_1_ak","v":0.1},null,null,null,{"$f":"D_udeolie_overskr_1","v":{"$error":"#DIV/0!"}}]
[]
["Aromatiske kulbrinter "]
[null,"C9-C10 aromatiske kulbr.",null,null,null,null,null,{"$f":"D_Olie_910_cl","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,{"$f":"D_udeolie_cf_910","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Olie_60_ak","v":0.03},null,null,null,{"$f":"D_Udeolie_overskr_910","v":{"$error":"#DIV/0!"}}]

{"sheet":"Dataark_Udeluft-Olie","index":50,"n_rows":125,"n_cols":24,"rows_kept":125,"cut":false,"hidden":true,"merged":[[40,1,40,16],[25,2,25,3],[26,2,26,3],[28,1,28,16],[23,1,23,16],[1,1,1,16],[3,1,3,16],[5,4,5,7],[5,8,5,11],[5,12,5,15],[5,16,5,19]]}
[]
[null,"Dataark - UdeOlieluft",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","SAMLET"]
[null,"Jordtype",null,null,null,null,{"$f":"UdeOlie_My_jord1","v":0},{"$f":"IF(ISTEXT(G8),G8,F8)","v":0},null,null,{"$f":"UdeOlie_My_jord2","v":0},{"$f":"IF(ISTEXT(K8),K8,J8)","v":0},null,null,{"$f":"UdeOlie_My_jord3","v":0},{"$f":"IF(ISTEXT(O8),O8,N8)","v":0},null,null,{"$f":"UdeOlie_My_jord4","v":0},{"$f":"IF(ISTEXT(S8),S8,R8)","v":0},null,null,"D_UdeOlie_jordtype_n","Input"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,null,{"$f":"UdeOlie_jord_df","v":0},{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",G9,\"\")","v":0},null,{"$f":"D_UdeOlie_lagtil_1","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",J9,\"\")","v":0},null,{"$f":"D_UdeOlie_lagtil_2","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",N9,\"\")","v":0},null,{"$f":"D_UdeOlie_lagtil_3","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",R9,\"\")","v":0},null,null,"D_UdeOlie_lagfra_n","Input"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"UdeOlie_jord_dt1","v":0},{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",G10,\"\")","v":0},null,null,{"$f":"UdeOlie_jord_dt2","v":0},{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",K10,\"\")","v":0},null,null,{"$f":"UdeOlie_jord_dt3","v":0},{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",O10,\"\")","v":0},null,null,{"$f":"UdeOlie_jord_dt4","v":0},{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",S10,\"\")","v":0},null,null,"D_UdeOlie_lagtil_n","Input"]
[null,"Tykkelse af jordlag","X","m",null,{"$f":"B_UdeOlie_X_1","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",F11,\"\")","v":0},null,{"$f":"B_UdeOlie_X_2","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",J11,\"\")","v":0},null,{"$f":"B_UdeOlie_X_3","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",N11,\"\")","v":0},null,{"$f":"B_UdeOlie_X_4","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",R11,\"\")","v":0},null,null,"D_UdeOlie_X_n","Beregnes"]
[null,"Check af negativ højde",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_udeolie_negativ_x","v":" "},null,"D_UdeOlie_negativ_X_n","Beregnes"]
[null,"Poreluftvolumen","VL",null,null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VL1),UdeOlie_My_VL1,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",IF(ISNUMBER(G13),G13,F13),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VL1),UdeOlie_My_VL1,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",IF(ISNUMBER(K13),K13,J13),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VL3),UdeOlie_My_VL3,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",IF(ISNUMBER(O13),O13,N13),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VL4),UdeOlie_My_VL4,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",IF(ISNUMBER(S13),S13,R13),\"\")","v":0},null,null,"D_UdeOlie_VL_n","Input"]
[null,"Vand-indhold","VV",null,null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VV1),UdeOlie_My_VV1,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",IF(ISNUMBER(G14),G14,F14),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VV2),UdeOlie_My_VV2,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",IF(ISNUMBER(K14),K14,J14),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VV3),UdeOlie_My_VV3,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",IF(ISNUMBER(O14),O14,N14),\"\")","v":0},null,null,{"$f":"IF(ISNUMBER(UdeOlie_My_VV4),UdeOlie_My_VV4,\"-\")","v":"-"},{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",IF(ISNUMBER(S14),S14,R14),\"\")","v":0},null,null,"D_UdeOlie_VV_n","Input"]
[null,"Samlet\nporøsitet","e=VL+VV",null,null,null,null,{"$f":"B_UdeOlie_porositet_1","v":0},null,null,null,{"$f":"B_UdeOlie_porositet_2","v":0},null,null,null,{"$f":"B_UdeOlie_porositet_3","v":0},null,null,null,{"$f":"B_UdeOlie_porositet_4","v":0},null,null,"D_UdeOlie_porositet_n","Beregnes"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,{"$f":"B_UdeOlie_VJ_1","v":0},null,null,null,{"$f":"B_UdeOlie_VJ_2","v":0},null,null,null,{"$f":"B_UdeOlie_VJ_3","v":0},null,null,null,{"$f":"B_UdeOlie_VJ_4","v":0},null,null,"D_UdeOlie_VJ_n","Beregnes"]
[null,"Materialekonstant (app 5.3 - lign 18)-korrigeret","t",null,null,null,null,{"$f":"B_UdeOlie_N_1","v":0},null,{"$f":"B_UdeOlie_N_2","v":0},null,{"$f":"B_UdeOlie_N_2","v":0},null,{"$f":"B_UdeOlie_N_3","v":0},null,{"$f":"B_UdeOlie_N_3","v":0},null,{"$f":"B_UdeOlie_N_4","v":0},null,{"$f":"B_UdeOlie_N_4","v":0},null,null,"D_UdeOlie_N_n","Beregnes"]
[null,"Korigeret materialekonstant (app. 5.3 - Lign 63)",null,null,null,null,null,{"$f":"B_UdeOlie_N_koor_1","v":1},null,{"$f":"B_UdeOlie_N_koor_2","v":1},null,{"$f":"B_UdeOlie_N_koor_2","v":1},null,{"$f":"B_UdeOlie_N_koor_3","v":1},null,{"$f":"B_UdeOlie_N_koor_3","v":1},null,{"$f":"B_UdeOlie_N_koor_4","v":1},null,{"$f":"B_UdeOlie_N_koor_4","v":1},null,null,"D_UdeOlie_N_koor_n","Beregnes"]
[null,"Mellemregning (app. 5.3 - Lign 63)",null,null,null,{"$f":"B_UdeOlie_Bereg_1","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",F19,\"\")","v":0},null,{"$f":"B_UdeOlie_Bereg_2","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",J19,\"\")","v":0},null,{"$f":"B_UdeOlie_Bereg_3","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",N19,\"\")","v":0},null,{"$f":"B_UdeOlie_Bereg_4","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",R19,\"\")","v":0},null,null,"D_UdeOlie_Bereg_n","Beregnes"]
[null,"Check af manglende jordtype",null,null,null,null,null,{"$f":"IF(AND(D_UdeOlie_lagtil_1>0,D_UdeOlie_jordtype_1=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_UdeOlie_lagtil_2>0,D_UdeOlie_jordtype_2=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_UdeOlie_lagtil_3>0,D_UdeOlie_jordtype_3=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,null,{"$f":"IF(AND(D_UdeOlie_lagtil_4>0,D_UdeOlie_jordtype_4=0),\"Fejl! Jordtype mangler\",\"\")","v":""},null,null,"D_udeolie_mangeljt_x","Beregnes i Dataarket"]
[null,"Samlet ækivalente materialekonstant/tykkelse  (app 5.3 - lign. 51)","t*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_UdeOlie_N_tot","v":{"$error":"#DIV/0!"}},null,"D_UdeOlie_N_tot","Beregnes"]
[null,"Tykkelse af jordlag","X","m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"B_UdeOlie_X_tot","v":0},null,"D_UdeOlie_X_tot","Beregnes"]
[]
[null,"Stamdata"]
[]
[null,"Målepunkt",{"$f":"D_olie_målepunkt","v":""}]
[null,"Dato",{"$f":"D_olie_dato","v":""}]
[]
[null,"Det forurenede område"]
[]
[null,null,null,null,"Systemværdi","Indtastet","Beregnes","Anvendes"]
[null,"Længde af det forurenede område","l","m",100,{"$f":"UdeOlie_l","v":0},{"$f":"IF(F32>0,F32,E32)","v":100},{"$f":"IF(VALUE(F32),F32,E32)","v":100},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Udeolie_l","Input"]
[null,"Opblandingshøjde ","h","m",8,{"$f":"UdeOlie_h","v":0},{"$f":"IF(F33>0,F33,H32*E34)","v":8},{"$f":"IF(VALUE(F33),F33,G33)","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Udeolie_h","Input"]
[null,"Opblandingshøjde/længde","h/l"," -",{"$f":"E33/E32","v":0.08},{"$f":"IF(OR(F32=0,F33=0),\"\",F33/F32)","v":""},{"$f":"G33/G32","v":0.08},{"$f":"IF(F34=\"\",E34,F34)","v":0.08},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D_Udeolie_hl","Input"]
[]
[null,"Anvendt brugerdata",null,null,null,null,{"$f":"SUM(G13,G14,K13,K14,O13,O14,S13,S14,F32)","v":0}]
[null,"Anvendt brugerdata i oliefugacitetsmodul",null,null,null,{"$f":"Olie_bruger","v":"Nej"},{"$f":"IF(F37=\"Nej\",0,10)","v":0}]
[null,"Samlet brugerdata",null,null,null,null,{"$f":"SUM(G36:G37)","v":0},{"$f":"IF(G38>0,\"Ja\",\"Nej\")","v":"Nej"}]
[]
[]
[null,"Oliestoffer"]
[]
[null,null,null,null,null,"Beregnet CL fra fugacitets\nmodul","Diffusionkoef. Luft","Vind\nhastighed \n(stofspecifik)","Flux ","Udeluft\nkonc. ","Afdampnings\nkriteriet","Overskridelse af AKK",null,"Udeluft\nkonc. ",null,"Overskridelse af akK"]
["x",null,null,null,null,"mg/m3","m2/s","m/s","(mg/m2/s","(mg/m3)","(mg/m3)","gange"]
[50,"C5-C6"]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},null,{"$f":"B_Udeolie_J_51","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_51","v":{"$error":"#DIV/0!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},null,{"$f":"B_Udeolie_J_511","v":{"$error":"#DIV/0!"}},{"$f":"B_Udeolie_CL_511","v":{"$error":"#DIV/0!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},null,{"$f":"B_Udeolie_J_512","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_512","v":{"$error":"#DIV/0!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},null,{"$f":"B_Udeolie_J_513","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_513","v":{"$error":"#DIV/0!"}}]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"B_UdeOlie_CL_510","v":{"$error":"#DIV/0!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_52","v":9.3000000000000007E-6},1,{"$f":"B_Udeolie_J_52","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_52","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},{"$f":"IF(J51/K51>1,J51/K51,\"Nej\")","v":{"$error":"#DIV/0!"}},null,"D_udeolie_cf_x",null,"D_udeolie_oversk_CK_x"]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},1,{"$f":"B_Udeolie_J_53","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_53","v":{"$error":"#DIV/0!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},1,{"$f":"B_Udeolie_J_54","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_54","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_54_ak","v":0.4},{"$f":"IF(J53/K53>1,J53/K53,\"Nej\")","v":{"$error":"#DIV/0!"}}]
[55,">8 - 10, alifater",">8 - 10, alifater",null,null,{"$f":"D_Olie_55B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55B","v":6.2232552378840063E-6},1,{"$f":"B_Udeolie_J_55","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_55","v":{"$error":"#DIV/0!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},1,{"$f":"B_Udeolie_J_57","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_57","v":{"$error":"#DIV/0!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},1,{"$f":"B_Udeolie_J_58","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_58","v":{"$error":"#DIV/0!"}}]
["57a",null,"Sum af xylener +ethylbenzen",null,null,{"$f":"SUM(F58:F59)","v":{"$error":"#DIV/0!"}},null,1,{"$f":"SUM(I58:I59)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(J58:J59)","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_57_ak","v":0.1},{"$f":"IF(J60/K60>1,J60/K60,\"Nej\")","v":{"$error":"#DIV/0!"}}]
[59,null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},0.1,{"$f":"B_Udeolie_J_59","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_59","v":{"$error":"#DIV/0!"}}]
[60,null,">8 -10, aromater,øvrige",null,null,{"$f":"D_Olie_60_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_60B","v":6.4381431991356133E-6},0.1,{"$f":"B_Udeolie_J_60","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_60","v":{"$error":"#DIV/0!"}}]
[910,"Sum C9-C10 aromater",null,null,null,{"$f":"F62+F61","v":{"$error":"#DIV/0!"}},null,null,{"$f":"B_Udeolie_J_910","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_910","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_60_ak","v":0.03},{"$f":"IF(J63/K63>1,J63/K63,\"Nej\")","v":{"$error":"#DIV/0!"}}]
[]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"B_UdeOlie_CL_1015","v":{"$error":"#DIV/0!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},0.1,{"$f":"B_Udeolie_J_101","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_101","v":{"$error":"#DIV/0!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},0.1,{"$f":"B_Udeolie_J_103","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_103","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_103_ak","v":0.04},{"$f":"IF(J68/K68>1,J68/K68,\"Nej\")","v":{"$error":"#DIV/0!"}}]
[104,null,">10 - 12, aromater, øvrige",null,null,{"$f":"D_Olie_104B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104B","v":5.5260438461528997E-6},0.1,{"$f":"B_Udeolie_J_104","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_104","v":{"$error":"#DIV/0!"}}]
[105,">12 - 16, alifater",">12 - 16, alifater",null,null,{"$f":"D_Olie_105B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105B","v":5.0933919872504982E-6},0.1,{"$f":"B_Udeolie_J_105","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_105","v":{"$error":"#DIV/0!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},0.1,{"$f":"B_Udeolie_J_107","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_107","v":{"$error":"#DIV/0!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},0.1,{"$f":"B_Udeolie_J_108","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_108","v":{"$error":"#DIV/0!"}}]
[109,null,">12 - 16, aromater,øvrige",null,null,{"$f":"D_Olie_109B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109B","v":5.9000000000000003E-6},0.1,{"$f":"B_Udeolie_J_109","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_109","v":{"$error":"#DIV/0!"}}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"B_UdeOlie_CL_1520","v":{"$error":"#DIV/0!"}}]
[151,">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"D_Olie_151B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151B","v":4.4721099862171762E-6},0.1,{"$f":"B_Udeolie_J_151","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_151","v":{"$error":"#DIV/0!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},0.1,{"$f":"B_Udeolie_J_153","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_153","v":{"$error":"#DIV/0!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},0.1,{"$f":"B_Udeolie_J_154","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_154","v":{"$error":"#DIV/0!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},0.1,{"$f":"B_Udeolie_J_155","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_155","v":{"$error":"#DIV/0!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},0.1,{"$f":"B_Udeolie_J_156","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_156","v":{"$error":"#DIV/0!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},0.1,{"$f":"B_Udeolie_J_157","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_157","v":{"$error":"#DIV/0!"}}]
[]
[2025,"C21-C25"]
[201,">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"D_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201B","v":3.9528308464137552E-6},0.1,{"$f":"B_Udeolie_J_201","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_201","v":{"$error":"#DIV/0!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter"]
[]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"B_UdeOlie_CL_2535","v":{"$error":"#DIV/0!"}}]
[251,">25 - 35, alifater",">25 - 35, alifater",null,null,{"$f":"D_Olie_251B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251B","v":3.6715492605442101E-6},0.1,{"$f":"B_Udeolie_J_251","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_251","v":{"$error":"#DIV/0!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater"]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},0.1,{"$f":"B_Udeolie_J_253","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_253","v":{"$error":"#DIV/0!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},0.1,{"$f":"B_Udeolie_J_254","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_254","v":{"$error":"#DIV/0!"}}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},0.1,{"$f":"B_Udeolie_J_255","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_255","v":{"$error":"#DIV/0!"}}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},0.1,{"$f":"B_Udeolie_J_256","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_256","v":{"$error":"#DIV/0!"}}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},0.1,{"$f":"B_Udeolie_J_257","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_257","v":{"$error":"#DIV/0!"}}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},0.1,{"$f":"B_Udeolie_J_258","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_258","v":{"$error":"#DIV/0!"}}]
[259,null,">25 - 35, aromater, øvrige",null,null,{"$f":"D_Olie_259B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259B","v":4.4493993711079091E-6},0.1,{"$f":"B_Udeolie_J_259","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_259","v":{"$error":"#DIV/0!"}}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"B_UdeOlie_CL_3540","v":{"$error":"#DIV/0!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},0.1,{"$f":"B_Udeolie_J_351","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_351","v":{"$error":"#DIV/0!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},0.1,{"$f":"B_Udeolie_J_352","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_352","v":{"$error":"#DIV/0!"}}]
[]
[2040,"C21-C40",null,null,null,{"$f":"IF(D_Olie_2040_cl>0,D_Olie_2040_cl,0)","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"IF(B_UdeOlie_CL_2040>0,B_UdeOlie_CL_2040,0)","v":{"$error":"#DIV/0!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand"]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},0.1,{"$f":"B_Udeolie_J_10","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_10","v":{"$error":"#DIV/0!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},0.1,{"$f":"B_Udeolie_J_11","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_11","v":{"$error":"#DIV/0!"}}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},0.1,{"$f":"B_Udeolie_J_12","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_12","v":{"$error":"#DIV/0!"}}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},0.1,{"$f":"B_Udeolie_J_13","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_13","v":{"$error":"#DIV/0!"}}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},0.1,{"$f":"B_Udeolie_J_14","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_14","v":{"$error":"#DIV/0!"}}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},0.1,{"$f":"B_Udeolie_J_15","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_15","v":{"$error":"#DIV/0!"}}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},0.1,{"$f":"B_Udeolie_J_16","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_16","v":{"$error":"#DIV/0!"}}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"B_UdeOlie_CL_1","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_1_ak","v":0.1},{"$f":"IF(J118/K118>1,J118/K118,\"Nej\")","v":{"$error":"#DIV/0!"}}]
[]
[null,"Bemærkninger"]
[null,"Jordparametre:","D_UdeOlie_Jord_Com"]
[null,null,false]
[null,"Forurenet område:","D_UdeOlie_ForOm_Com"]
[null,null,false]
[null,"Beregning","D_UdeOlie_Ber_Com"]

{"sheet":"Beregning_Udeluft-olie","index":51,"n_rows":98,"n_cols":24,"rows_kept":98,"cut":false,"hidden":true,"merged":[[20,1,20,16],[6,22,6,24],[1,1,1,16],[3,1,3,16],[5,4,5,7],[5,8,5,11],[5,12,5,15],[5,16,5,19]]}
[]
[null,"Beregningsark - UdeOlieluft",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,"Jord"]
[]
[null,null,null,null,"Jordlag 1",null,null,null,"Jordlag 2",null,null,null,"Jordlag 3",null,null,null,"Jordlag 4"]
[null,"Navn","Forkortelse","Enhed","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","Interval","Systemværdi","Indtastet","Anvendes","SAMLET",null,"Værditype"]
[null,"Jordtype",null,null,null,null,null,{"$f":"D_UdeOlie_jordtype_1","v":0},null,null,null,{"$f":"D_UdeOlie_jordtype_2","v":0},null,null,null,{"$f":"D_UdeOlie_jordtype_3","v":0},null,null,null,{"$f":"D_UdeOlie_jordtype_4","v":0},null,null,null,"Input"]
[null,"Jordlag, Dybde fra","x1","m u.t.",null,null,{"$f":"UdeOlie_jord_df","v":0},{"$f":"D_UdeOlie_lagfra_1","v":0},null,{"$f":"D_UdeOlie_lagtil_1","v":0},null,{"$f":"D_UdeOlie_lagfra_2","v":0},null,{"$f":"D_UdeOlie_lagtil_2","v":0},null,{"$f":"D_UdeOlie_lagfra_3","v":0},null,{"$f":"D_UdeOlie_lagtil_3","v":0},null,{"$f":"D_UdeOlie_lagfra_4","v":0},null,null,null,"Input"]
[null,"Jordlag, Dybde til","x2","m u.t.",null,null,{"$f":"UdeOlie_jord_dt1","v":0},{"$f":"D_UdeOlie_lagtil_1","v":0},null,null,{"$f":"UdeOlie_jord_dt2","v":0},{"$f":"D_UdeOlie_lagtil_2","v":0},null,null,{"$f":"UdeOlie_jord_dt3","v":0},{"$f":"D_UdeOlie_lagtil_3","v":0},null,null,{"$f":"UdeOlie_jord_dt4","v":0},{"$f":"D_UdeOlie_lagtil_4","v":0},null,null,null,"Input"]
[null,"Tykkelse af jordlag","X","m",null,{"$f":"IF(D_UdeOlie_lagtil_1>0,D_UdeOlie_lagtil_1-D_UdeOlie_lagfra_1,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",F11,\"\")","v":0},null,{"$f":"IF(D_UdeOlie_lagtil_2>0,D_UdeOlie_lagtil_2-D_UdeOlie_lagfra_2,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",J11,\"\")","v":0},null,{"$f":"IF(D_UdeOlie_lagtil_3>0,D_UdeOlie_lagtil_3-D_UdeOlie_lagfra_3,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",N11,\"\")","v":0},null,{"$f":"IF(D_UdeOlie_lagtil_4>0,D_UdeOlie_lagtil_4-D_UdeOlie_lagfra_4,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",R11,\"\")","v":0},null,null,"B_udeOlie_X_n","Beregnes"]
[null,"Check af negativ højde",null,null,null,{"$f":"IF(B_UdeOlie_X_1<0,1,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",F12,\"\")","v":0},null,{"$f":"IF(B_UdeOlie_X_2<0,1,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",J12,\"\")","v":0},null,{"$f":"IF(B_UdeOlie_X_3<0,1,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",N12,\"\")","v":0},null,{"$f":"IF(B_UdeOlie_X_4<0,1,0)","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",R12,\"\")","v":0},{"$f":"IF(F12+J12+N12+R12>0,\"FEJL!! Der er jordlag med negativ højde\",\" \")","v":" "},null,"B_udeOlie_negativ_X_n","Beregnes"]
[null,"Samlet\nporøsitet","e=VL+VV",null,null,{"$f":"D_UdeOlie_VL_1+D_UdeOlie_VV_1","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_1<>\"\",F13,\"\")","v":0},null,{"$f":"D_UdeOlie_VL_2+D_UdeOlie_VV_2","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_2<>\"\",J13,\"\")","v":0},null,{"$f":"D_UdeOlie_VL_3+D_UdeOlie_VV_3","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_3<>\"\",N13,\"\")","v":0},null,{"$f":"D_UdeOlie_VL_4+D_UdeOlie_VV_4","v":0},null,{"$f":"IF(D_UdeOlie_jordtype_4<>\"\",R13,\"\")","v":0},null,null,"B_udeOlie_porositet_n","Beregnes"]
[null,"Volumen af jordskellet","VJ",null,null,null,null,{"$f":"IF(B_UdeOlie_porositet_1>0,1-B_UdeOlie_porositet_1,0)","v":0},null,null,null,{"$f":"IF(B_UdeOlie_porositet_2>0,1-B_UdeOlie_porositet_2,0)","v":0},null,null,null,{"$f":"IF(B_UdeOlie_porositet_3>0,1-B_UdeOlie_porositet_3,0)","v":0},null,null,null,{"$f":"IF(B_UdeOlie_porositet_4>0,1-B_UdeOlie_porositet_4,0)","v":0},null,null,"B_udeOlie_VJ_n","Beregnes"]
[null,"Materialekonstant (app 5.3 - nyt lign. 64 ersatter lign 18)","t",null,null,null,null,{"$f":"IF(D_UdeOlie_VL_1=0,0,POWER(D_UdeOlie_VL_1,2.5)/B_UdeOlie_porositet_1)","v":0},null,null,null,{"$f":"IF(D_UdeOlie_VL_2=0,0,POWER(D_UdeOlie_VL_2,2.5)/B_UdeOlie_porositet_2)","v":0},null,null,null,{"$f":"IF(D_UdeOlie_VL_3=0,0,POWER(D_UdeOlie_VL_3,2.5)/B_UdeOlie_porositet_3)","v":0},null,null,null,{"$f":"IF(D_UdeOlie_VL_4=0,0,POWER(D_UdeOlie_VL_4,2.5)/B_UdeOlie_porositet_4)","v":0},null,null,"B_udeOlie_N_n","Beregnes"]
[null,"Korigeret materialekonstant",null,null,null,null,null,{"$f":"IF(B_UdeOlie_N_1=0,1,B_UdeOlie_N_1)","v":1},null,null,null,{"$f":"IF(B_UdeOlie_N_2=0,1,B_UdeOlie_N_2)","v":1},null,null,null,{"$f":"IF(B_UdeOlie_N_3=0,1,B_UdeOlie_N_3)","v":1},null,null,null,{"$f":"IF(B_UdeOlie_N_4=0,1,B_UdeOlie_N_4)","v":1},null,null,"B_udeOlie_N_koor_n","Beregnes"]
[null,"Mellemregning (app. 5.3 - Lign 63)",null,null,null,null,null,{"$f":"B_UdeOlie_X_1*(B_UdeOlie_N_koor_2*B_UdeOlie_N_koor_3*B_UdeOlie_N_koor_4)","v":0},null,null,null,{"$f":"B_UdeOlie_X_2*(B_UdeOlie_N_koor_1*B_UdeOlie_N_koor_3*B_UdeOlie_N_koor_4)","v":0},null,null,null,{"$f":"B_UdeOlie_X_3*(B_UdeOlie_N_koor_1*B_UdeOlie_N_koor_2*B_UdeOlie_N_koor_4)","v":0},null,null,null,{"$f":"B_UdeOlie_X_4*(B_UdeOlie_N_koor_1*B_UdeOlie_N_koor_2*B_UdeOlie_N_koor_3)","v":0},null,null,"B_udeOlie_Bereg_n","Beregnes"]
[null,"Samlet ækivalente materialekonstant/tykkelse  (app 5.3 - lign. 51)","t*",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(B_UdeOlie_N_koor_1*B_UdeOlie_N_koor_2*B_UdeOlie_N_koor_3*B_UdeOlie_N_koor_4)/(B_UdeOlie_Bereg_1+B_UdeOlie_Bereg_2+B_UdeOlie_Bereg_3+B_UdeOlie_Bereg_4)","v":{"$error":"#DIV/0!"}},null,"B_udeOlie_N_tot","Beregnes"]
[null,"Tykkelse af jordlag","X","m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(B_UdeOlie_X_1+B_UdeOlie_X_2+B_UdeOlie_X_3+B_UdeOlie_X_4)","v":0},null,"B_udeOlie_X_tot","Beregnes"]
[]
[null,"Oliestoffer"]
[]
[null,null,null,null,null,"Beregnet CL fra fugacitets\nmodul","Diffusionkoef. Luft","Vind\nhastighed \n(stofspecifik)","Flux ","Udeluft\nkonc. "]
["x",null,null,null,null,"mg/m3","m2/s","m/s","(mg/m2/s","(mg/m3)",null,"Flux",null,"Udeluftkonc."]
[50,"C5-C6"]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},0.1,{"$f":"D_UdeOlie_N_tot*G26*F26","v":{"$error":"#DIV/0!"}},{"$f":"I26/(H26*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}},null,"B_Udeolie_J_x",null,"B_udeolie_Cl_x"]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},0.1,{"$f":"D_UdeOlie_N_tot*G27*F27","v":{"$error":"#DIV/0!"}},{"$f":"I27/(H27*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},0.1,{"$f":"D_UdeOlie_N_tot*G28*F28","v":{"$error":"#DIV/0!"}},{"$f":"I28/(H28*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},0.1,{"$f":"D_UdeOlie_N_tot*G29*F29","v":{"$error":"#DIV/0!"}},{"$f":"I29/(H29*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J32:J42)","v":{"$error":"#DIV/0!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_52","v":9.3000000000000007E-6},1,{"$f":"D_UdeOlie_N_tot*G32*F32","v":{"$error":"#DIV/0!"}},{"$f":"I32/(H32*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},1,{"$f":"D_UdeOlie_N_tot*G33*F33","v":{"$error":"#DIV/0!"}},{"$f":"I33/(H33*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},1,{"$f":"D_UdeOlie_N_tot*G34*F34","v":{"$error":"#DIV/0!"}},{"$f":"I34/(H34*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[55,">8 - 10, alifater",">8 - 10, alifater",null,null,{"$f":"D_Olie_55B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_55B","v":6.2232552378840063E-6},1,{"$f":"D_UdeOlie_N_tot*G35*F35","v":{"$error":"#DIV/0!"}},{"$f":"I35/(H35*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},1,{"$f":"D_UdeOlie_N_tot*G39*F39","v":{"$error":"#DIV/0!"}},{"$f":"I39/(H39*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},1,{"$f":"D_UdeOlie_N_tot*G40*F40","v":{"$error":"#DIV/0!"}},{"$f":"I40/(H40*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[59,null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},0.1,{"$f":"D_UdeOlie_N_tot*G41*F41","v":{"$error":"#DIV/0!"}},{"$f":"I41/(H41*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[60,null,">8 -10, aromater,øvrige",null,null,{"$f":"D_Olie_60_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_60B","v":6.4381431991356133E-6},0.1,{"$f":"D_UdeOlie_N_tot*G42*F42","v":{"$error":"#DIV/0!"}},{"$f":"I42/(H42*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[910,"C9-C10 aromater",null,null,null,null,null,null,{"$f":"B_Udeolie_J_60+B_Udeolie_J_59","v":{"$error":"#DIV/0!"}},{"$f":"B_UdeOlie_CL_60+B_UdeOlie_CL_59","v":{"$error":"#DIV/0!"}}]
[]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J46:J54)","v":{"$error":"#DIV/0!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},0.1,{"$f":"D_UdeOlie_N_tot*G46*F46","v":{"$error":"#DIV/0!"}},{"$f":"I46/(H46*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},0.1,{"$f":"D_UdeOlie_N_tot*G48*F48","v":{"$error":"#DIV/0!"}},{"$f":"I48/(H48*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[104,null,">10 - 12, aromater, øvrige",null,null,{"$f":"D_Olie_104B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_104B","v":5.5260438461528997E-6},0.1,{"$f":"D_UdeOlie_N_tot*G49*F49","v":{"$error":"#DIV/0!"}},{"$f":"I49/(H49*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[105,">12 - 16, alifater",">12 - 16, alifater",null,null,{"$f":"D_Olie_105B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_105B","v":5.0933919872504982E-6},0.1,{"$f":"D_UdeOlie_N_tot*G50*F50","v":{"$error":"#DIV/0!"}},{"$f":"I50/(H50*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater"]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},0.1,{"$f":"D_UdeOlie_N_tot*G52*F52","v":{"$error":"#DIV/0!"}},{"$f":"I52/(H52*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},0.1,{"$f":"D_UdeOlie_N_tot*G53*F53","v":{"$error":"#DIV/0!"}},{"$f":"I53/(H53*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[109,null,">12 - 16, aromater,øvrige",null,null,{"$f":"D_Olie_109B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_109B","v":5.9000000000000003E-6},0.1,{"$f":"D_UdeOlie_N_tot*G54*F54","v":{"$error":"#DIV/0!"}},{"$f":"I54/(H54*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J57:J63)","v":{"$error":"#DIV/0!"}}]
[151,">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"D_Olie_151B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_151B","v":4.4721099862171762E-6},0.1,{"$f":"D_UdeOlie_N_tot*G57*F57","v":{"$error":"#DIV/0!"}},{"$f":"I57/(H57*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater"]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},0.1,{"$f":"D_UdeOlie_N_tot*G59*F59","v":{"$error":"#DIV/0!"}},{"$f":"I59/(H59*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},0.1,{"$f":"D_UdeOlie_N_tot*G60*F60","v":{"$error":"#DIV/0!"}},{"$f":"I60/(H60*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},0.1,{"$f":"D_UdeOlie_N_tot*G61*F61","v":{"$error":"#DIV/0!"}},{"$f":"I61/(H61*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},0.1,{"$f":"D_UdeOlie_N_tot*G62*F62","v":{"$error":"#DIV/0!"}},{"$f":"I62/(H62*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},0.1,{"$f":"D_UdeOlie_N_tot*G63*F63","v":{"$error":"#DIV/0!"}},{"$f":"I63/(H63*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[]
[2025,"C21-C25"]
[201,">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"D_Olie_201B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_201B","v":3.9528308464137552E-6},0.1,{"$f":"D_UdeOlie_N_tot*G66*F66","v":{"$error":"#DIV/0!"}},{"$f":"I66/(H66*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter"]
[]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J70:J78)","v":{"$error":"#DIV/0!"}}]
[251,">25 - 35, alifater",">25 - 35, alifater",null,null,{"$f":"D_Olie_251B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_251B","v":3.6715492605442101E-6},0.1,{"$f":"D_UdeOlie_N_tot*G70*F70","v":{"$error":"#DIV/0!"}},{"$f":"I70/(H70*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,0.1]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},0.1,{"$f":"D_UdeOlie_N_tot*G72*F72","v":{"$error":"#DIV/0!"}},{"$f":"I72/(H72*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[259,null,">25 - 35, aromater, øvrige",null,null,{"$f":"D_Olie_259B_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_259B","v":4.4493993711079091E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J81:J82)","v":{"$error":"#DIV/0!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},0.1,{"$f":"D_UdeOlie_N_tot*G81*F81","v":{"$error":"#DIV/0!"}},{"$f":"I81/(H81*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},0.1,{"$f":"D_UdeOlie_N_tot*G82*F82","v":{"$error":"#DIV/0!"}},{"$f":"I82/(H82*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J69+J66)","v":{"$error":"#DIV/0!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand"]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},0.1,{"$f":"D_UdeOlie_N_tot*G90*F90","v":{"$error":"#DIV/0!"}},{"$f":"I90/(H90*D_UdeOlie_hl)","v":{"$error":"#DIV/0!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cl","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},0.1,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cl","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"SUM(J90:J96)+J84+J45+J56+J31","v":{"$error":"#DIV/0!"}}]

{"sheet":"Udskrift_Udeluft-Olie","index":52,"n_rows":71,"n_cols":11,"rows_kept":71,"cut":false,"hidden":true,"merged":[[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,10],[2,8,2,11],[3,8,3,11],[11,8,11,9],[22,0,22,1],[18,2,18,3],[19,2,19,3],[20,2,20,3],[8,2,8,3],[8,4,8,5],[8,6,8,7],[14,6,14,8],[17,2,17,3],[30,12,30,14],[30,4,30,5],[30,2,30,3],[31,12,31,14],[34,12,34,14],[28,6,28,7],[29,4,29,5],[29,2,29,3],[33,6,33,7],[34,6,34,7],[30,8,30,9],[33,8,33,9],[34,8,34,9],[31,2,31,3],[30,6,30,7],[31,4,31,5],[32,4,32,5],[23,4,23,5],[23,6,23,7],[24,6,24,7],[24,8,24,10],[32,8,32,9],[37,6,37,7],[37,2,37,3],[33,4,33,5],[34,4,34,5],[37,4,37,5],[34,2,34,3],[33,2,33,3],[36,12,36,14],[32,12,32,14],[33,12,33,14],[32,2,32,3],[17,4,17,5],[17,6,17,7],[17,8,17,9],[8,8,8,9],[9,2,9,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[10,2,10,3],[10,4,10,5],[10,6,10,7],[10,8,10,9],[11,2,11,3],[11,4,11,5],[11,6,11,7],[23,2,23,3],[38,2,38,3],[40,8,40,9],[39,8,39,9],[44,6,44,7],[47,1,47,4],[48,1,48,4],[24,2,24,3],[24,4,24,5],[38,8,38,9],[38,6,38,7],[38,4,38,5],[29,6,29,7],[27,8,27,9],[28,8,28,9],[29,8,29,9],[28,2,28,3],[27,4,27,5],[27,6,27,7],[27,2,27,3],[28,4,28,5],[37,8,37,9],[31,6,31,7],[32,6,32,7],[31,8,31,9],[84,1,97,9],[44,2,44,3],[40,2,40,3],[39,2,39,3],[41,2,41,3],[39,4,39,5],[40,4,40,5],[41,4,41,5],[41,6,41,7],[44,4,44,5],[41,8,41,9],[44,8,44,9],[39,6,39,7],[40,6,40,7],[54,1,67,11],[69,1,82,11]]}
["Udeluft-Olie"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
["Jordparametre"]
["Kommentar",{"$f":"IF( D_UdeOlie_Jord_ComUds,\"ja\",\"nej\")","v":"nej"},"Indtastede data (angives med fed)"]
[null,null,"Jordlag 1",null,"Jordlag 2",null,"Jordlag 3",null,"Jordlag 4"]
["Jordlag, Dybde fra","m u.t.",{"$f":"IF(UdeOlie_jord_df<>\"\",UdeOlie_jord_df,\"\")","v":""},null,{"$f":"IF(UdeOlie_jord_dt2<>\"\",D_UdeOlie_lagfra_2,\"\")","v":""},null,{"$f":"IF(UdeOlie_jord_dt3<>\"\",D_UdeOlie_lagfra_3,\"\")","v":""},null,{"$f":"IF(UdeOlie_jord_dt4<>\"\",D_UdeOlie_lagfra_4,\"\")","v":""}]
["Jordlag, Dybde til","m u.t.",{"$f":"IF(UdeOlie_jord_dt1<>\"\",UdeOlie_jord_dt1,\"\")","v":""},null,{"$f":"IF(UdeOlie_jord_dt2<>\"\",UdeOlie_jord_dt2,\"\")","v":""},null,{"$f":"IF(UdeOlie_jord_dt3<>\"\",UdeOlie_jord_dt3,\"\")","v":""},null,{"$f":"IF(UdeOlie_jord_dt4<>\"\",UdeOlie_jord_dt4,\"\")","v":""}]
["Jordtype",null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst1=\"\",UdeOlie_My_jord1=\"\"),\"\",D_UdeOlie_jordtype_1)","v":""},null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst2=\"\",UdeOlie_My_jord2=\"\"),\"\",D_UdeOlie_jordtype_2)","v":""},null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst3=\"\",UdeOlie_My_jord3=\"\"),\"\",D_UdeOlie_jordtype_3)","v":""},null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst4=\"\",UdeOlie_My_jord4=\"\"),\"\",D_UdeOlie_jordtype_4)","v":""}]
["Materialekonstant",null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst1=\"\",UdeOlie_My_jord1=\"\"),\"\",D_UdeOlie_N_1)","v":""},null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst2=\"\",UdeOlie_My_jord2=\"\"),\"\",D_UdeOlie_N_2)","v":""},null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst3=\"\",UdeOlie_My_jord3=\"\"),\"\",D_UdeOlie_N_3)","v":""},null,{"$f":"IF(AND(D_UdeOlie_jordtype_syst4=\"\",UdeOlie_My_jord4=\"\"),\"\",D_UdeOlie_N_4)","v":""}]
[]
["Samlet ækivalent jordlagtykkelse  (app 5.3/lign. 51)",null,null,null,{"$f":"D_UdeOlie_N_tot","v":{"$error":"#DIV/0!"}},"m","Tykkelse af jordlag",null,null,{"$f":"D_UdeOlie_X_tot","v":0},"m"]
[]
["Det forurenede område "]
["Kommentar",{"$f":"IF(D_UdeOlie_ForOm_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Længde af det forurenede område","l",{"$f":"IF(D_UdeOlie_l<>\"\",D_UdeOlie_l,\"\")","v":100},null,"m"]
["Opblandingshøjde ","h/l",{"$f":"IF(D_UdeOlie_h<>\"\",D_UdeOlie_h,\"\")","v":8},null,"m"]
["Opblandingshøjde/\nlængde","h/l",{"$f":"IF(D_UdeOlie_hl<>\"\",D_UdeOlie_hl,\"\")","v":0.08}]
[]
["Beregning: Udeluft"]
[null,null,"Målepunkt",null,"Dato",null,"Fri fase?",null,"Anvendt brugerdata"]
["Angiv signifikant ciffer",1,{"$f":"IF(Olie_målepunkt<>\"\",D_olie_målepunkt,\"\")","v":""},null,{"$f":"IF(Olie_dato<>\"\",D_olie_dato,\"\")","v":""},null,{"$f":"Olie_frifase","v":"Nej"},null,{"$f":"D_Udeolie_bruger","v":"Nej"}]
[]
[]
["Oliestofgrupper",null,"Poreluftkonc.",null,"Total bidrag til udeluft",null,"Afdampnings\nkriteriet",null,"Overskridelse"]
["BTEX'er",null,"mg/m3",null,"mg/m3",null,"mg/m3",null,"gange"]
["Benzen",null,{"$f":"IF(D_Udeolie_CF_52>0,ROUND(D_Udeolie_CF_52,Udeolie_ciffer-(INT(LOG(D_Udeolie_CF_52))+1)),D_Udeolie_CF_52)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_Udeolie_CL_52=0,0,(ROUND(D_Udeolie_CL_52,Udeolie_ciffer-(INT(LOG(D_Udeolie_CL_52))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_52_ak","v":1.2999999999999999E-4},null,{"$f":"D_udeolie_overskr_52","v":{"$error":"#DIV/0!"}}]
["Toluen",null,{"$f":"IF(D_Udeolie_CF_54>0,ROUND(D_Udeolie_CF_54,Udeolie_ciffer-(INT(LOG(D_Udeolie_CF_54))+1)),D_Udeolie_CF_54)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_udeolie_CL_54=0,0,(ROUND(D_udeolie_CL_54,Udeolie_ciffer-(INT(LOG(D_udeolie_CL_54))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_54_ak","v":0.4},null,{"$f":"D_udeolie_overskr_54","v":{"$error":"#DIV/0!"}}]
["Ethylbenzen",null,{"$f":"IF(D_udeolie_cf_58>0,ROUND(D_udeolie_cf_58,Udeolie_ciffer-(INT(LOG(D_udeolie_cf_58))+1)),D_Udeolie_CF_52)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_udeolie_CL_58=0,0,(ROUND(D_udeolie_CL_58,Udeolie_ciffer-(INT(LOG(D_udeolie_CL_58))+1))))","v":{"$error":"#DIV/0!"}}]
["Sum Xylener",null,{"$f":"IF(D_Udeolie_Cf_57>0,ROUND(D_Udeolie_Cf_57,Udeolie_ciffer-(INT(LOG(D_Udeolie_Cf_57))+1)),D_Udeolie_Cf_57)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_udeolie_CL_57=0,0,(ROUND(D_udeolie_CL_57,Udeolie_ciffer-(INT(LOG(D_udeolie_CL_57))+1))))","v":{"$error":"#DIV/0!"}}]
["∑Xylener+Ethylbenzen",null,{"$f":"IF(D_udeolie_cf_57a>0,ROUND(D_udeolie_cf_57a,Udeolie_ciffer-(INT(LOG(D_udeolie_cf_57a))+1)),D_udeolie_cf_57a)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_udeolie_CL_57=0,0,(ROUND(D_udeolie_cl_57a,Udeolie_ciffer-(INT(LOG(D_udeolie_cl_57a))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_57_ak","v":0.1},null,{"$f":"D_udeolie_overskr_57a","v":{"$error":"#DIV/0!"}}]
["Naphthalen",null,{"$f":"IF(D_Udeolie_Cf_103>0,ROUND(D_Udeolie_Cf_103,Udeolie_ciffer-(INT(LOG(D_Udeolie_Cf_103))+1)),D_Udeolie_Cf_103)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_udeolie_CL_103=0,0,(ROUND(D_udeolie_CL_103,Udeolie_ciffer-(INT(LOG(D_udeolie_CL_103))+1))))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_103_ak","v":0.04},null,{"$f":"D_udeolie_overskr_103","v":{"$error":"#DIV/0!"}}]
[]
["Kulbrintefraktioner"]
["C6-C10",null,{"$f":"IF(D_Olie_510_cl>0,ROUND(D_Olie_510_cl,Udeolie_ciffer-(INT(LOG(D_Olie_510_cl))+1)),D_Olie_510_cl)","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_udeolie_cf_510,Udeolie_ciffer-(INT(LOG(D_udeolie_cf_510))+1))","v":{"$error":"#DIV/0!"}}]
["C10-C15",null,{"$f":"IF(D_Olie_1015_cl>0,ROUND(D_Olie_1015_cl,Udeolie_ciffer-(INT(LOG(D_Olie_1015_cl))+1)),D_Olie_1015_cl)","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_udeolie_cf_1015,Udeolie_ciffer-(INT(LOG(D_udeolie_cf_1015))+1))","v":{"$error":"#DIV/0!"}}]
["C15-C20",null,{"$f":"IF(D_Olie_1520_cl>0,ROUND(D_Olie_1520_cl,Udeolie_ciffer-(INT(LOG(D_Olie_1520_cl))+1)),D_Olie_1520_cl)","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_Udeolie_cf_1520,Udeolie_ciffer-(INT(LOG(D_Udeolie_cf_1520))+1))","v":{"$error":"#DIV/0!"}}]
["C20-C35",null,{"$f":"IF(D_Olie_2040_cl>0,ROUND(D_Olie_2040_cl,Udeolie_ciffer-(INT(LOG(D_Olie_2040_cl))+1)),D_Olie_2040_cl)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(D_udeolie_cf_2040>0,ROUND(D_udeolie_cf_2040,Udeolie_ciffer-(INT(LOG(D_udeolie_cf_2040))+1)),0)","v":{"$error":"#DIV/0!"}}]
["Sum af kulbrinter",null,{"$f":"IF(D_Olie_1_cl>0,ROUND(D_Olie_1_cl,Udeolie_ciffer-(INT(LOG(D_Olie_1_cl))+1)),D_Olie_1_cl)","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_Udeolie_cf_1,Udeolie_ciffer-(INT(LOG(D_Udeolie_cf_1))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_1_ak","v":0.1},null,{"$f":"D_udeolie_overskr_1","v":{"$error":"#DIV/0!"}}]
[]
["Aromatiske kulbrinter "]
["C9-C10 aromatiske kulbr.",null,{"$f":"IF(D_Olie_910_cl>0,ROUND(D_Olie_910_cl,Udeolie_ciffer-(INT(LOG(D_Olie_910_cl))+1)),D_Olie_910_cl)","v":{"$error":"#DIV/0!"}},null,{"$f":"ROUND(D_udeolie_cf_910,Udeolie_ciffer-(INT(LOG(D_udeolie_cf_910))+1))","v":{"$error":"#DIV/0!"}},null,{"$f":"D_Olie_60_ak","v":0.03},null,{"$f":"D_Udeolie_overskr_910","v":{"$error":"#DIV/0!"}}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"Lok_firma","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler"]
[]
["Bemærkninger",{"$f":"IF(D_UdeOlie_Jord_Com<>\"\",D_UdeOlie_Jord_Com,\"\")","v":""}]
["om jordlag"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_UdeOlie_ForOm_Com<>\"\",D_UdeOlie_ForOm_Com,\"\")","v":""}]
["om forurenet område"]

{"sheet":"Vejledning_Udeluft-Olie","index":53,"n_rows":87,"n_cols":2,"rows_kept":87,"cut":false,"hidden":true,"merged":[[86,1,87,15],[57,1,67,15],[68,1,68,15],[69,1,69,15],[70,1,71,15],[72,1,72,15],[73,1,73,15],[74,1,76,15],[78,1,78,15],[79,1,83,15],[84,1,84,15],[85,1,85,15],[56,1,56,15],[28,1,28,15],[29,1,29,15],[30,1,32,14],[33,1,33,15],[35,1,40,15],[41,1,41,15],[42,1,42,15],[43,1,44,15],[45,1,45,15],[46,1,54,15],[55,1,55,15],[20,1,27,15],[1,1,1,15],[2,1,3,15],[4,1,4,15],[5,1,5,15],[6,1,6,15],[7,1,10,15],[11,1,11,15],[12,1,12,15],[13,1,17,15],[18,1,18,15],[19,1,19,15]]}
[null,"Vejledning - Udeluft for oliestoffer"]
[null,"Formål"]
[null,"I dette regneark kan der foretages en beregning af konsekvenser for udeluft, jf. appendiks 5.3 i MST´s Oprydningsvejledning fra 1998. "]
[]
[]
[null,"BEREGNINGER"]
[null,"Jordtype:"]
[null,"Man kan vælge op til 4 forskellige jordlag enten som standardjordtyper fra listen eller oprette eller hente egenskaber fra egen liste ved at markere den ønskede jordtype. \n\nDet er også muligt at anvende og oprette egne \"jordtyper\" ved at klikke på knappen \"Egen liste\". "]
[]
[]
[]
[]
[null,"Det forurenede område:"]
[null,"Såfremt der kun indtastes oplysninger om længden af det forurenede område, vil opblandingshøjden blive justeret i henhold til en default opblandingsforhold på 0,08, jf. MST´s Oprydningsvejledning. Ved at indtaste en opblandingshøjde, for eksempel 1,6 m (indåndingshøjden), fås et lavere eller højere udeluftbidrag, afhængig af længden af det forurenede område. Opblandingshøjden er højde, hvorved der kan forventes fuld opblanding af forurening i atmosfæren for enden af det forurenede område, nedstrøms vind-retningen. "]
[]
[]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata, dvs. målte eller beregnede poreluftkoncentrationer fra fugacitetsmodulet overføres til udeluftmodulet.\n\nDer er også mulighed for at indtaste en baggrundskoncentration for udeluft, men denne påvirker kun diffusionsfluxen og vil derfor sjældent have betydning for bidraget til udeluften.\n\nHerudover kan der afprøves andre poreluftkoncentrationer, og i så fald ses en bemærkning i både brugerfladen og udskriften om, der er anvendt brugerdata. "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GENERELT"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under Enkeltstof-modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under Enkeltstof-modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks.. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTVÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Vertikal Transport-Olie","index":54,"n_rows":159,"n_cols":33,"rows_kept":159,"cut":false,"hidden":true,"merged":[[77,10,77,11],[77,13,77,14],[54,7,54,11],[54,14,54,26],[73,10,73,11],[73,13,73,14],[75,10,75,11],[75,13,75,14],[109,7,109,8],[109,10,109,11],[109,13,109,14],[109,16,109,17],[109,19,109,21],[109,23,109,25],[101,19,101,21],[103,19,103,21],[107,7,107,8],[107,10,107,11],[107,13,107,14],[107,16,107,17],[107,19,107,21],[107,23,107,25],[105,7,105,8],[105,10,105,11],[158,7,158,8],[158,10,158,11],[158,13,158,14],[158,16,158,17],[158,19,158,21],[158,23,158,25],[156,7,156,8],[156,10,156,11],[156,13,156,14],[156,16,156,17],[156,19,156,21],[156,23,156,25],[154,7,154,8],[154,10,154,11],[154,13,154,14],[154,16,154,17],[154,19,154,21],[154,23,154,25],[152,7,152,8],[152,10,152,11],[152,13,152,14],[152,16,152,17],[152,19,152,21],[152,23,152,25],[150,7,150,8],[150,10,150,11],[150,13,150,14],[150,16,150,17],[150,19,150,21],[150,23,150,25],[148,7,148,8],[148,10,148,11],[148,13,148,14],[148,16,148,17],[148,19,148,21],[148,23,148,25],[146,7,146,8],[146,10,146,11],[146,13,146,14],[146,16,146,17],[146,19,146,21],[146,23,146,25],[144,7,144,8],[144,10,144,11],[144,13,144,14],[144,16,144,17],[144,19,144,21],[144,23,144,25],[141,7,141,8],[141,10,141,11],[141,13,141,14],[141,16,141,17],[141,19,141,21],[141,23,141,25],[139,7,139,8],[139,10,139,11],[139,13,139,14],[139,16,139,17],[139,19,139,21],[139,23,139,25],[137,7,137,8],[137,10,137,11],[137,13,137,14],[137,16,137,17],[137,19,137,21],[137,23,137,25],[133,23,133,25],[135,7,135,8],[135,10,135,11],[135,13,135,14],[135,16,135,17],[135,19,135,21],[135,23,135,25],[129,10,129,11],[129,13,129,14],[129,16,129,17],[129,19,129,21],[129,23,129,25],[133,7,133,8],[133,10,133,11],[133,13,133,14],[133,16,133,17],[133,19,133,21],[131,7,131,8],[131,10,131,11],[131,13,131,14],[131,16,131,17],[131,19,131,21],[131,23,131,25],[127,7,127,8],[127,10,127,11],[127,13,127,14],[127,16,127,17],[127,19,127,21],[127,23,127,25],[123,10,123,11],[123,13,123,14],[123,16,123,17],[123,19,123,21],[123,23,123,25],[125,10,125,11],[125,13,125,14],[125,16,125,17],[125,19,125,21],[125,23,125,25],[122,7,122,8],[122,10,122,11],[122,13,122,14],[122,16,122,17],[122,19,122,21],[122,23,122,25],[120,7,120,8],[120,10,120,11],[120,13,120,14],[120,16,120,17],[120,19,120,21],[120,23,120,25],[118,7,118,8],[118,10,118,11],[118,13,118,14],[118,16,118,17],[118,19,118,21],[118,23,118,25],[116,7,116,8],[116,10,116,11],[116,13,116,14],[116,16,116,17],[116,19,116,21],[116,23,116,25],[114,7,114,8],[114,10,114,11],[114,13,114,14],[114,16,114,17],[114,19,114,21],[114,23,114,25],[111,7,111,8],[111,10,111,11],[111,13,111,14],[111,16,111,17],[111,19,111,21],[111,23,111,25],[105,13,105,14],[105,16,105,17],[105,19,105,21],[105,23,105,25],[103,7,103,8],[103,10,103,11],[103,13,103,14],[103,16,103,17],[103,23,103,25],[101,7,101,8],[101,10,101,11],[101,13,101,14],[101,16,101,17],[101,23,101,25],[99,19,99,20],[99,23,99,25],[100,7,100,8],[100,10,100,11],[100,13,100,14],[100,19,100,21],[90,28,90,35],[95,13,95,14],[95,16,95,17],[97,13,97,14],[99,7,99,8],[99,10,99,11],[99,13,99,14],[99,16,99,17],[92,23,95,25],[94,7,94,8],[94,13,94,14],[94,16,94,17],[94,19,94,20],[85,7,85,11],[86,7,86,11],[88,7,88,11],[90,7,90,11],[92,7,93,8],[92,10,93,11],[92,13,93,14],[92,16,93,17],[92,19,93,20],[66,13,66,14],[66,22,66,23],[66,28,66,29],[67,4,67,8],[67,10,67,11],[67,13,67,14],[67,22,67,23],[67,28,67,29],[64,28,64,29],[65,4,66,8],[65,10,65,11],[65,13,65,14],[65,16,67,17],[65,19,67,20],[65,22,65,23],[65,25,67,26],[65,28,65,29],[66,10,66,11],[64,10,64,11],[64,13,64,14],[64,16,64,17],[64,19,64,20],[64,22,64,23],[64,25,64,26],[60,7,60,31],[61,10,63,11],[61,13,63,14],[61,16,63,17],[61,19,63,20],[61,22,63,23],[61,25,63,26],[61,28,63,29],[63,4,63,8],[27,17,27,23],[27,25,27,30],[50,19,50,23],[51,7,51,11],[51,13,51,17],[51,19,51,23],[41,7,41,11],[44,7,44,11],[46,7,46,11],[48,7,49,11],[49,13,49,17],[50,7,50,11],[50,13,50,17],[42,13,42,14],[41,13,41,14],[36,24,36,26],[10,3,10,30],[161,7,161,26],[16,32,27,37],[34,0,34,4],[34,10,34,11],[36,10,36,11],[40,13,40,14],[40,7,40,11],[3,7,3,23],[5,7,5,15],[5,19,5,23],[7,7,7,15],[7,19,7,23],[31,7,31,28],[38,7,38,11],[38,13,38,14],[39,13,39,14],[11,7,11,30],[13,3,13,7],[13,10,13,14],[13,17,13,22],[13,25,13,30],[27,3,27,8],[27,10,27,15]]}
["Vertikal transport til det førstkommende betydende grundvandsmagasin - Oliestoffer"]
[]
[]
["Lokalitetsnavn:",null,null,null,null,null,null,{"$f":"IF(Ops_navn<>\"\",Ops_navn,\"\")","v":""}]
[]
["Adresse:",null,null,null,null,null,null,{"$f":"IF(Ops_adr<>\"\",Ops_adr,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Postnr./By:",null,{"$f":"IF(Ops_post<>\"\",Ops_post,\"\")","v":""}]
[]
["Lokalitetsnummer:",null,null,null,null,null,null,{"$f":"IF(Ops_lok<>\"\",Ops_lok,\"\")","v":""},null,null,null,null,null,null,null,null,null,"Projektnr:",null,{"$f":"IF(Ops_pro<>\"\",Ops_pro,\"\")","v":""}]
[]
[]
[]
[null,null,null,null,null,null,null,"Der skal vælges mellem de følgende beregningsmodeller for vertikal transport af organiske stoffer igennem et jordlag ned til førstkommende grundvandsmagasin"]
[]
[null,null,null,"Model A+C*",null,null,null,null,null,null,"Model B\n DTU V1D model 1a**",null,null,null,null,null,null,"Model B\n DTU V1D model 1b**",null,null,null,null,null,null,null,"Model B\n DTU V1D model 2**"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Der henvises til følgende Miljøprojekter:\n\n* JAGG 2 - Vertikal transport ned til førstkommende betydende magasin.\nChristensen, A.G., Binning, P. J., Troldborg, M., Kjeldsen, P. og Broholm, M.\nMiljøprojekt nr. 1828, 2016.\nMiljøstyrelsen\n\n** A risk assessment tool for contaminated sites in low-permeability fractured media.\nChambon, J., Bjerg, P.L. og Binning, P.J.\nEnvironmental Project No. 1786, 2015.\nThe Danish Environmental Protection Agency"]
[null,"Tid = 0"]
[]
[]
[]
[]
[]
[null,"Tid = x"]
[]
[]
[]
[null,null,null,"Stationære forhold kan opnås.\nKontinuer kilde. Dermed kan der beregnes en flux og en koncentration, som kan overføres til grundvandsmodulet. ",null,null,null,null,null,null,"Indledende stigende og herefter faldende koncentrationsbidrag til det førstkommende grundvandsmagasin.",null,null,null,null,null,null,"Stationære forhold kan opnås.\nKontinuer kilde. Dermed kan der beregnes en flux og koncentration, som kan overføres til grundvandsmodulet. ",null,null,null,null,null,null,null,"Aftagende koncentrationsbidrag til førstkommende grundvandsmagasin, da kilden i matrix udvaskes. "]
[]
[]
[]
["Kildeområde",null,null,null,null,null,null,"Indtast data om kildeområde.\n"]
[]
[]
["Længde af kildeområde",null,null,null,null,"Y",null,null,null,null,null,null,null,"m",{"$f":"IF(ISTEXT(Verolie_Y),\"Tjek decimal\",\"\")","v":""}]
[]
["Bredde af kildeområde",null,null,null,null,"X",null,null,null,null,null,null,null,"m",{"$f":"IF(ISTEXT(Verolie_X),\"Tjek decimal\",\"\")","v":""},null,null,"Areal af det forurenede område ",null,null,null,null,null,null,{"$f":"D_VerOlie_areal","v":0},null,null,null,"m2"]
[]
[null,null,null,null,null,null,null,"Kommune/Egn",null,null,null,null,null,"Nettonedbør"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"N"]
["Nettonedbør",null,null,null,null,null,null,{"$f":"IF(D_VerOlie_egn_syst<>\"\",D_VerOlie_egn_syst,\"\")","v":""},null,null,null,null,null,{"$f":"IF(ISNUMBER(D_VerOlie_infiltration_syst),D_VerOlie_infiltration_syst,\"\")","v":""}]
["Kommune/Egn"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"mm/år"]
[]
["Afstand til grundvandsspejl",null,null,null,null,"z",null,null,null,null,null,null,null,"m",{"$f":"IF(ISTEXT(Verolie_z),\"Tjek decimal\",\"\")","v":""}]
[]
["Porevandshastighed",null,null,null,null,"Vw",null,{"$f":"D_verolie_Vw_year","v":""},null,null,null,null,null,"m/år",null,null,"(Porevandshastigheden vises kun efter indtastning af jordparametre)"]
[]
[null,null,null,null,null,null,null,"Normalrange (stiger med afstand z)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Beregnet iht.  z "]
[null,null,null,null,null,null,null,"2-20 m",null,null,null,null,null,"jf. app. 5.8 figur 2.0",null,null,null,null,null,"Brugerdata"]
["Longitudinal dispersivitet",null,null,null,null,"αL,W",null,"0,004-0,07",null,null,null,null,null,{"$f":"D_verolie_alfaLw_beregn","v":9.9999999999999994E-37},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Verolie_alfaLw),\"Tjek decimal\",\"\")","v":""}]
[]
[]
["Varighed af spild",null,null,null,null,"a",null,null,null,null,null,null,null,"år",{"$f":"IF(OR(D_verOlie_AC,D_verOlie_DTU1b,D_verOlie_DTU2),\"DTU V1D model 1a er ikke valgt og dette felt skal derfor være tomt\",IF(ISNUMBER(VerOlie_a_tjek),\"\",\"DTU V1D model 1a er valgt - Tast varighed af spild\"))","v":"DTU V1D model 1a er ikke valgt og dette felt skal derfor være tomt"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(D_verOlie_AC,D_verOlie_DTU1b,D_verOlie_DTU2),0,VerOlie_a_tjek)","v":0}]
["(DTU V1D-model 1a)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(D_verOlie_AC,D_verOlie_DTU1b,D_verOlie_DTU2),1,\"\")","v":1}]
[]
[]
[]
["Jordparametre"]
[null,null,null,null,null,null,null,"Vælg jordart for fugacitetsberegning eller indtast egne jordartsdata"]
[null,null,null,null,null,null,null,null,null,null,"Poreluft-volumen",null,null,"Vand-indhold",null,null,"Samlet\nporøsitet",null,null,"Volumen\naf jordskellet",null,null,"Korn-rumvægt\n(kg/l)",null,null,"Bulk\nmassefylde\n (kg/l)",null,null,"% indhold af organisk kulstof"]
[]
[null,null,null,null,"Jordtype"]
[null,null,null,null,null,null,null,null,null,null,"VL",null,null,"VV",null,null,"e=VL+VV",null,null,"VJ",null,null,"d",null,null,"r",null,null,"foc"]
[null,null,null,null,{"$f":"IF(D_VerOlie_jord_syst<>\"\",D_VerOlie_jord_syst,)","v":0},null,null,null,null,null,{"$f":"IF(D_VerOlie_thetaa_int<>\"\",D_VerOlie_thetaa_int,\"\")","v":""},null,null,{"$f":"IF(D_VerOlie_thetaw_int<>\"\",D_VerOlie_thetaw_int,\"\")","v":""},null,null,{"$f":"D_VerOlie_ntotal","v":{"$error":"#VALUE!"}},null,null,{"$f":"D_Verolie_volj","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(D_VerOlie_d_int<>\"\",D_VerOlie_d_int,\"\")","v":""},null,null,{"$f":"D_Verolie_rhob","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(D_VerOlie_foc_int<>\"\",D_VerOlie_foc_int,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_VerOlie_thetaa_syst<>\"\",D_VerOlie_thetaa_syst,\"\")","v":""},null,null,{"$f":"IF(D_VerOlie_thetaw_syst<>\"\",D_VerOlie_thetaw_syst,\"\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(D_VerOlie_d_syst<>\"\",D_VerOlie_d_syst,\"\")","v":""},null,null,null,null,null,{"$f":"IF(D_VerOlie_foc_syst<>\"\",D_VerOlie_foc_syst,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Verolie_My_VL),\"Tjek decimal\",IF(ISTEXT(Verolie_My_VV),\"Tjek decimal\",IF(ISTEXT(Verolie_My_d),\"Tjek decimal\",IF(ISTEXT(Verolie_My_foc),\"Tjek decimal\",\"\"))))","v":""}]
[]
[]
["Ved sprækketransport",null,null,null,null,null,null,"Indtast sprækkeegenskaber eller anvend standard forslag"]
[null,null,null,null,null,null,null,null,null,null,"Standardforslag",null,null,"Brugerdata"]
[]
[null,"Sprækkeafstand (2B) ",null,null,null,null,null,null,null,null,5,null,null,null,null,null,"m","Normalinterval er fra 1 m i oxideret ler (de øvre jordlag) og 5 m i reduceret ler i større dyber"]
[]
[null,"Sprækkeapertur (2b)",null,null,null,null,"Beregnes",null,null,null,null,null,null,{"$f":"D_verOlie_2bapertur","v":7.9418567312567668E-5},null,null,"m"]
[]
[null,"Bulk-hydraulisk ledningsevne (Kb)",null,null,null,null,null,null,null,null,6.2999999999999995E-8,null,null,null,null,null,"m/s","Normalinterval er fra 2,4 x10-6 m/s i oxideret ler (de øvre jordlag) og 6,3 x10-8 m/s i reduceret ler i større dybder"]
[]
[]
[]
[{"$f":"CONCATENATE(\"Beregning: Stationær (ligevægt) koncentration efter vertikal transport  ned til grundvandsspejlet i \", Verolie_z,\" m´s dybde (z)\")","v":"Beregning: Stationær (ligevægt) koncentration efter vertikal transport  ned til grundvandsspejlet i  m´s dybde (z)"}]
[]
["Data for forurening er overført fra fugacitetsmodulet for oliestoffer "]
[]
["Målepunkt",null,null,null,null,null,null,{"$f":"IF(Olie_målepunkt<>\"\",D_olie_målepunkt,\"\")","v":""}]
["Dato",null,null,null,null,null,null,{"$f":"IF(Olie_dato<>\"\",D_olie_dato,\"\")","v":""}]
[]
["Fri fase i jord?",null,null,null,null,null,null,{"$f":"D_Olie_FF","v":"Nej"}]
[]
["Anvendt Brugerdata",null,null,null,null,null,null,{"$f":"D_verolie_bruger","v":"Nej"},null,null,null,null,null,"Den anvendte vertikale transportmodel er",null,null,null,null,null,null,{"$f":"D_Verolie_model","v":"Model A + C"},null,null,null,null,null,null,null,{"$f":"IF(D_verOlie_DTU1a,IF(ISTEXT(D_Verolie_a),\"Husk at indtaste varighed af spild\",\"\"),\"\")","v":""}]
[]
[null,null,null,null,null,null,null,"Porevands-konc\nkonc.",null,null,"Nedbrydnings-konstant anvendt for alle oliestoffer",null,null,"Stationær (ligevægt) porevandskonc. i toppen af GV-magasin",null,null,{"$f":"CONCATENATE(\"Transient porevandskonc. i toppen af GV-magasin efter\", Verolie_t,\" år\")","v":"Transient porevandskonc. i toppen af GV-magasin efter år"},null,null,"Grundvands-\nkriterium",null,null,null,"Overskridelse \naf kriteriet i toppen af GV-magasin under stationære forhold"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Default",0]
[]
[null,null,null,null,null,null,null,null,null,null,"Bruger",null,null,null,null,null,null,"år",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(Verolie_t),\"Tjek decimal\",IF(ISTEXT(Verolie_My_ned),\"Tjek decimal\",\"\"))","v":""}]
[]
[null,null,null,null,null,null,null,"µg/l",null,null,"dage-1",null,null,"µg/l",null,null,"µg/l",null,null,"µg/l",null,null,null,"gange"]
["BTEX'er"]
[null,"Benzen",null,null,null,null,null,{"$f":"D_verolie_cv_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_52","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_52","v":1},null,null,null,{"$f":"D_VerOlie_overskr_52","v":""}]
[]
[null,"Toluen",null,null,null,null,null,{"$f":"D_verolie_cv_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_54","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_54","v":5},null,null,null,{"$f":"D_VerOlie_overskr_54","v":""}]
[]
[null,"Ethylbenzen",null,null,null,null,null,{"$f":"D_verolie_cv_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_58","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum Xylener",null,null,null,null,null,{"$f":"D_verolie_cv_57","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_57","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_57","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum Xylener + ethylbenzen",null,null,null,null,null,{"$f":"D_VerOlie_cv_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_VerOlie_cz_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_VerOLie_czt_57_58","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_57","v":5},null,null,null,{"$f":"D_VerOlie_overskr_57","v":""}]
[]
[null,"Naphthalen",null,null,null,null,null,{"$f":"D_verolie_cv_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_103","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_103","v":1},null,null,null,{"$f":"D_VerOlie_overskr_103","v":""}]
[]
["Kulbrintefraktioner"]
[null,"C6-C10",null,null,null,null,null,{"$f":"D_verolie_cv_510","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_510","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_510","v":{"$error":"#DIV/0!"}}]
[]
[null,"C10-C15",null,null,null,null,null,{"$f":"D_verolie_cv_1015","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_1015","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_1015","v":{"$error":"#DIV/0!"}}]
[]
[null,"C15-C20",null,null,null,null,null,{"$f":"D_verolie_cv_1520","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_1520","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_1520","v":{"$error":"#DIV/0!"}}]
[]
[null,"C20-C35",null,null,null,null,null,{"$f":"D_verolie_cv_2040","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_2040","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_2040","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af kulbrinter",null,null,null,null,null,{"$f":"D_verolie_cv_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_1","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_1","v":9},null,null,null,{"$f":"D_VerOlie_overskr_1","v":""}]
[]
[]
["Alkylbenzener, aromatiske kulbrinter "]
[]
[null,"C9-C10 aromatiske kulbrinter",null,null,null,null,null,{"$f":"D_Verolie_910_cv","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_cz_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_czt_910","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_60","v":1},null,null,null,{"$f":"D_VerOlie_overskr_910","v":""}]
[]
["Polyaromatiske Kulbrinter (PAH)"]
[]
[null,"Fluoranthen",null,null,null,null,null,{"$f":"D_verolie_cv_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_verolie_Cz_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_156","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_156","v":0.1},null,null,null,{"$f":"D_VerOlie_overskr_156","v":""}]
[]
[null,"Benzo(a)pyren",null,null,null,null,null,{"$f":"D_verolie_cv_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_256","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_256","v":0.01},null,null,null,{"$f":"D_VerOlie_overskr_256","v":""}]
[]
[null,"Benzo(b+k)fluoranthen",null,null,null,null,null,{"$f":"D_verolie_cv_255","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_255","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_255","v":{"$error":"#DIV/0!"}}]
[]
[null,"Benzo(ghi)perylen",null,null,null,null,null,{"$f":"D_verolie_cv_258","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_258","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_258","v":{"$error":"#DIV/0!"}}]
[]
[null,"Indeno(1,2,3-cd)pyren",null,null,null,null,null,{"$f":"D_verolie_cv_352","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_352","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_352","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af 4 PAH`er",null,null,null,null,null,{"$f":"D_verolie_cv_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_21","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_verolie_gkk_21","v":0.1},null,null,null,{"$f":"D_VerOlie_overskr_21","v":""}]
[]
["NSO-forbindelser"]
[null,"Benzo(b)thiophen",null,null,null,null,null,{"$f":"D_verolie_cv_10","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_10","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_10","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dibenzofuran",null,null,null,null,null,{"$f":"D_verolie_cv_11","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_11","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_11","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dibenzothiophen",null,null,null,null,null,{"$f":"D_verolie_cv_12","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_12","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_12","v":{"$error":"#DIV/0!"}}]
[]
[null,"Acridin",null,null,null,null,null,{"$f":"D_verolie_cv_13","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_13","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_13","v":{"$error":"#DIV/0!"}}]
[]
[null,"Carbazol",null,null,null,null,null,{"$f":"D_verolie_cv_14","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_14","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_14","v":{"$error":"#DIV/0!"}}]
[]
[null,"Anilin",null,null,null,null,null,{"$f":"D_verolie_cv_15","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_15","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_15","v":{"$error":"#DIV/0!"}}]
[]
[null,"Dimethyldisulfid",null,null,null,null,null,{"$f":"D_verolie_cv_16","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_16","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_16","v":{"$error":"#DIV/0!"}}]
[]
[null,"Sum af NSO-forbindelser",null,null,null,null,null,{"$f":"D_verolie_cv_nso","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_lambda","v":0},null,null,{"$f":"D_Verolie_Cz_nso","v":{"$error":"#DIV/0!"}},null,null,{"$f":"D_Verolie_Czt_nso","v":{"$error":"#DIV/0!"}}]

{"sheet":"Dataark_Vertikal-Olie","index":55,"n_rows":187,"n_cols":17,"rows_kept":187,"cut":false,"hidden":true,"merged":[[153,6,153,7],[7,1,7,10],[9,2,9,10],[35,2,35,6],[35,8,35,10],[145,8,145,13]]}
[]
[]
[null,"Vertikal transport igennem enten homogen vandmættet ler eller umættet ler og sand fra en overliggende kontinuert kilde","Model A + C",true]
[null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kilde, hvor varigheden af spildet er kendt","Model B DTU V1D Model 1a",false]
[null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kontinuert kilde","Model B DTU V1D Model 1b",false]
[null,"Vertikal transport igennem homogen vandmættet sprækket ler fra den aftagende kilde i lermatrix","Model B DTU V1D Model 2",false]
[null,"Den anvendte model for vertikaltransport - Oliestoffer er ",null,{"$f":"IF(D_verOlie_AC,C$3,IF(D_verOlie_DTU1a,C$4,IF(D_verOlie_DTU1b,C$5,C$6)))","v":"Model A + C"}]
[null,"DATAARK - Vertikal Transport i umættede zone  - Oliestoffer (MODEL A+C, FINAL DOMENICO)",null,null,null,null,null,null,null,null,null,null,"Systemnavn","Oprindelsessted"]
[]
[null,null,"Lokalitetsspecifikke data/umættet zone"]
[null,null,null,"Forkortelse","Enhed","Oprindelsessted",null,"Interval","Default/Beregnet","Indtastet","Anvendt"]
[null,null,"Jordtype",null,null,null,null,null,null,{"$f":"Verolie_My_jord","v":0},{"$f":"IF(ISTEXT(J12),J12,I12)","v":0},null,"D_Verolie_jord","Input"]
[null,null,"Porevandshastighed","Vw","m/dag","beregnes",null,null,{"$f":"B_Verolie_Vw","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J13),J13,IF(I13<>0,I13,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Verolie_Vw","Beregnes"]
[null,null,"Porevandshastighed","Vw","m/år","Enhed konvertere",null,null,null,null,{"$f":"IF(ISNUMBER(D_Verolie_Vw),D_Verolie_Vw*365,\"\")","v":""},null,"D_verolie_vw_year","Beregnes i dataarket"]
[null,null,"Darcy hastighed (vand)","qw","m/dag","input",null,null,{"$f":"D_Verolie_infiltration","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J15),J15,IF(I15<>0,I15,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Verolie_qw","Input"]
[null,null,"Vandindhold","qw","-","input",null,null,null,{"$f":"Verolie_My_VV","v":0},{"$f":"IF(VALUE(J16),J16,IF(I16<>0,I16,\"\"))","v":""},null,"D_Verolie_thetaw","Input"]
[null,null,"Luftindhold","qa","-","input",null,null,null,{"$f":"IF(ISNUMBER(Verolie_My_VL),Verolie_My_VL,\"-\")","v":"-"},{"$f":"IF(ISNUMBER(J17),J17,IF(I17<>0,I17,0))","v":0},null,"D_Verolie_thetaa","Input"]
[null,null,"Total porøsitet (VL+VV)","n","-","input",null,null,{"$f":"SUM(D_VerOlie_thetaw+D_VerOlie_thetaa)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J18),J18,IF(I18<>0,I18,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Verolie_ntotal","Beregnes i dataarket"]
[null,null,"Volumen af jordskellet","Vj",null,null,null,null,{"$f":"1-D_VerOlie_ntotal","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Verolie_volj","Beregnes i dataarket"]
[null,null,"Kildens længde","Y","m","input",null,null,null,{"$f":"Verolie_Y","v":0},{"$f":"J20","v":0},null,"D_Verolie_Y","Input"]
[null,null,"Kildens bredde","X","m","input",null,null,null,{"$f":"Verolie_X","v":0},{"$f":"J21","v":0},null,"D_Verolie_X","Input"]
[null,null,"Areal Kilden",null,null,null,null,null,null,null,{"$f":"D_Verolie_Y*D_Verolie_X","v":0}]
[null,null,"Afstand fra kildens underkant til GV-spejl","Z","m","input",null,null,null,{"$f":"Verolie_z","v":0},{"$f":"J23","v":0},null,"D_Verolie_Z","Input"]
[null,null,"% Indhold organisk kulstof","foc (%)","-","input",null,null,null,{"$f":"Verolie_My_foc","v":0},"",null,null,"Input"]
[null,null,"Fraktion organisk indhold","foc",null,"Enhed konverteres ",null,null,{"$f":"B_verolie_foc","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Verolie_foc","Beregnes"]
[null,null,"Korn rumvægt","d","kg/l","input",null,null,null,{"$f":"Verolie_My_d","v":0},{"$f":"IF(VALUE(J26),J26,IF(I26<>0,I26,\"\"))","v":""},null,"D_Verolie_d","Input"]
[null,null,"Bulkmassefylde= volumenvægt","(rho)r","kg/l","Beregnet",null,null,{"$f":"B_verolie_rhob","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(J27),J27,IF(I27<>0,I27,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Verolie_rhob","Beregnes"]
[null,null,"Nettoinfiltration= nettonedbør","N","m/dag","Enhed konverteres",null,null,{"$f":"B_VerOlie_infiltration","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},null,"D_Verolie_infiltration","Beregnes"]
[null,null,"Kommune/Egn",null,null,null,null,null,null,{"$f":"Verolie_My_Egn","v":0},{"$f":"IF(ISTEXT(J29),J29,I29)","v":0},null,"D_Verolie_Egn","Input"]
[null,null,"Nettoinfiltration= nettonedbør","N","mm/år","input",null,null,null,{"$f":"Verolie_My_N","v":0},"",null,"D_Verolie_infiltration_Temp","Input"]
[null,null,"Long. dispersivitet (vand)","(alfa)L,w","m","Bergenes",null,null,{"$f":"B_verolie_alfaLw","v":9.9999999999999994E-37},{"$f":"Verolie_alfaLw","v":0},9.9999999999999994E-37,null,"D_Verolie_alfaLw","Standardværdi"]
[null,null,"Trans. dispersivitet (vand)","(alfa)T,w","m","Beregnes",null,null,{"$f":"B_Verolie_alfaTw","v":1.0000000000000001E-37},null,1.0000000000000001E-37,null,"D_Verolie_alfaTw","Standardværdi"]
[null,null,"Transient løsning, tid","t","år","input",null,null,null,{"$f":"Verolie_t","v":0},null,null,null,"Input"]
[null,null,"Transient løsning, tid (dage)","t","dage","Beregnes",null,null,{"$f":"B_Verolie_t","v":0},null,"",null,"D_Verolie_t","Beregnes"]
[]
[null,null,"Stoffer"]
[null,null,null,"Forkortelse","Enhed","Oprindelsessted",null,null,"Default/Ber./overført","Indtastet","Anvendt"]
[null,null,"Nedbrydning (1. orden) default/ bruger","(lambda)_ae_n","dag^-1","input",null,null,{"$f":"Verolie_ned","v":0},{"$f":"Verolie_My_ned","v":0},{"$f":"IF(ISNUMBER(J38),J38,I38)","v":0},null,"D_VerOlie_lambda","Input"]
[]
[null,null,"Anvendt brugerdata -fugacitet-olie",null,null,null,null,null,{"$f":"D_Olie_bruger","v":"Nej"},{"$f":"IF(I40=\"nej\",0,1)","v":0}]
[null,null,"Anvendt brugerdata",null,null,null,null,null,null,{"$f":"SUM($J16:$J17,$J24:$J26,$J30:J37,J38,J40)","v":0},{"$f":"IF(J41>0,\"Ja, se bemærkning\",\"Nej\")","v":"Nej"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(VALUE(J42),J42,IF(I42<>0,I42,\"\"))","v":""},null,"FALSE generes for Czt såfremt R >8.700"]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"D_Verolie_model","v":"Model A + C"},{"$f":"D_Verolie_model","v":"Model A + C"},{"$f":"D_Verolie_model","v":"Model A + C"},{"$f":"D_Verolie_model","v":"Model A + C"}]
[null,null,null,null,null,"Overført fra Oliestoffer","Overført fra Oliestoffer","Overført fra Oliestoffer","Overført fra Oliestoffer","Imput","Beregnet","Beregnet","Beregnet","Beregnet","Beregnet","Overført fra Oliestoffer","Beregnet"]
[null,null,null,null,null,"Beregnet kildekonc Cv","Log Kow","DL","Henry","Nedbrydningskonstant","Retardation","Stationær konc ved z","Transient konc ved t","Flux (stationært)","Flux, transient (t) i toppen af GV magasin","Grundvands\nkriteriet","Overskridelse"]
[null,null,null,null,null,"µg/l",null,"m²/s",null,null,null,"µg/l","µg/l","mg/år","mg/år","µg/l","gange"]
[50,"C5-C6",null,null,null,null,null,null,null,null,null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_50,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_50, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_50,IF(ISNUMBER(B_VerOlie_DTU_czt_50),B_VerOlie_DTU_czt_50,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_50","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_50","v":{"$error":"#DIV/0!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_51","v":2.72},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},{"$f":"B_olie_kH_51","v":141.86000000000001},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_verolie_R_51","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_51,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_51, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_51,IF(ISNUMBER(B_VerOlie_DTU_czt_51),B_VerOlie_DTU_czt_51,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_51","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_51","v":{"$error":"#DIV/0!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_511","v":3.39},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},{"$f":"B_olie_kH_511","v":126.66},0,{"$f":"B_VerOlie_R_511","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_511,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_511, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_511,IF(ISNUMBER(B_VerOlie_DTU_czt_511),B_VerOlie_DTU_czt_511,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_511","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_511","v":{"$error":"#DIV/0!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_512","v":3.21},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},{"$f":"B_olie_kH_512","v":173.27},0,{"$f":"B_VerOlie_R_512","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_512,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_512, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_512,IF(ISNUMBER(B_VerOlie_DTU_czt_512),B_VerOlie_DTU_czt_512,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_512","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_512","v":{"$error":"#DIV/0!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_513","v":3.6},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},{"$f":"B_olie_kH_513","v":170.226},0,{"$f":"B_VerOlie_R_513","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_513,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_513, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_513,IF(ISNUMBER(B_VerOlie_DTU_czt_513),B_VerOlie_DTU_czt_513,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_513","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_513","v":{"$error":"#DIV/0!"}}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cv","v":{"$error":"#DIV/0!"}},null,null,null,0,null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_510,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_510, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_510,IF(ISNUMBER(B_VerOlie_DTU_czt_510),B_VerOlie_DTU_czt_510,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_510","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_510","v":{"$error":"#DIV/0!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_52","v":2.13},{"$f":"B_olie_DL_52","v":9.3000000000000007E-6},{"$f":"B_olie_kH_52","v":0.56240000000000001},0,{"$f":"B_VerOlie_R_52","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_52,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_52, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_52,IF(ISNUMBER(B_VerOlie_DTU_czt_52),B_VerOlie_DTU_czt_52,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_52","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_52","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_52_gkk","v":1},{"$f":"IF(ISNUMBER(D_Verolie_Cz_52),IF(D_Verolie_Cz_52/P55>1,D_Verolie_Cz_52/P55,\"Nej\"),\"\")","v":""}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_53","v":4.29},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},{"$f":"B_olie_kH_53","v":308.16000000000003},0,{"$f":"B_VerOlie_R_53","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_53,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_53, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_53,IF(ISNUMBER(B_VerOlie_DTU_czt_53),B_VerOlie_DTU_czt_53,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_53","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_53","v":{"$error":"#DIV/0!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_54","v":2.73},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},{"$f":"B_olie_kH_54","v":0.67379999999999995},0,{"$f":"B_VerOlie_R_54","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_54,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_54, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_54,IF(ISNUMBER(B_VerOlie_DTU_czt_54),B_VerOlie_DTU_czt_54,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_54","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_54","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_54_gkk","v":5},{"$f":"IF(ISNUMBER(D_Verolie_Cz_54),IF(D_Verolie_Cz_54/P57>1,D_Verolie_Cz_54/P57,\"Nej\"),\"\")","v":""}]
[55,">8 - 10, alifater",">8 - 10, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_55B_cv,D_Olie_55A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_55b,B_olie_kow_55a)","v":5.15},{"$f":"IF(D_Olie_profil=1,B_olie_DL_55B,B_olie_DL_55A)","v":6.2232552378840063E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_55b,B_olie_kH_55a)","v":534.27},0,{"$f":"B_VerOlie_R_55","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_55,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_55, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_55,IF(ISNUMBER(B_VerOlie_DTU_czt_55),B_VerOlie_DTU_czt_55,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_55","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_55","v":{"$error":"#DIV/0!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_57","v":3.2},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},{"$f":"B_olie_kH_57","v":0.72750000000000004},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_57","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_57,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_57, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_57,IF(ISNUMBER(B_VerOlie_DTU_czt_57),B_VerOlie_DTU_czt_57,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_57","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_57","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_57_gkk","v":5},{"$f":"IF(ISNUMBER(D_Verolie_Cz_57),IF(D_Verolie_Cz_57/P62>1,D_Verolie_Cz_57/P62,\"Nej\"),\"\")","v":""}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_58","v":3.15},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},{"$f":"B_olie_kH_58","v":0.7984},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_58","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_58,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_58, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_58,IF(ISNUMBER(B_VerOlie_DTU_czt_58),B_VerOlie_DTU_czt_58,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_58","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_58","v":{"$error":"#DIV/0!"}}]
[null,null,"Sum af xylener + Ethylbenzen",null,null,{"$f":"SUM(F62:F63)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,{"$f":"IF(OR(D_verOlie_AC,D_verOlie_DTU1b),SUM(L62:L63),\"ikke stationær\")","v":{"$error":"#DIV/0!"}},{"$f":"SUM(M62:M63)","v":{"$error":"#DIV/0!"}}]
[59,null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"B_olie_kH_59","v":0.89},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_59","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_59,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_59, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_59,IF(ISNUMBER(B_VerOlie_DTU_czt_59),B_VerOlie_DTU_czt_59,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_59","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_59","v":{"$error":"#DIV/0!"}}]
[60,null,">8 -10, aromater,øvrige",null,null,{"$f":"D_olie_60_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"B_olie_kH_59","v":0.89},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_59","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_60,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_60, \"ikke stationær\"))","v":{"$error":"#NAME?"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_60,IF(ISNUMBER(B_VerOlie_DTU_czt_60),B_VerOlie_DTU_czt_60,\"\"))","v":{"$error":"#NAME?"}},{"$f":"B_VerOlie_fluxstat_60","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_60","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_60_gkk","v":1},{"$f":"IF(ISNUMBER(D_Verolie_Cz_60),IF(D_Verolie_Cz_60/P66>1,D_Verolie_Cz_60/P66,\"Nej\"),\"\")","v":""}]
[910,null,null,null,null,{"$f":"D_olie_910_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"B_olie_kH_59","v":0.89},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_59","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_verolie_cz_910,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_910, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_Verolie_czt_910,IF(ISNUMBER(B_VerOlie_DTU_czt_910),B_VerOlie_DTU_czt_910,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_Verolie_fluxstat_910","v":{"$error":"#DIV/0!"}},{"$f":"B_verolie_fluxtrans_910","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_60_gkk","v":1},{"$f":"IF(ISNUMBER(D_Verolie_cz_910),IF(D_Verolie_cz_910/P67>1,D_Verolie_cz_910/P67,\"Nej\"),\"\")","v":""}]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cv","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Verolie_lambda","v":0},null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_1015,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_1015, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_1015,IF(ISNUMBER(B_VerOlie_DTU_czt_1015),B_VerOlie_DTU_czt_1015,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_1015","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_1015","v":{"$error":"#DIV/0!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_101","v":6.1},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},{"$f":"B_olie_kH_101","v":828.83849999999995},0,{"$f":"B_VerOlie_R_101","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_101,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_101, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_101,IF(ISNUMBER(B_VerOlie_DTU_czt_101),B_VerOlie_DTU_czt_101,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_101","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_101","v":{"$error":"#DIV/0!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater",null,null,null,null,null,null,0,null,null,{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_102,IF(ISNUMBER(B_VerOlie_DTU_czt_102),B_VerOlie_DTU_czt_102,\"\"))","v":{"$error":"#NAME?"}}]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_103","v":3.3},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},{"$f":"B_olie_kH_103","v":4.4582999999999998E-2},0,{"$f":"B_VerOlie_R_103","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_103,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_103, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_103,IF(ISNUMBER(B_VerOlie_DTU_czt_103),B_VerOlie_DTU_czt_103,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_103","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_103","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_103_gkk","v":1},{"$f":"IF(ISNUMBER(D_Verolie_Cz_103),IF(D_Verolie_Cz_103/P71>1,D_Verolie_Cz_103/P71,\"Nej\"),\"\")","v":""}]
[104,null,">10 - 12, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_104B_cv,D_Olie_104A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_104b,B_olie_kow_104a)","v":4.7300000000000004},{"$f":"IF(D_Olie_profil=1,B_olie_DL_104B,B_olie_DL_104A)","v":5.5260438461528997E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_104b,B_olie_kH_104a)","v":0.16700000000000001},0,{"$f":"B_VerOlie_R_104","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_104,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_104, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_104,IF(ISNUMBER(B_VerOlie_DTU_czt_104),B_VerOlie_DTU_czt_104,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_104","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_104","v":{"$error":"#DIV/0!"}}]
[105,">12 - 16, alifater",">12 - 16, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_105B_cv,D_Olie_105A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_105b,B_olie_kow_105a)","v":7.72},{"$f":"IF(D_Olie_profil=1,B_olie_DL_105B,B_olie_DL_105A)","v":5.0933919872504982E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_105b,B_olie_kH_105a)","v":726.05},0,{"$f":"B_VerOlie_R_105","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_105,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_105, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_105,IF(ISNUMBER(B_VerOlie_DTU_czt_105),B_VerOlie_DTU_czt_105,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_105","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_105","v":{"$error":"#DIV/0!"}}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater",null,null,null,null,null,null,0]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_107","v":4.07},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},{"$f":"B_olie_kH_107","v":0.11550000000000001},0,{"$f":"B_VerOlie_R_107","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_107,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_107, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_107,IF(ISNUMBER(B_VerOlie_DTU_czt_107),B_VerOlie_DTU_czt_107,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_107","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_107","v":{"$error":"#DIV/0!"}}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_108","v":3.92},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},{"$f":"B_olie_kH_108","v":0.18643799999999999},0,{"$f":"B_VerOlie_R_108","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_108,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_108, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_108,IF(ISNUMBER(B_VerOlie_DTU_czt_108),B_VerOlie_DTU_czt_108,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_108","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_108","v":{"$error":"#DIV/0!"}}]
[109,null,">12 - 16, aromater,øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_109B_cv,D_Olie_109A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_109b,B_olie_kow_109a)","v":4.4000000000000004},{"$f":"IF(D_Olie_profil=1,B_olie_DL_109B,B_olie_DL_109A)","v":5.9000000000000003E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_109b,B_olie_kH_109a)","v":7.8600000000000003E-2},0,{"$f":"B_VerOlie_R_109","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_109,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_109, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_109,IF(ISNUMBER(B_VerOlie_DTU_czt_109),B_VerOlie_DTU_czt_109,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_109","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_109","v":{"$error":"#DIV/0!"}}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cv","v":{"$error":"#DIV/0!"}},null,null,null,0,null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_1520,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_1520, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_1520,IF(ISNUMBER(B_VerOlie_DTU_czt_1520),B_VerOlie_DTU_czt_1520,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_1520","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_1520","v":{"$error":"#DIV/0!"}}]
[151,">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_151B_cv,D_Olie_151A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_151b,B_olie_kow_151a)","v":9.84},{"$f":"IF(D_Olie_profil=1,B_olie_DL_151B,B_olie_DL_151A)","v":4.4721099862171762E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_151b,B_olie_kH_151a)","v":8341.59},0,{"$f":"B_VerOlie_R_151","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_151,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_151, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_151,IF(ISNUMBER(B_VerOlie_DTU_czt_151),B_VerOlie_DTU_czt_151,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_151","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_151","v":{"$error":"#DIV/0!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater",null,null,null,null,null,null,0]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_153","v":4.18},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},{"$f":"B_olie_kH_153","v":9.7474650000000003E-3},0,{"$f":"B_VerOlie_R_153","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_153,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_153, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_153,IF(ISNUMBER(B_VerOlie_DTU_czt_153),B_VerOlie_DTU_czt_153,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_153","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_153","v":{"$error":"#DIV/0!"}}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_154","v":4.46},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},{"$f":"B_olie_kH_154","v":4.2860475E-3},0,{"$f":"B_VerOlie_R_154","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_154,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_154, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_154,IF(ISNUMBER(B_VerOlie_DTU_czt_154),B_VerOlie_DTU_czt_154,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_154","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_154","v":{"$error":"#DIV/0!"}}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_155","v":4.45},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},{"$f":"B_olie_kH_155","v":5.6336700000000003E-3},0,{"$f":"B_VerOlie_R_155","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_155,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_155, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_155,IF(ISNUMBER(B_VerOlie_DTU_czt_155),B_VerOlie_DTU_czt_155,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_155","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_155","v":{"$error":"#DIV/0!"}}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_156","v":5.16},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},{"$f":"B_olie_kH_156","v":8.977395E-4},0,{"$f":"B_VerOlie_R_156","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_156,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_156, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_156,IF(ISNUMBER(B_VerOlie_DTU_czt_156),B_VerOlie_DTU_czt_156,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_156","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_156","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_156_gkk","v":0.1},{"$f":"IF(ISNUMBER(D_verolie_Cz_156),IF(D_verolie_Cz_156/P85>1,D_verolie_Cz_156/P85,\"Nej\"),\"\")","v":""}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_157","v":4.88},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},{"$f":"B_olie_kH_157","v":1.2057674999999999E-3},0,{"$f":"B_VerOlie_R_157","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_157,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_157, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_157,IF(ISNUMBER(B_VerOlie_DTU_czt_157),B_VerOlie_DTU_czt_157,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_157","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_157","v":{"$error":"#DIV/0!"}}]
[]
[2025,"C21-C25",null,null,null,null,null,null,null,0]
[201,">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_201B_cv,D_Olie_201A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_201b,B_olie_kow_201a)","v":12.62},{"$f":"IF(D_Olie_profil=1,B_olie_DL_201B,B_olie_DL_201A)","v":3.9528308464137552E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_201b,B_olie_kH_201a)","v":37693},0,{"$f":"B_VerOlie_R_201","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_201,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_201, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_201,IF(ISNUMBER(B_VerOlie_DTU_czt_201),B_VerOlie_DTU_czt_201,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_201","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_201","v":{"$error":"#DIV/0!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter",null,null,null,null,null,null,0]
[]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cv","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Verolie_lambda","v":0},null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_2535,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_2535, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_2535,IF(ISNUMBER(B_VerOlie_DTU_czt_2535),B_VerOlie_DTU_czt_2535,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_2535","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_2535","v":{"$error":"#DIV/0!"}}]
[251,">25 - 35, alifater",">25 - 35, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_251B_cv,D_Olie_251A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_251b,B_olie_kow_251a)","v":14.58},{"$f":"IF(D_Olie_profil=1,B_olie_DL_251B,B_olie_DL_251A)","v":3.6715492605442101E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_251b,B_olie_kH_251a)","v":757252},0,{"$f":"B_VerOlie_R_251","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_251,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_251, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_251,IF(ISNUMBER(B_VerOlie_DTU_czt_251),B_VerOlie_DTU_czt_251,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_251","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_251","v":{"$error":"#DIV/0!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,null,null,0]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_253","v":5.76},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},{"$f":"B_olie_kH_253","v":1.2159E-3},0,{"$f":"B_VerOlie_R_253","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_253,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_253, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_253,IF(ISNUMBER(B_VerOlie_DTU_czt_253),B_VerOlie_DTU_czt_253,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_253","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_253","v":{"$error":"#DIV/0!"}}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_254","v":5.81},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},{"$f":"B_olie_kH_254","v":5.2992974999999999E-4},0,{"$f":"B_VerOlie_R_254","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_254,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_254, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_254,IF(ISNUMBER(B_VerOlie_DTU_czt_254),B_VerOlie_DTU_czt_254,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_254","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_254","v":{"$error":"#DIV/0!"}}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_255","v":5.78},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},{"$f":"B_olie_kH_255","v":6.6570524999999997E-5},0,{"$f":"B_VerOlie_R_255","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_255,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_255, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_255,IF(ISNUMBER(B_VerOlie_DTU_czt_255),B_VerOlie_DTU_czt_255,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_255","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_255","v":{"$error":"#DIV/0!"}}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_256","v":6.13},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},{"$f":"B_olie_kH_256","v":4.6305525000000001E-5},0,{"$f":"B_VerOlie_R_256","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_256,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_256, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_256,IF(ISNUMBER(B_VerOlie_DTU_czt_256),B_VerOlie_DTU_czt_256,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_256","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_256","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_256_gkk","v":0.01},{"$f":"IF(ISNUMBER(D_Verolie_Cz_256),IF(D_Verolie_Cz_256/P98>1,D_Verolie_Cz_256/P98,\"Nej\"),\"\")","v":""}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_257","v":6.75},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},{"$f":"B_olie_kH_257","v":1.4286825E-5},0,{"$f":"B_VerOlie_R_257","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_257,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_257, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_257,IF(ISNUMBER(B_VerOlie_DTU_czt_257),B_VerOlie_DTU_czt_257,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_257","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_257","v":{"$error":"#DIV/0!"}}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_258","v":6.63},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},{"$f":"B_olie_kH_258","v":3.3538575000000003E-5},0,{"$f":"B_VerOlie_R_258","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_258,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_258, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_258,IF(ISNUMBER(B_VerOlie_DTU_czt_258),B_VerOlie_DTU_czt_258,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_258","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_258","v":{"$error":"#DIV/0!"}}]
[259,null,">25 - 35, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_259B_cv,D_Olie_259A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_259b,B_olie_kow_259a)","v":7.11},{"$f":"IF(D_Olie_profil=1,B_olie_DL_259B,B_olie_DL_259A)","v":4.4493993711079091E-6},{"$f":"IF(D_Olie_profil=1,B_olie_kH_259b,B_olie_kH_259a)","v":4.95479E-5},0,{"$f":"B_VerOlie_R_259","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_259,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_259, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_259,IF(ISNUMBER(B_VerOlie_DTU_czt_259),B_VerOlie_DTU_czt_259,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_259","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_259","v":{"$error":"#DIV/0!"}}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cv","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Verolie_lambda","v":0},null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_3540,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_3540, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_3540,IF(ISNUMBER(B_VerOlie_DTU_czt_3540),B_VerOlie_DTU_czt_3540,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_3540","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_3540","v":{"$error":"#DIV/0!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_351","v":17.53},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},{"$f":"B_olie_kH_351","v":640374},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_351","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_351,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_351, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_351,IF(ISNUMBER(B_VerOlie_DTU_czt_351),B_VerOlie_DTU_czt_351,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_351","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_351","v":{"$error":"#DIV/0!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_352","v":6.7},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},{"$f":"B_olie_kH_352","v":3.52611E-5},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_352","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_352,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_352, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_352,IF(ISNUMBER(B_VerOlie_DTU_czt_352),B_VerOlie_DTU_czt_352,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_352","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_352","v":{"$error":"#DIV/0!"}}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cv","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Verolie_lambda","v":0},null,{"$f":"IF(D_verOlie_AC,B_Verolie_cz_2040,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_2040, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_2040,IF(ISNUMBER(B_VerOlie_DTU_czt_2040),B_VerOlie_DTU_czt_2040,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_2040","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_2040","v":{"$error":"#DIV/0!"}}]
[]
[20,"Sum af 7 PAH'er jord",null,null,null,null,null,null,null,{"$f":"D_Verolie_lambda","v":0}]
[21,"Sum af 4 PAH'er vand",null,null,null,{"$f":"SUM(F97+F100+F105)","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Verolie_lambda","v":0},null,{"$f":"IF(D_verOlie_AC,B_Verolie_cz_21,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_21, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_21,IF(ISNUMBER(B_VerOlie_DTU_czt_21),B_VerOlie_DTU_czt_21,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_21","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_21","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_21_gkk","v":0.1},{"$f":"IF(ISNUMBER(D_Verolie_Cz_21),IF(D_Verolie_Cz_21/P110>1,D_Verolie_Cz_21/P110,\"Nej\"),\"\")","v":""}]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_10","v":3.12},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},{"$f":"B_olie_kH_10","v":3.267666769230769E-2},{"$f":"D_Verolie_lambda","v":0},{"$f":"B_VerOlie_R_10","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_10,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_10, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_10,IF(ISNUMBER(B_VerOlie_DTU_czt_10),B_VerOlie_DTU_czt_10,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_10","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_10","v":{"$error":"#DIV/0!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_11","v":4.12},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},{"$f":"B_olie_kH_11","v":1.7893245806451612E-2},0,{"$f":"B_VerOlie_R_11","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_11,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_11, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_11,IF(ISNUMBER(B_VerOlie_DTU_czt_11),B_VerOlie_DTU_czt_11,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_11","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_11","v":{"$error":"#DIV/0!"}}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_12","v":4.38},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},{"$f":"B_olie_kH_12","v":3.4173988095238094E-3},0,{"$f":"B_VerOlie_R_12","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_12,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_12, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_12,IF(ISNUMBER(B_VerOlie_DTU_czt_12),B_VerOlie_DTU_czt_12,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_12","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_12","v":{"$error":"#DIV/0!"}}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_13","v":3.4},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},{"$f":"B_olie_kH_13","v":8.4009375000000007E-5},0,{"$f":"B_VerOlie_R_13","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_13,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_13, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_13,IF(ISNUMBER(B_VerOlie_DTU_czt_13),B_VerOlie_DTU_czt_13,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_13","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_13","v":{"$error":"#DIV/0!"}}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_14","v":2.36},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},{"$f":"B_olie_kH_14","v":9.2662208333333337E-6},0,{"$f":"B_VerOlie_R_14","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_14,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_14, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_14,IF(ISNUMBER(B_VerOlie_DTU_czt_14),B_VerOlie_DTU_czt_14,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_14","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_14","v":{"$error":"#DIV/0!"}}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_15","v":0.9},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},{"$f":"B_olie_kH_15","v":1.6859116944444445E-4},0,{"$f":"B_VerOlie_R_15","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_15,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_15, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_15,IF(ISNUMBER(B_VerOlie_DTU_czt_15),B_VerOlie_DTU_czt_15,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_15","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_15","v":{"$error":"#DIV/0!"}}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_16","v":1.77},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},{"$f":"B_olie_kH_16","v":0.11932},0,{"$f":"B_VerOlie_R_16","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_cz_16,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_16, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_czt_16,IF(ISNUMBER(B_VerOlie_DTU_czt_16),B_VerOlie_DTU_czt_16,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_16","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_16","v":{"$error":"#DIV/0!"}}]
[null,null,"sum af NSO",null,null,{"$f":"SUM(F113:F119)","v":{"$error":"#DIV/0!"}},null,null,null,0,null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_NSO,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_NSO, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_nso,IF(ISNUMBER(B_VerOlie_DTU_czt_NSO),B_VerOlie_DTU_czt_NSO,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_nso","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_nso","v":{"$error":"#DIV/0!"}}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cv","v":{"$error":"#DIV/0!"}},null,null,null,{"$f":"D_Verolie_lambda","v":0},null,{"$f":"IF(D_verOlie_AC,B_VerOlie_Cz_1,IF(D_verOlie_DTU1b,B_VerOlie_DTU_cz_1, \"ikke stationær\"))","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,B_VerOlie_Czt_1,IF(ISNUMBER(B_VerOlie_DTU_czt_1),B_VerOlie_DTU_czt_1,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_1","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_1","v":{"$error":"#DIV/0!"}},{"$f":"D_Olie_1_gkk","v":9},{"$f":"IF(ISNUMBER(D_Verolie_Cz_1),IF(D_Verolie_Cz_1/P122>1,D_Verolie_Cz_1/P122,\"Nej\"),\"\")","v":""}]
[]
[]
[]
[]
[null,"Kilde data:","D_VerOlie_Kil_Com"]
[null,null,false]
[null,"Jord data:","D_Verolie_Jord_Com"]
[null,null,false]
[null,"Beregning:","D_Verolie_ber_Com"]
[null,null,false]
[]
[]
[null,null,"SprækkeTransport - DTU-V1D-remtec"]
[]
[]
[null,null,"Model 1a og 1b og C"]
[]
[null,null,"Presence of fractures",null,"yes","For alle beregninger antages sprækker"]
[]
[null,null,"If initially contaminated (yes/no)",null,{"$f":"IF(D_verOlie_DTU2,\"yes\",\"no\")","v":"no"}]
[]
[]
[]
[null,null,"INPUT"]
[null,null,"BOX 1: General Input"]
[]
[null,null,"Input concentration",null,"stofafhængig","Se oven: Overført fra oliestoffer",null,null,"D_Olie_xx_cv"]
[null,null,"Matrix porosity","f",{"$f":"D_VerOlie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"D_Verolie_jord","v":0},null,null,"D_VerOlie_ntotal  ","input  fra jordparametre og defineret i dataark"]
[null,null,"Diffusion coefficient in matrix","Dm (m2/year)","stofafhængig","Se oven: beregnes for hver stofgruppe"]
[null,null,"Degradation rate","l (dag-1)",{"$f":"D_Verolie_lambda","v":0},"Bruger data - standard for alle stofgrupper",null,null,"D_VerOlie_lambda","input fra Vertikal transport-olie"]
[null,null,"Degradation rate","l (year-1)",{"$f":"B_Verolie_lambdayear","v":0},"Beregnet i beregningsark",null,null,"B_Ver_lambdayear","enhederne omregnes"]
[null,null,"Retardation, fracture","Rf","stofafhængig","Se oven:stof afhængig = Rm","jf. Chambon et al.J. of contaminant Hydrology 124 (2011),82-98",null,"D_VerOlie_R_xX","B_VerOlie_R_xx beregnes ovenover i Domenico for hver stofgruppe"]
[null,null,"Retardation, matrix","Rm","stofafhængig","Se oven: stof afhængig",null,null,"D_VerOlie_R_xx","B_VerOlie_R_xx beregnes ovenover i Domenico for hver stofgruppe"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_verOlie_2bapertur","v":7.9418567312567668E-5}]
[null,null,"Water velocity","vf (m/year)",{"$f":"B_verolie_Vvel","v":{"$error":"#VALUE!"}},null,null,null,"D_VerOlie_Vvel","Beregnes"]
[null,null,"Average velocity in EPM","vEPM (m/year)",{"$f":"B_verOlie_EPM","v":{"$error":"#VALUE!"}},null,null,null,"B_verOlie_EPM","Beregnes"]
[null,null,"Longitudinal dispersivity","α (m)",{"$f":"D_Verolie_alfaLw","v":9.9999999999999994E-37},null,null,null,"D_VerOlie_alfaLw","input"]
[null,null,"Spill time","a (year)",{"$f":"IF(D_verOlie_DTU2,\"Aftagende\",IF(VerOlie_a>0,VerOlie_a,\"Vedvarende\"))","v":"Vedvarende"},null,null,null,"Verolie_a","input"]
[]
[null,null,"BOX 2: Hydrogeological properties"]
[null,null,"calculated using from Box 3"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_verolie_2B","v":5}]
[null,null,"Fracture aperture","2*b (m)",{"$f":"B_verOlie_2bapertur","v":7.9418567312567668E-5},null,null,null,"B_verOlie_2bapertur","Beregnes"]
[null,null,"Bulk hydrualic conductivity","Kb (m/s)",{"$f":"D_verolie_Kb","v":6.2999999999999995E-8}]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_verolie_inf","v":""},null,null,null,"D_VerOlie_inf","input"]
[null,null,"Vertical gradient","i (-)",{"$f":"B_verOlie_Vgrad","v":{"$error":"#VALUE!"}},null,null,null,"B_VerOlie_Vgrad","Beregnes"]
[]
[null,null,"BOX 3: Specific Input depending on conceptual model",null,null,"Default/Ber./overført","Indtastet","Anvendt"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_verolie_2B","v":5},{"$f":"VerOlie_2B","v":5},{"$f":"VerOlie_My_2B","v":0},{"$f":"IF(VALUE(G171),G171,IF(F171<>0,F171,\"\"))","v":5},"D_VerOlie_2B","input"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_verOlie_2bapertur","v":7.9418567312567668E-5}]
[null,null,"Bulk hydraulic conductivity","Kb (m/s)",{"$f":"D_verolie_Kb","v":6.2999999999999995E-8},{"$f":"VerOlie_Kb","v":6.2999999999999995E-8},{"$f":"VerOlie_My_Kb","v":0},{"$f":"IF(VALUE(G173),G173,IF(F173<>0,F173,\"\"))","v":6.2999999999999995E-8},"D_VerOlie_Kb","Input"]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_Verolie_infiltration_temp","v":""},null,null,null,"D_verOlie_inf","input"]
[null,null,"Vertical gradient","i (-)",{"$f":"B_verOlie_Vgrad","v":{"$error":"#VALUE!"}}]
[]
[null,null,"BOX 4: Calculated Parameters-"]
[null,null,"A",null,"stofafhængig",null,null,null,null,"Beregnes"]
[null,null,"B ",null,"stofafhængig",null,null,null,null,"Beregnes"]
[null,null,"G",null,"stofafhængig",null,null,null,null,"Beregnes"]
[]
[null,null,"BOX 5: Calculation and graphic parameters"]
[null,null,"Time increment","(year)",null,"Udgør , da ingen figurer"]
[null,null,"Depth increment","(m)",null,"Udgør , da ingen figurer"]
[null,null,"Time plot",null,null,"Udgør , da ingen figurer"]
[null,null,"Time","t (year)",{"$f":"Verolie_t","v":0},null,null,null,"VerOlie_t","input"]
[null,null,"Depth","z(m)",{"$f":"Verolie_z","v":0},null,null,null,"VerOlie_z","input"]

{"sheet":"Beregning_Vertikal-Olie","index":56,"n_rows":167,"n_cols":30,"rows_kept":167,"cut":false,"hidden":true,"merged":[[125,8,125,13],[34,28,34,29],[33,28,33,29],[7,1,7,14],[9,2,9,9],[29,2,29,6],[29,7,29,9]]}
[]
[]
[null,"Vertikal transport igennem enten homogen vandmættet ler eller umættet ler og sand fra en overliggende kontinuert kilde","Domenico Model A + C",{"$f":"D_verOlie_AC","v":true}]
[null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kilde, hvor varigheden af spildet er kendt","DTU V1D Model 1a",{"$f":"D_verOlie_DTU1a","v":false}]
[null,"Vertikal transport igennem homogen vandmættet sprækket ler fra en overliggende kontinuert kilde","DTU V1D Model 1b",{"$f":"D_verOlie_DTU1b","v":false}]
[null,"Vertikal transport igennem homogen vandmættet sprækket ler fra den aftagende kilde i lermatrix","DTU V1D Model 2",{"$f":"D_verOlie_DTU2","v":false}]
[]
[null,"BEREGNINGSARK Vertikal transport - Oliestoffer (MODEL A+C, FINAL DOMENICO)"]
[]
[null,null,"Lokalitetsspecifikke data/umættet zone"]
[null,"Bemærkninger",null,"Forkortelse","Enhed","Oprindelsessted","Note","Default/Beregnet","Indtastet","Anvendt"]
[null,null,"Jordtype",null,null,null,null,{"$f":"D_VerOlie_jord_syst","v":0},{"$f":"Ver_My_jord","v":0},{"$f":"D_Verolie_jord","v":0}]
[null,null,"Porevandshastighed","Vw","m/dag","beregnes",null,{"$f":"D_Verolie_infiltration/(D_VerOlie_thetaw)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I13),I13,IF(H13<>0,H13,\"\"))","v":{"$error":"#VALUE!"}},null,"B_Verolie_Vw"]
[null,null,"Vandindhold","qw","-","input",null,{"$f":"D_VerOlie_thetaw_syst","v":0},{"$f":"Verolie_My_VV","v":0},{"$f":"D_VerOlie_thetaw","v":""},null,"B_Verolie_thetaw"]
[null,null,"Luftindhold","qa","-","input",null,{"$f":"D_VerOlie_thetaa_syst","v":0},{"$f":"Ver_My_VL","v":0},{"$f":"D_VerOlie_thetaa","v":0},null,"B_Verolie_thetaa"]
[null,null,"Total porøsitet (VL+VV)","n","-","Beregnes ",null,{"$f":"SUM(B_verolie_thetaw+B_verolie_thetaa)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I16),I16,IF(H16<>0,H16,\"\"))","v":{"$error":"#VALUE!"}},null,"B_Verolie_ntotal"]
[null,null,"Volumen af jordskellet","Vj",null,"Beregnes",null,{"$f":"1-B_verolie_ntotal","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I17),I17,IF(H17<>0,H17,\"\"))","v":{"$error":"#VALUE!"}},null,"D_Verolie_volj"]
[null,null,"% Indhold organisk kulstof","foc (%)","-","input",null,{"$f":"D_VerOlie_foc_syst","v":0},{"$f":"Verolie_My_foc","v":0},{"$f":"IF(VALUE(I18),I18,IF(H18<>0,H18,\"\"))","v":""}]
[null,null,"Fraktion organisk indhold","foc",null,"Enhed konverteres",null,null,null,{"$f":"J18/100","v":{"$error":"#VALUE!"}},null,"B_Verolie_foc"]
[null,null,"Korn rumvægt","d","kg/l","input",null,{"$f":"D_VerOlie_d_syst","v":0},{"$f":"Verolie_My_d","v":0},{"$f":"IF(VALUE(I20),I20,IF(H20<>0,H20,\"\"))","v":""},null,"B_Verolie_d"]
[null,null,"Bulkmassefylde= volumenvægt","(rho)r","kg/l","Beregnet",null,{"$f":"(B_verolie_d*B_verolie_volj)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I21),I21,IF(H21<>0,H21,\"\"))","v":{"$error":"#VALUE!"}},null,"B_Verolie_rhob"]
[null,null,"Nettoinfiltration= nettonedbør","N","m/dag","Beregnes",null,{"$f":"(D_Verolie_infiltration_temp)/(1000*365)","v":{"$error":"#VALUE!"}},null,{"$f":"IF(VALUE(I22),I22,IF(H22<>0,H22,\"\"))","v":{"$error":"#VALUE!"}},null,"B_Verolie_infiltration"]
[null,null,"Kildens længde","Y","m","input",null,null,{"$f":"Verolie_Y","v":0},{"$f":"I23","v":0},null,"D_Verolie_Y"]
[null,null,"Kildens bredde","X","m","input",null,null,{"$f":"Verolie_X","v":0},{"$f":"I24","v":0},null,"D_Verolie_X"]
[null,null,"Afstand fra kildens underkant til GV-spejl","Z","m","input",null,null,{"$f":"Verolie_z","v":0},{"$f":"I25","v":0},null,"D_Verolie_Z"]
[null,null,"Long. dispersivitet (vand)","(alfa)L,w","m","Bergenes",null,{"$f":"(0.0000042*(POWER(D_Verolie_z,2))+(0.0036*D_Verolie_z)-0.008)","v":-8.0000000000000002E-3},null,{"$f":"IF(H26<0,1E-36,H26)","v":9.9999999999999994E-37},null,"B_Verolie_alfaLw"]
[null,null,"Trans. dispersivitet (vand)","(alfa)T,w","m","beregnes",null,{"$f":"B_verolie_alfaLw*0.1","v":1.0000000000000001E-37},null,{"$f":"IF(H27<0,1E-36,H27)","v":1.0000000000000001E-37},null,"B_Verolie_alfaTw"]
[null,null,"Transient løsning, tid","t","dage","beregnes",null,{"$f":"Verolie_t*365","v":0},null,{"$f":"IF(H28<0,1E-36,H28)","v":0},null,"B_Verolie_t"]
[]
[null,null,null,null,null,null,null,"Fælles for alle oliestoffer"]
[null,null,null,"Forkortelse","Enhed","Oprindelsessted","Note","Default/Ber./overført","Indtastet","Anvendt"]
[null,null,"Anvendt nedbrydningskonstant","(lambda)_n","dag^-1","Beregnes","fælles for alle oliestoffer",{"$f":"Verolie_ned","v":0},{"$f":"Verolie_My_ned","v":0},{"$f":"D_Verolie_lambda","v":0},null,"B_Verolie_lambda"]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(VALUE(I33),I33,IF(H33<>0,H33,\"\"))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DTU V1D","Anvendt model",null,null,{"$f":"IF(D_verOlie_AC,\"DTU V1D ikke valgt\",D_Verolie_model)","v":"DTU V1D ikke valgt"},null,null,null,"Flux beregning for valgt model"]
[null,null,null,null,null,"Cv","Log Kow","DL","Da",null,"Dw","kH","Dz","R","u","Argz\nRqw+KHqa ","Cz","Cz, t",null,null,"Diffusionskøefficient i matrix","A","B ","G","Cz","Cz, t","T´","T``",{"$f":"D_Verolie_model","v":"Model A + C"}]
[null,null,null,null,null,"Overført fra Oliestoffer","Overført fra Oliestoffer","Overført fra Oliestoffer","Beregnes","Beregnes","Beregnes","Overført fra Oliestoffer","Beregnes","Beregnes","Beregnes","Beregnes","Beregnes","Beregnes","Beregnes","Beregnes",null,null,null,null,"Beregnes","Beregnes",null,null,"Beregnes","Beregnes"]
[null,null,null,null,null,"Beregnet kildekonc Cv","Log Kow","Diffusionskoefficient (luft)","Effektiv diffusions\nkoefficient (luft)","Diffusions\nkoefficient (vand)","Effektiv diffusionskoefficient (vand)","Henry","Hydrodynamisk long. disp (vand)","Retardation","Hjælpe\nkonstanter","Hjælpe\nkonstanter","Stationær konc ved z","Transient konc ved t","Flux (stationært)","Flux, transient (t) i toppen ag GV magasin",null,null,null,null,"Stationær konc ved z","Transient konc ved t","Ligning rettet da R er meget højt for flere stoffer og der kan ikke laves SQRT af en negativ nr. \nDefalt er sat til en meget lav værdi på 1*e-25, såfremt R er højt.",null,"Flux (stationært)","Flux, transient (t) i toppen ag GV magasin"]
[null,null,null,null,null,"µg/L",null,"m²/s","m²/dage","m²/s","m²/dage","Kpa.m³/mol","m²/dage",null,null,null,"µg/l","µg/l","mg/år","mg/år","m/year",null,null,null,"µg/l","µg/l",null,null,"mg/år","mg/år"]
[50,"C5-C6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q41:Q43)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R40:R43)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S40:S43)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T40:T43)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y41:Y43)","v":0},{"$f":"SUM(Z40:Z43)","v":0},null,null,{"$f":"SUM(AC40:AC43)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD40:AD43)","v":{"$error":"#DIV/0!"}}]
[51,">5 - 6, alifater","2-methylbutan",null,null,{"$f":"D_Olie_51_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_51","v":2.72},{"$f":"B_olie_DL_51","v":8.7395009776804372E-6},{"$f":"H40*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H40/10000","v":8.7395009776804368E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J40*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_51","v":141.86000000000001},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I40*((L40*1000)/(8.314*298))+K40*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G40-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M40/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N40*B_verolie_thetaw+B_verolie_thetaa*((L40*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F40*EXP((B_Verolie_Vw-O40)*B_verolie_z/(2*M40))","v":{"$error":"#DIV/0!"}},{"$f":"F40/2*(EXP((B_Verolie_Vw-O40)*B_verolie_z/(2*M40))*(1-fejlfunkk((B_verolie_z*P40-O40*B_Verolie_t)/(2*SQRT(M40*P40*B_Verolie_t))))+EXP((B_Verolie_Vw+O40)*B_verolie_z/(2*M40))*(1-fejlfunkk((B_verolie_z*P40+O40*B_Verolie_t)/(2*SQRT(M40*P40*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q40*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J40*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N40/(D_VerOlie_ntotal*SQRT(N40*U40))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N40)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(N40/U40)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F40*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N40*Verolie_z/D_verOlie_Vvel*W40/V40)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F40*(EXP(-D_VerOlie_lambdayear*Verolie_t/N40)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA40^2/N40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AA40)*SQRT(2))))),(IF(AND(AA40>0,AB40=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N40*Verolie_z/D_verOlie_Vvel*W40/V40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AA40)-W40*AA40)*SQRT(2))+EXP(N40*Verolie_z/D_verOlie_Vvel*W40/V40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AA40)+W40*AA40)*SQRT(2)))*F40,IF(AB40>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N40*Verolie_z/D_verOlie_Vvel*W40/V40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AA40)-W40*AA40)*SQRT(2))+EXP(N40*Verolie_z/D_verOlie_Vvel*W40/V40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AA40)+W40*AA40)*SQRT(2)))-(EXP(-N40*Verolie_z/D_verOlie_Vvel*W40/V40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AB40)-W40*AB40)*SQRT(2))+EXP(N40*Verolie_z/D_verOlie_Vvel*W40/V40)*2*NORMSDIST(-(N40*Verolie_z/D_verOlie_Vvel/(2*V40*AB40)+W40*AB40)*SQRT(2))))*F40)))))","v":0},{"$f":"IF(Verolie_t-N40/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N40/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N40/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N40/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q40*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y40*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R40*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z40*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[511,null,"Pentan",null,null,{"$f":"D_Olie_511_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_511","v":3.39},{"$f":"B_olie_DL_511","v":9.6725251295755997E-6},{"$f":"H41*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H41/10000","v":9.6725251295756004E-10},{"$error":"#VALUE!"},{"$f":"B_olie_kH_511","v":126.66},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I41*((L41*1000)/(8.314*298))+K41*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G41-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M41/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N41*B_verolie_thetaw+B_verolie_thetaa*((L41*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F41*EXP((B_Verolie_Vw-O41)*B_verolie_z/(2*M41))","v":{"$error":"#DIV/0!"}},{"$f":"F41/2*(EXP((B_Verolie_Vw-O41)*B_verolie_z/(2*M41))*(1-fejlfunkk((B_verolie_z*P41-O41*B_Verolie_t)/(2*SQRT(M41*P41*B_Verolie_t))))+EXP((B_Verolie_Vw+O41)*B_verolie_z/(2*M41))*(1-fejlfunkk((B_verolie_z*P41+O41*B_Verolie_t)/(2*SQRT(M41*P41*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J41*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N41/(D_VerOlie_ntotal*SQRT(N41*U41))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N41)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(N41/U41)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F41*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N41*Verolie_z/D_verOlie_Vvel*W41/V41)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F41*(EXP(-D_VerOlie_lambdayear*Verolie_t/N41)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA41^2/N41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AA41)*SQRT(2))))),(IF(AND(AA41>0,AB41=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N41*Verolie_z/D_verOlie_Vvel*W41/V41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AA41)-W41*AA41)*SQRT(2))+EXP(N41*Verolie_z/D_verOlie_Vvel*W41/V41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AA41)+W41*AA41)*SQRT(2)))*F41,IF(AB41>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N41*Verolie_z/D_verOlie_Vvel*W41/V41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AA41)-W41*AA41)*SQRT(2))+EXP(N41*Verolie_z/D_verOlie_Vvel*W41/V41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AA41)+W41*AA41)*SQRT(2)))-(EXP(-N41*Verolie_z/D_verOlie_Vvel*W41/V41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AB41)-W41*AB41)*SQRT(2))+EXP(N41*Verolie_z/D_verOlie_Vvel*W41/V41)*2*NORMSDIST(-(N41*Verolie_z/D_verOlie_Vvel/(2*V41*AB41)+W41*AB41)*SQRT(2))))*F41)))))","v":0},{"$f":"IF(Verolie_t-N41/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N41/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N41/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N41/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q41*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y41*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R41*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z41*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[512,null,"2-methylpentan",null,null,{"$f":"D_Olie_512_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_512","v":3.21},{"$f":"B_olie_DL_512","v":7.996529764863221E-6},{"$f":"H42*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},7.9965297648632211E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_512","v":173.27},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I42*((L42*1000)/(8.314*298))+K42*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G42-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M42/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N42*B_verolie_thetaw+B_verolie_thetaa*((L42*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F42*EXP((B_Verolie_Vw-O42)*B_verolie_z/(2*M42))","v":{"$error":"#DIV/0!"}},{"$f":"F42/2*(EXP((B_Verolie_Vw-O42)*B_verolie_z/(2*M42))*(1-fejlfunkk((B_verolie_z*P42-O42*B_Verolie_t)/(2*SQRT(M42*P42*B_Verolie_t))))+EXP((B_Verolie_Vw+O42)*B_verolie_z/(2*M42))*(1-fejlfunkk((B_verolie_z*P42+O42*B_Verolie_t)/(2*SQRT(M42*P42*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J42*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N42/(D_VerOlie_ntotal*SQRT(N42*U42))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N42)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F42*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N42*Verolie_z/D_verOlie_Vvel*W42/V42)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F42*(EXP(-D_VerOlie_lambdayear*Verolie_t/N42)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA42^2/N42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AA42)*SQRT(2))))),(IF(AND(AA42>0,AB42=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N42*Verolie_z/D_verOlie_Vvel*W42/V42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AA42)-W42*AA42)*SQRT(2))+EXP(N42*Verolie_z/D_verOlie_Vvel*W42/V42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AA42)+W42*AA42)*SQRT(2)))*F42,IF(AB42>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N42*Verolie_z/D_verOlie_Vvel*W42/V42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AA42)-W42*AA42)*SQRT(2))+EXP(N42*Verolie_z/D_verOlie_Vvel*W42/V42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AA42)+W42*AA42)*SQRT(2)))-(EXP(-N42*Verolie_z/D_verOlie_Vvel*W42/V42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AB42)-W42*AB42)*SQRT(2))+EXP(N42*Verolie_z/D_verOlie_Vvel*W42/V42)*2*NORMSDIST(-(N42*Verolie_z/D_verOlie_Vvel/(2*V42*AB42)+W42*AB42)*SQRT(2))))*F42)))))","v":0},{"$f":"IF(Verolie_t-N42/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N42/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N42/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N42/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q42*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y42*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R42*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z42*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[513,null,"3-methylpentan (C6)",null,null,{"$f":"D_Olie_513_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_513","v":3.6},{"$f":"B_olie_DL_513","v":7.996529764863221E-6},{"$f":"H43*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},7.9965297648632211E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_513","v":170.226},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I43*((L43*1000)/(8.314*298))+K43*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G43-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M43/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N43*B_verolie_thetaw+B_verolie_thetaa*((L43*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F43*EXP((B_Verolie_Vw-O43)*B_verolie_z/(2*M43))","v":{"$error":"#DIV/0!"}},{"$f":"F43/2*(EXP((B_Verolie_Vw-O43)*B_verolie_z/(2*M43))*(1-fejlfunkk((B_verolie_z*P43-O43*B_Verolie_t)/(2*SQRT(M43*P43*B_Verolie_t))))+EXP((B_Verolie_Vw+O43)*B_verolie_z/(2*M43))*(1-fejlfunkk((B_verolie_z*P43+O43*B_Verolie_t)/(2*SQRT(M43*P43*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J43*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N43/(D_VerOlie_ntotal*SQRT(N43*U43))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N43)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F43*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N43*Verolie_z/D_verOlie_Vvel*W43/V43)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F43*(EXP(-D_VerOlie_lambdayear*Verolie_t/N43)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA43^2/N43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AA43)*SQRT(2))))),(IF(AND(AA43>0,AB43=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N43*Verolie_z/D_verOlie_Vvel*W43/V43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AA43)-W43*AA43)*SQRT(2))+EXP(N43*Verolie_z/D_verOlie_Vvel*W43/V43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AA43)+W43*AA43)*SQRT(2)))*F43,IF(AB43>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N43*Verolie_z/D_verOlie_Vvel*W43/V43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AA43)-W43*AA43)*SQRT(2))+EXP(N43*Verolie_z/D_verOlie_Vvel*W43/V43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AA43)+W43*AA43)*SQRT(2)))-(EXP(-N43*Verolie_z/D_verOlie_Vvel*W43/V43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AB43)-W43*AB43)*SQRT(2))+EXP(N43*Verolie_z/D_verOlie_Vvel*W43/V43)*2*NORMSDIST(-(N43*Verolie_z/D_verOlie_Vvel/(2*V43*AB43)+W43*AB43)*SQRT(2))))*F43)))))","v":0},{"$f":"IF(Verolie_t-N43/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N43/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N43/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N43/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q43*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y43*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R43*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z43*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[]
[510,"C6-C10",null,null,null,{"$f":"D_Olie_510_cv","v":{"$error":"#DIV/0!"}},null,null,null,0,{"$error":"#VALUE!"},null,null,null,null,null,{"$f":"SUM(Q46:Q56)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R46:R56)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S46:S56)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T46:T56)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y46:Y56)","v":0},{"$f":"SUM(Z46:Z56)","v":0},null,null,{"$f":"SUM(AC46:AC56)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD46:AD56)","v":{"$error":"#DIV/0!"}}]
[52,">5 - 7, aromater","Benzen (C6) (>5-7, aromater)",null,null,{"$f":"D_Olie_52_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_52","v":2.13},{"$f":"B_olie_DL_52","v":9.3000000000000007E-6},{"$f":"H46*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},9.300000000000001E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_52","v":0.56240000000000001},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I46*((L46*1000)/(8.314*298))+K46*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G46-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M46/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N46*B_verolie_thetaw+B_verolie_thetaa*((L46*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F46*EXP((B_Verolie_Vw-O46)*B_verolie_z/(2*M46))","v":{"$error":"#DIV/0!"}},{"$f":"F46/2*(EXP((B_Verolie_Vw-O46)*B_verolie_z/(2*M46))*(1-fejlfunkk((B_verolie_z*P46-O46*B_Verolie_t)/(2*SQRT(M46*P46*B_Verolie_t))))+EXP((B_Verolie_Vw+O46)*B_verolie_z/(2*M46))*(1-fejlfunkk((B_verolie_z*P46+O46*B_Verolie_t)/(2*SQRT(M46*P46*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q46*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J46*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N46/(D_VerOlie_ntotal*SQRT(N46*U46))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N46)","v":{"$error":"#VALUE!"}},{"$f":"SQRT(N46/U46)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F46*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N46*Verolie_z/D_verOlie_Vvel*W46/V46)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F46*(EXP(-D_VerOlie_lambdayear*Verolie_t/N46)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA46^2/N46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AA46)*SQRT(2))))),(IF(AND(AA46>0,AB46=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N46*Verolie_z/D_verOlie_Vvel*W46/V46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AA46)-W46*AA46)*SQRT(2))+EXP(N46*Verolie_z/D_verOlie_Vvel*W46/V46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AA46)+W46*AA46)*SQRT(2)))*F46,IF(AB46>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N46*Verolie_z/D_verOlie_Vvel*W46/V46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AA46)-W46*AA46)*SQRT(2))+EXP(N46*Verolie_z/D_verOlie_Vvel*W46/V46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AA46)+W46*AA46)*SQRT(2)))-(EXP(-N46*Verolie_z/D_verOlie_Vvel*W46/V46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AB46)-W46*AB46)*SQRT(2))+EXP(N46*Verolie_z/D_verOlie_Vvel*W46/V46)*2*NORMSDIST(-(N46*Verolie_z/D_verOlie_Vvel/(2*V46*AB46)+W46*AB46)*SQRT(2))))*F46)))))","v":0},{"$f":"IF(Verolie_t-N46/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N46/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N46/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N46/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q46*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y46*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R46*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z46*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[53,">6 - 8, alifater",">6 - 8, alifater",null,null,{"$f":"D_Olie_53_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_53","v":4.29},{"$f":"B_olie_DL_53","v":7.1005946686005421E-6},{"$f":"H47*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},7.1005946686005418E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_53","v":308.16000000000003},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I47*((L47*1000)/(8.314*298))+K47*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G47-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M47/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N47*B_verolie_thetaw+B_verolie_thetaa*((L47*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F47*EXP((B_Verolie_Vw-O47)*B_verolie_z/(2*M47))","v":{"$error":"#DIV/0!"}},{"$f":"F47/2*(EXP((B_Verolie_Vw-O47)*B_verolie_z/(2*M47))*(1-fejlfunkk((B_verolie_z*P47-O47*B_Verolie_t)/(2*SQRT(M47*P47*B_Verolie_t))))+EXP((B_Verolie_Vw+O47)*B_verolie_z/(2*M47))*(1-fejlfunkk((B_verolie_z*P47+O47*B_Verolie_t)/(2*SQRT(M47*P47*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J47*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N47/(D_VerOlie_ntotal*SQRT(N47*U47))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N47)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F47*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N47*Verolie_z/D_verOlie_Vvel*W47/V47)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F47*(EXP(-D_VerOlie_lambdayear*Verolie_t/N47)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA47^2/N47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AA47)*SQRT(2))))),(IF(AND(AA47>0,AB47=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N47*Verolie_z/D_verOlie_Vvel*W47/V47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AA47)-W47*AA47)*SQRT(2))+EXP(N47*Verolie_z/D_verOlie_Vvel*W47/V47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AA47)+W47*AA47)*SQRT(2)))*F47,IF(AB47>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N47*Verolie_z/D_verOlie_Vvel*W47/V47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AA47)-W47*AA47)*SQRT(2))+EXP(N47*Verolie_z/D_verOlie_Vvel*W47/V47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AA47)+W47*AA47)*SQRT(2)))-(EXP(-N47*Verolie_z/D_verOlie_Vvel*W47/V47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AB47)-W47*AB47)*SQRT(2))+EXP(N47*Verolie_z/D_verOlie_Vvel*W47/V47)*2*NORMSDIST(-(N47*Verolie_z/D_verOlie_Vvel/(2*V47*AB47)+W47*AB47)*SQRT(2))))*F47)))))","v":0},{"$f":"IF(Verolie_t-N47/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N47/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N47/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N47/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q47*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y47*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R47*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z47*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[54,">7 - 8, aromater","Toluen (C7)(>7-8, aromater",null,null,{"$f":"D_Olie_54_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_54","v":2.73},{"$f":"B_olie_DL_54","v":8.5640392765120893E-6},{"$f":"H48*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},8.5640392765120896E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_54","v":0.67379999999999995},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I48*((L48*1000)/(8.314*298))+K48*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G48-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M48/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N48*B_verolie_thetaw+B_verolie_thetaa*((L48*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F48*EXP((B_Verolie_Vw-O48)*B_verolie_z/(2*M48))","v":{"$error":"#DIV/0!"}},{"$f":"F48/2*(EXP((B_Verolie_Vw-O48)*B_verolie_z/(2*M48))*(1-fejlfunkk((B_verolie_z*P48-O48*B_Verolie_t)/(2*SQRT(M48*P48*B_Verolie_t))))+EXP((B_Verolie_Vw+O48)*B_verolie_z/(2*M48))*(1-fejlfunkk((B_verolie_z*P48+O48*B_Verolie_t)/(2*SQRT(M48*P48*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J48*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N48/(D_VerOlie_ntotal*SQRT(N48*U48))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N48)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F48*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N48*Verolie_z/D_verOlie_Vvel*W48/V48)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F48*(EXP(-D_VerOlie_lambdayear*Verolie_t/N48)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA48^2/N48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AA48)*SQRT(2))))),(IF(AND(AA48>0,AB48=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N48*Verolie_z/D_verOlie_Vvel*W48/V48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AA48)-W48*AA48)*SQRT(2))+EXP(N48*Verolie_z/D_verOlie_Vvel*W48/V48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AA48)+W48*AA48)*SQRT(2)))*F48,IF(AB48>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N48*Verolie_z/D_verOlie_Vvel*W48/V48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AA48)-W48*AA48)*SQRT(2))+EXP(N48*Verolie_z/D_verOlie_Vvel*W48/V48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AA48)+W48*AA48)*SQRT(2)))-(EXP(-N48*Verolie_z/D_verOlie_Vvel*W48/V48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AB48)-W48*AB48)*SQRT(2))+EXP(N48*Verolie_z/D_verOlie_Vvel*W48/V48)*2*NORMSDIST(-(N48*Verolie_z/D_verOlie_Vvel/(2*V48*AB48)+W48*AB48)*SQRT(2))))*F48)))))","v":0},{"$f":"IF(Verolie_t-N48/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N48/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N48/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N48/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q48*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y48*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R48*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z48*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[55,">8 - 10, alifater",">8 - 10, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_55B_cv,D_Olie_55A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_55b,B_olie_kow_55a)","v":5.15},{"$f":"IF(D_Olie_profil=1,B_olie_DL_55B,B_olie_DL_55A)","v":6.2232552378840063E-6},{"$f":"H49*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},6.2232552378840062E-10,{"$error":"#VALUE!"},{"$f":"IF(D_Olie_profil=1,B_olie_kH_55b,B_olie_kH_55a)","v":534.27},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I49*((L49*1000)/(8.314*298))+K49*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G49-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M49/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N49*B_verolie_thetaw+B_verolie_thetaa*((L49*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F49*EXP((B_Verolie_Vw-O49)*B_verolie_z/(2*M49))","v":{"$error":"#DIV/0!"}},{"$f":"F49/2*(EXP((B_Verolie_Vw-O49)*B_verolie_z/(2*M49))*(1-fejlfunkk((B_verolie_z*P49-O49*B_Verolie_t)/(2*SQRT(M49*P49*B_Verolie_t))))+EXP((B_Verolie_Vw+O49)*B_verolie_z/(2*M49))*(1-fejlfunkk((B_verolie_z*P49+O49*B_Verolie_t)/(2*SQRT(M49*P49*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J49*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N49/(D_VerOlie_ntotal*SQRT(N49*U49))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N49)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F49*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N49*Verolie_z/D_verOlie_Vvel*W49/V49)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F49*(EXP(-D_VerOlie_lambdayear*Verolie_t/N49)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA49^2/N49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AA49)*SQRT(2))))),(IF(AND(AA49>0,AB49=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N49*Verolie_z/D_verOlie_Vvel*W49/V49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AA49)-W49*AA49)*SQRT(2))+EXP(N49*Verolie_z/D_verOlie_Vvel*W49/V49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AA49)+W49*AA49)*SQRT(2)))*F49,IF(AB49>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N49*Verolie_z/D_verOlie_Vvel*W49/V49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AA49)-W49*AA49)*SQRT(2))+EXP(N49*Verolie_z/D_verOlie_Vvel*W49/V49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AA49)+W49*AA49)*SQRT(2)))-(EXP(-N49*Verolie_z/D_verOlie_Vvel*W49/V49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AB49)-W49*AB49)*SQRT(2))+EXP(N49*Verolie_z/D_verOlie_Vvel*W49/V49)*2*NORMSDIST(-(N49*Verolie_z/D_verOlie_Vvel/(2*V49*AB49)+W49*AB49)*SQRT(2))))*F49)))))","v":0},{"$f":"IF(Verolie_t-N49/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N49/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N49/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N49/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q49*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y49*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R49*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z49*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[56,">8 -10, aromater","Sum >8-10, aromater"]
[571,null,"o-Xylen"]
[572,null,"m+p-Xylen"]
[57,null,"Sum Xylener regnes som m-Xylen (C8)",null,null,{"$f":"D_Olie_57_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_57","v":3.2},{"$f":"B_olie_DL_57","v":7.9752849160092975E-6},{"$f":"H53*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H53/10000","v":7.9752849160092973E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J53*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_57","v":0.72750000000000004},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I53*((L53*1000)/(8.314*298))+K53*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G53-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M53/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N53*B_verolie_thetaw+B_verolie_thetaa*((L53*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F53*EXP((B_Verolie_Vw-O53)*B_verolie_z/(2*M53))","v":{"$error":"#DIV/0!"}},{"$f":"F53/2*(EXP((B_Verolie_Vw-O53)*B_verolie_z/(2*M53))*(1-fejlfunkk((B_verolie_z*P53-O53*B_Verolie_t)/(2*SQRT(M53*P53*B_Verolie_t))))+EXP((B_Verolie_Vw+O53)*B_verolie_z/(2*M53))*(1-fejlfunkk((B_verolie_z*P53+O53*B_Verolie_t)/(2*SQRT(M53*P53*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q53*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J53*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N53/(D_VerOlie_ntotal*SQRT(N53*U53))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N53)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F53*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N53*Verolie_z/D_verOlie_Vvel*W53/V53)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F53*(EXP(-D_VerOlie_lambdayear*Verolie_t/N53)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA53^2/N53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AA53)*SQRT(2))))),(IF(AND(AA53>0,AB53=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N53*Verolie_z/D_verOlie_Vvel*W53/V53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AA53)-W53*AA53)*SQRT(2))+EXP(N53*Verolie_z/D_verOlie_Vvel*W53/V53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AA53)+W53*AA53)*SQRT(2)))*F53,IF(AB53>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N53*Verolie_z/D_verOlie_Vvel*W53/V53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AA53)-W53*AA53)*SQRT(2))+EXP(N53*Verolie_z/D_verOlie_Vvel*W53/V53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AA53)+W53*AA53)*SQRT(2)))-(EXP(-N53*Verolie_z/D_verOlie_Vvel*W53/V53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AB53)-W53*AB53)*SQRT(2))+EXP(N53*Verolie_z/D_verOlie_Vvel*W53/V53)*2*NORMSDIST(-(N53*Verolie_z/D_verOlie_Vvel/(2*V53*AB53)+W53*AB53)*SQRT(2))))*F53)))))","v":0},{"$f":"IF(Verolie_t-N53/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N53/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N53/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N53/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q53*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y53*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R53*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z53*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[58,null,"Ethylbenzen (C8)",null,null,{"$f":"D_Olie_58_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_58","v":3.15},{"$f":"B_olie_DL_58","v":7.9752849160092975E-6},{"$f":"H54*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H54/10000","v":7.9752849160092973E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J54*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_58","v":0.7984},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I54*((L54*1000)/(8.314*298))+K54*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G54-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M54/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N54*B_verolie_thetaw+B_verolie_thetaa*((L54*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F54*EXP((B_Verolie_Vw-O54)*B_verolie_z/(2*M54))","v":{"$error":"#DIV/0!"}},{"$f":"F54/2*(EXP((B_Verolie_Vw-O54)*B_verolie_z/(2*M54))*(1-fejlfunkk((B_verolie_z*P54-O54*B_Verolie_t)/(2*SQRT(M54*P54*B_Verolie_t))))+EXP((B_Verolie_Vw+O54)*B_verolie_z/(2*M54))*(1-fejlfunkk((B_verolie_z*P54+O54*B_Verolie_t)/(2*SQRT(M54*P54*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J54*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N54/(D_VerOlie_ntotal*SQRT(N54*U54))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N54)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F54*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N54*Verolie_z/D_verOlie_Vvel*W54/V54)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F54*(EXP(-D_VerOlie_lambdayear*Verolie_t/N54)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA54^2/N54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AA54)*SQRT(2))))),(IF(AND(AA54>0,AB54=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N54*Verolie_z/D_verOlie_Vvel*W54/V54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AA54)-W54*AA54)*SQRT(2))+EXP(N54*Verolie_z/D_verOlie_Vvel*W54/V54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AA54)+W54*AA54)*SQRT(2)))*F54,IF(AB54>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N54*Verolie_z/D_verOlie_Vvel*W54/V54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AA54)-W54*AA54)*SQRT(2))+EXP(N54*Verolie_z/D_verOlie_Vvel*W54/V54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AA54)+W54*AA54)*SQRT(2)))-(EXP(-N54*Verolie_z/D_verOlie_Vvel*W54/V54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AB54)-W54*AB54)*SQRT(2))+EXP(N54*Verolie_z/D_verOlie_Vvel*W54/V54)*2*NORMSDIST(-(N54*Verolie_z/D_verOlie_Vvel/(2*V54*AB54)+W54*AB54)*SQRT(2))))*F54)))))","v":0},{"$f":"IF(Verolie_t-N54/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N54/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N54/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N54/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q54*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y54*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R54*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z54*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[59,null,"1,3,5-trimethylbenzen (C9)",null,null,{"$f":"D_Olie_59_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"H55*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H55/10000","v":7.4964600630922754E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J55*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_59","v":0.89},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I55*((L55*1000)/(8.314*298))+K55*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G55-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M55/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N55*B_verolie_thetaw+B_verolie_thetaa*((L55*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F55*EXP((B_Verolie_Vw-O55)*B_verolie_z/(2*M55))","v":{"$error":"#DIV/0!"}},{"$f":"F55/2*(EXP((B_Verolie_Vw-O55)*B_verolie_z/(2*M55))*(1-fejlfunkk((B_verolie_z*P55-O55*B_Verolie_t)/(2*SQRT(M55*P55*B_Verolie_t))))+EXP((B_Verolie_Vw+O55)*B_verolie_z/(2*M55))*(1-fejlfunkk((B_verolie_z*P55+O55*B_Verolie_t)/(2*SQRT(M55*P55*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J55*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N55/(D_VerOlie_ntotal*SQRT(N55*U55))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N55)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F55*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N55*Verolie_z/D_verOlie_Vvel*W55/V55)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F55*(EXP(-D_VerOlie_lambdayear*Verolie_t/N55)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA55^2/N55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AA55)*SQRT(2))))),(IF(AND(AA55>0,AB55=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N55*Verolie_z/D_verOlie_Vvel*W55/V55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AA55)-W55*AA55)*SQRT(2))+EXP(N55*Verolie_z/D_verOlie_Vvel*W55/V55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AA55)+W55*AA55)*SQRT(2)))*F55,IF(AB55>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N55*Verolie_z/D_verOlie_Vvel*W55/V55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AA55)-W55*AA55)*SQRT(2))+EXP(N55*Verolie_z/D_verOlie_Vvel*W55/V55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AA55)+W55*AA55)*SQRT(2)))-(EXP(-N55*Verolie_z/D_verOlie_Vvel*W55/V55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AB55)-W55*AB55)*SQRT(2))+EXP(N55*Verolie_z/D_verOlie_Vvel*W55/V55)*2*NORMSDIST(-(N55*Verolie_z/D_verOlie_Vvel/(2*V55*AB55)+W55*AB55)*SQRT(2))))*F55)))))","v":0},{"$f":"IF(Verolie_t-N55/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N55/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N55/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N55/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q55*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y55*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R55*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z55*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[60,null,">8 -10, aromater,øvrige",null,null,{"$f":"D_olie_60_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"H56*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H56/10000","v":7.4964600630922754E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J56*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_59","v":0.89},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I56*((L56*1000)/(8.314*298))+K56*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G56-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M56/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N56*B_verolie_thetaw+B_verolie_thetaa*((L56*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F56*EXP((B_Verolie_Vw-O56)*B_verolie_z/(2*M56))","v":{"$error":"#DIV/0!"}},{"$f":"F56/2*(EXP((B_Verolie_Vw-O56)*B_verolie_z/(2*M56))*(1-fejlfunkk((B_verolie_z*P56-O56*B_Verolie_t)/(2*SQRT(M56*P56*B_Verolie_t))))+EXP((B_Verolie_Vw+O56)*B_verolie_z/(2*M56))*(1-fejlfunkk((B_verolie_z*P56+O56*B_Verolie_t)/(2*SQRT(M56*P56*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J56*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N56/(D_VerOlie_ntotal*SQRT(N56*U56))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N56)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F56*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N56*Verolie_z/D_verOlie_Vvel*W56/V56)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F56*(EXP(-D_VerOlie_lambdayear*Verolie_t/N56)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA56^2/N56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AA56)*SQRT(2))))),(IF(AND(AA56>0,AB56=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N56*Verolie_z/D_verOlie_Vvel*W56/V56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AA56)-W56*AA56)*SQRT(2))+EXP(N56*Verolie_z/D_verOlie_Vvel*W56/V56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AA56)+W56*AA56)*SQRT(2)))*F56,IF(AB56>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N56*Verolie_z/D_verOlie_Vvel*W56/V56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AA56)-W56*AA56)*SQRT(2))+EXP(N56*Verolie_z/D_verOlie_Vvel*W56/V56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AA56)+W56*AA56)*SQRT(2)))-(EXP(-N56*Verolie_z/D_verOlie_Vvel*W56/V56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AB56)-W56*AB56)*SQRT(2))+EXP(N56*Verolie_z/D_verOlie_Vvel*W56/V56)*2*NORMSDIST(-(N56*Verolie_z/D_verOlie_Vvel/(2*V56*AB56)+W56*AB56)*SQRT(2))))*F56)))))","v":0},{"$f":"IF(Verolie_t-N56/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N56/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N56/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N56/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q56*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y56*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R56*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z56*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[910,null,null,null,null,{"$f":"D_olie_910_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_59","v":3.42},{"$f":"B_olie_DL_59","v":7.4964600630922756E-6},{"$f":"H57*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H57/10000","v":7.4964600630922754E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J57*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_59","v":0.89},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I57*((L57*1000)/(8.314*298))+K57*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G57-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M57/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N57*B_verolie_thetaw+B_verolie_thetaa*((L57*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F57*EXP((B_Verolie_Vw-O57)*B_verolie_z/(2*M57))","v":{"$error":"#DIV/0!"}},{"$f":"F57/2*(EXP((B_Verolie_Vw-O57)*B_verolie_z/(2*M57))*(1-fejlfunkk((B_verolie_z*P57-O57*B_Verolie_t)/(2*SQRT(M57*P57*B_Verolie_t))))+EXP((B_Verolie_Vw+O57)*B_verolie_z/(2*M57))*(1-fejlfunkk((B_verolie_z*P57+O57*B_Verolie_t)/(2*SQRT(M57*P57*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q57*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R57*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J57*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N57/(D_VerOlie_ntotal*SQRT(N57*U57))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N57)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F57*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N57*Verolie_z/D_verOlie_Vvel*W57/V57)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F57*(EXP(-D_VerOlie_lambdayear*Verolie_t/N57)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA57^2/N57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AA57)*SQRT(2))))),(IF(AND(AA57>0,AB57=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N57*Verolie_z/D_verOlie_Vvel*W57/V57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AA57)-W57*AA57)*SQRT(2))+EXP(N57*Verolie_z/D_verOlie_Vvel*W57/V57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AA57)+W57*AA57)*SQRT(2)))*F57,IF(AB57>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N57*Verolie_z/D_verOlie_Vvel*W57/V57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AA57)-W57*AA57)*SQRT(2))+EXP(N57*Verolie_z/D_verOlie_Vvel*W57/V57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AA57)+W57*AA57)*SQRT(2)))-(EXP(-N57*Verolie_z/D_verOlie_Vvel*W57/V57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AB57)-W57*AB57)*SQRT(2))+EXP(N57*Verolie_z/D_verOlie_Vvel*W57/V57)*2*NORMSDIST(-(N57*Verolie_z/D_verOlie_Vvel/(2*V57*AB57)+W57*AB57)*SQRT(2))))*F57)))))","v":0},{"$f":"IF(Verolie_t-N57/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N57/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N57/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N57/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q57*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y57*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R57*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z57*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[1015,"C11-C15",null,null,null,{"$f":"D_Olie_1015_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q59:Q67)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R59:R67)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S59:S67)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T59:T67)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y59:Y67)","v":0},{"$f":"SUM(Z59:Z67)","v":0},null,null,{"$f":"SUM(AC59:AC67)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD59:AD67)","v":{"$error":"#DIV/0!"}}]
[101,">10 - 12, alifater","Dodecan(C12)",null,null,{"$f":"D_Olie_101_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_101","v":6.1},{"$f":"B_olie_DL_101","v":5.6878283496407569E-6},{"$f":"H59*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H59/10000","v":5.6878283496407574E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J59*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_101","v":828.83849999999995},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I59*((L59*1000)/(8.314*298))+K59*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G59-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M59/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N59*B_verolie_thetaw+B_verolie_thetaa*((L59*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F59*EXP((B_Verolie_Vw-O59)*B_verolie_z/(2*M59))","v":{"$error":"#DIV/0!"}},{"$f":"F59/2*(EXP((B_Verolie_Vw-O59)*B_verolie_z/(2*M59))*(1-fejlfunkk((B_verolie_z*P59-O59*B_Verolie_t)/(2*SQRT(M59*P59*B_Verolie_t))))+EXP((B_Verolie_Vw+O59)*B_verolie_z/(2*M59))*(1-fejlfunkk((B_verolie_z*P59+O59*B_Verolie_t)/(2*SQRT(M59*P59*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q59*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R59*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J59*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N59/(D_VerOlie_ntotal*SQRT(N59*U59))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N59)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F59*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N59*Verolie_z/D_verOlie_Vvel*W59/V59)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F59*(EXP(-D_VerOlie_lambdayear*Verolie_t/N59)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA59^2/N59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AA59)*SQRT(2))))),(IF(AND(AA59>0,AB59=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N59*Verolie_z/D_verOlie_Vvel*W59/V59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AA59)-W59*AA59)*SQRT(2))+EXP(N59*Verolie_z/D_verOlie_Vvel*W59/V59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AA59)+W59*AA59)*SQRT(2)))*F59,IF(AB59>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N59*Verolie_z/D_verOlie_Vvel*W59/V59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AA59)-W59*AA59)*SQRT(2))+EXP(N59*Verolie_z/D_verOlie_Vvel*W59/V59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AA59)+W59*AA59)*SQRT(2)))-(EXP(-N59*Verolie_z/D_verOlie_Vvel*W59/V59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AB59)-W59*AB59)*SQRT(2))+EXP(N59*Verolie_z/D_verOlie_Vvel*W59/V59)*2*NORMSDIST(-(N59*Verolie_z/D_verOlie_Vvel/(2*V59*AB59)+W59*AB59)*SQRT(2))))*F59)))))","v":0},{"$f":"IF(Verolie_t-N59/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N59/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N59/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N59/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q59*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y59*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R59*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z59*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[102,">10 - 12, aromater","Sum >10 - 12 aromater"]
[103,null,"Naphthalen (C10)",null,null,{"$f":"D_Olie_103_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_103","v":3.3},{"$f":"B_olie_DL_103","v":7.2587936878955403E-6},{"$f":"H61*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H61/10000","v":7.25879368789554E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J61*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_103","v":4.4582999999999998E-2},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I61*((L61*1000)/(8.314*298))+K61*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G61-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M61/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N61*B_verolie_thetaw+B_verolie_thetaa*((L61*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F61*EXP((B_Verolie_Vw-O61)*B_verolie_z/(2*M61))","v":{"$error":"#DIV/0!"}},{"$f":"F61/2*(EXP((B_Verolie_Vw-O61)*B_verolie_z/(2*M61))*(1-fejlfunkk((B_verolie_z*P61-O61*B_Verolie_t)/(2*SQRT(M61*P61*B_Verolie_t))))+EXP((B_Verolie_Vw+O61)*B_verolie_z/(2*M61))*(1-fejlfunkk((B_verolie_z*P61+O61*B_Verolie_t)/(2*SQRT(M61*P61*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q61*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J61*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N61/(D_VerOlie_ntotal*SQRT(N61*U61))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N61)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F61*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N61*Verolie_z/D_verOlie_Vvel*W61/V61)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F61*(EXP(-D_VerOlie_lambdayear*Verolie_t/N61)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA61^2/N61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AA61)*SQRT(2))))),(IF(AND(AA61>0,AB61=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N61*Verolie_z/D_verOlie_Vvel*W61/V61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AA61)-W61*AA61)*SQRT(2))+EXP(N61*Verolie_z/D_verOlie_Vvel*W61/V61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AA61)+W61*AA61)*SQRT(2)))*F61,IF(AB61>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N61*Verolie_z/D_verOlie_Vvel*W61/V61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AA61)-W61*AA61)*SQRT(2))+EXP(N61*Verolie_z/D_verOlie_Vvel*W61/V61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AA61)+W61*AA61)*SQRT(2)))-(EXP(-N61*Verolie_z/D_verOlie_Vvel*W61/V61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AB61)-W61*AB61)*SQRT(2))+EXP(N61*Verolie_z/D_verOlie_Vvel*W61/V61)*2*NORMSDIST(-(N61*Verolie_z/D_verOlie_Vvel/(2*V61*AB61)+W61*AB61)*SQRT(2))))*F61)))))","v":0},{"$f":"IF(Verolie_t-N61/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N61/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N61/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N61/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q61*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y61*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R61*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z61*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[104,null,">10 - 12, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_104B_cv,D_Olie_104A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_104b,B_olie_kow_104a)","v":4.7300000000000004},{"$f":"IF(D_Olie_profil=1,B_olie_DL_104B,B_olie_DL_104A)","v":5.5260438461528997E-6},{"$f":"H62*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H62/10000","v":5.5260438461529001E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J62*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kH_104b,B_olie_kH_104a)","v":0.16700000000000001},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I62*((L62*1000)/(8.314*298))+K62*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G62-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M62/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N62*B_verolie_thetaw+B_verolie_thetaa*((L62*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F62*EXP((B_Verolie_Vw-O62)*B_verolie_z/(2*M62))","v":{"$error":"#DIV/0!"}},{"$f":"F62/2*(EXP((B_Verolie_Vw-O62)*B_verolie_z/(2*M62))*(1-fejlfunkk((B_verolie_z*P62-O62*B_Verolie_t)/(2*SQRT(M62*P62*B_Verolie_t))))+EXP((B_Verolie_Vw+O62)*B_verolie_z/(2*M62))*(1-fejlfunkk((B_verolie_z*P62+O62*B_Verolie_t)/(2*SQRT(M62*P62*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J62*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N62/(D_VerOlie_ntotal*SQRT(N62*U62))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N62)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F62*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N62*Verolie_z/D_verOlie_Vvel*W62/V62)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F62*(EXP(-D_VerOlie_lambdayear*Verolie_t/N62)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA62^2/N62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AA62)*SQRT(2))))),(IF(AND(AA62>0,AB62=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N62*Verolie_z/D_verOlie_Vvel*W62/V62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AA62)-W62*AA62)*SQRT(2))+EXP(N62*Verolie_z/D_verOlie_Vvel*W62/V62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AA62)+W62*AA62)*SQRT(2)))*F62,IF(AB62>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N62*Verolie_z/D_verOlie_Vvel*W62/V62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AA62)-W62*AA62)*SQRT(2))+EXP(N62*Verolie_z/D_verOlie_Vvel*W62/V62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AA62)+W62*AA62)*SQRT(2)))-(EXP(-N62*Verolie_z/D_verOlie_Vvel*W62/V62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AB62)-W62*AB62)*SQRT(2))+EXP(N62*Verolie_z/D_verOlie_Vvel*W62/V62)*2*NORMSDIST(-(N62*Verolie_z/D_verOlie_Vvel/(2*V62*AB62)+W62*AB62)*SQRT(2))))*F62)))))","v":0},{"$f":"IF(Verolie_t-N62/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N62/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N62/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N62/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[105,">12 - 16, alifater",">12 - 16, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_105B_cv,D_Olie_105A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_105b,B_olie_kow_105a)","v":7.72},{"$f":"IF(D_Olie_profil=1,B_olie_DL_105B,B_olie_DL_105A)","v":5.0933919872504982E-6},{"$f":"H63*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H63/10000","v":5.0933919872504985E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J63*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kH_105b,B_olie_kH_105a)","v":726.05},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I63*((L63*1000)/(8.314*298))+K63*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G63-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M63/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N63*B_verolie_thetaw+B_verolie_thetaa*((L63*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F63*EXP((B_Verolie_Vw-O63)*B_verolie_z/(2*M63))","v":{"$error":"#DIV/0!"}},{"$f":"F63/2*(EXP((B_Verolie_Vw-O63)*B_verolie_z/(2*M63))*(1-fejlfunkk((B_verolie_z*P63-O63*B_Verolie_t)/(2*SQRT(M63*P63*B_Verolie_t))))+EXP((B_Verolie_Vw+O63)*B_verolie_z/(2*M63))*(1-fejlfunkk((B_verolie_z*P63+O63*B_Verolie_t)/(2*SQRT(M63*P63*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J63*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N63/(D_VerOlie_ntotal*SQRT(N63*U63))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N63)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F63*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N63*Verolie_z/D_verOlie_Vvel*W63/V63)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F63*(EXP(-D_VerOlie_lambdayear*Verolie_t/N63)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA63^2/N63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AA63)*SQRT(2))))),(IF(AND(AA63>0,AB63=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N63*Verolie_z/D_verOlie_Vvel*W63/V63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AA63)-W63*AA63)*SQRT(2))+EXP(N63*Verolie_z/D_verOlie_Vvel*W63/V63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AA63)+W63*AA63)*SQRT(2)))*F63,IF(AB63>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N63*Verolie_z/D_verOlie_Vvel*W63/V63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AA63)-W63*AA63)*SQRT(2))+EXP(N63*Verolie_z/D_verOlie_Vvel*W63/V63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AA63)+W63*AA63)*SQRT(2)))-(EXP(-N63*Verolie_z/D_verOlie_Vvel*W63/V63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AB63)-W63*AB63)*SQRT(2))+EXP(N63*Verolie_z/D_verOlie_Vvel*W63/V63)*2*NORMSDIST(-(N63*Verolie_z/D_verOlie_Vvel/(2*V63*AB63)+W63*AB63)*SQRT(2))))*F63)))))","v":0},{"$f":"IF(Verolie_t-N63/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N63/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N63/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N63/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[106,">12 - 16, aromater","Sum >10 - 12 aromater",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[107,null,"Acenaphthylen (C12)",null,null,{"$f":"D_Olie_107_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_107","v":4.07},{"$f":"B_olie_DL_107","v":6.6619464783515415E-6},{"$f":"H65*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H65/10000","v":6.6619464783515417E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J65*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_107","v":0.11550000000000001},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I65*((L65*1000)/(8.314*298))+K65*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G65-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M65/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N65*B_verolie_thetaw+B_verolie_thetaa*((L65*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F65*EXP((B_Verolie_Vw-O65)*B_verolie_z/(2*M65))","v":{"$error":"#DIV/0!"}},{"$f":"F65/2*(EXP((B_Verolie_Vw-O65)*B_verolie_z/(2*M65))*(1-fejlfunkk((B_verolie_z*P65-O65*B_Verolie_t)/(2*SQRT(M65*P65*B_Verolie_t))))+EXP((B_Verolie_Vw+O65)*B_verolie_z/(2*M65))*(1-fejlfunkk((B_verolie_z*P65+O65*B_Verolie_t)/(2*SQRT(M65*P65*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q65*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J65*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N65/(D_VerOlie_ntotal*SQRT(N65*U65))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N65)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F65*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N65*Verolie_z/D_verOlie_Vvel*W65/V65)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F65*(EXP(-D_VerOlie_lambdayear*Verolie_t/N65)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA65^2/N65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AA65)*SQRT(2))))),(IF(AND(AA65>0,AB65=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N65*Verolie_z/D_verOlie_Vvel*W65/V65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AA65)-W65*AA65)*SQRT(2))+EXP(N65*Verolie_z/D_verOlie_Vvel*W65/V65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AA65)+W65*AA65)*SQRT(2)))*F65,IF(AB65>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N65*Verolie_z/D_verOlie_Vvel*W65/V65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AA65)-W65*AA65)*SQRT(2))+EXP(N65*Verolie_z/D_verOlie_Vvel*W65/V65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AA65)+W65*AA65)*SQRT(2)))-(EXP(-N65*Verolie_z/D_verOlie_Vvel*W65/V65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AB65)-W65*AB65)*SQRT(2))+EXP(N65*Verolie_z/D_verOlie_Vvel*W65/V65)*2*NORMSDIST(-(N65*Verolie_z/D_verOlie_Vvel/(2*V65*AB65)+W65*AB65)*SQRT(2))))*F65)))))","v":0},{"$f":"IF(Verolie_t-N65/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N65/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N65/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N65/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[108,null,"Acenaphthen (C12)",null,null,{"$f":"D_Olie_108_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_108","v":3.92},{"$f":"B_olie_DL_108","v":6.6186021894078394E-6},{"$f":"H66*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H66/10000","v":6.6186021894078393E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J66*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_108","v":0.18643799999999999},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I66*((L66*1000)/(8.314*298))+K66*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G66-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M66/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N66*B_verolie_thetaw+B_verolie_thetaa*((L66*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F66*EXP((B_Verolie_Vw-O66)*B_verolie_z/(2*M66))","v":{"$error":"#DIV/0!"}},{"$f":"F66/2*(EXP((B_Verolie_Vw-O66)*B_verolie_z/(2*M66))*(1-fejlfunkk((B_verolie_z*P66-O66*B_Verolie_t)/(2*SQRT(M66*P66*B_Verolie_t))))+EXP((B_Verolie_Vw+O66)*B_verolie_z/(2*M66))*(1-fejlfunkk((B_verolie_z*P66+O66*B_Verolie_t)/(2*SQRT(M66*P66*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J66*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N66/(D_VerOlie_ntotal*SQRT(N66*U66))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N66)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F66*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N66*Verolie_z/D_verOlie_Vvel*W66/V66)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F66*(EXP(-D_VerOlie_lambdayear*Verolie_t/N66)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA66^2/N66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AA66)*SQRT(2))))),(IF(AND(AA66>0,AB66=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N66*Verolie_z/D_verOlie_Vvel*W66/V66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AA66)-W66*AA66)*SQRT(2))+EXP(N66*Verolie_z/D_verOlie_Vvel*W66/V66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AA66)+W66*AA66)*SQRT(2)))*F66,IF(AB66>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N66*Verolie_z/D_verOlie_Vvel*W66/V66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AA66)-W66*AA66)*SQRT(2))+EXP(N66*Verolie_z/D_verOlie_Vvel*W66/V66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AA66)+W66*AA66)*SQRT(2)))-(EXP(-N66*Verolie_z/D_verOlie_Vvel*W66/V66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AB66)-W66*AB66)*SQRT(2))+EXP(N66*Verolie_z/D_verOlie_Vvel*W66/V66)*2*NORMSDIST(-(N66*Verolie_z/D_verOlie_Vvel/(2*V66*AB66)+W66*AB66)*SQRT(2))))*F66)))))","v":0},{"$f":"IF(Verolie_t-N66/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N66/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N66/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N66/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[109,null,">12 - 16, aromater,øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_109B_cv,D_Olie_109A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_109b,B_olie_kow_109a)","v":4.4000000000000004},{"$f":"IF(D_Olie_profil=1,B_olie_DL_109B,B_olie_DL_109A)","v":5.9000000000000003E-6},{"$f":"H67*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H67/10000","v":5.9000000000000003E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J67*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kH_109b,B_olie_kH_109a)","v":7.8600000000000003E-2},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I67*((L67*1000)/(8.314*298))+K67*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G67-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M67/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N67*B_verolie_thetaw+B_verolie_thetaa*((L67*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F67*EXP((B_Verolie_Vw-O67)*B_verolie_z/(2*M67))","v":{"$error":"#DIV/0!"}},{"$f":"F67/2*(EXP((B_Verolie_Vw-O67)*B_verolie_z/(2*M67))*(1-fejlfunkk((B_verolie_z*P67-O67*B_Verolie_t)/(2*SQRT(M67*P67*B_Verolie_t))))+EXP((B_Verolie_Vw+O67)*B_verolie_z/(2*M67))*(1-fejlfunkk((B_verolie_z*P67+O67*B_Verolie_t)/(2*SQRT(M67*P67*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J67*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N67/(D_VerOlie_ntotal*SQRT(N67*U67))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N67)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F67*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N67*Verolie_z/D_verOlie_Vvel*W67/V67)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F67*(EXP(-D_VerOlie_lambdayear*Verolie_t/N67)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA67^2/N67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AA67)*SQRT(2))))),(IF(AND(AA67>0,AB67=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N67*Verolie_z/D_verOlie_Vvel*W67/V67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AA67)-W67*AA67)*SQRT(2))+EXP(N67*Verolie_z/D_verOlie_Vvel*W67/V67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AA67)+W67*AA67)*SQRT(2)))*F67,IF(AB67>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N67*Verolie_z/D_verOlie_Vvel*W67/V67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AA67)-W67*AA67)*SQRT(2))+EXP(N67*Verolie_z/D_verOlie_Vvel*W67/V67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AA67)+W67*AA67)*SQRT(2)))-(EXP(-N67*Verolie_z/D_verOlie_Vvel*W67/V67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AB67)-W67*AB67)*SQRT(2))+EXP(N67*Verolie_z/D_verOlie_Vvel*W67/V67)*2*NORMSDIST(-(N67*Verolie_z/D_verOlie_Vvel/(2*V67*AB67)+W67*AB67)*SQRT(2))))*F67)))))","v":0},{"$f":"IF(Verolie_t-N67/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N67/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N67/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N67/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[1520,"C16-C20",null,null,null,{"$f":"D_Olie_1520_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q70:Q76)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R70:R76)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S70:S76)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T70:T76)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y70:Y76)","v":0},{"$f":"SUM(Z70:Z76)","v":0},null,null,{"$f":"SUM(AC70:AC76)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD70:AD76)","v":{"$error":"#DIV/0!"}}]
[151,">16 - 21, alifater",">16 - 21, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_151B_cv,D_Olie_151A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_151b,B_olie_kow_151a)","v":9.84},{"$f":"IF(D_Olie_profil=1,B_olie_DL_151B,B_olie_DL_151A)","v":4.4721099862171762E-6},{"$f":"H70*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H70/10000","v":4.472109986217176E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J70*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kH_151b,B_olie_kH_151a)","v":8341.59},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I70*((L70*1000)/(8.314*298))+K70*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G70-0.84))*D_Verolie_foc*D_Verolie_rhob/D_VerOlie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"D_Verolie_Vw*SQRT(1+4*D_Verolie_lambda*M70/D_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N70*B_verolie_thetaw+B_verolie_thetaa*((L70*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F70*EXP((D_Verolie_Vw-O70)*D_Verolie_z/(2*M70))","v":{"$error":"#DIV/0!"}},{"$f":"F70/2*(EXP((D_Verolie_Vw-O70)*D_Verolie_z/(2*M70))*(1-fejlfunkk((D_Verolie_z*P70-O70*B_Verolie_t)/(2*SQRT(M70*P70*B_Verolie_t))))+EXP((D_Verolie_Vw+O70)*D_Verolie_z/(2*M70))*(1-fejlfunkk((D_Verolie_z*P70+O70*B_Verolie_t)/(2*SQRT(M70*P70*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q70*D_Verolie_Y*D_Verolie_X*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R70*D_Verolie_Y*D_Verolie_X*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J70*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N70/(D_VerOlie_ntotal*SQRT(N70*U70))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N70)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F70*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N70*Verolie_z/D_verOlie_Vvel*W70/V70)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F70*(EXP(-D_VerOlie_lambdayear*Verolie_t/N70)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA70^2/N70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AA70)*SQRT(2))))),(IF(AND(AA70>0,AB70=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N70*Verolie_z/D_verOlie_Vvel*W70/V70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AA70)-W70*AA70)*SQRT(2))+EXP(N70*Verolie_z/D_verOlie_Vvel*W70/V70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AA70)+W70*AA70)*SQRT(2)))*F70,IF(AB70>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N70*Verolie_z/D_verOlie_Vvel*W70/V70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AA70)-W70*AA70)*SQRT(2))+EXP(N70*Verolie_z/D_verOlie_Vvel*W70/V70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AA70)+W70*AA70)*SQRT(2)))-(EXP(-N70*Verolie_z/D_verOlie_Vvel*W70/V70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AB70)-W70*AB70)*SQRT(2))+EXP(N70*Verolie_z/D_verOlie_Vvel*W70/V70)*2*NORMSDIST(-(N70*Verolie_z/D_verOlie_Vvel/(2*V70*AB70)+W70*AB70)*SQRT(2))))*F70)))))","v":0},{"$f":"IF(Verolie_t-N70/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N70/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N70/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N70/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q70*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y70*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R70*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z70*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[152,">16 - 21, aromater","Sum >16 - 21 aromater",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[153,null,"Fluoren (C13)",null,null,{"$f":"D_Olie_153_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_153","v":4.18},{"$f":"B_olie_DL_153","v":6.3751874043382609E-6},{"$f":"H72*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H72/10000","v":6.375187404338261E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J72*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_153","v":9.7474650000000003E-3},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I72*((L72*1000)/(8.314*298))+K72*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G72-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M72/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N72*B_verolie_thetaw+B_verolie_thetaa*((L72*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F72*EXP((B_Verolie_Vw-O72)*B_verolie_z/(2*M72))","v":{"$error":"#DIV/0!"}},{"$f":"F72/2*(EXP((B_Verolie_Vw-O72)*B_verolie_z/(2*M72))*(1-fejlfunkk((B_verolie_z*P72-O72*B_Verolie_t)/(2*SQRT(M72*P72*B_Verolie_t))))+EXP((B_Verolie_Vw+O72)*B_verolie_z/(2*M72))*(1-fejlfunkk((B_verolie_z*P72+O72*B_Verolie_t)/(2*SQRT(M72*P72*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q72*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J72*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N72/(D_VerOlie_ntotal*SQRT(N72*U72))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N72)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F72*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N72*Verolie_z/D_verOlie_Vvel*W72/V72)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F72*(EXP(-D_VerOlie_lambdayear*Verolie_t/N72)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA72^2/N72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AA72)*SQRT(2))))),(IF(AND(AA72>0,AB72=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N72*Verolie_z/D_verOlie_Vvel*W72/V72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AA72)-W72*AA72)*SQRT(2))+EXP(N72*Verolie_z/D_verOlie_Vvel*W72/V72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AA72)+W72*AA72)*SQRT(2)))*F72,IF(AB72>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N72*Verolie_z/D_verOlie_Vvel*W72/V72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AA72)-W72*AA72)*SQRT(2))+EXP(N72*Verolie_z/D_verOlie_Vvel*W72/V72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AA72)+W72*AA72)*SQRT(2)))-(EXP(-N72*Verolie_z/D_verOlie_Vvel*W72/V72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AB72)-W72*AB72)*SQRT(2))+EXP(N72*Verolie_z/D_verOlie_Vvel*W72/V72)*2*NORMSDIST(-(N72*Verolie_z/D_verOlie_Vvel/(2*V72*AB72)+W72*AB72)*SQRT(2))))*F72)))))","v":0},{"$f":"IF(Verolie_t-N72/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N72/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N72/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N72/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[154,null,"Phenanthren (C14)",null,null,{"$f":"D_Olie_154_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_154","v":4.46},{"$f":"B_olie_DL_154","v":6.1567938987033759E-6},{"$f":"H73*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H73/10000","v":6.1567938987033764E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J73*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_154","v":4.2860475E-3},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I73*((L73*1000)/(8.314*298))+K73*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G73-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M73/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N73*B_verolie_thetaw+B_verolie_thetaa*((L73*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F73*EXP((B_Verolie_Vw-O73)*B_verolie_z/(2*M73))","v":{"$error":"#DIV/0!"}},{"$f":"F73/2*(EXP((B_Verolie_Vw-O73)*B_verolie_z/(2*M73))*(1-fejlfunkk((B_verolie_z*P73-O73*B_Verolie_t)/(2*SQRT(M73*P73*B_Verolie_t))))+EXP((B_Verolie_Vw+O73)*B_verolie_z/(2*M73))*(1-fejlfunkk((B_verolie_z*P73+O73*B_Verolie_t)/(2*SQRT(M73*P73*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J73*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N73/(D_VerOlie_ntotal*SQRT(N73*U73))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N73)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F73*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N73*Verolie_z/D_verOlie_Vvel*W73/V73)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F73*(EXP(-D_VerOlie_lambdayear*Verolie_t/N73)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA73^2/N73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AA73)*SQRT(2))))),(IF(AND(AA73>0,AB73=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N73*Verolie_z/D_verOlie_Vvel*W73/V73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AA73)-W73*AA73)*SQRT(2))+EXP(N73*Verolie_z/D_verOlie_Vvel*W73/V73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AA73)+W73*AA73)*SQRT(2)))*F73,IF(AB73>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N73*Verolie_z/D_verOlie_Vvel*W73/V73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AA73)-W73*AA73)*SQRT(2))+EXP(N73*Verolie_z/D_verOlie_Vvel*W73/V73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AA73)+W73*AA73)*SQRT(2)))-(EXP(-N73*Verolie_z/D_verOlie_Vvel*W73/V73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AB73)-W73*AB73)*SQRT(2))+EXP(N73*Verolie_z/D_verOlie_Vvel*W73/V73)*2*NORMSDIST(-(N73*Verolie_z/D_verOlie_Vvel/(2*V73*AB73)+W73*AB73)*SQRT(2))))*F73)))))","v":0},{"$f":"IF(Verolie_t-N73/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N73/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N73/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N73/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[155,null,"Anthracen (C14)",null,null,{"$f":"D_Olie_155_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_155","v":4.45},{"$f":"B_olie_DL_155","v":6.1567938987033759E-6},{"$f":"H74*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H74/10000","v":6.1567938987033764E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J74*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_155","v":5.6336700000000003E-3},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I74*((L74*1000)/(8.314*298))+K74*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G74-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M74/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N74*B_verolie_thetaw+B_verolie_thetaa*((L74*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F74*EXP((B_Verolie_Vw-O74)*B_verolie_z/(2*M74))","v":{"$error":"#DIV/0!"}},{"$f":"F74/2*(EXP((B_Verolie_Vw-O74)*B_verolie_z/(2*M74))*(1-fejlfunkk((B_verolie_z*P74-O74*B_Verolie_t)/(2*SQRT(M74*P74*B_Verolie_t))))+EXP((B_Verolie_Vw+O74)*B_verolie_z/(2*M74))*(1-fejlfunkk((B_verolie_z*P74+O74*B_Verolie_t)/(2*SQRT(M74*P74*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J74*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N74/(D_VerOlie_ntotal*SQRT(N74*U74))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N74)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F74*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N74*Verolie_z/D_verOlie_Vvel*W74/V74)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F74*(EXP(-D_VerOlie_lambdayear*Verolie_t/N74)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA74^2/N74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AA74)*SQRT(2))))),(IF(AND(AA74>0,AB74=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N74*Verolie_z/D_verOlie_Vvel*W74/V74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AA74)-W74*AA74)*SQRT(2))+EXP(N74*Verolie_z/D_verOlie_Vvel*W74/V74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AA74)+W74*AA74)*SQRT(2)))*F74,IF(AB74>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N74*Verolie_z/D_verOlie_Vvel*W74/V74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AA74)-W74*AA74)*SQRT(2))+EXP(N74*Verolie_z/D_verOlie_Vvel*W74/V74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AA74)+W74*AA74)*SQRT(2)))-(EXP(-N74*Verolie_z/D_verOlie_Vvel*W74/V74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AB74)-W74*AB74)*SQRT(2))+EXP(N74*Verolie_z/D_verOlie_Vvel*W74/V74)*2*NORMSDIST(-(N74*Verolie_z/D_verOlie_Vvel/(2*V74*AB74)+W74*AB74)*SQRT(2))))*F74)))))","v":0},{"$f":"IF(Verolie_t-N74/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N74/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N74/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N74/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[156,null,"Fluoranthen (C16)",null,null,{"$f":"D_Olie_156_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_156","v":5.16},{"$f":"B_olie_DL_156","v":5.7784388814859601E-6},{"$f":"H75*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H75/10000","v":5.7784388814859598E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J75*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_156","v":8.977395E-4},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I75*((L75*1000)/(8.314*298))+K75*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G75-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M75/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N75*B_verolie_thetaw+B_verolie_thetaa*((L75*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F75*EXP((B_Verolie_Vw-O75)*B_verolie_z/(2*M75))","v":{"$error":"#DIV/0!"}},{"$f":"F75/2*(EXP((B_Verolie_Vw-O75)*B_verolie_z/(2*M75))*(1-fejlfunkk((B_verolie_z*P75-O75*B_Verolie_t)/(2*SQRT(M75*P75*B_Verolie_t))))+EXP((B_Verolie_Vw+O75)*B_verolie_z/(2*M75))*(1-fejlfunkk((B_verolie_z*P75+O75*B_Verolie_t)/(2*SQRT(M75*P75*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J75*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N75/(D_VerOlie_ntotal*SQRT(N75*U75))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N75)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F75*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N75*Verolie_z/D_verOlie_Vvel*W75/V75)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F75*(EXP(-D_VerOlie_lambdayear*Verolie_t/N75)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA75^2/N75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AA75)*SQRT(2))))),(IF(AND(AA75>0,AB75=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N75*Verolie_z/D_verOlie_Vvel*W75/V75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AA75)-W75*AA75)*SQRT(2))+EXP(N75*Verolie_z/D_verOlie_Vvel*W75/V75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AA75)+W75*AA75)*SQRT(2)))*F75,IF(AB75>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N75*Verolie_z/D_verOlie_Vvel*W75/V75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AA75)-W75*AA75)*SQRT(2))+EXP(N75*Verolie_z/D_verOlie_Vvel*W75/V75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AA75)+W75*AA75)*SQRT(2)))-(EXP(-N75*Verolie_z/D_verOlie_Vvel*W75/V75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AB75)-W75*AB75)*SQRT(2))+EXP(N75*Verolie_z/D_verOlie_Vvel*W75/V75)*2*NORMSDIST(-(N75*Verolie_z/D_verOlie_Vvel/(2*V75*AB75)+W75*AB75)*SQRT(2))))*F75)))))","v":0},{"$f":"IF(Verolie_t-N75/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N75/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N75/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N75/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[157,null,"Pyren (C16)",null,null,{"$f":"D_Olie_157_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_157","v":4.88},{"$f":"B_olie_DL_157","v":5.7784388814859601E-6},{"$f":"H76*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H76/10000","v":5.7784388814859598E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J76*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_157","v":1.2057674999999999E-3},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I76*((L76*1000)/(8.314*298))+K76*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G76-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M76/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N76*B_verolie_thetaw+B_verolie_thetaa*((L76*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F76*EXP((B_Verolie_Vw-O76)*B_verolie_z/(2*M76))","v":{"$error":"#DIV/0!"}},{"$f":"F76/2*(EXP((B_Verolie_Vw-O76)*B_verolie_z/(2*M76))*(1-fejlfunkk((B_verolie_z*P76-O76*B_Verolie_t)/(2*SQRT(M76*P76*B_Verolie_t))))+EXP((B_Verolie_Vw+O76)*B_verolie_z/(2*M76))*(1-fejlfunkk((B_verolie_z*P76+O76*B_Verolie_t)/(2*SQRT(M76*P76*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"J76*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N76/(D_VerOlie_ntotal*SQRT(N76*U76))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N76)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F76*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N76*Verolie_z/D_verOlie_Vvel*W76/V76)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F76*(EXP(-D_VerOlie_lambdayear*Verolie_t/N76)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA76^2/N76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AA76)*SQRT(2))))),(IF(AND(AA76>0,AB76=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N76*Verolie_z/D_verOlie_Vvel*W76/V76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AA76)-W76*AA76)*SQRT(2))+EXP(N76*Verolie_z/D_verOlie_Vvel*W76/V76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AA76)+W76*AA76)*SQRT(2)))*F76,IF(AB76>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N76*Verolie_z/D_verOlie_Vvel*W76/V76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AA76)-W76*AA76)*SQRT(2))+EXP(N76*Verolie_z/D_verOlie_Vvel*W76/V76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AA76)+W76*AA76)*SQRT(2)))-(EXP(-N76*Verolie_z/D_verOlie_Vvel*W76/V76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AB76)-W76*AB76)*SQRT(2))+EXP(N76*Verolie_z/D_verOlie_Vvel*W76/V76)*2*NORMSDIST(-(N76*Verolie_z/D_verOlie_Vvel/(2*V76*AB76)+W76*AB76)*SQRT(2))))*F76)))))","v":0},{"$f":"IF(Verolie_t-N76/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N76/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N76/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N76/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[2025,"C21-C25",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D_verOlie_AC,Q78*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y78*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_verOlie_AC,R78*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z78*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#VALUE!"}}]
[201,">21 - 25, alifater",">21 - 25, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_201B_cv,D_Olie_201A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_201b,B_olie_kow_201a)","v":12.62},{"$f":"IF(D_Olie_profil=1,B_olie_DL_201B,B_olie_DL_201A)","v":3.9528308464137552E-6},{"$f":"H79*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H79/10000","v":3.9528308464137553E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J79*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kH_201b,B_olie_kH_201a)","v":37693},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I79*((L79*1000)/(8.314*298))+K79*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G79-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M79/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N79*B_verolie_thetaw+B_verolie_thetaa*((L79*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F79*EXP((B_Verolie_Vw-O79)*B_verolie_z/(2*M79))","v":{"$error":"#DIV/0!"}},{"$f":"F79/2*(EXP((B_Verolie_Vw-O79)*B_verolie_z/(2*M79))*(1-fejlfunkk((B_verolie_z*P79-O79*B_Verolie_t)/(2*SQRT(M79*P79*B_Verolie_t))))+EXP((B_Verolie_Vw+O79)*B_verolie_z/(2*M79))*(1-fejlfunkk((B_verolie_z*P79+O79*B_Verolie_t)/(2*SQRT(M79*P79*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q79*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R79*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J79*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N79/(D_VerOlie_ntotal*SQRT(N79*U79))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N79)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F79*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N79*Verolie_z/D_verOlie_Vvel*W79/V79)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F79*(EXP(-D_VerOlie_lambdayear*Verolie_t/N79)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA79^2/N79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AA79)*SQRT(2))))),(IF(AND(AA79>0,AB79=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N79*Verolie_z/D_verOlie_Vvel*W79/V79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AA79)-W79*AA79)*SQRT(2))+EXP(N79*Verolie_z/D_verOlie_Vvel*W79/V79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AA79)+W79*AA79)*SQRT(2)))*F79,IF(AB79>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N79*Verolie_z/D_verOlie_Vvel*W79/V79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AA79)-W79*AA79)*SQRT(2))+EXP(N79*Verolie_z/D_verOlie_Vvel*W79/V79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AA79)+W79*AA79)*SQRT(2)))-(EXP(-N79*Verolie_z/D_verOlie_Vvel*W79/V79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AB79)-W79*AB79)*SQRT(2))+EXP(N79*Verolie_z/D_verOlie_Vvel*W79/V79)*2*NORMSDIST(-(N79*Verolie_z/D_verOlie_Vvel/(2*V79*AB79)+W79*AB79)*SQRT(2))))*F79)))))","v":0},{"$f":"IF(Verolie_t-N79/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N79/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N79/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N79/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q79*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y79*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R79*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z79*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[202,">21 - 25, aromater","Ingen repræsentanter"]
[]
[2535,"C25-C35",null,null,null,{"$f":"D_Olie_2535_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q83:Q91)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R83:R91)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S83:S91)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T83:T91)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y83:Y91)","v":0},{"$f":"SUM(Z83:Z91)","v":0},null,null,{"$f":"SUM(AC83:AC91)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD83:AD91)","v":{"$error":"#DIV/0!"}}]
[251,">25 - 35, alifater",">25 - 35, alifater",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_251B_cv,D_Olie_251A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_251b,B_olie_kow_251a)","v":14.58},{"$f":"IF(D_Olie_profil=1,B_olie_DL_251B,B_olie_DL_251A)","v":3.6715492605442101E-6},{"$f":"H83*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H83/10000","v":3.6715492605442102E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J83*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kH_251b,B_olie_kH_251a)","v":757252},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I83*((L83*1000)/(8.314*298))+K83*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G83-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M83/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N83*B_verolie_thetaw+B_verolie_thetaa*((L83*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F83*EXP((B_Verolie_Vw-O83)*B_verolie_z/(2*M83))","v":{"$error":"#DIV/0!"}},{"$f":"F83/2*(EXP((B_Verolie_Vw-O83)*B_verolie_z/(2*M83))*(1-fejlfunkk((B_verolie_z*P83-O83*B_Verolie_t)/(2*SQRT(M83*P83*B_Verolie_t))))+EXP((B_Verolie_Vw+O83)*B_verolie_z/(2*M83))*(1-fejlfunkk((B_verolie_z*P83+O83*B_Verolie_t)/(2*SQRT(M83*P83*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q83*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R83*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J83*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N83/(D_VerOlie_ntotal*SQRT(N83*U83))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N83)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F83*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N83*Verolie_z/D_verOlie_Vvel*W83/V83)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F83*(EXP(-D_VerOlie_lambdayear*Verolie_t/N83)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA83^2/N83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AA83)*SQRT(2))))),(IF(AND(AA83>0,AB83=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N83*Verolie_z/D_verOlie_Vvel*W83/V83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AA83)-W83*AA83)*SQRT(2))+EXP(N83*Verolie_z/D_verOlie_Vvel*W83/V83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AA83)+W83*AA83)*SQRT(2)))*F83,IF(AB83>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N83*Verolie_z/D_verOlie_Vvel*W83/V83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AA83)-W83*AA83)*SQRT(2))+EXP(N83*Verolie_z/D_verOlie_Vvel*W83/V83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AA83)+W83*AA83)*SQRT(2)))-(EXP(-N83*Verolie_z/D_verOlie_Vvel*W83/V83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AB83)-W83*AB83)*SQRT(2))+EXP(N83*Verolie_z/D_verOlie_Vvel*W83/V83)*2*NORMSDIST(-(N83*Verolie_z/D_verOlie_Vvel/(2*V83*AB83)+W83*AB83)*SQRT(2))))*F83)))))","v":0},{"$f":"IF(Verolie_t-N83/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N83/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N83/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N83/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q83*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y83*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R83*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z83*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[252,">25 - 35, aromater","Sum >25 - 35 aromater",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[253,null,"Benzo(a)anthracen (C18)",null,null,{"$f":"D_Olie_253_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_253","v":5.76},{"$f":"B_olie_DL_253","v":5.4394565218975376E-6},{"$f":"H85*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H85/10000","v":5.439456521897538E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J85*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_253","v":1.2159E-3},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I85*((L85*1000)/(8.314*298))+K85*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G85-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M85/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N85*B_verolie_thetaw+B_verolie_thetaa*((L85*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F85*EXP((B_Verolie_Vw-O85)*B_verolie_z/(2*M85))","v":{"$error":"#DIV/0!"}},{"$f":"F85/2*(EXP((B_Verolie_Vw-O85)*B_verolie_z/(2*M85))*(1-fejlfunkk((B_verolie_z*P85-O85*B_Verolie_t)/(2*SQRT(M85*P85*B_Verolie_t))))+EXP((B_Verolie_Vw+O85)*B_verolie_z/(2*M85))*(1-fejlfunkk((B_verolie_z*P85+O85*B_Verolie_t)/(2*SQRT(M85*P85*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q85*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J85*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N85/(D_VerOlie_ntotal*SQRT(N85*U85))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N85)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F85*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N85*Verolie_z/D_verOlie_Vvel*W85/V85)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F85*(EXP(-D_VerOlie_lambdayear*Verolie_t/N85)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA85^2/N85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AA85)*SQRT(2))))),(IF(AND(AA85>0,AB85=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N85*Verolie_z/D_verOlie_Vvel*W85/V85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AA85)-W85*AA85)*SQRT(2))+EXP(N85*Verolie_z/D_verOlie_Vvel*W85/V85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AA85)+W85*AA85)*SQRT(2)))*F85,IF(AB85>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N85*Verolie_z/D_verOlie_Vvel*W85/V85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AA85)-W85*AA85)*SQRT(2))+EXP(N85*Verolie_z/D_verOlie_Vvel*W85/V85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AA85)+W85*AA85)*SQRT(2)))-(EXP(-N85*Verolie_z/D_verOlie_Vvel*W85/V85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AB85)-W85*AB85)*SQRT(2))+EXP(N85*Verolie_z/D_verOlie_Vvel*W85/V85)*2*NORMSDIST(-(N85*Verolie_z/D_verOlie_Vvel/(2*V85*AB85)+W85*AB85)*SQRT(2))))*F85)))))","v":0},{"$f":"IF(Verolie_t-N85/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N85/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N85/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N85/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[254,null,"Chrysen (C18)",null,null,{"$f":"D_Olie_254_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_254","v":5.81},{"$f":"B_olie_DL_254","v":5.4394565218975376E-6},{"$error":"#VALUE!"},5.439456521897538E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_254","v":5.2992974999999999E-4},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[255,null,"Benzo(b)fluoranthen (C20)",null,null,{"$f":"D_Olie_255_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_255","v":5.78},{"$f":"B_olie_DL_255","v":5.1742789740511641E-6},{"$error":"#VALUE!"},5.1742789740511642E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_255","v":6.6570524999999997E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[256,null,"Benzo(a)pyren",null,null,{"$f":"D_Olie_256_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_256","v":6.13},{"$f":"B_olie_DL_256","v":5.1742789740511641E-6},{"$error":"#VALUE!"},5.1742789740511642E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_256","v":4.6305525000000001E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[257,null,"Dibenz(a,h)anthracen (C22)",null,null,{"$f":"D_Olie_257_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_257","v":6.75},{"$f":"B_olie_DL_257","v":4.9257668316019948E-6},{"$error":"#VALUE!"},4.9257668316019945E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_257","v":1.4286825E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[258,null,"Benzo(ghi)perylen (C22)",null,null,{"$f":"D_Olie_258_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_258","v":6.63},{"$f":"B_olie_DL_258","v":4.9444503816447828E-6},{"$error":"#VALUE!"},4.9444503816447827E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_258","v":3.3538575000000003E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[259,null,">25 - 35, aromater, øvrige",null,null,{"$f":"IF(D_Olie_profil=1,D_Olie_259B_cv,D_Olie_259A_cv)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_Olie_profil=1,B_olie_kow_259b,B_olie_kow_259a)","v":7.11},{"$f":"IF(D_Olie_profil=1,B_olie_DL_259B,B_olie_DL_259A)","v":4.4493993711079091E-6},{"$error":"#VALUE!"},4.4493993711079089E-10,{"$error":"#VALUE!"},{"$f":"IF(D_Olie_profil=1,B_olie_kH_259b,B_olie_kH_259a)","v":4.95479E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[3540,">C35",null,null,null,{"$f":"D_Olie_3540_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q94:Q95)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R94:R95)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S94:S95)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T94:T95)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y94:Y95)","v":0},{"$f":"SUM(Z94:Z95)","v":0},null,null,{"$f":"SUM(AC94:AC95)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD94:AD95)","v":{"$error":"#DIV/0!"}}]
[351,">35 - 44, alifater","Pentatriacontan (C35)",null,null,{"$f":"D_Olie_351_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_351","v":17.53},{"$f":"B_olie_DL_351","v":3.7017352631160009E-6},{"$f":"H94*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H94/10000","v":3.7017352631160008E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J94*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_351","v":640374},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I94*((L94*1000)/(8.314*298))+K94*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G94-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M94/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N94*B_verolie_thetaw+B_verolie_thetaa*((L94*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F94*EXP((B_Verolie_Vw-O94)*B_verolie_z/(2*M94))","v":{"$error":"#DIV/0!"}},{"$f":"F94/2*(EXP((B_Verolie_Vw-O94)*B_verolie_z/(2*M94))*(1-fejlfunkk((B_verolie_z*P94-O94*B_Verolie_t)/(2*SQRT(M94*P94*B_Verolie_t))))+EXP((B_Verolie_Vw+O94)*B_verolie_z/(2*M94))*(1-fejlfunkk((B_verolie_z*P94+O94*B_Verolie_t)/(2*SQRT(M94*P94*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q94*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R94*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J94*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N94/(D_VerOlie_ntotal*SQRT(N94*U94))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N94)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F94*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N94*Verolie_z/D_verOlie_Vvel*W94/V94)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F94*(EXP(-D_VerOlie_lambdayear*Verolie_t/N94)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA94^2/N94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AA94)*SQRT(2))))),(IF(AND(AA94>0,AB94=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N94*Verolie_z/D_verOlie_Vvel*W94/V94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AA94)-W94*AA94)*SQRT(2))+EXP(N94*Verolie_z/D_verOlie_Vvel*W94/V94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AA94)+W94*AA94)*SQRT(2)))*F94,IF(AB94>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N94*Verolie_z/D_verOlie_Vvel*W94/V94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AA94)-W94*AA94)*SQRT(2))+EXP(N94*Verolie_z/D_verOlie_Vvel*W94/V94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AA94)+W94*AA94)*SQRT(2)))-(EXP(-N94*Verolie_z/D_verOlie_Vvel*W94/V94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AB94)-W94*AB94)*SQRT(2))+EXP(N94*Verolie_z/D_verOlie_Vvel*W94/V94)*2*NORMSDIST(-(N94*Verolie_z/D_verOlie_Vvel/(2*V94*AB94)+W94*AB94)*SQRT(2))))*F94)))))","v":0},{"$f":"IF(Verolie_t-N94/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N94/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N94/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N94/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q94*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y94*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R94*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z94*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[352,">35 - 44, aromater","Indeno(1,2,3-cd)pyren (C22)",null,null,{"$f":"D_Olie_352_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_352","v":6.7},{"$f":"B_olie_DL_352","v":4.9441211424116288E-6},{"$f":"H95*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H95/10000","v":4.9441211424116287E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J95*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_352","v":3.52611E-5},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I95*((L95*1000)/(8.314*298))+K95*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G95-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M95/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N95*B_verolie_thetaw+B_verolie_thetaa*((L95*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F95*EXP((B_Verolie_Vw-O95)*B_verolie_z/(2*M95))","v":{"$error":"#DIV/0!"}},{"$f":"F95/2*(EXP((B_Verolie_Vw-O95)*B_verolie_z/(2*M95))*(1-fejlfunkk((B_verolie_z*P95-O95*B_Verolie_t)/(2*SQRT(M95*P95*B_Verolie_t))))+EXP((B_Verolie_Vw+O95)*B_verolie_z/(2*M95))*(1-fejlfunkk((B_verolie_z*P95+O95*B_Verolie_t)/(2*SQRT(M95*P95*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q95*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"R95*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$f":"J95*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N95/(D_VerOlie_ntotal*SQRT(N95*U95))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N95)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F95*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N95*Verolie_z/D_verOlie_Vvel*W95/V95)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F95*(EXP(-D_VerOlie_lambdayear*Verolie_t/N95)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA95^2/N95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AA95)*SQRT(2))))),(IF(AND(AA95>0,AB95=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N95*Verolie_z/D_verOlie_Vvel*W95/V95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AA95)-W95*AA95)*SQRT(2))+EXP(N95*Verolie_z/D_verOlie_Vvel*W95/V95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AA95)+W95*AA95)*SQRT(2)))*F95,IF(AB95>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N95*Verolie_z/D_verOlie_Vvel*W95/V95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AA95)-W95*AA95)*SQRT(2))+EXP(N95*Verolie_z/D_verOlie_Vvel*W95/V95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AA95)+W95*AA95)*SQRT(2)))-(EXP(-N95*Verolie_z/D_verOlie_Vvel*W95/V95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AB95)-W95*AB95)*SQRT(2))+EXP(N95*Verolie_z/D_verOlie_Vvel*W95/V95)*2*NORMSDIST(-(N95*Verolie_z/D_verOlie_Vvel/(2*V95*AB95)+W95*AB95)*SQRT(2))))*F95)))))","v":0},{"$f":"IF(Verolie_t-N95/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N95/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N95/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N95/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q95*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y95*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R95*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z95*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[]
[2040,"C21-C35",null,null,null,{"$f":"D_Olie_2040_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(B_VerOlie_Cz_2535+B_VerOlie_cz_201)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_Czt_2535+B_VerOlie_czt_201)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxstat_2535+B_VerOlie_fluxstat_201)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxtrans_2535+B_VerOlie_fluxtrans_201)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(B_VerOlie_DTU_cz_2535+B_VerOlie_DTU_cz_201)","v":0},{"$f":"SUM(B_VerOlie_DTU_czt_2535+B_VerOlie_DTU_czt_201)","v":0},null,null,{"$f":"SUM(B_VerOlie_fluxstat_2535+B_VerOlie_fluxstat_201)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxtrans_2535+B_VerOlie_fluxtrans_201)","v":{"$error":"#DIV/0!"}}]
[]
[20,"Sum af 7 PAH'er jord"]
[21,"Sum af 4 PAH'er vand",null,null,null,{"$f":"SUM(F87+F90+F95)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"B_VerOlie_cz_352+B_VerOlie_cz_255+B_VerOlie_cz_258","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_czt_352+B_VerOlie_czt_255+B_VerOlie_czt_258","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxstat_352+B_VerOlie_fluxstat_255+B_VerOlie_fluxstat_258","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_352+B_VerOlie_fluxtrans_255+B_VerOlie_fluxtrans_258","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"B_VerOlie_DTU_cz_352+B_VerOlie_DTU_cz_255+B_VerOlie_DTU_cz_258","v":0},{"$f":"B_VerOlie_DTU_czt_352+B_VerOlie_DTU_czt_255+B_VerOlie_DTU_czt_258","v":0},null,null,{"$f":"B_VerOlie_fluxstat_352+B_VerOlie_fluxstat_255+B_VerOlie_fluxstat_258","v":{"$error":"#DIV/0!"}},{"$f":"B_VerOlie_fluxtrans_352+B_VerOlie_fluxtrans_255+B_VerOlie_fluxtrans_258","v":{"$error":"#DIV/0!"}}]
[]
[null,"NSO-forbindelser"]
[10,null,"Benzo(b)thiophen",null,null,{"$f":"D_Olie_10_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_10","v":3.12},{"$f":"B_olie_DL_10","v":7.9048861340223873E-6},{"$f":"H103*24*60*60*POWER(B_verolie_thetaa,2.5)/B_verolie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"H103/10000","v":7.9048861340223877E-10},{"$f":"1.1*B_verolie_thetaw*(B_verolie_thetaw-0.039*0.00312^0.52)*(J103*24*60*60)","v":{"$error":"#VALUE!"}},{"$f":"B_olie_kH_10","v":3.267666769230769E-2},{"$f":"(B_Verolie_Vw*B_verolie_alfaLw*B_verolie_thetaw+B_verolie_thetaa*I103*((L103*1000)/(8.314*298))+K103*B_verolie_thetaw)/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"1+(POWER(10,(1.04*G103-0.84))*B_verolie_foc*B_verolie_rhob/B_verolie_thetaw)","v":{"$error":"#VALUE!"}},{"$f":"B_Verolie_Vw*SQRT(1+4*B_verolie_lambda*M103/B_Verolie_Vw^2)","v":{"$error":"#VALUE!"}},{"$f":"(N103*B_verolie_thetaw+B_verolie_thetaa*((L103*1000)/(8.314*298)))/B_verolie_thetaw","v":{"$error":"#VALUE!"}},{"$f":"F103*EXP((B_Verolie_Vw-O103)*B_verolie_z/(2*M103))","v":{"$error":"#DIV/0!"}},{"$f":"F103/2*(EXP((B_Verolie_Vw-O103)*B_verolie_z/(2*M103))*(1-fejlfunkk((B_verolie_z*P103-O103*B_Verolie_t)/(2*SQRT(M103*P103*B_Verolie_t))))+EXP((B_Verolie_Vw+O103)*B_verolie_z/(2*M103))*(1-fejlfunkk((B_verolie_z*P103+O103*B_Verolie_t)/(2*SQRT(M103*P103*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$f":"Q103*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"J103*D_VerOlie_ntotal*60*60*24*365","v":{"$error":"#VALUE!"}},{"$f":"D_verOlie_2bapertur/2*N103/(D_VerOlie_ntotal*SQRT(N103*U103))","v":{"$error":"#VALUE!"}},{"$f":"SQRT(D_VerOlie_lambdayear/N103)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,0,IF(D_verOlie_DTU1a,0,(F103*EXP(D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-N103*Verolie_z/D_verOlie_Vvel*W103/V103)))))","v":0},{"$f":"IF(D_verOlie_AC,0,IF(D_verOlie_DTU2,(F103*(EXP(-D_VerOlie_lambdayear*Verolie_t/N103)-EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*EXP(-D_VerOlie_lambdayear*AA103^2/N103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AA103)*SQRT(2))))),(IF(AND(AA103>0,AB103=0),0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*(EXP(-N103*Verolie_z/D_verOlie_Vvel*W103/V103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AA103)-W103*AA103)*SQRT(2))+EXP(N103*Verolie_z/D_verOlie_Vvel*W103/V103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AA103)+W103*AA103)*SQRT(2)))*F103,IF(AB103>0,0.5*EXP(-D_VerOlie_lambdayear*Verolie_z/D_verOlie_Vvel)*((EXP(-N103*Verolie_z/D_verOlie_Vvel*W103/V103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AA103)-W103*AA103)*SQRT(2))+EXP(N103*Verolie_z/D_verOlie_Vvel*W103/V103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AA103)+W103*AA103)*SQRT(2)))-(EXP(-N103*Verolie_z/D_verOlie_Vvel*W103/V103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AB103)-W103*AB103)*SQRT(2))+EXP(N103*Verolie_z/D_verOlie_Vvel*W103/V103)*2*NORMSDIST(-(N103*Verolie_z/D_verOlie_Vvel/(2*V103*AB103)+W103*AB103)*SQRT(2))))*F103)))))","v":0},{"$f":"IF(Verolie_t-N103/D_verOlie_Vvel*Verolie_z>0,SQRT(Verolie_t-N103/D_verOlie_Vvel*Verolie_z),1E-25)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISTEXT(D_Verolie_a),0,(IF(Verolie_t-(N103/D_verOlie_Vvel*Verolie_z+D_Verolie_a)>0,SQRT(Verolie_t-(N103/D_verOlie_Vvel*Verolie_z+D_Verolie_a)),0)))","v":0},{"$f":"IF(D_verOlie_AC,Q103*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Y103*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}},{"$f":"IF(D_verOlie_AC,R103*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365,Z103*B_verolie_Y*B_verolie_x*B_VerOlie_infiltration*365)","v":{"$error":"#DIV/0!"}}]
[11,null,"Dibenzofuran",null,null,{"$f":"D_Olie_11_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_11","v":4.12},{"$f":"B_olie_DL_11","v":6.3372733653665426E-6},{"$error":"#VALUE!"},6.3372733653665431E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_11","v":1.7893245806451612E-2},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[12,null,"Dibenzothiophen",null,null,{"$f":"D_Olie_12_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_12","v":4.38},{"$f":"B_olie_DL_12","v":6.0547830833864374E-6},{"$error":"#VALUE!"},6.054783083386437E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_12","v":3.4173988095238094E-3},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,null,"Acridin",null,null,{"$f":"D_Olie_13_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_13","v":3.4},{"$f":"B_olie_DL_13","v":6.1392350270271861E-6},{"$error":"#VALUE!"},6.1392350270271863E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_13","v":8.4009375000000007E-5},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[14,null,"Carbazol",null,null,{"$f":"D_Olie_14_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_14","v":2.36},{"$f":"B_olie_DL_14","v":1.2376252771055592E-5},{"$error":"#VALUE!"},1.2376252771055592E-9,{"$error":"#VALUE!"},{"$f":"B_olie_kH_14","v":9.2662208333333337E-6},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,null,"Anilin",null,null,{"$f":"D_Olie_15_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_15","v":0.9},{"$f":"B_olie_DL_15","v":8.5166407345416544E-6},{"$error":"#VALUE!"},8.5166407345416548E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_15","v":1.6859116944444445E-4},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[16,null,"Dimethyldisulfid",null,null,{"$f":"D_Olie_16_cv","v":{"$error":"#DIV/0!"}},{"$f":"B_olie_kow_16","v":1.77},{"$f":"B_olie_DL_16","v":8.468518688960739E-6},{"$error":"#VALUE!"},8.468518688960739E-10,{"$error":"#VALUE!"},{"$f":"B_olie_kH_16","v":0.11932},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$f":"F109/2*(EXP((B_Verolie_Vw-O109)*B_verolie_z/(2*M109))*(1-fejlfunkk((B_verolie_z*P109-O109*B_Verolie_t)/(2*SQRT(M109*P109*B_Verolie_t))))+EXP((B_Verolie_Vw+O109)*B_verolie_z/(2*M109))*(1-fejlfunkk((B_verolie_z*P109+O109*B_Verolie_t)/(2*SQRT(M109*P109*B_Verolie_t)))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,0,{"$error":"#VALUE!"},0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["NSO","Sum af NSO-forbindelser ",null,null,null,{"$f":"SUM(F103:F109)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q103:Q109)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(R103:R109)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S103:S109)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(T103:T109)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(Y103:Y109)","v":0},{"$f":"SUM(Z103:Z109)","v":0},null,null,{"$f":"SUM(AC103:AC109)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AD103:AD109)","v":{"$error":"#DIV/0!"}}]
[]
[1,"Sum af kulbrinter",null,null,null,{"$f":"D_Olie_1_cv","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"D_Gruolie_cg*B_GruOlie_trin2a_Qg_2a","v":{"$error":"#VALUE!"}},{"$f":"(H112+K112)/(B_GruOlie_trin1a_Q0+B_GruOlie_trin2a_Qg_2a)","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"SUM(B_VerOlie_Cz_510+B_VerOlie_Cz_1015+B_VerOlie_Cz_1520+B_VerOlie_cz_201+B_VerOlie_Cz_2535+B_VerOlie_Cz_3540)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_czt_510+B_VerOlie_Czt_1015+B_VerOlie_Czt_1520+B_VerOlie_czt_201+B_VerOlie_Czt_2535+B_VerOlie_Czt_3540)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxstat_510+B_VerOlie_fluxstat_1015+B_VerOlie_fluxstat_1520+B_VerOlie_fluxstat_201+B_VerOlie_fluxstat_2535+B_VerOlie_fluxstat_3540)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxtrans_510+B_VerOlie_fluxtrans_1015+B_VerOlie_fluxtrans_1520+B_VerOlie_fluxtrans_201+B_VerOlie_fluxtrans_2535+B_VerOlie_fluxtrans_3540)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(B_VerOlie_DTU_cz_510+B_VerOlie_DTU_cz_1015+B_VerOlie_DTU_cz_1520+B_VerOlie_DTU_cz_201+B_VerOlie_DTU_cz_2535+B_VerOlie_DTU_cz_3540)","v":0},{"$f":"SUM(B_VerOlie_DTU_czt_510+B_VerOlie_DTU_czt_1015+B_VerOlie_DTU_czt_1520+B_VerOlie_DTU_czt_201+B_VerOlie_DTU_czt_2535+B_VerOlie_DTU_czt_3540)","v":0},null,null,{"$f":"SUM(B_VerOlie_fluxstat_510+B_VerOlie_fluxstat_1015+B_VerOlie_fluxstat_1520+B_VerOlie_fluxstat_201+B_VerOlie_fluxstat_2535+B_VerOlie_fluxstat_3540)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxtrans_510+B_VerOlie_fluxtrans_1015+B_VerOlie_fluxtrans_1520+B_VerOlie_fluxtrans_201+B_VerOlie_fluxtrans_2535+B_VerOlie_fluxtrans_3540)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(B_VerOlie_Cz_50+B_VerOlie_Cz_510+B_VerOlie_Cz_1015+B_VerOlie_Cz_1520+B_VerOlie_cz_201+B_VerOlie_Cz_2535+B_VerOlie_Cz_3540+B_VerOlie_Cz_NSO)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_Czt_50+B_VerOlie_czt_510+B_VerOlie_Czt_1015+B_VerOlie_Czt_1520+B_VerOlie_czt_201+B_VerOlie_Czt_2535+B_VerOlie_Czt_3540+B_VerOlie_Czt_nso)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxstat_50+B_VerOlie_fluxstat_510+B_VerOlie_fluxstat_1015+B_VerOlie_fluxstat_1520+B_VerOlie_fluxstat_201+B_VerOlie_fluxstat_2535+B_VerOlie_fluxstat_3540+B_VerOlie_fluxstat_nso)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxtrans_50+B_VerOlie_fluxtrans_510+B_VerOlie_fluxtrans_1015+B_VerOlie_fluxtrans_1520+B_VerOlie_fluxtrans_201+B_VerOlie_fluxtrans_2535+B_VerOlie_fluxtrans_3540+B_VerOlie_fluxtrans_nso)","v":{"$error":"#DIV/0!"}},null,null,null,null,{"$f":"SUM(B_VerOlie_DTU_cz_50+B_VerOlie_DTU_cz_510+B_VerOlie_DTU_cz_1015+B_VerOlie_DTU_cz_1520+B_VerOlie_DTU_cz_201+B_VerOlie_DTU_cz_2535+B_VerOlie_DTU_cz_3540+B_VerOlie_DTU_cz_NSO)","v":0},{"$f":"SUM(B_VerOlie_DTU_czt_50+B_VerOlie_DTU_czt_510+B_VerOlie_DTU_czt_1015+B_VerOlie_DTU_czt_1520+B_VerOlie_DTU_czt_201+B_VerOlie_DTU_czt_2535+B_VerOlie_DTU_czt_3540+B_VerOlie_DTU_czt_NSO)","v":0},null,null,{"$f":"SUM(B_VerOlie_fluxstat_50+B_VerOlie_fluxstat_510+B_VerOlie_fluxstat_1015+B_VerOlie_fluxstat_1520+B_VerOlie_fluxstat_201+B_VerOlie_fluxstat_2535+B_VerOlie_fluxstat_3540+B_VerOlie_fluxstat_nso)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B_VerOlie_fluxtrans_50+B_VerOlie_fluxtrans_510+B_VerOlie_fluxtrans_1015+B_VerOlie_fluxtrans_1520+B_VerOlie_fluxtrans_201+B_VerOlie_fluxtrans_2535+B_VerOlie_fluxtrans_3540+B_VerOlie_fluxtrans_nso)","v":{"$error":"#DIV/0!"}}]
[]
[null,null,"SprækkeTransport - DTU-V1D-remtec"]
[]
[]
[null,null,"DTU Model 1a og 1b og C"]
[]
[null,null,"Presence of fractures",null,"yes"]
[null,null,{"$f":"IF(E120=\"yes\",\"\",\"Advection in low-permeability media (yes/no)\")","v":""}]
[null,null,"If initially contaminated (yes/no)",null,{"$f":"IF(D_verOlie_DTU2,\"yes\",\"no\")","v":"no"}]
[]
[]
[]
[null,null,"INPUT"]
[null,null,"BOX 1: General Input"]
[]
[null,null,"Input concentration",null,"stofafhængig","Se oven: Overført fra oliestoffer",null,null,"D_Olie_xx_cv"]
[null,null,"Matrix porosity","f",{"$f":"D_VerOlie_ntotal","v":{"$error":"#VALUE!"}},{"$f":"D_Verolie_jord","v":0},null,null,"D_VerOlie_ntotal  ","input  fra jordparametre og defineret i dataark"]
[null,null,"Diffusion coefficient in matrix","Dm (m2/year)","stofafhængig","Se oven: beregnes for hver stofgruppe"]
[null,null,"Degradation rate","l (dag-1)",{"$f":"D_Verolie_lambda","v":0},"Bruger data - standard for alle stofgrupper",null,null,"D_VerOlie_lambda","input fra Vertikal transport-olie"]
[null,null,"Degradation rate","l (year-1)",{"$f":"D_Verolie_lambda*365","v":0},"Omregnet til (år-1)",null,null,"B_Ver_lambdayear","enhederne omregnes"]
[null,null,"Retardation, fracture","Rf","stofafhængig","lige med Rm","jf. Chambon et al.J. of contaminant Hydrology 124 (2011),82-98",null,"D_VerOlie_R_xX","B_VerOlie_R_xx beregnes ovenover i Domenico for hver stofgruppe"]
[null,null,"Retardation, matrix","Rm","stofafhængig","stof afhængig beregnes",null,null,"D_VerOlie_R_xx","B_VerOlie_R_xx beregnes ovenover i Domenico for hver stofgruppe"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_verOlie_2bapertur","v":7.9418567312567668E-5}]
[null,null,"Water velocity","vf (m/year)",{"$f":"D_verOlie_2bapertur^2*1000*9.81/(12*0.0013)*D_verOlie_Vgrad*3600*24*365","v":{"$error":"#VALUE!"}},null,null,null,"D_VerOlie_Vvel","Beregnes"]
[null,null,"Average velocity in EPM","vEPM (m/year)",{"$f":"D_verolie_Kb*D_verOlie_Vgrad*3600*24*365/D_VerOlie_ntotal","v":{"$error":"#VALUE!"}},null,null,null,"B_verOlie_EPM","Beregnes"]
[null,null,"Longitudinal dispersivity","α (m)",{"$f":"D_Verolie_alfaLw","v":9.9999999999999994E-37},null,null,null,"D_VerOlie_alfaLw","input"]
[null,null,"Spill time","a (year)",{"$f":"IF(VerOlie_a>0,VerOlie_a,\"constant\")","v":"constant"},null,null,null,"Verolie_a","input"]
[]
[null,null,"BOX 2: Hydrogeological properties"]
[null,null,"calculated using from Box 3"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_verolie_2B","v":5}]
[null,null,"Fracture aperture","2*b (m)",{"$f":"(D_verolie_Kb*12*0.0013*D_verolie_2B/(1000*9.81))^(1/3)","v":7.9418567312567668E-5},null,null,null,"B_verOlie_2bapertur","Beregnes"]
[null,null,"Bulk hydrualic conductivity","Kb (m/s)",{"$f":"D_verolie_Kb","v":6.2999999999999995E-8}]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_verolie_inf","v":""},null,null,null,"D_VerOlie_inf","input"]
[null,null,"Vertical gradient","i (-)",{"$f":"D_verolie_inf/1000/3600/24/365/D_verolie_Kb","v":{"$error":"#VALUE!"}},null,null,null,"B_VerOlie_Vgrad","Beregnes"]
[]
[null,null,"BOX 3: Specific Input depending on conceptual model"]
[null,null,"Fracture spacing","2*B (m)",{"$f":"D_verolie_2B","v":5},null,null,null,"D_VerOlie_2B","input"]
[null,null,"Fracture aperture","2*b (m)",{"$f":"D_verOlie_2bapertur","v":7.9418567312567668E-5}]
[null,null,"Bulk hydraulic conductivity","Kb (m/s)",{"$f":"D_verolie_Kb","v":6.2999999999999995E-8},null,null,null,"D_VerOlie_Kb","Input"]
[null,null,"Infiltration","I (mm/year)",{"$f":"D_verolie_inf","v":""},null,null,null,"D_verOlie_inf","input"]
[null,null,"Vertical gradient","i (-)",{"$f":"B_verOlie_Vgrad","v":{"$error":"#VALUE!"}}]
[]
[null,null,"BOX 4: Calculated Parameters-"]
[null,null,"A",null,"stofafhængig",null,null,null,null,"Beregnes"]
[null,null,"B ",null,"stofafhængig",null,null,null,null,"Beregnes"]
[null,null,"G",null,"stofafhængig",null,null,null,null,"Beregnes"]
[]
[null,null,"BOX 5: Calculation and graphic parameters"]
[null,null,"Time increment","(year)",null,"Udgør , da ingen figurer"]
[null,null,"Depth increment","(m)",null,"Udgør , da ingen figurer"]
[null,null,"Time plot",null,null,"Udgør , da ingen figurer"]
[null,null,"Time","t (year)",{"$f":"Verolie_t","v":0},null,null,null,"VerOlie_t","input"]
[null,null,"Depth","z(m)",{"$f":"Verolie_z","v":0},null,null,null,"VerOlie_z","input"]

{"sheet":"Vejledning_Vertikal-Olie","index":57,"n_rows":153,"n_cols":2,"rows_kept":153,"cut":false,"hidden":true,"merged":[[152,1,153,15],[123,1,133,15],[134,1,134,15],[135,1,135,15],[136,1,137,15],[138,1,138,15],[139,1,139,15],[140,1,142,15],[144,1,144,15],[145,1,149,15],[150,1,150,15],[151,1,151,15],[122,1,122,15],[94,1,94,15],[95,1,95,15],[96,1,98,14],[99,1,99,15],[101,1,106,15],[107,1,107,15],[108,1,108,15],[109,1,110,15],[111,1,111,15],[112,1,120,15],[121,1,121,15],[79,1,93,15],[1,1,1,15],[43,1,43,15],[65,1,65,15],[66,1,71,15],[72,1,72,15],[73,1,73,15],[74,1,76,15],[77,1,77,15],[78,1,78,15],[45,1,63,15],[2,1,9,15]]}
[null,"Vejledning - Vertikal transport"]
[null,"Formål"]
[null,"I dette regneark kan der foretages en beregning af vertikal transport og evt. nedbrydning igennem enten et homogent jordlag eller sprækker i moræneler og ned til det førstkommende betydende grundvandsmagasin. Vertikal transport i et homogent jordlag er baseret på beregninger for konceptuel model A og C, beskrevet i Miljøprojektet om vertikal transport ned til det førstkommende betydende magasin. Beregninger af vertikal transport i vandmættet sprækket ler – konceptuel model B - er baseret på DTU V1D model. DTU Miljø. Manual. DTU V1D – DTU Vertical 1D Transport Model. A spreadsheet for risk assessment in low-permeability media. http://www.sara.env.dtu.dk/Modelvaerktoejer."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEREGNINGER"]
[null,"Valg af model"]
[null,"Der kan vælges imellem 4 forskellige beregningsmodeller for vertikal transport af organiske stoffer igennem et jordlag og ned til førstkommende grundvandsmagasin.\n\nFor model A eller C er der tale om en kontinuer kilde, som nedsives igennem et homogent vandmættet ler eller et umættet sand- eller lerlag. Da kildekoncentrationen er kontinuert (ikke aftager) vil der med tiden opnås stationære forhold, og koncentrationen lige over grundvandet vil være lig kildekoncentrationen, med mindre der sker nedbrydning under transport.\n \nFor DTUV1D model 1a er der en kendt spildperiode, hvorefter kildekoncentrationen aftager og  koncentrationen lige over grundvandsspejlet ligeledes vil aftage med tiden. Der skal kun indtastes varighed af spild, såfremt der vælges Model B- DTU V1D model1a.\n\nFor DTUV1D model 1b er der tale om en kontinuert kilde, som nedsives igennem en sprækket vandmættet ler. Da kildekoncentrationen er kontinuert (ikke aftager) vil der med tiden opnås stationære forhold og koncentrationen lige over grundvandet vil være lig kildekoncentrationen, med mindre der sker nedbrydning under transport.\n\nFor DTUV1D model 2 er der tale om en aftagende kilde, idet der antages, at forureningskilden er ophørt, og nedsivningen styres af diffusion fra matrix til sprækker og herefter igennem den sprækkede vandmættede ler."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Kildeområde:"]
[null,"Længden x og bredden y af kilden, hvorfra nedsivning sker, skal angives.\nz er afstanden fra bunden af kilden til grundvandsspejlet dvs. svarende til tykkelsen af det homogene jordlag (enten mættet ler eller umættet sand og ler). \nDer skal enten vælges nedbørsdata fra standardlisten ved at vælge det geografiske område, som forureningen er beliggende i, eller indtastes nye værdier. Det er også muligt at anvende og oprette egne nedbørsdata ved at klikke på knappen \"Egen liste\"."]
[]
[]
[]
[]
[]
[]
[null,"Jordtype:"]
[null,"Jordtypen i den umættede zone skal enten vælges som standardjordtyper fra listen (klik på \"Jordtype\") eller indtaste egne værdier. Egne jordtyper kan oprettes svarende til for nedbørsdata. OBS: For mættede forhold bør VV sættes til maks. porøsitet og VL til nul."]
[]
[]
[]
[null,"Forurening:"]
[null,"Forureningsdata for porevand overføres fra \"Enkeltstoffer\". Hvis der i dette ark er indtastet en målt grundvandskoncentration, indtastes denne, ellers overføres vandkoncentrationen beregnet ud fra en jordkoncentration eller alternativt en indtastet poreluftkoncentration. Der kan også indtastes værdier direkte i de hvide felter. Af udskriften vil det så fremgå, at der ikke er anvendt målte værdier. \n\nHerudover skal der vælges nedbrydningsforhold (aerobe eller anaerobe). Nedbrydningskonstanter for nedbrydning i den umættede zone hentes fra kemiske data i \"Enkeltstoffer\", hvor det er muligt at indsætte andre værdier, såfremt standardværdier fra databasen ikke ønskes anvendt. Standardværdier er af Miljøstyrelsen defineret som nul, dvs. at der i standardberegninger ikke antages at foregå nedbrydning under den vertikale transport.  Beregninger uden nedbrydning viser dermed at koncentrationen i det førstkommende betydende magasin under stationære forhold vil være lig porevandskoncentrationen.\n\nDer kan indsættes en tid, t (år) og beregne de transiente porevandskoncentrationer lige over grundvandspejl efter tid, t. Desuden vises udvikling i de transiente porevandkoncentrationer i forskellige dybder igennem den umættede zone med tiden på en figur."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GENERELT"]
[null,"Hvis der er anført værdier i de hvide felter vil beregningen altid blive foretaget med disse. \nVed at klikke på Knappe \"Bemærkninger\" er det muligt at indføre oplysninger om hvorfor der er valgt andre værdier end standardværdierne"]
[]
[]
[]
[null,"OVERFØR VÆRDIER:"]
[null,"Knappen anvendes til at overføre data fra det ark man står i til det tilsvarende ark under Enkeltstof-modulet, således at data kun skal indtastes en gang.\nDet er kun data om f.eks. akvifermateriale og bygningsdata som overføres. Data om stoffer og koncen-trationer overføres ikke.\nHvis der allerede er indtastet data i til det tilsvarende ark under Enkeltstof-modulet, så vil disse data blive slettet og erstattet af de data som overføres."]
[]
[]
[]
[]
[]
[]
[null,"ANVENDELSEN AF LISTEVÆRDIER"]
[null,"Der findes i JAGG 2.0 to typer af listeværdier: Standardlisteværdier, hvis indhold er godkendt af Miljøstyrelsen, og listeværdier med brugerens egne indtastede værdier."]
[]
[]
[null,"Når en Standardværdiliste er åbnet er der mulighed for følgende operationer:\n· At navigere ned gennem listen ved at anvende rullebjælken\n· At sortere forekomsterne ved at klikke på sorteringsknapperne\n· At vælge en forekomst ved at klikke på den ønskede værdi og herefter klikke [OK], eller ved at dobbeltklikke på den ønskede værdi\n· At vælge en forekomst ved at skrive dens navn i søgefeltet og herefter klikke [OK]\n· At fortryde og lukke standardlisten ved at klikke [Fortryd]\n· At slette en valgt forekomst ved at sætte flueben ved \"Nulstil systemværdier\" /\"Nulstil indtastede værdier\"\n· At slette indtastede værdier"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"BEMÆRKNINGER:"]
[null,"Der er mulighed for at indtaste bemærkninger til de valgte date. Bemærkningerne knytter sig normalt til et dataområde, f.eks. jordforhold, kemiske stoffer, og beregninger.\n\nBemærkninger indtastes ved at klikke på bemærkningsfeltet. Et bemærkningsfelt kan maksimalt indeholde 500 tegn. \nHvis der er indtastet data i et bemærkningsfelt skifter knappen farve fra mørkeblå til lyseblå.\n\nNår bemærkningsfeltet er åbent er der mulighed for følgende operationer: \n[OK] Den indtastede tekst gemmes\n[Fortryd] Bemærkningsfeltet lukkes uden at gemme ændringer\n[Slet tekst] Alt tekst i bemærkningsfeltet slettes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NULSTIL VÆRDIER:"]
[null,"Den røde knap [Nulstil værdier] sletter alle indtastede værdier i dette ark, både data til beregninger og data i bemærkningsfelter."]
[]
[]
[null,"SLETNING AF ENKELTVÆRDIER:"]
[null,"Værdier der fremkommet fra valglister kan slettes / nulstilles ved at åbne valglisten igen, og sætte flueben i feltet  “Nulstil systemværdier” og herefter klikke \"OK\". Dette gælder både for systemvalglister og Egne lister."]
[]
[]
[]
[null,"UDSKRIV VÆRDIER:"]
[null,"Der er udarbejdet et særskilt udskriftsark, hvor data er tilpasset A4 formatet. Udskriftarket åbnes ved at klikke på knappen [Udskrift]. Udskriftsarket åbnes som en form for \"vis udskrift\".\n\nUdover at vise data er udskriftarket også indrettet så der med rødt markers hvis der mangler vitale oplysninger for at beregningerne kan gennemføres."]
[]
[]
[]
[]
[]
[null,"DATAARKET:"]
[null,"Dataarket viser alle data der indgår i beregningerne inkl. resultat af mellemberegninger."]

{"sheet":"Udskrift_Vertikal-Olie","index":58,"n_rows":105,"n_cols":12,"rows_kept":105,"cut":false,"hidden":true,"merged":[[5,1,5,10],[3,8,3,10],[2,1,2,5],[3,1,3,5],[4,1,4,5],[4,8,4,10],[2,8,2,10],[63,9,63,10],[36,9,37,10],[44,4,44,5],[44,6,44,7],[44,9,44,10],[63,6,63,7],[38,9,38,10],[40,9,40,10],[41,9,41,10],[42,9,42,10],[43,9,43,10],[45,9,45,10],[48,9,48,10],[49,9,49,10],[50,9,50,10],[51,9,51,10],[55,9,55,10],[48,4,48,5],[49,4,49,5],[50,4,50,5],[51,4,51,5],[52,4,52,5],[55,4,55,5],[60,4,60,5],[63,4,63,5],[48,6,48,7],[49,6,49,7],[50,6,50,7],[60,6,60,7],[58,4,58,5],[58,6,58,7],[59,4,59,5],[60,9,60,10],[51,6,51,7],[52,6,52,7],[55,6,55,7],[59,6,59,7],[59,9,59,10],[103,1,116,9],[73,1,86,9],[88,1,101,9],[52,9,52,10],[58,9,58,10],[39,13,39,15],[34,2,34,3],[34,4,34,5],[34,6,34,7],[34,8,34,9],[13,2,13,3],[13,4,13,5],[15,4,15,5],[17,2,17,3],[17,4,17,5],[15,2,15,3],[18,2,18,3],[18,4,18,5],[21,2,21,3],[21,4,21,5],[22,2,22,3],[22,4,22,5],[26,2,26,3],[26,4,26,5],[30,2,30,3],[30,4,30,5],[33,2,33,3],[33,4,33,5],[23,2,23,3],[7,0,7,1],[9,4,9,5],[10,4,10,5],[12,2,12,3],[12,4,12,5],[9,2,9,3],[10,2,10,3],[23,4,23,5],[24,2,24,3],[24,4,24,5],[33,8,33,9],[39,5,39,6],[36,4,36,5],[38,4,38,5],[36,6,36,7],[38,6,38,7],[40,4,40,5],[41,4,41,5],[42,4,42,5],[29,4,29,5],[25,2,25,3],[25,4,25,5],[40,6,40,7],[41,6,41,7],[42,6,42,7],[43,6,43,7],[45,6,45,7],[33,6,33,7],[43,4,43,5],[45,4,45,5],[27,2,27,3],[27,4,27,5],[28,2,28,3],[28,4,28,5],[29,2,29,3]]}
["Vertikal transport - oliestoffer"]
["Lokaliteten"]
["Navn:",{"$f":"Lok_navn","v":""},null,null,null,null,null,"Lokalitetsnr.:",{"$f":"Lok_Loknr","v":""}]
["Adresse:",{"$f":"Lok_adr","v":""},null,null,null,null,null,"Postnr/by:",{"$f":"Lok_postnr","v":""}]
["Matrikel nr.:",{"$f":"Lok_matr","v":""},null,null,null,null,null,"Projekt nr.:",{"$f":"Lok_projekt","v":""}]
["Note",{"$f":"Lok_note","v":""}]
[]
["Kildeområde",null,null,null,null,null,null,"Kommentar",null,{"$f":"IF(D_VerOlie_Kil_ComUds,\"ja\",\"nej\")","v":"nej"}]
[null,null,"Standard data",null,"Indtastede data (angives med fed)"]
["Længde af kildeområde","Y",null,null,{"$f":"IF(D_Verolie_Y<>\"\",D_Verolie_Y,\"\")","v":0},null,"m"]
["Bredde af kildeområde","x",null,null,{"$f":"IF(D_Verolie_X<>\"\",D_Verolie_X,\"\")","v":0},null,"m"]
[]
["Nettonedbør","N",{"$f":"IF(D_VerOlie_infiltration_syst<>\"\",D_VerOlie_infiltration_syst,\"\")","v":""},null,{"$f":"IF(Verolie_My_N<>\"\",Verolie_My_N,\"\")","v":""},null,"mm/år"]
["Kommune/Egn",null,{"$f":"IF(D_Ver_Egn_syst<>\"\",D_Ver_Egn_syst,\"\")","v":""},null,{"$f":"IF(Ver_My_Egn<>\"\",Ver_My_Egn,\"\")","v":""}]
[]
["Afstand til grundvandsspejl","Z",null,null,{"$f":"IF(D_Verolie_z<>\"\",D_Verolie_z,\"\")","v":0},null,"m",null,null,"Beregnet porevandshastighed",{"$f":"D_verolie_Vw_year","v":""},"m/år"]
[]
["Longitudinal dispersivitet","αL,W",{"$f":"IF(D_verolie_alfaLw_beregn<>\"\",D_verolie_alfaLw_beregn,\"\")","v":9.9999999999999994E-37},null,{"$f":"IF(Verolie_alfaLw<>\"\",Verolie_alfaLw,\"\")","v":""}]
["Varighed af spild","a",null,null,{"$f":"D_Verolie_a","v":"Vedvarende"},null,null,"Kun for Model B DTU V1D"]
[]
["Jordparametre",null,null,null,null,null,null,"Kommentar",null,{"$f":"IF(D_Verolie_jord_ComUds,\"ja\",\"nej\")","v":"nej"}]
["Jordtype",null,{"$f":"IF(D_Verolie_jord<>\"\",D_Verolie_jord,\"\")","v":0},null,{"$f":"IF(Verolie_My_jord<>\"\",Verolie_My_jord,\"\")","v":""}]
["Vandindhold","qw",{"$f":"IF(D_VerOlie_thetaw_syst<>\"\",D_VerOlie_thetaw_syst,\"\")","v":""},null,{"$f":"IF(Verolie_My_VV<>\"\",Verolie_My_VV,\"\")","v":""}]
["Luftindhold","qa",{"$f":"IF(D_VerOlie_thetaa_syst<>\"\",D_VerOlie_thetaa_syst,\"\")","v":""},null,{"$f":"IF(Verolie_My_VL<>\"\",Verolie_My_VL,\"\")","v":""}]
["Total porøsitet (VL+VV)","n",{"$f":"D_VerOlie_ntotal","v":{"$error":"#VALUE!"}}]
["% organisk indhold","foc",{"$f":"IF(D_VerOlie_foc_syst<>\"\",D_VerOlie_foc_syst,\"\")","v":""},null,{"$f":"IF(Verolie_My_foc<>\"\",Verolie_My_foc,\"\")","v":""}]
["Bulkmassefylde","r",{"$f":"IF(D_Verolie_rhob<>\"\",D_Verolie_rhob,\"\")","v":{"$error":"#VALUE!"}},null,null,null,"kg/l"]
["Sprækkeafstand (2B)","2B",{"$f":"IF(VerOlie_2B<>\"\",VerOlie_2B,\"\")","v":5},null,{"$f":"IF(VerOlie_My_2B<>\"\",VerOlie_My_2B,\"\")","v":""},null,"m","Kun hvis sprækketransport"]
["Sprækkeapertur (2b)","2b",{"$f":"IF(D_verOlie_2bapertur<>\"\",D_verOlie_2bapertur,\"\")","v":7.9418567312567668E-5},null,null,null,"m","Kun hvis sprækketransport"]
["Bulk-hydraulisk ledningsevne","Kb",{"$f":"IF(VerOlie_Kb<>\"\",VerOlie_Kb,\"\")","v":6.2999999999999995E-8},null,{"$f":"IF(VerOlie_My_Kb<>\"\",VerOlie_My_Kb,\"\")","v":""},null,"m/s","Kun hvis sprækketransport"]
[]
["Beregning: Vertikal transport",null,null,null,null,null,null,"Kommentar",null,{"$f":"IF(D_Verolie_ber_ComUds,\"ja\",\"nej\")","v":"nej"}]
[]
[{"$f":"D_Verolie_model","v":"Model A + C"},null,"Målepunkt",null,"Dato",null,"Fri fase?",null,"Anvendt brugerdata"]
["Angiv signifikant ciffer",3,{"$f":"IF(Olie_målepunkt<>\"\",D_olie_målepunkt,\"\")","v":""},null,{"$f":"IF(Olie_dato<>\"\",D_olie_dato,\"\")","v":""},null,{"$f":"Olie_frifase","v":"Nej"},null,{"$f":"D_gruolie_bruger","v":"Nej"}]
[]
[null,null,"Pore-\nvands\nkonc.","Nedbryd-nings\nkonstant","Stationær porevandskonc. i toppen af GV magasin",null,"Transient porevandskonc. i toppen af GV magasin efter",null,"Grund\nvands-\nkriterium","Over-\nskridelse \naf kriteriet (stationær forhold)"]
[null,null,null,null,null,null,{"$f":"Verolie_t","v":0},"år"]
[null,null,"µg/l","dage-1","µg/l",null,"µg/l",null,"µg/l","gange"]
["BTEX'er"]
["Benzen",null,{"$f":"IF(D_verolie_cv_52>0,ROUND(D_verolie_cv_52,3-(INT(LOG(D_verolie_cv_52))+1)),D_verolie_cv_52)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_52),IF(D_Verolie_Cz_52>0,ROUND(D_Verolie_Cz_52,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_52))+1)),D_Verolie_Cz_52),D_Verolie_Cz_52)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_52>0,ROUND(D_Verolie_Czt_52,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_52))+1)),D_Verolie_Czt_52))","v":""},null,{"$f":"D_verolie_gkk_52","v":1},{"$f":"D_VerOlie_overskr_52","v":""}]
["Toluen",null,{"$f":"IF(D_verolie_cv_54>0,ROUND(D_verolie_cv_54,3-(INT(LOG(D_verolie_cv_54))+1)),D_verolie_cv_54)","v":{"$error":"#DIV/0!"}},0,{"$f":"IF(ISNUMBER(D_Verolie_Cz_54),IF(D_Verolie_Cz_54>0,ROUND(D_Verolie_Cz_54,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_54))+1)),D_Verolie_Cz_54),D_Verolie_Cz_54)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_54>0,ROUND(D_Verolie_Czt_54,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_54))+1)),D_Verolie_Czt_54))","v":""},null,{"$f":"D_verolie_gkk_54","v":5},{"$f":"D_VerOlie_overskr_54","v":""}]
["Ethylbenzen",null,{"$f":"IF(D_verolie_cv_58>0,ROUND(D_verolie_cv_58,3-(INT(LOG(D_verolie_cv_58))+1)),D_verolie_cv_58)","v":{"$error":"#DIV/0!"}},0,{"$f":"IF(ISNUMBER(D_Verolie_Cz_58),IF(D_Verolie_Cz_58>0,ROUND(D_Verolie_Cz_58,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_58))+1)),D_Verolie_Cz_58),D_Verolie_Cz_58)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_58>0,ROUND(D_Verolie_Czt_58,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_58))+1)),D_Verolie_Czt_58))","v":""}]
["Sum Xylener",null,{"$f":"IF(D_verolie_cv_57>0,ROUND(D_verolie_cv_57,3-(INT(LOG(D_verolie_cv_57))+1)),D_verolie_cv_57)","v":{"$error":"#DIV/0!"}},0,{"$f":"IF(ISNUMBER(D_Verolie_Cz_57),IF(D_Verolie_Cz_57>0,ROUND(D_Verolie_Cz_57,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_57))+1)),D_Verolie_Cz_57),D_Verolie_Cz_57)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_57>0,ROUND(D_Verolie_Czt_57,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_57))+1)),D_Verolie_Czt_57))","v":""}]
["Sum Xylener+ethylbenzen",null,{"$f":"IF(D_VerOlie_cv_57_58>0,ROUND(D_VerOlie_cv_57_58,3-(INT(LOG(D_VerOlie_cv_57_58))+1)),D_VerOlie_cv_57_58)","v":{"$error":"#DIV/0!"}},0,{"$f":"IF(ISNUMBER(D_VerOlie_cz_57_58),IF(D_VerOlie_cz_57_58>0,ROUND(D_VerOlie_cz_57_58,Verolie_ciffer-(INT(LOG(D_VerOlie_cz_57_58))+1)),D_VerOlie_cz_57_58),D_VerOlie_cz_57_58)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_VerOLie_czt_57_58>0,ROUND(D_VerOLie_czt_57_58,Verolie_ciffer-(INT(LOG(D_VerOLie_czt_57_58))+1)),D_VerOLie_czt_57_58))","v":""},null,{"$f":"D_verolie_gkk_57","v":5},{"$f":"D_VerOlie_overskr_57","v":""}]
["Naphthalen",null,{"$f":"IF(D_verolie_cv_103>0,ROUND(D_verolie_cv_103,3-(INT(LOG(D_verolie_cv_103))+1)),D_verolie_cv_103)","v":{"$error":"#DIV/0!"}},0,{"$f":"IF(ISNUMBER(D_Verolie_Cz_103),IF(D_Verolie_Cz_103>0,ROUND(D_Verolie_Cz_103,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_103))+1)),D_Verolie_Cz_103),D_Verolie_Cz_103)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_103>0,ROUND(D_Verolie_Czt_103,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_103))+1)),D_Verolie_Czt_103))","v":""},null,{"$f":"D_verolie_gkk_103","v":1},{"$f":"D_VerOlie_overskr_103","v":""}]
[]
["Kulbrintefraktioner"]
["C6-C10 ",null,{"$f":"IF(D_verolie_cv_510>0,ROUND(D_verolie_cv_510,3-(INT(LOG(D_verolie_cv_510))+1)),D_verolie_cv_510)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_510),IF(D_Verolie_Cz_510>0,ROUND(D_Verolie_Cz_510,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_510))+1)),D_Verolie_Cz_510),D_Verolie_Cz_510)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_510>0,ROUND(D_Verolie_Czt_510,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_510))+1)),D_Verolie_Czt_510))","v":""}]
["C10-C15 ",null,{"$f":"IF(D_verolie_cv_1015>0,ROUND(D_verolie_cv_1015,3-(INT(LOG(D_verolie_cv_1015))+1)),D_verolie_cv_1015)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_1015),IF(D_Verolie_Cz_1015>0,ROUND(D_Verolie_Cz_1015,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_1015))+1)),D_Verolie_Cz_1015),D_Verolie_Cz_1015)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_1015>0,ROUND(D_Verolie_Czt_1015,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_1015))+1)),D_Verolie_Czt_1015))","v":""}]
["C15-C20 ",null,{"$f":"IF(D_verolie_cv_1520>0,ROUND(D_verolie_cv_1520,3-(INT(LOG(D_verolie_cv_1520))+1)),D_verolie_cv_1520)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_1520),IF(D_Verolie_Cz_1520>0,ROUND(D_Verolie_Cz_1520,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_1520))+1)),D_Verolie_Cz_1520),D_Verolie_Cz_1520)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_1520>0,ROUND(D_Verolie_Czt_1520,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_1520))+1)),D_Verolie_Czt_1520))","v":""}]
["C20-C35",null,{"$f":"IF(D_verolie_cv_2040>0,ROUND(D_verolie_cv_2040,3-(INT(LOG(D_verolie_cv_2040))+1)),D_verolie_cv_2040)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_2040),IF(D_Verolie_Cz_2040>0,ROUND(D_Verolie_Cz_2040,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_2040))+1)),D_Verolie_Cz_2040),D_Verolie_Cz_2040)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_2040>0,ROUND(D_Verolie_Czt_2040,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_2040))+1)),D_Verolie_Czt_2040))","v":""}]
["Sum af kulbrinter",null,{"$f":"IF(D_verolie_cv_1>0,ROUND(D_verolie_cv_1,3-(INT(LOG(D_verolie_cv_1))+1)),D_verolie_cv_1)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_1),IF(D_Verolie_Cz_1>0,ROUND(D_Verolie_Cz_1,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_1))+1)),D_Verolie_Cz_1),D_Verolie_Cz_1)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_1>0,ROUND(D_Verolie_Czt_1,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_1))+1)),D_Verolie_Czt_1))","v":""},null,{"$f":"D_verolie_gkk_1","v":9},{"$f":"D_VerOlie_overskr_1","v":""}]
[]
["Alkylbenzener"]
["C9-C10 aromatiske kulbrinter",null,{"$f":"IF(D_Verolie_910_cv>0,ROUND(D_Verolie_910_cv,3-(INT(LOG(D_Verolie_910_cv))+1)),D_Verolie_910_cv)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_cz_910),IF(D_Verolie_cz_910>0,ROUND(D_Verolie_cz_910,Verolie_ciffer-(INT(LOG(D_Verolie_cz_910))+1)),D_Verolie_cz_910),D_Verolie_cz_910)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_verolie_czt_910>0,ROUND(D_verolie_czt_910,Verolie_ciffer-(INT(LOG(D_verolie_czt_910))+1)),D_verolie_czt_910))","v":""},null,{"$f":"D_verolie_gkk_910","v":1},{"$f":"D_VerOlie_overskr_910","v":""}]
[]
["Polyaromatiske Kulbrinter (PAH)"]
["Fluoranthen",null,{"$f":"IF(D_verolie_cv_156>0,ROUND(D_verolie_cv_156,3-(INT(LOG(D_verolie_cv_156))+1)),D_verolie_cv_156)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_verolie_Cz_156),IF(D_verolie_Cz_156>0,ROUND(D_verolie_Cz_156,Verolie_ciffer-(INT(LOG(D_verolie_Cz_156))+1)),D_verolie_Cz_156),D_verolie_Cz_156)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_156>0,ROUND(D_Verolie_Czt_156,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_156))+1)),D_Verolie_Czt_156))","v":""},null,{"$f":"D_verolie_gkk_156","v":0.1},{"$f":"D_VerOlie_overskr_156","v":""}]
["Benzo(a)pyren",null,{"$f":"IF(D_verolie_cv_256>0,ROUND(D_verolie_cv_256,3-(INT(LOG(D_verolie_cv_256))+1)),D_verolie_cv_256)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_256),IF(D_Verolie_Cz_256>0,ROUND(D_Verolie_Cz_256,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_256))+1)),D_Verolie_Cz_256),D_Verolie_Cz_256)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_256>0,ROUND(D_Verolie_Czt_256,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_256))+1)),D_Verolie_Czt_256))","v":""},null,{"$f":"D_verolie_gkk_256","v":0.01},{"$f":"D_VerOlie_overskr_256","v":""}]
["Sum af 4 PAH`er",null,{"$f":"IF(D_verolie_cv_21>0,ROUND(D_verolie_cv_21,3-(INT(LOG(D_verolie_cv_21))+1)),D_verolie_cv_21)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_21),IF(D_Verolie_Cz_21>0,ROUND(D_Verolie_Cz_21,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_21))+1)),D_Verolie_Cz_21),D_Verolie_Cz_21)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_21>0,ROUND(D_Verolie_Czt_21,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_21))+1)),D_Verolie_Czt_21))","v":""},null,{"$f":"D_verolie_gkk_21","v":0.1},{"$f":"D_VerOlie_overskr_21","v":""}]
[]
["NSO-forbindelser"]
["Sum af NSO-forbindelser",null,{"$f":"IF(D_verolie_cv_nso>0,ROUND(D_verolie_cv_nso,3-(INT(LOG(D_verolie_cv_nso))+1)),D_verolie_cv_nso)","v":{"$error":"#DIV/0!"}},{"$f":"D_Verolie_lambda","v":0},{"$f":"IF(ISNUMBER(D_Verolie_Cz_nso),IF(D_Verolie_Cz_nso>0,ROUND(D_Verolie_Cz_nso,Verolie_ciffer-(INT(LOG(D_Verolie_Cz_nso))+1)),D_Verolie_Cz_nso),D_Verolie_Cz_nso)","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(Verolie_t=0,\"\",IF(D_Verolie_Czt_nso>0,ROUND(D_Verolie_Czt_nso,Verolie_ciffer-(INT(LOG(D_Verolie_Czt_nso))+1)),D_Verolie_Czt_nso))","v":""}]
[]
["Beregningerne udført af",null,null,null,null,null,null,null,null,null,"Beregningerne kontrolleret /godkendt af"]
["Firmanavn",{"$f":"IF(Lok_firma<>\"\",Lok_firma,\"\")","v":""},null,null,null,null,"Kontrolleret"]
["Navn/initialer",{"$f":"Lok_init","v":""},null,null,null,null,"Godkendt"]
["Dato/Underskrift"]
[]
["Beregningerne er udført med de ovenfor angivne data og uden at der er foretaget ændringer af beregningsformler."]
[]
[]
["Bemærkninger",{"$f":"IF(D_VerOlie_Kil_Com <> \"\", D_VerOlie_Kil_Com, \"\")","v":""}]
["om kildeområde"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_Verolie_jord_com <> \"\", D_Verolie_jord_com, \"\")","v":""}]
["om jordparametre"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Bemærkninger",{"$f":"IF(D_verolie_ber_com <> \"\", D_verolie_ber_com, \"\")","v":""}]
["om beregning"]

{"sheet":"Aquifermateriale","index":59,"n_rows":16,"n_cols":11,"rows_kept":16,"cut":false,"hidden":true,"merged":[[0,1,0,2],[0,3,0,4],[0,5,0,6],[0,7,0,8],[0,9,0,10]]}
["Aquifermateriale","Hydrauliske ledningsevne (m/s)",null,"Effektiv porositet",null,"Vandmættede porøsitet",null,"Volumenvægt (kg/l)",null,"% Indhold af organisk kulstof "]
[null,"Interval","Defaultværdi","Interval","Defaultværdi","Interval","Defaultværdi","Interval","Defaultværdi","Interval","Defaultværdi"]
[]
["Lerjorde (overfladenært)","1E-08-1E-06",1E-8,"0,01 - 0,2",0.1,"0,35 - 0,45",0.4,"1,4 - 1,8",1.8,null,1]
["Dybe lerlag","1E-08-1E-02",1E-8,"0,01 - 0,2",0.1,"0,35 - 0,45",0.4,"1,4 - 1,8",1.8,null,0.1]
["Silt","1E-05-5E-05",1.0000000000000001E-5,"0,01 - 0,2",0.15,"0,35 - 0,45",0.4,"1,4 - 1,8",1.8,null,0.1]
["Sand, fint","1E-05-5E-05",1.0000000000000001E-5,"0,1 - 0,3",0.2,"0,35 - 0,5",0.45,"1,4 - 1,7",1.7,null,0.01]
["Sand, mellemkornet","5E-05-1E-04",5.0000000000000002E-5,"0,15 - 0,3",0.2,"0,35 - 0,5",0.45,"1,4 - 1,7",1.7,null,0.01]
["Sand, groft","2E-04-1E-03",2.0000000000000001E-4,"0,2 - 0,35",0.25,"0,35 - 0,5",0.45,"1,4 - 1,7",1.8,null,0.01]
["Grus","1E-03-5E-02",1E-3,"0,1 - 0,35",0.2,"0,25 - 0,4",0.35,"1,4 - 1,9",1.9,null,0.01]
["Sandsten","1E-08-1E-05",1E-8,"0,1 - 0,4",0.25,"0,05 - 0,3",0.25,"1,4 - 1,9",1.7,null,0.01]
["Kalk","1E-07-1E-05",9.9999999999999995E-8,"0,01 - 0,24",0.15,"0,05 - 0,5",0.3,"1,4 - 1,9",1.9,null,0.01]
["Klippe, opsprækket, forvitr.","1E-08-1E-04",1E-8,"0,1 - 0,4",0.25,"0,00 - 0,5",0.3,"1,5 - 1,9",1.9,null,0.01]
["Moræneler, 1-1,5 m.u.t.",1.2999999999999999E-5,1.2999999999999999E-5,"0,01 - 0,2",0.1,"0,35 - 0,45",0.4,"1,4 - 1,8",1.8,null,0.1]
["Moræneler, 2-2,5 m.u.t.",4.1999999999999996E-6,4.1999999999999996E-6,"0,01 - 0,2",0.1,"0,35 - 0,45",0.4,"1,4 - 1,8",1.8,null,0.1]
["Moræneler, 4-4,5 m.u.t.",2.4999999999999999E-7,2.4999999999999999E-7,"0,01 - 0,2",0.1,"0,35 - 0,45",0.4,"1,4 - 1,8",1.8,null,0.1]

{"sheet":"Eget Aquifermateriale","index":60,"n_rows":2,"n_cols":8,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Aquifermateriale","Hydrauliske ledningsevne (m/s)","Effektiv porositet","Vandmættede porøsitet","Volumenvægt (kg/l)","% Indhold af organisk kulstof ","Indsat af","Dato"]
[null,"Defaultværdi","Defaultværdi","Defaultværdi","Defaultværdi","Defaultværdi","Initial"]

{"sheet":"Beton","index":61,"n_rows":6,"n_cols":10,"rows_kept":6,"cut":false,"hidden":true,"merged":[[0,0,1,0]]}
["Beton­type","Beton­tværsnit","Relativ luftfugtighed","Vand/cement-tallet","Cement­indhold","Svindtid","Materiale­konstant for beton","Armerings­diameter","Armerings­konstant","afstand mellem armeringsjern"]
[null,"hb","RF %","v/c","CM","ts","Nb","da","k","Db"]
[]
["Armeret beton (beton 20)",80,60,0.67,220,7300,2E-3,3,1,50]
["Klaplag",80,60,1.1000000000000001,165,7300,2E-3]
["Uarmeret beton (beton 10)",80,60,0.82,220,7300,2E-3]

{"sheet":"Min Beton","index":62,"n_rows":2,"n_cols":12,"rows_kept":2,"cut":false,"hidden":true,"merged":[[0,0,1,0]]}
["Beton­type","Beton­tværsnit","Relativ luftfugtighed","Vand/cement-tallet","Cement­indhold","Svindtid","Materiale­konstant for beton","Armerings­diameter","Armerings­konstant","afstand mellem armeringsjern","Indsat af","Dato"]
[null,"hb","RF","v/c","CM","ts","Nb","da","k","Db","Initial"]

{"sheet":"Jordtyper","index":63,"n_rows":9,"n_cols":14,"rows_kept":9,"cut":false,"hidden":true,"merged":[[0,11,0,12],[0,7,0,8],[0,9,0,10],[0,1,0,3],[0,4,0,6]]}
[null,"Poreluft volumen",null,null,"Vandindhold",null,null,"Vandmættet porøsitet",null,"Kornrumvægt",null,"% Indhold af organisk kulstof"]
[null,"Interval","Ubefæstet areal","Under bygning","Interval","Ubefæstet areal","Under bygning","Interval","Værdi","Interval","Værdi","Interval","Værdi","Index nr"]
[]
["Ler","0,00 - 0,25",0.1,0.25,"0,20 - 0,40",0.3,0.2,"0,35 - 0,45",0.4,"2,7 - 2,8",2.7,null,0.1,1]
["Sand","0,0 - 0,45",0.3,0.4,"0,05 - 0,35",0.15,0.05,"0,35 - 0,50",0.45,"2,6 - 2,7",2.65,null,0.1,2]
["Lermuld","0,0 - 0,2",0.1,0.2,"0,25 - 0,35",0.3,0.25,"0,35 - 0,45",0.4,"2,6 - 2,7",2.65,null,1,3]
["Sandmuld","0,05 - 0,30",0.1,0.3,"0,15 - 0,35",0.35,0.15,"0,40 - 0,45",0.45,"2,5 - 2,6",2.6,null,2,4]
["Grus","0,0 - 0,35",0.2,0.3,"0,05 - 0,25",0.15,0.05,"0,25 - 0,40",0.35,"2,6 - 2,7",2.65,null,0.1,5]
["Fyld","0,0 - 0,35",0.1,0.3,"0,15 - 0,40",0.3,0.15,"0,25 - 0,50",0.4,"2,5 - 2,7",2.6,null,null,6]

{"sheet":"Mine Jordtyper","index":64,"n_rows":2,"n_cols":9,"rows_kept":2,"cut":false,"hidden":true,"merged":[[0,1,0,2],[0,3,0,4]]}
[null,"Poreluft volumen",null,"Vandindhold",null,"Vandmættet porøsitet","Kornrumvægt","% Indhold organisk kulstof"]
[null,"Ubefæstet areal","Under bygning","Ubefæstet areal","Under bygning","Værdi","Værdi","Værdi","Index nr"]

{"sheet":"Membraner","index":65,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":true,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4]]}
["Navn","Beskrivelse","Tykkelse (mm)","Interval","Værdi (ubenævnt)"]
[]
[]
["Dampspærre","Dampspærre 0,15 mm plastfolie",0.15,"7E-5–8,8E-5",8.8000000000000011E-5]

{"sheet":"Mine Membraner","index":66,"n_rows":1,"n_cols":7,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,6,1,6],[0,3,1,3],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,4,1,4],[0,5,1,5]]}
["Navn","Beskrivelse","Tykkelse (mm)","Værdi (ubenævnt)","indsat af","dato","Bemærkning"]

{"sheet":"Netto Nedbør","index":67,"n_rows":101,"n_cols":3,"rows_kept":101,"cut":false,"hidden":true,"merged":[]}
["Kommunenavn","Kommunenavn før strukturreform","Nettonedbør (mm/år)"]
[]
[]
["Aabenraa","Bov, Lundtoft, Rødekro, Tinglev og Aabenraa",540]
["Aalborg","Hals, Nibe, Sejlflod, Aalborg",325]
["Albertslund","Albertslund",300]
["Allerød","Allerød",300]
["Assens","Glamsbjerg, Haarby, Tommerup, Vissenbjerg, Aarup og Assens",300]
["Ballerup","Ballerup",300]
["Billund","Billund og Grindsted   ",650]
["Bornholm","Bornholm",340]
["Brøndby","Brøndby",300]
["Brønderslev-Dronninglund","Brønderslev og Dronninglund",375]
["Dragør","Dragør",250]
["Egedal  ","Ledøje-Smørum, Stenløse og Ølstykke",250]
["Esbjerg","Bramming, Esbjerg og Ribe",550]
["Fanø","Fanø",500]
["Favrskov  ","Hammel, Hadsten, Hinnerup og Hvorslev",375]
["Faxe","Haslev, Fakse og Rønnede",300]
["Fredensborg","Fredensborg-Humlebæk og Karlebo",300]
["Fredericia","Fredericia",400]
["Frederiksberg","Frederiksberg",300]
["Frederikshavn   ","Frederikshavn, Skagen og Sæby",370]
["Frederikssund","Frederikssund, Slangerup, Skibby og Jægerspris",250]
["Frederiksværk-Hundested","Frederiksværk og Hundested",250]
["Furesø","Farum og Værløse",300]
["Faaborg-Midtfyn","Broby, Ryslinge, Ringe, Faaborg, Årslev",300]
["Gentofte","Gentofte",300]
["Gladsaxe","Gladsaxe",300]
["Glostrup","Glostrup",300]
["Greve","Greve",250]
["Gribskov","Græsted-Gilleleje og Helsinge",275]
["Guldborgsund","Nykøbing Falster, Nysted, Nørre Alslev, Sakskøbing, Stubbekøbing og Sydfalster",250]
["Haderslev","Gram, Haderslev og Vojens",533]
["Hedensted","Hedensted, Juelsminde og Tørring-Uldum",433]
["Helsingør","Helsingør",300]
["Herlev","Herlev",300]
["Herning ","Aulum-Haderup, Herning, Trehøje og Aaskov",563]
["Hillerød ","Hillerød og Skævinge",275]
["Hjørring ","Hirtshals, Hjørring, Løkken-Vrå og Sindal",400]
["Holbæk ","Holbæk, Jernløse, Svinninge, Tornved og Tølløse",250]
["Holstebro","Holstebro, Ulfborg-Vemb og Vinderup",567]
["Horsens","Brædstrup, Gedved og Horsens",433]
["Hvidovre","Hvidovre",300]
["Høje-Taastrup","Høje-Taastrup",250]
["Hørsholm","Hørsholm",300]
["Ikast-Brande","Nørre-Snede, Brande og Ikast",550]
["Ishøj","Ishøj",250]
["Jammerbugt","Brovst, Fjerritslev, Pandrup, Aabybro",400]
["Kalundborg","Bjergsted, Gørlev, Hvidebæk, Høng og Kalundborg",200]
["Kerteminde","Kerteminde, Langeskov og Munkebo",267]
["Kolding","Christiansfeld, Kolding, Lunderskov, Vamdrup og Vester Nebel",513]
["København","København",300]
["Køge","Køge og Skovbo",250]
["Langeland","Rudkøbing, Sydlangeland og Tranekær",250]
["Lejre","Bramsnæs, Hvalsø og Lejre",283]
["Lemvig   ","Lemvig og Thyborøn-Harboøre",525]
["Lolland ","Nakskov, Rudbjerg, Ravnsborg, Holeby, Højreby, Maribo og Rødby",243]
["Lyngby-Taarbæk","Lyngby-Taarbæk",300]
["Læsø","Læsø",200]
["Mariagerfjord","Arden, Hadsund, Hobro og Mariager",363]
["Middelfart","Ejby, Middelfart og Nørre Aaby",300]
["Morsø","Morsø",500]
["Norddjurs","Grenaa, Nørre Djurs, Rougsø og Sønderhald Øst",313]
["Nordfyn","Bogense, Otterup og Søndersø",283]
["Nyborg","Nyborg, Ullerslev og Ørbæk",250]
["Næstved","Fuglebjerg, Fladså, Holmegaard, Næstved og Suså",270]
["Odder","Odder",350]
["Odense","Odense",300]
["Odsherred ","Dragsholm, Nykøbing-Rørvig og Trundholm",250]
["Randers","Langå, Nørhald, Purhus, Randers, Sønderhald Vest samt Havndal-området fra Mariager",350]
["Rebild","Nørager, Skørping og Støvring",400]
["Ringkøbing-Skjern","Holmsland, Egvad, Ringkøbing, Skjern og Videbæk",540]
["Ringsted","Ringsted",300]
["Roskilde","Gundsø, Ramsø og Roskilde",283]
["Rudersdal","Søllerød og Birkerød",300]
["Rødovre","Rødovre",300]
["Samsø","Samsø",250]
["Silkeborg","Gjern, Silkeborg, Them og Kjellerup",488]
["Skanderborg","Galten, Hørning, Ry og Skanderborg",413]
["Skive","Sallingsund, Skive, Spøttrup og Sundsøre",500]
["Slagelse","Hashøj, Korsør, Skælskør, Slagelse",225]
["Solrød","Solrød",250]
["Sorø","Dianalund, Sorø og Stenlille",275]
["Stevns","Vallø og Stevns",250]
["Struer","Struer og Thyholm",525]
["Svendborg","Egebjerg, Gudme og Svendborg",300]
["Syddjurs","Ebeltoft, Midtdjurs, Rosenholm og Rønde",313]
["Sønderborg","Augustenborg, Broager, Gråsten, Nordborg, Sønderborg, Sundeved og Sydals",393]
["Thisted","Hanstholm, Sydthy og Thisted",500]
["Tønder","Bredebro, Højer, Løgumkloster, Nørre-Rangstrup, Skærbæk og Tønder",583]
["Tårnby","Tårnby",300]
["Vallensbæk","Vallensbæk",300]
["Varde","Blaabjerg, Blåvandshuk, Helle, Varde og Ølgod",550]
["Vejen","Rødding, Holsted, Brørup og Vejen",613]
["Vejle","Børkop, Egtved, Give, Jelling og Vejle",510]
["Vesthimmerland","Farsø, Løgstør, Aars og Aalestrup",438]
["Viborg","Bjerringbro, Fjends, Karup, Møldrup, Tjele og Viborg",458]
["Vordingborg","Møn, Langebæk, Præstø og Vordingborg",263]
["Ærø","Ærøskøbing og Marstal",250]
["Århus","Århus",350]

{"sheet":"Egen Netto Nedbør","index":68,"n_rows":1,"n_cols":4,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Kommune/egn","Nettonedbør (mm/år)","Indsat af","Dato"]

{"sheet":"Stofdatabase","index":69,"n_rows":222,"n_cols":23,"rows_kept":222,"cut":false,"hidden":true,"merged":[]}
["Stofnavn","Gruppe","CAS-nummer","Grundvands-kvalitets-kriterie","Afdampnings-kriterie","Jordkvalitets-kriterie","molvægt","damptryk","vand-opløselig-hed","log Kow (okt/vand \nford. Koeff.)","KOC","Henrys\n konstant","Diff. Koeff.\nI luft","Diff. Koef. vand","Vind-\nhastighed","1. ordens nedbrydning grundvand\n(Nye værdier fra Miljøprojektnr. 2013, 2018 er mærkeret som lyserøde felter) \n\nAnaerob","1. ordens nedbrydning grundvand\n(Nye værdier fra Miljøprojektnr. 2013, 2018 er mærkeret som lyserøde felter) \n\nAerob","1. ordens nedbrydning umættet zone anaerob","1. ordens nedbrydning umættet zone aerob","1. ordens nedbrydning poreluft aerob","Indsat af","dato"]
[null,null,null,"μg/l","mg/m³","mg/kg","g/mol","Pa","mg/l",null,null,null,"DL m2/s","DW m2/s","m/s","dag-1","dag-1","dag-1","dag-1","dag-1"]
[]
["1-propanol","Additiver: Alkoholer","CAS 71-23-8",null,null,null,60.1,2799.8,1000000,0.25,{"$f":"POWER(10,(1.04*J4-0.84))","v":0.2630267991895382},{"$f":"H4*G4/(8.314*I4*298)","v":6.7916484364531087E-5},{"$f":"0.0000093*(78.1/G4)^0.5","v":1.0601595491013365E-5},{"$f":"M4*0.0001","v":1.0601595491013366E-9},0.1,0.06,0.4,0,0,0]
["2-butoxy ethanol","Additiver: Alkoholer","CAS 111-76-2",null,null,null,118.1754,117.32368421052631,1000000,0.83,1.0548725713234373,5.5961131749360377E-6,7.5604026385441442E-6,7.5604026385441446E-10,0.1,0,0.1,0,0,0]
["2-ethyl-1-hexanol","Additiver: Alkoholer","CAS 104-76-7",null,null,null,130.2296,18.131842105263157,880,2.73,99.815962749172499,1.0830354662436645E-3,7.2020082110938378E-6,7.2020082110938381E-10,0.1,0,0.04,0,0,0]
["2-propanol","Additiver: Alkoholer","CAS 67-63-0",10,1,null,60.095599999999997,6052.8355263157891,1000000,0.05,0.16292960326397224,1.46816634453111E-4,1.060198359069418E-5,1.0601983590694181E-9,0.1,0.04,7.0000000000000007E-2,0,0,0]
["Ethanol","Additiver: Alkoholer","CAS 64-17-5",null,null,null,46.07,7906.0164473684208,1000000,-0.31,6.8801831614303824E-2,1.4701093559753788E-4,1.2108751299870264E-5,1.2108751299870264E-9,0.1,0.1,0.2,0,0,0]
["Isopropanol","Additiver: Alkoholer","CAS 67-63-0",10,1,null,60.1,6052.8355263157891,1000000,0.05,0.16292960326397224,1.4682738387888583E-4,1.0601595491013365E-5,1.0601595491013366E-9,0.1,0.04,7.0000000000000007E-2,0,0,0]
["diethanolamin","Additiver: Aminer","CAS 111-42-2",null,null,null,105.13639999999999,3.7330263157894734E-2,1000000,-1.43,4.7076048325658312E-3,1.5841192423363212E-9,8.0155239187872624E-6,8.015523918787263E-10,0.1,0,0.01,0,0,0]
["triethanolamin","Additiver: Aminer"," CAS 102-71-6",null,null,null,149.18940000000001,4.7862730263157895E-4,1000000,-1,1.3182567385564075E-2,2.8821007059824571E-11,6.7288288469740935E-6,6.7288288469740936E-10,0.1,0,0.12,0,0,0]
["2-ethylhexyl nitrat","Additiver: Andet","CAS 27247-96-7",null,null,null,175.22720000000001,35.063782894736846,17.600000000000001,4.12,2784.8384078050103,0.14090335623611619,6.2088004919072391E-6,6.2088004919072397E-10,0.1,0,4.4999999999999998E-2,0,0,0]
["butylacetat ","Additiver: Estere","n-butylacetat, CAS 123-86-4",10,0.1,null,116.16,1533.2072368421052,8400,1.78,10.261243651933427,8.5575982411303011E-3,7.6257078658014081E-6,7.6257078658014086E-10,0.1,0,0.04,0,0,0]
["1,2-dibromethan","Additiver: Halogenerede alifater","CAS 106-93-4",0.01,9.9999999999999995E-7,0.02,187.86,2319.8092105263154,4321,1.76,9.7813770432298615,4.0707650376269999E-2,5.9964098169712604E-6,5.9964098169712608E-10,0.1,0.04,2E-3,0,0,0]
["Acetone","Additiver: Ketoner","CAS 67-64-1",10,0.4,null,58.08,30930.78947368421,1000000,-0.24,8.1357950560539627E-2,7.2508901966585786E-4,1.0784379486511541E-5,1.0784379486511542E-9,0.1,0.04,0.09,0,0,0]
["Methylisobutylketon","Additiver: Ketoner","CAS 108-10-1",10,0.2,null,100.16,2133.1578947368421,19000,1.3,3.2508729738543449,4.5387622435624385E-3,8.2122338461839333E-6,8.2122338461839332E-10,0.1,0.02,0.06,0,0,0]
["Diethylether","Additiver: Ætere","CAS 60-29-7",10,1,null,74.12,58928.48684210526,64000,0.89,1.2178673848912598,2.7545739871137211E-2,9.5464248951357362E-6,9.546424895135736E-10,0.1,0,0,0,0,0]
["MTBE","Additiver: Ætere","CAS 1634-04-4",5,0.03,null,88.149199999999993,33330.59210526316,51000,0.94,1.372777018208549,2.3252247856996356E-2,8.7538535742201766E-6,8.7538535742201772E-10,0.1,1E-3,1E-3,0,0,0]
["Decan","Aliphatiske kulbr: Alkaner","CAS 124-18-5",null,0.1,null,142.29,190.65098684210525,5.1999999999999998E-2,5.01,23463.889244641345,210.56384822413571,6.8900325848001511E-6,6.8900325848001514E-10,0.1,0,0,0,0,0]
["dodecan","Aliphatiske kulbr: Alkaner","CAS 112-40-3",null,0.1,null,170.3374,17.998519736842105,3.7000000000000002E-3,6.1,319153.78551007615,334.4404462745772,6.2972865897445786E-6,6.2972865897445784E-10,0.1,0,0.01,0,0,0]
["eicosan","Aliphatiske kulbr: Alkaner","CAS 112-95-8",null,0.1,null,282.55180000000001,6.1594934210526314E-4,1.9E-3,10.16,5325985748.4906187,3.6971169507604068E-2,4.8894434361812199E-6,4.8894434361812198E-10,0.1,0,0,0,0,0]
["Ethan","Aliphatiske kulbr: Alkaner","CAS 74-84-0",null,0.1,null,30.1,4199654.6052631577,60.2,1.81,11.025543321022241,847.53432095276287,1.4980462359076049E-5,1.498046235907605E-9,0.1,0,0,0,0,0]
["hexacosan","Aliphatiske kulbr: Alkaner","CAS 630-01-3",null,0.1,null,366.71260000000001,6.2528190789473679E-5,1.6999999999999999E-3,13.11,6228737089440.2988,5.4441049585699577E-3,4.2918600243411986E-6,4.2918600243411989E-10,0.1,0,0,0,0,0]
["hexadecan","Aliphatiske kulbr: Alkaner","CAS 544-76-3",null,0.1,null,226.44460000000001,0.1906509868421053,8.9999999999999998E-4,8.25,54954087.38576249,19.361198273087883,5.4616954683079556E-6,5.4616954683079557E-10,0.1,0,8.9999999999999993E-3,0,0,0]
["Methan","Aliphatiske kulbr: Alkaner","CAS 74-82-8",null,0.1,null,16,62128223.684210524,22,1.0900000000000001,1.9660746338791013,18237.275316086005,2.0547002518615706E-5,2.0547002518615708E-9,0.1,0,0,0,0,0]
["n-Butan","Aliphatiske kulbr: Alkaner","CAS 106-97-8",null,0.1,null,58.1,242646.71052631579,61.2,2.89,146.41986429352787,92.976423037853579,1.0782523151273327E-5,1.0782523151273328E-9,0.1,0,1E-4,0,0,0]
["n-Heptan","Aliphatiske kulbr: Alkaner","CAS 142-82-5",null,0.1,null,100.2,6132.8289473684208,3.4,4.66,10148.456628180971,72.949676790578437,8.2105945141292352E-6,8.2105945141292353E-10,0.1,0,0.03,0,0,0]
["n-Hexan","Aliphatiske kulbr: Alkaner","CAS 110-54-3",null,0.1,null,86.2,20131.677631578947,9.5,3.9,1644.3717232149334,73.728830264897923,8.8522736864578243E-6,8.8522736864578242E-10,0.1,0,0.08,0,0,0]
["n-Oktan","Aliphatiske kulbr: Alkaner","CAS 111-65-9",null,0.1,null,114.2,1879.8453947368421,0.66,5.18,35253.318119588643,131.2858792000537,7.6908689918231638E-6,7.6908689918231637E-10,0.1,0,0.04,0,0,0]
["n-Pentan","Aliphatiske kulbr: Alkaner","CAS 109-66-0",null,0.1,null,72.2,68527.697368421053,38,3.39,484.84173870844694,52.552509069363069,9.6725251295755997E-6,9.6725251295756004E-10,0.1,0,0.15,0,0,0]
["octadecan","Aliphatiske kulbr: Alkaner","CAS 593-45-3",null,0.1,null,254.4982,4.5462927631578949E-2,6.0000000000000001E-3,9.18,509565480.60811609,0.77833145037205131,5.1518843808499462E-6,5.1518843808499461E-10,0.1,0,0,0,0,0]
["pentacosan","Aliphatiske kulbr: Alkaner","CAS 629-99-2",null,0.1,null,352.68579999999997,2.0131677631578945E-4,2.9000000000000002E-8,12.62,1926637459524.0872,988.19729221488706,4.3763744951513593E-6,4.3763744951513595E-10,0.1,0,0,0,0,0]
["pentadecan","Aliphatiske kulbr: Alkaner","CAS 629-62-9",null,0.1,null,212.4178,0.45729572368421045,7.6000000000000004E-5,7.71,15079953.418017916,515.87938118027546,5.6391417592337585E-6,5.6391417592337588E-10,0.1,0,0.01,0,0,0]
["pentatriacontan","Aliphatiske kulbr: Alkaner","CAS 630-07-9",null,0.1,null,492.9538,7.1860756578947366E-10,2.4700000000000001E-13,17.53,2.4615009062337795E+17,578.86163453161453,3.7017352631160009E-6,3.7017352631160013E-10,0.1,0,0,0,0,0]
["Propan","Aliphatiske kulbr: Alkaner","CAS 74-98-6",null,0.1,null,44.1,953254.93421052629,62.4,2.36,41.152857843551061,271.91726130567821,1.2376252771055592E-5,1.2376252771055592E-9,0.1,0,0.03,0,0,0]
["tetradecan","Aliphatiske kulbr: Alkaner","CAS 629-59-4",null,0.1,null,198.39099999999999,1.5465394736842104,2.2000000000000001E-3,7.2,{"$f":"POWER(10,(1.04*J36-0.84))","v":4446312.6746910987},{"$f":"H36*G36/(8.314*I36*298)","v":56.2903580095359},{"$f":"0.0000093*(78.1/G36)^0.5","v":5.8350889691650888E-6},{"$f":"M36*0.0001","v":5.8350889691650895E-10},0.1,0,0.01,0,0,0]
["2-methylhexan","Aliphatiske kulbr: Iso-alkaner","CAS 591-76-4",null,0.1,null,100.2034,8799.2763157894733,2.54,3.71,1043.2778814599669,140.11009018938717,8.2104552161705016E-6,8.2104552161705018E-10,0.1,0,0,0,0,0]
["Cycloheptan","Aliphatiske kulbr: Naphthener","CAS 291-64-5",null,0.1,null,98.2,2879.7631578947367,30,4,2089.2961308540421,3.8047026430885178,8.2937840194020483E-6,8.2937840194020485E-10,0.1,0,0,0,0,0]
["Cyclohexan","Aliphatiske kulbr: Naphthener","CAS 110-82-7",null,0.1,null,84.2,12918.9375,55,3.44,546.51237451987242,7.9827019612896688,8.9567905740378567E-6,8.956790574037857E-10,0.1,0,0,0,0,0]
["Cyclooktan","Aliphatiske kulbr: Naphthener","CAS 292-64-8",null,0.1,null,112.2,734.60625000000005,7.9,4.45,6137.6200516479512,4.2110858988793174,7.7591122900375518E-6,7.7591122900375521E-10,0.1,0,0,0,0,0]
["Cyclopentan","Aliphatiske kulbr: Naphthener","CAS 287-92-3",null,0.1,null,70.099999999999994,42396.51315789474,156,3,190.54607179632498,7.6894853788420043,9.816336931669714E-6,9.8163369316697135E-10,0.1,0,0,0,0,0]
["4-methylanilin","Aliphatiske kulbr: NSO-forbindelser","CAS 106-49-0",null,null,null,107.15479999999999,39.996710526315788,6500,1.39,4.0327379297611321,2.6613148909840036E-4,7.9396736279112657E-6,7.9396736279112662E-10,0.1,0,0.2,0,0,0]
["4-methylquinolin","Aliphatiske kulbr: NSO-forbindelser","CAS 491-35-0",null,null,null,143.18780000000001,0.84721000000000002,479,2.61,74.8858907521644,1.0221986241887629E-4,6.8683980661423817E-6,6.8683980661423825E-10,0.1,0.08,0,0,0,0]
["acridin","Aliphatiske kulbr: NSO-forbindelser","CAS 260-94-6",null,null,null,179.2208,1.7999999999999999E-2,38.4,3.4,496.59232145033644,3.3908096313649006E-5,6.1392350270271861E-6,6.1392350270271863E-10,0.1,0.1,0,0,0,0]
["anilin","Aliphatiske kulbr: NSO-forbindelser","CAS 62-53-3",null,null,null,93.128,65.327960526315792,36000,0.9,1.2473835142429432,6.8210399221212633E-5,8.5166407345416544E-6,8.5166407345416548E-10,0.1,0,0,0,0,0]
["benzo(b)thiophen","Aliphatiske kulbr: NSO-forbindelser","CAS 95-15-8",null,null,null,134.19540000000001,31.654,130,3.12,253.98028137728187,1.3188536045649657E-2,7.0947917264519743E-6,7.0947917264519749E-10,0.1,0,0,0,0,0]
["carbazol","Aliphatiske kulbr: NSO-forbindelser","CAS 86-74-8",null,null,null,167.2098,9.9749999999999999E-5,1.8,3.72,1068.5626745999625,3.7400365155886487E-6,6.3559079926145256E-6,6.3559079926145254E-10,0.1,0,0,0,0,0]
["dibenzofuran","Aliphatiske kulbr: NSO-forbindelser","CAS 132-64-9",null,null,null,168.19460000000001,0.35063782894736845,3.1,4.12,2784.8384078050103,7.6786140448574262E-3,6.3372733653665426E-6,6.3372733653665431E-10,0.1,0,1.7999999999999999E-2,0,0,0]
["dibenzothiophen","Aliphatiske kulbr: NSO-forbindelser","CAS 132-65-0",null,null,null,184.2552,2.7265000000000001E-2,1.47,4.38,5190.3901019708328,1.3793727315060298E-3,6.0547830833864374E-6,6.0547830833864381E-10,0.1,0,0.06,0,0,0]
["dimethyldisulfid","Aliphatiske kulbr: NSO-forbindelser","CAS 624-92-0",null,null,null,94.189400000000006,3817.1,3000,1.77,10.018437657240259,4.8371330041400748E-2,8.468518688960739E-6,8.468518688960739E-10,0.1,0,0,0,0,0]
["quinolin","Aliphatiske kulbr: NSO-forbindelser","CAS 91-22-5",null,null,null,129.161,7.98,6110,2.0299999999999998,18.672393883829486,6.8087407088534866E-5,7.2317393735017901E-6,7.2317393735017909E-10,0.1,0.2,0.18,0,0,0]
["thiophen","Aliphatiske kulbr: NSO-forbindelser","CAS 110-02-1",null,null,null,84.14,10625.792763157895,3010,1.81,11.025543321022241,0.11988671749971522,8.9599835361406009E-6,8.9599835361406015E-10,0.1,0,0,0,0,0]
["1-Hexen","Aliphatiske kulbr: Olefiner","CAS 592-41-6",null,0.1,null,84.2,24531.315789473683,50,3.39,484.84173870844694,16.673879019246943,8.9567905740378567E-6,8.956790574037857E-10,0.1,0,8.9999999999999993E-3,0,0,0]
["1-Okten","Aliphatiske kulbr: Olefiner","CAS 111-66-0",null,0.1,null,112.2,2319.8092105263154,4.0999999999999996,4.57,8180.879579457488,25.623295456595589,7.7591122900375518E-6,7.7591122900375521E-10,0.1,0,0,0,0,0]
["cyanid, total","Cyanider","CN-- , CAS 57-12-5",50,null,500,26.017700000000001,41063.289473684214,95400,-0.69,2.7694912668096826E-2,4.5200993379879767E-3,1.6112911236524748E-5,1.6112911236524749E-9,0.1,0,0,0,0,0]
["cyanider, syreflygtige","Cyanider","CHN, CAS 74-90-8",null,0.06,10,27.025600000000001,98925.197368421053,1000000,-0.25,7.9432823472428096E-2,1.0790858203111758E-3,1.5809596769332241E-5,1.5809596769332241E-9,0.1,0,0.06,0,0,0]
["1,1,1-Trichlorethan","Klorerede alifater","CAS 71-55-6",1,0.5,200,133.41,16531.973684210527,1290,2.4900000000000002,56.18236281342287,0.69007627247595449,7.1156450071498109E-6,7.1156450071498117E-10,0.1,4.0000000000000001E-3,5.0000000000000001E-3,0,0,0]
["1,1,-Dichlorethan","Klorerede alifater","CAS 75-34-3",1,null,null,98.96,30264.177631578947,5040,1.79,10.509934271862177,0.23984559313601905,8.2618750428658061E-6,8.2618750428658068E-10,0.1,0.1,0,0,0,0]
["1,1-Dichlorethylen","Klorerede alifater","CAS 75-35-4",1,0.01,5,96.94,79993.421052631573,2420,2.13,23.724660151048106,1.2933487142567623,8.3475101884450271E-6,8.3475101884450275E-10,0.1,0.03,0.4,0,0,0]
["1,2 - dichlorethan","Klorerede alifater","CAS 107-06-2 ",1,1E-4,1,98.96,10519.134868421053,8600,1.48,5.0026486242100612,4.8855670107620527E-2,8.2618750428658061E-6,8.2618750428658068E-10,0.1,6.9999999999999999E-4,2E-3,0,0,0]
["Chlorethan","Klorerede alifater","CAS 75-00-3",1,null,null,64.52,134655.59210526315,6710,1.43,4.4381298030813898,0.52260065319945104,1.0232017779926358E-5,1.0232017779926359E-9,0.1,0,0,0,0,0]
["Chlormethan","Klorerede alifater","CAS 74-87-3",1,null,null,50.49,573286.18421052629,5320,0.91,1.2776149939707953,2.1960333431088612,1.1566601683718686E-5,1.1566601683718686E-9,1,0,0,0,0,0]
["cis-1,2-Dichlorethylen","Klorerede alifater","CAS 156-59-2",1,0.4,85,96.94,26664.473684210527,6410,1.86,12.427964384409158,0.16276151266257752,8.3475101884450271E-6,8.3475101884450275E-10,0.1,6.9999999999999999E-4,0.3,0,0,0]
["Dichlormethan","Klorerede alifater","CAS 75-09-2",1,5.9999999999999995E-4,8,84.93,57995.230263157893,13000,1.3,3.2508729738543449,0.1529268576173646,8.9182142885661583E-6,8.9182142885661583E-10,1,6.0000000000000001E-3,0,0,0,0]
["Tetrachlorethylen","Klorerede alifater","CAS 127-18-4",1,6.0000000000000001E-3,5,165.83,2466.4638157894738,206,3.4,496.59232145033644,0.8013907857008904,6.3822956026606838E-6,6.3822956026606842E-10,1,6.9999999999999999E-4,0,0,0,0]
["Tetrachlormethan","Klorerede alifater","CAS 56-23-5",1,5.0000000000000001E-3,5,153.82,15332.072368421053,793,2.73,99.815962749172499,1.2003674103668776,6.6267725100053721E-6,6.6267725100053728E-10,1,0.1,0,0,0,0]
["trans-1,2-Dichlorethylen","Klorerede alifater","CAS 156-60-5",1,0.4,85,96.94,44129.70394736842,4520,2.09,21.557579680386297,0.38200523122933333,8.3475101884450271E-6,8.3475101884450275E-10,0.1,2E-3,0.4,0,0,0]
["Trichlorethylen","Klorerede alifater","CAS 79-01-6",1,1E-3,5,131.38999999999999,9199.2434210526317,1280,2.42,{"$f":"POWER(10,(1.04*J68-0.84))","v":47.511637637756166},{"$f":"H68*G68/(8.314*I68*298)","v":0.38113441843595547},{"$f":"0.0000093*(78.1/G68)^0.5","v":7.1701346118734786E-6},{"$f":"M68*0.0001","v":7.1701346118734787E-10},1,5.9999999999999995E-4,0,0,0,0]
["Trichlormethan (Chloroform)","Klorerede alifater","CAS 67-66-3",null,0.02,50,119.38,26264.50657894737,7950,1.97,16.173350557998518,0.1591869302614527,7.5221619290677847E-6,7.5221619290677854E-10,1,0.03,0,0,0,0]
["Vinylchlorid","Klorerede alifater","CAS 75-01-4",0.2,4.0000000000000003E-5,0.4,62.5,397300.65789473685,8800,1.62,6.995197810512134,1.1389124623192795,1.0396052327686697E-5,1.0396052327686698E-9,1,6.9999999999999999E-4,2.9999999999999997E-4,0,0,0]
["1,2,3-Trimethylbenzen","Monoaromat. Kulbr.","CAS 526-73-8",1,0.03,null,120.2,225.31480263157894,75,3.66,925.55024476343749,0.14574935609710254,7.4964600630922756E-6,7.4964600630922764E-10,0.1,0,1,0,0,0]
["1,2,4-Trimethylbenzen","Monoaromat. Kulbr.","CAS 95-63-6",1,0.03,null,120.2,279.97697368421052,57,3.63,861.39034577242865,0.2383008780784143,7.4964600630922756E-6,7.4964600630922764E-10,0.1,5.0000000000000001E-4,1.1499999999999999,0,0,0]
["1,3,5-Trimethylbenzen","Monoaromat. Kulbr.","CAS 108-67-8",1,0.03,null,120.2,330.63947368421054,48.2,3.42,520.95474732855575,0.33280193761277066,7.4964600630922756E-6,7.4964600630922764E-10,0.1,4.0000000000000001E-3,1.1000000000000001,0,0,0]
["1-Ethyl-2-methylbenzen","Monoaromat. Kulbr.","CAS 611-14-3",null,null,null,120.2,347.97138157894739,74.599999999999994,3.53,677.95364492419515,0.22629912952716519,7.4964600630922756E-6,7.4964600630922764E-10,0.1,0,0,0,0,0]
["1-Ethyl-4-methylbenzen","Monoaromat. Kulbr.","CAS 622-96-8",null,null,null,120.2,399.96710526315792,94.9,3.63,861.39034577242865,0.20447313036985723,7.4964600630922756E-6,7.4964600630922764E-10,0.1,0,0,0,0,0]
["Benzen","Monoaromat. Kulbr.","CAS 71-43-2",1,1.2999999999999999E-4,1.5,78.099999999999994,12638.96052631579,1790,2.13,23.724660151048106,0.22257843072504188,9.3000000000000007E-6,9.300000000000001E-10,1,4.0000000000000001E-3,7.0000000000000001E-3,0,0,0]
["Ethylbenzen","Monoaromat. Kulbr.","CAS 100-41-4",5,0.1,null,106.2,1279.8947368421052,169,3.15,272.89777828080423,0.32462785419282836,7.9752849160092975E-6,7.9752849160092983E-10,0.1,4.0000000000000001E-3,8.0000000000000004E-4,0,0,0]
["m-Xylen","Monoaromat. Kulbr.","CAS 108-38-3",5,0.1,null,106.2,1105.2424342105262,161,3.2,307.60968147407124,0.29425910326261284,7.9752849160092975E-6,7.9752849160092983E-10,1,3.0000000000000001E-3,8.0000000000000002E-3,0,0,0]
["o-Xylen","Monoaromat. Kulbr.","CAS 95-47-6",5,0.1,null,106.2,881.26085526315785,152,3.12,253.98028137728187,0.24851872919426166,7.9752849160092975E-6,7.9752849160092983E-10,1,3.0000000000000001E-3,0.04,0,0,0]
["p-Xylen","Monoaromat. Kulbr.","CAS 106-42-3",5,0.1,null,106.2,1178.5697368421052,162,3.15,272.89777828080423,0.31184479748580107,7.9752849160092975E-6,7.9752849160092983E-10,1,3.0000000000000001E-3,0.01,0,0,0]
["Styren","Monoaromat. Kulbr.","CAS 100-42-5",1,0.2,40,104.15,853.26315789473688,9600,3,190.54607179632498,3.7363259059145092E-3,8.0533918034034747E-6,8.053391803403475E-10,1,0,5.0000000000000001E-3,0,0,0]
["Toluen","Monoaromat. Kulbr.","CAS 108-88-3",5,0.4,null,92.1,3786.3552631578946,530,2.73,99.815962749172499,0.26556989173487688,8.5640392765120893E-6,8.5640392765120896E-10,1,4.0000000000000001E-3,0.1,0,0,0]
["1-methylnaphthalen","PAH","CAS 90-12-0",null,null,null,142.19999999999999,8.9325986842105269,25.8,3.87,1530.3825321774382,1.9871535596026463E-2,6.8922126299693384E-6,6.8922126299693383E-10,0.1,0,0.02,0,0,0]
["2-methylnaphthalen","PAH","CAS 91-57-6",null,null,null,142.19999999999999,7.3327302631578943,24.6,3.86,1494.1699574067029,1.7108184086131264E-2,6.8922126299693384E-6,6.8922126299693383E-10,0.1,0,0.04,0,0,0]
["Acenaphthen","PAH","CAS 83-32-9",null,null,null,154.19999999999999,0.28664309210526318,3.9,3.92,1725.0432972458477,4.5744086841753287E-3,6.6186021894078394E-6,6.6186021894078393E-10,0.1,0,0.02,0,0,0]
["Acenaphthylen","PAH","CAS 208-96-8",null,null,null,152.19999999999999,0.89059342105263162,16.100000000000001,4.07,2470.5861360384356,3.3981455347545709E-3,6.6619464783515415E-6,6.6619464783515417E-10,0.1,0,0,0,0,0]
["Anthracen","PAH","CAS 120-12-7",null,null,null,178.2,1.4E-3,4.3400000000000001E-2,4.45,6137.6200516479512,2.3201695437203005E-3,6.1567938987033759E-6,6.1567938987033764E-10,0.1,0,0.03,0,0,0]
["Benzo(a)anthracen","PAH","CAS 56-55-3",null,null,null,228.3,2.6999999999999999E-5,9.4000000000000004E-3,5.76,141383.91390945684,2.6467659432256104E-4,5.4394565218975376E-6,5.439456521897538E-10,0.1,0,2E-3,0,0,0]
["Benzo(a)pyren","PAH","CAS 50-32-8",0.01,null,0.3,252.3,7.3E-7,1.6199999999999999E-3,6.13,342925.67329756083,4.5887966420649232E-5,5.1742789740511641E-6,5.1742789740511642E-10,0.1,0,0.06,0,0,0]
["Benzo(e)pyren","PAH","CAS 192-97-2",null,null,null,252.3,7.4000000000000001E-7,6.3E-3,6.44,720443.62041528628,1.1961403380098781E-5,5.1742789740511641E-6,5.1742789740511642E-10,0.1,0,0,0,0,0]
["Benzo(g,h,i)perylen","PAH","CAS 205-99-2",0.2,null,null,252.3,4.9999999999999998E-7,1.5E-3,5.78,148320.09671818794,3.3944523105685727E-5,5.1742789740511641E-6,5.1742789740511642E-10,0.1,0,0,0,0,0]
["Benzo(g,h,i)perylen","PAH","CAS 191-24-2",0.2,null,null,276.3,1.3000000000000001E-8,2.5999999999999998E-4,6.63,1135533.6278419381,5.5760236231278057E-6,4.9444503816447828E-6,4.9444503816447827E-10,0.1,0,0.1,0,0,0]
["Benzo(k)fluoranthen","PAH","CAS 207-08-9",0.2,null,null,252.3,1.3000000000000001E-8,8.0000000000000004E-4,6.11,326888.76924727304,1.6547955014021792E-6,5.1742789740511641E-6,5.1742789740511642E-10,0.1,0,0.03,0,0,0]
["Biphenyl","PAH","CAS 92-52-4",null,null,null,154.19999999999999,1.19056875,6.94,3.98,1991.5902890576137,1.067709478210402E-2,6.6186021894078394E-6,6.6186021894078393E-10,0.1,0,0.03,0,0,0]
["Chrysen","PAH","CAS 218-01-9",null,null,null,228.3,8.4E-7,2.0999999999999999E-3,5.81,159367.58810287697,3.6858666468623316E-5,5.4394565218975376E-6,5.439456521897538E-10,0.1,0,0.06,0,0,0]
["coronen","PAH","CAS 191-07-1",null,null,null,300.35879999999997,2.8930953947368418E-10,1.3999999999999999E-4,7.64,12752637.064597305,2.5052368697161236E-7,4.7422919309149883E-6,4.7422919309149886E-10,0.1,0,0,0,0,0]
["Dibenzo(a,h)anthracen","PAH","CAS 53-70-3",null,null,0.3,278.39999999999998,3.7000000000000001E-10,2.49E-3,6.75,1513561.248436213,1.6697264377703322E-8,4.9257668316019948E-6,4.9257668316019955E-10,0.1,0,0.01,0,0,0]
["Fluoranthen","PAH","CAS 206-44-0",0.1,null,null,202.3,1.2999999999999999E-3,0.26,5.16,33604.698246070009,4.0826260548633897E-4,5.7784388814859601E-6,5.7784388814859608E-10,0.1,2E-3,2E-3,0,0,0]
["Fluoren","PAH","CAS 86-73-7",null,null,null,166.2,7.9993421052631575E-2,1.69,4.18,3215.1408248326975,3.1752088845838087E-3,6.3751874043382609E-6,6.375187404338261E-10,0.1,0,0.05,0,0,0]
["indeno(1,2,3-cd)pyren","PAH","CAS 193-39-5",null,null,null,276.33679999999998,1.6665296052631579E-8,1.9000000000000001E-4,6.7,{"$f":"POWER(10,(1.04*J100-0.84))","v":1342764.9611378692},9.782995912375082E-6,4.9441211424116288E-6,{"$f":"M100*0.0001","v":4.9441211424116287E-10},0.1,0,0.05,0,0,0]
["Naphthalen","PAH","CAS 91-20-3",1,0.04,null,128.19999999999999,11.332401315789474,31,3.3,390.84089579240231,1.8915681506241185E-2,7.2587936878955403E-6,7.2587936878955411E-10,0.1,4.0000000000000002E-4,3.0000000000000001E-3,0,0,0]
["Phenanthren","PAH","CAS 85-01-8",null,null,null,178.2,1.613200657894737E-2,1.1499999999999999,4.46,6286.3708841305079,1.0089553918701264E-3,6.1567938987033759E-6,6.1567938987033764E-10,0.1,0,0,0,0,0]
["Pyren","PAH","CAS 129-00-0",null,null,null,202.3,6.0999999999999997E-4,0.13500000000000001,4.88,17186.996953977399,3.6894842866172864E-4,5.7784388814859601E-6,5.7784388814859608E-10,0.1,0,0.02,0,0,0]
["NN-DMS","Pesticid","3984-14-3",0.1,null,null,124.17,17,42370,-1.1000000000000001,5.6,2.0000000000000002E-5,7.4000000000000003E-6,7.4000000000000003E-10,0.1,null,null,null,null,null,"JAF (PubChem /Chemspider)","2022-08-11"]
["TFA","Pesticid","76-05-1",9,null,null,114.02,11000,1000,-2.1,2.738,0.5,7.6969372714615459E-6,7.6969372714615454E-10,0.1,null,null,null,null,null,"JAF (PubChem /Chemspider)","2022-08-12"]
["2,3,6-TBA","Pesticider",null,0.1,null,null,225.5,7.3099999999999998E-2,7700,2.7092699609758308,{"$f":"POWER(10,(1.04*J106-0.84))","v":94.981879559306932},{"$f":"H106*G106/(8.314*I106*298)","v":8.6406599456472471E-7},{"$f":"0.0000093*(78.1/G106)^0.5","v":5.4731227987988462E-6},{"$f":"M106*0.0001","v":5.4731227987988466E-10},0.1,6.9999999999999994E-5,1.38629436111989E-2,0,0,0]
["2,4,5-T","Pesticider","CAS 93-76-5",0.1,null,null,255.48,8.6659539473684202E-4,220,3.4,496.59232145033644,4.0618540954129215E-7,5.1419756032816814E-6,5.1419756032816812E-10,0.1,0,0,0,0,0]
["2,4-D","Pesticider",null,0.1,null,null,221.04,1.9000000000000001E-5,23180,-0.82390874094431876,2.0097170149791895E-2,7.3128178663971214E-11,5.5280635823662561E-6,5.5280635823662567E-10,0.1,2E-3,0.02,0,0,0]
["2,6-DCPP","Pesticider",null,0.1,null,null,221.4,8.0999999999999996E-3,491.1,2.6190933306267428,76.534467319252215,1.4738945638149898E-6,5.5235673932674597E-6,5.5235673932674601E-10,0.1,2.9999999999999997E-4,2.7725887222397813E-3,0,0,0]
["4-nitrophenol","Pesticider","CAS 100-02-7",0.5,5.0000000000000001E-3,125,139.11000000000001,0.13300000000000001,10000,1.9100905455940682,14.011807669324655,7.4676457434940344E-7,6.9683393184783224E-6,6.9683393184783225E-10,0.1,0.1,0.09,0,0,0]
["Aldicarb","Pesticider",null,0.1,null,null,190.3,1.2999999999999999E-2,4930,1.1492191126553799,2.2656242117973262,2.025391285636387E-7,5.9578432300419953E-6,5.9578432300419952E-10,0.1,6.0000000000000001E-3,1.1571739241401423E-3,0,0,0]
["alfa-Endosulfan","Pesticider","CAS 959-98-8",0.1,null,null,406.92,6.1061644736842106E-3,0.32,3.55,711.21351365332896,3.1340164478968458E-3,4.0743088527434311E-6,4.0743088527434311E-10,0.1,0,0,0,0,0]
["Amitrol","Pesticider",null,0.1,null,null,84.08,3.3000000000000003E-5,264000,-0.95860731484177497,1.4556212685090974E-2,4.2420563357997267E-12,8.9631799154096989E-6,8.9631799154096997E-10,0.1,1E-3,7.6170019841752231E-3,0,0,0]
["AMPA","Pesticider",null,0.1,null,null,111.04,7.6600000000000001E-3,100000,-2.1739251972991736,7.9271631180743963E-4,3.4330643065065314E-9,7.7995354965879879E-6,7.7995354965879883E-10,0.1,3.0000000000000001E-3,2.7725887222397813E-3,0,0,0]
["Atrazin","Pesticider",null,0.1,null,null,215.7,3.8999999999999999E-5,33,2.4996870826184039,57.500889889081044,1.0289032238747523E-7,5.5960732805544273E-6,5.5960732805544271E-10,0.1,0,4.0000000000000002E-4,0,0,0]
["Atrazin, deethyl","Pesticider",null,0.1,null,null,187.63,1.2E-2,3200,1.5092025223311027,5.3650110800245514,2.8399275581093106E-7,6.0000839412131741E-6,6.0000839412131743E-10,0.1,6.0000000000000002E-5,4.6209812037329686E-3,0,0,0]
["Atrazin, desisopropyl","Pesticider","CAS 330-54-1",0.1,null,null,173.61,2.8000000000000001E-2,6160,1.3617278360175928,3.7687467021867511,3.1851198013069395E-7,6.2376513571282984E-6,6.2376513571282987E-10,0.1,6.0000000000000002E-5,4.6209812037329686E-3,0,0,0]
["Atrazin, hydroxy","Pesticider",null,0.1,null,null,197.24,1.1000000000000001E-3,739.1,2.0899051114393981,21.552681739428735,1.1848358668538445E-7,5.8520896225809749E-6,5.8520896225809751E-10,0.1,0,6.9999999999999999E-4,0,0,0]
["BAM","Pesticider",null,0.1,null,null,190.3,4.3899999999999998E-3,2730,0.77085201164214423,0.91555848556506259,1.2351348542587383E-7,5.9578432300419953E-6,5.9578432300419952E-10,0.1,0,0,0,0,0]
["Bentazon","Pesticider",null,0.1,null,null,240.3,1.7000000000000001E-4,570,-0.45593195564972439,4.8509943201196892E-2,2.8926877221986519E-8,5.3019005849538595E-6,5.3019005849538593E-10,0.1,0,0,0,0,0]
["beta-Endosulfan","Pesticider","CAS 33213-65-9",0.1,null,null,406.92,3.199736842105263E-3,0.33,3.62,841.00775406923424,1.5925133200904976E-3,4.0743088527434311E-6,4.0743088527434311E-10,0.1,0,0,0,0,0]
["Bromophenoxim","Pesticider",null,0.1,null,null,461,1E-8,9,3.1702617153949575,286.46540639964633,2.0674362731828673E-10,3.8278772513792683E-6,3.8278772513792686E-10,0.1,1E-3,0.7,0,0,0]
["Bromoxynil","Pesticider",null,0.1,null,null,276.89999999999998,1.7000000000000001E-4,130,1.0398105541483504,1.7434238238463862,1.4615115120771465E-7,4.9390905422572884E-6,4.9390905422572889E-10,0.1,1E-3,0.05,0,0,0]
["Captan","Pesticider",null,0.1,null,null,300.60000000000002,1.2999999999999999E-3,3.3,2.7993405494535817,117.84581694887621,4.7796060747450257E-5,4.7403889529393791E-6,4.7403889529393789E-10,0.1,2.9999999999999997E-4,6,0,0,0]
["Chlordan","Pesticider","CAS 57-74-9",0.1,null,null,409.78,1.3332236842105263E-3,3.4000000000000002E-2,6,251188.64315095844,6.4855763592908148E-3,4.0600659341593597E-6,4.06006593415936E-10,0.1,0,0,0,0,0]
["Chloridazon","Pesticider",null,0.1,null,null,221.6,1.0000000000000001E-5,340,1.1903316981702914,2.5000285373955147,2.6306589914737206E-9,5.5210742460435099E-6,5.5210742460435101E-10,0.1,0,0.01,0,0,0]
["Chlormequat-chlorid","Pesticider",null,0.1,null,null,158.1,1.0000000000000001E-5,1000000,-1.585026652029182,3.2476729037936346E-3,6.3812474470974007E-13,6.5364588362237143E-6,6.5364588362237141E-10,0.1,1E-3,1.2999999999999999E-2,0,0,0]
["Chlorpyrifos","Pesticider","CAS 2921-88-2",0.1,null,null,350.59,6.7061151315789477E-3,0.73,5.27,43732.066516964536,1.2999342462636494E-3,4.3894358190619116E-6,4.389435819061912E-10,0.1,0,0,0,0,0]
["Clopyralid","Pesticider",null,0.1,null,null,190.2,1.33E-3,143000,-2.630784142589857,2.6545107699191522E-4,7.1400266349192142E-10,5.9594092290781189E-6,5.9594092290781187E-10,0.1,2.0000000000000001E-4,4.6993029190504762E-3,0,0,0]
["Cyanazin","Pesticider",null,0.1,null,null,240.7,1.9999999999999999E-7,171,2.1003705451175629,22.099648537452143,1.1362756272522344E-10,5.2974933517857652E-6,5.297493351785765E-10,0.1,1E-3,3.4657359027997266E-3,0,0,0]
["Dalapon","Pesticider","CAS 1582-09-8",0.1,null,null,143,1.0000000000000001E-5,502000,0.78031731214015132,0.93654792207310289,1.1497569304501517E-12,6.8729066743151811E-6,6.8729066743151817E-10,0.1,2.0000000000000001E-4,2.7725887222397813E-3,0,0,0]
["DDT","Pesticider","CAS 50-29-3",0.1,null,0.5,354.49,1.7198585526315791E-5,7.7000000000000002E-3,6.19,395913.21672816743,3.1958008612703614E-4,4.365223366587167E-6,4.3652233665871671E-10,0.1,0,0,0,0,0]
["Dicamba","Pesticider",null,0.1,null,null,221,1.67E-3,250000,-1.8860566476931633,1.5794325587258507E-3,5.9585755731821318E-10,5.5285638369785971E-6,5.5285638369785974E-10,0.1,1E-3,2.1000000000000001E-2,0,0,0]
["Dichlobenil","Pesticider",null,0.1,null,null,172,8.7999999999999995E-2,21,2.6998377258672459,92.86054642898695,2.9091461509974477E-4,6.2667770174186442E-6,6.2667770174186447E-10,0.1,6.9999999999999999E-4,0,0,0,0]
["Dichlorprop","Pesticider",null,0.1,null,null,235.1,1.0000000000000001E-5,350,1.7708520116421442,10.038899167159663,2.7111796779842754E-9,5.3602142741758642E-6,5.3602142741758642E-10,0.1,5.0000000000000001E-4,0.02,0,0,0]
["Dieldrin","Pesticider","CAS 60-57-1",0.03,null,null,380.91,4.1329934210526312E-4,0.2,5.16,33604.698246070009,3.1770994425452782E-4,4.2111167138085211E-6,4.2111167138085215E-10,0.1,0,0,0,0,0]
["Difenzoquat-methyl sulfat","Pesticider",null,0.1,null,null,360.4,1.0000000000000001E-5,8.1700000000000002E-3,-0.61978875828839397,3.276571816784829E-2,1.7804773019368641E-4,4.3292839798313559E-6,4.3292839798313559E-10,0.1,6.0000000000000002E-5,6.9314718055994533E-4,0,0,0]
["Dimethoat","Pesticider",null,0.1,null,null,229.3,2.4699999999999999E-4,39800,0.70671778233675875,{"$f":"POWER(10,(1.04*J138-0.84))","v":0.78521121450259668},{"$f":"H138*G138/(8.314*I138*298)","v":5.7436987242664961E-10},{"$f":"0.0000093*(78.1/G138)^0.5","v":5.4275825576779521E-6},{"$f":"M138*0.0001","v":5.4275825576779522E-10},0.1,1E-3,0,0,0,0]
["Dinoseb","Pesticider",null,0.1,null,null,240.2,1.2999999999999999E-4,52,3.5599066250361124,728.28755710835708,2.4237438911967036E-7,5.3030041130301153E-6,5.3030041130301159E-10,0.1,7.0000000000000001E-3,7.0000000000000001E-3,0,0,0]
["Diuron","Pesticider",null,0.1,null,null,233.1,1.15E-6,37,2.869818207979328,139.511798143829,2.9242338870474802E-9,5.3831605018257624E-6,5.3831605018257628E-10,0.1,0,0.1,0,0,0]
["DNOC","Pesticider",null,0.1,null,null,198.13,1.6E-2,198,1.7799570512469061,10.260188348734598,6.4621754889484751E-6,5.8389310349713213E-6,5.8389310349713216E-10,0.1,6.0000000000000001E-3,6.8999999999999999E-3,0,0,0]
["Endosulfan-sulfat","Pesticider","CAS 1031-07-8",0.1,null,null,422.92,1.2998930921052632E-3,0.11700000000000001,3.66,925.55024476343749,1.8965037831605422E-3,3.9964957340020199E-6,3.9964957340020202E-10,0.1,0,0,0,0,0]
["Endrin","Pesticider","CAS 72-20-8",0.1,null,null,380.92,2.6664473684210522E-5,0.23,5.2,36982.817978026731,1.7824307717726789E-5,4.2110614378404439E-6,4.2110614378404439E-10,0.1,0,0,0,0,0]
["Ethofumesat","Pesticider",null,0.1,null,null,286.3,6.4999999999999997E-4,50,2.6998377258672459,92.86054642898695,1.5022368673846817E-6,4.8573320318197262E-6,4.8573320318197266E-10,0.1,2.0000000000000001E-4,5.5451774444795626E-3,0,0,0]
["Ethylenthiurea","Pesticider",null,0.1,null,null,102.16,0.66,20000,-0.65757731917779372,2.9930887050576924E-2,1.3607192848482305E-6,8.131450514553618E-6,8.1314505145536184E-10,0.1,0.02,0.03,0,0,0]
["Fenpropimorph","Pesticider",null,0.1,null,null,303.5,3.5000000000000001E-3,4.3,4.1000257301078626,2654.7691321114507,9.9708458006843065E-5,4.717686934979309E-6,4.7176869349793089E-10,0.1,2.0000000000000001E-4,1.9E-2,0,0,0]
["Fluazifop-butyl","Pesticider",null,0.1,null,null,383.4,5.5000000000000002E-5,1,4.5000030680516936,6918.3605383919203,8.5111552762139689E-6,4.1974198423952463E-6,4.1974198423952467E-10,0.1,1E-3,0.27,0,0,0]
["Glyphosat","Pesticider",null,0.1,null,null,169,1.31E-5,10500,-3.2006594505464183,6.7813189520507275E-5,8.5102519340555605E-11,6.3221546211125239E-6,6.3221546211125243E-10,0.1,0.03,5.0000000000000001E-3,0,0,0]
["Heptachlor","Pesticider","CAS 76-44-8",0.03,null,null,373.32,3.9996710526315787E-2,0.56000000000000005,5.44,65705.239096355523,1.0761956214220592E-2,4.2537095955233306E-6,4.253709595523331E-10,0.1,0,0,0,0,0]
["Hexazinon","Pesticider",null,0.1,null,null,252.3,3.0000000000000001E-5,33000,1.1986570869544226,2.5503710528832153,9.2575972106415629E-11,5.1742789740511641E-6,5.1742789740511642E-10,0.1,2.9999999999999997E-4,4.0000000000000001E-3,0,0,0]
["Isoproturon","Pesticider",null,0.1,null,null,206.3,3.1499999999999999E-6,70.2,2.4996870826184039,57.500889889081044,3.7363399659227995E-9,5.722144905279318E-6,5.7221449052793187E-10,0.1,0,0,0,0,0]
["Lenacil","Pesticider",null,0.1,null,null,234.3,1.9999999999999999E-7,3,2.3010299956639813,35.733141200232112,6.3045594638622006E-9,5.3693575034635196E-6,5.36935750346352E-10,0.1,0,8.0000000000000002E-3,0,0,0]
["Linuron","Pesticider",null,0.1,null,null,249.1,5.1000000000000004E-3,63.8,3,190.54607179632498,8.0370550059255866E-6,5.207407949372151E-6,5.2074079493721516E-10,0.1,0.03,0.02,0,0,0]
["Malathion","Pesticider",null,0.1,null,null,330.4,4.4999999999999999E-4,145,2.7497363155690611,104.64675557404051,4.138645861128667E-7,4.5215615405668394E-6,4.5215615405668396E-10,0.1,0.3,0.2,0,0,0]
["Maleinhydrazid","Pesticider",null,0.1,null,null,112.1,1.0000000000000001E-5,144,-1.9586073148417751,1.327542374877296E-3,3.1420770908866516E-9,7.7625723179865743E-6,7.7625723179865744E-10,0.1,1E-3,1.2E-2,0,0,0]
["MCPA","Pesticider",null,0.1,null,null,200.6,2.3E-5,273.89999999999998,-0.72124639904717103,2.5698261553296454E-2,6.7989280961273608E-9,5.8028721358414597E-6,5.8028721358414604E-10,0.1,0,7.0000000000000007E-2,0,0,0]
["Mechlorprop-MCPP","Pesticider",null,0.1,null,null,214.6,1.6000000000000001E-3,250000,0.10037054511756291,0.18381687007554795,5.5434917733975036E-10,5.6103971681129828E-6,5.6103971681129831E-10,0.1,0,2.9999999999999997E-4,0,0,0]
["Metamitron","Pesticider",null,0.1,null,null,202.2,8.6000000000000002E-7,1700,0.82994669594163595,1.0547379290035384,4.1286151023948405E-11,5.7798675967708619E-6,5.7798675967708619E-10,0.1,1E-3,0.02,0,0,0]
["Methabenzthiazuron","Pesticider",null,0.1,null,null,221.3,5.9000000000000003E-6,59,2.6394864892685859,80.364814915350181,8.9321319420787779E-9,5.5248152341041783E-6,5.5248152341041788E-10,0.1,6.0000000000000002E-5,1.8990333713971104E-3,0,0,0]
["Metribuzin","Pesticider",null,0.1,null,null,214.3,1.21E-4,1000,1.6020599913279623,6.7010427871772684,1.0466012693072088E-8,5.6143228109266796E-6,5.6143228109266797E-10,0.1,4.0000000000000001E-3,0.01,0,0,0]
["Mevinphos","Pesticider","CAS 7786-34-7",0.1,null,null,224.16,0.39996710526315793,100000000,0.13,0.19733312795365029,3.6187293978051691E-10,5.489457240227965E-6,5.4894572402279657E-10,0.1,0,0.03,0,0,0]
["p,p'-DDD","Pesticider","CAS 75-54-8",0.1,null,0.5,320.5,1.0999095394736843E-3,0.16,6.2,405508.53544838459,8.8928043110683501E-4,4.590864223800662E-6,4.590864223800662E-10,0.1,0,0,0,0,0]
["p,p'-DDE","Pesticider","CAS 72-55-9",0.1,null,0.5,319.02999999999997,1.8665131578947368E-3,1.2999999999999999E-3,6.9,2167704.1048197038,0.18488128165029744,4.6014287700684043E-6,4.6014287700684047E-10,0.1,0,0,0,0,0]
["Parathion","Pesticider",null,0.1,null,0.1,291.60000000000002,5.0299999999999997E-3,11,3.8299466959416359,1390.4153823199463,5.3819112935053861E-5,4.8129871887438415E-6,4.8129871887438417E-10,0.1,1E-3,3.0000000000000001E-3,0,0,0]
["Pendimethalin","Pesticider",null,0.1,null,null,281.3,1.9400000000000001E-3,0.33,5.2000018654066018,36982.983183148506,6.6746921191514533E-4,4.9003105018534477E-6,4.9003105018534485E-10,0.1,2.9999999999999997E-4,0.03,0,0,0]
["Phenmedipham","Pesticider",null,0.1,null,null,300.3,6.9999999999999997E-7,1.8,3.5899496013257077,782.61395089726091,4.7136201625354718E-8,4.7427561885191046E-6,4.742756188519105E-10,0.1,1E-3,3.46,0,0,0]
["Pirimicarb","Pesticider",null,0.1,null,null,238.8,4.2999999999999999E-4,3000,1.6989700043360187,8.451402868501253,1.3815138369339013E-8,5.3185262155532937E-6,5.3185262155532937E-10,0.1,1E-3,0.03,0,0,0]
["Prochloraz","Pesticider",null,0.1,null,null,376.7,1.4999999999999999E-4,34.4,4.1199813073041538,2784.7137523617475,6.6298263352278973E-7,4.2345830556772318E-6,4.2345830556772321E-10,0.1,2.9999999999999997E-4,3.0000000000000001E-3,0,0,0]
["Propiconazol","Pesticider",null,0.1,null,null,342.2,5.3000000000000001E-5,150,3.7199938263676038,1068.546877164714,4.8802079885737593E-8,4.4429196886100616E-6,4.4429196886100617E-10,0.1,6.0000000000000002E-5,1.0898540574841907E-3,0,0,0]
["Quintozen","Pesticider",null,0.1,null,null,295.35000000000002,1.2699999999999999E-2,0.44,4.0934216851622347,{"$f":"POWER(10,(1.04*J170-0.84))","v":2613.1151784079102},3.4408182688535393E-3,4.7823348123048891E-6,{"$f":"M170*0.0001","v":4.7823348123048897E-10},0.1,6.0000000000000002E-5,6.9314718055994527E-5,0,0,0]
["Silfotep","Pesticider","CAS 3689-24-5",0.1,null,null,322.3,2.266480263157895E-2,30,3.02,199.89411112356615,9.8279900485339356E-5,4.5780266103476501E-6,4.5780266103476502E-10,0.1,0,0,0,0,0]
["Simazin","Pesticider",null,0.1,null,null,201.66,2.9399999999999998E-6,6.2,2.1000257301078626,22.081407847319863,3.8596606261187134E-8,5.7876010140958739E-6,5.7876010140958742E-10,0.1,2.9999999999999997E-4,2E-3,0,0,0]
["Simazin, hydroxy","Pesticider",null,0.1,null,null,183.21,6.6000000000000003E-6,32.799999999999997,1.67,5,1.487965912969161E-8,6.0720295739734434E-6,6.0720295739734433E-10,0.1,0,6.9314718055994533E-4,0,0,0]
["Sum af pesticider","Pesticider",null,0.5,null,null," -"," -"," -"," -"," -"," -"," -"," -"," -",null,null,null,null,null,"JAF (ift GVK)","2022-08-10"]
["Terbuthylazin","Pesticider",null,null,null,null,229.7,1.4999999999999999E-4,8.5,3.2041199826559246,{"$f":"POWER(10,(1.04*J175-0.84))","v":310.65960231886771},{"$f":"H175*G175/(8.314*I175*298)","v":1.6360894503831595E-6},{"$f":"0.0000093*(78.1/G175)^0.5","v":5.4228546974099102E-6},{"$f":"M175*0.0001","v":5.4228546974099101E-10},0.1,2.9999999999999997E-4,2E-3,0,0,0]
["Terbuthylazin, hydroxy","Pesticider",null,null,null,null,211.27,2.9500000000000001E-6,10220,-0.86012091359876341,1.8427832236223587E-2,2.4614026750127123E-11,5.6544393393962514E-6,5.654439339396252E-10,0.1,6.0000000000000002E-5,6.9314718055994533E-4,0,0,0]
["Thiram","Pesticider",null,null,null,null,240.4,2.2000000000000001E-3,18,1.7299742856995557,9.102763451944389,1.1859280869424674E-5,5.3007977455066823E-6,5.3007977455066828E-10,0.1,1E-3,0.19804205158855578,0,0,0]
["Triadimenol","Pesticider",null,null,null,null,295.8,6.9999999999999997E-7,62,3.0799044676667209,230.72818320380591,1.347963820770835E-9,4.7786957491433089E-6,4.7786957491433086E-10,0.1,6.0000000000000002E-5,1.3078248689810288E-2,0,0,0]
["Trichloreddikesyre","Pesticider",null,null,null,null,163.4,21.28,100000000,1.3222192947339193,3.4285308887816059,1.4034514435907414E-8,6.4295775572162975E-6,6.4295775572162983E-10,0.1,1E-3,9.2419624074659368E-2,0,0,0]
["Tridemorph","Pesticider",null,null,null,null,297.5,1.2E-2,1.1000000000000001,4.1986570869544222,3362.0438262824969,1.3099334935390559E-3,4.7650227719085172E-6,4.7650227719085171E-10,0.1,1E-3,2.166084939249829E-2,0,0,0]
["Trifluralin","Pesticider",null,null,null,null,335.5,9.4999999999999998E-3,0.221,5.2699983355133169,43731.892204482341,5.8209996324455823E-3,4.4870633720639649E-6,4.487063372063965E-10,0.1,6.0000000000000002E-5,6.9314718055994527E-5,0,0,0]
["6:2 FTS","PFAS","27619‐97‐2",null,null,null,428.17,0.11,1300,4.4400000000000004,145,1.0000000000000001E-5,3.9719186777396401E-6,3.9719186777396402E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFBA","PFAS","375-22-4",null,null,null,214.04,3900,560000,2.82,71,5.9999999999999995E-4,5.6177317085828246E-6,5.6177317085828247E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFBS","PFAS","375-73-5",null,null,null,300.10000000000002,631,30000,3.9,63,2E-3,4.7443363172281195E-6,4.74433631722812E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFDA","PFAS","335-76-2",null,null,null,514.09,6.6,5140,6.5,2006,0.05,3.624840382343389E-6,3.6248403823433891E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFDoDA","PFAS","307-55-1",null,null,null,614.1,0.7,0.7,7.77,108579,0.26,3.3165680815815481E-6,3.316568081581548E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFDoDS","PFAS","79780-39-5",null,null,null,700.16,1.6000000000000001E-3,23.88,7.07,6734,7.0000000000000007E-2,3.1060598335626011E-6,3.1060598335626011E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10","Koc og Henry er bedst bud baseret på PFDS"]
["PFDS","PFAS","335-77-3",null,null,null,600.14,0.71,190,7.66,6734,7.0000000000000007E-2,3.3549200764397997E-6,3.3549200764397998E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFHpA","PFAS","375-85-9",null,null,null,364.06,158,4200,4.67,163,6.0000000000000001E-3,4.3074672396625154E-6,4.3074672396625153E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFHpS","PFAS","375-92-8",null,null,null,450.12,21,465,4.8099999999999996,400,8.0000000000000002E-3,3.8738634696925221E-6,3.8738634696925223E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10","Henry er bedst bud baseret på PFHxS og PFOS"]
["PFHxA","PFAS","307-24-4",null,null,null,314.05,457,21700,4.0599999999999996,62,3.0000000000000001E-3,4.6377685013920626E-6,4.6377685013920628E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFHxS","PFAS","307-55-1",null,null,null,400.11,58.9,2300,5.17,145,4.0000000000000001E-3,4.108835577667208E-6,4.1088355776672078E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFNA","PFAS","375-95-1",null,null,null,464.08,18.600000000000001,1200,5.92,392,0.03,3.8151537028336713E-6,3.8151537028336715E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFNS","PFAS","68259-12-1",null,null,null,550.1,1.5,222,6.78,2397,2E-3,3.5041899764971909E-6,3.5041899764971907E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFOA","PFAS","335-67-1",null,null,null,414.07,54,9500,5.3,166,0.01,4.0389788808176352E-6,4.0389788808176354E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFOS","PFAS","1763-23-1",null,null,null,500.13,6.8,570,6.43,889,0.02,3.6750818196525783E-6,3.6750818196525785E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFOSA","PFAS","754-91-6",null,null,null,499.14,0.25,4.5,5.62,1690,0.01,3.6787246139703015E-6,3.6787246139703014E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFPeA","PFAS","2706-90-3",null,null,null,264.05,1350,112600,3.43,56,1E-3,5.0578434105768386E-6,5.0578434105768388E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFPeS","PFAS","2706-91-4",null,null,null,350.1,11,1720,3.38,69,3.0000000000000001E-3,4.3925064724528124E-6,4.3925064724528126E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10","Henry er bedst bud baseret på PFBS og PFHxS"]
["PFTrDA","PFAS","72629-94-8",null,null,null,664.11,0.3,0.2,8.25,108579,0.42,3.1892492025042839E-6,3.1892492025042838E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10","Koc er bedst bud baseret på PFDoDA"]
["PFTrDS","PFAS","791563-89-8",null,null,null,750.16,3.0000000000000001E-3,54.84,7.44,6734,7.0000000000000007E-2,3.0007617407665062E-6,3.0007617407665063E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10","Koc og Henry er bedst bud baseret på PFDS"]
["PFUnDA","PFAS","2058-94-8",null,null,null,564.09,2.2000000000000002,93,7.15,7267,0.12,3.4604634388496535E-6,3.4604634388496536E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["PFUnDS","PFAS","749786-16-1",null,null,null,650.15,1.4E-3,34.979999999999997,6.49,6734,7.0000000000000007E-2,3.2233070795071708E-6,3.2233070795071708E-10,0.1,null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10","Koc og Henry er bedst bud baseret på PFDS"]
["Sum af 22 PFAS","PFAS",null,0.1,null,0.4," -"," -"," -"," -"," -"," -"," -"," -"," -",null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["Sum af 4 PFAS","PFAS",null,2E-3,null,0.01," -"," -"," -"," -"," -"," -"," -"," -"," -",null,null,null,null,null,"JAF-VMR Håndbogen 2022","2022-08-10"]
["2,4,5-Trichlorphenol","Phenoler","CAS 95-95-4",0.1,2.0000000000000002E-5,3,197.5,0.99991776315789471,1200,3.72,{"$f":"POWER(10,(1.04*J206-0.84))","v":1068.5626745999625},{"$f":"H206*G206/(8.314*I206*298)","v":6.6423820788956628E-5},{"$f":"0.0000093*(78.1/G206)^0.5","v":5.8482363456370664E-6},{"$f":"M206*0.0001","v":5.848236345637067E-10},1,5.0000000000000001E-3,0.03,0,0,0]
["2,4,6-Trichlorphenol","Phenoler","CAS 88-06-2",0.1,2.0000000000000002E-5,3,197.5,1.0665789473684211,800,3.69,994.48903715479378,1.0627811326233061E-4,5.8482363456370664E-6,5.848236345637067E-10,1,0,0.11,0,0,0]
["2,4-Dichlorphenol","Phenoler","CAS 120-83-2",0.1,2.0000000000000002E-5,3,163,11.999013157894737,4500,3.06,219.98851090492525,1.7542615151149254E-4,6.437461775453851E-6,6.4374617754538508E-10,1,0,0.02,0,0,0]
["2,4-Dimethylphenol","Phenoler","CAS 105-67-9",0.5,2E-3,70,122.2,13.598881578947369,7870,2.2999999999999998,35.645113342624434,8.5226250298167596E-5,7.4348611549106079E-6,7.4348611549106078E-10,0.1,1.2E-2,0,0,0,0]
["2-Chlorphenol","Phenoler","CAS 95-57-8",0.1,2.0000000000000002E-5,3,128.6,337.30559210526314,11300,2.15,24.888573182823915,1.5493865520244364E-3,7.2474959476817983E-6,7.247495947681799E-10,1,3.5000000000000003E-2,6.9999999999999999E-6,0,0,0]
["2-nitrophenol","Phenoler","CAS 88-75-5",0.5,5.0000000000000001E-3,125,139.11000000000001,15.065427631578947,2100,1.89,13.35365033327186,4.0280442723550992E-4,6.9683393184783224E-6,6.9683393184783225E-10,1,0.23,0.01,0,0,0]
["4-nitrophenol","Phenoler","CAS 100-02-7",0.5,5.0000000000000001E-3,125,139.11000000000001,1.3052259868421052E-2,111300,2.04,19.124936418442086,6.5844971491662095E-9,6.9683393184783224E-6,6.9683393184783225E-10,1,0.1,0,0,0,0]
["o-Cresol","Phenoler","CAS 95-48-7",0.5,3.0000000000000001E-3,70,108.1,39.863388157894732,25900,1.95,15.417004529495602,6.7154304267703875E-5,7.9048861340223873E-6,7.9048861340223877E-10,0.1,0.03,0.2,0,0,0]
["p-Cresol","Phenoler","CAS 106-44-5",0.5,3.0000000000000001E-3,70,108.1,14.665460526315789,21500,1.94,15.052200686321303,2.9761626018307287E-5,7.9048861340223873E-6,7.9048861340223877E-10,0.1,0.05,0.7,0,0,0]
["Pentachlorphenol","Phenoler","CAS 87-86-5",0.01,9.9999999999999995E-7,0.15,266.3,1.466546052631579E-2,14,5.12,30535.145939402995,1.1259330096902172E-4,5.0364309287617318E-6,5.0364309287617321E-10,1,0.04,0.2,0,0,0]
["Phenol","Phenoler","CAS 108-95-2",0.5,0.02,70,94.1,46.662828947368418,82800,1.46,4.7686999810177797,2.1404449705221416E-5,8.4725405053171745E-6,8.4725405053171748E-10,0.1,0.03,0.2,0,0,0]
["butyl benzyl phthalat (BBP)","Phthalater","CAS 85-68-7",1,null,250,312.3646,1.0999095394736843E-3,2.69,4.7300000000000004,12000.518202042691,5.1551370342671204E-5,4.6502634827001655E-6,4.650263482700166E-10,0.1,3.0000000000000001E-5,0.3,0,0,0]
["di-butyl phthalat (DBP)","Phthalater","CAS 84-74-2",1,null,250,278.34739999999999,2.6797796052631579E-3,11.2,4.5,6918.3097091893687,2.6880784526213941E-5,4.9262322268167983E-6,4.9262322268167981E-10,0.1,7.0000000000000001E-3,0.3,0,0,0]
["diethyl phthalate (DEP)","Phthalater","CAS 84-66-2",1,null,250,222.24,0.27997697368421054,1080,2.42,47.511637637756166,2.3253830554140992E-5,5.5131188035162695E-6,5.5131188035162696E-10,0.1,0.02,0.23,0,0,0]
["di-ethylhexyl phthalat (DEHP)","Phthalater","CAS 117-81-7",1,5.0000000000000001E-3,25,390.56180000000001,1.8931776315789473E-5,0.27,7.6,11587773.561551293,1.1053277660984978E-5,4.158757371519899E-6,4.1587573715198992E-10,0.1,1E-3,0.2,0,0,0]
["dimethyl phthalate (DMP)","Phthalater","CAS 131-11-3",1,null,250,194.19,0.41063289473684206,4000,1.6,6.6680676921362245,8.0462648339732758E-6,5.8978678130056403E-6,5.897867813005641E-10,0.1,0.02,0.05,0,0,0]
["di-n-octyl phthalate (DOP)","Phthalater","CAS 117-84-0",1,null,250,390.57,1.3332236842105261E-5,2.1999999999999999E-2,8.1,38370724.549227931,9.553289458427724E-5,4.1587137148265543E-6,4.1587137148265547E-10,0.1,null,null,0,0,0]

{"sheet":"Egen Stofdatabase","index":70,"n_rows":7,"n_cols":22,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["Stofnavn","Gruppe","CAS-nummer","Grundvands-kvalitets-kriterie","Afdampnings-kriterie","Jordkvalitets-kriterie","Indsat af (Initialer)","Dato","molvægt","damptryk","vand-opløselighed","okt/vand \nford. Koeff.","KOC","Henrys konstant","Diff. Koeff.\nI luft","Diffusionskoefficient vand","Vindhastighed","1. ordens nedbrydning grundvand\nanaerob","1. ordens nedbrydning grundvand\naerob","1. ordens nedbrydning umættet zone anaerob","1. ordens nedbrydning umættet zone aerob","1. ordens nedbrydning poreluft aerob"]
[null,null,null,"μg/l","mg/m³","mg/kg",null,null,"g/mol","Pa","mg/l","log Kow",null,null,"D m2/s",null,"m/s","dag-1","dag-1","dag-1","dag-1","dag-1"]
[]
[]
["Freon 113","Klorfluorkulbrinte","76-13-1",1,109,null,"JAF -MST","2014-06-06",187.38,39368,62,3.2,308,21.8,6.0000000000000002E-6,6E-10,0.1]
["Freon 11","Klorfluorkulbrinte","75-69-4",15000,570,null,"JAF -MST","2014-06-06",137.37,94962,62,2.44,49.84,4.5199999999999996,7.4699999999999996E-6,7.4700000000000001E-10,0.1]
["Freon 12","Klorfluorkulbrinte","75-71-8",10000,14,null,"JAF -MST","2014-06-06",120.91,642390,1300,2.0499999999999998,19.59,0.37,7.4699999999999996E-6,7.4700000000000001E-10,0.1]

{"sheet":"Etageadskillelse","index":71,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["Etageadskillelse"]
["Type","Reduktionsfaktor (Rkr)"]
[]
["Træ med indskud",1]
["Betondæk",10]